(module SOIC-24W_7.5x15.4mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
  (descr "24-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
  (tags "SOIC 1.27")
  (attr smd)
  (fp_text reference REF** (at 0 -8.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SOIC-24W_7.5x15.4mm_Pitch1.27mm (at 0 8.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.75 -7.7) (end 3.75 -7.7) (layer F.Fab) (width 0.15))
  (fp_line (start 3.75 -7.7) (end 3.75 7.7) (layer F.Fab) (width 0.15))
  (fp_line (start 3.75 7.7) (end -3.75 7.7) (layer F.Fab) (width 0.15))
  (fp_line (start -3.75 7.7) (end -3.75 -6.7) (layer F.Fab) (width 0.15))
  (fp_line (start -3.75 -6.7) (end -2.75 -7.7) (layer F.Fab) (width 0.15))
  (fp_line (start -5.95 -8.05) (end -5.95 8.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start 5.95 -8.05) (end 5.95 8.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.95 -8.05) (end 5.95 -8.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.95 8.05) (end 5.95 8.05) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.875 -7.875) (end -3.875 -7.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.875 -7.875) (end 3.875 -7.51) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.875 7.875) (end 3.875 7.51) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.875 7.875) (end -3.875 7.51) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.875 -7.875) (end 3.875 -7.875) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.875 7.875) (end 3.875 7.875) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.875 -7.6) (end -5.7 -7.6) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask))
  (model Housings_SOIC.3dshapes/SOIC-24_7.5x15.4mm_Pitch1.27mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
