Inlined call (byte~) vicSelectGfxBank::$0 ← call toDd00 (byte*) vicSelectGfxBank::gfx 

CONTROL FLOW GRAPH SSA
@begin: scope:[]  from
  (byte*) PROCPORT_DDR#0 ← ((byte*)) (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) PROCPORT_DDR_MEMORY_MASK#0 ← (byte/signed byte/word/signed word/dword/signed dword) 7
  (byte*) PROCPORT#0 ← ((byte*)) (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) PROCPORT_RAM_ALL#0 ← (byte/signed byte/word/signed word/dword/signed dword) 48
  (byte) PROCPORT_RAM_IO#0 ← (byte/signed byte/word/signed word/dword/signed dword) 53
  (byte) PROCPORT_RAM_CHARROM#0 ← (byte/signed byte/word/signed word/dword/signed dword) 49
  (byte) PROCPORT_KERNEL_IO#0 ← (byte/signed byte/word/signed word/dword/signed dword) 54
  (byte) PROCPORT_BASIC_KERNEL_IO#0 ← (byte/signed byte/word/signed word/dword/signed dword) 55
  (byte*) CHARGEN#0 ← ((byte*)) (word/dword/signed dword) 53248
  (word) SPRITE_PTRS#0 ← (word/signed word/dword/signed dword) 1016
  (byte*) SPRITES_XPOS#0 ← ((byte*)) (word/dword/signed dword) 53248
  (byte*) SPRITES_YPOS#0 ← ((byte*)) (word/dword/signed dword) 53249
  (byte*) SPRITES_XMSB#0 ← ((byte*)) (word/dword/signed dword) 53264
  (byte*) RASTER#0 ← ((byte*)) (word/dword/signed dword) 53266
  (byte*) SPRITES_ENABLE#0 ← ((byte*)) (word/dword/signed dword) 53269
  (byte*) SPRITES_EXPAND_Y#0 ← ((byte*)) (word/dword/signed dword) 53271
  (byte*) SPRITES_PRIORITY#0 ← ((byte*)) (word/dword/signed dword) 53275
  (byte*) SPRITES_MC#0 ← ((byte*)) (word/dword/signed dword) 53276
  (byte*) SPRITES_EXPAND_X#0 ← ((byte*)) (word/dword/signed dword) 53277
  (byte*) BORDERCOL#0 ← ((byte*)) (word/dword/signed dword) 53280
  (byte*) BGCOL#0 ← ((byte*)) (word/dword/signed dword) 53281
  (byte*) BGCOL1#0 ← ((byte*)) (word/dword/signed dword) 53281
  (byte*) BGCOL2#0 ← ((byte*)) (word/dword/signed dword) 53282
  (byte*) BGCOL3#0 ← ((byte*)) (word/dword/signed dword) 53283
  (byte*) BGCOL4#0 ← ((byte*)) (word/dword/signed dword) 53284
  (byte*) SPRITES_MC1#0 ← ((byte*)) (word/dword/signed dword) 53285
  (byte*) SPRITES_MC2#0 ← ((byte*)) (word/dword/signed dword) 53286
  (byte*) SPRITES_COLS#0 ← ((byte*)) (word/dword/signed dword) 53287
  (byte*) VIC_CONTROL#0 ← ((byte*)) (word/dword/signed dword) 53265
  (byte*) D011#0 ← ((byte*)) (word/dword/signed dword) 53265
  (byte) VIC_RST8#0 ← (byte/word/signed word/dword/signed dword) 128
  (byte) VIC_ECM#0 ← (byte/signed byte/word/signed word/dword/signed dword) 64
  (byte) VIC_BMM#0 ← (byte/signed byte/word/signed word/dword/signed dword) 32
  (byte) VIC_DEN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) VIC_RSEL#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte*) VIC_CONTROL2#0 ← ((byte*)) (word/dword/signed dword) 53270
  (byte*) D016#0 ← ((byte*)) (word/dword/signed dword) 53270
  (byte) VIC_MCM#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) VIC_CSEL#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte*) D018#0 ← ((byte*)) (word/dword/signed dword) 53272
  (byte*) VIC_MEMORY#0 ← ((byte*)) (word/dword/signed dword) 53272
  (byte*) LIGHTPEN_X#0 ← ((byte*)) (word/dword/signed dword) 53267
  (byte*) LIGHTPEN_Y#0 ← ((byte*)) (word/dword/signed dword) 53268
  (byte*) IRQ_STATUS#0 ← ((byte*)) (word/dword/signed dword) 53273
  (byte*) IRQ_ENABLE#0 ← ((byte*)) (word/dword/signed dword) 53274
  (byte) IRQ_RASTER#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) IRQ_COLLISION_BG#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) IRQ_COLLISION_SPRITE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) IRQ_LIGHTPEN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte*) COLS#0 ← ((byte*)) (word/dword/signed dword) 55296
  (byte*) CIA1_PORT_A#0 ← ((byte*)) (word/dword/signed dword) 56320
  (byte*) CIA1_PORT_B#0 ← ((byte*)) (word/dword/signed dword) 56321
  (byte*) CIA1_PORT_A_DDR#0 ← ((byte*)) (word/dword/signed dword) 56322
  (byte*) CIA1_PORT_B_DDR#0 ← ((byte*)) (word/dword/signed dword) 56323
  (byte*) CIA1_INTERRUPT#0 ← ((byte*)) (word/dword/signed dword) 56333
  (byte) CIA_INTERRUPT_CLEAR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 127
  (byte*) CIA2_PORT_A#0 ← ((byte*)) (word/dword/signed dword) 56576
  (byte*) CIA2_PORT_B#0 ← ((byte*)) (word/dword/signed dword) 56577
  (byte*) CIA2_PORT_A_DDR#0 ← ((byte*)) (word/dword/signed dword) 56578
  (byte*) CIA2_PORT_B_DDR#0 ← ((byte*)) (word/dword/signed dword) 56579
  (byte*) CIA2_INTERRUPT#0 ← ((byte*)) (word/dword/signed dword) 56589
  (void()**) KERNEL_IRQ#0 ← ((void()**)) (word/signed word/dword/signed dword) 788
  (void()**) HARDWARE_IRQ#0 ← ((void()**)) (word/dword/signed dword) 65534
  (byte) BLACK#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) WHITE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) RED#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) CYAN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 3
  (byte) PURPLE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) GREEN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 5
  (byte) BLUE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 6
  (byte) YELLOW#0 ← (byte/signed byte/word/signed word/dword/signed dword) 7
  (byte) ORANGE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) BROWN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 9
  (byte) PINK#0 ← (byte/signed byte/word/signed word/dword/signed dword) 10
  (byte) DARK_GREY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 11
  (byte) GREY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 12
  (byte) LIGHT_GREEN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 13
  (byte) LIGHT_BLUE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 14
  (byte) LIGHT_GREY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 15
  to:@4
@4: scope:[]  from @begin
  (byte*) DTV_FEATURE#0 ← ((byte*)) (word/dword/signed dword) 53311
  (byte) DTV_FEATURE_ENABLE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_FEATURE_DISABLE_TIL_RESET#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte*) DTV_CONTROL#0 ← ((byte*)) (word/dword/signed dword) 53308
  (byte) DTV_LINEAR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BORDER_OFF#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_HIGHCOLOR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_OVERSCAN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) DTV_COLORRAM_OFF#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) DTV_BADLINE_OFF#0 ← (byte/signed byte/word/signed word/dword/signed dword) 32
  (byte) DTV_CHUNKY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 64
  (byte*) DTV_PALETTE#0 ← ((byte*)) (word/dword/signed dword) 53760
  (byte[16]) DTV_PALETTE_DEFAULT#0 ← { (byte/signed byte/word/signed word/dword/signed dword) 0, (byte/signed byte/word/signed word/dword/signed dword) 15, (byte/signed byte/word/signed word/dword/signed dword) 54, (byte/word/signed word/dword/signed dword) 190, (byte/signed byte/word/signed word/dword/signed dword) 88, (byte/word/signed word/dword/signed dword) 219, (byte/word/signed word/dword/signed dword) 134, (byte/word/signed word/dword/signed dword) 255, (byte/signed byte/word/signed word/dword/signed dword) 41, (byte/signed byte/word/signed word/dword/signed dword) 38, (byte/signed byte/word/signed word/dword/signed dword) 59, (byte/signed byte/word/signed word/dword/signed dword) 5, (byte/signed byte/word/signed word/dword/signed dword) 7, (byte/word/signed word/dword/signed dword) 223, (byte/word/signed word/dword/signed dword) 154, (byte/signed byte/word/signed word/dword/signed dword) 10 }
  (byte*) DTV_PLANEA_START_LO#0 ← ((byte*)) (word/dword/signed dword) 53306
  (byte*) DTV_PLANEA_START_MI#0 ← ((byte*)) (word/dword/signed dword) 53307
  (byte*) DTV_PLANEA_START_HI#0 ← ((byte*)) (word/dword/signed dword) 53317
  (byte*) DTV_PLANEA_STEP#0 ← ((byte*)) (word/dword/signed dword) 53318
  (byte*) DTV_PLANEA_MODULO_LO#0 ← ((byte*)) (word/dword/signed dword) 53304
  (byte*) DTV_PLANEA_MODULO_HI#0 ← ((byte*)) (word/dword/signed dword) 53305
  (byte*) DTV_PLANEB_START_LO#0 ← ((byte*)) (word/dword/signed dword) 53321
  (byte*) DTV_PLANEB_START_MI#0 ← ((byte*)) (word/dword/signed dword) 53322
  (byte*) DTV_PLANEB_START_HI#0 ← ((byte*)) (word/dword/signed dword) 53323
  (byte*) DTV_PLANEB_STEP#0 ← ((byte*)) (word/dword/signed dword) 53324
  (byte*) DTV_PLANEB_MODULO_LO#0 ← ((byte*)) (word/dword/signed dword) 53319
  (byte*) DTV_PLANEB_MODULO_HI#0 ← ((byte*)) (word/dword/signed dword) 53320
  (byte*) DTV_SPRITE_BANK#0 ← ((byte*)) (word/dword/signed dword) 53325
  (byte*) DTV_COLOR_BANK_LO#0 ← ((byte*)) (word/dword/signed dword) 53302
  (byte*) DTV_COLOR_BANK_HI#0 ← ((byte*)) (word/dword/signed dword) 53303
  (dword) DTV_COLOR_BANK_DEFAULT#0 ← (dword/signed dword) 120832
  (byte*) DTV_GRAPHICS_VIC_BANK#0 ← ((byte*)) (word/dword/signed dword) 53309
  (byte*) DTV_GRAPHICS_HICOL_BANK#0 ← ((byte*)) (word/dword/signed dword) 53310
  to:@5
dtvSetCpuBankSegment1: scope:[dtvSetCpuBankSegment1]  from gfx_init_chunky gfx_init_chunky::@4 gfx_init_chunky::@6
  (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 ← phi( gfx_init_chunky/(byte) dtvSetCpuBankSegment1::cpuBankIdx#0 gfx_init_chunky::@4/(byte) dtvSetCpuBankSegment1::cpuBankIdx#1 gfx_init_chunky::@6/(byte) dtvSetCpuBankSegment1::cpuBankIdx#2 )
  (byte*) dtvSetCpuBankSegment1::cpuBank#0 ← ((byte*)) (byte/word/signed word/dword/signed dword) 255
  *((byte*) dtvSetCpuBankSegment1::cpuBank#0) ← (byte) dtvSetCpuBankSegment1::cpuBankIdx#3
  asm { .byte$32,$dd lda$ff .byte$32,$00  }
  to:dtvSetCpuBankSegment1::@return
dtvSetCpuBankSegment1::@return: scope:[dtvSetCpuBankSegment1]  from dtvSetCpuBankSegment1
  return 
  to:@return
@5: scope:[]  from @4
  (byte*) DTV_BLITTER_SRCA_LO#0 ← ((byte*)) (word/dword/signed dword) 54048
  (byte*) DTV_BLITTER_SRCA_MI#0 ← ((byte*)) (word/dword/signed dword) 54049
  (byte*) DTV_BLITTER_SRCA_HI#0 ← ((byte*)) (word/dword/signed dword) 54050
  (byte*) DTV_BLITTER_SRCA_MOD_LO#0 ← ((byte*)) (word/dword/signed dword) 54051
  (byte*) DTV_BLITTER_SRCA_MOD_HI#0 ← ((byte*)) (word/dword/signed dword) 54052
  (byte*) DTV_BLITTER_SRCA_LIN_LO#0 ← ((byte*)) (word/dword/signed dword) 54053
  (byte*) DTV_BLITTER_SRCA_LIN_HI#0 ← ((byte*)) (word/dword/signed dword) 54054
  (byte*) DTV_BLITTER_SRCA_STEP#0 ← ((byte*)) (word/dword/signed dword) 54055
  (byte*) DTV_BLITTER_SRCB_LO#0 ← ((byte*)) (word/dword/signed dword) 54056
  (byte*) DTV_BLITTER_SRCB_MI#0 ← ((byte*)) (word/dword/signed dword) 54057
  (byte*) DTV_BLITTER_SRCB_HI#0 ← ((byte*)) (word/dword/signed dword) 54058
  (byte*) DTV_BLITTER_SRCB_MOD_LO#0 ← ((byte*)) (word/dword/signed dword) 54059
  (byte*) DTV_BLITTER_SRCB_MOD_HI#0 ← ((byte*)) (word/dword/signed dword) 54060
  (byte*) DTV_BLITTER_SRCB_LIN_LO#0 ← ((byte*)) (word/dword/signed dword) 54061
  (byte*) DTV_BLITTER_SRCB_LIN_HI#0 ← ((byte*)) (word/dword/signed dword) 54062
  (byte*) DTV_BLITTER_SRCB_STEP#0 ← ((byte*)) (word/dword/signed dword) 54063
  (byte*) DTV_BLITTER_DEST_LO#0 ← ((byte*)) (word/dword/signed dword) 54064
  (byte*) DTV_BLITTER_DEST_MI#0 ← ((byte*)) (word/dword/signed dword) 54065
  (byte*) DTV_BLITTER_DEST_HI#0 ← ((byte*)) (word/dword/signed dword) 54066
  (byte*) DTV_BLITTER_DEST_MOD_LO#0 ← ((byte*)) (word/dword/signed dword) 54067
  (byte*) DTV_BLITTER_DEST_MOD_HI#0 ← ((byte*)) (word/dword/signed dword) 54068
  (byte*) DTV_BLITTER_DEST_LIN_LO#0 ← ((byte*)) (word/dword/signed dword) 54069
  (byte*) DTV_BLITTER_DEST_LIN_HI#0 ← ((byte*)) (word/dword/signed dword) 54070
  (byte*) DTV_BLITTER_DEST_STEP#0 ← ((byte*)) (word/dword/signed dword) 54071
  (byte*) DTV_BLITTER_LEN_LO#0 ← ((byte*)) (word/dword/signed dword) 54072
  (byte*) DTV_BLITTER_LEN_HI#0 ← ((byte*)) (word/dword/signed dword) 54073
  (byte*) DTV_BLITTER_CONTROL#0 ← ((byte*)) (word/dword/signed dword) 54074
  (byte) DTV_BLIT_FORCE_START#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_SRCA_FWD#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_BLIT_SRCB_FWD#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_BLIT_DEST_FWD#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) DTV_BLIT_VIC_IRQ#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) DTV_BLIT_CIA_IRQ#0 ← (byte/signed byte/word/signed word/dword/signed dword) 32
  (byte) DTV_BLIT_VBLANK#0 ← (byte/signed byte/word/signed word/dword/signed dword) 64
  (byte) DTV_BLIT_IRQ_EN#0 ← (byte/word/signed word/dword/signed dword) 128
  (byte*) DTV_BLITTER_TRANSPARANCY#0 ← ((byte*)) (word/dword/signed dword) 54075
  (byte) DTV_BLIT_DISABLE_B#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_WRITE_TRANSPARENT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_BLIT_WRITE_NONTRANSPARENT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_BLIT_TRANSPARANCY_NONE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte*) DTV_BLITTER_ALU#0 ← ((byte*)) (word/dword/signed dword) 54078
  (byte) DTV_BLIT_SHIFT0#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) DTV_BLIT_SHIFT1#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_SHIFT2#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_BLIT_SHIFT3#0 ← (byte/signed byte/word/signed word/dword/signed dword) 3
  (byte) DTV_BLIT_SHIFT4#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_BLIT_SHIFT5#0 ← (byte/signed byte/word/signed word/dword/signed dword) 5
  (byte) DTV_BLIT_SHIFT6#0 ← (byte/signed byte/word/signed word/dword/signed dword) 6
  (byte) DTV_BLIT_SHIFT7#0 ← (byte/signed byte/word/signed word/dword/signed dword) 7
  (byte) DTV_BLIT_AND#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) DTV_BLIT_NAND#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) DTV_BLIT_NOR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) DTV_BLIT_OR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 24
  (byte) DTV_BLIT_XOR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 32
  (byte) DTV_BLIT_XNOR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 40
  (byte) DTV_BLIT_ADD#0 ← (byte/signed byte/word/signed word/dword/signed dword) 48
  (byte) DTV_BLIT_SUB#0 ← (byte/signed byte/word/signed word/dword/signed dword) 56
  (byte*) DTV_BLITTER_CONTROL2#0 ← ((byte*)) (word/dword/signed dword) 54079
  (byte) DTV_BLIT_CLEAR_IRQ#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_SRCA_CONT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_BLIT_SRCB_CONT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_BLIT_DEST_CONT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) DTV_BLIT_STATUS_BUSY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_STATUS_IRQ#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte*) CHUNKY#0 ← ((byte*)) (word/dword/signed dword) 32768
  to:@7
main: scope:[main]  from @7
  asm { sei  }
  *((byte*) PROCPORT_DDR#0) ← (byte) PROCPORT_DDR_MEMORY_MASK#0
  *((byte*) PROCPORT#0) ← (byte) PROCPORT_RAM_IO#0
  call gfx_init_chunky 
  to:main::@17
main::@17: scope:[main]  from main
  *((byte*) DTV_FEATURE#0) ← (byte) DTV_FEATURE_ENABLE#0
  (byte~) main::$1 ← (byte) DTV_HIGHCOLOR#0 | (byte) DTV_LINEAR#0
  (byte~) main::$2 ← (byte~) main::$1 | (byte) DTV_COLORRAM_OFF#0
  (byte~) main::$3 ← (byte~) main::$2 | (byte) DTV_CHUNKY#0
  (byte~) main::$4 ← (byte~) main::$3 | (byte) DTV_BADLINE_OFF#0
  *((byte*) DTV_CONTROL#0) ← (byte~) main::$4
  (byte~) main::$5 ← (byte) VIC_DEN#0 | (byte) VIC_ECM#0
  (byte~) main::$6 ← (byte~) main::$5 | (byte) VIC_RSEL#0
  (byte/word/dword~) main::$7 ← (byte~) main::$6 | (byte/signed byte/word/signed word/dword/signed dword) 3
  *((byte*) VIC_CONTROL#0) ← (byte/word/dword~) main::$7
  (byte~) main::$8 ← (byte) VIC_MCM#0 | (byte) VIC_CSEL#0
  *((byte*) VIC_CONTROL2#0) ← (byte~) main::$8
  (byte~) main::$9 ← < (byte*) CHUNKY#0
  *((byte*) DTV_PLANEB_START_LO#0) ← (byte~) main::$9
  (byte~) main::$10 ← > (byte*) CHUNKY#0
  *((byte*) DTV_PLANEB_START_MI#0) ← (byte~) main::$10
  *((byte*) DTV_PLANEB_START_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  *((byte*) DTV_PLANEB_STEP#0) ← (byte/signed byte/word/signed word/dword/signed dword) 8
  *((byte*) DTV_PLANEB_MODULO_LO#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  *((byte*) DTV_PLANEB_MODULO_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  *((byte*) CIA2_PORT_A_DDR#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3
  (word~) main::$11 ← ((word)) (byte*) CHUNKY#0
  (word/signed dword/dword~) main::$12 ← (word~) main::$11 / (word/signed word/dword/signed dword) 16384
  (byte~) main::$13 ← ((byte)) (word/signed dword/dword~) main::$12
  (byte/word/dword~) main::$14 ← (byte/signed byte/word/signed word/dword/signed dword) 3 ^ (byte~) main::$13
  *((byte*) CIA2_PORT_A#0) ← (byte/word/dword~) main::$14
  (word~) main::$15 ← ((word)) (byte*) CHUNKY#0
  (word~) main::$16 ← (word~) main::$15 & (word/signed word/dword/signed dword) 16383
  (word~) main::$17 ← (word~) main::$16 >> (byte/signed byte/word/signed word/dword/signed dword) 6
  (byte~) main::$18 ← ((byte)) (word~) main::$17
  (word~) main::$19 ← ((word)) (byte*) CHUNKY#0
  (word~) main::$20 ← (word~) main::$19 & (word/signed word/dword/signed dword) 16383
  (byte~) main::$21 ← > (word~) main::$20
  (byte~) main::$22 ← (byte~) main::$21 >> (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte~) main::$23 ← (byte~) main::$18 | (byte~) main::$22
  *((byte*) VIC_MEMORY#0) ← (byte~) main::$23
  (byte) main::j#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  to:main::@1
main::@1: scope:[main]  from main::@1 main::@17
  (byte) main::j#2 ← phi( main::@1/(byte) main::j#1 main::@17/(byte) main::j#0 )
  *((byte*) DTV_PALETTE#0 + (byte) main::j#2) ← (byte) main::j#2
  (byte) main::j#1 ← (byte) main::j#2 + rangenext(0,15)
  (bool~) main::$24 ← (byte) main::j#1 != rangelast(0,15)
  if((bool~) main::$24) goto main::@1
  to:main::@2
main::@2: scope:[main]  from main::@1 main::@8
  if(true) goto main::@3
  to:main::@return
main::@3: scope:[main]  from main::@2
  asm { ldx#$ff rff: cpxRASTER bnerff stabilize: nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop cpxRASTER beqeat+0 eat: inx cpx#$08 bnestabilize  }
  (byte~) main::$25 ← (byte) VIC_DEN#0 | (byte) VIC_ECM#0
  (byte~) main::$26 ← (byte~) main::$25 | (byte) VIC_RSEL#0
  (byte/word/dword~) main::$27 ← (byte~) main::$26 | (byte/signed byte/word/signed word/dword/signed dword) 3
  *((byte*) VIC_CONTROL#0) ← (byte/word/dword~) main::$27
  *((byte*) BORDERCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) main::rst#0 ← (byte/signed byte/word/signed word/dword/signed dword) 66
  to:main::@5
main::@5: scope:[main]  from main::@3 main::@6
  (byte) main::rst#2 ← phi( main::@3/(byte) main::rst#0 main::@6/(byte) main::rst#3 )
  (bool~) main::$28 ← *((byte*) RASTER#0) != (byte) main::rst#2
  if((bool~) main::$28) goto main::@6
  to:main::@7
main::@6: scope:[main]  from main::@5
  (byte) main::rst#3 ← phi( main::@5/(byte) main::rst#2 )
  to:main::@5
main::@7: scope:[main]  from main::@5
  asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
  to:main::@8
main::@8: scope:[main]  from main::@7 main::@8
  (byte) main::rst#1 ← *((byte*) RASTER#0)
  (byte~) main::$29 ← (byte) VIC_DEN#0 | (byte) VIC_ECM#0
  (byte~) main::$30 ← (byte~) main::$29 | (byte) VIC_RSEL#0
  (byte~) main::$31 ← (byte) main::rst#1 & (byte/signed byte/word/signed word/dword/signed dword) 7
  (byte~) main::$32 ← (byte~) main::$30 | (byte~) main::$31
  *((byte*) VIC_CONTROL#0) ← (byte~) main::$32
  (byte~) main::$33 ← (byte) main::rst#1 << (byte/signed byte/word/signed word/dword/signed dword) 4
  *((byte*) BORDERCOL#0) ← (byte~) main::$33
  asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
  (bool~) main::$34 ← (byte) main::rst#1 != (byte/word/signed word/dword/signed dword) 242
  if((bool~) main::$34) goto main::@8
  to:main::@2
main::@return: scope:[main]  from main::@2
  return 
  to:@return
gfx_init_chunky: scope:[gfx_init_chunky]  from main
  (byte*~) gfx_init_chunky::$0 ← (byte*) CHUNKY#0 / (word/signed word/dword/signed dword) 16384
  (byte~) gfx_init_chunky::$1 ← ((byte)) (byte*~) gfx_init_chunky::$0
  (byte) gfx_init_chunky::gfxbCpuBank#0 ← (byte~) gfx_init_chunky::$1
  (byte) dtvSetCpuBankSegment1::cpuBankIdx#0 ← (byte) gfx_init_chunky::gfxbCpuBank#0
  call dtvSetCpuBankSegment1 
  to:gfx_init_chunky::@7
gfx_init_chunky::@7: scope:[gfx_init_chunky]  from gfx_init_chunky
  (byte) gfx_init_chunky::gfxbCpuBank#3 ← phi( gfx_init_chunky/(byte) gfx_init_chunky::gfxbCpuBank#0 )
  (byte) gfx_init_chunky::gfxbCpuBank#1 ← ++ (byte) gfx_init_chunky::gfxbCpuBank#3
  (byte*) gfx_init_chunky::gfxb#0 ← ((byte*)) (word/signed word/dword/signed dword) 16384
  (byte) gfx_init_chunky::y#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  to:gfx_init_chunky::@1
gfx_init_chunky::@1: scope:[gfx_init_chunky]  from gfx_init_chunky::@5 gfx_init_chunky::@7
  (byte) gfx_init_chunky::gfxbCpuBank#7 ← phi( gfx_init_chunky::@5/(byte) gfx_init_chunky::gfxbCpuBank#9 gfx_init_chunky::@7/(byte) gfx_init_chunky::gfxbCpuBank#1 )
  (byte) gfx_init_chunky::y#6 ← phi( gfx_init_chunky::@5/(byte) gfx_init_chunky::y#1 gfx_init_chunky::@7/(byte) gfx_init_chunky::y#0 )
  (byte*) gfx_init_chunky::gfxb#5 ← phi( gfx_init_chunky::@5/(byte*) gfx_init_chunky::gfxb#6 gfx_init_chunky::@7/(byte*) gfx_init_chunky::gfxb#0 )
  (word) gfx_init_chunky::x#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  to:gfx_init_chunky::@2
gfx_init_chunky::@2: scope:[gfx_init_chunky]  from gfx_init_chunky::@1 gfx_init_chunky::@3
  (byte) gfx_init_chunky::gfxbCpuBank#6 ← phi( gfx_init_chunky::@1/(byte) gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::@3/(byte) gfx_init_chunky::gfxbCpuBank#8 )
  (byte) gfx_init_chunky::y#4 ← phi( gfx_init_chunky::@1/(byte) gfx_init_chunky::y#6 gfx_init_chunky::@3/(byte) gfx_init_chunky::y#2 )
  (word) gfx_init_chunky::x#3 ← phi( gfx_init_chunky::@1/(word) gfx_init_chunky::x#0 gfx_init_chunky::@3/(word) gfx_init_chunky::x#1 )
  (byte*) gfx_init_chunky::gfxb#3 ← phi( gfx_init_chunky::@1/(byte*) gfx_init_chunky::gfxb#5 gfx_init_chunky::@3/(byte*) gfx_init_chunky::gfxb#1 )
  (bool~) gfx_init_chunky::$3 ← (byte*) gfx_init_chunky::gfxb#3 == (word/dword/signed dword) 32768
  (bool~) gfx_init_chunky::$4 ← ! (bool~) gfx_init_chunky::$3
  if((bool~) gfx_init_chunky::$4) goto gfx_init_chunky::@3
  to:gfx_init_chunky::@4
gfx_init_chunky::@3: scope:[gfx_init_chunky]  from gfx_init_chunky::@2 gfx_init_chunky::@8
  (byte) gfx_init_chunky::gfxbCpuBank#8 ← phi( gfx_init_chunky::@2/(byte) gfx_init_chunky::gfxbCpuBank#6 gfx_init_chunky::@8/(byte) gfx_init_chunky::gfxbCpuBank#2 )
  (byte*) gfx_init_chunky::gfxb#4 ← phi( gfx_init_chunky::@2/(byte*) gfx_init_chunky::gfxb#3 gfx_init_chunky::@8/(byte*) gfx_init_chunky::gfxb#2 )
  (byte) gfx_init_chunky::y#2 ← phi( gfx_init_chunky::@2/(byte) gfx_init_chunky::y#4 gfx_init_chunky::@8/(byte) gfx_init_chunky::y#5 )
  (word) gfx_init_chunky::x#2 ← phi( gfx_init_chunky::@2/(word) gfx_init_chunky::x#3 gfx_init_chunky::@8/(word) gfx_init_chunky::x#4 )
  (word~) gfx_init_chunky::$6 ← (word) gfx_init_chunky::x#2 + (byte) gfx_init_chunky::y#2
  (byte~) gfx_init_chunky::$7 ← ((byte)) (word~) gfx_init_chunky::$6
  (byte) gfx_init_chunky::c#0 ← (byte~) gfx_init_chunky::$7
  *((byte*) gfx_init_chunky::gfxb#4) ← (byte) gfx_init_chunky::c#0
  (byte*) gfx_init_chunky::gfxb#1 ← ++ (byte*) gfx_init_chunky::gfxb#4
  (word) gfx_init_chunky::x#1 ← (word) gfx_init_chunky::x#2 + rangenext(0,319)
  (bool~) gfx_init_chunky::$8 ← (word) gfx_init_chunky::x#1 != rangelast(0,319)
  if((bool~) gfx_init_chunky::$8) goto gfx_init_chunky::@2
  to:gfx_init_chunky::@5
gfx_init_chunky::@4: scope:[gfx_init_chunky]  from gfx_init_chunky::@2
  (byte) gfx_init_chunky::y#7 ← phi( gfx_init_chunky::@2/(byte) gfx_init_chunky::y#4 )
  (word) gfx_init_chunky::x#5 ← phi( gfx_init_chunky::@2/(word) gfx_init_chunky::x#3 )
  (byte) gfx_init_chunky::gfxbCpuBank#4 ← phi( gfx_init_chunky::@2/(byte) gfx_init_chunky::gfxbCpuBank#6 )
  (byte) dtvSetCpuBankSegment1::cpuBankIdx#1 ← (byte) gfx_init_chunky::gfxbCpuBank#4
  call dtvSetCpuBankSegment1 
  to:gfx_init_chunky::@8
gfx_init_chunky::@8: scope:[gfx_init_chunky]  from gfx_init_chunky::@4
  (byte) gfx_init_chunky::y#5 ← phi( gfx_init_chunky::@4/(byte) gfx_init_chunky::y#7 )
  (word) gfx_init_chunky::x#4 ← phi( gfx_init_chunky::@4/(word) gfx_init_chunky::x#5 )
  (byte) gfx_init_chunky::gfxbCpuBank#5 ← phi( gfx_init_chunky::@4/(byte) gfx_init_chunky::gfxbCpuBank#4 )
  (byte) gfx_init_chunky::gfxbCpuBank#2 ← ++ (byte) gfx_init_chunky::gfxbCpuBank#5
  (byte*) gfx_init_chunky::gfxb#2 ← ((byte*)) (word/signed word/dword/signed dword) 16384
  to:gfx_init_chunky::@3
gfx_init_chunky::@5: scope:[gfx_init_chunky]  from gfx_init_chunky::@3
  (byte) gfx_init_chunky::gfxbCpuBank#9 ← phi( gfx_init_chunky::@3/(byte) gfx_init_chunky::gfxbCpuBank#8 )
  (byte*) gfx_init_chunky::gfxb#6 ← phi( gfx_init_chunky::@3/(byte*) gfx_init_chunky::gfxb#1 )
  (byte) gfx_init_chunky::y#3 ← phi( gfx_init_chunky::@3/(byte) gfx_init_chunky::y#2 )
  (byte) gfx_init_chunky::y#1 ← (byte) gfx_init_chunky::y#3 + rangenext(0,50)
  (bool~) gfx_init_chunky::$9 ← (byte) gfx_init_chunky::y#1 != rangelast(0,50)
  if((bool~) gfx_init_chunky::$9) goto gfx_init_chunky::@1
  to:gfx_init_chunky::@6
gfx_init_chunky::@6: scope:[gfx_init_chunky]  from gfx_init_chunky::@5
  (byte/signed byte/word/signed word/dword/signed dword~) gfx_init_chunky::$10 ← (word/signed word/dword/signed dword) 16384 / (word/signed word/dword/signed dword) 16384
  (byte~) gfx_init_chunky::$11 ← ((byte)) (byte/signed byte/word/signed word/dword/signed dword~) gfx_init_chunky::$10
  (byte) dtvSetCpuBankSegment1::cpuBankIdx#2 ← (byte~) gfx_init_chunky::$11
  call dtvSetCpuBankSegment1 
  to:gfx_init_chunky::@9
gfx_init_chunky::@9: scope:[gfx_init_chunky]  from gfx_init_chunky::@6
  to:gfx_init_chunky::@return
gfx_init_chunky::@return: scope:[gfx_init_chunky]  from gfx_init_chunky::@9
  return 
  to:@return
@7: scope:[]  from @5
  call main 
  to:@8
@8: scope:[]  from @7
  to:@end
@end: scope:[]  from @8

SYMBOL TABLE SSA
(label) @4
(label) @5
(label) @7
(label) @8
(label) @begin
(label) @end
(byte*) BGCOL
(byte*) BGCOL#0
(byte*) BGCOL1
(byte*) BGCOL1#0
(byte*) BGCOL2
(byte*) BGCOL2#0
(byte*) BGCOL3
(byte*) BGCOL3#0
(byte*) BGCOL4
(byte*) BGCOL4#0
(byte) BLACK
(byte) BLACK#0
(byte) BLUE
(byte) BLUE#0
(byte*) BORDERCOL
(byte*) BORDERCOL#0
(byte) BROWN
(byte) BROWN#0
(byte*) CHARGEN
(byte*) CHARGEN#0
(byte*) CHUNKY
(byte*) CHUNKY#0
(byte*) CIA1_INTERRUPT
(byte*) CIA1_INTERRUPT#0
(byte*) CIA1_PORT_A
(byte*) CIA1_PORT_A#0
(byte*) CIA1_PORT_A_DDR
(byte*) CIA1_PORT_A_DDR#0
(byte*) CIA1_PORT_B
(byte*) CIA1_PORT_B#0
(byte*) CIA1_PORT_B_DDR
(byte*) CIA1_PORT_B_DDR#0
(byte*) CIA2_INTERRUPT
(byte*) CIA2_INTERRUPT#0
(byte*) CIA2_PORT_A
(byte*) CIA2_PORT_A#0
(byte*) CIA2_PORT_A_DDR
(byte*) CIA2_PORT_A_DDR#0
(byte*) CIA2_PORT_B
(byte*) CIA2_PORT_B#0
(byte*) CIA2_PORT_B_DDR
(byte*) CIA2_PORT_B_DDR#0
(byte) CIA_INTERRUPT_CLEAR
(byte) CIA_INTERRUPT_CLEAR#0
(byte*) COLS
(byte*) COLS#0
(byte) CYAN
(byte) CYAN#0
(byte*) D011
(byte*) D011#0
(byte*) D016
(byte*) D016#0
(byte*) D018
(byte*) D018#0
(byte) DARK_GREY
(byte) DARK_GREY#0
(byte) DTV_BADLINE_OFF
(byte) DTV_BADLINE_OFF#0
(byte*) DTV_BLITTER_ALU
(byte*) DTV_BLITTER_ALU#0
(byte*) DTV_BLITTER_CONTROL
(byte*) DTV_BLITTER_CONTROL#0
(byte*) DTV_BLITTER_CONTROL2
(byte*) DTV_BLITTER_CONTROL2#0
(byte*) DTV_BLITTER_DEST_HI
(byte*) DTV_BLITTER_DEST_HI#0
(byte*) DTV_BLITTER_DEST_LIN_HI
(byte*) DTV_BLITTER_DEST_LIN_HI#0
(byte*) DTV_BLITTER_DEST_LIN_LO
(byte*) DTV_BLITTER_DEST_LIN_LO#0
(byte*) DTV_BLITTER_DEST_LO
(byte*) DTV_BLITTER_DEST_LO#0
(byte*) DTV_BLITTER_DEST_MI
(byte*) DTV_BLITTER_DEST_MI#0
(byte*) DTV_BLITTER_DEST_MOD_HI
(byte*) DTV_BLITTER_DEST_MOD_HI#0
(byte*) DTV_BLITTER_DEST_MOD_LO
(byte*) DTV_BLITTER_DEST_MOD_LO#0
(byte*) DTV_BLITTER_DEST_STEP
(byte*) DTV_BLITTER_DEST_STEP#0
(byte*) DTV_BLITTER_LEN_HI
(byte*) DTV_BLITTER_LEN_HI#0
(byte*) DTV_BLITTER_LEN_LO
(byte*) DTV_BLITTER_LEN_LO#0
(byte*) DTV_BLITTER_SRCA_HI
(byte*) DTV_BLITTER_SRCA_HI#0
(byte*) DTV_BLITTER_SRCA_LIN_HI
(byte*) DTV_BLITTER_SRCA_LIN_HI#0
(byte*) DTV_BLITTER_SRCA_LIN_LO
(byte*) DTV_BLITTER_SRCA_LIN_LO#0
(byte*) DTV_BLITTER_SRCA_LO
(byte*) DTV_BLITTER_SRCA_LO#0
(byte*) DTV_BLITTER_SRCA_MI
(byte*) DTV_BLITTER_SRCA_MI#0
(byte*) DTV_BLITTER_SRCA_MOD_HI
(byte*) DTV_BLITTER_SRCA_MOD_HI#0
(byte*) DTV_BLITTER_SRCA_MOD_LO
(byte*) DTV_BLITTER_SRCA_MOD_LO#0
(byte*) DTV_BLITTER_SRCA_STEP
(byte*) DTV_BLITTER_SRCA_STEP#0
(byte*) DTV_BLITTER_SRCB_HI
(byte*) DTV_BLITTER_SRCB_HI#0
(byte*) DTV_BLITTER_SRCB_LIN_HI
(byte*) DTV_BLITTER_SRCB_LIN_HI#0
(byte*) DTV_BLITTER_SRCB_LIN_LO
(byte*) DTV_BLITTER_SRCB_LIN_LO#0
(byte*) DTV_BLITTER_SRCB_LO
(byte*) DTV_BLITTER_SRCB_LO#0
(byte*) DTV_BLITTER_SRCB_MI
(byte*) DTV_BLITTER_SRCB_MI#0
(byte*) DTV_BLITTER_SRCB_MOD_HI
(byte*) DTV_BLITTER_SRCB_MOD_HI#0
(byte*) DTV_BLITTER_SRCB_MOD_LO
(byte*) DTV_BLITTER_SRCB_MOD_LO#0
(byte*) DTV_BLITTER_SRCB_STEP
(byte*) DTV_BLITTER_SRCB_STEP#0
(byte*) DTV_BLITTER_TRANSPARANCY
(byte*) DTV_BLITTER_TRANSPARANCY#0
(byte) DTV_BLIT_ADD
(byte) DTV_BLIT_ADD#0
(byte) DTV_BLIT_AND
(byte) DTV_BLIT_AND#0
(byte) DTV_BLIT_CIA_IRQ
(byte) DTV_BLIT_CIA_IRQ#0
(byte) DTV_BLIT_CLEAR_IRQ
(byte) DTV_BLIT_CLEAR_IRQ#0
(byte) DTV_BLIT_DEST_CONT
(byte) DTV_BLIT_DEST_CONT#0
(byte) DTV_BLIT_DEST_FWD
(byte) DTV_BLIT_DEST_FWD#0
(byte) DTV_BLIT_DISABLE_B
(byte) DTV_BLIT_DISABLE_B#0
(byte) DTV_BLIT_FORCE_START
(byte) DTV_BLIT_FORCE_START#0
(byte) DTV_BLIT_IRQ_EN
(byte) DTV_BLIT_IRQ_EN#0
(byte) DTV_BLIT_NAND
(byte) DTV_BLIT_NAND#0
(byte) DTV_BLIT_NOR
(byte) DTV_BLIT_NOR#0
(byte) DTV_BLIT_OR
(byte) DTV_BLIT_OR#0
(byte) DTV_BLIT_SHIFT0
(byte) DTV_BLIT_SHIFT0#0
(byte) DTV_BLIT_SHIFT1
(byte) DTV_BLIT_SHIFT1#0
(byte) DTV_BLIT_SHIFT2
(byte) DTV_BLIT_SHIFT2#0
(byte) DTV_BLIT_SHIFT3
(byte) DTV_BLIT_SHIFT3#0
(byte) DTV_BLIT_SHIFT4
(byte) DTV_BLIT_SHIFT4#0
(byte) DTV_BLIT_SHIFT5
(byte) DTV_BLIT_SHIFT5#0
(byte) DTV_BLIT_SHIFT6
(byte) DTV_BLIT_SHIFT6#0
(byte) DTV_BLIT_SHIFT7
(byte) DTV_BLIT_SHIFT7#0
(byte) DTV_BLIT_SRCA_CONT
(byte) DTV_BLIT_SRCA_CONT#0
(byte) DTV_BLIT_SRCA_FWD
(byte) DTV_BLIT_SRCA_FWD#0
(byte) DTV_BLIT_SRCB_CONT
(byte) DTV_BLIT_SRCB_CONT#0
(byte) DTV_BLIT_SRCB_FWD
(byte) DTV_BLIT_SRCB_FWD#0
(byte) DTV_BLIT_STATUS_BUSY
(byte) DTV_BLIT_STATUS_BUSY#0
(byte) DTV_BLIT_STATUS_IRQ
(byte) DTV_BLIT_STATUS_IRQ#0
(byte) DTV_BLIT_SUB
(byte) DTV_BLIT_SUB#0
(byte) DTV_BLIT_TRANSPARANCY_NONE
(byte) DTV_BLIT_TRANSPARANCY_NONE#0
(byte) DTV_BLIT_VBLANK
(byte) DTV_BLIT_VBLANK#0
(byte) DTV_BLIT_VIC_IRQ
(byte) DTV_BLIT_VIC_IRQ#0
(byte) DTV_BLIT_WRITE_NONTRANSPARENT
(byte) DTV_BLIT_WRITE_NONTRANSPARENT#0
(byte) DTV_BLIT_WRITE_TRANSPARENT
(byte) DTV_BLIT_WRITE_TRANSPARENT#0
(byte) DTV_BLIT_XNOR
(byte) DTV_BLIT_XNOR#0
(byte) DTV_BLIT_XOR
(byte) DTV_BLIT_XOR#0
(byte) DTV_BORDER_OFF
(byte) DTV_BORDER_OFF#0
(byte) DTV_CHUNKY
(byte) DTV_CHUNKY#0
(byte) DTV_COLORRAM_OFF
(byte) DTV_COLORRAM_OFF#0
(dword) DTV_COLOR_BANK_DEFAULT
(dword) DTV_COLOR_BANK_DEFAULT#0
(byte*) DTV_COLOR_BANK_HI
(byte*) DTV_COLOR_BANK_HI#0
(byte*) DTV_COLOR_BANK_LO
(byte*) DTV_COLOR_BANK_LO#0
(byte*) DTV_CONTROL
(byte*) DTV_CONTROL#0
(byte*) DTV_FEATURE
(byte*) DTV_FEATURE#0
(byte) DTV_FEATURE_DISABLE_TIL_RESET
(byte) DTV_FEATURE_DISABLE_TIL_RESET#0
(byte) DTV_FEATURE_ENABLE
(byte) DTV_FEATURE_ENABLE#0
(byte*) DTV_GRAPHICS_HICOL_BANK
(byte*) DTV_GRAPHICS_HICOL_BANK#0
(byte*) DTV_GRAPHICS_VIC_BANK
(byte*) DTV_GRAPHICS_VIC_BANK#0
(byte) DTV_HIGHCOLOR
(byte) DTV_HIGHCOLOR#0
(byte) DTV_LINEAR
(byte) DTV_LINEAR#0
(byte) DTV_OVERSCAN
(byte) DTV_OVERSCAN#0
(byte*) DTV_PALETTE
(byte*) DTV_PALETTE#0
(byte[16]) DTV_PALETTE_DEFAULT
(byte[16]) DTV_PALETTE_DEFAULT#0
(byte*) DTV_PLANEA_MODULO_HI
(byte*) DTV_PLANEA_MODULO_HI#0
(byte*) DTV_PLANEA_MODULO_LO
(byte*) DTV_PLANEA_MODULO_LO#0
(byte*) DTV_PLANEA_START_HI
(byte*) DTV_PLANEA_START_HI#0
(byte*) DTV_PLANEA_START_LO
(byte*) DTV_PLANEA_START_LO#0
(byte*) DTV_PLANEA_START_MI
(byte*) DTV_PLANEA_START_MI#0
(byte*) DTV_PLANEA_STEP
(byte*) DTV_PLANEA_STEP#0
(byte*) DTV_PLANEB_MODULO_HI
(byte*) DTV_PLANEB_MODULO_HI#0
(byte*) DTV_PLANEB_MODULO_LO
(byte*) DTV_PLANEB_MODULO_LO#0
(byte*) DTV_PLANEB_START_HI
(byte*) DTV_PLANEB_START_HI#0
(byte*) DTV_PLANEB_START_LO
(byte*) DTV_PLANEB_START_LO#0
(byte*) DTV_PLANEB_START_MI
(byte*) DTV_PLANEB_START_MI#0
(byte*) DTV_PLANEB_STEP
(byte*) DTV_PLANEB_STEP#0
(byte*) DTV_SPRITE_BANK
(byte*) DTV_SPRITE_BANK#0
(byte) GREEN
(byte) GREEN#0
(byte) GREY
(byte) GREY#0
(void()**) HARDWARE_IRQ
(void()**) HARDWARE_IRQ#0
(byte) IRQ_COLLISION_BG
(byte) IRQ_COLLISION_BG#0
(byte) IRQ_COLLISION_SPRITE
(byte) IRQ_COLLISION_SPRITE#0
(byte*) IRQ_ENABLE
(byte*) IRQ_ENABLE#0
(byte) IRQ_LIGHTPEN
(byte) IRQ_LIGHTPEN#0
(byte) IRQ_RASTER
(byte) IRQ_RASTER#0
(byte*) IRQ_STATUS
(byte*) IRQ_STATUS#0
(void()**) KERNEL_IRQ
(void()**) KERNEL_IRQ#0
(byte*) LIGHTPEN_X
(byte*) LIGHTPEN_X#0
(byte*) LIGHTPEN_Y
(byte*) LIGHTPEN_Y#0
(byte) LIGHT_BLUE
(byte) LIGHT_BLUE#0
(byte) LIGHT_GREEN
(byte) LIGHT_GREEN#0
(byte) LIGHT_GREY
(byte) LIGHT_GREY#0
(byte) ORANGE
(byte) ORANGE#0
(byte) PINK
(byte) PINK#0
(byte*) PROCPORT
(byte*) PROCPORT#0
(byte) PROCPORT_BASIC_KERNEL_IO
(byte) PROCPORT_BASIC_KERNEL_IO#0
(byte*) PROCPORT_DDR
(byte*) PROCPORT_DDR#0
(byte) PROCPORT_DDR_MEMORY_MASK
(byte) PROCPORT_DDR_MEMORY_MASK#0
(byte) PROCPORT_KERNEL_IO
(byte) PROCPORT_KERNEL_IO#0
(byte) PROCPORT_RAM_ALL
(byte) PROCPORT_RAM_ALL#0
(byte) PROCPORT_RAM_CHARROM
(byte) PROCPORT_RAM_CHARROM#0
(byte) PROCPORT_RAM_IO
(byte) PROCPORT_RAM_IO#0
(byte) PURPLE
(byte) PURPLE#0
(byte*) RASTER
(byte*) RASTER#0
(byte) RED
(byte) RED#0
(byte*) SPRITES_COLS
(byte*) SPRITES_COLS#0
(byte*) SPRITES_ENABLE
(byte*) SPRITES_ENABLE#0
(byte*) SPRITES_EXPAND_X
(byte*) SPRITES_EXPAND_X#0
(byte*) SPRITES_EXPAND_Y
(byte*) SPRITES_EXPAND_Y#0
(byte*) SPRITES_MC
(byte*) SPRITES_MC#0
(byte*) SPRITES_MC1
(byte*) SPRITES_MC1#0
(byte*) SPRITES_MC2
(byte*) SPRITES_MC2#0
(byte*) SPRITES_PRIORITY
(byte*) SPRITES_PRIORITY#0
(byte*) SPRITES_XMSB
(byte*) SPRITES_XMSB#0
(byte*) SPRITES_XPOS
(byte*) SPRITES_XPOS#0
(byte*) SPRITES_YPOS
(byte*) SPRITES_YPOS#0
(word) SPRITE_PTRS
(word) SPRITE_PTRS#0
(byte) VIC_BMM
(byte) VIC_BMM#0
(byte*) VIC_CONTROL
(byte*) VIC_CONTROL#0
(byte*) VIC_CONTROL2
(byte*) VIC_CONTROL2#0
(byte) VIC_CSEL
(byte) VIC_CSEL#0
(byte) VIC_DEN
(byte) VIC_DEN#0
(byte) VIC_ECM
(byte) VIC_ECM#0
(byte) VIC_MCM
(byte) VIC_MCM#0
(byte*) VIC_MEMORY
(byte*) VIC_MEMORY#0
(byte) VIC_RSEL
(byte) VIC_RSEL#0
(byte) VIC_RST8
(byte) VIC_RST8#0
(byte) WHITE
(byte) WHITE#0
(byte) YELLOW
(byte) YELLOW#0
(void()) dtvSetCpuBankSegment1((byte) dtvSetCpuBankSegment1::cpuBankIdx)
(label) dtvSetCpuBankSegment1::@return
(byte*) dtvSetCpuBankSegment1::cpuBank
(byte*) dtvSetCpuBankSegment1::cpuBank#0
(byte) dtvSetCpuBankSegment1::cpuBankIdx
(byte) dtvSetCpuBankSegment1::cpuBankIdx#0
(byte) dtvSetCpuBankSegment1::cpuBankIdx#1
(byte) dtvSetCpuBankSegment1::cpuBankIdx#2
(byte) dtvSetCpuBankSegment1::cpuBankIdx#3
(void()) gfx_init_chunky()
(byte*~) gfx_init_chunky::$0
(byte~) gfx_init_chunky::$1
(byte/signed byte/word/signed word/dword/signed dword~) gfx_init_chunky::$10
(byte~) gfx_init_chunky::$11
(bool~) gfx_init_chunky::$3
(bool~) gfx_init_chunky::$4
(word~) gfx_init_chunky::$6
(byte~) gfx_init_chunky::$7
(bool~) gfx_init_chunky::$8
(bool~) gfx_init_chunky::$9
(label) gfx_init_chunky::@1
(label) gfx_init_chunky::@2
(label) gfx_init_chunky::@3
(label) gfx_init_chunky::@4
(label) gfx_init_chunky::@5
(label) gfx_init_chunky::@6
(label) gfx_init_chunky::@7
(label) gfx_init_chunky::@8
(label) gfx_init_chunky::@9
(label) gfx_init_chunky::@return
(byte) gfx_init_chunky::c
(byte) gfx_init_chunky::c#0
(byte*) gfx_init_chunky::gfxb
(byte*) gfx_init_chunky::gfxb#0
(byte*) gfx_init_chunky::gfxb#1
(byte*) gfx_init_chunky::gfxb#2
(byte*) gfx_init_chunky::gfxb#3
(byte*) gfx_init_chunky::gfxb#4
(byte*) gfx_init_chunky::gfxb#5
(byte*) gfx_init_chunky::gfxb#6
(byte) gfx_init_chunky::gfxbCpuBank
(byte) gfx_init_chunky::gfxbCpuBank#0
(byte) gfx_init_chunky::gfxbCpuBank#1
(byte) gfx_init_chunky::gfxbCpuBank#2
(byte) gfx_init_chunky::gfxbCpuBank#3
(byte) gfx_init_chunky::gfxbCpuBank#4
(byte) gfx_init_chunky::gfxbCpuBank#5
(byte) gfx_init_chunky::gfxbCpuBank#6
(byte) gfx_init_chunky::gfxbCpuBank#7
(byte) gfx_init_chunky::gfxbCpuBank#8
(byte) gfx_init_chunky::gfxbCpuBank#9
(word) gfx_init_chunky::x
(word) gfx_init_chunky::x#0
(word) gfx_init_chunky::x#1
(word) gfx_init_chunky::x#2
(word) gfx_init_chunky::x#3
(word) gfx_init_chunky::x#4
(word) gfx_init_chunky::x#5
(byte) gfx_init_chunky::y
(byte) gfx_init_chunky::y#0
(byte) gfx_init_chunky::y#1
(byte) gfx_init_chunky::y#2
(byte) gfx_init_chunky::y#3
(byte) gfx_init_chunky::y#4
(byte) gfx_init_chunky::y#5
(byte) gfx_init_chunky::y#6
(byte) gfx_init_chunky::y#7
(void()) main()
(byte~) main::$1
(byte~) main::$10
(word~) main::$11
(word/signed dword/dword~) main::$12
(byte~) main::$13
(byte/word/dword~) main::$14
(word~) main::$15
(word~) main::$16
(word~) main::$17
(byte~) main::$18
(word~) main::$19
(byte~) main::$2
(word~) main::$20
(byte~) main::$21
(byte~) main::$22
(byte~) main::$23
(bool~) main::$24
(byte~) main::$25
(byte~) main::$26
(byte/word/dword~) main::$27
(bool~) main::$28
(byte~) main::$29
(byte~) main::$3
(byte~) main::$30
(byte~) main::$31
(byte~) main::$32
(byte~) main::$33
(bool~) main::$34
(byte~) main::$4
(byte~) main::$5
(byte~) main::$6
(byte/word/dword~) main::$7
(byte~) main::$8
(byte~) main::$9
(label) main::@1
(label) main::@17
(label) main::@2
(label) main::@3
(label) main::@5
(label) main::@6
(label) main::@7
(label) main::@8
(label) main::@return
(byte) main::j
(byte) main::j#0
(byte) main::j#1
(byte) main::j#2
(byte) main::rst
(byte) main::rst#0
(byte) main::rst#1
(byte) main::rst#2
(byte) main::rst#3

Culled Empty Block (label) gfx_init_chunky::@9
Culled Empty Block (label) @8
Successful SSA optimization Pass2CullEmptyBlocks
Inversing boolean not [264] (bool~) gfx_init_chunky::$4 ← (byte*) gfx_init_chunky::gfxb#3 != (word/dword/signed dword) 32768 from [263] (bool~) gfx_init_chunky::$3 ← (byte*) gfx_init_chunky::gfxb#3 == (word/dword/signed dword) 32768
Successful SSA optimization Pass2UnaryNotSimplification
Alias (byte) main::rst#2 = (byte) main::rst#3 
Alias (byte) gfx_init_chunky::gfxbCpuBank#0 = (byte~) gfx_init_chunky::$1 (byte) gfx_init_chunky::gfxbCpuBank#3 
Alias (byte) gfx_init_chunky::c#0 = (byte~) gfx_init_chunky::$7 
Alias (byte) gfx_init_chunky::gfxbCpuBank#4 = (byte) gfx_init_chunky::gfxbCpuBank#6 (byte) gfx_init_chunky::gfxbCpuBank#5 
Alias (word) gfx_init_chunky::x#3 = (word) gfx_init_chunky::x#5 (word) gfx_init_chunky::x#4 
Alias (byte) gfx_init_chunky::y#4 = (byte) gfx_init_chunky::y#7 (byte) gfx_init_chunky::y#5 
Alias (byte) gfx_init_chunky::y#2 = (byte) gfx_init_chunky::y#3 
Alias (byte*) gfx_init_chunky::gfxb#1 = (byte*) gfx_init_chunky::gfxb#6 
Alias (byte) gfx_init_chunky::gfxbCpuBank#8 = (byte) gfx_init_chunky::gfxbCpuBank#9 
Alias (byte) dtvSetCpuBankSegment1::cpuBankIdx#2 = (byte~) gfx_init_chunky::$11 
Successful SSA optimization Pass2AliasElimination
Alias (word) gfx_init_chunky::x#2 = (word) gfx_init_chunky::x#3 
Alias (byte) gfx_init_chunky::y#2 = (byte) gfx_init_chunky::y#4 
Successful SSA optimization Pass2AliasElimination
Self Phi Eliminated (byte) main::rst#2
Self Phi Eliminated (byte) gfx_init_chunky::y#2
Successful SSA optimization Pass2SelfPhiElimination
Redundant Phi (byte) main::rst#2 (byte) main::rst#0
Redundant Phi (byte) gfx_init_chunky::y#2 (byte) gfx_init_chunky::y#6
Successful SSA optimization Pass2RedundantPhiElimination
Simple Condition (bool~) main::$24 [225] if((byte) main::j#1!=rangelast(0,15)) goto main::@1
Simple Condition (bool~) main::$28 [236] if(*((byte*) RASTER#0)!=(byte) main::rst#0) goto main::@6
Simple Condition (bool~) main::$34 [249] if((byte) main::rst#1!=(byte/word/signed word/dword/signed dword) 242) goto main::@8
Simple Condition (bool~) gfx_init_chunky::$4 [265] if((byte*) gfx_init_chunky::gfxb#3!=(word/dword/signed dword) 32768) goto gfx_init_chunky::@3
Simple Condition (bool~) gfx_init_chunky::$8 [274] if((word) gfx_init_chunky::x#1!=rangelast(0,319)) goto gfx_init_chunky::@2
Simple Condition (bool~) gfx_init_chunky::$9 [284] if((byte) gfx_init_chunky::y#1!=rangelast(0,50)) goto gfx_init_chunky::@1
Successful SSA optimization Pass2ConditionalJumpSimplification
Constant (const byte*) PROCPORT_DDR#0 = ((byte*))0
Constant (const byte) PROCPORT_DDR_MEMORY_MASK#0 = 7
Constant (const byte*) PROCPORT#0 = ((byte*))1
Constant (const byte) PROCPORT_RAM_ALL#0 = 48
Constant (const byte) PROCPORT_RAM_IO#0 = 53
Constant (const byte) PROCPORT_RAM_CHARROM#0 = 49
Constant (const byte) PROCPORT_KERNEL_IO#0 = 54
Constant (const byte) PROCPORT_BASIC_KERNEL_IO#0 = 55
Constant (const byte*) CHARGEN#0 = ((byte*))53248
Constant (const word) SPRITE_PTRS#0 = 1016
Constant (const byte*) SPRITES_XPOS#0 = ((byte*))53248
Constant (const byte*) SPRITES_YPOS#0 = ((byte*))53249
Constant (const byte*) SPRITES_XMSB#0 = ((byte*))53264
Constant (const byte*) RASTER#0 = ((byte*))53266
Constant (const byte*) SPRITES_ENABLE#0 = ((byte*))53269
Constant (const byte*) SPRITES_EXPAND_Y#0 = ((byte*))53271
Constant (const byte*) SPRITES_PRIORITY#0 = ((byte*))53275
Constant (const byte*) SPRITES_MC#0 = ((byte*))53276
Constant (const byte*) SPRITES_EXPAND_X#0 = ((byte*))53277
Constant (const byte*) BORDERCOL#0 = ((byte*))53280
Constant (const byte*) BGCOL#0 = ((byte*))53281
Constant (const byte*) BGCOL1#0 = ((byte*))53281
Constant (const byte*) BGCOL2#0 = ((byte*))53282
Constant (const byte*) BGCOL3#0 = ((byte*))53283
Constant (const byte*) BGCOL4#0 = ((byte*))53284
Constant (const byte*) SPRITES_MC1#0 = ((byte*))53285
Constant (const byte*) SPRITES_MC2#0 = ((byte*))53286
Constant (const byte*) SPRITES_COLS#0 = ((byte*))53287
Constant (const byte*) VIC_CONTROL#0 = ((byte*))53265
Constant (const byte*) D011#0 = ((byte*))53265
Constant (const byte) VIC_RST8#0 = 128
Constant (const byte) VIC_ECM#0 = 64
Constant (const byte) VIC_BMM#0 = 32
Constant (const byte) VIC_DEN#0 = 16
Constant (const byte) VIC_RSEL#0 = 8
Constant (const byte*) VIC_CONTROL2#0 = ((byte*))53270
Constant (const byte*) D016#0 = ((byte*))53270
Constant (const byte) VIC_MCM#0 = 16
Constant (const byte) VIC_CSEL#0 = 8
Constant (const byte*) D018#0 = ((byte*))53272
Constant (const byte*) VIC_MEMORY#0 = ((byte*))53272
Constant (const byte*) LIGHTPEN_X#0 = ((byte*))53267
Constant (const byte*) LIGHTPEN_Y#0 = ((byte*))53268
Constant (const byte*) IRQ_STATUS#0 = ((byte*))53273
Constant (const byte*) IRQ_ENABLE#0 = ((byte*))53274
Constant (const byte) IRQ_RASTER#0 = 1
Constant (const byte) IRQ_COLLISION_BG#0 = 2
Constant (const byte) IRQ_COLLISION_SPRITE#0 = 4
Constant (const byte) IRQ_LIGHTPEN#0 = 8
Constant (const byte*) COLS#0 = ((byte*))55296
Constant (const byte*) CIA1_PORT_A#0 = ((byte*))56320
Constant (const byte*) CIA1_PORT_B#0 = ((byte*))56321
Constant (const byte*) CIA1_PORT_A_DDR#0 = ((byte*))56322
Constant (const byte*) CIA1_PORT_B_DDR#0 = ((byte*))56323
Constant (const byte*) CIA1_INTERRUPT#0 = ((byte*))56333
Constant (const byte) CIA_INTERRUPT_CLEAR#0 = 127
Constant (const byte*) CIA2_PORT_A#0 = ((byte*))56576
Constant (const byte*) CIA2_PORT_B#0 = ((byte*))56577
Constant (const byte*) CIA2_PORT_A_DDR#0 = ((byte*))56578
Constant (const byte*) CIA2_PORT_B_DDR#0 = ((byte*))56579
Constant (const byte*) CIA2_INTERRUPT#0 = ((byte*))56589
Constant (const void()**) KERNEL_IRQ#0 = ((void()**))788
Constant (const void()**) HARDWARE_IRQ#0 = ((void()**))65534
Constant (const byte) BLACK#0 = 0
Constant (const byte) WHITE#0 = 1
Constant (const byte) RED#0 = 2
Constant (const byte) CYAN#0 = 3
Constant (const byte) PURPLE#0 = 4
Constant (const byte) GREEN#0 = 5
Constant (const byte) BLUE#0 = 6
Constant (const byte) YELLOW#0 = 7
Constant (const byte) ORANGE#0 = 8
Constant (const byte) BROWN#0 = 9
Constant (const byte) PINK#0 = 10
Constant (const byte) DARK_GREY#0 = 11
Constant (const byte) GREY#0 = 12
Constant (const byte) LIGHT_GREEN#0 = 13
Constant (const byte) LIGHT_BLUE#0 = 14
Constant (const byte) LIGHT_GREY#0 = 15
Constant (const byte*) DTV_FEATURE#0 = ((byte*))53311
Constant (const byte) DTV_FEATURE_ENABLE#0 = 1
Constant (const byte) DTV_FEATURE_DISABLE_TIL_RESET#0 = 2
Constant (const byte*) DTV_CONTROL#0 = ((byte*))53308
Constant (const byte) DTV_LINEAR#0 = 1
Constant (const byte) DTV_BORDER_OFF#0 = 2
Constant (const byte) DTV_HIGHCOLOR#0 = 4
Constant (const byte) DTV_OVERSCAN#0 = 8
Constant (const byte) DTV_COLORRAM_OFF#0 = 16
Constant (const byte) DTV_BADLINE_OFF#0 = 32
Constant (const byte) DTV_CHUNKY#0 = 64
Constant (const byte*) DTV_PALETTE#0 = ((byte*))53760
Constant (const byte[16]) DTV_PALETTE_DEFAULT#0 = { 0, 15, 54, 190, 88, 219, 134, 255, 41, 38, 59, 5, 7, 223, 154, 10 }
Constant (const byte*) DTV_PLANEA_START_LO#0 = ((byte*))53306
Constant (const byte*) DTV_PLANEA_START_MI#0 = ((byte*))53307
Constant (const byte*) DTV_PLANEA_START_HI#0 = ((byte*))53317
Constant (const byte*) DTV_PLANEA_STEP#0 = ((byte*))53318
Constant (const byte*) DTV_PLANEA_MODULO_LO#0 = ((byte*))53304
Constant (const byte*) DTV_PLANEA_MODULO_HI#0 = ((byte*))53305
Constant (const byte*) DTV_PLANEB_START_LO#0 = ((byte*))53321
Constant (const byte*) DTV_PLANEB_START_MI#0 = ((byte*))53322
Constant (const byte*) DTV_PLANEB_START_HI#0 = ((byte*))53323
Constant (const byte*) DTV_PLANEB_STEP#0 = ((byte*))53324
Constant (const byte*) DTV_PLANEB_MODULO_LO#0 = ((byte*))53319
Constant (const byte*) DTV_PLANEB_MODULO_HI#0 = ((byte*))53320
Constant (const byte*) DTV_SPRITE_BANK#0 = ((byte*))53325
Constant (const byte*) DTV_COLOR_BANK_LO#0 = ((byte*))53302
Constant (const byte*) DTV_COLOR_BANK_HI#0 = ((byte*))53303
Constant (const dword) DTV_COLOR_BANK_DEFAULT#0 = 120832
Constant (const byte*) DTV_GRAPHICS_VIC_BANK#0 = ((byte*))53309
Constant (const byte*) DTV_GRAPHICS_HICOL_BANK#0 = ((byte*))53310
Constant (const byte*) dtvSetCpuBankSegment1::cpuBank#0 = ((byte*))255
Constant (const byte*) DTV_BLITTER_SRCA_LO#0 = ((byte*))54048
Constant (const byte*) DTV_BLITTER_SRCA_MI#0 = ((byte*))54049
Constant (const byte*) DTV_BLITTER_SRCA_HI#0 = ((byte*))54050
Constant (const byte*) DTV_BLITTER_SRCA_MOD_LO#0 = ((byte*))54051
Constant (const byte*) DTV_BLITTER_SRCA_MOD_HI#0 = ((byte*))54052
Constant (const byte*) DTV_BLITTER_SRCA_LIN_LO#0 = ((byte*))54053
Constant (const byte*) DTV_BLITTER_SRCA_LIN_HI#0 = ((byte*))54054
Constant (const byte*) DTV_BLITTER_SRCA_STEP#0 = ((byte*))54055
Constant (const byte*) DTV_BLITTER_SRCB_LO#0 = ((byte*))54056
Constant (const byte*) DTV_BLITTER_SRCB_MI#0 = ((byte*))54057
Constant (const byte*) DTV_BLITTER_SRCB_HI#0 = ((byte*))54058
Constant (const byte*) DTV_BLITTER_SRCB_MOD_LO#0 = ((byte*))54059
Constant (const byte*) DTV_BLITTER_SRCB_MOD_HI#0 = ((byte*))54060
Constant (const byte*) DTV_BLITTER_SRCB_LIN_LO#0 = ((byte*))54061
Constant (const byte*) DTV_BLITTER_SRCB_LIN_HI#0 = ((byte*))54062
Constant (const byte*) DTV_BLITTER_SRCB_STEP#0 = ((byte*))54063
Constant (const byte*) DTV_BLITTER_DEST_LO#0 = ((byte*))54064
Constant (const byte*) DTV_BLITTER_DEST_MI#0 = ((byte*))54065
Constant (const byte*) DTV_BLITTER_DEST_HI#0 = ((byte*))54066
Constant (const byte*) DTV_BLITTER_DEST_MOD_LO#0 = ((byte*))54067
Constant (const byte*) DTV_BLITTER_DEST_MOD_HI#0 = ((byte*))54068
Constant (const byte*) DTV_BLITTER_DEST_LIN_LO#0 = ((byte*))54069
Constant (const byte*) DTV_BLITTER_DEST_LIN_HI#0 = ((byte*))54070
Constant (const byte*) DTV_BLITTER_DEST_STEP#0 = ((byte*))54071
Constant (const byte*) DTV_BLITTER_LEN_LO#0 = ((byte*))54072
Constant (const byte*) DTV_BLITTER_LEN_HI#0 = ((byte*))54073
Constant (const byte*) DTV_BLITTER_CONTROL#0 = ((byte*))54074
Constant (const byte) DTV_BLIT_FORCE_START#0 = 1
Constant (const byte) DTV_BLIT_SRCA_FWD#0 = 2
Constant (const byte) DTV_BLIT_SRCB_FWD#0 = 4
Constant (const byte) DTV_BLIT_DEST_FWD#0 = 8
Constant (const byte) DTV_BLIT_VIC_IRQ#0 = 16
Constant (const byte) DTV_BLIT_CIA_IRQ#0 = 32
Constant (const byte) DTV_BLIT_VBLANK#0 = 64
Constant (const byte) DTV_BLIT_IRQ_EN#0 = 128
Constant (const byte*) DTV_BLITTER_TRANSPARANCY#0 = ((byte*))54075
Constant (const byte) DTV_BLIT_DISABLE_B#0 = 1
Constant (const byte) DTV_BLIT_WRITE_TRANSPARENT#0 = 2
Constant (const byte) DTV_BLIT_WRITE_NONTRANSPARENT#0 = 4
Constant (const byte) DTV_BLIT_TRANSPARANCY_NONE#0 = 0
Constant (const byte*) DTV_BLITTER_ALU#0 = ((byte*))54078
Constant (const byte) DTV_BLIT_SHIFT0#0 = 0
Constant (const byte) DTV_BLIT_SHIFT1#0 = 1
Constant (const byte) DTV_BLIT_SHIFT2#0 = 2
Constant (const byte) DTV_BLIT_SHIFT3#0 = 3
Constant (const byte) DTV_BLIT_SHIFT4#0 = 4
Constant (const byte) DTV_BLIT_SHIFT5#0 = 5
Constant (const byte) DTV_BLIT_SHIFT6#0 = 6
Constant (const byte) DTV_BLIT_SHIFT7#0 = 7
Constant (const byte) DTV_BLIT_AND#0 = 0
Constant (const byte) DTV_BLIT_NAND#0 = 8
Constant (const byte) DTV_BLIT_NOR#0 = 16
Constant (const byte) DTV_BLIT_OR#0 = 24
Constant (const byte) DTV_BLIT_XOR#0 = 32
Constant (const byte) DTV_BLIT_XNOR#0 = 40
Constant (const byte) DTV_BLIT_ADD#0 = 48
Constant (const byte) DTV_BLIT_SUB#0 = 56
Constant (const byte*) DTV_BLITTER_CONTROL2#0 = ((byte*))54079
Constant (const byte) DTV_BLIT_CLEAR_IRQ#0 = 1
Constant (const byte) DTV_BLIT_SRCA_CONT#0 = 2
Constant (const byte) DTV_BLIT_SRCB_CONT#0 = 4
Constant (const byte) DTV_BLIT_DEST_CONT#0 = 8
Constant (const byte) DTV_BLIT_STATUS_BUSY#0 = 1
Constant (const byte) DTV_BLIT_STATUS_IRQ#0 = 2
Constant (const byte*) CHUNKY#0 = ((byte*))32768
Constant (const byte) main::j#0 = 0
Constant (const byte) main::rst#0 = 66
Constant (const byte*) gfx_init_chunky::gfxb#0 = ((byte*))16384
Constant (const byte) gfx_init_chunky::y#0 = 0
Constant (const word) gfx_init_chunky::x#0 = 0
Constant (const byte*) gfx_init_chunky::gfxb#2 = ((byte*))16384
Constant (const byte/signed byte/word/signed word/dword/signed dword) gfx_init_chunky::$10 = 16384/16384
Successful SSA optimization Pass2ConstantIdentification
Constant (const byte) main::$1 = DTV_HIGHCOLOR#0|DTV_LINEAR#0
Constant (const byte) main::$5 = VIC_DEN#0|VIC_ECM#0
Constant (const byte) main::$8 = VIC_MCM#0|VIC_CSEL#0
Constant (const byte) main::$9 = <CHUNKY#0
Constant (const byte) main::$10 = >CHUNKY#0
Constant (const word) main::$11 = ((word))CHUNKY#0
Constant (const word) main::$15 = ((word))CHUNKY#0
Constant (const word) main::$19 = ((word))CHUNKY#0
Constant (const byte) main::$25 = VIC_DEN#0|VIC_ECM#0
Constant (const byte) main::$29 = VIC_DEN#0|VIC_ECM#0
Constant (const byte*) gfx_init_chunky::$0 = CHUNKY#0/16384
Constant (const byte) dtvSetCpuBankSegment1::cpuBankIdx#2 = ((byte))gfx_init_chunky::$10
Successful SSA optimization Pass2ConstantIdentification
Constant (const byte) main::$2 = main::$1|DTV_COLORRAM_OFF#0
Constant (const byte) main::$6 = main::$5|VIC_RSEL#0
Constant (const word/signed dword/dword) main::$12 = main::$11/16384
Constant (const word) main::$16 = main::$15&16383
Constant (const word) main::$20 = main::$19&16383
Constant (const byte) main::$26 = main::$25|VIC_RSEL#0
Constant (const byte) main::$30 = main::$29|VIC_RSEL#0
Constant (const byte) gfx_init_chunky::gfxbCpuBank#0 = ((byte))gfx_init_chunky::$0
Successful SSA optimization Pass2ConstantIdentification
Constant (const byte) main::$3 = main::$2|DTV_CHUNKY#0
Constant (const byte/word/dword) main::$7 = main::$6|3
Constant (const byte) main::$13 = ((byte))main::$12
Constant (const word) main::$17 = main::$16>>6
Constant (const byte) main::$21 = >main::$20
Constant (const byte/word/dword) main::$27 = main::$26|3
Constant (const byte) dtvSetCpuBankSegment1::cpuBankIdx#0 = gfx_init_chunky::gfxbCpuBank#0
Constant (const byte) gfx_init_chunky::gfxbCpuBank#1 = ++gfx_init_chunky::gfxbCpuBank#0
Successful SSA optimization Pass2ConstantIdentification
Constant (const byte) main::$4 = main::$3|DTV_BADLINE_OFF#0
Constant (const byte/word/dword) main::$14 = 3^main::$13
Constant (const byte) main::$18 = ((byte))main::$17
Constant (const byte) main::$22 = main::$21>>2
Successful SSA optimization Pass2ConstantIdentification
Constant (const byte) main::$23 = main::$18|main::$22
Successful SSA optimization Pass2ConstantIdentification
if() condition always true - replacing block destination [25] if(true) goto main::@3
Successful SSA optimization Pass2ConstantIfs
Successful SSA optimization PassNEliminateUnusedVars
Removing unused block main::@return
Successful SSA optimization Pass2EliminateUnusedBlocks
Resolved ranged next value main::j#1 ← ++ main::j#2 to ++
Resolved ranged comparison value if(main::j#1!=rangelast(0,15)) goto main::@1 to (byte/signed byte/word/signed word/dword/signed dword) 16
Resolved ranged next value gfx_init_chunky::x#1 ← ++ gfx_init_chunky::x#2 to ++
Resolved ranged comparison value if(gfx_init_chunky::x#1!=rangelast(0,319)) goto gfx_init_chunky::@2 to (word/signed word/dword/signed dword) 320
Resolved ranged next value gfx_init_chunky::y#1 ← ++ gfx_init_chunky::y#6 to ++
Resolved ranged comparison value if(gfx_init_chunky::y#1!=rangelast(0,50)) goto gfx_init_chunky::@1 to (byte/signed byte/word/signed word/dword/signed dword) 51
Culled Empty Block (label) @4
Culled Empty Block (label) @5
Culled Empty Block (label) main::@2
Culled Empty Block (label) main::@6
Culled Empty Block (label) gfx_init_chunky::@7
Successful SSA optimization Pass2CullEmptyBlocks
Inlining constant with var siblings (const byte) dtvSetCpuBankSegment1::cpuBankIdx#2
Inlining constant with var siblings (const byte) dtvSetCpuBankSegment1::cpuBankIdx#0
Inlining constant with var siblings (const byte) main::j#0
Inlining constant with var siblings (const byte) main::rst#0
Inlining constant with var siblings (const byte*) gfx_init_chunky::gfxb#0
Inlining constant with var siblings (const byte) gfx_init_chunky::y#0
Inlining constant with var siblings (const word) gfx_init_chunky::x#0
Inlining constant with var siblings (const byte*) gfx_init_chunky::gfxb#2
Inlining constant with var siblings (const byte) gfx_init_chunky::gfxbCpuBank#0
Inlining constant with var siblings (const byte) gfx_init_chunky::gfxbCpuBank#1
Constant inlined dtvSetCpuBankSegment1::cpuBankIdx#0 = ((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384
Constant inlined main::rst#0 = (byte/signed byte/word/signed word/dword/signed dword) 66
Constant inlined dtvSetCpuBankSegment1::cpuBankIdx#2 = ((byte))(word/signed word/dword/signed dword) 16384/(word/signed word/dword/signed dword) 16384
Constant inlined main::$12 = ((word))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384
Constant inlined main::$13 = ((byte))((word))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384
Constant inlined main::$14 = (byte/signed byte/word/signed word/dword/signed dword) 3^((byte))((word))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384
Constant inlined gfx_init_chunky::y#0 = (byte/signed byte/word/signed word/dword/signed dword) 0
Constant inlined main::$15 = ((word))(const byte*) CHUNKY#0
Constant inlined gfx_init_chunky::x#0 = (byte/signed byte/word/signed word/dword/signed dword) 0
Constant inlined main::$30 = (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0
Constant inlined main::$10 = >(const byte*) CHUNKY#0
Constant inlined main::$11 = ((word))(const byte*) CHUNKY#0
Constant inlined main::$16 = ((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383
Constant inlined main::$17 = ((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 6
Constant inlined main::$18 = ((byte))((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 6
Constant inlined main::$19 = ((word))(const byte*) CHUNKY#0
Constant inlined main::j#0 = (byte/signed byte/word/signed word/dword/signed dword) 0
Constant inlined main::$23 = ((byte))((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 6|>((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 2
Constant inlined gfx_init_chunky::gfxbCpuBank#1 = ++((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384
Constant inlined main::$25 = (const byte) VIC_DEN#0|(const byte) VIC_ECM#0
Constant inlined main::$26 = (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0
Constant inlined gfx_init_chunky::gfxb#2 = ((byte*))(word/signed word/dword/signed dword) 16384
Constant inlined main::$20 = ((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383
Constant inlined gfx_init_chunky::gfxb#0 = ((byte*))(word/signed word/dword/signed dword) 16384
Constant inlined main::$21 = >((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383
Constant inlined main::$22 = >((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 2
Constant inlined gfx_init_chunky::gfxbCpuBank#0 = ((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384
Constant inlined main::$1 = (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0
Constant inlined main::$27 = (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3
Constant inlined gfx_init_chunky::$10 = (word/signed word/dword/signed dword) 16384/(word/signed word/dword/signed dword) 16384
Constant inlined main::$2 = (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0|(const byte) DTV_COLORRAM_OFF#0
Constant inlined main::$29 = (const byte) VIC_DEN#0|(const byte) VIC_ECM#0
Constant inlined main::$5 = (const byte) VIC_DEN#0|(const byte) VIC_ECM#0
Constant inlined main::$6 = (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0
Constant inlined main::$3 = (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0|(const byte) DTV_COLORRAM_OFF#0|(const byte) DTV_CHUNKY#0
Constant inlined main::$4 = (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0|(const byte) DTV_COLORRAM_OFF#0|(const byte) DTV_CHUNKY#0|(const byte) DTV_BADLINE_OFF#0
Constant inlined gfx_init_chunky::$0 = (const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384
Constant inlined main::$9 = <(const byte*) CHUNKY#0
Constant inlined main::$7 = (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3
Constant inlined main::$8 = (const byte) VIC_MCM#0|(const byte) VIC_CSEL#0
Successful SSA optimization Pass2ConstantInlining
Added new block during phi lifting main::@18(between main::@1 and main::@1)
Added new block during phi lifting gfx_init_chunky::@10(between gfx_init_chunky::@5 and gfx_init_chunky::@1)
Added new block during phi lifting gfx_init_chunky::@11(between gfx_init_chunky::@3 and gfx_init_chunky::@2)
Added new block during phi lifting gfx_init_chunky::@12(between gfx_init_chunky::@2 and gfx_init_chunky::@3)
Adding NOP phi() at start of @begin
Adding NOP phi() at start of @7
Adding NOP phi() at start of @end
Adding NOP phi() at start of gfx_init_chunky
Adding NOP phi() at start of gfx_init_chunky::@6
CALL GRAPH
Calls in [] to main:2 
Calls in [main] to gfx_init_chunky:7 
Calls in [gfx_init_chunky] to dtvSetCpuBankSegment1:40 dtvSetCpuBankSegment1:48 dtvSetCpuBankSegment1:61 

Created 10 initial phi equivalence classes
Coalesced [38] main::j#3 ← main::j#1
Coalesced [42] gfx_init_chunky::gfxb#8 ← gfx_init_chunky::gfxb#5
Coalesced [43] gfx_init_chunky::gfxbCpuBank#11 ← gfx_init_chunky::gfxbCpuBank#7
Coalesced [47] dtvSetCpuBankSegment1::cpuBankIdx#4 ← dtvSetCpuBankSegment1::cpuBankIdx#1
Coalesced [50] gfx_init_chunky::gfxbCpuBank#14 ← gfx_init_chunky::gfxbCpuBank#2
Coalesced [63] gfx_init_chunky::gfxb#7 ← gfx_init_chunky::gfxb#1
Coalesced [64] gfx_init_chunky::y#8 ← gfx_init_chunky::y#1
Coalesced [65] gfx_init_chunky::gfxbCpuBank#10 ← gfx_init_chunky::gfxbCpuBank#8
Coalesced (already) [66] gfx_init_chunky::gfxb#9 ← gfx_init_chunky::gfxb#1
Coalesced [67] gfx_init_chunky::x#6 ← gfx_init_chunky::x#1
Coalesced (already) [68] gfx_init_chunky::gfxbCpuBank#12 ← gfx_init_chunky::gfxbCpuBank#8
Coalesced [69] gfx_init_chunky::gfxb#10 ← gfx_init_chunky::gfxb#3
Coalesced (already) [70] gfx_init_chunky::gfxbCpuBank#13 ← gfx_init_chunky::gfxbCpuBank#4
Coalesced down to 6 phi equivalence classes
Culled Empty Block (label) main::@18
Culled Empty Block (label) gfx_init_chunky::@10
Culled Empty Block (label) gfx_init_chunky::@11
Culled Empty Block (label) gfx_init_chunky::@12
Adding NOP phi() at start of @begin
Adding NOP phi() at start of @7
Adding NOP phi() at start of @end
Adding NOP phi() at start of gfx_init_chunky
Adding NOP phi() at start of gfx_init_chunky::@6

FINAL CONTROL FLOW GRAPH
@begin: scope:[]  from
  [0] phi()
  to:@7
@7: scope:[]  from @begin
  [1] phi()
  [2] call main 
  to:@end
@end: scope:[]  from @7
  [3] phi()
main: scope:[main]  from @7
  asm { sei  }
  [5] *((const byte*) PROCPORT_DDR#0) ← (const byte) PROCPORT_DDR_MEMORY_MASK#0
  [6] *((const byte*) PROCPORT#0) ← (const byte) PROCPORT_RAM_IO#0
  [7] call gfx_init_chunky 
  to:main::@17
main::@17: scope:[main]  from main
  [8] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0
  [9] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0|(const byte) DTV_COLORRAM_OFF#0|(const byte) DTV_CHUNKY#0|(const byte) DTV_BADLINE_OFF#0
  [10] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3
  [11] *((const byte*) VIC_CONTROL2#0) ← (const byte) VIC_MCM#0|(const byte) VIC_CSEL#0
  [12] *((const byte*) DTV_PLANEB_START_LO#0) ← <(const byte*) CHUNKY#0
  [13] *((const byte*) DTV_PLANEB_START_MI#0) ← >(const byte*) CHUNKY#0
  [14] *((const byte*) DTV_PLANEB_START_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  [15] *((const byte*) DTV_PLANEB_STEP#0) ← (byte/signed byte/word/signed word/dword/signed dword) 8
  [16] *((const byte*) DTV_PLANEB_MODULO_LO#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  [17] *((const byte*) DTV_PLANEB_MODULO_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  [18] *((const byte*) CIA2_PORT_A_DDR#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3
  [19] *((const byte*) CIA2_PORT_A#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3^((byte))((word))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384
  [20] *((const byte*) VIC_MEMORY#0) ← ((byte))((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 6|>((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 2
  to:main::@1
main::@1: scope:[main]  from main::@1 main::@17
  [21] (byte) main::j#2 ← phi( main::@1/(byte) main::j#1 main::@17/(byte/signed byte/word/signed word/dword/signed dword) 0 )
  [22] *((const byte*) DTV_PALETTE#0 + (byte) main::j#2) ← (byte) main::j#2
  [23] (byte) main::j#1 ← ++ (byte) main::j#2
  [24] if((byte) main::j#1!=(byte/signed byte/word/signed word/dword/signed dword) 16) goto main::@1
  to:main::@3
main::@3: scope:[main]  from main::@1 main::@8
  asm { ldx#$ff rff: cpxRASTER bnerff stabilize: nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop cpxRASTER beqeat+0 eat: inx cpx#$08 bnestabilize  }
  [26] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3
  [27] *((const byte*) BORDERCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  to:main::@5
main::@5: scope:[main]  from main::@3 main::@5
  [28] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 66) goto main::@5
  to:main::@7
main::@7: scope:[main]  from main::@5
  asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
  to:main::@8
main::@8: scope:[main]  from main::@7 main::@8
  [30] (byte) main::rst#1 ← *((const byte*) RASTER#0)
  [31] (byte~) main::$31 ← (byte) main::rst#1 & (byte/signed byte/word/signed word/dword/signed dword) 7
  [32] (byte~) main::$32 ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0 | (byte~) main::$31
  [33] *((const byte*) VIC_CONTROL#0) ← (byte~) main::$32
  [34] (byte~) main::$33 ← (byte) main::rst#1 << (byte/signed byte/word/signed word/dword/signed dword) 4
  [35] *((const byte*) BORDERCOL#0) ← (byte~) main::$33
  asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
  [37] if((byte) main::rst#1!=(byte/word/signed word/dword/signed dword) 242) goto main::@8
  to:main::@3
gfx_init_chunky: scope:[gfx_init_chunky]  from main
  [38] phi()
  [39] call dtvSetCpuBankSegment1 
  to:gfx_init_chunky::@1
gfx_init_chunky::@1: scope:[gfx_init_chunky]  from gfx_init_chunky gfx_init_chunky::@5
  [40] (byte) gfx_init_chunky::gfxbCpuBank#7 ← phi( gfx_init_chunky::@5/(byte) gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky/++((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 )
  [40] (byte) gfx_init_chunky::y#6 ← phi( gfx_init_chunky::@5/(byte) gfx_init_chunky::y#1 gfx_init_chunky/(byte/signed byte/word/signed word/dword/signed dword) 0 )
  [40] (byte*) gfx_init_chunky::gfxb#5 ← phi( gfx_init_chunky::@5/(byte*) gfx_init_chunky::gfxb#1 gfx_init_chunky/((byte*))(word/signed word/dword/signed dword) 16384 )
  to:gfx_init_chunky::@2
gfx_init_chunky::@2: scope:[gfx_init_chunky]  from gfx_init_chunky::@1 gfx_init_chunky::@3
  [41] (byte) gfx_init_chunky::gfxbCpuBank#4 ← phi( gfx_init_chunky::@1/(byte) gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::@3/(byte) gfx_init_chunky::gfxbCpuBank#8 )
  [41] (word) gfx_init_chunky::x#2 ← phi( gfx_init_chunky::@1/(byte/signed byte/word/signed word/dword/signed dword) 0 gfx_init_chunky::@3/(word) gfx_init_chunky::x#1 )
  [41] (byte*) gfx_init_chunky::gfxb#3 ← phi( gfx_init_chunky::@1/(byte*) gfx_init_chunky::gfxb#5 gfx_init_chunky::@3/(byte*) gfx_init_chunky::gfxb#1 )
  [42] if((byte*) gfx_init_chunky::gfxb#3!=(word/dword/signed dword) 32768) goto gfx_init_chunky::@3
  to:gfx_init_chunky::@4
gfx_init_chunky::@4: scope:[gfx_init_chunky]  from gfx_init_chunky::@2
  [43] (byte) dtvSetCpuBankSegment1::cpuBankIdx#1 ← (byte) gfx_init_chunky::gfxbCpuBank#4
  [44] call dtvSetCpuBankSegment1 
  to:gfx_init_chunky::@8
gfx_init_chunky::@8: scope:[gfx_init_chunky]  from gfx_init_chunky::@4
  [45] (byte) gfx_init_chunky::gfxbCpuBank#2 ← ++ (byte) gfx_init_chunky::gfxbCpuBank#4
  to:gfx_init_chunky::@3
gfx_init_chunky::@3: scope:[gfx_init_chunky]  from gfx_init_chunky::@2 gfx_init_chunky::@8
  [46] (byte) gfx_init_chunky::gfxbCpuBank#8 ← phi( gfx_init_chunky::@2/(byte) gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::@8/(byte) gfx_init_chunky::gfxbCpuBank#2 )
  [46] (byte*) gfx_init_chunky::gfxb#4 ← phi( gfx_init_chunky::@2/(byte*) gfx_init_chunky::gfxb#3 gfx_init_chunky::@8/((byte*))(word/signed word/dword/signed dword) 16384 )
  [47] (word~) gfx_init_chunky::$6 ← (word) gfx_init_chunky::x#2 + (byte) gfx_init_chunky::y#6
  [48] (byte) gfx_init_chunky::c#0 ← ((byte)) (word~) gfx_init_chunky::$6
  [49] *((byte*) gfx_init_chunky::gfxb#4) ← (byte) gfx_init_chunky::c#0
  [50] (byte*) gfx_init_chunky::gfxb#1 ← ++ (byte*) gfx_init_chunky::gfxb#4
  [51] (word) gfx_init_chunky::x#1 ← ++ (word) gfx_init_chunky::x#2
  [52] if((word) gfx_init_chunky::x#1!=(word/signed word/dword/signed dword) 320) goto gfx_init_chunky::@2
  to:gfx_init_chunky::@5
gfx_init_chunky::@5: scope:[gfx_init_chunky]  from gfx_init_chunky::@3
  [53] (byte) gfx_init_chunky::y#1 ← ++ (byte) gfx_init_chunky::y#6
  [54] if((byte) gfx_init_chunky::y#1!=(byte/signed byte/word/signed word/dword/signed dword) 51) goto gfx_init_chunky::@1
  to:gfx_init_chunky::@6
gfx_init_chunky::@6: scope:[gfx_init_chunky]  from gfx_init_chunky::@5
  [55] phi()
  [56] call dtvSetCpuBankSegment1 
  to:gfx_init_chunky::@return
gfx_init_chunky::@return: scope:[gfx_init_chunky]  from gfx_init_chunky::@6
  [57] return 
  to:@return
dtvSetCpuBankSegment1: scope:[dtvSetCpuBankSegment1]  from gfx_init_chunky gfx_init_chunky::@4 gfx_init_chunky::@6
  [58] (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 ← phi( gfx_init_chunky/((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 gfx_init_chunky::@4/(byte) dtvSetCpuBankSegment1::cpuBankIdx#1 gfx_init_chunky::@6/((byte))(word/signed word/dword/signed dword) 16384/(word/signed word/dword/signed dword) 16384 )
  [59] *((const byte*) dtvSetCpuBankSegment1::cpuBank#0) ← (byte) dtvSetCpuBankSegment1::cpuBankIdx#3
  asm { .byte$32,$dd lda$ff .byte$32,$00  }
  to:dtvSetCpuBankSegment1::@return
dtvSetCpuBankSegment1::@return: scope:[dtvSetCpuBankSegment1]  from dtvSetCpuBankSegment1
  [61] return 
  to:@return


VARIABLE REGISTER WEIGHTS
(byte*) BGCOL
(byte*) BGCOL1
(byte*) BGCOL2
(byte*) BGCOL3
(byte*) BGCOL4
(byte) BLACK
(byte) BLUE
(byte*) BORDERCOL
(byte) BROWN
(byte*) CHARGEN
(byte*) CHUNKY
(byte*) CIA1_INTERRUPT
(byte*) CIA1_PORT_A
(byte*) CIA1_PORT_A_DDR
(byte*) CIA1_PORT_B
(byte*) CIA1_PORT_B_DDR
(byte*) CIA2_INTERRUPT
(byte*) CIA2_PORT_A
(byte*) CIA2_PORT_A_DDR
(byte*) CIA2_PORT_B
(byte*) CIA2_PORT_B_DDR
(byte) CIA_INTERRUPT_CLEAR
(byte*) COLS
(byte) CYAN
(byte*) D011
(byte*) D016
(byte*) D018
(byte) DARK_GREY
(byte) DTV_BADLINE_OFF
(byte*) DTV_BLITTER_ALU
(byte*) DTV_BLITTER_CONTROL
(byte*) DTV_BLITTER_CONTROL2
(byte*) DTV_BLITTER_DEST_HI
(byte*) DTV_BLITTER_DEST_LIN_HI
(byte*) DTV_BLITTER_DEST_LIN_LO
(byte*) DTV_BLITTER_DEST_LO
(byte*) DTV_BLITTER_DEST_MI
(byte*) DTV_BLITTER_DEST_MOD_HI
(byte*) DTV_BLITTER_DEST_MOD_LO
(byte*) DTV_BLITTER_DEST_STEP
(byte*) DTV_BLITTER_LEN_HI
(byte*) DTV_BLITTER_LEN_LO
(byte*) DTV_BLITTER_SRCA_HI
(byte*) DTV_BLITTER_SRCA_LIN_HI
(byte*) DTV_BLITTER_SRCA_LIN_LO
(byte*) DTV_BLITTER_SRCA_LO
(byte*) DTV_BLITTER_SRCA_MI
(byte*) DTV_BLITTER_SRCA_MOD_HI
(byte*) DTV_BLITTER_SRCA_MOD_LO
(byte*) DTV_BLITTER_SRCA_STEP
(byte*) DTV_BLITTER_SRCB_HI
(byte*) DTV_BLITTER_SRCB_LIN_HI
(byte*) DTV_BLITTER_SRCB_LIN_LO
(byte*) DTV_BLITTER_SRCB_LO
(byte*) DTV_BLITTER_SRCB_MI
(byte*) DTV_BLITTER_SRCB_MOD_HI
(byte*) DTV_BLITTER_SRCB_MOD_LO
(byte*) DTV_BLITTER_SRCB_STEP
(byte*) DTV_BLITTER_TRANSPARANCY
(byte) DTV_BLIT_ADD
(byte) DTV_BLIT_AND
(byte) DTV_BLIT_CIA_IRQ
(byte) DTV_BLIT_CLEAR_IRQ
(byte) DTV_BLIT_DEST_CONT
(byte) DTV_BLIT_DEST_FWD
(byte) DTV_BLIT_DISABLE_B
(byte) DTV_BLIT_FORCE_START
(byte) DTV_BLIT_IRQ_EN
(byte) DTV_BLIT_NAND
(byte) DTV_BLIT_NOR
(byte) DTV_BLIT_OR
(byte) DTV_BLIT_SHIFT0
(byte) DTV_BLIT_SHIFT1
(byte) DTV_BLIT_SHIFT2
(byte) DTV_BLIT_SHIFT3
(byte) DTV_BLIT_SHIFT4
(byte) DTV_BLIT_SHIFT5
(byte) DTV_BLIT_SHIFT6
(byte) DTV_BLIT_SHIFT7
(byte) DTV_BLIT_SRCA_CONT
(byte) DTV_BLIT_SRCA_FWD
(byte) DTV_BLIT_SRCB_CONT
(byte) DTV_BLIT_SRCB_FWD
(byte) DTV_BLIT_STATUS_BUSY
(byte) DTV_BLIT_STATUS_IRQ
(byte) DTV_BLIT_SUB
(byte) DTV_BLIT_TRANSPARANCY_NONE
(byte) DTV_BLIT_VBLANK
(byte) DTV_BLIT_VIC_IRQ
(byte) DTV_BLIT_WRITE_NONTRANSPARENT
(byte) DTV_BLIT_WRITE_TRANSPARENT
(byte) DTV_BLIT_XNOR
(byte) DTV_BLIT_XOR
(byte) DTV_BORDER_OFF
(byte) DTV_CHUNKY
(byte) DTV_COLORRAM_OFF
(dword) DTV_COLOR_BANK_DEFAULT
(byte*) DTV_COLOR_BANK_HI
(byte*) DTV_COLOR_BANK_LO
(byte*) DTV_CONTROL
(byte*) DTV_FEATURE
(byte) DTV_FEATURE_DISABLE_TIL_RESET
(byte) DTV_FEATURE_ENABLE
(byte*) DTV_GRAPHICS_HICOL_BANK
(byte*) DTV_GRAPHICS_VIC_BANK
(byte) DTV_HIGHCOLOR
(byte) DTV_LINEAR
(byte) DTV_OVERSCAN
(byte*) DTV_PALETTE
(byte[16]) DTV_PALETTE_DEFAULT
(byte*) DTV_PLANEA_MODULO_HI
(byte*) DTV_PLANEA_MODULO_LO
(byte*) DTV_PLANEA_START_HI
(byte*) DTV_PLANEA_START_LO
(byte*) DTV_PLANEA_START_MI
(byte*) DTV_PLANEA_STEP
(byte*) DTV_PLANEB_MODULO_HI
(byte*) DTV_PLANEB_MODULO_LO
(byte*) DTV_PLANEB_START_HI
(byte*) DTV_PLANEB_START_LO
(byte*) DTV_PLANEB_START_MI
(byte*) DTV_PLANEB_STEP
(byte*) DTV_SPRITE_BANK
(byte) GREEN
(byte) GREY
(void()**) HARDWARE_IRQ
(byte) IRQ_COLLISION_BG
(byte) IRQ_COLLISION_SPRITE
(byte*) IRQ_ENABLE
(byte) IRQ_LIGHTPEN
(byte) IRQ_RASTER
(byte*) IRQ_STATUS
(void()**) KERNEL_IRQ
(byte*) LIGHTPEN_X
(byte*) LIGHTPEN_Y
(byte) LIGHT_BLUE
(byte) LIGHT_GREEN
(byte) LIGHT_GREY
(byte) ORANGE
(byte) PINK
(byte*) PROCPORT
(byte) PROCPORT_BASIC_KERNEL_IO
(byte*) PROCPORT_DDR
(byte) PROCPORT_DDR_MEMORY_MASK
(byte) PROCPORT_KERNEL_IO
(byte) PROCPORT_RAM_ALL
(byte) PROCPORT_RAM_CHARROM
(byte) PROCPORT_RAM_IO
(byte) PURPLE
(byte*) RASTER
(byte) RED
(byte*) SPRITES_COLS
(byte*) SPRITES_ENABLE
(byte*) SPRITES_EXPAND_X
(byte*) SPRITES_EXPAND_Y
(byte*) SPRITES_MC
(byte*) SPRITES_MC1
(byte*) SPRITES_MC2
(byte*) SPRITES_PRIORITY
(byte*) SPRITES_XMSB
(byte*) SPRITES_XPOS
(byte*) SPRITES_YPOS
(word) SPRITE_PTRS
(byte) VIC_BMM
(byte*) VIC_CONTROL
(byte*) VIC_CONTROL2
(byte) VIC_CSEL
(byte) VIC_DEN
(byte) VIC_ECM
(byte) VIC_MCM
(byte*) VIC_MEMORY
(byte) VIC_RSEL
(byte) VIC_RST8
(byte) WHITE
(byte) YELLOW
(void()) dtvSetCpuBankSegment1((byte) dtvSetCpuBankSegment1::cpuBankIdx)
(byte*) dtvSetCpuBankSegment1::cpuBank
(byte) dtvSetCpuBankSegment1::cpuBankIdx
(byte) dtvSetCpuBankSegment1::cpuBankIdx#1 202.0
(byte) dtvSetCpuBankSegment1::cpuBankIdx#3 103.0
(void()) gfx_init_chunky()
(word~) gfx_init_chunky::$6 202.0
(byte) gfx_init_chunky::c
(byte) gfx_init_chunky::c#0 202.0
(byte*) gfx_init_chunky::gfxb
(byte*) gfx_init_chunky::gfxb#1 42.599999999999994
(byte*) gfx_init_chunky::gfxb#3 157.0
(byte*) gfx_init_chunky::gfxb#4 75.75
(byte*) gfx_init_chunky::gfxb#5 22.0
(byte) gfx_init_chunky::gfxbCpuBank
(byte) gfx_init_chunky::gfxbCpuBank#2 202.0
(byte) gfx_init_chunky::gfxbCpuBank#4 103.75
(byte) gfx_init_chunky::gfxbCpuBank#7 22.0
(byte) gfx_init_chunky::gfxbCpuBank#8 34.888888888888886
(word) gfx_init_chunky::x
(word) gfx_init_chunky::x#1 151.5
(word) gfx_init_chunky::x#2 30.299999999999997
(byte) gfx_init_chunky::y
(byte) gfx_init_chunky::y#1 16.5
(byte) gfx_init_chunky::y#6 9.461538461538462
(void()) main()
(byte~) main::$31 202.0
(byte~) main::$32 202.0
(byte~) main::$33 202.0
(byte) main::j
(byte) main::j#1 16.5
(byte) main::j#2 22.0
(byte) main::rst
(byte) main::rst#1 57.714285714285715

Initial phi equivalence classes
[ main::j#2 main::j#1 ]
[ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
[ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ]
[ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ]
[ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ]
[ dtvSetCpuBankSegment1::cpuBankIdx#3 dtvSetCpuBankSegment1::cpuBankIdx#1 ]
Added variable main::rst#1 to zero page equivalence class [ main::rst#1 ]
Added variable main::$31 to zero page equivalence class [ main::$31 ]
Added variable main::$32 to zero page equivalence class [ main::$32 ]
Added variable main::$33 to zero page equivalence class [ main::$33 ]
Added variable gfx_init_chunky::$6 to zero page equivalence class [ gfx_init_chunky::$6 ]
Added variable gfx_init_chunky::c#0 to zero page equivalence class [ gfx_init_chunky::c#0 ]
Complete equivalence classes
[ main::j#2 main::j#1 ]
[ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
[ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ]
[ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ]
[ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ]
[ dtvSetCpuBankSegment1::cpuBankIdx#3 dtvSetCpuBankSegment1::cpuBankIdx#1 ]
[ main::rst#1 ]
[ main::$31 ]
[ main::$32 ]
[ main::$33 ]
[ gfx_init_chunky::$6 ]
[ gfx_init_chunky::c#0 ]
Allocated zp ZP_BYTE:2 [ main::j#2 main::j#1 ]
Allocated zp ZP_BYTE:3 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
Allocated zp ZP_WORD:4 [ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ]
Allocated zp ZP_BYTE:6 [ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ]
Allocated zp ZP_WORD:7 [ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ]
Allocated zp ZP_BYTE:9 [ dtvSetCpuBankSegment1::cpuBankIdx#3 dtvSetCpuBankSegment1::cpuBankIdx#1 ]
Allocated zp ZP_BYTE:10 [ main::rst#1 ]
Allocated zp ZP_BYTE:11 [ main::$31 ]
Allocated zp ZP_BYTE:12 [ main::$32 ]
Allocated zp ZP_BYTE:13 [ main::$33 ]
Allocated zp ZP_WORD:14 [ gfx_init_chunky::$6 ]
Allocated zp ZP_BYTE:16 [ gfx_init_chunky::c#0 ]

INITIAL ASM
//SEG0 File Comments
// C64DTV 8bpp charmode stretcher
//SEG1 Basic Upstart
.pc = $801 "Basic"
:BasicUpstart(bbegin)
.pc = $80d "Program"
//SEG2 Global Constants & labels
  // Processor port data direction register
  .label PROCPORT_DDR = 0
  // Mask for PROCESSOR_PORT_DDR which allows only memory configuration to be written
  .const PROCPORT_DDR_MEMORY_MASK = 7
  // Processor Port Register controlling RAM/ROM configuration and the datasette
  .label PROCPORT = 1
  // RAM in $A000, $E000 I/O in $D000
  .const PROCPORT_RAM_IO = $35
  .label RASTER = $d012
  .label BORDERCOL = $d020
  .label VIC_CONTROL = $d011
  .const VIC_ECM = $40
  .const VIC_DEN = $10
  .const VIC_RSEL = 8
  .label VIC_CONTROL2 = $d016
  .const VIC_MCM = $10
  .const VIC_CSEL = 8
  .label VIC_MEMORY = $d018
  // CIA#2 Port A: Serial bus, RS-232, VIC memory bank
  .label CIA2_PORT_A = $dd00
  // CIA #2 Port A data direction register.
  .label CIA2_PORT_A_DDR = $dd02
  // Feature enables or disables the extra C64 DTV features
  .label DTV_FEATURE = $d03f
  .const DTV_FEATURE_ENABLE = 1
  // Controls the graphics modes of the C64 DTV
  .label DTV_CONTROL = $d03c
  .const DTV_LINEAR = 1
  .const DTV_HIGHCOLOR = 4
  .const DTV_COLORRAM_OFF = $10
  .const DTV_BADLINE_OFF = $20
  .const DTV_CHUNKY = $40
  // Defines colors for the 16 first colors ($00-$0f)
  .label DTV_PALETTE = $d200
  // Linear Graphics Plane B Counter Control
  .label DTV_PLANEB_START_LO = $d049
  .label DTV_PLANEB_START_MI = $d04a
  .label DTV_PLANEB_START_HI = $d04b
  .label DTV_PLANEB_STEP = $d04c
  .label DTV_PLANEB_MODULO_LO = $d047
  .label DTV_PLANEB_MODULO_HI = $d048
  // Plane with all pixels
  .label CHUNKY = $8000
//SEG3 @begin
bbegin:
//SEG4 [1] phi from @begin to @7 [phi:@begin->@7]
b7_from_bbegin:
  jmp b7
//SEG5 @7
b7:
//SEG6 [2] call main 
  jsr main
//SEG7 [3] phi from @7 to @end [phi:@7->@end]
bend_from_b7:
  jmp bend
//SEG8 @end
bend:
//SEG9 main
main: {
    .label _31 = $b
    .label _32 = $c
    .label _33 = $d
    .label j = 2
    .label rst = $a
  //SEG10 asm { sei  }
    sei
  //SEG11 [5] *((const byte*) PROCPORT_DDR#0) ← (const byte) PROCPORT_DDR_MEMORY_MASK#0 -- _deref_pbuc1=vbuc2 
    // Disable normal interrupt (prevent keyboard reading glitches and allows to hide basic/kernal)
    // Disable kernal & basic
    lda #PROCPORT_DDR_MEMORY_MASK
    sta PROCPORT_DDR
  //SEG12 [6] *((const byte*) PROCPORT#0) ← (const byte) PROCPORT_RAM_IO#0 -- _deref_pbuc1=vbuc2 
    lda #PROCPORT_RAM_IO
    sta PROCPORT
  //SEG13 [7] call gfx_init_chunky 
  //SEG14 [38] phi from main to gfx_init_chunky [phi:main->gfx_init_chunky]
  gfx_init_chunky_from_main:
    jsr gfx_init_chunky
    jmp b17
  //SEG15 main::@17
  b17:
  //SEG16 [8] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 -- _deref_pbuc1=vbuc2 
    // Enable DTV extended modes
    lda #DTV_FEATURE_ENABLE
    sta DTV_FEATURE
  //SEG17 [9] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0|(const byte) DTV_COLORRAM_OFF#0|(const byte) DTV_CHUNKY#0|(const byte) DTV_BADLINE_OFF#0 -- _deref_pbuc1=vbuc2 
    // 8BPP Pixel Cell Mode
    lda #DTV_HIGHCOLOR|DTV_LINEAR|DTV_COLORRAM_OFF|DTV_CHUNKY|DTV_BADLINE_OFF
    sta DTV_CONTROL
  //SEG18 [10] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 -- _deref_pbuc1=vbuc2 
    lda #VIC_DEN|VIC_ECM|VIC_RSEL|3
    sta VIC_CONTROL
  //SEG19 [11] *((const byte*) VIC_CONTROL2#0) ← (const byte) VIC_MCM#0|(const byte) VIC_CSEL#0 -- _deref_pbuc1=vbuc2 
    lda #VIC_MCM|VIC_CSEL
    sta VIC_CONTROL2
  //SEG20 [12] *((const byte*) DTV_PLANEB_START_LO#0) ← <(const byte*) CHUNKY#0 -- _deref_pbuc1=vbuc2 
    // Plane B: CHUNKY
    lda #<CHUNKY
    sta DTV_PLANEB_START_LO
  //SEG21 [13] *((const byte*) DTV_PLANEB_START_MI#0) ← >(const byte*) CHUNKY#0 -- _deref_pbuc1=vbuc2 
    lda #>CHUNKY
    sta DTV_PLANEB_START_MI
  //SEG22 [14] *((const byte*) DTV_PLANEB_START_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta DTV_PLANEB_START_HI
  //SEG23 [15] *((const byte*) DTV_PLANEB_STEP#0) ← (byte/signed byte/word/signed word/dword/signed dword) 8 -- _deref_pbuc1=vbuc2 
    lda #8
    sta DTV_PLANEB_STEP
  //SEG24 [16] *((const byte*) DTV_PLANEB_MODULO_LO#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta DTV_PLANEB_MODULO_LO
  //SEG25 [17] *((const byte*) DTV_PLANEB_MODULO_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta DTV_PLANEB_MODULO_HI
  //SEG26 [18] *((const byte*) CIA2_PORT_A_DDR#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3 -- _deref_pbuc1=vbuc2 
    // VIC Graphics Bank
    lda #3
    sta CIA2_PORT_A_DDR
  //SEG27 [19] *((const byte*) CIA2_PORT_A#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3^((byte))((word))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 -- _deref_pbuc1=vbuc2 
    // Set VIC Bank bits to output - all others to input
    lda #3^CHUNKY/$4000
    sta CIA2_PORT_A
  //SEG28 [20] *((const byte*) VIC_MEMORY#0) ← ((byte))((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 6|>((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 2 -- _deref_pbuc1=vbuc2 
    // Set VIC Bank
    // VIC memory
    lda #(CHUNKY&$3fff)>>6|(0)>>2
    sta VIC_MEMORY
  //SEG29 [21] phi from main::@17 to main::@1 [phi:main::@17->main::@1]
  b1_from_b17:
  //SEG30 [21] phi (byte) main::j#2 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:main::@17->main::@1#0] -- vbuz1=vbuc1 
    lda #0
    sta j
    jmp b1
  // DTV Palette - Grey Tones
  //SEG31 [21] phi from main::@1 to main::@1 [phi:main::@1->main::@1]
  b1_from_b1:
  //SEG32 [21] phi (byte) main::j#2 = (byte) main::j#1 [phi:main::@1->main::@1#0] -- register_copy 
    jmp b1
  //SEG33 main::@1
  b1:
  //SEG34 [22] *((const byte*) DTV_PALETTE#0 + (byte) main::j#2) ← (byte) main::j#2 -- pbuc1_derefidx_vbuz1=vbuz1 
    ldy j
    tya
    sta DTV_PALETTE,y
  //SEG35 [23] (byte) main::j#1 ← ++ (byte) main::j#2 -- vbuz1=_inc_vbuz1 
    inc j
  //SEG36 [24] if((byte) main::j#1!=(byte/signed byte/word/signed word/dword/signed dword) 16) goto main::@1 -- vbuz1_neq_vbuc1_then_la1 
    lda j
    cmp #$10
    bne b1_from_b1
    jmp b3
  //SEG37 main::@3
  b3:
  //SEG38 asm { ldx#$ff rff: cpxRASTER bnerff stabilize: nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop cpxRASTER beqeat+0 eat: inx cpx#$08 bnestabilize  }
    // Stabilize Raster
    ldx #$ff
  rff:
    cpx RASTER
    bne rff
  stabilize:
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    cpx RASTER
    beq eat+0
  eat:
    inx
    cpx #8
    bne stabilize
  //SEG39 [26] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 -- _deref_pbuc1=vbuc2 
    lda #VIC_DEN|VIC_ECM|VIC_RSEL|3
    sta VIC_CONTROL
  //SEG40 [27] *((const byte*) BORDERCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta BORDERCOL
    jmp b5
  //SEG41 main::@5
  b5:
  //SEG42 [28] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 66) goto main::@5 -- _deref_pbuc1_neq_vbuc2_then_la1 
    lda RASTER
    cmp #$42
    bne b5
    jmp b7
  //SEG43 main::@7
  b7:
  //SEG44 asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    jmp b8
  //SEG45 main::@8
  b8:
  //SEG46 [30] (byte) main::rst#1 ← *((const byte*) RASTER#0) -- vbuz1=_deref_pbuc1 
    lda RASTER
    sta rst
  //SEG47 [31] (byte~) main::$31 ← (byte) main::rst#1 & (byte/signed byte/word/signed word/dword/signed dword) 7 -- vbuz1=vbuz2_band_vbuc1 
    lda #7
    and rst
    sta _31
  //SEG48 [32] (byte~) main::$32 ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0 | (byte~) main::$31 -- vbuz1=vbuc1_bor_vbuz2 
    lda #VIC_DEN|VIC_ECM|VIC_RSEL
    ora _31
    sta _32
  //SEG49 [33] *((const byte*) VIC_CONTROL#0) ← (byte~) main::$32 -- _deref_pbuc1=vbuz1 
    lda _32
    sta VIC_CONTROL
  //SEG50 [34] (byte~) main::$33 ← (byte) main::rst#1 << (byte/signed byte/word/signed word/dword/signed dword) 4 -- vbuz1=vbuz2_rol_4 
    lda rst
    asl
    asl
    asl
    asl
    sta _33
  //SEG51 [35] *((const byte*) BORDERCOL#0) ← (byte~) main::$33 -- _deref_pbuc1=vbuz1 
    lda _33
    sta BORDERCOL
  //SEG52 asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
  //SEG53 [37] if((byte) main::rst#1!=(byte/word/signed word/dword/signed dword) 242) goto main::@8 -- vbuz1_neq_vbuc1_then_la1 
    lda rst
    cmp #$f2
    bne b8
    jmp b3
}
//SEG54 gfx_init_chunky
// Initialize Plane with 8bpp chunky
gfx_init_chunky: {
    .label _6 = $e
    .label c = $10
    .label gfxb = 7
    .label x = 4
    .label gfxbCpuBank = 6
    .label y = 3
  //SEG55 [39] call dtvSetCpuBankSegment1 
  //SEG56 [58] phi from gfx_init_chunky to dtvSetCpuBankSegment1 [phi:gfx_init_chunky->dtvSetCpuBankSegment1]
  dtvSetCpuBankSegment1_from_gfx_init_chunky:
  //SEG57 [58] phi (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 = ((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky->dtvSetCpuBankSegment1#0] -- vbuz1=vbuc1 
    lda #$ff&CHUNKY/$4000
    sta dtvSetCpuBankSegment1.cpuBankIdx
    jsr dtvSetCpuBankSegment1
  //SEG58 [40] phi from gfx_init_chunky to gfx_init_chunky::@1 [phi:gfx_init_chunky->gfx_init_chunky::@1]
  b1_from_gfx_init_chunky:
  //SEG59 [40] phi (byte) gfx_init_chunky::gfxbCpuBank#7 = ++((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky->gfx_init_chunky::@1#0] -- vbuz1=vbuc1 
    lda #($ff&CHUNKY/$4000)+1
    sta gfxbCpuBank
  //SEG60 [40] phi (byte) gfx_init_chunky::y#6 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:gfx_init_chunky->gfx_init_chunky::@1#1] -- vbuz1=vbuc1 
    lda #0
    sta y
  //SEG61 [40] phi (byte*) gfx_init_chunky::gfxb#5 = ((byte*))(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky->gfx_init_chunky::@1#2] -- pbuz1=pbuc1 
    lda #<$4000
    sta gfxb
    lda #>$4000
    sta gfxb+1
    jmp b1
  //SEG62 [40] phi from gfx_init_chunky::@5 to gfx_init_chunky::@1 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1]
  b1_from_b5:
  //SEG63 [40] phi (byte) gfx_init_chunky::gfxbCpuBank#7 = (byte) gfx_init_chunky::gfxbCpuBank#8 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1#0] -- register_copy 
  //SEG64 [40] phi (byte) gfx_init_chunky::y#6 = (byte) gfx_init_chunky::y#1 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1#1] -- register_copy 
  //SEG65 [40] phi (byte*) gfx_init_chunky::gfxb#5 = (byte*) gfx_init_chunky::gfxb#1 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1#2] -- register_copy 
    jmp b1
  //SEG66 gfx_init_chunky::@1
  b1:
  //SEG67 [41] phi from gfx_init_chunky::@1 to gfx_init_chunky::@2 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2]
  b2_from_b1:
  //SEG68 [41] phi (byte) gfx_init_chunky::gfxbCpuBank#4 = (byte) gfx_init_chunky::gfxbCpuBank#7 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2#0] -- register_copy 
  //SEG69 [41] phi (word) gfx_init_chunky::x#2 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2#1] -- vwuz1=vbuc1 
    lda #<0
    sta x
    lda #>0
    sta x+1
  //SEG70 [41] phi (byte*) gfx_init_chunky::gfxb#3 = (byte*) gfx_init_chunky::gfxb#5 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2#2] -- register_copy 
    jmp b2
  //SEG71 [41] phi from gfx_init_chunky::@3 to gfx_init_chunky::@2 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2]
  b2_from_b3:
  //SEG72 [41] phi (byte) gfx_init_chunky::gfxbCpuBank#4 = (byte) gfx_init_chunky::gfxbCpuBank#8 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2#0] -- register_copy 
  //SEG73 [41] phi (word) gfx_init_chunky::x#2 = (word) gfx_init_chunky::x#1 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2#1] -- register_copy 
  //SEG74 [41] phi (byte*) gfx_init_chunky::gfxb#3 = (byte*) gfx_init_chunky::gfxb#1 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2#2] -- register_copy 
    jmp b2
  //SEG75 gfx_init_chunky::@2
  b2:
  //SEG76 [42] if((byte*) gfx_init_chunky::gfxb#3!=(word/dword/signed dword) 32768) goto gfx_init_chunky::@3 -- pbuz1_neq_vwuc1_then_la1 
    lda gfxb+1
    cmp #>$8000
    bne b3_from_b2
    lda gfxb
    cmp #<$8000
    bne b3_from_b2
    jmp b4
  //SEG77 gfx_init_chunky::@4
  b4:
  //SEG78 [43] (byte) dtvSetCpuBankSegment1::cpuBankIdx#1 ← (byte) gfx_init_chunky::gfxbCpuBank#4 -- vbuz1=vbuz2 
    lda gfxbCpuBank
    sta dtvSetCpuBankSegment1.cpuBankIdx
  //SEG79 [44] call dtvSetCpuBankSegment1 
  //SEG80 [58] phi from gfx_init_chunky::@4 to dtvSetCpuBankSegment1 [phi:gfx_init_chunky::@4->dtvSetCpuBankSegment1]
  dtvSetCpuBankSegment1_from_b4:
  //SEG81 [58] phi (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 = (byte) dtvSetCpuBankSegment1::cpuBankIdx#1 [phi:gfx_init_chunky::@4->dtvSetCpuBankSegment1#0] -- register_copy 
    jsr dtvSetCpuBankSegment1
    jmp b8
  //SEG82 gfx_init_chunky::@8
  b8:
  //SEG83 [45] (byte) gfx_init_chunky::gfxbCpuBank#2 ← ++ (byte) gfx_init_chunky::gfxbCpuBank#4 -- vbuz1=_inc_vbuz1 
    inc gfxbCpuBank
  //SEG84 [46] phi from gfx_init_chunky::@8 to gfx_init_chunky::@3 [phi:gfx_init_chunky::@8->gfx_init_chunky::@3]
  b3_from_b8:
  //SEG85 [46] phi (byte) gfx_init_chunky::gfxbCpuBank#8 = (byte) gfx_init_chunky::gfxbCpuBank#2 [phi:gfx_init_chunky::@8->gfx_init_chunky::@3#0] -- register_copy 
  //SEG86 [46] phi (byte*) gfx_init_chunky::gfxb#4 = ((byte*))(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky::@8->gfx_init_chunky::@3#1] -- pbuz1=pbuc1 
    lda #<$4000
    sta gfxb
    lda #>$4000
    sta gfxb+1
    jmp b3
  //SEG87 [46] phi from gfx_init_chunky::@2 to gfx_init_chunky::@3 [phi:gfx_init_chunky::@2->gfx_init_chunky::@3]
  b3_from_b2:
  //SEG88 [46] phi (byte) gfx_init_chunky::gfxbCpuBank#8 = (byte) gfx_init_chunky::gfxbCpuBank#4 [phi:gfx_init_chunky::@2->gfx_init_chunky::@3#0] -- register_copy 
  //SEG89 [46] phi (byte*) gfx_init_chunky::gfxb#4 = (byte*) gfx_init_chunky::gfxb#3 [phi:gfx_init_chunky::@2->gfx_init_chunky::@3#1] -- register_copy 
    jmp b3
  //SEG90 gfx_init_chunky::@3
  b3:
  //SEG91 [47] (word~) gfx_init_chunky::$6 ← (word) gfx_init_chunky::x#2 + (byte) gfx_init_chunky::y#6 -- vwuz1=vwuz2_plus_vbuz3 
    lda y
    clc
    adc x
    sta _6
    lda #0
    adc x+1
    sta _6+1
  //SEG92 [48] (byte) gfx_init_chunky::c#0 ← ((byte)) (word~) gfx_init_chunky::$6 -- vbuz1=_byte_vwuz2 
    lda _6
    sta c
  //SEG93 [49] *((byte*) gfx_init_chunky::gfxb#4) ← (byte) gfx_init_chunky::c#0 -- _deref_pbuz1=vbuz2 
    lda c
    ldy #0
    sta (gfxb),y
  //SEG94 [50] (byte*) gfx_init_chunky::gfxb#1 ← ++ (byte*) gfx_init_chunky::gfxb#4 -- pbuz1=_inc_pbuz1 
    inc gfxb
    bne !+
    inc gfxb+1
  !:
  //SEG95 [51] (word) gfx_init_chunky::x#1 ← ++ (word) gfx_init_chunky::x#2 -- vwuz1=_inc_vwuz1 
    inc x
    bne !+
    inc x+1
  !:
  //SEG96 [52] if((word) gfx_init_chunky::x#1!=(word/signed word/dword/signed dword) 320) goto gfx_init_chunky::@2 -- vwuz1_neq_vwuc1_then_la1 
    lda x+1
    cmp #>$140
    bne b2_from_b3
    lda x
    cmp #<$140
    bne b2_from_b3
    jmp b5
  //SEG97 gfx_init_chunky::@5
  b5:
  //SEG98 [53] (byte) gfx_init_chunky::y#1 ← ++ (byte) gfx_init_chunky::y#6 -- vbuz1=_inc_vbuz1 
    inc y
  //SEG99 [54] if((byte) gfx_init_chunky::y#1!=(byte/signed byte/word/signed word/dword/signed dword) 51) goto gfx_init_chunky::@1 -- vbuz1_neq_vbuc1_then_la1 
    lda y
    cmp #$33
    bne b1_from_b5
  //SEG100 [55] phi from gfx_init_chunky::@5 to gfx_init_chunky::@6 [phi:gfx_init_chunky::@5->gfx_init_chunky::@6]
  b6_from_b5:
    jmp b6
  //SEG101 gfx_init_chunky::@6
  b6:
  //SEG102 [56] call dtvSetCpuBankSegment1 
  //SEG103 [58] phi from gfx_init_chunky::@6 to dtvSetCpuBankSegment1 [phi:gfx_init_chunky::@6->dtvSetCpuBankSegment1]
  dtvSetCpuBankSegment1_from_b6:
  //SEG104 [58] phi (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 = ((byte))(word/signed word/dword/signed dword) 16384/(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky::@6->dtvSetCpuBankSegment1#0] -- vbuz1=vbuc1 
    lda #$4000/$4000
    sta dtvSetCpuBankSegment1.cpuBankIdx
    jsr dtvSetCpuBankSegment1
    jmp breturn
  //SEG105 gfx_init_chunky::@return
  breturn:
  //SEG106 [57] return 
    rts
}
//SEG107 dtvSetCpuBankSegment1
// Set the memory pointed to by CPU BANK 1 SEGMENT ($4000-$7fff)
// This sets which actual memory is addressed when the CPU reads/writes to $4000-$7fff
// The actual memory addressed will be $4000*cpuSegmentIdx
// dtvSetCpuBankSegment1(byte zeropage(9) cpuBankIdx)
dtvSetCpuBankSegment1: {
    // Move CPU BANK 1 SEGMENT ($4000-$7fff)
    .label cpuBank = $ff
    .label cpuBankIdx = 9
  //SEG108 [59] *((const byte*) dtvSetCpuBankSegment1::cpuBank#0) ← (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 -- _deref_pbuc1=vbuz1 
    lda cpuBankIdx
    sta cpuBank
  //SEG109 asm { .byte$32,$dd lda$ff .byte$32,$00  }
    .byte $32, $dd
    lda $ff
    .byte $32, $00
    jmp breturn
  //SEG110 dtvSetCpuBankSegment1::@return
  breturn:
  //SEG111 [61] return 
    rts
}

REGISTER UPLIFT POTENTIAL REGISTERS
Statement [5] *((const byte*) PROCPORT_DDR#0) ← (const byte) PROCPORT_DDR_MEMORY_MASK#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [6] *((const byte*) PROCPORT#0) ← (const byte) PROCPORT_RAM_IO#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [8] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [9] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0|(const byte) DTV_COLORRAM_OFF#0|(const byte) DTV_CHUNKY#0|(const byte) DTV_BADLINE_OFF#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [10] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [11] *((const byte*) VIC_CONTROL2#0) ← (const byte) VIC_MCM#0|(const byte) VIC_CSEL#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [12] *((const byte*) DTV_PLANEB_START_LO#0) ← <(const byte*) CHUNKY#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [13] *((const byte*) DTV_PLANEB_START_MI#0) ← >(const byte*) CHUNKY#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [14] *((const byte*) DTV_PLANEB_START_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [15] *((const byte*) DTV_PLANEB_STEP#0) ← (byte/signed byte/word/signed word/dword/signed dword) 8 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [16] *((const byte*) DTV_PLANEB_MODULO_LO#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [17] *((const byte*) DTV_PLANEB_MODULO_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [18] *((const byte*) CIA2_PORT_A_DDR#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [19] *((const byte*) CIA2_PORT_A#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3^((byte))((word))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [20] *((const byte*) VIC_MEMORY#0) ← ((byte))((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 6|>((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 2 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement asm { ldx#$ff rff: cpxRASTER bnerff stabilize: nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop cpxRASTER beqeat+0 eat: inx cpx#$08 bnestabilize  } always clobbers reg byte x 
Statement [26] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [27] *((const byte*) BORDERCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [28] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 66) goto main::@5 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [31] (byte~) main::$31 ← (byte) main::rst#1 & (byte/signed byte/word/signed word/dword/signed dword) 7 [ main::rst#1 main::$31 ] ( main:2 [ main::rst#1 main::$31 ] ) always clobbers reg byte a 
Removing always clobbered register reg byte a as potential for zp ZP_BYTE:10 [ main::rst#1 ]
Statement [32] (byte~) main::$32 ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0 | (byte~) main::$31 [ main::rst#1 main::$32 ] ( main:2 [ main::rst#1 main::$32 ] ) always clobbers reg byte a 
Statement [34] (byte~) main::$33 ← (byte) main::rst#1 << (byte/signed byte/word/signed word/dword/signed dword) 4 [ main::rst#1 main::$33 ] ( main:2 [ main::rst#1 main::$33 ] ) always clobbers reg byte a 
Statement [42] if((byte*) gfx_init_chunky::gfxb#3!=(word/dword/signed dword) 32768) goto gfx_init_chunky::@3 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxb#3 gfx_init_chunky::x#2 gfx_init_chunky::gfxbCpuBank#4 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxb#3 gfx_init_chunky::x#2 gfx_init_chunky::gfxbCpuBank#4 ] ) always clobbers reg byte a 
Removing always clobbered register reg byte a as potential for zp ZP_BYTE:3 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
Removing always clobbered register reg byte a as potential for zp ZP_BYTE:6 [ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ]
Statement [47] (word~) gfx_init_chunky::$6 ← (word) gfx_init_chunky::x#2 + (byte) gfx_init_chunky::y#6 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 gfx_init_chunky::$6 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 gfx_init_chunky::$6 ] ) always clobbers reg byte a 
Statement [48] (byte) gfx_init_chunky::c#0 ← ((byte)) (word~) gfx_init_chunky::$6 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 gfx_init_chunky::c#0 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 gfx_init_chunky::c#0 ] ) always clobbers reg byte a 
Statement [49] *((byte*) gfx_init_chunky::gfxb#4) ← (byte) gfx_init_chunky::c#0 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 ] ) always clobbers reg byte y 
Removing always clobbered register reg byte y as potential for zp ZP_BYTE:3 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
Removing always clobbered register reg byte y as potential for zp ZP_BYTE:6 [ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ]
Statement [52] if((word) gfx_init_chunky::x#1!=(word/signed word/dword/signed dword) 320) goto gfx_init_chunky::@2 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxb#1 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#1 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxb#1 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#1 ] ) always clobbers reg byte a 
Statement asm { .byte$32,$dd lda$ff .byte$32,$00  } always clobbers reg byte a 
Statement [5] *((const byte*) PROCPORT_DDR#0) ← (const byte) PROCPORT_DDR_MEMORY_MASK#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [6] *((const byte*) PROCPORT#0) ← (const byte) PROCPORT_RAM_IO#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [8] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [9] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0|(const byte) DTV_COLORRAM_OFF#0|(const byte) DTV_CHUNKY#0|(const byte) DTV_BADLINE_OFF#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [10] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [11] *((const byte*) VIC_CONTROL2#0) ← (const byte) VIC_MCM#0|(const byte) VIC_CSEL#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [12] *((const byte*) DTV_PLANEB_START_LO#0) ← <(const byte*) CHUNKY#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [13] *((const byte*) DTV_PLANEB_START_MI#0) ← >(const byte*) CHUNKY#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [14] *((const byte*) DTV_PLANEB_START_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [15] *((const byte*) DTV_PLANEB_STEP#0) ← (byte/signed byte/word/signed word/dword/signed dword) 8 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [16] *((const byte*) DTV_PLANEB_MODULO_LO#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [17] *((const byte*) DTV_PLANEB_MODULO_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [18] *((const byte*) CIA2_PORT_A_DDR#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [19] *((const byte*) CIA2_PORT_A#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3^((byte))((word))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [20] *((const byte*) VIC_MEMORY#0) ← ((byte))((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 6|>((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 2 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement asm { ldx#$ff rff: cpxRASTER bnerff stabilize: nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop cpxRASTER beqeat+0 eat: inx cpx#$08 bnestabilize  } always clobbers reg byte x 
Statement [26] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [27] *((const byte*) BORDERCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [28] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 66) goto main::@5 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [31] (byte~) main::$31 ← (byte) main::rst#1 & (byte/signed byte/word/signed word/dword/signed dword) 7 [ main::rst#1 main::$31 ] ( main:2 [ main::rst#1 main::$31 ] ) always clobbers reg byte a 
Statement [32] (byte~) main::$32 ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0 | (byte~) main::$31 [ main::rst#1 main::$32 ] ( main:2 [ main::rst#1 main::$32 ] ) always clobbers reg byte a 
Statement [34] (byte~) main::$33 ← (byte) main::rst#1 << (byte/signed byte/word/signed word/dword/signed dword) 4 [ main::rst#1 main::$33 ] ( main:2 [ main::rst#1 main::$33 ] ) always clobbers reg byte a 
Statement [42] if((byte*) gfx_init_chunky::gfxb#3!=(word/dword/signed dword) 32768) goto gfx_init_chunky::@3 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxb#3 gfx_init_chunky::x#2 gfx_init_chunky::gfxbCpuBank#4 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxb#3 gfx_init_chunky::x#2 gfx_init_chunky::gfxbCpuBank#4 ] ) always clobbers reg byte a 
Statement [47] (word~) gfx_init_chunky::$6 ← (word) gfx_init_chunky::x#2 + (byte) gfx_init_chunky::y#6 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 gfx_init_chunky::$6 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 gfx_init_chunky::$6 ] ) always clobbers reg byte a 
Statement [48] (byte) gfx_init_chunky::c#0 ← ((byte)) (word~) gfx_init_chunky::$6 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 gfx_init_chunky::c#0 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 gfx_init_chunky::c#0 ] ) always clobbers reg byte a 
Statement [49] *((byte*) gfx_init_chunky::gfxb#4) ← (byte) gfx_init_chunky::c#0 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#2 gfx_init_chunky::gfxb#4 ] ) always clobbers reg byte y 
Statement [52] if((word) gfx_init_chunky::x#1!=(word/signed word/dword/signed dword) 320) goto gfx_init_chunky::@2 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxb#1 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#1 ] ( main:2::gfx_init_chunky:7 [ gfx_init_chunky::y#6 gfx_init_chunky::gfxb#1 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::x#1 ] ) always clobbers reg byte a 
Statement asm { .byte$32,$dd lda$ff .byte$32,$00  } always clobbers reg byte a 
Potential registers zp ZP_BYTE:2 [ main::j#2 main::j#1 ] : zp ZP_BYTE:2 , reg byte a , reg byte x , reg byte y , 
Potential registers zp ZP_BYTE:3 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ] : zp ZP_BYTE:3 , reg byte x , 
Potential registers zp ZP_WORD:4 [ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ] : zp ZP_WORD:4 , 
Potential registers zp ZP_BYTE:6 [ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ] : zp ZP_BYTE:6 , reg byte x , 
Potential registers zp ZP_WORD:7 [ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ] : zp ZP_WORD:7 , 
Potential registers zp ZP_BYTE:9 [ dtvSetCpuBankSegment1::cpuBankIdx#3 dtvSetCpuBankSegment1::cpuBankIdx#1 ] : zp ZP_BYTE:9 , reg byte a , reg byte x , reg byte y , 
Potential registers zp ZP_BYTE:10 [ main::rst#1 ] : zp ZP_BYTE:10 , reg byte x , reg byte y , 
Potential registers zp ZP_BYTE:11 [ main::$31 ] : zp ZP_BYTE:11 , reg byte a , reg byte x , reg byte y , 
Potential registers zp ZP_BYTE:12 [ main::$32 ] : zp ZP_BYTE:12 , reg byte a , reg byte x , reg byte y , 
Potential registers zp ZP_BYTE:13 [ main::$33 ] : zp ZP_BYTE:13 , reg byte a , reg byte x , reg byte y , 
Potential registers zp ZP_WORD:14 [ gfx_init_chunky::$6 ] : zp ZP_WORD:14 , 
Potential registers zp ZP_BYTE:16 [ gfx_init_chunky::c#0 ] : zp ZP_BYTE:16 , reg byte a , reg byte x , reg byte y , 

REGISTER UPLIFT SCOPES
Uplift Scope [gfx_init_chunky] 362.64: zp ZP_BYTE:6 [ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ] 297.35: zp ZP_WORD:7 [ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ] 202: zp ZP_WORD:14 [ gfx_init_chunky::$6 ] 202: zp ZP_BYTE:16 [ gfx_init_chunky::c#0 ] 181.8: zp ZP_WORD:4 [ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ] 25.96: zp ZP_BYTE:3 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ] 
Uplift Scope [main] 202: zp ZP_BYTE:11 [ main::$31 ] 202: zp ZP_BYTE:12 [ main::$32 ] 202: zp ZP_BYTE:13 [ main::$33 ] 57.71: zp ZP_BYTE:10 [ main::rst#1 ] 38.5: zp ZP_BYTE:2 [ main::j#2 main::j#1 ] 
Uplift Scope [dtvSetCpuBankSegment1] 305: zp ZP_BYTE:9 [ dtvSetCpuBankSegment1::cpuBankIdx#3 dtvSetCpuBankSegment1::cpuBankIdx#1 ] 
Uplift Scope [] 

Uplifting [gfx_init_chunky] best 25250 combination reg byte x [ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ] zp ZP_WORD:7 [ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ] zp ZP_WORD:14 [ gfx_init_chunky::$6 ] reg byte a [ gfx_init_chunky::c#0 ] zp ZP_WORD:4 [ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ] zp ZP_BYTE:3 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ] 
Uplifting [main] best 22650 combination reg byte a [ main::$31 ] reg byte a [ main::$32 ] reg byte a [ main::$33 ] reg byte x [ main::rst#1 ] zp ZP_BYTE:2 [ main::j#2 main::j#1 ] 
Limited combination testing to 100 combinations of 768 possible.
Uplifting [dtvSetCpuBankSegment1] best 22541 combination reg byte a [ dtvSetCpuBankSegment1::cpuBankIdx#3 dtvSetCpuBankSegment1::cpuBankIdx#1 ] 
Uplifting [] best 22541 combination 
Attempting to uplift remaining variables inzp ZP_BYTE:2 [ main::j#2 main::j#1 ]
Uplifting [main] best 22421 combination reg byte x [ main::j#2 main::j#1 ] 
Attempting to uplift remaining variables inzp ZP_BYTE:3 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
Uplifting [gfx_init_chunky] best 22421 combination zp ZP_BYTE:3 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ] 
Allocated (was zp ZP_BYTE:3) zp ZP_BYTE:2 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
Allocated (was zp ZP_WORD:4) zp ZP_WORD:3 [ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ]
Allocated (was zp ZP_WORD:7) zp ZP_WORD:5 [ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ]
Allocated (was zp ZP_WORD:14) zp ZP_WORD:7 [ gfx_init_chunky::$6 ]

ASSEMBLER BEFORE OPTIMIZATION
//SEG0 File Comments
// C64DTV 8bpp charmode stretcher
//SEG1 Basic Upstart
.pc = $801 "Basic"
:BasicUpstart(bbegin)
.pc = $80d "Program"
//SEG2 Global Constants & labels
  // Processor port data direction register
  .label PROCPORT_DDR = 0
  // Mask for PROCESSOR_PORT_DDR which allows only memory configuration to be written
  .const PROCPORT_DDR_MEMORY_MASK = 7
  // Processor Port Register controlling RAM/ROM configuration and the datasette
  .label PROCPORT = 1
  // RAM in $A000, $E000 I/O in $D000
  .const PROCPORT_RAM_IO = $35
  .label RASTER = $d012
  .label BORDERCOL = $d020
  .label VIC_CONTROL = $d011
  .const VIC_ECM = $40
  .const VIC_DEN = $10
  .const VIC_RSEL = 8
  .label VIC_CONTROL2 = $d016
  .const VIC_MCM = $10
  .const VIC_CSEL = 8
  .label VIC_MEMORY = $d018
  // CIA#2 Port A: Serial bus, RS-232, VIC memory bank
  .label CIA2_PORT_A = $dd00
  // CIA #2 Port A data direction register.
  .label CIA2_PORT_A_DDR = $dd02
  // Feature enables or disables the extra C64 DTV features
  .label DTV_FEATURE = $d03f
  .const DTV_FEATURE_ENABLE = 1
  // Controls the graphics modes of the C64 DTV
  .label DTV_CONTROL = $d03c
  .const DTV_LINEAR = 1
  .const DTV_HIGHCOLOR = 4
  .const DTV_COLORRAM_OFF = $10
  .const DTV_BADLINE_OFF = $20
  .const DTV_CHUNKY = $40
  // Defines colors for the 16 first colors ($00-$0f)
  .label DTV_PALETTE = $d200
  // Linear Graphics Plane B Counter Control
  .label DTV_PLANEB_START_LO = $d049
  .label DTV_PLANEB_START_MI = $d04a
  .label DTV_PLANEB_START_HI = $d04b
  .label DTV_PLANEB_STEP = $d04c
  .label DTV_PLANEB_MODULO_LO = $d047
  .label DTV_PLANEB_MODULO_HI = $d048
  // Plane with all pixels
  .label CHUNKY = $8000
//SEG3 @begin
bbegin:
//SEG4 [1] phi from @begin to @7 [phi:@begin->@7]
b7_from_bbegin:
  jmp b7
//SEG5 @7
b7:
//SEG6 [2] call main 
  jsr main
//SEG7 [3] phi from @7 to @end [phi:@7->@end]
bend_from_b7:
  jmp bend
//SEG8 @end
bend:
//SEG9 main
main: {
  //SEG10 asm { sei  }
    sei
  //SEG11 [5] *((const byte*) PROCPORT_DDR#0) ← (const byte) PROCPORT_DDR_MEMORY_MASK#0 -- _deref_pbuc1=vbuc2 
    // Disable normal interrupt (prevent keyboard reading glitches and allows to hide basic/kernal)
    // Disable kernal & basic
    lda #PROCPORT_DDR_MEMORY_MASK
    sta PROCPORT_DDR
  //SEG12 [6] *((const byte*) PROCPORT#0) ← (const byte) PROCPORT_RAM_IO#0 -- _deref_pbuc1=vbuc2 
    lda #PROCPORT_RAM_IO
    sta PROCPORT
  //SEG13 [7] call gfx_init_chunky 
  //SEG14 [38] phi from main to gfx_init_chunky [phi:main->gfx_init_chunky]
  gfx_init_chunky_from_main:
    jsr gfx_init_chunky
    jmp b17
  //SEG15 main::@17
  b17:
  //SEG16 [8] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 -- _deref_pbuc1=vbuc2 
    // Enable DTV extended modes
    lda #DTV_FEATURE_ENABLE
    sta DTV_FEATURE
  //SEG17 [9] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0|(const byte) DTV_COLORRAM_OFF#0|(const byte) DTV_CHUNKY#0|(const byte) DTV_BADLINE_OFF#0 -- _deref_pbuc1=vbuc2 
    // 8BPP Pixel Cell Mode
    lda #DTV_HIGHCOLOR|DTV_LINEAR|DTV_COLORRAM_OFF|DTV_CHUNKY|DTV_BADLINE_OFF
    sta DTV_CONTROL
  //SEG18 [10] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 -- _deref_pbuc1=vbuc2 
    lda #VIC_DEN|VIC_ECM|VIC_RSEL|3
    sta VIC_CONTROL
  //SEG19 [11] *((const byte*) VIC_CONTROL2#0) ← (const byte) VIC_MCM#0|(const byte) VIC_CSEL#0 -- _deref_pbuc1=vbuc2 
    lda #VIC_MCM|VIC_CSEL
    sta VIC_CONTROL2
  //SEG20 [12] *((const byte*) DTV_PLANEB_START_LO#0) ← <(const byte*) CHUNKY#0 -- _deref_pbuc1=vbuc2 
    // Plane B: CHUNKY
    lda #<CHUNKY
    sta DTV_PLANEB_START_LO
  //SEG21 [13] *((const byte*) DTV_PLANEB_START_MI#0) ← >(const byte*) CHUNKY#0 -- _deref_pbuc1=vbuc2 
    lda #>CHUNKY
    sta DTV_PLANEB_START_MI
  //SEG22 [14] *((const byte*) DTV_PLANEB_START_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta DTV_PLANEB_START_HI
  //SEG23 [15] *((const byte*) DTV_PLANEB_STEP#0) ← (byte/signed byte/word/signed word/dword/signed dword) 8 -- _deref_pbuc1=vbuc2 
    lda #8
    sta DTV_PLANEB_STEP
  //SEG24 [16] *((const byte*) DTV_PLANEB_MODULO_LO#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta DTV_PLANEB_MODULO_LO
  //SEG25 [17] *((const byte*) DTV_PLANEB_MODULO_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta DTV_PLANEB_MODULO_HI
  //SEG26 [18] *((const byte*) CIA2_PORT_A_DDR#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3 -- _deref_pbuc1=vbuc2 
    // VIC Graphics Bank
    lda #3
    sta CIA2_PORT_A_DDR
  //SEG27 [19] *((const byte*) CIA2_PORT_A#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3^((byte))((word))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 -- _deref_pbuc1=vbuc2 
    // Set VIC Bank bits to output - all others to input
    lda #3^CHUNKY/$4000
    sta CIA2_PORT_A
  //SEG28 [20] *((const byte*) VIC_MEMORY#0) ← ((byte))((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 6|>((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 2 -- _deref_pbuc1=vbuc2 
    // Set VIC Bank
    // VIC memory
    lda #(CHUNKY&$3fff)>>6|(0)>>2
    sta VIC_MEMORY
  //SEG29 [21] phi from main::@17 to main::@1 [phi:main::@17->main::@1]
  b1_from_b17:
  //SEG30 [21] phi (byte) main::j#2 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:main::@17->main::@1#0] -- vbuxx=vbuc1 
    ldx #0
    jmp b1
  // DTV Palette - Grey Tones
  //SEG31 [21] phi from main::@1 to main::@1 [phi:main::@1->main::@1]
  b1_from_b1:
  //SEG32 [21] phi (byte) main::j#2 = (byte) main::j#1 [phi:main::@1->main::@1#0] -- register_copy 
    jmp b1
  //SEG33 main::@1
  b1:
  //SEG34 [22] *((const byte*) DTV_PALETTE#0 + (byte) main::j#2) ← (byte) main::j#2 -- pbuc1_derefidx_vbuxx=vbuxx 
    txa
    sta DTV_PALETTE,x
  //SEG35 [23] (byte) main::j#1 ← ++ (byte) main::j#2 -- vbuxx=_inc_vbuxx 
    inx
  //SEG36 [24] if((byte) main::j#1!=(byte/signed byte/word/signed word/dword/signed dword) 16) goto main::@1 -- vbuxx_neq_vbuc1_then_la1 
    cpx #$10
    bne b1_from_b1
    jmp b3
  //SEG37 main::@3
  b3:
  //SEG38 asm { ldx#$ff rff: cpxRASTER bnerff stabilize: nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop cpxRASTER beqeat+0 eat: inx cpx#$08 bnestabilize  }
    // Stabilize Raster
    ldx #$ff
  rff:
    cpx RASTER
    bne rff
  stabilize:
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    cpx RASTER
    beq eat+0
  eat:
    inx
    cpx #8
    bne stabilize
  //SEG39 [26] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 -- _deref_pbuc1=vbuc2 
    lda #VIC_DEN|VIC_ECM|VIC_RSEL|3
    sta VIC_CONTROL
  //SEG40 [27] *((const byte*) BORDERCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta BORDERCOL
    jmp b5
  //SEG41 main::@5
  b5:
  //SEG42 [28] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 66) goto main::@5 -- _deref_pbuc1_neq_vbuc2_then_la1 
    lda RASTER
    cmp #$42
    bne b5
    jmp b7
  //SEG43 main::@7
  b7:
  //SEG44 asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    jmp b8
  //SEG45 main::@8
  b8:
  //SEG46 [30] (byte) main::rst#1 ← *((const byte*) RASTER#0) -- vbuxx=_deref_pbuc1 
    ldx RASTER
  //SEG47 [31] (byte~) main::$31 ← (byte) main::rst#1 & (byte/signed byte/word/signed word/dword/signed dword) 7 -- vbuaa=vbuxx_band_vbuc1 
    txa
    and #7
  //SEG48 [32] (byte~) main::$32 ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0 | (byte~) main::$31 -- vbuaa=vbuc1_bor_vbuaa 
    ora #VIC_DEN|VIC_ECM|VIC_RSEL
  //SEG49 [33] *((const byte*) VIC_CONTROL#0) ← (byte~) main::$32 -- _deref_pbuc1=vbuaa 
    sta VIC_CONTROL
  //SEG50 [34] (byte~) main::$33 ← (byte) main::rst#1 << (byte/signed byte/word/signed word/dword/signed dword) 4 -- vbuaa=vbuxx_rol_4 
    txa
    asl
    asl
    asl
    asl
  //SEG51 [35] *((const byte*) BORDERCOL#0) ← (byte~) main::$33 -- _deref_pbuc1=vbuaa 
    sta BORDERCOL
  //SEG52 asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
  //SEG53 [37] if((byte) main::rst#1!=(byte/word/signed word/dword/signed dword) 242) goto main::@8 -- vbuxx_neq_vbuc1_then_la1 
    cpx #$f2
    bne b8
    jmp b3
}
//SEG54 gfx_init_chunky
// Initialize Plane with 8bpp chunky
gfx_init_chunky: {
    .label _6 = 7
    .label gfxb = 5
    .label x = 3
    .label y = 2
  //SEG55 [39] call dtvSetCpuBankSegment1 
  //SEG56 [58] phi from gfx_init_chunky to dtvSetCpuBankSegment1 [phi:gfx_init_chunky->dtvSetCpuBankSegment1]
  dtvSetCpuBankSegment1_from_gfx_init_chunky:
  //SEG57 [58] phi (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 = ((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky->dtvSetCpuBankSegment1#0] -- vbuaa=vbuc1 
    lda #$ff&CHUNKY/$4000
    jsr dtvSetCpuBankSegment1
  //SEG58 [40] phi from gfx_init_chunky to gfx_init_chunky::@1 [phi:gfx_init_chunky->gfx_init_chunky::@1]
  b1_from_gfx_init_chunky:
  //SEG59 [40] phi (byte) gfx_init_chunky::gfxbCpuBank#7 = ++((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky->gfx_init_chunky::@1#0] -- vbuxx=vbuc1 
    ldx #($ff&CHUNKY/$4000)+1
  //SEG60 [40] phi (byte) gfx_init_chunky::y#6 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:gfx_init_chunky->gfx_init_chunky::@1#1] -- vbuz1=vbuc1 
    lda #0
    sta y
  //SEG61 [40] phi (byte*) gfx_init_chunky::gfxb#5 = ((byte*))(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky->gfx_init_chunky::@1#2] -- pbuz1=pbuc1 
    lda #<$4000
    sta gfxb
    lda #>$4000
    sta gfxb+1
    jmp b1
  //SEG62 [40] phi from gfx_init_chunky::@5 to gfx_init_chunky::@1 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1]
  b1_from_b5:
  //SEG63 [40] phi (byte) gfx_init_chunky::gfxbCpuBank#7 = (byte) gfx_init_chunky::gfxbCpuBank#8 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1#0] -- register_copy 
  //SEG64 [40] phi (byte) gfx_init_chunky::y#6 = (byte) gfx_init_chunky::y#1 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1#1] -- register_copy 
  //SEG65 [40] phi (byte*) gfx_init_chunky::gfxb#5 = (byte*) gfx_init_chunky::gfxb#1 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1#2] -- register_copy 
    jmp b1
  //SEG66 gfx_init_chunky::@1
  b1:
  //SEG67 [41] phi from gfx_init_chunky::@1 to gfx_init_chunky::@2 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2]
  b2_from_b1:
  //SEG68 [41] phi (byte) gfx_init_chunky::gfxbCpuBank#4 = (byte) gfx_init_chunky::gfxbCpuBank#7 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2#0] -- register_copy 
  //SEG69 [41] phi (word) gfx_init_chunky::x#2 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2#1] -- vwuz1=vbuc1 
    lda #<0
    sta x
    lda #>0
    sta x+1
  //SEG70 [41] phi (byte*) gfx_init_chunky::gfxb#3 = (byte*) gfx_init_chunky::gfxb#5 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2#2] -- register_copy 
    jmp b2
  //SEG71 [41] phi from gfx_init_chunky::@3 to gfx_init_chunky::@2 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2]
  b2_from_b3:
  //SEG72 [41] phi (byte) gfx_init_chunky::gfxbCpuBank#4 = (byte) gfx_init_chunky::gfxbCpuBank#8 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2#0] -- register_copy 
  //SEG73 [41] phi (word) gfx_init_chunky::x#2 = (word) gfx_init_chunky::x#1 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2#1] -- register_copy 
  //SEG74 [41] phi (byte*) gfx_init_chunky::gfxb#3 = (byte*) gfx_init_chunky::gfxb#1 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2#2] -- register_copy 
    jmp b2
  //SEG75 gfx_init_chunky::@2
  b2:
  //SEG76 [42] if((byte*) gfx_init_chunky::gfxb#3!=(word/dword/signed dword) 32768) goto gfx_init_chunky::@3 -- pbuz1_neq_vwuc1_then_la1 
    lda gfxb+1
    cmp #>$8000
    bne b3_from_b2
    lda gfxb
    cmp #<$8000
    bne b3_from_b2
    jmp b4
  //SEG77 gfx_init_chunky::@4
  b4:
  //SEG78 [43] (byte) dtvSetCpuBankSegment1::cpuBankIdx#1 ← (byte) gfx_init_chunky::gfxbCpuBank#4 -- vbuaa=vbuxx 
    txa
  //SEG79 [44] call dtvSetCpuBankSegment1 
  //SEG80 [58] phi from gfx_init_chunky::@4 to dtvSetCpuBankSegment1 [phi:gfx_init_chunky::@4->dtvSetCpuBankSegment1]
  dtvSetCpuBankSegment1_from_b4:
  //SEG81 [58] phi (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 = (byte) dtvSetCpuBankSegment1::cpuBankIdx#1 [phi:gfx_init_chunky::@4->dtvSetCpuBankSegment1#0] -- register_copy 
    jsr dtvSetCpuBankSegment1
    jmp b8
  //SEG82 gfx_init_chunky::@8
  b8:
  //SEG83 [45] (byte) gfx_init_chunky::gfxbCpuBank#2 ← ++ (byte) gfx_init_chunky::gfxbCpuBank#4 -- vbuxx=_inc_vbuxx 
    inx
  //SEG84 [46] phi from gfx_init_chunky::@8 to gfx_init_chunky::@3 [phi:gfx_init_chunky::@8->gfx_init_chunky::@3]
  b3_from_b8:
  //SEG85 [46] phi (byte) gfx_init_chunky::gfxbCpuBank#8 = (byte) gfx_init_chunky::gfxbCpuBank#2 [phi:gfx_init_chunky::@8->gfx_init_chunky::@3#0] -- register_copy 
  //SEG86 [46] phi (byte*) gfx_init_chunky::gfxb#4 = ((byte*))(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky::@8->gfx_init_chunky::@3#1] -- pbuz1=pbuc1 
    lda #<$4000
    sta gfxb
    lda #>$4000
    sta gfxb+1
    jmp b3
  //SEG87 [46] phi from gfx_init_chunky::@2 to gfx_init_chunky::@3 [phi:gfx_init_chunky::@2->gfx_init_chunky::@3]
  b3_from_b2:
  //SEG88 [46] phi (byte) gfx_init_chunky::gfxbCpuBank#8 = (byte) gfx_init_chunky::gfxbCpuBank#4 [phi:gfx_init_chunky::@2->gfx_init_chunky::@3#0] -- register_copy 
  //SEG89 [46] phi (byte*) gfx_init_chunky::gfxb#4 = (byte*) gfx_init_chunky::gfxb#3 [phi:gfx_init_chunky::@2->gfx_init_chunky::@3#1] -- register_copy 
    jmp b3
  //SEG90 gfx_init_chunky::@3
  b3:
  //SEG91 [47] (word~) gfx_init_chunky::$6 ← (word) gfx_init_chunky::x#2 + (byte) gfx_init_chunky::y#6 -- vwuz1=vwuz2_plus_vbuz3 
    lda y
    clc
    adc x
    sta _6
    lda #0
    adc x+1
    sta _6+1
  //SEG92 [48] (byte) gfx_init_chunky::c#0 ← ((byte)) (word~) gfx_init_chunky::$6 -- vbuaa=_byte_vwuz1 
    lda _6
  //SEG93 [49] *((byte*) gfx_init_chunky::gfxb#4) ← (byte) gfx_init_chunky::c#0 -- _deref_pbuz1=vbuaa 
    ldy #0
    sta (gfxb),y
  //SEG94 [50] (byte*) gfx_init_chunky::gfxb#1 ← ++ (byte*) gfx_init_chunky::gfxb#4 -- pbuz1=_inc_pbuz1 
    inc gfxb
    bne !+
    inc gfxb+1
  !:
  //SEG95 [51] (word) gfx_init_chunky::x#1 ← ++ (word) gfx_init_chunky::x#2 -- vwuz1=_inc_vwuz1 
    inc x
    bne !+
    inc x+1
  !:
  //SEG96 [52] if((word) gfx_init_chunky::x#1!=(word/signed word/dword/signed dword) 320) goto gfx_init_chunky::@2 -- vwuz1_neq_vwuc1_then_la1 
    lda x+1
    cmp #>$140
    bne b2_from_b3
    lda x
    cmp #<$140
    bne b2_from_b3
    jmp b5
  //SEG97 gfx_init_chunky::@5
  b5:
  //SEG98 [53] (byte) gfx_init_chunky::y#1 ← ++ (byte) gfx_init_chunky::y#6 -- vbuz1=_inc_vbuz1 
    inc y
  //SEG99 [54] if((byte) gfx_init_chunky::y#1!=(byte/signed byte/word/signed word/dword/signed dword) 51) goto gfx_init_chunky::@1 -- vbuz1_neq_vbuc1_then_la1 
    lda y
    cmp #$33
    bne b1_from_b5
  //SEG100 [55] phi from gfx_init_chunky::@5 to gfx_init_chunky::@6 [phi:gfx_init_chunky::@5->gfx_init_chunky::@6]
  b6_from_b5:
    jmp b6
  //SEG101 gfx_init_chunky::@6
  b6:
  //SEG102 [56] call dtvSetCpuBankSegment1 
  //SEG103 [58] phi from gfx_init_chunky::@6 to dtvSetCpuBankSegment1 [phi:gfx_init_chunky::@6->dtvSetCpuBankSegment1]
  dtvSetCpuBankSegment1_from_b6:
  //SEG104 [58] phi (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 = ((byte))(word/signed word/dword/signed dword) 16384/(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky::@6->dtvSetCpuBankSegment1#0] -- vbuaa=vbuc1 
    lda #$4000/$4000
    jsr dtvSetCpuBankSegment1
    jmp breturn
  //SEG105 gfx_init_chunky::@return
  breturn:
  //SEG106 [57] return 
    rts
}
//SEG107 dtvSetCpuBankSegment1
// Set the memory pointed to by CPU BANK 1 SEGMENT ($4000-$7fff)
// This sets which actual memory is addressed when the CPU reads/writes to $4000-$7fff
// The actual memory addressed will be $4000*cpuSegmentIdx
// dtvSetCpuBankSegment1(byte register(A) cpuBankIdx)
dtvSetCpuBankSegment1: {
    // Move CPU BANK 1 SEGMENT ($4000-$7fff)
    .label cpuBank = $ff
  //SEG108 [59] *((const byte*) dtvSetCpuBankSegment1::cpuBank#0) ← (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 -- _deref_pbuc1=vbuaa 
    sta cpuBank
  //SEG109 asm { .byte$32,$dd lda$ff .byte$32,$00  }
    .byte $32, $dd
    lda $ff
    .byte $32, $00
    jmp breturn
  //SEG110 dtvSetCpuBankSegment1::@return
  breturn:
  //SEG111 [61] return 
    rts
}

ASSEMBLER OPTIMIZATIONS
Removing instruction jmp b7
Removing instruction jmp bend
Removing instruction jmp b17
Removing instruction jmp b1
Removing instruction jmp b3
Removing instruction jmp b5
Removing instruction jmp b7
Removing instruction jmp b8
Removing instruction jmp b1
Removing instruction jmp b2
Removing instruction jmp b4
Removing instruction jmp b8
Removing instruction jmp b3
Removing instruction jmp b5
Removing instruction jmp b6
Removing instruction jmp breturn
Removing instruction jmp breturn
Succesful ASM optimization Pass5NextJumpElimination
Removing instruction lda #0
Removing instruction lda #>0
Succesful ASM optimization Pass5UnnecesaryLoadElimination
Replacing label b1_from_b1 with b1
Replacing label b3_from_b2 with b3
Replacing label b3_from_b2 with b3
Replacing label b2_from_b3 with b2
Replacing label b2_from_b3 with b2
Replacing label b1_from_b5 with b1
Removing instruction b7_from_bbegin:
Removing instruction b7:
Removing instruction bend_from_b7:
Removing instruction b1_from_b1:
Removing instruction b1_from_b5:
Removing instruction b2_from_b1:
Removing instruction b2_from_b3:
Removing instruction b3_from_b2:
Removing instruction b6_from_b5:
Removing instruction dtvSetCpuBankSegment1_from_b6:
Succesful ASM optimization Pass5RedundantLabelElimination
Removing instruction bend:
Removing instruction gfx_init_chunky_from_main:
Removing instruction b17:
Removing instruction b1_from_b17:
Removing instruction b7:
Removing instruction dtvSetCpuBankSegment1_from_gfx_init_chunky:
Removing instruction b1_from_gfx_init_chunky:
Removing instruction b4:
Removing instruction dtvSetCpuBankSegment1_from_b4:
Removing instruction b8:
Removing instruction b3_from_b8:
Removing instruction b5:
Removing instruction b6:
Removing instruction breturn:
Removing instruction breturn:
Succesful ASM optimization Pass5UnusedLabelElimination
Updating BasicUpstart to call main directly
Removing instruction jsr main
Succesful ASM optimization Pass5SkipBegin
Removing instruction jmp b1
Removing instruction jmp b1
Removing instruction jmp b2
Removing instruction jmp b3
Succesful ASM optimization Pass5NextJumpElimination
Removing instruction bbegin:
Succesful ASM optimization Pass5UnusedLabelElimination

FINAL SYMBOL TABLE
(label) @7
(label) @begin
(label) @end
(byte*) BGCOL
(byte*) BGCOL1
(byte*) BGCOL2
(byte*) BGCOL3
(byte*) BGCOL4
(byte) BLACK
(byte) BLUE
(byte*) BORDERCOL
(const byte*) BORDERCOL#0 BORDERCOL = ((byte*))(word/dword/signed dword) 53280
(byte) BROWN
(byte*) CHARGEN
(byte*) CHUNKY
(const byte*) CHUNKY#0 CHUNKY = ((byte*))(word/dword/signed dword) 32768
(byte*) CIA1_INTERRUPT
(byte*) CIA1_PORT_A
(byte*) CIA1_PORT_A_DDR
(byte*) CIA1_PORT_B
(byte*) CIA1_PORT_B_DDR
(byte*) CIA2_INTERRUPT
(byte*) CIA2_PORT_A
(const byte*) CIA2_PORT_A#0 CIA2_PORT_A = ((byte*))(word/dword/signed dword) 56576
(byte*) CIA2_PORT_A_DDR
(const byte*) CIA2_PORT_A_DDR#0 CIA2_PORT_A_DDR = ((byte*))(word/dword/signed dword) 56578
(byte*) CIA2_PORT_B
(byte*) CIA2_PORT_B_DDR
(byte) CIA_INTERRUPT_CLEAR
(byte*) COLS
(byte) CYAN
(byte*) D011
(byte*) D016
(byte*) D018
(byte) DARK_GREY
(byte) DTV_BADLINE_OFF
(const byte) DTV_BADLINE_OFF#0 DTV_BADLINE_OFF = (byte/signed byte/word/signed word/dword/signed dword) 32
(byte*) DTV_BLITTER_ALU
(byte*) DTV_BLITTER_CONTROL
(byte*) DTV_BLITTER_CONTROL2
(byte*) DTV_BLITTER_DEST_HI
(byte*) DTV_BLITTER_DEST_LIN_HI
(byte*) DTV_BLITTER_DEST_LIN_LO
(byte*) DTV_BLITTER_DEST_LO
(byte*) DTV_BLITTER_DEST_MI
(byte*) DTV_BLITTER_DEST_MOD_HI
(byte*) DTV_BLITTER_DEST_MOD_LO
(byte*) DTV_BLITTER_DEST_STEP
(byte*) DTV_BLITTER_LEN_HI
(byte*) DTV_BLITTER_LEN_LO
(byte*) DTV_BLITTER_SRCA_HI
(byte*) DTV_BLITTER_SRCA_LIN_HI
(byte*) DTV_BLITTER_SRCA_LIN_LO
(byte*) DTV_BLITTER_SRCA_LO
(byte*) DTV_BLITTER_SRCA_MI
(byte*) DTV_BLITTER_SRCA_MOD_HI
(byte*) DTV_BLITTER_SRCA_MOD_LO
(byte*) DTV_BLITTER_SRCA_STEP
(byte*) DTV_BLITTER_SRCB_HI
(byte*) DTV_BLITTER_SRCB_LIN_HI
(byte*) DTV_BLITTER_SRCB_LIN_LO
(byte*) DTV_BLITTER_SRCB_LO
(byte*) DTV_BLITTER_SRCB_MI
(byte*) DTV_BLITTER_SRCB_MOD_HI
(byte*) DTV_BLITTER_SRCB_MOD_LO
(byte*) DTV_BLITTER_SRCB_STEP
(byte*) DTV_BLITTER_TRANSPARANCY
(byte) DTV_BLIT_ADD
(byte) DTV_BLIT_AND
(byte) DTV_BLIT_CIA_IRQ
(byte) DTV_BLIT_CLEAR_IRQ
(byte) DTV_BLIT_DEST_CONT
(byte) DTV_BLIT_DEST_FWD
(byte) DTV_BLIT_DISABLE_B
(byte) DTV_BLIT_FORCE_START
(byte) DTV_BLIT_IRQ_EN
(byte) DTV_BLIT_NAND
(byte) DTV_BLIT_NOR
(byte) DTV_BLIT_OR
(byte) DTV_BLIT_SHIFT0
(byte) DTV_BLIT_SHIFT1
(byte) DTV_BLIT_SHIFT2
(byte) DTV_BLIT_SHIFT3
(byte) DTV_BLIT_SHIFT4
(byte) DTV_BLIT_SHIFT5
(byte) DTV_BLIT_SHIFT6
(byte) DTV_BLIT_SHIFT7
(byte) DTV_BLIT_SRCA_CONT
(byte) DTV_BLIT_SRCA_FWD
(byte) DTV_BLIT_SRCB_CONT
(byte) DTV_BLIT_SRCB_FWD
(byte) DTV_BLIT_STATUS_BUSY
(byte) DTV_BLIT_STATUS_IRQ
(byte) DTV_BLIT_SUB
(byte) DTV_BLIT_TRANSPARANCY_NONE
(byte) DTV_BLIT_VBLANK
(byte) DTV_BLIT_VIC_IRQ
(byte) DTV_BLIT_WRITE_NONTRANSPARENT
(byte) DTV_BLIT_WRITE_TRANSPARENT
(byte) DTV_BLIT_XNOR
(byte) DTV_BLIT_XOR
(byte) DTV_BORDER_OFF
(byte) DTV_CHUNKY
(const byte) DTV_CHUNKY#0 DTV_CHUNKY = (byte/signed byte/word/signed word/dword/signed dword) 64
(byte) DTV_COLORRAM_OFF
(const byte) DTV_COLORRAM_OFF#0 DTV_COLORRAM_OFF = (byte/signed byte/word/signed word/dword/signed dword) 16
(dword) DTV_COLOR_BANK_DEFAULT
(byte*) DTV_COLOR_BANK_HI
(byte*) DTV_COLOR_BANK_LO
(byte*) DTV_CONTROL
(const byte*) DTV_CONTROL#0 DTV_CONTROL = ((byte*))(word/dword/signed dword) 53308
(byte*) DTV_FEATURE
(const byte*) DTV_FEATURE#0 DTV_FEATURE = ((byte*))(word/dword/signed dword) 53311
(byte) DTV_FEATURE_DISABLE_TIL_RESET
(byte) DTV_FEATURE_ENABLE
(const byte) DTV_FEATURE_ENABLE#0 DTV_FEATURE_ENABLE = (byte/signed byte/word/signed word/dword/signed dword) 1
(byte*) DTV_GRAPHICS_HICOL_BANK
(byte*) DTV_GRAPHICS_VIC_BANK
(byte) DTV_HIGHCOLOR
(const byte) DTV_HIGHCOLOR#0 DTV_HIGHCOLOR = (byte/signed byte/word/signed word/dword/signed dword) 4
(byte) DTV_LINEAR
(const byte) DTV_LINEAR#0 DTV_LINEAR = (byte/signed byte/word/signed word/dword/signed dword) 1
(byte) DTV_OVERSCAN
(byte*) DTV_PALETTE
(const byte*) DTV_PALETTE#0 DTV_PALETTE = ((byte*))(word/dword/signed dword) 53760
(byte[16]) DTV_PALETTE_DEFAULT
(byte*) DTV_PLANEA_MODULO_HI
(byte*) DTV_PLANEA_MODULO_LO
(byte*) DTV_PLANEA_START_HI
(byte*) DTV_PLANEA_START_LO
(byte*) DTV_PLANEA_START_MI
(byte*) DTV_PLANEA_STEP
(byte*) DTV_PLANEB_MODULO_HI
(const byte*) DTV_PLANEB_MODULO_HI#0 DTV_PLANEB_MODULO_HI = ((byte*))(word/dword/signed dword) 53320
(byte*) DTV_PLANEB_MODULO_LO
(const byte*) DTV_PLANEB_MODULO_LO#0 DTV_PLANEB_MODULO_LO = ((byte*))(word/dword/signed dword) 53319
(byte*) DTV_PLANEB_START_HI
(const byte*) DTV_PLANEB_START_HI#0 DTV_PLANEB_START_HI = ((byte*))(word/dword/signed dword) 53323
(byte*) DTV_PLANEB_START_LO
(const byte*) DTV_PLANEB_START_LO#0 DTV_PLANEB_START_LO = ((byte*))(word/dword/signed dword) 53321
(byte*) DTV_PLANEB_START_MI
(const byte*) DTV_PLANEB_START_MI#0 DTV_PLANEB_START_MI = ((byte*))(word/dword/signed dword) 53322
(byte*) DTV_PLANEB_STEP
(const byte*) DTV_PLANEB_STEP#0 DTV_PLANEB_STEP = ((byte*))(word/dword/signed dword) 53324
(byte*) DTV_SPRITE_BANK
(byte) GREEN
(byte) GREY
(void()**) HARDWARE_IRQ
(byte) IRQ_COLLISION_BG
(byte) IRQ_COLLISION_SPRITE
(byte*) IRQ_ENABLE
(byte) IRQ_LIGHTPEN
(byte) IRQ_RASTER
(byte*) IRQ_STATUS
(void()**) KERNEL_IRQ
(byte*) LIGHTPEN_X
(byte*) LIGHTPEN_Y
(byte) LIGHT_BLUE
(byte) LIGHT_GREEN
(byte) LIGHT_GREY
(byte) ORANGE
(byte) PINK
(byte*) PROCPORT
(const byte*) PROCPORT#0 PROCPORT = ((byte*))(byte/signed byte/word/signed word/dword/signed dword) 1
(byte) PROCPORT_BASIC_KERNEL_IO
(byte*) PROCPORT_DDR
(const byte*) PROCPORT_DDR#0 PROCPORT_DDR = ((byte*))(byte/signed byte/word/signed word/dword/signed dword) 0
(byte) PROCPORT_DDR_MEMORY_MASK
(const byte) PROCPORT_DDR_MEMORY_MASK#0 PROCPORT_DDR_MEMORY_MASK = (byte/signed byte/word/signed word/dword/signed dword) 7
(byte) PROCPORT_KERNEL_IO
(byte) PROCPORT_RAM_ALL
(byte) PROCPORT_RAM_CHARROM
(byte) PROCPORT_RAM_IO
(const byte) PROCPORT_RAM_IO#0 PROCPORT_RAM_IO = (byte/signed byte/word/signed word/dword/signed dword) 53
(byte) PURPLE
(byte*) RASTER
(const byte*) RASTER#0 RASTER = ((byte*))(word/dword/signed dword) 53266
(byte) RED
(byte*) SPRITES_COLS
(byte*) SPRITES_ENABLE
(byte*) SPRITES_EXPAND_X
(byte*) SPRITES_EXPAND_Y
(byte*) SPRITES_MC
(byte*) SPRITES_MC1
(byte*) SPRITES_MC2
(byte*) SPRITES_PRIORITY
(byte*) SPRITES_XMSB
(byte*) SPRITES_XPOS
(byte*) SPRITES_YPOS
(word) SPRITE_PTRS
(byte) VIC_BMM
(byte*) VIC_CONTROL
(const byte*) VIC_CONTROL#0 VIC_CONTROL = ((byte*))(word/dword/signed dword) 53265
(byte*) VIC_CONTROL2
(const byte*) VIC_CONTROL2#0 VIC_CONTROL2 = ((byte*))(word/dword/signed dword) 53270
(byte) VIC_CSEL
(const byte) VIC_CSEL#0 VIC_CSEL = (byte/signed byte/word/signed word/dword/signed dword) 8
(byte) VIC_DEN
(const byte) VIC_DEN#0 VIC_DEN = (byte/signed byte/word/signed word/dword/signed dword) 16
(byte) VIC_ECM
(const byte) VIC_ECM#0 VIC_ECM = (byte/signed byte/word/signed word/dword/signed dword) 64
(byte) VIC_MCM
(const byte) VIC_MCM#0 VIC_MCM = (byte/signed byte/word/signed word/dword/signed dword) 16
(byte*) VIC_MEMORY
(const byte*) VIC_MEMORY#0 VIC_MEMORY = ((byte*))(word/dword/signed dword) 53272
(byte) VIC_RSEL
(const byte) VIC_RSEL#0 VIC_RSEL = (byte/signed byte/word/signed word/dword/signed dword) 8
(byte) VIC_RST8
(byte) WHITE
(byte) YELLOW
(void()) dtvSetCpuBankSegment1((byte) dtvSetCpuBankSegment1::cpuBankIdx)
(label) dtvSetCpuBankSegment1::@return
(byte*) dtvSetCpuBankSegment1::cpuBank
(const byte*) dtvSetCpuBankSegment1::cpuBank#0 cpuBank = ((byte*))(byte/word/signed word/dword/signed dword) 255
(byte) dtvSetCpuBankSegment1::cpuBankIdx
(byte) dtvSetCpuBankSegment1::cpuBankIdx#1 reg byte a 202.0
(byte) dtvSetCpuBankSegment1::cpuBankIdx#3 reg byte a 103.0
(void()) gfx_init_chunky()
(word~) gfx_init_chunky::$6 $6 zp ZP_WORD:7 202.0
(label) gfx_init_chunky::@1
(label) gfx_init_chunky::@2
(label) gfx_init_chunky::@3
(label) gfx_init_chunky::@4
(label) gfx_init_chunky::@5
(label) gfx_init_chunky::@6
(label) gfx_init_chunky::@8
(label) gfx_init_chunky::@return
(byte) gfx_init_chunky::c
(byte) gfx_init_chunky::c#0 reg byte a 202.0
(byte*) gfx_init_chunky::gfxb
(byte*) gfx_init_chunky::gfxb#1 gfxb zp ZP_WORD:5 42.599999999999994
(byte*) gfx_init_chunky::gfxb#3 gfxb zp ZP_WORD:5 157.0
(byte*) gfx_init_chunky::gfxb#4 gfxb zp ZP_WORD:5 75.75
(byte*) gfx_init_chunky::gfxb#5 gfxb zp ZP_WORD:5 22.0
(byte) gfx_init_chunky::gfxbCpuBank
(byte) gfx_init_chunky::gfxbCpuBank#2 reg byte x 202.0
(byte) gfx_init_chunky::gfxbCpuBank#4 reg byte x 103.75
(byte) gfx_init_chunky::gfxbCpuBank#7 reg byte x 22.0
(byte) gfx_init_chunky::gfxbCpuBank#8 reg byte x 34.888888888888886
(word) gfx_init_chunky::x
(word) gfx_init_chunky::x#1 x zp ZP_WORD:3 151.5
(word) gfx_init_chunky::x#2 x zp ZP_WORD:3 30.299999999999997
(byte) gfx_init_chunky::y
(byte) gfx_init_chunky::y#1 y zp ZP_BYTE:2 16.5
(byte) gfx_init_chunky::y#6 y zp ZP_BYTE:2 9.461538461538462
(void()) main()
(byte~) main::$31 reg byte a 202.0
(byte~) main::$32 reg byte a 202.0
(byte~) main::$33 reg byte a 202.0
(label) main::@1
(label) main::@17
(label) main::@3
(label) main::@5
(label) main::@7
(label) main::@8
(byte) main::j
(byte) main::j#1 reg byte x 16.5
(byte) main::j#2 reg byte x 22.0
(byte) main::rst
(byte) main::rst#1 reg byte x 57.714285714285715

reg byte x [ main::j#2 main::j#1 ]
zp ZP_BYTE:2 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
zp ZP_WORD:3 [ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ]
reg byte x [ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ]
zp ZP_WORD:5 [ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ]
reg byte a [ dtvSetCpuBankSegment1::cpuBankIdx#3 dtvSetCpuBankSegment1::cpuBankIdx#1 ]
reg byte x [ main::rst#1 ]
reg byte a [ main::$31 ]
reg byte a [ main::$32 ]
reg byte a [ main::$33 ]
zp ZP_WORD:7 [ gfx_init_chunky::$6 ]
reg byte a [ gfx_init_chunky::c#0 ]


FINAL ASSEMBLER
Score: 19882

//SEG0 File Comments
// C64DTV 8bpp charmode stretcher
//SEG1 Basic Upstart
.pc = $801 "Basic"
:BasicUpstart(main)
.pc = $80d "Program"
//SEG2 Global Constants & labels
  // Processor port data direction register
  .label PROCPORT_DDR = 0
  // Mask for PROCESSOR_PORT_DDR which allows only memory configuration to be written
  .const PROCPORT_DDR_MEMORY_MASK = 7
  // Processor Port Register controlling RAM/ROM configuration and the datasette
  .label PROCPORT = 1
  // RAM in $A000, $E000 I/O in $D000
  .const PROCPORT_RAM_IO = $35
  .label RASTER = $d012
  .label BORDERCOL = $d020
  .label VIC_CONTROL = $d011
  .const VIC_ECM = $40
  .const VIC_DEN = $10
  .const VIC_RSEL = 8
  .label VIC_CONTROL2 = $d016
  .const VIC_MCM = $10
  .const VIC_CSEL = 8
  .label VIC_MEMORY = $d018
  // CIA#2 Port A: Serial bus, RS-232, VIC memory bank
  .label CIA2_PORT_A = $dd00
  // CIA #2 Port A data direction register.
  .label CIA2_PORT_A_DDR = $dd02
  // Feature enables or disables the extra C64 DTV features
  .label DTV_FEATURE = $d03f
  .const DTV_FEATURE_ENABLE = 1
  // Controls the graphics modes of the C64 DTV
  .label DTV_CONTROL = $d03c
  .const DTV_LINEAR = 1
  .const DTV_HIGHCOLOR = 4
  .const DTV_COLORRAM_OFF = $10
  .const DTV_BADLINE_OFF = $20
  .const DTV_CHUNKY = $40
  // Defines colors for the 16 first colors ($00-$0f)
  .label DTV_PALETTE = $d200
  // Linear Graphics Plane B Counter Control
  .label DTV_PLANEB_START_LO = $d049
  .label DTV_PLANEB_START_MI = $d04a
  .label DTV_PLANEB_START_HI = $d04b
  .label DTV_PLANEB_STEP = $d04c
  .label DTV_PLANEB_MODULO_LO = $d047
  .label DTV_PLANEB_MODULO_HI = $d048
  // Plane with all pixels
  .label CHUNKY = $8000
//SEG3 @begin
//SEG4 [1] phi from @begin to @7 [phi:@begin->@7]
//SEG5 @7
//SEG6 [2] call main 
//SEG7 [3] phi from @7 to @end [phi:@7->@end]
//SEG8 @end
//SEG9 main
main: {
  //SEG10 asm { sei  }
    sei
  //SEG11 [5] *((const byte*) PROCPORT_DDR#0) ← (const byte) PROCPORT_DDR_MEMORY_MASK#0 -- _deref_pbuc1=vbuc2 
    // Disable normal interrupt (prevent keyboard reading glitches and allows to hide basic/kernal)
    // Disable kernal & basic
    lda #PROCPORT_DDR_MEMORY_MASK
    sta PROCPORT_DDR
  //SEG12 [6] *((const byte*) PROCPORT#0) ← (const byte) PROCPORT_RAM_IO#0 -- _deref_pbuc1=vbuc2 
    lda #PROCPORT_RAM_IO
    sta PROCPORT
  //SEG13 [7] call gfx_init_chunky 
  //SEG14 [38] phi from main to gfx_init_chunky [phi:main->gfx_init_chunky]
    jsr gfx_init_chunky
  //SEG15 main::@17
  //SEG16 [8] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 -- _deref_pbuc1=vbuc2 
    // Enable DTV extended modes
    lda #DTV_FEATURE_ENABLE
    sta DTV_FEATURE
  //SEG17 [9] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_LINEAR#0|(const byte) DTV_COLORRAM_OFF#0|(const byte) DTV_CHUNKY#0|(const byte) DTV_BADLINE_OFF#0 -- _deref_pbuc1=vbuc2 
    // 8BPP Pixel Cell Mode
    lda #DTV_HIGHCOLOR|DTV_LINEAR|DTV_COLORRAM_OFF|DTV_CHUNKY|DTV_BADLINE_OFF
    sta DTV_CONTROL
  //SEG18 [10] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 -- _deref_pbuc1=vbuc2 
    lda #VIC_DEN|VIC_ECM|VIC_RSEL|3
    sta VIC_CONTROL
  //SEG19 [11] *((const byte*) VIC_CONTROL2#0) ← (const byte) VIC_MCM#0|(const byte) VIC_CSEL#0 -- _deref_pbuc1=vbuc2 
    lda #VIC_MCM|VIC_CSEL
    sta VIC_CONTROL2
  //SEG20 [12] *((const byte*) DTV_PLANEB_START_LO#0) ← <(const byte*) CHUNKY#0 -- _deref_pbuc1=vbuc2 
    // Plane B: CHUNKY
    lda #<CHUNKY
    sta DTV_PLANEB_START_LO
  //SEG21 [13] *((const byte*) DTV_PLANEB_START_MI#0) ← >(const byte*) CHUNKY#0 -- _deref_pbuc1=vbuc2 
    lda #>CHUNKY
    sta DTV_PLANEB_START_MI
  //SEG22 [14] *((const byte*) DTV_PLANEB_START_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta DTV_PLANEB_START_HI
  //SEG23 [15] *((const byte*) DTV_PLANEB_STEP#0) ← (byte/signed byte/word/signed word/dword/signed dword) 8 -- _deref_pbuc1=vbuc2 
    lda #8
    sta DTV_PLANEB_STEP
  //SEG24 [16] *((const byte*) DTV_PLANEB_MODULO_LO#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta DTV_PLANEB_MODULO_LO
  //SEG25 [17] *((const byte*) DTV_PLANEB_MODULO_HI#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    sta DTV_PLANEB_MODULO_HI
  //SEG26 [18] *((const byte*) CIA2_PORT_A_DDR#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3 -- _deref_pbuc1=vbuc2 
    // VIC Graphics Bank
    lda #3
    sta CIA2_PORT_A_DDR
  //SEG27 [19] *((const byte*) CIA2_PORT_A#0) ← (byte/signed byte/word/signed word/dword/signed dword) 3^((byte))((word))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 -- _deref_pbuc1=vbuc2 
    // Set VIC Bank bits to output - all others to input
    lda #3^CHUNKY/$4000
    sta CIA2_PORT_A
  //SEG28 [20] *((const byte*) VIC_MEMORY#0) ← ((byte))((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 6|>((word))(const byte*) CHUNKY#0&(word/signed word/dword/signed dword) 16383>>(byte/signed byte/word/signed word/dword/signed dword) 2 -- _deref_pbuc1=vbuc2 
    // Set VIC Bank
    // VIC memory
    lda #(CHUNKY&$3fff)>>6|(0)>>2
    sta VIC_MEMORY
  //SEG29 [21] phi from main::@17 to main::@1 [phi:main::@17->main::@1]
  //SEG30 [21] phi (byte) main::j#2 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:main::@17->main::@1#0] -- vbuxx=vbuc1 
    ldx #0
  // DTV Palette - Grey Tones
  //SEG31 [21] phi from main::@1 to main::@1 [phi:main::@1->main::@1]
  //SEG32 [21] phi (byte) main::j#2 = (byte) main::j#1 [phi:main::@1->main::@1#0] -- register_copy 
  //SEG33 main::@1
  b1:
  //SEG34 [22] *((const byte*) DTV_PALETTE#0 + (byte) main::j#2) ← (byte) main::j#2 -- pbuc1_derefidx_vbuxx=vbuxx 
    txa
    sta DTV_PALETTE,x
  //SEG35 [23] (byte) main::j#1 ← ++ (byte) main::j#2 -- vbuxx=_inc_vbuxx 
    inx
  //SEG36 [24] if((byte) main::j#1!=(byte/signed byte/word/signed word/dword/signed dword) 16) goto main::@1 -- vbuxx_neq_vbuc1_then_la1 
    cpx #$10
    bne b1
  //SEG37 main::@3
  b3:
  //SEG38 asm { ldx#$ff rff: cpxRASTER bnerff stabilize: nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop cpxRASTER beqeat+0 eat: inx cpx#$08 bnestabilize  }
    // Stabilize Raster
    ldx #$ff
  rff:
    cpx RASTER
    bne rff
  stabilize:
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    cpx RASTER
    beq eat+0
  eat:
    inx
    cpx #8
    bne stabilize
  //SEG39 [26] *((const byte*) VIC_CONTROL#0) ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0|(byte/signed byte/word/signed word/dword/signed dword) 3 -- _deref_pbuc1=vbuc2 
    lda #VIC_DEN|VIC_ECM|VIC_RSEL|3
    sta VIC_CONTROL
  //SEG40 [27] *((const byte*) BORDERCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    lda #0
    sta BORDERCOL
  //SEG41 main::@5
  b5:
  //SEG42 [28] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 66) goto main::@5 -- _deref_pbuc1_neq_vbuc2_then_la1 
    lda RASTER
    cmp #$42
    bne b5
  //SEG43 main::@7
  //SEG44 asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
  //SEG45 main::@8
  b8:
  //SEG46 [30] (byte) main::rst#1 ← *((const byte*) RASTER#0) -- vbuxx=_deref_pbuc1 
    ldx RASTER
  //SEG47 [31] (byte~) main::$31 ← (byte) main::rst#1 & (byte/signed byte/word/signed word/dword/signed dword) 7 -- vbuaa=vbuxx_band_vbuc1 
    txa
    and #7
  //SEG48 [32] (byte~) main::$32 ← (const byte) VIC_DEN#0|(const byte) VIC_ECM#0|(const byte) VIC_RSEL#0 | (byte~) main::$31 -- vbuaa=vbuc1_bor_vbuaa 
    ora #VIC_DEN|VIC_ECM|VIC_RSEL
  //SEG49 [33] *((const byte*) VIC_CONTROL#0) ← (byte~) main::$32 -- _deref_pbuc1=vbuaa 
    sta VIC_CONTROL
  //SEG50 [34] (byte~) main::$33 ← (byte) main::rst#1 << (byte/signed byte/word/signed word/dword/signed dword) 4 -- vbuaa=vbuxx_rol_4 
    txa
    asl
    asl
    asl
    asl
  //SEG51 [35] *((const byte*) BORDERCOL#0) ← (byte~) main::$33 -- _deref_pbuc1=vbuaa 
    sta BORDERCOL
  //SEG52 asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
  //SEG53 [37] if((byte) main::rst#1!=(byte/word/signed word/dword/signed dword) 242) goto main::@8 -- vbuxx_neq_vbuc1_then_la1 
    cpx #$f2
    bne b8
    jmp b3
}
//SEG54 gfx_init_chunky
// Initialize Plane with 8bpp chunky
gfx_init_chunky: {
    .label _6 = 7
    .label gfxb = 5
    .label x = 3
    .label y = 2
  //SEG55 [39] call dtvSetCpuBankSegment1 
  //SEG56 [58] phi from gfx_init_chunky to dtvSetCpuBankSegment1 [phi:gfx_init_chunky->dtvSetCpuBankSegment1]
  //SEG57 [58] phi (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 = ((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky->dtvSetCpuBankSegment1#0] -- vbuaa=vbuc1 
    lda #$ff&CHUNKY/$4000
    jsr dtvSetCpuBankSegment1
  //SEG58 [40] phi from gfx_init_chunky to gfx_init_chunky::@1 [phi:gfx_init_chunky->gfx_init_chunky::@1]
  //SEG59 [40] phi (byte) gfx_init_chunky::gfxbCpuBank#7 = ++((byte))(const byte*) CHUNKY#0/(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky->gfx_init_chunky::@1#0] -- vbuxx=vbuc1 
    ldx #($ff&CHUNKY/$4000)+1
  //SEG60 [40] phi (byte) gfx_init_chunky::y#6 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:gfx_init_chunky->gfx_init_chunky::@1#1] -- vbuz1=vbuc1 
    lda #0
    sta y
  //SEG61 [40] phi (byte*) gfx_init_chunky::gfxb#5 = ((byte*))(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky->gfx_init_chunky::@1#2] -- pbuz1=pbuc1 
    lda #<$4000
    sta gfxb
    lda #>$4000
    sta gfxb+1
  //SEG62 [40] phi from gfx_init_chunky::@5 to gfx_init_chunky::@1 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1]
  //SEG63 [40] phi (byte) gfx_init_chunky::gfxbCpuBank#7 = (byte) gfx_init_chunky::gfxbCpuBank#8 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1#0] -- register_copy 
  //SEG64 [40] phi (byte) gfx_init_chunky::y#6 = (byte) gfx_init_chunky::y#1 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1#1] -- register_copy 
  //SEG65 [40] phi (byte*) gfx_init_chunky::gfxb#5 = (byte*) gfx_init_chunky::gfxb#1 [phi:gfx_init_chunky::@5->gfx_init_chunky::@1#2] -- register_copy 
  //SEG66 gfx_init_chunky::@1
  b1:
  //SEG67 [41] phi from gfx_init_chunky::@1 to gfx_init_chunky::@2 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2]
  //SEG68 [41] phi (byte) gfx_init_chunky::gfxbCpuBank#4 = (byte) gfx_init_chunky::gfxbCpuBank#7 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2#0] -- register_copy 
  //SEG69 [41] phi (word) gfx_init_chunky::x#2 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2#1] -- vwuz1=vbuc1 
    lda #<0
    sta x
    sta x+1
  //SEG70 [41] phi (byte*) gfx_init_chunky::gfxb#3 = (byte*) gfx_init_chunky::gfxb#5 [phi:gfx_init_chunky::@1->gfx_init_chunky::@2#2] -- register_copy 
  //SEG71 [41] phi from gfx_init_chunky::@3 to gfx_init_chunky::@2 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2]
  //SEG72 [41] phi (byte) gfx_init_chunky::gfxbCpuBank#4 = (byte) gfx_init_chunky::gfxbCpuBank#8 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2#0] -- register_copy 
  //SEG73 [41] phi (word) gfx_init_chunky::x#2 = (word) gfx_init_chunky::x#1 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2#1] -- register_copy 
  //SEG74 [41] phi (byte*) gfx_init_chunky::gfxb#3 = (byte*) gfx_init_chunky::gfxb#1 [phi:gfx_init_chunky::@3->gfx_init_chunky::@2#2] -- register_copy 
  //SEG75 gfx_init_chunky::@2
  b2:
  //SEG76 [42] if((byte*) gfx_init_chunky::gfxb#3!=(word/dword/signed dword) 32768) goto gfx_init_chunky::@3 -- pbuz1_neq_vwuc1_then_la1 
    lda gfxb+1
    cmp #>$8000
    bne b3
    lda gfxb
    cmp #<$8000
    bne b3
  //SEG77 gfx_init_chunky::@4
  //SEG78 [43] (byte) dtvSetCpuBankSegment1::cpuBankIdx#1 ← (byte) gfx_init_chunky::gfxbCpuBank#4 -- vbuaa=vbuxx 
    txa
  //SEG79 [44] call dtvSetCpuBankSegment1 
  //SEG80 [58] phi from gfx_init_chunky::@4 to dtvSetCpuBankSegment1 [phi:gfx_init_chunky::@4->dtvSetCpuBankSegment1]
  //SEG81 [58] phi (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 = (byte) dtvSetCpuBankSegment1::cpuBankIdx#1 [phi:gfx_init_chunky::@4->dtvSetCpuBankSegment1#0] -- register_copy 
    jsr dtvSetCpuBankSegment1
  //SEG82 gfx_init_chunky::@8
  //SEG83 [45] (byte) gfx_init_chunky::gfxbCpuBank#2 ← ++ (byte) gfx_init_chunky::gfxbCpuBank#4 -- vbuxx=_inc_vbuxx 
    inx
  //SEG84 [46] phi from gfx_init_chunky::@8 to gfx_init_chunky::@3 [phi:gfx_init_chunky::@8->gfx_init_chunky::@3]
  //SEG85 [46] phi (byte) gfx_init_chunky::gfxbCpuBank#8 = (byte) gfx_init_chunky::gfxbCpuBank#2 [phi:gfx_init_chunky::@8->gfx_init_chunky::@3#0] -- register_copy 
  //SEG86 [46] phi (byte*) gfx_init_chunky::gfxb#4 = ((byte*))(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky::@8->gfx_init_chunky::@3#1] -- pbuz1=pbuc1 
    lda #<$4000
    sta gfxb
    lda #>$4000
    sta gfxb+1
  //SEG87 [46] phi from gfx_init_chunky::@2 to gfx_init_chunky::@3 [phi:gfx_init_chunky::@2->gfx_init_chunky::@3]
  //SEG88 [46] phi (byte) gfx_init_chunky::gfxbCpuBank#8 = (byte) gfx_init_chunky::gfxbCpuBank#4 [phi:gfx_init_chunky::@2->gfx_init_chunky::@3#0] -- register_copy 
  //SEG89 [46] phi (byte*) gfx_init_chunky::gfxb#4 = (byte*) gfx_init_chunky::gfxb#3 [phi:gfx_init_chunky::@2->gfx_init_chunky::@3#1] -- register_copy 
  //SEG90 gfx_init_chunky::@3
  b3:
  //SEG91 [47] (word~) gfx_init_chunky::$6 ← (word) gfx_init_chunky::x#2 + (byte) gfx_init_chunky::y#6 -- vwuz1=vwuz2_plus_vbuz3 
    lda y
    clc
    adc x
    sta _6
    lda #0
    adc x+1
    sta _6+1
  //SEG92 [48] (byte) gfx_init_chunky::c#0 ← ((byte)) (word~) gfx_init_chunky::$6 -- vbuaa=_byte_vwuz1 
    lda _6
  //SEG93 [49] *((byte*) gfx_init_chunky::gfxb#4) ← (byte) gfx_init_chunky::c#0 -- _deref_pbuz1=vbuaa 
    ldy #0
    sta (gfxb),y
  //SEG94 [50] (byte*) gfx_init_chunky::gfxb#1 ← ++ (byte*) gfx_init_chunky::gfxb#4 -- pbuz1=_inc_pbuz1 
    inc gfxb
    bne !+
    inc gfxb+1
  !:
  //SEG95 [51] (word) gfx_init_chunky::x#1 ← ++ (word) gfx_init_chunky::x#2 -- vwuz1=_inc_vwuz1 
    inc x
    bne !+
    inc x+1
  !:
  //SEG96 [52] if((word) gfx_init_chunky::x#1!=(word/signed word/dword/signed dword) 320) goto gfx_init_chunky::@2 -- vwuz1_neq_vwuc1_then_la1 
    lda x+1
    cmp #>$140
    bne b2
    lda x
    cmp #<$140
    bne b2
  //SEG97 gfx_init_chunky::@5
  //SEG98 [53] (byte) gfx_init_chunky::y#1 ← ++ (byte) gfx_init_chunky::y#6 -- vbuz1=_inc_vbuz1 
    inc y
  //SEG99 [54] if((byte) gfx_init_chunky::y#1!=(byte/signed byte/word/signed word/dword/signed dword) 51) goto gfx_init_chunky::@1 -- vbuz1_neq_vbuc1_then_la1 
    lda y
    cmp #$33
    bne b1
  //SEG100 [55] phi from gfx_init_chunky::@5 to gfx_init_chunky::@6 [phi:gfx_init_chunky::@5->gfx_init_chunky::@6]
  //SEG101 gfx_init_chunky::@6
  //SEG102 [56] call dtvSetCpuBankSegment1 
  //SEG103 [58] phi from gfx_init_chunky::@6 to dtvSetCpuBankSegment1 [phi:gfx_init_chunky::@6->dtvSetCpuBankSegment1]
  //SEG104 [58] phi (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 = ((byte))(word/signed word/dword/signed dword) 16384/(word/signed word/dword/signed dword) 16384 [phi:gfx_init_chunky::@6->dtvSetCpuBankSegment1#0] -- vbuaa=vbuc1 
    lda #$4000/$4000
    jsr dtvSetCpuBankSegment1
  //SEG105 gfx_init_chunky::@return
  //SEG106 [57] return 
    rts
}
//SEG107 dtvSetCpuBankSegment1
// Set the memory pointed to by CPU BANK 1 SEGMENT ($4000-$7fff)
// This sets which actual memory is addressed when the CPU reads/writes to $4000-$7fff
// The actual memory addressed will be $4000*cpuSegmentIdx
// dtvSetCpuBankSegment1(byte register(A) cpuBankIdx)
dtvSetCpuBankSegment1: {
    // Move CPU BANK 1 SEGMENT ($4000-$7fff)
    .label cpuBank = $ff
  //SEG108 [59] *((const byte*) dtvSetCpuBankSegment1::cpuBank#0) ← (byte) dtvSetCpuBankSegment1::cpuBankIdx#3 -- _deref_pbuc1=vbuaa 
    sta cpuBank
  //SEG109 asm { .byte$32,$dd lda$ff .byte$32,$00  }
    .byte $32, $dd
    lda $ff
    .byte $32, $00
  //SEG110 dtvSetCpuBankSegment1::@return
  //SEG111 [61] return 
    rts
}

