(label) @6
(label) @begin
(label) @end
(byte*) BGCOL
(const byte*) BGCOL#0 BGCOL = ((byte*))(word/dword/signed dword) 53281
(byte*) BGCOL1
(byte*) BGCOL2
(byte*) BGCOL3
(byte*) BGCOL4
(byte) BLACK
(byte) BLUE
(byte*) BORDERCOL
(byte) BROWN
(byte*) CHARGEN
(byte*) CIA1_INTERRUPT
(byte*) CIA1_PORT_A
(byte*) CIA1_PORT_A_DDR
(byte*) CIA1_PORT_B
(byte*) CIA1_PORT_B_DDR
(byte*) CIA2_INTERRUPT
(byte*) CIA2_PORT_A
(byte*) CIA2_PORT_A_DDR
(byte*) CIA2_PORT_B
(byte*) CIA2_PORT_B_DDR
(byte) CIA_INTERRUPT_CLEAR
(byte*) COLS
(byte) CYAN
(byte*) D011
(byte*) D016
(byte*) D018
(byte) DARK_GREY
(byte) DTV_BADLINE_OFF
(const byte) DTV_BADLINE_OFF#0 DTV_BADLINE_OFF = (byte/signed byte/word/signed word/dword/signed dword) 32
(byte*) DTV_BLITTER_ALU
(byte*) DTV_BLITTER_CONTROL
(byte*) DTV_BLITTER_CONTROL2
(byte*) DTV_BLITTER_DEST_HI
(byte*) DTV_BLITTER_DEST_LIN_HI
(byte*) DTV_BLITTER_DEST_LIN_LO
(byte*) DTV_BLITTER_DEST_LO
(byte*) DTV_BLITTER_DEST_MI
(byte*) DTV_BLITTER_DEST_MOD_HI
(byte*) DTV_BLITTER_DEST_MOD_LO
(byte*) DTV_BLITTER_DEST_STEP
(byte*) DTV_BLITTER_LEN_HI
(byte*) DTV_BLITTER_LEN_LO
(byte*) DTV_BLITTER_SRCA_HI
(byte*) DTV_BLITTER_SRCA_LIN_HI
(byte*) DTV_BLITTER_SRCA_LIN_LO
(byte*) DTV_BLITTER_SRCA_LO
(byte*) DTV_BLITTER_SRCA_MI
(byte*) DTV_BLITTER_SRCA_MOD_HI
(byte*) DTV_BLITTER_SRCA_MOD_LO
(byte*) DTV_BLITTER_SRCA_STEP
(byte*) DTV_BLITTER_SRCB_HI
(byte*) DTV_BLITTER_SRCB_LIN_HI
(byte*) DTV_BLITTER_SRCB_LIN_LO
(byte*) DTV_BLITTER_SRCB_LO
(byte*) DTV_BLITTER_SRCB_MI
(byte*) DTV_BLITTER_SRCB_MOD_HI
(byte*) DTV_BLITTER_SRCB_MOD_LO
(byte*) DTV_BLITTER_SRCB_STEP
(byte*) DTV_BLITTER_TRANSPARANCY
(byte) DTV_BLIT_ADD
(byte) DTV_BLIT_AND
(byte) DTV_BLIT_CIA_IRQ
(byte) DTV_BLIT_CLEAR_IRQ
(byte) DTV_BLIT_DEST_CONT
(byte) DTV_BLIT_DEST_FWD
(byte) DTV_BLIT_DISABLE_B
(byte) DTV_BLIT_FORCE_START
(byte) DTV_BLIT_IRQ_EN
(byte) DTV_BLIT_NAND
(byte) DTV_BLIT_NOR
(byte) DTV_BLIT_OR
(byte) DTV_BLIT_SHIFT0
(byte) DTV_BLIT_SHIFT1
(byte) DTV_BLIT_SHIFT2
(byte) DTV_BLIT_SHIFT3
(byte) DTV_BLIT_SHIFT4
(byte) DTV_BLIT_SHIFT5
(byte) DTV_BLIT_SHIFT6
(byte) DTV_BLIT_SHIFT7
(byte) DTV_BLIT_SRCA_CONT
(byte) DTV_BLIT_SRCA_FWD
(byte) DTV_BLIT_SRCB_CONT
(byte) DTV_BLIT_SRCB_FWD
(byte) DTV_BLIT_STATUS_BUSY
(byte) DTV_BLIT_STATUS_IRQ
(byte) DTV_BLIT_SUB
(byte) DTV_BLIT_TRANSPARANCY_NONE
(byte) DTV_BLIT_VBLANK
(byte) DTV_BLIT_VIC_IRQ
(byte) DTV_BLIT_WRITE_NONTRANSPARENT
(byte) DTV_BLIT_WRITE_TRANSPARENT
(byte) DTV_BLIT_XNOR
(byte) DTV_BLIT_XOR
(byte) DTV_BORDER_OFF
(const byte) DTV_BORDER_OFF#0 DTV_BORDER_OFF = (byte/signed byte/word/signed word/dword/signed dword) 2
(byte) DTV_CHUNKY
(byte) DTV_COLORRAM_OFF
(dword) DTV_COLOR_BANK_DEFAULT
(byte*) DTV_COLOR_BANK_HI
(byte*) DTV_COLOR_BANK_LO
(byte*) DTV_CONTROL
(const byte*) DTV_CONTROL#0 DTV_CONTROL = ((byte*))(word/dword/signed dword) 53308
(byte*) DTV_FEATURE
(const byte*) DTV_FEATURE#0 DTV_FEATURE = ((byte*))(word/dword/signed dword) 53311
(byte) DTV_FEATURE_DISABLE_TIL_RESET
(byte) DTV_FEATURE_ENABLE
(const byte) DTV_FEATURE_ENABLE#0 DTV_FEATURE_ENABLE = (byte/signed byte/word/signed word/dword/signed dword) 1
(byte*) DTV_GRAPHICS_HICOL_BANK
(byte*) DTV_GRAPHICS_VIC_BANK
(byte) DTV_HIGHCOLOR
(const byte) DTV_HIGHCOLOR#0 DTV_HIGHCOLOR = (byte/signed byte/word/signed word/dword/signed dword) 4
(byte) DTV_LINEAR
(byte) DTV_OVERSCAN
(byte*) DTV_PALETTE
(const byte*) DTV_PALETTE#0 DTV_PALETTE = ((byte*))(word/dword/signed dword) 53760
(byte[16]) DTV_PALETTE_DEFAULT
(byte*) DTV_PLANEA_MODULO_HI
(byte*) DTV_PLANEA_MODULO_LO
(byte*) DTV_PLANEA_START_HI
(byte*) DTV_PLANEA_START_LO
(byte*) DTV_PLANEA_START_MI
(byte*) DTV_PLANEA_STEP
(byte*) DTV_PLANEB_MODULO_HI
(byte*) DTV_PLANEB_MODULO_LO
(byte*) DTV_PLANEB_START_HI
(byte*) DTV_PLANEB_START_LO
(byte*) DTV_PLANEB_START_MI
(byte*) DTV_PLANEB_STEP
(byte*) DTV_SPRITE_BANK
(byte) GREEN
(byte) GREY
(void()**) HARDWARE_IRQ
(byte) IRQ_COLLISION_BG
(byte) IRQ_COLLISION_SPRITE
(byte*) IRQ_ENABLE
(byte) IRQ_LIGHTPEN
(byte) IRQ_RASTER
(byte*) IRQ_STATUS
(void()**) KERNEL_IRQ
(byte*) LIGHTPEN_X
(byte*) LIGHTPEN_Y
(byte) LIGHT_BLUE
(byte) LIGHT_GREEN
(byte) LIGHT_GREY
(byte) ORANGE
(byte) PINK
(byte*) PROCPORT
(byte) PROCPORT_BASIC_KERNEL_IO
(byte*) PROCPORT_DDR
(byte) PROCPORT_DDR_MEMORY_MASK
(byte) PROCPORT_KERNEL_IO
(byte) PROCPORT_RAM_ALL
(byte) PROCPORT_RAM_CHARROM
(byte) PROCPORT_RAM_IO
(byte) PURPLE
(byte*) RASTER
(const byte*) RASTER#0 RASTER = ((byte*))(word/dword/signed dword) 53266
(byte) RED
(byte*) SPRITES_COLS
(byte*) SPRITES_ENABLE
(byte*) SPRITES_EXPAND_X
(byte*) SPRITES_EXPAND_Y
(byte*) SPRITES_MC
(byte*) SPRITES_MC1
(byte*) SPRITES_MC2
(byte*) SPRITES_PRIORITY
(byte*) SPRITES_XMSB
(byte*) SPRITES_XPOS
(byte*) SPRITES_YPOS
(word) SPRITE_PTRS
(byte) VIC_BMM
(byte*) VIC_CONTROL
(byte*) VIC_CONTROL2
(byte) VIC_CSEL
(byte) VIC_DEN
(byte) VIC_ECM
(byte) VIC_MCM
(byte*) VIC_MEMORY
(byte) VIC_RSEL
(byte) VIC_RST8
(byte) WHITE
(byte) YELLOW
(void()) main()
(label) main::@4
(label) main::@6
(label) main::@7
(label) main::@8
(byte) main::c
(byte) main::c#1 reg byte x 151.5
(byte) main::c#2 reg byte x 201.99999999999997
(byte[16]) main::palette
(const byte[16]) main::palette#0 palette = { (byte/signed byte/word/signed word/dword/signed dword) 0, (byte/signed byte/word/signed word/dword/signed dword) 1, (byte/signed byte/word/signed word/dword/signed dword) 2, (byte/signed byte/word/signed word/dword/signed dword) 3, (byte/signed byte/word/signed word/dword/signed dword) 4, (byte/signed byte/word/signed word/dword/signed dword) 5, (byte/signed byte/word/signed word/dword/signed dword) 6, (byte/signed byte/word/signed word/dword/signed dword) 7, (byte/signed byte/word/signed word/dword/signed dword) 8, (byte/signed byte/word/signed word/dword/signed dword) 9, (byte/signed byte/word/signed word/dword/signed dword) 10, (byte/signed byte/word/signed word/dword/signed dword) 11, (byte/signed byte/word/signed word/dword/signed dword) 12, (byte/signed byte/word/signed word/dword/signed dword) 13, (byte/signed byte/word/signed word/dword/signed dword) 14, (byte/signed byte/word/signed word/dword/signed dword) 15 }
(byte) main::r
(byte) main::r#1 reg byte x 151.5
(byte) main::r#2 reg byte x 67.33333333333333

reg byte x [ main::r#2 main::r#1 ]
reg byte x [ main::c#2 main::c#1 ]
