Inlined call (byte~) vicSelectGfxBank::$0 ← call toDd00 (byte*) vicSelectGfxBank::gfx 

CONTROL FLOW GRAPH SSA
@begin: scope:[]  from
  (byte*) PROCPORT_DDR#0 ← ((byte*)) (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) PROCPORT_DDR_MEMORY_MASK#0 ← (byte/signed byte/word/signed word/dword/signed dword) 7
  (byte*) PROCPORT#0 ← ((byte*)) (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) PROCPORT_RAM_ALL#0 ← (byte/signed byte/word/signed word/dword/signed dword) 48
  (byte) PROCPORT_RAM_IO#0 ← (byte/signed byte/word/signed word/dword/signed dword) 53
  (byte) PROCPORT_RAM_CHARROM#0 ← (byte/signed byte/word/signed word/dword/signed dword) 49
  (byte) PROCPORT_KERNEL_IO#0 ← (byte/signed byte/word/signed word/dword/signed dword) 54
  (byte) PROCPORT_BASIC_KERNEL_IO#0 ← (byte/signed byte/word/signed word/dword/signed dword) 55
  (byte*) CHARGEN#0 ← ((byte*)) (word/dword/signed dword) 53248
  (word) SPRITE_PTRS#0 ← (word/signed word/dword/signed dword) 1016
  (byte*) SPRITES_XPOS#0 ← ((byte*)) (word/dword/signed dword) 53248
  (byte*) SPRITES_YPOS#0 ← ((byte*)) (word/dword/signed dword) 53249
  (byte*) SPRITES_XMSB#0 ← ((byte*)) (word/dword/signed dword) 53264
  (byte*) RASTER#0 ← ((byte*)) (word/dword/signed dword) 53266
  (byte*) SPRITES_ENABLE#0 ← ((byte*)) (word/dword/signed dword) 53269
  (byte*) SPRITES_EXPAND_Y#0 ← ((byte*)) (word/dword/signed dword) 53271
  (byte*) SPRITES_PRIORITY#0 ← ((byte*)) (word/dword/signed dword) 53275
  (byte*) SPRITES_MC#0 ← ((byte*)) (word/dword/signed dword) 53276
  (byte*) SPRITES_EXPAND_X#0 ← ((byte*)) (word/dword/signed dword) 53277
  (byte*) BORDERCOL#0 ← ((byte*)) (word/dword/signed dword) 53280
  (byte*) BGCOL#0 ← ((byte*)) (word/dword/signed dword) 53281
  (byte*) BGCOL1#0 ← ((byte*)) (word/dword/signed dword) 53281
  (byte*) BGCOL2#0 ← ((byte*)) (word/dword/signed dword) 53282
  (byte*) BGCOL3#0 ← ((byte*)) (word/dword/signed dword) 53283
  (byte*) BGCOL4#0 ← ((byte*)) (word/dword/signed dword) 53284
  (byte*) SPRITES_MC1#0 ← ((byte*)) (word/dword/signed dword) 53285
  (byte*) SPRITES_MC2#0 ← ((byte*)) (word/dword/signed dword) 53286
  (byte*) SPRITES_COLS#0 ← ((byte*)) (word/dword/signed dword) 53287
  (byte*) VIC_CONTROL#0 ← ((byte*)) (word/dword/signed dword) 53265
  (byte*) D011#0 ← ((byte*)) (word/dword/signed dword) 53265
  (byte) VIC_RST8#0 ← (byte/word/signed word/dword/signed dword) 128
  (byte) VIC_ECM#0 ← (byte/signed byte/word/signed word/dword/signed dword) 64
  (byte) VIC_BMM#0 ← (byte/signed byte/word/signed word/dword/signed dword) 32
  (byte) VIC_DEN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) VIC_RSEL#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte*) VIC_CONTROL2#0 ← ((byte*)) (word/dword/signed dword) 53270
  (byte*) D016#0 ← ((byte*)) (word/dword/signed dword) 53270
  (byte) VIC_MCM#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) VIC_CSEL#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte*) D018#0 ← ((byte*)) (word/dword/signed dword) 53272
  (byte*) VIC_MEMORY#0 ← ((byte*)) (word/dword/signed dword) 53272
  (byte*) LIGHTPEN_X#0 ← ((byte*)) (word/dword/signed dword) 53267
  (byte*) LIGHTPEN_Y#0 ← ((byte*)) (word/dword/signed dword) 53268
  (byte*) IRQ_STATUS#0 ← ((byte*)) (word/dword/signed dword) 53273
  (byte*) IRQ_ENABLE#0 ← ((byte*)) (word/dword/signed dword) 53274
  (byte) IRQ_RASTER#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) IRQ_COLLISION_BG#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) IRQ_COLLISION_SPRITE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) IRQ_LIGHTPEN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte*) COLS#0 ← ((byte*)) (word/dword/signed dword) 55296
  (byte*) CIA1_PORT_A#0 ← ((byte*)) (word/dword/signed dword) 56320
  (byte*) CIA1_PORT_B#0 ← ((byte*)) (word/dword/signed dword) 56321
  (byte*) CIA1_PORT_A_DDR#0 ← ((byte*)) (word/dword/signed dword) 56322
  (byte*) CIA1_PORT_B_DDR#0 ← ((byte*)) (word/dword/signed dword) 56323
  (byte*) CIA1_INTERRUPT#0 ← ((byte*)) (word/dword/signed dword) 56333
  (byte) CIA_INTERRUPT_CLEAR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 127
  (byte*) CIA2_PORT_A#0 ← ((byte*)) (word/dword/signed dword) 56576
  (byte*) CIA2_PORT_B#0 ← ((byte*)) (word/dword/signed dword) 56577
  (byte*) CIA2_PORT_A_DDR#0 ← ((byte*)) (word/dword/signed dword) 56578
  (byte*) CIA2_PORT_B_DDR#0 ← ((byte*)) (word/dword/signed dword) 56579
  (byte*) CIA2_INTERRUPT#0 ← ((byte*)) (word/dword/signed dword) 56589
  (void()**) KERNEL_IRQ#0 ← ((void()**)) (word/signed word/dword/signed dword) 788
  (void()**) HARDWARE_IRQ#0 ← ((void()**)) (word/dword/signed dword) 65534
  (byte) BLACK#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) WHITE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) RED#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) CYAN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 3
  (byte) PURPLE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) GREEN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 5
  (byte) BLUE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 6
  (byte) YELLOW#0 ← (byte/signed byte/word/signed word/dword/signed dword) 7
  (byte) ORANGE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) BROWN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 9
  (byte) PINK#0 ← (byte/signed byte/word/signed word/dword/signed dword) 10
  (byte) DARK_GREY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 11
  (byte) GREY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 12
  (byte) LIGHT_GREEN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 13
  (byte) LIGHT_BLUE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 14
  (byte) LIGHT_GREY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 15
  to:@4
@4: scope:[]  from @begin
  (byte*) DTV_FEATURE#0 ← ((byte*)) (word/dword/signed dword) 53311
  (byte) DTV_FEATURE_ENABLE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_FEATURE_DISABLE_TIL_RESET#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte*) DTV_CONTROL#0 ← ((byte*)) (word/dword/signed dword) 53308
  (byte) DTV_LINEAR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BORDER_OFF#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_HIGHCOLOR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_OVERSCAN#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) DTV_COLORRAM_OFF#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) DTV_BADLINE_OFF#0 ← (byte/signed byte/word/signed word/dword/signed dword) 32
  (byte) DTV_CHUNKY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 64
  (byte*) DTV_PALETTE#0 ← ((byte*)) (word/dword/signed dword) 53760
  (byte[16]) DTV_PALETTE_DEFAULT#0 ← { (byte/signed byte/word/signed word/dword/signed dword) 0, (byte/signed byte/word/signed word/dword/signed dword) 15, (byte/signed byte/word/signed word/dword/signed dword) 54, (byte/word/signed word/dword/signed dword) 190, (byte/signed byte/word/signed word/dword/signed dword) 88, (byte/word/signed word/dword/signed dword) 219, (byte/word/signed word/dword/signed dword) 134, (byte/word/signed word/dword/signed dword) 255, (byte/signed byte/word/signed word/dword/signed dword) 41, (byte/signed byte/word/signed word/dword/signed dword) 38, (byte/signed byte/word/signed word/dword/signed dword) 59, (byte/signed byte/word/signed word/dword/signed dword) 5, (byte/signed byte/word/signed word/dword/signed dword) 7, (byte/word/signed word/dword/signed dword) 223, (byte/word/signed word/dword/signed dword) 154, (byte/signed byte/word/signed word/dword/signed dword) 10 }
  (byte*) DTV_PLANEA_START_LO#0 ← ((byte*)) (word/dword/signed dword) 53306
  (byte*) DTV_PLANEA_START_MI#0 ← ((byte*)) (word/dword/signed dword) 53307
  (byte*) DTV_PLANEA_START_HI#0 ← ((byte*)) (word/dword/signed dword) 53317
  (byte*) DTV_PLANEA_STEP#0 ← ((byte*)) (word/dword/signed dword) 53318
  (byte*) DTV_PLANEA_MODULO_LO#0 ← ((byte*)) (word/dword/signed dword) 53304
  (byte*) DTV_PLANEA_MODULO_HI#0 ← ((byte*)) (word/dword/signed dword) 53305
  (byte*) DTV_PLANEB_START_LO#0 ← ((byte*)) (word/dword/signed dword) 53321
  (byte*) DTV_PLANEB_START_MI#0 ← ((byte*)) (word/dword/signed dword) 53322
  (byte*) DTV_PLANEB_START_HI#0 ← ((byte*)) (word/dword/signed dword) 53323
  (byte*) DTV_PLANEB_STEP#0 ← ((byte*)) (word/dword/signed dword) 53324
  (byte*) DTV_PLANEB_MODULO_LO#0 ← ((byte*)) (word/dword/signed dword) 53319
  (byte*) DTV_PLANEB_MODULO_HI#0 ← ((byte*)) (word/dword/signed dword) 53320
  (byte*) DTV_SPRITE_BANK#0 ← ((byte*)) (word/dword/signed dword) 53325
  (byte*) DTV_COLOR_BANK_LO#0 ← ((byte*)) (word/dword/signed dword) 53302
  (byte*) DTV_COLOR_BANK_HI#0 ← ((byte*)) (word/dword/signed dword) 53303
  (dword) DTV_COLOR_BANK_DEFAULT#0 ← (dword/signed dword) 120832
  (byte*) DTV_GRAPHICS_VIC_BANK#0 ← ((byte*)) (word/dword/signed dword) 53309
  (byte*) DTV_GRAPHICS_HICOL_BANK#0 ← ((byte*)) (word/dword/signed dword) 53310
  to:@5
@5: scope:[]  from @4
  (byte*) DTV_BLITTER_SRCA_LO#0 ← ((byte*)) (word/dword/signed dword) 54048
  (byte*) DTV_BLITTER_SRCA_MI#0 ← ((byte*)) (word/dword/signed dword) 54049
  (byte*) DTV_BLITTER_SRCA_HI#0 ← ((byte*)) (word/dword/signed dword) 54050
  (byte*) DTV_BLITTER_SRCA_MOD_LO#0 ← ((byte*)) (word/dword/signed dword) 54051
  (byte*) DTV_BLITTER_SRCA_MOD_HI#0 ← ((byte*)) (word/dword/signed dword) 54052
  (byte*) DTV_BLITTER_SRCA_LIN_LO#0 ← ((byte*)) (word/dword/signed dword) 54053
  (byte*) DTV_BLITTER_SRCA_LIN_HI#0 ← ((byte*)) (word/dword/signed dword) 54054
  (byte*) DTV_BLITTER_SRCA_STEP#0 ← ((byte*)) (word/dword/signed dword) 54055
  (byte*) DTV_BLITTER_SRCB_LO#0 ← ((byte*)) (word/dword/signed dword) 54056
  (byte*) DTV_BLITTER_SRCB_MI#0 ← ((byte*)) (word/dword/signed dword) 54057
  (byte*) DTV_BLITTER_SRCB_HI#0 ← ((byte*)) (word/dword/signed dword) 54058
  (byte*) DTV_BLITTER_SRCB_MOD_LO#0 ← ((byte*)) (word/dword/signed dword) 54059
  (byte*) DTV_BLITTER_SRCB_MOD_HI#0 ← ((byte*)) (word/dword/signed dword) 54060
  (byte*) DTV_BLITTER_SRCB_LIN_LO#0 ← ((byte*)) (word/dword/signed dword) 54061
  (byte*) DTV_BLITTER_SRCB_LIN_HI#0 ← ((byte*)) (word/dword/signed dword) 54062
  (byte*) DTV_BLITTER_SRCB_STEP#0 ← ((byte*)) (word/dword/signed dword) 54063
  (byte*) DTV_BLITTER_DEST_LO#0 ← ((byte*)) (word/dword/signed dword) 54064
  (byte*) DTV_BLITTER_DEST_MI#0 ← ((byte*)) (word/dword/signed dword) 54065
  (byte*) DTV_BLITTER_DEST_HI#0 ← ((byte*)) (word/dword/signed dword) 54066
  (byte*) DTV_BLITTER_DEST_MOD_LO#0 ← ((byte*)) (word/dword/signed dword) 54067
  (byte*) DTV_BLITTER_DEST_MOD_HI#0 ← ((byte*)) (word/dword/signed dword) 54068
  (byte*) DTV_BLITTER_DEST_LIN_LO#0 ← ((byte*)) (word/dword/signed dword) 54069
  (byte*) DTV_BLITTER_DEST_LIN_HI#0 ← ((byte*)) (word/dword/signed dword) 54070
  (byte*) DTV_BLITTER_DEST_STEP#0 ← ((byte*)) (word/dword/signed dword) 54071
  (byte*) DTV_BLITTER_LEN_LO#0 ← ((byte*)) (word/dword/signed dword) 54072
  (byte*) DTV_BLITTER_LEN_HI#0 ← ((byte*)) (word/dword/signed dword) 54073
  (byte*) DTV_BLITTER_CONTROL#0 ← ((byte*)) (word/dword/signed dword) 54074
  (byte) DTV_BLIT_FORCE_START#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_SRCA_FWD#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_BLIT_SRCB_FWD#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_BLIT_DEST_FWD#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) DTV_BLIT_VIC_IRQ#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) DTV_BLIT_CIA_IRQ#0 ← (byte/signed byte/word/signed word/dword/signed dword) 32
  (byte) DTV_BLIT_VBLANK#0 ← (byte/signed byte/word/signed word/dword/signed dword) 64
  (byte) DTV_BLIT_IRQ_EN#0 ← (byte/word/signed word/dword/signed dword) 128
  (byte*) DTV_BLITTER_TRANSPARANCY#0 ← ((byte*)) (word/dword/signed dword) 54075
  (byte) DTV_BLIT_DISABLE_B#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_WRITE_TRANSPARENT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_BLIT_WRITE_NONTRANSPARENT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_BLIT_TRANSPARANCY_NONE#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte*) DTV_BLITTER_ALU#0 ← ((byte*)) (word/dword/signed dword) 54078
  (byte) DTV_BLIT_SHIFT0#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) DTV_BLIT_SHIFT1#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_SHIFT2#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_BLIT_SHIFT3#0 ← (byte/signed byte/word/signed word/dword/signed dword) 3
  (byte) DTV_BLIT_SHIFT4#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_BLIT_SHIFT5#0 ← (byte/signed byte/word/signed word/dword/signed dword) 5
  (byte) DTV_BLIT_SHIFT6#0 ← (byte/signed byte/word/signed word/dword/signed dword) 6
  (byte) DTV_BLIT_SHIFT7#0 ← (byte/signed byte/word/signed word/dword/signed dword) 7
  (byte) DTV_BLIT_AND#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) DTV_BLIT_NAND#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) DTV_BLIT_NOR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 16
  (byte) DTV_BLIT_OR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 24
  (byte) DTV_BLIT_XOR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 32
  (byte) DTV_BLIT_XNOR#0 ← (byte/signed byte/word/signed word/dword/signed dword) 40
  (byte) DTV_BLIT_ADD#0 ← (byte/signed byte/word/signed word/dword/signed dword) 48
  (byte) DTV_BLIT_SUB#0 ← (byte/signed byte/word/signed word/dword/signed dword) 56
  (byte*) DTV_BLITTER_CONTROL2#0 ← ((byte*)) (word/dword/signed dword) 54079
  (byte) DTV_BLIT_CLEAR_IRQ#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_SRCA_CONT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  (byte) DTV_BLIT_SRCB_CONT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 4
  (byte) DTV_BLIT_DEST_CONT#0 ← (byte/signed byte/word/signed word/dword/signed dword) 8
  (byte) DTV_BLIT_STATUS_BUSY#0 ← (byte/signed byte/word/signed word/dword/signed dword) 1
  (byte) DTV_BLIT_STATUS_IRQ#0 ← (byte/signed byte/word/signed word/dword/signed dword) 2
  to:@6
main: scope:[main]  from @6
  asm { sei  }
  *((byte*) DTV_FEATURE#0) ← (byte) DTV_FEATURE_ENABLE#0
  (byte~) main::$0 ← (byte) DTV_HIGHCOLOR#0 | (byte) DTV_BORDER_OFF#0
  (byte~) main::$1 ← (byte~) main::$0 | (byte) DTV_BADLINE_OFF#0
  *((byte*) DTV_CONTROL#0) ← (byte~) main::$1
  (byte[16]) main::palette#0 ← { (byte/signed byte/word/signed word/dword/signed dword) 0, (byte/signed byte/word/signed word/dword/signed dword) 1, (byte/signed byte/word/signed word/dword/signed dword) 2, (byte/signed byte/word/signed word/dword/signed dword) 3, (byte/signed byte/word/signed word/dword/signed dword) 4, (byte/signed byte/word/signed word/dword/signed dword) 5, (byte/signed byte/word/signed word/dword/signed dword) 6, (byte/signed byte/word/signed word/dword/signed dword) 7, (byte/signed byte/word/signed word/dword/signed dword) 8, (byte/signed byte/word/signed word/dword/signed dword) 9, (byte/signed byte/word/signed word/dword/signed dword) 10, (byte/signed byte/word/signed word/dword/signed dword) 11, (byte/signed byte/word/signed word/dword/signed dword) 12, (byte/signed byte/word/signed word/dword/signed dword) 13, (byte/signed byte/word/signed word/dword/signed dword) 14, (byte/signed byte/word/signed word/dword/signed dword) 15 }
  to:main::@1
main::@1: scope:[main]  from main main::@8
  if(true) goto main::@2
  to:main::@return
main::@2: scope:[main]  from main::@1
  to:main::@4
main::@4: scope:[main]  from main::@2 main::@5
  (bool~) main::$2 ← *((byte*) RASTER#0) != (byte/signed byte/word/signed word/dword/signed dword) 64
  if((bool~) main::$2) goto main::@5
  to:main::@6
main::@5: scope:[main]  from main::@4
  to:main::@4
main::@6: scope:[main]  from main::@4
  *((byte*) BGCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  (byte) main::r#0 ← (byte/signed byte/word/signed word/dword/signed dword) 49
  to:main::@7
main::@7: scope:[main]  from main::@6 main::@7
  (byte) main::r#2 ← phi( main::@6/(byte) main::r#0 main::@7/(byte) main::r#1 )
  asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
  *((byte*) BGCOL#0) ← ++ *((byte*) BGCOL#0)
  (byte) main::r#1 ← (byte) main::r#2 + rangenext(49,255)
  (bool~) main::$3 ← (byte) main::r#1 != rangelast(49,255)
  if((bool~) main::$3) goto main::@7
  to:main::@14
main::@14: scope:[main]  from main::@7
  (byte) main::c#0 ← (byte/signed byte/word/signed word/dword/signed dword) 0
  to:main::@8
main::@8: scope:[main]  from main::@14 main::@8
  (byte) main::c#2 ← phi( main::@14/(byte) main::c#0 main::@8/(byte) main::c#1 )
  *((byte*) DTV_PALETTE#0 + (byte) main::c#2) ← *((byte[16]) main::palette#0 + (byte) main::c#2)
  *((byte[16]) main::palette#0 + (byte) main::c#2) ← ++ *((byte[16]) main::palette#0 + (byte) main::c#2)
  (byte) main::c#1 ← (byte) main::c#2 + rangenext(0,15)
  (bool~) main::$4 ← (byte) main::c#1 != rangelast(0,15)
  if((bool~) main::$4) goto main::@8
  to:main::@1
main::@return: scope:[main]  from main::@1
  return 
  to:@return
@6: scope:[]  from @5
  call main 
  to:@7
@7: scope:[]  from @6
  to:@end
@end: scope:[]  from @7

SYMBOL TABLE SSA
(label) @4
(label) @5
(label) @6
(label) @7
(label) @begin
(label) @end
(byte*) BGCOL
(byte*) BGCOL#0
(byte*) BGCOL1
(byte*) BGCOL1#0
(byte*) BGCOL2
(byte*) BGCOL2#0
(byte*) BGCOL3
(byte*) BGCOL3#0
(byte*) BGCOL4
(byte*) BGCOL4#0
(byte) BLACK
(byte) BLACK#0
(byte) BLUE
(byte) BLUE#0
(byte*) BORDERCOL
(byte*) BORDERCOL#0
(byte) BROWN
(byte) BROWN#0
(byte*) CHARGEN
(byte*) CHARGEN#0
(byte*) CIA1_INTERRUPT
(byte*) CIA1_INTERRUPT#0
(byte*) CIA1_PORT_A
(byte*) CIA1_PORT_A#0
(byte*) CIA1_PORT_A_DDR
(byte*) CIA1_PORT_A_DDR#0
(byte*) CIA1_PORT_B
(byte*) CIA1_PORT_B#0
(byte*) CIA1_PORT_B_DDR
(byte*) CIA1_PORT_B_DDR#0
(byte*) CIA2_INTERRUPT
(byte*) CIA2_INTERRUPT#0
(byte*) CIA2_PORT_A
(byte*) CIA2_PORT_A#0
(byte*) CIA2_PORT_A_DDR
(byte*) CIA2_PORT_A_DDR#0
(byte*) CIA2_PORT_B
(byte*) CIA2_PORT_B#0
(byte*) CIA2_PORT_B_DDR
(byte*) CIA2_PORT_B_DDR#0
(byte) CIA_INTERRUPT_CLEAR
(byte) CIA_INTERRUPT_CLEAR#0
(byte*) COLS
(byte*) COLS#0
(byte) CYAN
(byte) CYAN#0
(byte*) D011
(byte*) D011#0
(byte*) D016
(byte*) D016#0
(byte*) D018
(byte*) D018#0
(byte) DARK_GREY
(byte) DARK_GREY#0
(byte) DTV_BADLINE_OFF
(byte) DTV_BADLINE_OFF#0
(byte*) DTV_BLITTER_ALU
(byte*) DTV_BLITTER_ALU#0
(byte*) DTV_BLITTER_CONTROL
(byte*) DTV_BLITTER_CONTROL#0
(byte*) DTV_BLITTER_CONTROL2
(byte*) DTV_BLITTER_CONTROL2#0
(byte*) DTV_BLITTER_DEST_HI
(byte*) DTV_BLITTER_DEST_HI#0
(byte*) DTV_BLITTER_DEST_LIN_HI
(byte*) DTV_BLITTER_DEST_LIN_HI#0
(byte*) DTV_BLITTER_DEST_LIN_LO
(byte*) DTV_BLITTER_DEST_LIN_LO#0
(byte*) DTV_BLITTER_DEST_LO
(byte*) DTV_BLITTER_DEST_LO#0
(byte*) DTV_BLITTER_DEST_MI
(byte*) DTV_BLITTER_DEST_MI#0
(byte*) DTV_BLITTER_DEST_MOD_HI
(byte*) DTV_BLITTER_DEST_MOD_HI#0
(byte*) DTV_BLITTER_DEST_MOD_LO
(byte*) DTV_BLITTER_DEST_MOD_LO#0
(byte*) DTV_BLITTER_DEST_STEP
(byte*) DTV_BLITTER_DEST_STEP#0
(byte*) DTV_BLITTER_LEN_HI
(byte*) DTV_BLITTER_LEN_HI#0
(byte*) DTV_BLITTER_LEN_LO
(byte*) DTV_BLITTER_LEN_LO#0
(byte*) DTV_BLITTER_SRCA_HI
(byte*) DTV_BLITTER_SRCA_HI#0
(byte*) DTV_BLITTER_SRCA_LIN_HI
(byte*) DTV_BLITTER_SRCA_LIN_HI#0
(byte*) DTV_BLITTER_SRCA_LIN_LO
(byte*) DTV_BLITTER_SRCA_LIN_LO#0
(byte*) DTV_BLITTER_SRCA_LO
(byte*) DTV_BLITTER_SRCA_LO#0
(byte*) DTV_BLITTER_SRCA_MI
(byte*) DTV_BLITTER_SRCA_MI#0
(byte*) DTV_BLITTER_SRCA_MOD_HI
(byte*) DTV_BLITTER_SRCA_MOD_HI#0
(byte*) DTV_BLITTER_SRCA_MOD_LO
(byte*) DTV_BLITTER_SRCA_MOD_LO#0
(byte*) DTV_BLITTER_SRCA_STEP
(byte*) DTV_BLITTER_SRCA_STEP#0
(byte*) DTV_BLITTER_SRCB_HI
(byte*) DTV_BLITTER_SRCB_HI#0
(byte*) DTV_BLITTER_SRCB_LIN_HI
(byte*) DTV_BLITTER_SRCB_LIN_HI#0
(byte*) DTV_BLITTER_SRCB_LIN_LO
(byte*) DTV_BLITTER_SRCB_LIN_LO#0
(byte*) DTV_BLITTER_SRCB_LO
(byte*) DTV_BLITTER_SRCB_LO#0
(byte*) DTV_BLITTER_SRCB_MI
(byte*) DTV_BLITTER_SRCB_MI#0
(byte*) DTV_BLITTER_SRCB_MOD_HI
(byte*) DTV_BLITTER_SRCB_MOD_HI#0
(byte*) DTV_BLITTER_SRCB_MOD_LO
(byte*) DTV_BLITTER_SRCB_MOD_LO#0
(byte*) DTV_BLITTER_SRCB_STEP
(byte*) DTV_BLITTER_SRCB_STEP#0
(byte*) DTV_BLITTER_TRANSPARANCY
(byte*) DTV_BLITTER_TRANSPARANCY#0
(byte) DTV_BLIT_ADD
(byte) DTV_BLIT_ADD#0
(byte) DTV_BLIT_AND
(byte) DTV_BLIT_AND#0
(byte) DTV_BLIT_CIA_IRQ
(byte) DTV_BLIT_CIA_IRQ#0
(byte) DTV_BLIT_CLEAR_IRQ
(byte) DTV_BLIT_CLEAR_IRQ#0
(byte) DTV_BLIT_DEST_CONT
(byte) DTV_BLIT_DEST_CONT#0
(byte) DTV_BLIT_DEST_FWD
(byte) DTV_BLIT_DEST_FWD#0
(byte) DTV_BLIT_DISABLE_B
(byte) DTV_BLIT_DISABLE_B#0
(byte) DTV_BLIT_FORCE_START
(byte) DTV_BLIT_FORCE_START#0
(byte) DTV_BLIT_IRQ_EN
(byte) DTV_BLIT_IRQ_EN#0
(byte) DTV_BLIT_NAND
(byte) DTV_BLIT_NAND#0
(byte) DTV_BLIT_NOR
(byte) DTV_BLIT_NOR#0
(byte) DTV_BLIT_OR
(byte) DTV_BLIT_OR#0
(byte) DTV_BLIT_SHIFT0
(byte) DTV_BLIT_SHIFT0#0
(byte) DTV_BLIT_SHIFT1
(byte) DTV_BLIT_SHIFT1#0
(byte) DTV_BLIT_SHIFT2
(byte) DTV_BLIT_SHIFT2#0
(byte) DTV_BLIT_SHIFT3
(byte) DTV_BLIT_SHIFT3#0
(byte) DTV_BLIT_SHIFT4
(byte) DTV_BLIT_SHIFT4#0
(byte) DTV_BLIT_SHIFT5
(byte) DTV_BLIT_SHIFT5#0
(byte) DTV_BLIT_SHIFT6
(byte) DTV_BLIT_SHIFT6#0
(byte) DTV_BLIT_SHIFT7
(byte) DTV_BLIT_SHIFT7#0
(byte) DTV_BLIT_SRCA_CONT
(byte) DTV_BLIT_SRCA_CONT#0
(byte) DTV_BLIT_SRCA_FWD
(byte) DTV_BLIT_SRCA_FWD#0
(byte) DTV_BLIT_SRCB_CONT
(byte) DTV_BLIT_SRCB_CONT#0
(byte) DTV_BLIT_SRCB_FWD
(byte) DTV_BLIT_SRCB_FWD#0
(byte) DTV_BLIT_STATUS_BUSY
(byte) DTV_BLIT_STATUS_BUSY#0
(byte) DTV_BLIT_STATUS_IRQ
(byte) DTV_BLIT_STATUS_IRQ#0
(byte) DTV_BLIT_SUB
(byte) DTV_BLIT_SUB#0
(byte) DTV_BLIT_TRANSPARANCY_NONE
(byte) DTV_BLIT_TRANSPARANCY_NONE#0
(byte) DTV_BLIT_VBLANK
(byte) DTV_BLIT_VBLANK#0
(byte) DTV_BLIT_VIC_IRQ
(byte) DTV_BLIT_VIC_IRQ#0
(byte) DTV_BLIT_WRITE_NONTRANSPARENT
(byte) DTV_BLIT_WRITE_NONTRANSPARENT#0
(byte) DTV_BLIT_WRITE_TRANSPARENT
(byte) DTV_BLIT_WRITE_TRANSPARENT#0
(byte) DTV_BLIT_XNOR
(byte) DTV_BLIT_XNOR#0
(byte) DTV_BLIT_XOR
(byte) DTV_BLIT_XOR#0
(byte) DTV_BORDER_OFF
(byte) DTV_BORDER_OFF#0
(byte) DTV_CHUNKY
(byte) DTV_CHUNKY#0
(byte) DTV_COLORRAM_OFF
(byte) DTV_COLORRAM_OFF#0
(dword) DTV_COLOR_BANK_DEFAULT
(dword) DTV_COLOR_BANK_DEFAULT#0
(byte*) DTV_COLOR_BANK_HI
(byte*) DTV_COLOR_BANK_HI#0
(byte*) DTV_COLOR_BANK_LO
(byte*) DTV_COLOR_BANK_LO#0
(byte*) DTV_CONTROL
(byte*) DTV_CONTROL#0
(byte*) DTV_FEATURE
(byte*) DTV_FEATURE#0
(byte) DTV_FEATURE_DISABLE_TIL_RESET
(byte) DTV_FEATURE_DISABLE_TIL_RESET#0
(byte) DTV_FEATURE_ENABLE
(byte) DTV_FEATURE_ENABLE#0
(byte*) DTV_GRAPHICS_HICOL_BANK
(byte*) DTV_GRAPHICS_HICOL_BANK#0
(byte*) DTV_GRAPHICS_VIC_BANK
(byte*) DTV_GRAPHICS_VIC_BANK#0
(byte) DTV_HIGHCOLOR
(byte) DTV_HIGHCOLOR#0
(byte) DTV_LINEAR
(byte) DTV_LINEAR#0
(byte) DTV_OVERSCAN
(byte) DTV_OVERSCAN#0
(byte*) DTV_PALETTE
(byte*) DTV_PALETTE#0
(byte[16]) DTV_PALETTE_DEFAULT
(byte[16]) DTV_PALETTE_DEFAULT#0
(byte*) DTV_PLANEA_MODULO_HI
(byte*) DTV_PLANEA_MODULO_HI#0
(byte*) DTV_PLANEA_MODULO_LO
(byte*) DTV_PLANEA_MODULO_LO#0
(byte*) DTV_PLANEA_START_HI
(byte*) DTV_PLANEA_START_HI#0
(byte*) DTV_PLANEA_START_LO
(byte*) DTV_PLANEA_START_LO#0
(byte*) DTV_PLANEA_START_MI
(byte*) DTV_PLANEA_START_MI#0
(byte*) DTV_PLANEA_STEP
(byte*) DTV_PLANEA_STEP#0
(byte*) DTV_PLANEB_MODULO_HI
(byte*) DTV_PLANEB_MODULO_HI#0
(byte*) DTV_PLANEB_MODULO_LO
(byte*) DTV_PLANEB_MODULO_LO#0
(byte*) DTV_PLANEB_START_HI
(byte*) DTV_PLANEB_START_HI#0
(byte*) DTV_PLANEB_START_LO
(byte*) DTV_PLANEB_START_LO#0
(byte*) DTV_PLANEB_START_MI
(byte*) DTV_PLANEB_START_MI#0
(byte*) DTV_PLANEB_STEP
(byte*) DTV_PLANEB_STEP#0
(byte*) DTV_SPRITE_BANK
(byte*) DTV_SPRITE_BANK#0
(byte) GREEN
(byte) GREEN#0
(byte) GREY
(byte) GREY#0
(void()**) HARDWARE_IRQ
(void()**) HARDWARE_IRQ#0
(byte) IRQ_COLLISION_BG
(byte) IRQ_COLLISION_BG#0
(byte) IRQ_COLLISION_SPRITE
(byte) IRQ_COLLISION_SPRITE#0
(byte*) IRQ_ENABLE
(byte*) IRQ_ENABLE#0
(byte) IRQ_LIGHTPEN
(byte) IRQ_LIGHTPEN#0
(byte) IRQ_RASTER
(byte) IRQ_RASTER#0
(byte*) IRQ_STATUS
(byte*) IRQ_STATUS#0
(void()**) KERNEL_IRQ
(void()**) KERNEL_IRQ#0
(byte*) LIGHTPEN_X
(byte*) LIGHTPEN_X#0
(byte*) LIGHTPEN_Y
(byte*) LIGHTPEN_Y#0
(byte) LIGHT_BLUE
(byte) LIGHT_BLUE#0
(byte) LIGHT_GREEN
(byte) LIGHT_GREEN#0
(byte) LIGHT_GREY
(byte) LIGHT_GREY#0
(byte) ORANGE
(byte) ORANGE#0
(byte) PINK
(byte) PINK#0
(byte*) PROCPORT
(byte*) PROCPORT#0
(byte) PROCPORT_BASIC_KERNEL_IO
(byte) PROCPORT_BASIC_KERNEL_IO#0
(byte*) PROCPORT_DDR
(byte*) PROCPORT_DDR#0
(byte) PROCPORT_DDR_MEMORY_MASK
(byte) PROCPORT_DDR_MEMORY_MASK#0
(byte) PROCPORT_KERNEL_IO
(byte) PROCPORT_KERNEL_IO#0
(byte) PROCPORT_RAM_ALL
(byte) PROCPORT_RAM_ALL#0
(byte) PROCPORT_RAM_CHARROM
(byte) PROCPORT_RAM_CHARROM#0
(byte) PROCPORT_RAM_IO
(byte) PROCPORT_RAM_IO#0
(byte) PURPLE
(byte) PURPLE#0
(byte*) RASTER
(byte*) RASTER#0
(byte) RED
(byte) RED#0
(byte*) SPRITES_COLS
(byte*) SPRITES_COLS#0
(byte*) SPRITES_ENABLE
(byte*) SPRITES_ENABLE#0
(byte*) SPRITES_EXPAND_X
(byte*) SPRITES_EXPAND_X#0
(byte*) SPRITES_EXPAND_Y
(byte*) SPRITES_EXPAND_Y#0
(byte*) SPRITES_MC
(byte*) SPRITES_MC#0
(byte*) SPRITES_MC1
(byte*) SPRITES_MC1#0
(byte*) SPRITES_MC2
(byte*) SPRITES_MC2#0
(byte*) SPRITES_PRIORITY
(byte*) SPRITES_PRIORITY#0
(byte*) SPRITES_XMSB
(byte*) SPRITES_XMSB#0
(byte*) SPRITES_XPOS
(byte*) SPRITES_XPOS#0
(byte*) SPRITES_YPOS
(byte*) SPRITES_YPOS#0
(word) SPRITE_PTRS
(word) SPRITE_PTRS#0
(byte) VIC_BMM
(byte) VIC_BMM#0
(byte*) VIC_CONTROL
(byte*) VIC_CONTROL#0
(byte*) VIC_CONTROL2
(byte*) VIC_CONTROL2#0
(byte) VIC_CSEL
(byte) VIC_CSEL#0
(byte) VIC_DEN
(byte) VIC_DEN#0
(byte) VIC_ECM
(byte) VIC_ECM#0
(byte) VIC_MCM
(byte) VIC_MCM#0
(byte*) VIC_MEMORY
(byte*) VIC_MEMORY#0
(byte) VIC_RSEL
(byte) VIC_RSEL#0
(byte) VIC_RST8
(byte) VIC_RST8#0
(byte) WHITE
(byte) WHITE#0
(byte) YELLOW
(byte) YELLOW#0
(void()) main()
(byte~) main::$0
(byte~) main::$1
(bool~) main::$2
(bool~) main::$3
(bool~) main::$4
(label) main::@1
(label) main::@14
(label) main::@2
(label) main::@4
(label) main::@5
(label) main::@6
(label) main::@7
(label) main::@8
(label) main::@return
(byte) main::c
(byte) main::c#0
(byte) main::c#1
(byte) main::c#2
(byte[16]) main::palette
(byte[16]) main::palette#0
(byte) main::r
(byte) main::r#0
(byte) main::r#1
(byte) main::r#2

Culled Empty Block (label) main::@2
Culled Empty Block (label) main::@5
Culled Empty Block (label) @7
Successful SSA optimization Pass2CullEmptyBlocks
Simple Condition (bool~) main::$2 [182] if(*((byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 64) goto main::@4
Simple Condition (bool~) main::$3 [190] if((byte) main::r#1!=rangelast(49,255)) goto main::@7
Simple Condition (bool~) main::$4 [197] if((byte) main::c#1!=rangelast(0,15)) goto main::@8
Successful SSA optimization Pass2ConditionalJumpSimplification
Constant (const byte*) PROCPORT_DDR#0 = ((byte*))0
Constant (const byte) PROCPORT_DDR_MEMORY_MASK#0 = 7
Constant (const byte*) PROCPORT#0 = ((byte*))1
Constant (const byte) PROCPORT_RAM_ALL#0 = 48
Constant (const byte) PROCPORT_RAM_IO#0 = 53
Constant (const byte) PROCPORT_RAM_CHARROM#0 = 49
Constant (const byte) PROCPORT_KERNEL_IO#0 = 54
Constant (const byte) PROCPORT_BASIC_KERNEL_IO#0 = 55
Constant (const byte*) CHARGEN#0 = ((byte*))53248
Constant (const word) SPRITE_PTRS#0 = 1016
Constant (const byte*) SPRITES_XPOS#0 = ((byte*))53248
Constant (const byte*) SPRITES_YPOS#0 = ((byte*))53249
Constant (const byte*) SPRITES_XMSB#0 = ((byte*))53264
Constant (const byte*) RASTER#0 = ((byte*))53266
Constant (const byte*) SPRITES_ENABLE#0 = ((byte*))53269
Constant (const byte*) SPRITES_EXPAND_Y#0 = ((byte*))53271
Constant (const byte*) SPRITES_PRIORITY#0 = ((byte*))53275
Constant (const byte*) SPRITES_MC#0 = ((byte*))53276
Constant (const byte*) SPRITES_EXPAND_X#0 = ((byte*))53277
Constant (const byte*) BORDERCOL#0 = ((byte*))53280
Constant (const byte*) BGCOL#0 = ((byte*))53281
Constant (const byte*) BGCOL1#0 = ((byte*))53281
Constant (const byte*) BGCOL2#0 = ((byte*))53282
Constant (const byte*) BGCOL3#0 = ((byte*))53283
Constant (const byte*) BGCOL4#0 = ((byte*))53284
Constant (const byte*) SPRITES_MC1#0 = ((byte*))53285
Constant (const byte*) SPRITES_MC2#0 = ((byte*))53286
Constant (const byte*) SPRITES_COLS#0 = ((byte*))53287
Constant (const byte*) VIC_CONTROL#0 = ((byte*))53265
Constant (const byte*) D011#0 = ((byte*))53265
Constant (const byte) VIC_RST8#0 = 128
Constant (const byte) VIC_ECM#0 = 64
Constant (const byte) VIC_BMM#0 = 32
Constant (const byte) VIC_DEN#0 = 16
Constant (const byte) VIC_RSEL#0 = 8
Constant (const byte*) VIC_CONTROL2#0 = ((byte*))53270
Constant (const byte*) D016#0 = ((byte*))53270
Constant (const byte) VIC_MCM#0 = 16
Constant (const byte) VIC_CSEL#0 = 8
Constant (const byte*) D018#0 = ((byte*))53272
Constant (const byte*) VIC_MEMORY#0 = ((byte*))53272
Constant (const byte*) LIGHTPEN_X#0 = ((byte*))53267
Constant (const byte*) LIGHTPEN_Y#0 = ((byte*))53268
Constant (const byte*) IRQ_STATUS#0 = ((byte*))53273
Constant (const byte*) IRQ_ENABLE#0 = ((byte*))53274
Constant (const byte) IRQ_RASTER#0 = 1
Constant (const byte) IRQ_COLLISION_BG#0 = 2
Constant (const byte) IRQ_COLLISION_SPRITE#0 = 4
Constant (const byte) IRQ_LIGHTPEN#0 = 8
Constant (const byte*) COLS#0 = ((byte*))55296
Constant (const byte*) CIA1_PORT_A#0 = ((byte*))56320
Constant (const byte*) CIA1_PORT_B#0 = ((byte*))56321
Constant (const byte*) CIA1_PORT_A_DDR#0 = ((byte*))56322
Constant (const byte*) CIA1_PORT_B_DDR#0 = ((byte*))56323
Constant (const byte*) CIA1_INTERRUPT#0 = ((byte*))56333
Constant (const byte) CIA_INTERRUPT_CLEAR#0 = 127
Constant (const byte*) CIA2_PORT_A#0 = ((byte*))56576
Constant (const byte*) CIA2_PORT_B#0 = ((byte*))56577
Constant (const byte*) CIA2_PORT_A_DDR#0 = ((byte*))56578
Constant (const byte*) CIA2_PORT_B_DDR#0 = ((byte*))56579
Constant (const byte*) CIA2_INTERRUPT#0 = ((byte*))56589
Constant (const void()**) KERNEL_IRQ#0 = ((void()**))788
Constant (const void()**) HARDWARE_IRQ#0 = ((void()**))65534
Constant (const byte) BLACK#0 = 0
Constant (const byte) WHITE#0 = 1
Constant (const byte) RED#0 = 2
Constant (const byte) CYAN#0 = 3
Constant (const byte) PURPLE#0 = 4
Constant (const byte) GREEN#0 = 5
Constant (const byte) BLUE#0 = 6
Constant (const byte) YELLOW#0 = 7
Constant (const byte) ORANGE#0 = 8
Constant (const byte) BROWN#0 = 9
Constant (const byte) PINK#0 = 10
Constant (const byte) DARK_GREY#0 = 11
Constant (const byte) GREY#0 = 12
Constant (const byte) LIGHT_GREEN#0 = 13
Constant (const byte) LIGHT_BLUE#0 = 14
Constant (const byte) LIGHT_GREY#0 = 15
Constant (const byte*) DTV_FEATURE#0 = ((byte*))53311
Constant (const byte) DTV_FEATURE_ENABLE#0 = 1
Constant (const byte) DTV_FEATURE_DISABLE_TIL_RESET#0 = 2
Constant (const byte*) DTV_CONTROL#0 = ((byte*))53308
Constant (const byte) DTV_LINEAR#0 = 1
Constant (const byte) DTV_BORDER_OFF#0 = 2
Constant (const byte) DTV_HIGHCOLOR#0 = 4
Constant (const byte) DTV_OVERSCAN#0 = 8
Constant (const byte) DTV_COLORRAM_OFF#0 = 16
Constant (const byte) DTV_BADLINE_OFF#0 = 32
Constant (const byte) DTV_CHUNKY#0 = 64
Constant (const byte*) DTV_PALETTE#0 = ((byte*))53760
Constant (const byte[16]) DTV_PALETTE_DEFAULT#0 = { 0, 15, 54, 190, 88, 219, 134, 255, 41, 38, 59, 5, 7, 223, 154, 10 }
Constant (const byte*) DTV_PLANEA_START_LO#0 = ((byte*))53306
Constant (const byte*) DTV_PLANEA_START_MI#0 = ((byte*))53307
Constant (const byte*) DTV_PLANEA_START_HI#0 = ((byte*))53317
Constant (const byte*) DTV_PLANEA_STEP#0 = ((byte*))53318
Constant (const byte*) DTV_PLANEA_MODULO_LO#0 = ((byte*))53304
Constant (const byte*) DTV_PLANEA_MODULO_HI#0 = ((byte*))53305
Constant (const byte*) DTV_PLANEB_START_LO#0 = ((byte*))53321
Constant (const byte*) DTV_PLANEB_START_MI#0 = ((byte*))53322
Constant (const byte*) DTV_PLANEB_START_HI#0 = ((byte*))53323
Constant (const byte*) DTV_PLANEB_STEP#0 = ((byte*))53324
Constant (const byte*) DTV_PLANEB_MODULO_LO#0 = ((byte*))53319
Constant (const byte*) DTV_PLANEB_MODULO_HI#0 = ((byte*))53320
Constant (const byte*) DTV_SPRITE_BANK#0 = ((byte*))53325
Constant (const byte*) DTV_COLOR_BANK_LO#0 = ((byte*))53302
Constant (const byte*) DTV_COLOR_BANK_HI#0 = ((byte*))53303
Constant (const dword) DTV_COLOR_BANK_DEFAULT#0 = 120832
Constant (const byte*) DTV_GRAPHICS_VIC_BANK#0 = ((byte*))53309
Constant (const byte*) DTV_GRAPHICS_HICOL_BANK#0 = ((byte*))53310
Constant (const byte*) DTV_BLITTER_SRCA_LO#0 = ((byte*))54048
Constant (const byte*) DTV_BLITTER_SRCA_MI#0 = ((byte*))54049
Constant (const byte*) DTV_BLITTER_SRCA_HI#0 = ((byte*))54050
Constant (const byte*) DTV_BLITTER_SRCA_MOD_LO#0 = ((byte*))54051
Constant (const byte*) DTV_BLITTER_SRCA_MOD_HI#0 = ((byte*))54052
Constant (const byte*) DTV_BLITTER_SRCA_LIN_LO#0 = ((byte*))54053
Constant (const byte*) DTV_BLITTER_SRCA_LIN_HI#0 = ((byte*))54054
Constant (const byte*) DTV_BLITTER_SRCA_STEP#0 = ((byte*))54055
Constant (const byte*) DTV_BLITTER_SRCB_LO#0 = ((byte*))54056
Constant (const byte*) DTV_BLITTER_SRCB_MI#0 = ((byte*))54057
Constant (const byte*) DTV_BLITTER_SRCB_HI#0 = ((byte*))54058
Constant (const byte*) DTV_BLITTER_SRCB_MOD_LO#0 = ((byte*))54059
Constant (const byte*) DTV_BLITTER_SRCB_MOD_HI#0 = ((byte*))54060
Constant (const byte*) DTV_BLITTER_SRCB_LIN_LO#0 = ((byte*))54061
Constant (const byte*) DTV_BLITTER_SRCB_LIN_HI#0 = ((byte*))54062
Constant (const byte*) DTV_BLITTER_SRCB_STEP#0 = ((byte*))54063
Constant (const byte*) DTV_BLITTER_DEST_LO#0 = ((byte*))54064
Constant (const byte*) DTV_BLITTER_DEST_MI#0 = ((byte*))54065
Constant (const byte*) DTV_BLITTER_DEST_HI#0 = ((byte*))54066
Constant (const byte*) DTV_BLITTER_DEST_MOD_LO#0 = ((byte*))54067
Constant (const byte*) DTV_BLITTER_DEST_MOD_HI#0 = ((byte*))54068
Constant (const byte*) DTV_BLITTER_DEST_LIN_LO#0 = ((byte*))54069
Constant (const byte*) DTV_BLITTER_DEST_LIN_HI#0 = ((byte*))54070
Constant (const byte*) DTV_BLITTER_DEST_STEP#0 = ((byte*))54071
Constant (const byte*) DTV_BLITTER_LEN_LO#0 = ((byte*))54072
Constant (const byte*) DTV_BLITTER_LEN_HI#0 = ((byte*))54073
Constant (const byte*) DTV_BLITTER_CONTROL#0 = ((byte*))54074
Constant (const byte) DTV_BLIT_FORCE_START#0 = 1
Constant (const byte) DTV_BLIT_SRCA_FWD#0 = 2
Constant (const byte) DTV_BLIT_SRCB_FWD#0 = 4
Constant (const byte) DTV_BLIT_DEST_FWD#0 = 8
Constant (const byte) DTV_BLIT_VIC_IRQ#0 = 16
Constant (const byte) DTV_BLIT_CIA_IRQ#0 = 32
Constant (const byte) DTV_BLIT_VBLANK#0 = 64
Constant (const byte) DTV_BLIT_IRQ_EN#0 = 128
Constant (const byte*) DTV_BLITTER_TRANSPARANCY#0 = ((byte*))54075
Constant (const byte) DTV_BLIT_DISABLE_B#0 = 1
Constant (const byte) DTV_BLIT_WRITE_TRANSPARENT#0 = 2
Constant (const byte) DTV_BLIT_WRITE_NONTRANSPARENT#0 = 4
Constant (const byte) DTV_BLIT_TRANSPARANCY_NONE#0 = 0
Constant (const byte*) DTV_BLITTER_ALU#0 = ((byte*))54078
Constant (const byte) DTV_BLIT_SHIFT0#0 = 0
Constant (const byte) DTV_BLIT_SHIFT1#0 = 1
Constant (const byte) DTV_BLIT_SHIFT2#0 = 2
Constant (const byte) DTV_BLIT_SHIFT3#0 = 3
Constant (const byte) DTV_BLIT_SHIFT4#0 = 4
Constant (const byte) DTV_BLIT_SHIFT5#0 = 5
Constant (const byte) DTV_BLIT_SHIFT6#0 = 6
Constant (const byte) DTV_BLIT_SHIFT7#0 = 7
Constant (const byte) DTV_BLIT_AND#0 = 0
Constant (const byte) DTV_BLIT_NAND#0 = 8
Constant (const byte) DTV_BLIT_NOR#0 = 16
Constant (const byte) DTV_BLIT_OR#0 = 24
Constant (const byte) DTV_BLIT_XOR#0 = 32
Constant (const byte) DTV_BLIT_XNOR#0 = 40
Constant (const byte) DTV_BLIT_ADD#0 = 48
Constant (const byte) DTV_BLIT_SUB#0 = 56
Constant (const byte*) DTV_BLITTER_CONTROL2#0 = ((byte*))54079
Constant (const byte) DTV_BLIT_CLEAR_IRQ#0 = 1
Constant (const byte) DTV_BLIT_SRCA_CONT#0 = 2
Constant (const byte) DTV_BLIT_SRCB_CONT#0 = 4
Constant (const byte) DTV_BLIT_DEST_CONT#0 = 8
Constant (const byte) DTV_BLIT_STATUS_BUSY#0 = 1
Constant (const byte) DTV_BLIT_STATUS_IRQ#0 = 2
Constant (const byte[16]) main::palette#0 = { 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15 }
Constant (const byte) main::r#0 = 49
Constant (const byte) main::c#0 = 0
Successful SSA optimization Pass2ConstantIdentification
Constant (const byte) main::$0 = DTV_HIGHCOLOR#0|DTV_BORDER_OFF#0
Successful SSA optimization Pass2ConstantIdentification
Constant (const byte) main::$1 = main::$0|DTV_BADLINE_OFF#0
Successful SSA optimization Pass2ConstantIdentification
if() condition always true - replacing block destination [3] if(true) goto main::@4
Successful SSA optimization Pass2ConstantIfs
Successful SSA optimization PassNEliminateUnusedVars
Removing unused block main::@return
Successful SSA optimization Pass2EliminateUnusedBlocks
Resolved ranged next value main::r#1 ← ++ main::r#2 to ++
Resolved ranged comparison value if(main::r#1!=rangelast(49,255)) goto main::@7 to (byte/signed byte/word/signed word/dword/signed dword) 0
Resolved ranged next value main::c#1 ← ++ main::c#2 to ++
Resolved ranged comparison value if(main::c#1!=rangelast(0,15)) goto main::@8 to (byte/signed byte/word/signed word/dword/signed dword) 16
Culled Empty Block (label) @4
Culled Empty Block (label) @5
Culled Empty Block (label) main::@1
Culled Empty Block (label) main::@14
Successful SSA optimization Pass2CullEmptyBlocks
Inlining constant with var siblings (const byte) main::r#0
Inlining constant with var siblings (const byte) main::c#0
Constant inlined main::r#0 = (byte/signed byte/word/signed word/dword/signed dword) 49
Constant inlined main::c#0 = (byte/signed byte/word/signed word/dword/signed dword) 0
Constant inlined main::$1 = (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_BORDER_OFF#0|(const byte) DTV_BADLINE_OFF#0
Constant inlined main::$0 = (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_BORDER_OFF#0
Successful SSA optimization Pass2ConstantInlining
Added new block during phi lifting main::@17(between main::@7 and main::@7)
Added new block during phi lifting main::@18(between main::@8 and main::@8)
Adding NOP phi() at start of @begin
Adding NOP phi() at start of @6
Adding NOP phi() at start of @end
CALL GRAPH
Calls in [] to main:2 

Created 2 initial phi equivalence classes
Coalesced [19] main::c#3 ← main::c#1
Coalesced [20] main::r#3 ← main::r#1
Coalesced down to 2 phi equivalence classes
Culled Empty Block (label) main::@18
Culled Empty Block (label) main::@17
Adding NOP phi() at start of @begin
Adding NOP phi() at start of @6
Adding NOP phi() at start of @end

FINAL CONTROL FLOW GRAPH
@begin: scope:[]  from
  [0] phi()
  to:@6
@6: scope:[]  from @begin
  [1] phi()
  [2] call main 
  to:@end
@end: scope:[]  from @6
  [3] phi()
main: scope:[main]  from @6
  asm { sei  }
  [5] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0
  [6] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_BORDER_OFF#0|(const byte) DTV_BADLINE_OFF#0
  to:main::@4
main::@4: scope:[main]  from main main::@4 main::@8
  [7] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 64) goto main::@4
  to:main::@6
main::@6: scope:[main]  from main::@4
  [8] *((const byte*) BGCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0
  to:main::@7
main::@7: scope:[main]  from main::@6 main::@7
  [9] (byte) main::r#2 ← phi( main::@6/(byte/signed byte/word/signed word/dword/signed dword) 49 main::@7/(byte) main::r#1 )
  asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
  [11] *((const byte*) BGCOL#0) ← ++ *((const byte*) BGCOL#0)
  [12] (byte) main::r#1 ← ++ (byte) main::r#2
  [13] if((byte) main::r#1!=(byte/signed byte/word/signed word/dword/signed dword) 0) goto main::@7
  to:main::@8
main::@8: scope:[main]  from main::@7 main::@8
  [14] (byte) main::c#2 ← phi( main::@7/(byte/signed byte/word/signed word/dword/signed dword) 0 main::@8/(byte) main::c#1 )
  [15] *((const byte*) DTV_PALETTE#0 + (byte) main::c#2) ← *((const byte[16]) main::palette#0 + (byte) main::c#2)
  [16] *((const byte[16]) main::palette#0 + (byte) main::c#2) ← ++ *((const byte[16]) main::palette#0 + (byte) main::c#2)
  [17] (byte) main::c#1 ← ++ (byte) main::c#2
  [18] if((byte) main::c#1!=(byte/signed byte/word/signed word/dword/signed dword) 16) goto main::@8
  to:main::@4


VARIABLE REGISTER WEIGHTS
(byte*) BGCOL
(byte*) BGCOL1
(byte*) BGCOL2
(byte*) BGCOL3
(byte*) BGCOL4
(byte) BLACK
(byte) BLUE
(byte*) BORDERCOL
(byte) BROWN
(byte*) CHARGEN
(byte*) CIA1_INTERRUPT
(byte*) CIA1_PORT_A
(byte*) CIA1_PORT_A_DDR
(byte*) CIA1_PORT_B
(byte*) CIA1_PORT_B_DDR
(byte*) CIA2_INTERRUPT
(byte*) CIA2_PORT_A
(byte*) CIA2_PORT_A_DDR
(byte*) CIA2_PORT_B
(byte*) CIA2_PORT_B_DDR
(byte) CIA_INTERRUPT_CLEAR
(byte*) COLS
(byte) CYAN
(byte*) D011
(byte*) D016
(byte*) D018
(byte) DARK_GREY
(byte) DTV_BADLINE_OFF
(byte*) DTV_BLITTER_ALU
(byte*) DTV_BLITTER_CONTROL
(byte*) DTV_BLITTER_CONTROL2
(byte*) DTV_BLITTER_DEST_HI
(byte*) DTV_BLITTER_DEST_LIN_HI
(byte*) DTV_BLITTER_DEST_LIN_LO
(byte*) DTV_BLITTER_DEST_LO
(byte*) DTV_BLITTER_DEST_MI
(byte*) DTV_BLITTER_DEST_MOD_HI
(byte*) DTV_BLITTER_DEST_MOD_LO
(byte*) DTV_BLITTER_DEST_STEP
(byte*) DTV_BLITTER_LEN_HI
(byte*) DTV_BLITTER_LEN_LO
(byte*) DTV_BLITTER_SRCA_HI
(byte*) DTV_BLITTER_SRCA_LIN_HI
(byte*) DTV_BLITTER_SRCA_LIN_LO
(byte*) DTV_BLITTER_SRCA_LO
(byte*) DTV_BLITTER_SRCA_MI
(byte*) DTV_BLITTER_SRCA_MOD_HI
(byte*) DTV_BLITTER_SRCA_MOD_LO
(byte*) DTV_BLITTER_SRCA_STEP
(byte*) DTV_BLITTER_SRCB_HI
(byte*) DTV_BLITTER_SRCB_LIN_HI
(byte*) DTV_BLITTER_SRCB_LIN_LO
(byte*) DTV_BLITTER_SRCB_LO
(byte*) DTV_BLITTER_SRCB_MI
(byte*) DTV_BLITTER_SRCB_MOD_HI
(byte*) DTV_BLITTER_SRCB_MOD_LO
(byte*) DTV_BLITTER_SRCB_STEP
(byte*) DTV_BLITTER_TRANSPARANCY
(byte) DTV_BLIT_ADD
(byte) DTV_BLIT_AND
(byte) DTV_BLIT_CIA_IRQ
(byte) DTV_BLIT_CLEAR_IRQ
(byte) DTV_BLIT_DEST_CONT
(byte) DTV_BLIT_DEST_FWD
(byte) DTV_BLIT_DISABLE_B
(byte) DTV_BLIT_FORCE_START
(byte) DTV_BLIT_IRQ_EN
(byte) DTV_BLIT_NAND
(byte) DTV_BLIT_NOR
(byte) DTV_BLIT_OR
(byte) DTV_BLIT_SHIFT0
(byte) DTV_BLIT_SHIFT1
(byte) DTV_BLIT_SHIFT2
(byte) DTV_BLIT_SHIFT3
(byte) DTV_BLIT_SHIFT4
(byte) DTV_BLIT_SHIFT5
(byte) DTV_BLIT_SHIFT6
(byte) DTV_BLIT_SHIFT7
(byte) DTV_BLIT_SRCA_CONT
(byte) DTV_BLIT_SRCA_FWD
(byte) DTV_BLIT_SRCB_CONT
(byte) DTV_BLIT_SRCB_FWD
(byte) DTV_BLIT_STATUS_BUSY
(byte) DTV_BLIT_STATUS_IRQ
(byte) DTV_BLIT_SUB
(byte) DTV_BLIT_TRANSPARANCY_NONE
(byte) DTV_BLIT_VBLANK
(byte) DTV_BLIT_VIC_IRQ
(byte) DTV_BLIT_WRITE_NONTRANSPARENT
(byte) DTV_BLIT_WRITE_TRANSPARENT
(byte) DTV_BLIT_XNOR
(byte) DTV_BLIT_XOR
(byte) DTV_BORDER_OFF
(byte) DTV_CHUNKY
(byte) DTV_COLORRAM_OFF
(dword) DTV_COLOR_BANK_DEFAULT
(byte*) DTV_COLOR_BANK_HI
(byte*) DTV_COLOR_BANK_LO
(byte*) DTV_CONTROL
(byte*) DTV_FEATURE
(byte) DTV_FEATURE_DISABLE_TIL_RESET
(byte) DTV_FEATURE_ENABLE
(byte*) DTV_GRAPHICS_HICOL_BANK
(byte*) DTV_GRAPHICS_VIC_BANK
(byte) DTV_HIGHCOLOR
(byte) DTV_LINEAR
(byte) DTV_OVERSCAN
(byte*) DTV_PALETTE
(byte[16]) DTV_PALETTE_DEFAULT
(byte*) DTV_PLANEA_MODULO_HI
(byte*) DTV_PLANEA_MODULO_LO
(byte*) DTV_PLANEA_START_HI
(byte*) DTV_PLANEA_START_LO
(byte*) DTV_PLANEA_START_MI
(byte*) DTV_PLANEA_STEP
(byte*) DTV_PLANEB_MODULO_HI
(byte*) DTV_PLANEB_MODULO_LO
(byte*) DTV_PLANEB_START_HI
(byte*) DTV_PLANEB_START_LO
(byte*) DTV_PLANEB_START_MI
(byte*) DTV_PLANEB_STEP
(byte*) DTV_SPRITE_BANK
(byte) GREEN
(byte) GREY
(void()**) HARDWARE_IRQ
(byte) IRQ_COLLISION_BG
(byte) IRQ_COLLISION_SPRITE
(byte*) IRQ_ENABLE
(byte) IRQ_LIGHTPEN
(byte) IRQ_RASTER
(byte*) IRQ_STATUS
(void()**) KERNEL_IRQ
(byte*) LIGHTPEN_X
(byte*) LIGHTPEN_Y
(byte) LIGHT_BLUE
(byte) LIGHT_GREEN
(byte) LIGHT_GREY
(byte) ORANGE
(byte) PINK
(byte*) PROCPORT
(byte) PROCPORT_BASIC_KERNEL_IO
(byte*) PROCPORT_DDR
(byte) PROCPORT_DDR_MEMORY_MASK
(byte) PROCPORT_KERNEL_IO
(byte) PROCPORT_RAM_ALL
(byte) PROCPORT_RAM_CHARROM
(byte) PROCPORT_RAM_IO
(byte) PURPLE
(byte*) RASTER
(byte) RED
(byte*) SPRITES_COLS
(byte*) SPRITES_ENABLE
(byte*) SPRITES_EXPAND_X
(byte*) SPRITES_EXPAND_Y
(byte*) SPRITES_MC
(byte*) SPRITES_MC1
(byte*) SPRITES_MC2
(byte*) SPRITES_PRIORITY
(byte*) SPRITES_XMSB
(byte*) SPRITES_XPOS
(byte*) SPRITES_YPOS
(word) SPRITE_PTRS
(byte) VIC_BMM
(byte*) VIC_CONTROL
(byte*) VIC_CONTROL2
(byte) VIC_CSEL
(byte) VIC_DEN
(byte) VIC_ECM
(byte) VIC_MCM
(byte*) VIC_MEMORY
(byte) VIC_RSEL
(byte) VIC_RST8
(byte) WHITE
(byte) YELLOW
(void()) main()
(byte) main::c
(byte) main::c#1 151.5
(byte) main::c#2 201.99999999999997
(byte[16]) main::palette
(byte) main::r
(byte) main::r#1 151.5
(byte) main::r#2 67.33333333333333

Initial phi equivalence classes
[ main::r#2 main::r#1 ]
[ main::c#2 main::c#1 ]
Complete equivalence classes
[ main::r#2 main::r#1 ]
[ main::c#2 main::c#1 ]
Allocated zp ZP_BYTE:2 [ main::r#2 main::r#1 ]
Allocated zp ZP_BYTE:3 [ main::c#2 main::c#1 ]

INITIAL ASM
//SEG0 File Comments
// Test C64DTV v2 256-colors and the 16-color redefinable palette
//SEG1 Basic Upstart
.pc = $801 "Basic"
:BasicUpstart(bbegin)
.pc = $80d "Program"
//SEG2 Global Constants & labels
  .label RASTER = $d012
  .label BGCOL = $d021
  // Feature enables or disables the extra C64 DTV features
  .label DTV_FEATURE = $d03f
  .const DTV_FEATURE_ENABLE = 1
  // Controls the graphics modes of the C64 DTV
  .label DTV_CONTROL = $d03c
  .const DTV_BORDER_OFF = 2
  .const DTV_HIGHCOLOR = 4
  .const DTV_BADLINE_OFF = $20
  // Defines colors for the 16 first colors ($00-$0f)
  .label DTV_PALETTE = $d200
//SEG3 @begin
bbegin:
//SEG4 [1] phi from @begin to @6 [phi:@begin->@6]
b6_from_bbegin:
  jmp b6
//SEG5 @6
b6:
//SEG6 [2] call main 
  jsr main
//SEG7 [3] phi from @6 to @end [phi:@6->@end]
bend_from_b6:
  jmp bend
//SEG8 @end
bend:
//SEG9 main
main: {
    .label r = 2
    .label c = 3
  //SEG10 asm { sei  }
    sei
  //SEG11 [5] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 -- _deref_pbuc1=vbuc2 
    lda #DTV_FEATURE_ENABLE
    sta DTV_FEATURE
  //SEG12 [6] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_BORDER_OFF#0|(const byte) DTV_BADLINE_OFF#0 -- _deref_pbuc1=vbuc2 
    lda #DTV_HIGHCOLOR|DTV_BORDER_OFF|DTV_BADLINE_OFF
    sta DTV_CONTROL
    jmp b4
  //SEG13 main::@4
  b4:
  //SEG14 [7] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 64) goto main::@4 -- _deref_pbuc1_neq_vbuc2_then_la1 
    lda RASTER
    cmp #$40
    bne b4
    jmp b6
  //SEG15 main::@6
  b6:
  //SEG16 [8] *((const byte*) BGCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    // Create rasterbars
    lda #0
    sta BGCOL
  //SEG17 [9] phi from main::@6 to main::@7 [phi:main::@6->main::@7]
  b7_from_b6:
  //SEG18 [9] phi (byte) main::r#2 = (byte/signed byte/word/signed word/dword/signed dword) 49 [phi:main::@6->main::@7#0] -- vbuz1=vbuc1 
    lda #$31
    sta r
    jmp b7
  //SEG19 [9] phi from main::@7 to main::@7 [phi:main::@7->main::@7]
  b7_from_b7:
  //SEG20 [9] phi (byte) main::r#2 = (byte) main::r#1 [phi:main::@7->main::@7#0] -- register_copy 
    jmp b7
  //SEG21 main::@7
  b7:
  //SEG22 asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
  //SEG23 [11] *((const byte*) BGCOL#0) ← ++ *((const byte*) BGCOL#0) -- _deref_pbuc1=_inc__deref_pbuc1 
    inc BGCOL
  //SEG24 [12] (byte) main::r#1 ← ++ (byte) main::r#2 -- vbuz1=_inc_vbuz1 
    inc r
  //SEG25 [13] if((byte) main::r#1!=(byte/signed byte/word/signed word/dword/signed dword) 0) goto main::@7 -- vbuz1_neq_0_then_la1 
    lda r
    cmp #0
    bne b7_from_b7
  //SEG26 [14] phi from main::@7 to main::@8 [phi:main::@7->main::@8]
  b8_from_b7:
  //SEG27 [14] phi (byte) main::c#2 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:main::@7->main::@8#0] -- vbuz1=vbuc1 
    lda #0
    sta c
    jmp b8
  // Rotate palette
  //SEG28 [14] phi from main::@8 to main::@8 [phi:main::@8->main::@8]
  b8_from_b8:
  //SEG29 [14] phi (byte) main::c#2 = (byte) main::c#1 [phi:main::@8->main::@8#0] -- register_copy 
    jmp b8
  //SEG30 main::@8
  b8:
  //SEG31 [15] *((const byte*) DTV_PALETTE#0 + (byte) main::c#2) ← *((const byte[16]) main::palette#0 + (byte) main::c#2) -- pbuc1_derefidx_vbuz1=pbuc2_derefidx_vbuz1 
    ldy c
    lda palette,y
    sta DTV_PALETTE,y
  //SEG32 [16] *((const byte[16]) main::palette#0 + (byte) main::c#2) ← ++ *((const byte[16]) main::palette#0 + (byte) main::c#2) -- pbuc1_derefidx_vbuz1=_inc_pbuc1_derefidx_vbuz1 
    ldx c
    inc palette,x
  //SEG33 [17] (byte) main::c#1 ← ++ (byte) main::c#2 -- vbuz1=_inc_vbuz1 
    inc c
  //SEG34 [18] if((byte) main::c#1!=(byte/signed byte/word/signed word/dword/signed dword) 16) goto main::@8 -- vbuz1_neq_vbuc1_then_la1 
    lda c
    cmp #$10
    bne b8_from_b8
    jmp b4
    palette: .byte 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, $a, $b, $c, $d, $e, $f
}

REGISTER UPLIFT POTENTIAL REGISTERS
Statement [5] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [6] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_BORDER_OFF#0|(const byte) DTV_BADLINE_OFF#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [7] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 64) goto main::@4 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [8] *((const byte*) BGCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [15] *((const byte*) DTV_PALETTE#0 + (byte) main::c#2) ← *((const byte[16]) main::palette#0 + (byte) main::c#2) [ main::c#2 ] ( main:2 [ main::c#2 ] ) always clobbers reg byte a 
Removing always clobbered register reg byte a as potential for zp ZP_BYTE:3 [ main::c#2 main::c#1 ]
Statement [5] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [6] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_BORDER_OFF#0|(const byte) DTV_BADLINE_OFF#0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [7] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 64) goto main::@4 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [8] *((const byte*) BGCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 [ ] ( main:2 [ ] ) always clobbers reg byte a 
Statement [15] *((const byte*) DTV_PALETTE#0 + (byte) main::c#2) ← *((const byte[16]) main::palette#0 + (byte) main::c#2) [ main::c#2 ] ( main:2 [ main::c#2 ] ) always clobbers reg byte a 
Potential registers zp ZP_BYTE:2 [ main::r#2 main::r#1 ] : zp ZP_BYTE:2 , reg byte a , reg byte x , reg byte y , 
Potential registers zp ZP_BYTE:3 [ main::c#2 main::c#1 ] : zp ZP_BYTE:3 , reg byte x , reg byte y , 

REGISTER UPLIFT SCOPES
Uplift Scope [main] 353.5: zp ZP_BYTE:3 [ main::c#2 main::c#1 ] 218.83: zp ZP_BYTE:2 [ main::r#2 main::r#1 ] 
Uplift Scope [] 

Uplifting [main] best 11689 combination reg byte x [ main::c#2 main::c#1 ] reg byte x [ main::r#2 main::r#1 ] 
Uplifting [] best 11689 combination 

ASSEMBLER BEFORE OPTIMIZATION
//SEG0 File Comments
// Test C64DTV v2 256-colors and the 16-color redefinable palette
//SEG1 Basic Upstart
.pc = $801 "Basic"
:BasicUpstart(bbegin)
.pc = $80d "Program"
//SEG2 Global Constants & labels
  .label RASTER = $d012
  .label BGCOL = $d021
  // Feature enables or disables the extra C64 DTV features
  .label DTV_FEATURE = $d03f
  .const DTV_FEATURE_ENABLE = 1
  // Controls the graphics modes of the C64 DTV
  .label DTV_CONTROL = $d03c
  .const DTV_BORDER_OFF = 2
  .const DTV_HIGHCOLOR = 4
  .const DTV_BADLINE_OFF = $20
  // Defines colors for the 16 first colors ($00-$0f)
  .label DTV_PALETTE = $d200
//SEG3 @begin
bbegin:
//SEG4 [1] phi from @begin to @6 [phi:@begin->@6]
b6_from_bbegin:
  jmp b6
//SEG5 @6
b6:
//SEG6 [2] call main 
  jsr main
//SEG7 [3] phi from @6 to @end [phi:@6->@end]
bend_from_b6:
  jmp bend
//SEG8 @end
bend:
//SEG9 main
main: {
  //SEG10 asm { sei  }
    sei
  //SEG11 [5] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 -- _deref_pbuc1=vbuc2 
    lda #DTV_FEATURE_ENABLE
    sta DTV_FEATURE
  //SEG12 [6] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_BORDER_OFF#0|(const byte) DTV_BADLINE_OFF#0 -- _deref_pbuc1=vbuc2 
    lda #DTV_HIGHCOLOR|DTV_BORDER_OFF|DTV_BADLINE_OFF
    sta DTV_CONTROL
    jmp b4
  //SEG13 main::@4
  b4:
  //SEG14 [7] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 64) goto main::@4 -- _deref_pbuc1_neq_vbuc2_then_la1 
    lda RASTER
    cmp #$40
    bne b4
    jmp b6
  //SEG15 main::@6
  b6:
  //SEG16 [8] *((const byte*) BGCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    // Create rasterbars
    lda #0
    sta BGCOL
  //SEG17 [9] phi from main::@6 to main::@7 [phi:main::@6->main::@7]
  b7_from_b6:
  //SEG18 [9] phi (byte) main::r#2 = (byte/signed byte/word/signed word/dword/signed dword) 49 [phi:main::@6->main::@7#0] -- vbuxx=vbuc1 
    ldx #$31
    jmp b7
  //SEG19 [9] phi from main::@7 to main::@7 [phi:main::@7->main::@7]
  b7_from_b7:
  //SEG20 [9] phi (byte) main::r#2 = (byte) main::r#1 [phi:main::@7->main::@7#0] -- register_copy 
    jmp b7
  //SEG21 main::@7
  b7:
  //SEG22 asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
  //SEG23 [11] *((const byte*) BGCOL#0) ← ++ *((const byte*) BGCOL#0) -- _deref_pbuc1=_inc__deref_pbuc1 
    inc BGCOL
  //SEG24 [12] (byte) main::r#1 ← ++ (byte) main::r#2 -- vbuxx=_inc_vbuxx 
    inx
  //SEG25 [13] if((byte) main::r#1!=(byte/signed byte/word/signed word/dword/signed dword) 0) goto main::@7 -- vbuxx_neq_0_then_la1 
    cpx #0
    bne b7_from_b7
  //SEG26 [14] phi from main::@7 to main::@8 [phi:main::@7->main::@8]
  b8_from_b7:
  //SEG27 [14] phi (byte) main::c#2 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:main::@7->main::@8#0] -- vbuxx=vbuc1 
    ldx #0
    jmp b8
  // Rotate palette
  //SEG28 [14] phi from main::@8 to main::@8 [phi:main::@8->main::@8]
  b8_from_b8:
  //SEG29 [14] phi (byte) main::c#2 = (byte) main::c#1 [phi:main::@8->main::@8#0] -- register_copy 
    jmp b8
  //SEG30 main::@8
  b8:
  //SEG31 [15] *((const byte*) DTV_PALETTE#0 + (byte) main::c#2) ← *((const byte[16]) main::palette#0 + (byte) main::c#2) -- pbuc1_derefidx_vbuxx=pbuc2_derefidx_vbuxx 
    lda palette,x
    sta DTV_PALETTE,x
  //SEG32 [16] *((const byte[16]) main::palette#0 + (byte) main::c#2) ← ++ *((const byte[16]) main::palette#0 + (byte) main::c#2) -- pbuc1_derefidx_vbuxx=_inc_pbuc1_derefidx_vbuxx 
    inc palette,x
  //SEG33 [17] (byte) main::c#1 ← ++ (byte) main::c#2 -- vbuxx=_inc_vbuxx 
    inx
  //SEG34 [18] if((byte) main::c#1!=(byte/signed byte/word/signed word/dword/signed dword) 16) goto main::@8 -- vbuxx_neq_vbuc1_then_la1 
    cpx #$10
    bne b8_from_b8
    jmp b4
    palette: .byte 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, $a, $b, $c, $d, $e, $f
}

ASSEMBLER OPTIMIZATIONS
Removing instruction jmp b6
Removing instruction jmp bend
Removing instruction jmp b4
Removing instruction jmp b6
Removing instruction jmp b7
Removing instruction jmp b8
Succesful ASM optimization Pass5NextJumpElimination
Replacing label b7_from_b7 with b7
Replacing label b8_from_b8 with b8
Removing instruction b6_from_bbegin:
Removing instruction b6:
Removing instruction bend_from_b6:
Removing instruction b7_from_b7:
Removing instruction b8_from_b8:
Succesful ASM optimization Pass5RedundantLabelElimination
Removing instruction bend:
Removing instruction b6:
Removing instruction b7_from_b6:
Removing instruction b8_from_b7:
Succesful ASM optimization Pass5UnusedLabelElimination
Updating BasicUpstart to call main directly
Removing instruction jsr main
Succesful ASM optimization Pass5SkipBegin
Removing instruction jmp b7
Removing instruction jmp b8
Succesful ASM optimization Pass5NextJumpElimination
Removing instruction bbegin:
Succesful ASM optimization Pass5UnusedLabelElimination

FINAL SYMBOL TABLE
(label) @6
(label) @begin
(label) @end
(byte*) BGCOL
(const byte*) BGCOL#0 BGCOL = ((byte*))(word/dword/signed dword) 53281
(byte*) BGCOL1
(byte*) BGCOL2
(byte*) BGCOL3
(byte*) BGCOL4
(byte) BLACK
(byte) BLUE
(byte*) BORDERCOL
(byte) BROWN
(byte*) CHARGEN
(byte*) CIA1_INTERRUPT
(byte*) CIA1_PORT_A
(byte*) CIA1_PORT_A_DDR
(byte*) CIA1_PORT_B
(byte*) CIA1_PORT_B_DDR
(byte*) CIA2_INTERRUPT
(byte*) CIA2_PORT_A
(byte*) CIA2_PORT_A_DDR
(byte*) CIA2_PORT_B
(byte*) CIA2_PORT_B_DDR
(byte) CIA_INTERRUPT_CLEAR
(byte*) COLS
(byte) CYAN
(byte*) D011
(byte*) D016
(byte*) D018
(byte) DARK_GREY
(byte) DTV_BADLINE_OFF
(const byte) DTV_BADLINE_OFF#0 DTV_BADLINE_OFF = (byte/signed byte/word/signed word/dword/signed dword) 32
(byte*) DTV_BLITTER_ALU
(byte*) DTV_BLITTER_CONTROL
(byte*) DTV_BLITTER_CONTROL2
(byte*) DTV_BLITTER_DEST_HI
(byte*) DTV_BLITTER_DEST_LIN_HI
(byte*) DTV_BLITTER_DEST_LIN_LO
(byte*) DTV_BLITTER_DEST_LO
(byte*) DTV_BLITTER_DEST_MI
(byte*) DTV_BLITTER_DEST_MOD_HI
(byte*) DTV_BLITTER_DEST_MOD_LO
(byte*) DTV_BLITTER_DEST_STEP
(byte*) DTV_BLITTER_LEN_HI
(byte*) DTV_BLITTER_LEN_LO
(byte*) DTV_BLITTER_SRCA_HI
(byte*) DTV_BLITTER_SRCA_LIN_HI
(byte*) DTV_BLITTER_SRCA_LIN_LO
(byte*) DTV_BLITTER_SRCA_LO
(byte*) DTV_BLITTER_SRCA_MI
(byte*) DTV_BLITTER_SRCA_MOD_HI
(byte*) DTV_BLITTER_SRCA_MOD_LO
(byte*) DTV_BLITTER_SRCA_STEP
(byte*) DTV_BLITTER_SRCB_HI
(byte*) DTV_BLITTER_SRCB_LIN_HI
(byte*) DTV_BLITTER_SRCB_LIN_LO
(byte*) DTV_BLITTER_SRCB_LO
(byte*) DTV_BLITTER_SRCB_MI
(byte*) DTV_BLITTER_SRCB_MOD_HI
(byte*) DTV_BLITTER_SRCB_MOD_LO
(byte*) DTV_BLITTER_SRCB_STEP
(byte*) DTV_BLITTER_TRANSPARANCY
(byte) DTV_BLIT_ADD
(byte) DTV_BLIT_AND
(byte) DTV_BLIT_CIA_IRQ
(byte) DTV_BLIT_CLEAR_IRQ
(byte) DTV_BLIT_DEST_CONT
(byte) DTV_BLIT_DEST_FWD
(byte) DTV_BLIT_DISABLE_B
(byte) DTV_BLIT_FORCE_START
(byte) DTV_BLIT_IRQ_EN
(byte) DTV_BLIT_NAND
(byte) DTV_BLIT_NOR
(byte) DTV_BLIT_OR
(byte) DTV_BLIT_SHIFT0
(byte) DTV_BLIT_SHIFT1
(byte) DTV_BLIT_SHIFT2
(byte) DTV_BLIT_SHIFT3
(byte) DTV_BLIT_SHIFT4
(byte) DTV_BLIT_SHIFT5
(byte) DTV_BLIT_SHIFT6
(byte) DTV_BLIT_SHIFT7
(byte) DTV_BLIT_SRCA_CONT
(byte) DTV_BLIT_SRCA_FWD
(byte) DTV_BLIT_SRCB_CONT
(byte) DTV_BLIT_SRCB_FWD
(byte) DTV_BLIT_STATUS_BUSY
(byte) DTV_BLIT_STATUS_IRQ
(byte) DTV_BLIT_SUB
(byte) DTV_BLIT_TRANSPARANCY_NONE
(byte) DTV_BLIT_VBLANK
(byte) DTV_BLIT_VIC_IRQ
(byte) DTV_BLIT_WRITE_NONTRANSPARENT
(byte) DTV_BLIT_WRITE_TRANSPARENT
(byte) DTV_BLIT_XNOR
(byte) DTV_BLIT_XOR
(byte) DTV_BORDER_OFF
(const byte) DTV_BORDER_OFF#0 DTV_BORDER_OFF = (byte/signed byte/word/signed word/dword/signed dword) 2
(byte) DTV_CHUNKY
(byte) DTV_COLORRAM_OFF
(dword) DTV_COLOR_BANK_DEFAULT
(byte*) DTV_COLOR_BANK_HI
(byte*) DTV_COLOR_BANK_LO
(byte*) DTV_CONTROL
(const byte*) DTV_CONTROL#0 DTV_CONTROL = ((byte*))(word/dword/signed dword) 53308
(byte*) DTV_FEATURE
(const byte*) DTV_FEATURE#0 DTV_FEATURE = ((byte*))(word/dword/signed dword) 53311
(byte) DTV_FEATURE_DISABLE_TIL_RESET
(byte) DTV_FEATURE_ENABLE
(const byte) DTV_FEATURE_ENABLE#0 DTV_FEATURE_ENABLE = (byte/signed byte/word/signed word/dword/signed dword) 1
(byte*) DTV_GRAPHICS_HICOL_BANK
(byte*) DTV_GRAPHICS_VIC_BANK
(byte) DTV_HIGHCOLOR
(const byte) DTV_HIGHCOLOR#0 DTV_HIGHCOLOR = (byte/signed byte/word/signed word/dword/signed dword) 4
(byte) DTV_LINEAR
(byte) DTV_OVERSCAN
(byte*) DTV_PALETTE
(const byte*) DTV_PALETTE#0 DTV_PALETTE = ((byte*))(word/dword/signed dword) 53760
(byte[16]) DTV_PALETTE_DEFAULT
(byte*) DTV_PLANEA_MODULO_HI
(byte*) DTV_PLANEA_MODULO_LO
(byte*) DTV_PLANEA_START_HI
(byte*) DTV_PLANEA_START_LO
(byte*) DTV_PLANEA_START_MI
(byte*) DTV_PLANEA_STEP
(byte*) DTV_PLANEB_MODULO_HI
(byte*) DTV_PLANEB_MODULO_LO
(byte*) DTV_PLANEB_START_HI
(byte*) DTV_PLANEB_START_LO
(byte*) DTV_PLANEB_START_MI
(byte*) DTV_PLANEB_STEP
(byte*) DTV_SPRITE_BANK
(byte) GREEN
(byte) GREY
(void()**) HARDWARE_IRQ
(byte) IRQ_COLLISION_BG
(byte) IRQ_COLLISION_SPRITE
(byte*) IRQ_ENABLE
(byte) IRQ_LIGHTPEN
(byte) IRQ_RASTER
(byte*) IRQ_STATUS
(void()**) KERNEL_IRQ
(byte*) LIGHTPEN_X
(byte*) LIGHTPEN_Y
(byte) LIGHT_BLUE
(byte) LIGHT_GREEN
(byte) LIGHT_GREY
(byte) ORANGE
(byte) PINK
(byte*) PROCPORT
(byte) PROCPORT_BASIC_KERNEL_IO
(byte*) PROCPORT_DDR
(byte) PROCPORT_DDR_MEMORY_MASK
(byte) PROCPORT_KERNEL_IO
(byte) PROCPORT_RAM_ALL
(byte) PROCPORT_RAM_CHARROM
(byte) PROCPORT_RAM_IO
(byte) PURPLE
(byte*) RASTER
(const byte*) RASTER#0 RASTER = ((byte*))(word/dword/signed dword) 53266
(byte) RED
(byte*) SPRITES_COLS
(byte*) SPRITES_ENABLE
(byte*) SPRITES_EXPAND_X
(byte*) SPRITES_EXPAND_Y
(byte*) SPRITES_MC
(byte*) SPRITES_MC1
(byte*) SPRITES_MC2
(byte*) SPRITES_PRIORITY
(byte*) SPRITES_XMSB
(byte*) SPRITES_XPOS
(byte*) SPRITES_YPOS
(word) SPRITE_PTRS
(byte) VIC_BMM
(byte*) VIC_CONTROL
(byte*) VIC_CONTROL2
(byte) VIC_CSEL
(byte) VIC_DEN
(byte) VIC_ECM
(byte) VIC_MCM
(byte*) VIC_MEMORY
(byte) VIC_RSEL
(byte) VIC_RST8
(byte) WHITE
(byte) YELLOW
(void()) main()
(label) main::@4
(label) main::@6
(label) main::@7
(label) main::@8
(byte) main::c
(byte) main::c#1 reg byte x 151.5
(byte) main::c#2 reg byte x 201.99999999999997
(byte[16]) main::palette
(const byte[16]) main::palette#0 palette = { (byte/signed byte/word/signed word/dword/signed dword) 0, (byte/signed byte/word/signed word/dword/signed dword) 1, (byte/signed byte/word/signed word/dword/signed dword) 2, (byte/signed byte/word/signed word/dword/signed dword) 3, (byte/signed byte/word/signed word/dword/signed dword) 4, (byte/signed byte/word/signed word/dword/signed dword) 5, (byte/signed byte/word/signed word/dword/signed dword) 6, (byte/signed byte/word/signed word/dword/signed dword) 7, (byte/signed byte/word/signed word/dword/signed dword) 8, (byte/signed byte/word/signed word/dword/signed dword) 9, (byte/signed byte/word/signed word/dword/signed dword) 10, (byte/signed byte/word/signed word/dword/signed dword) 11, (byte/signed byte/word/signed word/dword/signed dword) 12, (byte/signed byte/word/signed word/dword/signed dword) 13, (byte/signed byte/word/signed word/dword/signed dword) 14, (byte/signed byte/word/signed word/dword/signed dword) 15 }
(byte) main::r
(byte) main::r#1 reg byte x 151.5
(byte) main::r#2 reg byte x 67.33333333333333

reg byte x [ main::r#2 main::r#1 ]
reg byte x [ main::c#2 main::c#1 ]


FINAL ASSEMBLER
Score: 10174

//SEG0 File Comments
// Test C64DTV v2 256-colors and the 16-color redefinable palette
//SEG1 Basic Upstart
.pc = $801 "Basic"
:BasicUpstart(main)
.pc = $80d "Program"
//SEG2 Global Constants & labels
  .label RASTER = $d012
  .label BGCOL = $d021
  // Feature enables or disables the extra C64 DTV features
  .label DTV_FEATURE = $d03f
  .const DTV_FEATURE_ENABLE = 1
  // Controls the graphics modes of the C64 DTV
  .label DTV_CONTROL = $d03c
  .const DTV_BORDER_OFF = 2
  .const DTV_HIGHCOLOR = 4
  .const DTV_BADLINE_OFF = $20
  // Defines colors for the 16 first colors ($00-$0f)
  .label DTV_PALETTE = $d200
//SEG3 @begin
//SEG4 [1] phi from @begin to @6 [phi:@begin->@6]
//SEG5 @6
//SEG6 [2] call main 
//SEG7 [3] phi from @6 to @end [phi:@6->@end]
//SEG8 @end
//SEG9 main
main: {
  //SEG10 asm { sei  }
    sei
  //SEG11 [5] *((const byte*) DTV_FEATURE#0) ← (const byte) DTV_FEATURE_ENABLE#0 -- _deref_pbuc1=vbuc2 
    lda #DTV_FEATURE_ENABLE
    sta DTV_FEATURE
  //SEG12 [6] *((const byte*) DTV_CONTROL#0) ← (const byte) DTV_HIGHCOLOR#0|(const byte) DTV_BORDER_OFF#0|(const byte) DTV_BADLINE_OFF#0 -- _deref_pbuc1=vbuc2 
    lda #DTV_HIGHCOLOR|DTV_BORDER_OFF|DTV_BADLINE_OFF
    sta DTV_CONTROL
  //SEG13 main::@4
  b4:
  //SEG14 [7] if(*((const byte*) RASTER#0)!=(byte/signed byte/word/signed word/dword/signed dword) 64) goto main::@4 -- _deref_pbuc1_neq_vbuc2_then_la1 
    lda RASTER
    cmp #$40
    bne b4
  //SEG15 main::@6
  //SEG16 [8] *((const byte*) BGCOL#0) ← (byte/signed byte/word/signed word/dword/signed dword) 0 -- _deref_pbuc1=vbuc2 
    // Create rasterbars
    lda #0
    sta BGCOL
  //SEG17 [9] phi from main::@6 to main::@7 [phi:main::@6->main::@7]
  //SEG18 [9] phi (byte) main::r#2 = (byte/signed byte/word/signed word/dword/signed dword) 49 [phi:main::@6->main::@7#0] -- vbuxx=vbuc1 
    ldx #$31
  //SEG19 [9] phi from main::@7 to main::@7 [phi:main::@7->main::@7]
  //SEG20 [9] phi (byte) main::r#2 = (byte) main::r#1 [phi:main::@7->main::@7#0] -- register_copy 
  //SEG21 main::@7
  b7:
  //SEG22 asm { nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop nop  }
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
    nop
  //SEG23 [11] *((const byte*) BGCOL#0) ← ++ *((const byte*) BGCOL#0) -- _deref_pbuc1=_inc__deref_pbuc1 
    inc BGCOL
  //SEG24 [12] (byte) main::r#1 ← ++ (byte) main::r#2 -- vbuxx=_inc_vbuxx 
    inx
  //SEG25 [13] if((byte) main::r#1!=(byte/signed byte/word/signed word/dword/signed dword) 0) goto main::@7 -- vbuxx_neq_0_then_la1 
    cpx #0
    bne b7
  //SEG26 [14] phi from main::@7 to main::@8 [phi:main::@7->main::@8]
  //SEG27 [14] phi (byte) main::c#2 = (byte/signed byte/word/signed word/dword/signed dword) 0 [phi:main::@7->main::@8#0] -- vbuxx=vbuc1 
    ldx #0
  // Rotate palette
  //SEG28 [14] phi from main::@8 to main::@8 [phi:main::@8->main::@8]
  //SEG29 [14] phi (byte) main::c#2 = (byte) main::c#1 [phi:main::@8->main::@8#0] -- register_copy 
  //SEG30 main::@8
  b8:
  //SEG31 [15] *((const byte*) DTV_PALETTE#0 + (byte) main::c#2) ← *((const byte[16]) main::palette#0 + (byte) main::c#2) -- pbuc1_derefidx_vbuxx=pbuc2_derefidx_vbuxx 
    lda palette,x
    sta DTV_PALETTE,x
  //SEG32 [16] *((const byte[16]) main::palette#0 + (byte) main::c#2) ← ++ *((const byte[16]) main::palette#0 + (byte) main::c#2) -- pbuc1_derefidx_vbuxx=_inc_pbuc1_derefidx_vbuxx 
    inc palette,x
  //SEG33 [17] (byte) main::c#1 ← ++ (byte) main::c#2 -- vbuxx=_inc_vbuxx 
    inx
  //SEG34 [18] if((byte) main::c#1!=(byte/signed byte/word/signed word/dword/signed dword) 16) goto main::@8 -- vbuxx_neq_vbuc1_then_la1 
    cpx #$10
    bne b8
    jmp b4
    palette: .byte 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, $a, $b, $c, $d, $e, $f
}

