(label) @7
(label) @begin
(label) @end
(byte*) BGCOL
(byte*) BGCOL1
(byte*) BGCOL2
(byte*) BGCOL3
(byte*) BGCOL4
(byte) BLACK
(byte) BLUE
(byte*) BORDERCOL
(const byte*) BORDERCOL#0 BORDERCOL = ((byte*))(word/dword/signed dword) 53280
(byte) BROWN
(byte*) CHARGEN
(byte*) CHUNKY
(const byte*) CHUNKY#0 CHUNKY = ((byte*))(word/dword/signed dword) 32768
(byte*) CIA1_INTERRUPT
(byte*) CIA1_PORT_A
(byte*) CIA1_PORT_A_DDR
(byte*) CIA1_PORT_B
(byte*) CIA1_PORT_B_DDR
(byte*) CIA2_INTERRUPT
(byte*) CIA2_PORT_A
(const byte*) CIA2_PORT_A#0 CIA2_PORT_A = ((byte*))(word/dword/signed dword) 56576
(byte*) CIA2_PORT_A_DDR
(const byte*) CIA2_PORT_A_DDR#0 CIA2_PORT_A_DDR = ((byte*))(word/dword/signed dword) 56578
(byte*) CIA2_PORT_B
(byte*) CIA2_PORT_B_DDR
(byte) CIA_INTERRUPT_CLEAR
(byte*) COLS
(byte) CYAN
(byte*) D011
(byte*) D016
(byte*) D018
(byte) DARK_GREY
(byte) DTV_BADLINE_OFF
(const byte) DTV_BADLINE_OFF#0 DTV_BADLINE_OFF = (byte/signed byte/word/signed word/dword/signed dword) 32
(byte*) DTV_BLITTER_ALU
(byte*) DTV_BLITTER_CONTROL
(byte*) DTV_BLITTER_CONTROL2
(byte*) DTV_BLITTER_DEST_HI
(byte*) DTV_BLITTER_DEST_LIN_HI
(byte*) DTV_BLITTER_DEST_LIN_LO
(byte*) DTV_BLITTER_DEST_LO
(byte*) DTV_BLITTER_DEST_MI
(byte*) DTV_BLITTER_DEST_MOD_HI
(byte*) DTV_BLITTER_DEST_MOD_LO
(byte*) DTV_BLITTER_DEST_STEP
(byte*) DTV_BLITTER_LEN_HI
(byte*) DTV_BLITTER_LEN_LO
(byte*) DTV_BLITTER_SRCA_HI
(byte*) DTV_BLITTER_SRCA_LIN_HI
(byte*) DTV_BLITTER_SRCA_LIN_LO
(byte*) DTV_BLITTER_SRCA_LO
(byte*) DTV_BLITTER_SRCA_MI
(byte*) DTV_BLITTER_SRCA_MOD_HI
(byte*) DTV_BLITTER_SRCA_MOD_LO
(byte*) DTV_BLITTER_SRCA_STEP
(byte*) DTV_BLITTER_SRCB_HI
(byte*) DTV_BLITTER_SRCB_LIN_HI
(byte*) DTV_BLITTER_SRCB_LIN_LO
(byte*) DTV_BLITTER_SRCB_LO
(byte*) DTV_BLITTER_SRCB_MI
(byte*) DTV_BLITTER_SRCB_MOD_HI
(byte*) DTV_BLITTER_SRCB_MOD_LO
(byte*) DTV_BLITTER_SRCB_STEP
(byte*) DTV_BLITTER_TRANSPARANCY
(byte) DTV_BLIT_ADD
(byte) DTV_BLIT_AND
(byte) DTV_BLIT_CIA_IRQ
(byte) DTV_BLIT_CLEAR_IRQ
(byte) DTV_BLIT_DEST_CONT
(byte) DTV_BLIT_DEST_FWD
(byte) DTV_BLIT_DISABLE_B
(byte) DTV_BLIT_FORCE_START
(byte) DTV_BLIT_IRQ_EN
(byte) DTV_BLIT_NAND
(byte) DTV_BLIT_NOR
(byte) DTV_BLIT_OR
(byte) DTV_BLIT_SHIFT0
(byte) DTV_BLIT_SHIFT1
(byte) DTV_BLIT_SHIFT2
(byte) DTV_BLIT_SHIFT3
(byte) DTV_BLIT_SHIFT4
(byte) DTV_BLIT_SHIFT5
(byte) DTV_BLIT_SHIFT6
(byte) DTV_BLIT_SHIFT7
(byte) DTV_BLIT_SRCA_CONT
(byte) DTV_BLIT_SRCA_FWD
(byte) DTV_BLIT_SRCB_CONT
(byte) DTV_BLIT_SRCB_FWD
(byte) DTV_BLIT_STATUS_BUSY
(byte) DTV_BLIT_STATUS_IRQ
(byte) DTV_BLIT_SUB
(byte) DTV_BLIT_TRANSPARANCY_NONE
(byte) DTV_BLIT_VBLANK
(byte) DTV_BLIT_VIC_IRQ
(byte) DTV_BLIT_WRITE_NONTRANSPARENT
(byte) DTV_BLIT_WRITE_TRANSPARENT
(byte) DTV_BLIT_XNOR
(byte) DTV_BLIT_XOR
(byte) DTV_BORDER_OFF
(byte) DTV_CHUNKY
(const byte) DTV_CHUNKY#0 DTV_CHUNKY = (byte/signed byte/word/signed word/dword/signed dword) 64
(byte) DTV_COLORRAM_OFF
(const byte) DTV_COLORRAM_OFF#0 DTV_COLORRAM_OFF = (byte/signed byte/word/signed word/dword/signed dword) 16
(dword) DTV_COLOR_BANK_DEFAULT
(byte*) DTV_COLOR_BANK_HI
(byte*) DTV_COLOR_BANK_LO
(byte*) DTV_CONTROL
(const byte*) DTV_CONTROL#0 DTV_CONTROL = ((byte*))(word/dword/signed dword) 53308
(byte*) DTV_FEATURE
(const byte*) DTV_FEATURE#0 DTV_FEATURE = ((byte*))(word/dword/signed dword) 53311
(byte) DTV_FEATURE_DISABLE_TIL_RESET
(byte) DTV_FEATURE_ENABLE
(const byte) DTV_FEATURE_ENABLE#0 DTV_FEATURE_ENABLE = (byte/signed byte/word/signed word/dword/signed dword) 1
(byte*) DTV_GRAPHICS_HICOL_BANK
(byte*) DTV_GRAPHICS_VIC_BANK
(byte) DTV_HIGHCOLOR
(const byte) DTV_HIGHCOLOR#0 DTV_HIGHCOLOR = (byte/signed byte/word/signed word/dword/signed dword) 4
(byte) DTV_LINEAR
(const byte) DTV_LINEAR#0 DTV_LINEAR = (byte/signed byte/word/signed word/dword/signed dword) 1
(byte) DTV_OVERSCAN
(byte*) DTV_PALETTE
(const byte*) DTV_PALETTE#0 DTV_PALETTE = ((byte*))(word/dword/signed dword) 53760
(byte[16]) DTV_PALETTE_DEFAULT
(byte*) DTV_PLANEA_MODULO_HI
(byte*) DTV_PLANEA_MODULO_LO
(byte*) DTV_PLANEA_START_HI
(byte*) DTV_PLANEA_START_LO
(byte*) DTV_PLANEA_START_MI
(byte*) DTV_PLANEA_STEP
(byte*) DTV_PLANEB_MODULO_HI
(const byte*) DTV_PLANEB_MODULO_HI#0 DTV_PLANEB_MODULO_HI = ((byte*))(word/dword/signed dword) 53320
(byte*) DTV_PLANEB_MODULO_LO
(const byte*) DTV_PLANEB_MODULO_LO#0 DTV_PLANEB_MODULO_LO = ((byte*))(word/dword/signed dword) 53319
(byte*) DTV_PLANEB_START_HI
(const byte*) DTV_PLANEB_START_HI#0 DTV_PLANEB_START_HI = ((byte*))(word/dword/signed dword) 53323
(byte*) DTV_PLANEB_START_LO
(const byte*) DTV_PLANEB_START_LO#0 DTV_PLANEB_START_LO = ((byte*))(word/dword/signed dword) 53321
(byte*) DTV_PLANEB_START_MI
(const byte*) DTV_PLANEB_START_MI#0 DTV_PLANEB_START_MI = ((byte*))(word/dword/signed dword) 53322
(byte*) DTV_PLANEB_STEP
(const byte*) DTV_PLANEB_STEP#0 DTV_PLANEB_STEP = ((byte*))(word/dword/signed dword) 53324
(byte*) DTV_SPRITE_BANK
(byte) GREEN
(byte) GREY
(void()**) HARDWARE_IRQ
(byte) IRQ_COLLISION_BG
(byte) IRQ_COLLISION_SPRITE
(byte*) IRQ_ENABLE
(byte) IRQ_LIGHTPEN
(byte) IRQ_RASTER
(byte*) IRQ_STATUS
(void()**) KERNEL_IRQ
(byte*) LIGHTPEN_X
(byte*) LIGHTPEN_Y
(byte) LIGHT_BLUE
(byte) LIGHT_GREEN
(byte) LIGHT_GREY
(byte) ORANGE
(byte) PINK
(byte*) PROCPORT
(const byte*) PROCPORT#0 PROCPORT = ((byte*))(byte/signed byte/word/signed word/dword/signed dword) 1
(byte) PROCPORT_BASIC_KERNEL_IO
(byte*) PROCPORT_DDR
(const byte*) PROCPORT_DDR#0 PROCPORT_DDR = ((byte*))(byte/signed byte/word/signed word/dword/signed dword) 0
(byte) PROCPORT_DDR_MEMORY_MASK
(const byte) PROCPORT_DDR_MEMORY_MASK#0 PROCPORT_DDR_MEMORY_MASK = (byte/signed byte/word/signed word/dword/signed dword) 7
(byte) PROCPORT_KERNEL_IO
(byte) PROCPORT_RAM_ALL
(byte) PROCPORT_RAM_CHARROM
(byte) PROCPORT_RAM_IO
(const byte) PROCPORT_RAM_IO#0 PROCPORT_RAM_IO = (byte/signed byte/word/signed word/dword/signed dword) 53
(byte) PURPLE
(byte*) RASTER
(const byte*) RASTER#0 RASTER = ((byte*))(word/dword/signed dword) 53266
(byte) RED
(byte*) SPRITES_COLS
(byte*) SPRITES_ENABLE
(byte*) SPRITES_EXPAND_X
(byte*) SPRITES_EXPAND_Y
(byte*) SPRITES_MC
(byte*) SPRITES_MC1
(byte*) SPRITES_MC2
(byte*) SPRITES_PRIORITY
(byte*) SPRITES_XMSB
(byte*) SPRITES_XPOS
(byte*) SPRITES_YPOS
(word) SPRITE_PTRS
(byte) VIC_BMM
(byte*) VIC_CONTROL
(const byte*) VIC_CONTROL#0 VIC_CONTROL = ((byte*))(word/dword/signed dword) 53265
(byte*) VIC_CONTROL2
(const byte*) VIC_CONTROL2#0 VIC_CONTROL2 = ((byte*))(word/dword/signed dword) 53270
(byte) VIC_CSEL
(const byte) VIC_CSEL#0 VIC_CSEL = (byte/signed byte/word/signed word/dword/signed dword) 8
(byte) VIC_DEN
(const byte) VIC_DEN#0 VIC_DEN = (byte/signed byte/word/signed word/dword/signed dword) 16
(byte) VIC_ECM
(const byte) VIC_ECM#0 VIC_ECM = (byte/signed byte/word/signed word/dword/signed dword) 64
(byte) VIC_MCM
(const byte) VIC_MCM#0 VIC_MCM = (byte/signed byte/word/signed word/dword/signed dword) 16
(byte*) VIC_MEMORY
(const byte*) VIC_MEMORY#0 VIC_MEMORY = ((byte*))(word/dword/signed dword) 53272
(byte) VIC_RSEL
(const byte) VIC_RSEL#0 VIC_RSEL = (byte/signed byte/word/signed word/dword/signed dword) 8
(byte) VIC_RST8
(byte) WHITE
(byte) YELLOW
(void()) dtvSetCpuBankSegment1((byte) dtvSetCpuBankSegment1::cpuBankIdx)
(label) dtvSetCpuBankSegment1::@return
(byte*) dtvSetCpuBankSegment1::cpuBank
(const byte*) dtvSetCpuBankSegment1::cpuBank#0 cpuBank = ((byte*))(byte/word/signed word/dword/signed dword) 255
(byte) dtvSetCpuBankSegment1::cpuBankIdx
(byte) dtvSetCpuBankSegment1::cpuBankIdx#1 reg byte a 202.0
(byte) dtvSetCpuBankSegment1::cpuBankIdx#3 reg byte a 103.0
(void()) gfx_init_chunky()
(word~) gfx_init_chunky::$6 $6 zp ZP_WORD:7 202.0
(label) gfx_init_chunky::@1
(label) gfx_init_chunky::@2
(label) gfx_init_chunky::@3
(label) gfx_init_chunky::@4
(label) gfx_init_chunky::@5
(label) gfx_init_chunky::@6
(label) gfx_init_chunky::@8
(label) gfx_init_chunky::@return
(byte) gfx_init_chunky::c
(byte) gfx_init_chunky::c#0 reg byte a 202.0
(byte*) gfx_init_chunky::gfxb
(byte*) gfx_init_chunky::gfxb#1 gfxb zp ZP_WORD:5 42.599999999999994
(byte*) gfx_init_chunky::gfxb#3 gfxb zp ZP_WORD:5 157.0
(byte*) gfx_init_chunky::gfxb#4 gfxb zp ZP_WORD:5 75.75
(byte*) gfx_init_chunky::gfxb#5 gfxb zp ZP_WORD:5 22.0
(byte) gfx_init_chunky::gfxbCpuBank
(byte) gfx_init_chunky::gfxbCpuBank#2 reg byte x 202.0
(byte) gfx_init_chunky::gfxbCpuBank#4 reg byte x 103.75
(byte) gfx_init_chunky::gfxbCpuBank#7 reg byte x 22.0
(byte) gfx_init_chunky::gfxbCpuBank#8 reg byte x 34.888888888888886
(word) gfx_init_chunky::x
(word) gfx_init_chunky::x#1 x zp ZP_WORD:3 151.5
(word) gfx_init_chunky::x#2 x zp ZP_WORD:3 30.299999999999997
(byte) gfx_init_chunky::y
(byte) gfx_init_chunky::y#1 y zp ZP_BYTE:2 16.5
(byte) gfx_init_chunky::y#6 y zp ZP_BYTE:2 9.461538461538462
(void()) main()
(byte~) main::$31 reg byte a 202.0
(byte~) main::$32 reg byte a 202.0
(byte~) main::$33 reg byte a 202.0
(label) main::@1
(label) main::@17
(label) main::@3
(label) main::@5
(label) main::@7
(label) main::@8
(byte) main::j
(byte) main::j#1 reg byte x 16.5
(byte) main::j#2 reg byte x 22.0
(byte) main::rst
(byte) main::rst#1 reg byte x 57.714285714285715

reg byte x [ main::j#2 main::j#1 ]
zp ZP_BYTE:2 [ gfx_init_chunky::y#6 gfx_init_chunky::y#1 ]
zp ZP_WORD:3 [ gfx_init_chunky::x#2 gfx_init_chunky::x#1 ]
reg byte x [ gfx_init_chunky::gfxbCpuBank#4 gfx_init_chunky::gfxbCpuBank#7 gfx_init_chunky::gfxbCpuBank#8 gfx_init_chunky::gfxbCpuBank#2 ]
zp ZP_WORD:5 [ gfx_init_chunky::gfxb#4 gfx_init_chunky::gfxb#3 gfx_init_chunky::gfxb#5 gfx_init_chunky::gfxb#1 ]
reg byte a [ dtvSetCpuBankSegment1::cpuBankIdx#3 dtvSetCpuBankSegment1::cpuBankIdx#1 ]
reg byte x [ main::rst#1 ]
reg byte a [ main::$31 ]
reg byte a [ main::$32 ]
reg byte a [ main::$33 ]
zp ZP_WORD:7 [ gfx_init_chunky::$6 ]
reg byte a [ gfx_init_chunky::c#0 ]
