(label) @7
(label) @begin
(label) @end
(byte*) BGCOL
(byte*) BGCOL1
(byte*) BGCOL2
(byte*) BGCOL3
(byte*) BGCOL4
(byte) BLACK
(byte) BLUE
(byte*) BORDERCOL
(const byte*) BORDERCOL#0 BORDERCOL = ((byte*))(word/dword/signed dword) 53280
(byte) BROWN
(byte*) CHARGEN
(byte*) CIA1_INTERRUPT
(const byte*) CIA1_INTERRUPT#0 CIA1_INTERRUPT = ((byte*))(word/dword/signed dword) 56333
(byte*) CIA1_PORT_A
(byte*) CIA1_PORT_A_DDR
(byte*) CIA1_PORT_B
(byte*) CIA1_PORT_B_DDR
(byte*) CIA2_INTERRUPT
(byte*) CIA2_PORT_A
(byte*) CIA2_PORT_A_DDR
(byte*) CIA2_PORT_B
(byte*) CIA2_PORT_B_DDR
(byte) CIA_INTERRUPT_CLEAR
(const byte) CIA_INTERRUPT_CLEAR#0 CIA_INTERRUPT_CLEAR = (byte/signed byte/word/signed word/dword/signed dword) 127
(byte*) COLS
(byte) CYAN
(byte*) D011
(byte*) D016
(byte*) D018
(byte) DARK_GREY
(byte*) GHOST_BYTE
(const byte*) GHOST_BYTE#0 GHOST_BYTE = ((byte*))(word/signed word/dword/signed dword) 16383
(byte) GREEN
(byte) GREY
(void()**) HARDWARE_IRQ
(byte) IRQ_COLLISION_BG
(byte) IRQ_COLLISION_SPRITE
(byte*) IRQ_ENABLE
(const byte*) IRQ_ENABLE#0 IRQ_ENABLE = ((byte*))(word/dword/signed dword) 53274
(byte) IRQ_LIGHTPEN
(byte) IRQ_RASTER
(const byte) IRQ_RASTER#0 IRQ_RASTER = (byte/signed byte/word/signed word/dword/signed dword) 1
(byte*) IRQ_STATUS
(const byte*) IRQ_STATUS#0 IRQ_STATUS = ((byte*))(word/dword/signed dword) 53273
(void()**) KERNEL_IRQ
(const void()**) KERNEL_IRQ#0 KERNEL_IRQ = ((void()**))(word/signed word/dword/signed dword) 788
(byte*) LIGHTPEN_X
(byte*) LIGHTPEN_Y
(byte) LIGHT_BLUE
(byte) LIGHT_GREEN
(byte) LIGHT_GREY
(byte) ORANGE
(byte) PINK
(byte*) PROCPORT
(byte) PROCPORT_BASIC_KERNEL_IO
(byte*) PROCPORT_DDR
(byte) PROCPORT_DDR_MEMORY_MASK
(byte) PROCPORT_KERNEL_IO
(byte) PROCPORT_RAM_ALL
(byte) PROCPORT_RAM_CHARROM
(byte) PROCPORT_RAM_IO
(byte) PURPLE
(byte*) RASTER
(const byte*) RASTER#0 RASTER = ((byte*))(word/dword/signed dword) 53266
(byte) RED
(const byte) RED#0 RED = (byte/signed byte/word/signed word/dword/signed dword) 2
(byte*) SPRITES_COLS
(byte*) SPRITES_ENABLE
(byte*) SPRITES_EXPAND_X
(byte*) SPRITES_EXPAND_Y
(byte*) SPRITES_MC
(byte*) SPRITES_MC1
(byte*) SPRITES_MC2
(byte*) SPRITES_PRIORITY
(byte*) SPRITES_XMSB
(byte*) SPRITES_XPOS
(byte*) SPRITES_YPOS
(word) SPRITE_PTRS
(byte) VIC_BMM
(byte*) VIC_CONTROL
(const byte*) VIC_CONTROL#0 VIC_CONTROL = ((byte*))(word/dword/signed dword) 53265
(byte*) VIC_CONTROL2
(byte) VIC_CSEL
(byte) VIC_DEN
(byte) VIC_ECM
(byte) VIC_MCM
(byte*) VIC_MEMORY
(byte) VIC_RSEL
(const byte) VIC_RSEL#0 VIC_RSEL = (byte/signed byte/word/signed word/dword/signed dword) 8
(byte) VIC_RST8
(byte) WHITE
(const byte) WHITE#0 WHITE = (byte/signed byte/word/signed word/dword/signed dword) 1
(byte) YELLOW
interrupt(KERNEL_MIN)(void()) irq_bottom_1()
(label) irq_bottom_1::@return
interrupt(KERNEL_KEYBOARD)(void()) irq_bottom_2()
(label) irq_bottom_2::@return
(void()) main()
(label) main::@return

