# -------------------------------------------------------------------------- #                                                                           
#                                                                           
# Copyright (C) 1991-2013 Altera Corporation                                                                           
# Your use of Altera Corporation's design tools, logic functions                                                                            
# and other software and tools, and its AMPP partner logic                                                                            
# functions, and any output files from any of the foregoing                                                                            
# (including device programming or simulation files), and any                                                                            
# associated documentation or information are expressly subject                                                                            
# to the terms and conditions of the Altera Program License                                                                            
# Subscription Agreement, Altera MegaCore Function License                                                                            
# Agreement, or other applicable license agreement, including,                                                                            
# without limitation, that your use is for the sole purpose of                                                                            
# programming logic devices manufactured by Altera and sold by                                                                            
# Altera or its authorized distributors.  Please refer to the                                                                            
# applicable agreement for further details.                                                                           
#                                                                           
# -------------------------------------------------------------------------- #                                                                           
#                                                                           
# Quartus II 64-Bit                                                                           
# Version 13.1.0 Build 162 10/23/2013 SJ Web Edition                                                                           
# Date created = 11:23:36  April 10, 2018                                                                           
#                                                                           
# -------------------------------------------------------------------------- #                                                                           
#                                                                           
# Notes:                                                                           
#                                                                           
# 1) The default values for assignments are stored in the file:                                                                           
#		apple-one_assignment_defaults.qdf                                                                           
#    If this file doesn't exist, see file:                                                                           
#		assignment_defaults.qdf                                                                           
#                                                                           
# 2) Altera recommends that you do not modify this file. This                                                                           
#    file is updated automatically by the Quartus II software                                                                           
#    and any changes you make may be lost or overwritten.                                                                           
#                                                                           
# -------------------------------------------------------------------------- #                                                                           
# Project-Wide Assignments                                                                           
# ========================                                                                           
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 13.1                                                                           
set_global_assignment -name PROJECT_CREATION_TIME_DATE "21:11:27  JANUARY 26, 2018"                                                                           
set_global_assignment -name LAST_QUARTUS_VERSION 13.1                                                                           
set_global_assignment -name PROJECT_OUTPUT_DIRECTORY output_files                                                                           
# Classic Timing Assignments                                                                           
# ==========================                                                                           
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0                                                                           
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85                                                                           
# Analysis & Synthesis Assignments                                                                           
# ================================                                                                           
set_global_assignment -name TOP_LEVEL_ENTITY apple1_mist                                                                           
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 144                                                                           
set_global_assignment -name DEVICE_FILTER_SPEED_GRADE 8                                                                           
# Fitter Assignments                                                                           
# ==================                                                                           
set_global_assignment -name DEVICE EP4CE22F17C8                                                                           
set_global_assignment -name FAMILY "Cyclone IV"                                                                           
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR 1                                                                           
set_global_assignment -name STRATIX_DEVICE_IO_STANDARD "2.5 V"                                                                           
set_global_assignment -name CRC_ERROR_OPEN_DRAIN OFF                                                                           
set_global_assignment -name CYCLONEII_RESERVE_NCEO_AFTER_CONFIGURATION "USE AS REGULAR IO"                                                                           
set_global_assignment -name ENABLE_CONFIGURATION_PINS OFF                                                                           
set_global_assignment -name ENABLE_NCE_PIN OFF                                                                           
set_global_assignment -name ENABLE_BOOT_SEL_PIN OFF                                                                           
set_global_assignment -name CYCLONEIII_CONFIGURATION_SCHEME "PASSIVE SERIAL"                                                                           
set_global_assignment -name FORCE_CONFIGURATION_VCCIO ON                                                                           
set_global_assignment -name RESERVE_DATA0_AFTER_CONFIGURATION "USE AS REGULAR IO"                                                                           
set_global_assignment -name RESERVE_DATA1_AFTER_CONFIGURATION "USE AS REGULAR IO"                                                                           
set_global_assignment -name RESERVE_FLASH_NCE_AFTER_CONFIGURATION "USE AS REGULAR IO"                                                                           
# EDA Netlist Writer Assignments                                                                           
# ==============================                                                                           
set_global_assignment -name EDA_SIMULATION_TOOL "ModelSim-Altera (VHDL)"                                                                           
# Assembler Assignments                                                                           
# =====================                                                                           
set_global_assignment -name USE_CONFIGURATION_DEVICE OFF                                                                           
set_global_assignment -name GENERATE_RBF_FILE ON                                                                           
# Power Estimation Assignments                                                                           
# ============================                                                                           
set_global_assignment -name POWER_PRESET_COOLING_SOLUTION "23 MM HEAT SINK WITH 200 LFPM AIRFLOW"                                                                           
set_global_assignment -name POWER_BOARD_THERMAL_MODEL "NONE (CONSERVATIVE)"                                                                           
# Advanced I/O Timing Assignments                                                                           
# ===============================                                                                           
set_global_assignment -name OUTPUT_IO_TIMING_NEAR_END_VMEAS "HALF VCCIO" -rise                                                                           
set_global_assignment -name OUTPUT_IO_TIMING_NEAR_END_VMEAS "HALF VCCIO" -fall                                                                           
set_global_assignment -name OUTPUT_IO_TIMING_FAR_END_VMEAS "HALF SIGNAL SWING" -rise                                                                           
set_global_assignment -name OUTPUT_IO_TIMING_FAR_END_VMEAS "HALF SIGNAL SWING" -fall                                                                           
# start EDA_TOOL_SETTINGS(eda_simulation)                                                                           
# ---------------------------------------                                                                           
	# EDA Netlist Writer Assignments                                                                           
	# ==============================                                                                           
set_global_assignment -name EDA_OUTPUT_DATA_FORMAT VHDL -section_id eda_simulation                                                                           
# end EDA_TOOL_SETTINGS(eda_simulation)                                                                           
# -------------------------------------                                                                           
	# start DESIGN_PARTITION(Top)                                                                           
	# ---------------------------                                                                           
		# Incremental Compilation Assignments                                                                           
		# ===================================                                                                           
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top                                                                           
set_global_assignment -name PARTITION_FITTER_PRESERVATION_LEVEL PLACEMENT_AND_ROUTING -section_id Top                                                                           
set_global_assignment -name PARTITION_COLOR 16764057 -section_id Top                                                                           
	# end DESIGN_PARTITION(Top)                                                                           
	# -------------------------                                                                           
# Pin & Location Assignments                                                                           
# ==========================                                                                           
set_location_assignment PIN_G1 -to LED                                                                           
set_location_assignment PIN_P16 -to VGA_R[5]                                                                           
set_location_assignment PIN_P15 -to VGA_R[4]                                                                           
set_location_assignment PIN_R16 -to VGA_R[3]                                                                           
set_location_assignment PIN_R14 -to VGA_R[2]                                                                           
set_location_assignment PIN_T15 -to VGA_R[1]                                                                           
set_location_assignment PIN_T14 -to VGA_R[0]                                                                           
set_location_assignment PIN_J16 -to VGA_B[5]                                                                           
set_location_assignment PIN_J15 -to VGA_B[4]                                                                           
set_location_assignment PIN_J14 -to VGA_B[3]                                                                           
set_location_assignment PIN_K16 -to VGA_B[2]                                                                           
set_location_assignment PIN_K15 -to VGA_B[1]                                                                           
set_location_assignment PIN_J13 -to VGA_B[0]                                                                           
set_location_assignment PIN_F16 -to VGA_G[5]                                                                           
set_location_assignment PIN_F15 -to VGA_G[4]                                                                           
set_location_assignment PIN_L16 -to VGA_G[3]                                                                           
set_location_assignment PIN_L15 -to VGA_G[2]                                                                           
set_location_assignment PIN_N15 -to VGA_G[1]                                                                           
set_location_assignment PIN_N16 -to VGA_G[0]                                                                           
set_location_assignment PIN_T10 -to VGA_VS                                                                           
set_location_assignment PIN_T11 -to VGA_HS                                                                           
set_location_assignment PIN_T12 -to AUDIO_L                                                                           
set_location_assignment PIN_T13 -to AUDIO_R                                                                           
set_location_assignment PIN_D1 -to UART_TX                                                                           
set_location_assignment PIN_B1 -to UART_RX                                                                           
set_location_assignment PIN_T2 -to SPI_DO                                                                           
set_location_assignment PIN_R1 -to SPI_DI                                                                           
set_location_assignment PIN_T3 -to SPI_SCK                                                                           
set_location_assignment PIN_T4 -to SPI_SS2                                                                           
set_location_assignment PIN_G15 -to SPI_SS3                                                                           
set_location_assignment PIN_G16 -to SPI_SS4                                                                           
set_location_assignment PIN_H2 -to CONF_DATA0                                                                           
set_location_assignment PIN_B14 -to SDRAM_A[0]                                                                           
set_location_assignment PIN_C14 -to SDRAM_A[1]                                                                           
set_location_assignment PIN_C15 -to SDRAM_A[2]                                                                           
set_location_assignment PIN_C16 -to SDRAM_A[3]                                                                           
set_location_assignment PIN_B16 -to SDRAM_A[4]                                                                           
set_location_assignment PIN_A15 -to SDRAM_A[5]                                                                           
set_location_assignment PIN_A14 -to SDRAM_A[6]                                                                           
set_location_assignment PIN_A13 -to SDRAM_A[7]                                                                           
set_location_assignment PIN_A12 -to SDRAM_A[8]                                                                           
set_location_assignment PIN_D16 -to SDRAM_A[9]                                                                           
set_location_assignment PIN_B13 -to SDRAM_A[10]                                                                           
set_location_assignment PIN_D15 -to SDRAM_A[11]                                                                           
set_location_assignment PIN_D14 -to SDRAM_A[12]                                                                           
set_location_assignment PIN_C3 -to SDRAM_DQ[0]                                                                           
set_location_assignment PIN_C2 -to SDRAM_DQ[1]                                                                           
set_location_assignment PIN_A4 -to SDRAM_DQ[2]                                                                           
set_location_assignment PIN_B4 -to SDRAM_DQ[3]                                                                           
set_location_assignment PIN_A6 -to SDRAM_DQ[4]                                                                           
set_location_assignment PIN_D6 -to SDRAM_DQ[5]                                                                           
set_location_assignment PIN_A7 -to SDRAM_DQ[6]                                                                           
set_location_assignment PIN_B7 -to SDRAM_DQ[7]                                                                           
set_location_assignment PIN_E6 -to SDRAM_DQ[8]                                                                           
set_location_assignment PIN_C6 -to SDRAM_DQ[9]                                                                           
set_location_assignment PIN_B6 -to SDRAM_DQ[10]                                                                           
set_location_assignment PIN_B5 -to SDRAM_DQ[11]                                                                           
set_location_assignment PIN_A5 -to SDRAM_DQ[12]                                                                           
set_location_assignment PIN_B3 -to SDRAM_DQ[13]                                                                           
set_location_assignment PIN_A3 -to SDRAM_DQ[14]                                                                           
set_location_assignment PIN_A2 -to SDRAM_DQ[15]                                                                           
set_location_assignment PIN_A11 -to SDRAM_BA[0]                                                                           
set_location_assignment PIN_B12 -to SDRAM_BA[1]                                                                           
set_location_assignment PIN_C9 -to SDRAM_DQMH                                                                           
set_location_assignment PIN_C8 -to SDRAM_DQML                                                                           
set_location_assignment PIN_A10 -to SDRAM_nRAS                                                                           
set_location_assignment PIN_B10 -to SDRAM_nCAS                                                                           
set_location_assignment PIN_D8 -to SDRAM_nWE                                                                           
set_location_assignment PIN_B11 -to SDRAM_nCS                                                                           
set_location_assignment PIN_C11 -to SDRAM_CKE                                                                           
set_location_assignment PIN_R4 -to SDRAM_CLK                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[0]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[1]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[2]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[3]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[4]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[5]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[6]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[7]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[8]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[9]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[10]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[11]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[12]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[13]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[14]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQ[15]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[0]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[1]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[2]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[3]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[4]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[5]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[6]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[7]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[8]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[9]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[10]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[11]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_A[12]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_BA[0]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_BA[1]                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQMH                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_DQML                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_nRAS                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_nCAS                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_nWE                                                                           
set_instance_assignment -name FAST_OUTPUT_REGISTER ON -to SDRAM_nCS                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[0]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[1]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[2]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[3]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[4]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[5]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[6]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[7]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[8]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[9]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[10]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[11]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[12]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[13]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[14]                                                                           
set_instance_assignment -name FAST_OUTPUT_ENABLE_REGISTER ON -to SDRAM_DQ[15]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[0]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[1]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[2]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[3]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[4]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[5]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[6]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[7]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[8]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[9]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[10]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[11]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[12]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[13]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[14]                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to SDRAM_DQ[15]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[0]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[1]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[2]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[3]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[4]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[5]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[6]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[7]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[8]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[9]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[10]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[11]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_A[12]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[0]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[1]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[2]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[3]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[4]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[5]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[6]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[7]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[8]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[9]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[10]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[11]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[12]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[13]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[14]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQ[15]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_BA[0]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_BA[1]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQML                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_DQMH                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_nRAS                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_nCAS                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_nWE                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_nCS                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_CKE                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SDRAM_CLK                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[5]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[4]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[3]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[2]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[1]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_R[0]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[5]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[4]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[3]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[2]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[1]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_G[0]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[5]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[4]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[3]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[2]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[1]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to VGA_B[0]                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to VGA_HS                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to VGA_VS                                                                           
set_instance_assignment -name GLOBAL_SIGNAL "GLOBAL CLOCK" -to SPI_SCK                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to UART_RX                                                                           
set_instance_assignment -name CURRENT_STRENGTH_NEW 4MA -to UART_TX                                                                           
set_location_assignment PLL_1 -to "pll:pll|altpll:altpll_component"                                                                           
set_global_assignment -name PRE_FLOW_SCRIPT_FILE "quartus_sh:rtl/build_id.tcl"                                                                           
# end ENTITY(apple1_mist)                                                                           
# -----------------------                                                                           
set_global_assignment -name VHDL_FILE rtl/pia6821/pia6821.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/T65/T65_Pack.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/T65/T65_MCode.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/T65/T65_ALU.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/T65/T65.vhd                                                                           
set_global_assignment -name QIP_FILE rtl/T65/T65.qip                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/wave_map.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/sid_top.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/sid_regs.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/sid_mixer.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/sid_filter.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/sid_debug_pkg.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/sid_ctrl.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/Q_table.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/oscillator.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/my_math_pkg.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/mult_acc.vhd                                                                           
set_global_assignment -name VHDL_FILE rtl/sid/adsr_multi.vhd                                                                           
set_global_assignment -name VERILOG_FILE rtl/aci.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/display_ram.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/tms9918/vram.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/tms9918/tms9918_async.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/tms9918/tms9918.v                                                                           
set_global_assignment -name SYSTEMVERILOG_FILE rtl/ram.sv                                                                           
set_global_assignment -name SYSTEMVERILOG_FILE rtl/downloader.sv                                                                           
set_global_assignment -name VERILOG_FILE rtl/display.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/sdram.v                                                                           
set_global_assignment -name VERILOG_FILE "rtl/mist-modules/user_io.v"                                                                           
set_global_assignment -name VERILOG_FILE "rtl/mist-modules/sd_card.v"                                                                           
set_global_assignment -name VERILOG_FILE "rtl/mist-modules/scandoubler.v"                                                                           
set_global_assignment -name VERILOG_FILE "rtl/mist-modules/rgb2ypbpr.v"                                                                           
set_global_assignment -name VERILOG_FILE "rtl/mist-modules/osd.v"                                                                           
set_global_assignment -name VERILOG_FILE "rtl/mist-modules/mist_video.v"                                                                           
set_global_assignment -name QIP_FILE "rtl/mist-modules/mist_core.qip"                                                                           
set_global_assignment -name VHDL_FILE "rtl/mist-modules/mist.vhd"                                                                           
set_global_assignment -name QIP_FILE "rtl/mist-modules/mist.qip"                                                                           
set_global_assignment -name VERILOG_FILE "rtl/mist-modules/data_io.v"                                                                           
set_global_assignment -name VHDL_FILE "rtl/mist-modules/dac.vhd"                                                                           
set_global_assignment -name SYSTEMVERILOG_FILE "rtl/mist-modules/cofi.sv"                                                                           
set_global_assignment -name VERILOG_FILE "rtl/mist-modules/arcade_inputs.v"                                                                           
set_global_assignment -name VERILOG_FILE rtl/apple1.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/clock.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/rom_basic.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/rom_wozmon.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/ps2keyboard.v                                                                           
set_global_assignment -name VERILOG_FILE rtl/font_rom.v                                                                           
set_global_assignment -name QIP_FILE rtl/pll.qip                                                                           
set_global_assignment -name SYSTEMVERILOG_FILE rtl/apple1_mist.sv                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_sprite-c.vhd"                                                                           
set_global_assignment -name VHDL_FILE rtl/tms9918/vdp18/vdp18_sprite.vhd                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_pattern-c.vhd"                                                                           
set_global_assignment -name VHDL_FILE rtl/tms9918/vdp18/vdp18_pattern.vhd                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_pack-p.vhd"                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_hor_vert-c.vhd"                                                                           
set_global_assignment -name VHDL_FILE rtl/tms9918/vdp18/vdp18_hor_vert.vhd                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_ctrl-c.vhd"                                                                           
set_global_assignment -name VHDL_FILE rtl/tms9918/vdp18/vdp18_ctrl.vhd                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_cpuio-c.vhd"                                                                           
set_global_assignment -name VHDL_FILE rtl/tms9918/vdp18/vdp18_cpuio.vhd                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_core-c.vhd"                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_core_comp_pack-p.vhd"                                                                           
set_global_assignment -name VHDL_FILE rtl/tms9918/vdp18/vdp18_core.vhd                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_comp_pack-p.vhd"                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_col_pack-p.vhd"                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_col_mux-c.vhd"                                                                           
set_global_assignment -name VHDL_FILE rtl/tms9918/vdp18/vdp18_col_mux.vhd                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_clk_gen-c.vhd"                                                                           
set_global_assignment -name VHDL_FILE rtl/tms9918/vdp18/vdp18_clk_gen.vhd                                                                           
set_global_assignment -name VHDL_FILE "rtl/tms9918/vdp18/vdp18_addr_mux-c.vhd"                                                                           
set_global_assignment -name VHDL_FILE rtl/tms9918/vdp18/vdp18_addr_mux.vhd                                                                           
set_location_assignment PIN_E1 -to CLOCK_27                                                                           
set_location_assignment PIN_M2 -to CLOCK_27_1                                                                           
set_instance_assignment -name FAST_INPUT_REGISTER ON -to CLOCK_27                                                                           

set_instance_assignment -name PARTITION_HIERARCHY root_partition -to | -section_id Top