(module Mini_Speaker (layer F.Cu) (tedit 5F837EBB)
  (fp_text reference LS1 (at 0 4.699) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Speaker (at 0 -4.572) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 23mm (at 0 -9.652) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 30mm (at 0 -13.335) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6.223 -3.048) (end 6.858 -3.048) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.223 -3.048) (end 5.588 -3.048) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.35 -3.048) (end -5.715 -3.048) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.35 -3.048) (end -6.985 -3.048) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.35 -2.54) (end -6.35 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.35 -3.683) (end -6.35 -2.54) (layer F.SilkS) (width 0.15))
  (fp_circle (center 0 0) (end -11.557 0) (layer F.SilkS) (width 0.15))
  (fp_circle (center 0 0) (end -15.113 0) (layer F.SilkS) (width 0.15))
  (pad 2 thru_hole circle (at 2.5 0.127) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -2.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 5 0.127) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at -7.5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 7.5 0.127) (size 2 2) (drill 1) (layers *.Cu *.Mask))
)
