(module "vdu_port:VDU Module" (layer F.Cu) (tedit 5C12714F)
  (fp_text reference U11 (at -7.62 -7.62) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value VDU_Port (at -7.62 -10.16) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.27 -5.08) (end -1.905 -4.445) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 -5.08) (end -1.905 -5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 -12.7) (end -1.905 -12.065) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 -12.7) (end -1.905 -13.335) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 -5.08) (end -2.54 -5.08) (layer F.SilkS) (width 0.15))
  (fp_line (start -15.24 -7.62) (end -13.97 -7.62) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.97 -7.62) (end -11.43 -5.08) (layer F.SilkS) (width 0.15))
  (fp_line (start -11.43 -5.08) (end -1.27 -5.08) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 -12.7) (end -11.43 -12.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -11.43 -12.7) (end -13.97 -10.16) (layer F.SilkS) (width 0.15))
  (fp_line (start -13.97 -10.16) (end -15.24 -10.16) (layer F.SilkS) (width 0.15))
  (fp_text user GND (at 1.27 -10.16) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at 1.27 -7.62) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user AUD (at 1.27 -5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VID (at 1.27 -12.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user AUD (at -16.51 -7.62) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VID (at -16.51 -10.16) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at -16.51 -5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VCC (at -16.51 -12.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole circle (at -19.05 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -19.05 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -19.05 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -19.05 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 3.81 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 3.81 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 3.81 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 3.81 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
