(kicad_pcb (version 4) (host pcbnew 4.0.7)

  (general
    (links 181)
    (no_connects 0)
    (area 62.154999 58.344999 161.365001 157.555001)
    (thickness 1.6)
    (drawings 219)
    (tracks 463)
    (zones 0)
    (modules 22)
    (nets 42)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory export/))
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 /A15)
  (net 5 /A14)
  (net 6 /A13)
  (net 7 /A12)
  (net 8 /A11)
  (net 9 /A10)
  (net 10 /A9)
  (net 11 /A8)
  (net 12 /A7)
  (net 13 /A6)
  (net 14 /A5)
  (net 15 /A4)
  (net 16 /A3)
  (net 17 /A2)
  (net 18 /A1)
  (net 19 /A0)
  (net 20 /PHI2)
  (net 21 /RESET)
  (net 22 /PHI0)
  (net 23 /IRQ)
  (net 24 /SPARE0)
  (net 25 /R/~W)
  (net 26 /RDY)
  (net 27 /SYNC)
  (net 28 /D0)
  (net 29 /D1)
  (net 30 /D2)
  (net 31 /D3)
  (net 32 /D4)
  (net 33 /D5)
  (net 34 /D6)
  (net 35 /D7)
  (net 36 /TX)
  (net 37 /RX)
  (net 38 /NMI)
  (net 39 /SPARE1)
  (net 40 /SPARE2)
  (net 41 "Net-(D1-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /IRQ)
    (add_net /NMI)
    (add_net /PHI0)
    (add_net /PHI2)
    (add_net /R/~W)
    (add_net /RDY)
    (add_net /RESET)
    (add_net /RX)
    (add_net /SPARE0)
    (add_net /SPARE1)
    (add_net /SPARE2)
    (add_net /SYNC)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net VCC)
  )

  (module Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm (layer F.Cu) (tedit 59650532) (tstamp 5C334988)
    (at 64.77 156.21 180)
    (descr "Through hole straight pin header, 1x39, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x39 2.54mm single row")
    (path /5C2F510F)
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RC6502_Backplane (at 0 98.85 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 97.79) (end -1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 97.79) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 97.85) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 98.3) (end 1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 98.3) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 48.26 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A15))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A14))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A13))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A12))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A11))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A10))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A9))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A8))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A7))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A6))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A5))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A4))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A3))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A2))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A1))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A0))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PHI2))
    (pad 20 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /RESET))
    (pad 21 thru_hole oval (at 0 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PHI0))
    (pad 22 thru_hole oval (at 0 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IRQ))
    (pad 23 thru_hole oval (at 0 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SPARE0))
    (pad 24 thru_hole oval (at 0 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /R/~W))
    (pad 25 thru_hole oval (at 0 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /RDY))
    (pad 26 thru_hole oval (at 0 63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SYNC))
    (pad 27 thru_hole oval (at 0 66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D0))
    (pad 28 thru_hole oval (at 0 68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D1))
    (pad 29 thru_hole oval (at 0 71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D2))
    (pad 30 thru_hole oval (at 0 73.66 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D3))
    (pad 31 thru_hole oval (at 0 76.2 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D4))
    (pad 32 thru_hole oval (at 0 78.74 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D5))
    (pad 33 thru_hole oval (at 0 81.28 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /D6))
    (pad 34 thru_hole oval (at 0 83.82 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /D7))
    (pad 35 thru_hole oval (at 0 86.36 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /TX))
    (pad 36 thru_hole oval (at 0 88.9 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /RX))
    (pad 37 thru_hole oval (at 0 91.44 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /NMI))
    (pad 38 thru_hole oval (at 0 93.98 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /SPARE1))
    (pad 39 thru_hole oval (at 0 96.52 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /SPARE2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x39_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5C61CEEE) (tstamp 5C334933)
    (at 154.305 79.375 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (path /5C2F607E)
    (fp_text reference C1 (at -8.89 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100uF (at 1.27 1.905 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_arc (start 1.25 0) (end -1.05558 -1.18) (angle 125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end -1.05558 1.18) (angle -125.8) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.25 0) (end 3.55558 -1.18) (angle 54.2) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.25 0) (end 3.75 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2 0) (end -1 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.Fab) (width 0.1))
    (fp_line (start 1.25 -2.55) (end 1.25 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.29 -2.55) (end 1.29 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 -2.549) (end 1.33 2.549) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.37 -2.548) (end 1.37 2.548) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.41 -2.546) (end 1.41 2.546) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.45 -2.543) (end 1.45 2.543) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.49 -2.539) (end 1.49 2.539) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 -2.535) (end 1.53 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.53 0.98) (end 1.53 2.535) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 -2.531) (end 1.57 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.57 0.98) (end 1.57 2.531) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -2.525) (end 1.61 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 0.98) (end 1.61 2.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 -2.519) (end 1.65 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.65 0.98) (end 1.65 2.519) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 -2.513) (end 1.69 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.69 0.98) (end 1.69 2.513) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 -2.506) (end 1.73 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.73 0.98) (end 1.73 2.506) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 -2.498) (end 1.77 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.77 0.98) (end 1.77 2.498) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 -2.489) (end 1.81 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.81 0.98) (end 1.81 2.489) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 -2.48) (end 1.85 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.85 0.98) (end 1.85 2.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 -2.47) (end 1.89 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.89 0.98) (end 1.89 2.47) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 -2.46) (end 1.93 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.93 0.98) (end 1.93 2.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 -2.448) (end 1.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.971 0.98) (end 1.971 2.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 -2.436) (end 2.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.011 0.98) (end 2.011 2.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 -2.424) (end 2.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.051 0.98) (end 2.051 2.424) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 -2.41) (end 2.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.091 0.98) (end 2.091 2.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 -2.396) (end 2.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.131 0.98) (end 2.131 2.396) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 -2.382) (end 2.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.171 0.98) (end 2.171 2.382) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 -2.366) (end 2.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.211 0.98) (end 2.211 2.366) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 -2.35) (end 2.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.251 0.98) (end 2.251 2.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 -2.333) (end 2.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.291 0.98) (end 2.291 2.333) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 -2.315) (end 2.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.331 0.98) (end 2.331 2.315) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 -2.296) (end 2.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.371 0.98) (end 2.371 2.296) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 -2.276) (end 2.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.411 0.98) (end 2.411 2.276) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 -2.256) (end 2.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.451 0.98) (end 2.451 2.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 -2.234) (end 2.491 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.491 0.98) (end 2.491 2.234) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 -2.212) (end 2.531 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.531 0.98) (end 2.531 2.212) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 -2.189) (end 2.571 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.571 0.98) (end 2.571 2.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 -2.165) (end 2.611 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.611 0.98) (end 2.611 2.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 -2.14) (end 2.651 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.651 0.98) (end 2.651 2.14) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 -2.113) (end 2.691 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.691 0.98) (end 2.691 2.113) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 -2.086) (end 2.731 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.731 0.98) (end 2.731 2.086) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 -2.058) (end 2.771 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.771 0.98) (end 2.771 2.058) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 -2.028) (end 2.811 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.811 0.98) (end 2.811 2.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 -1.997) (end 2.851 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.851 0.98) (end 2.851 1.997) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 -1.965) (end 2.891 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.891 0.98) (end 2.891 1.965) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 -1.932) (end 2.931 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.931 0.98) (end 2.931 1.932) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 -1.897) (end 2.971 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.971 0.98) (end 2.971 1.897) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 -1.861) (end 3.011 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.011 0.98) (end 3.011 1.861) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 -1.823) (end 3.051 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.051 0.98) (end 3.051 1.823) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 -1.783) (end 3.091 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.091 0.98) (end 3.091 1.783) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 -1.742) (end 3.131 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.131 0.98) (end 3.131 1.742) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 -1.699) (end 3.171 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.171 0.98) (end 3.171 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 -1.654) (end 3.211 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.211 0.98) (end 3.211 1.654) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 -1.606) (end 3.251 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.251 0.98) (end 3.251 1.606) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 -1.556) (end 3.291 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.291 0.98) (end 3.291 1.556) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 -1.504) (end 3.331 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.331 0.98) (end 3.331 1.504) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 -1.448) (end 3.371 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.371 0.98) (end 3.371 1.448) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 -1.39) (end 3.411 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.411 0.98) (end 3.411 1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 -1.327) (end 3.451 -0.98) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.451 0.98) (end 3.451 1.327) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.491 -1.261) (end 3.491 1.261) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.531 -1.189) (end 3.531 1.189) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.571 -1.112) (end 3.571 1.112) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.611 -1.028) (end 3.611 1.028) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.651 -0.934) (end 3.651 0.934) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.691 -0.829) (end 3.691 0.829) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.731 -0.707) (end 3.731 0.707) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.771 -0.559) (end 3.771 0.559) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.811 -0.354) (end 3.811 0.354) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.2 0) (end -1 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -0.65) (end -1.6 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.6 -2.85) (end -1.6 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 2.85) (end 4.1 2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 2.85) (end 4.1 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.1 -2.85) (end -1.6 -2.85) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at -8.89 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:CP_Radial_D4.0mm_P2.00mm (layer F.Cu) (tedit 5C3358C9) (tstamp 5C334939)
    (at 153.67 85.09 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 4mm Electrolytic Capacitor")
    (path /5C2F6198)
    (fp_text reference C2 (at -9.525 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10uF (at 1.27 1.905 180) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_arc (start 1 0) (end -0.845996 -0.98) (angle 124.1) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end -0.845996 0.98) (angle -124.1) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1 0) (end 2.845996 -0.98) (angle 55.9) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1 0) (end 3 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 0) (end -0.8 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.25 -0.45) (end -1.25 0.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -2.05) (end 1 2.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.04 -2.05) (end 1.04 2.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.08 -2.049) (end 1.08 2.049) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.12 -2.047) (end 1.12 2.047) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -2.044) (end 1.16 2.044) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.2 -2.041) (end 1.2 2.041) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 -2.037) (end 1.24 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.24 0.78) (end 1.24 2.037) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 -2.032) (end 1.28 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.28 0.78) (end 1.28 2.032) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 -2.026) (end 1.32 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.32 0.78) (end 1.32 2.026) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 -2.019) (end 1.36 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.36 0.78) (end 1.36 2.019) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 -2.012) (end 1.4 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.4 0.78) (end 1.4 2.012) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 -2.004) (end 1.44 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 0.78) (end 1.44 2.004) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 -1.995) (end 1.48 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.48 0.78) (end 1.48 1.995) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 -1.985) (end 1.52 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.52 0.78) (end 1.52 1.985) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 -1.974) (end 1.56 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.56 0.78) (end 1.56 1.974) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 -1.963) (end 1.6 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.6 0.78) (end 1.6 1.963) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 -1.95) (end 1.64 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.64 0.78) (end 1.64 1.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 -1.937) (end 1.68 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.68 0.78) (end 1.68 1.937) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 -1.923) (end 1.721 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.721 0.78) (end 1.721 1.923) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 -1.907) (end 1.761 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.761 0.78) (end 1.761 1.907) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 -1.891) (end 1.801 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.801 0.78) (end 1.801 1.891) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 -1.874) (end 1.841 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.841 0.78) (end 1.841 1.874) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 -1.856) (end 1.881 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.881 0.78) (end 1.881 1.856) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 -1.837) (end 1.921 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.921 0.78) (end 1.921 1.837) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 -1.817) (end 1.961 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.961 0.78) (end 1.961 1.817) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 -1.796) (end 2.001 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.001 0.78) (end 2.001 1.796) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 -1.773) (end 2.041 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.041 0.78) (end 2.041 1.773) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 -1.75) (end 2.081 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.081 0.78) (end 2.081 1.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 -1.725) (end 2.121 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.121 0.78) (end 2.121 1.725) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 -1.699) (end 2.161 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.161 0.78) (end 2.161 1.699) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 -1.672) (end 2.201 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.201 0.78) (end 2.201 1.672) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 -1.643) (end 2.241 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.241 0.78) (end 2.241 1.643) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 -1.613) (end 2.281 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.281 0.78) (end 2.281 1.613) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 -1.581) (end 2.321 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.321 0.78) (end 2.321 1.581) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 -1.547) (end 2.361 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.361 0.78) (end 2.361 1.547) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 -1.512) (end 2.401 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.401 0.78) (end 2.401 1.512) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 -1.475) (end 2.441 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.441 0.78) (end 2.441 1.475) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 -1.436) (end 2.481 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.481 0.78) (end 2.481 1.436) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 -1.395) (end 2.521 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.521 0.78) (end 2.521 1.395) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 -1.351) (end 2.561 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.561 0.78) (end 2.561 1.351) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 -1.305) (end 2.601 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.601 0.78) (end 2.601 1.305) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 -1.256) (end 2.641 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.641 0.78) (end 2.641 1.256) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 -1.204) (end 2.681 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.681 0.78) (end 2.681 1.204) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 -1.148) (end 2.721 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.721 0.78) (end 2.721 1.148) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 -1.088) (end 2.761 -0.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.761 0.78) (end 2.761 1.088) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.801 -1.023) (end 2.801 1.023) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.841 -0.952) (end 2.841 0.952) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.881 -0.874) (end 2.881 0.874) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.921 -0.786) (end 2.921 0.786) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.961 -0.686) (end 2.961 0.686) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.001 -0.567) (end 3.001 0.567) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.041 -0.415) (end 3.041 0.415) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.081 -0.165) (end 3.081 0.165) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.7 0) (end -0.8 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.25 -0.45) (end -1.25 0.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.35) (end -1.35 2.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 2.35) (end 3.35 2.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.35 2.35) (end 3.35 -2.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.35 -2.35) (end -1.35 -2.35) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at -9.525 0 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5C33507E) (tstamp 5C33493F)
    (at 151.765 93.98 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (path /5C2F4692)
    (fp_text reference C3 (at 2.54 0 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 2.56 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.09 -1.31) (end 4.91 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 1.31) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 -1.31) (end 0.09 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 0.996) (end 0.09 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 -1.31) (end 4.91 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 0.996) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 6.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 1.6) (end 6.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5C335110) (tstamp 5C334945)
    (at 68.58 111.76 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (path /5C2F4437)
    (fp_text reference C4 (at 2.54 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 2.56 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.09 -1.31) (end 4.91 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 1.31) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 -1.31) (end 0.09 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 0.996) (end 0.09 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 -1.31) (end 4.91 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 0.996) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 6.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 1.6) (end 6.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5C335117) (tstamp 5C33494B)
    (at 92.075 111.76 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (path /5C2F4504)
    (fp_text reference C5 (at 2.54 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 2.56 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.09 -1.31) (end 4.91 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 1.31) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 -1.31) (end 0.09 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 0.996) (end 0.09 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 -1.31) (end 4.91 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 0.996) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 6.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 1.6) (end 6.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5C335860) (tstamp 5C334951)
    (at 115.57 111.76 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (path /5C2F4527)
    (fp_text reference C6 (at 2.54 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 2.56 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.09 -1.31) (end 4.91 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 1.31) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 -1.31) (end 0.09 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 0.996) (end 0.09 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 -1.31) (end 4.91 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 0.996) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 6.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 1.6) (end 6.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5C335172) (tstamp 5C334957)
    (at 139.065 111.76 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (path /5C2F454F)
    (fp_text reference C7 (at 2.54 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 2.56 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.09 -1.31) (end 4.91 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 1.31) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 -1.31) (end 0.09 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 0.996) (end 0.09 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 -1.31) (end 4.91 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 0.996) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 6.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 1.6) (end 6.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.54 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5C33514D) (tstamp 5C33495D)
    (at 154.94 111.76 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (path /5C2F4586)
    (fp_text reference C8 (at 2.54 0 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100nF (at 2.5 2.56 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.15 -1.25) (end 0.15 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.15 1.25) (end 4.85 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 1.25) (end 4.85 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 4.85 -1.25) (end 0.15 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0.09 -1.31) (end 4.91 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 1.31) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 -1.31) (end 0.09 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.09 0.996) (end 0.09 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 -1.31) (end 4.91 -0.996) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.91 0.996) (end 4.91 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 6.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 1.6) (end 6.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.05 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5C335840) (tstamp 5C33498F)
    (at 145.415 68.58 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (path /5C2F5BA8)
    (fp_text reference J2 (at -12.065 0 540) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Barrel_Jack (at -6.2 -5.5 270) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1 -4.5) (end 1 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -4.5) (end 1 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -2) (end 2 -2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 -2) (end 2 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2 2) (end 1 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 2) (end 1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 4.75) (end -1 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 4.75) (end -1 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 6.75) (end -5 6.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 6.75) (end -5 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 4.75) (end -14 4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -14 4.75) (end -14 -4.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5 4.6) (end -13.8 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 4.6) (end -13.8 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 1.9) (end 0.9 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 4.6) (end -1 4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -13.8 -4.6) (end 0.9 -4.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.9 -4.6) (end 0.9 -2) (layer F.SilkS) (width 0.12))
    (fp_line (start -10.2 -4.5) (end -10.2 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 -4.5) (end -13.7 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start -13.7 4.5) (end 0.8 4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 4.5) (end 0.8 -4.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -4.5) (end -13.7 -4.5) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask))
  )

  (module Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm (layer F.Cu) (tedit 59650532) (tstamp 5C3349BA)
    (at 88.265 156.21 180)
    (descr "Through hole straight pin header, 1x39, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x39 2.54mm single row")
    (path /5C2F4F1A)
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RC6502_Backplane (at 0 98.85 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 97.79) (end -1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 97.79) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 97.85) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 98.3) (end 1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 98.3) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 48.26 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A15))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A14))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A13))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A12))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A11))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A10))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A9))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A8))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A7))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A6))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A5))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A4))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A3))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A2))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A1))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A0))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PHI2))
    (pad 20 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /RESET))
    (pad 21 thru_hole oval (at 0 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PHI0))
    (pad 22 thru_hole oval (at 0 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IRQ))
    (pad 23 thru_hole oval (at 0 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SPARE0))
    (pad 24 thru_hole oval (at 0 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /R/~W))
    (pad 25 thru_hole oval (at 0 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /RDY))
    (pad 26 thru_hole oval (at 0 63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SYNC))
    (pad 27 thru_hole oval (at 0 66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D0))
    (pad 28 thru_hole oval (at 0 68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D1))
    (pad 29 thru_hole oval (at 0 71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D2))
    (pad 30 thru_hole oval (at 0 73.66 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D3))
    (pad 31 thru_hole oval (at 0 76.2 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D4))
    (pad 32 thru_hole oval (at 0 78.74 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D5))
    (pad 33 thru_hole oval (at 0 81.28 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /D6))
    (pad 34 thru_hole oval (at 0 83.82 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /D7))
    (pad 35 thru_hole oval (at 0 86.36 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /TX))
    (pad 36 thru_hole oval (at 0 88.9 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /RX))
    (pad 37 thru_hole oval (at 0 91.44 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /NMI))
    (pad 38 thru_hole oval (at 0 93.98 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /SPARE1))
    (pad 39 thru_hole oval (at 0 96.52 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /SPARE2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x39_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm (layer F.Cu) (tedit 59650532) (tstamp 5C3349E5)
    (at 111.76 156.21 180)
    (descr "Through hole straight pin header, 1x39, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x39 2.54mm single row")
    (path /5C2F4E90)
    (fp_text reference J4 (at 0 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RC6502_Backplane (at 0 98.85 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 97.79) (end -1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 97.79) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 97.85) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 98.3) (end 1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 98.3) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 48.26 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A15))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A14))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A13))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A12))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A11))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A10))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A9))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A8))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A7))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A6))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A5))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A4))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A3))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A2))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A1))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A0))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PHI2))
    (pad 20 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /RESET))
    (pad 21 thru_hole oval (at 0 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PHI0))
    (pad 22 thru_hole oval (at 0 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IRQ))
    (pad 23 thru_hole oval (at 0 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SPARE0))
    (pad 24 thru_hole oval (at 0 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /R/~W))
    (pad 25 thru_hole oval (at 0 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /RDY))
    (pad 26 thru_hole oval (at 0 63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SYNC))
    (pad 27 thru_hole oval (at 0 66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D0))
    (pad 28 thru_hole oval (at 0 68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D1))
    (pad 29 thru_hole oval (at 0 71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D2))
    (pad 30 thru_hole oval (at 0 73.66 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D3))
    (pad 31 thru_hole oval (at 0 76.2 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D4))
    (pad 32 thru_hole oval (at 0 78.74 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D5))
    (pad 33 thru_hole oval (at 0 81.28 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /D6))
    (pad 34 thru_hole oval (at 0 83.82 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /D7))
    (pad 35 thru_hole oval (at 0 86.36 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /TX))
    (pad 36 thru_hole oval (at 0 88.9 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /RX))
    (pad 37 thru_hole oval (at 0 91.44 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /NMI))
    (pad 38 thru_hole oval (at 0 93.98 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /SPARE1))
    (pad 39 thru_hole oval (at 0 96.52 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /SPARE2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x39_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm (layer F.Cu) (tedit 5C61CC89) (tstamp 5C334A10)
    (at 135.255 156.21 180)
    (descr "Through hole straight pin header, 1x39, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x39 2.54mm single row")
    (path /5C2F4D1E)
    (fp_text reference J5 (at 0 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RC6502_Backplane (at 3.175 99.695 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 97.79) (end -1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 97.79) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 97.85) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 98.3) (end 1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 98.3) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 48.26 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A15))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A14))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A13))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A12))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A11))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A10))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A9))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A8))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A7))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A6))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A5))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A4))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A3))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A2))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A1))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A0))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PHI2))
    (pad 20 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /RESET))
    (pad 21 thru_hole oval (at 0 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PHI0))
    (pad 22 thru_hole oval (at 0 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IRQ))
    (pad 23 thru_hole oval (at 0 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SPARE0))
    (pad 24 thru_hole oval (at 0 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /R/~W))
    (pad 25 thru_hole oval (at 0 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /RDY))
    (pad 26 thru_hole oval (at 0 63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SYNC))
    (pad 27 thru_hole oval (at 0 66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D0))
    (pad 28 thru_hole oval (at 0 68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D1))
    (pad 29 thru_hole oval (at 0 71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D2))
    (pad 30 thru_hole oval (at 0 73.66 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D3))
    (pad 31 thru_hole oval (at 0 76.2 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D4))
    (pad 32 thru_hole oval (at 0 78.74 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D5))
    (pad 33 thru_hole oval (at 0 81.28 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /D6))
    (pad 34 thru_hole oval (at 0 83.82 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /D7))
    (pad 35 thru_hole oval (at 0 86.36 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /TX))
    (pad 36 thru_hole oval (at 0 88.9 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /RX))
    (pad 37 thru_hole oval (at 0 91.44 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /NMI))
    (pad 38 thru_hole oval (at 0 93.98 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /SPARE1))
    (pad 39 thru_hole oval (at 0 96.52 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /SPARE2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x39_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x39_Pitch2.54mm (layer F.Cu) (tedit 59650532) (tstamp 5C334A3B)
    (at 158.75 156.21 180)
    (descr "Through hole straight pin header, 1x39, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x39 2.54mm single row")
    (path /5C2E0F5B)
    (fp_text reference J6 (at 0 -2.33 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RC6502_Backplane (at 0 98.85 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 97.79) (end -1.27 97.79) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 97.79) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 97.85) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 97.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 98.3) (end 1.8 98.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 98.3) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 48.26 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /A15))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /A14))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /A13))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A12))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A11))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A10))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A9))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A8))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A7))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A6))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A5))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A4))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /A3))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /A2))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /A1))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A0))
    (pad 17 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 19 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PHI2))
    (pad 20 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /RESET))
    (pad 21 thru_hole oval (at 0 50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PHI0))
    (pad 22 thru_hole oval (at 0 53.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /IRQ))
    (pad 23 thru_hole oval (at 0 55.88 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SPARE0))
    (pad 24 thru_hole oval (at 0 58.42 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /R/~W))
    (pad 25 thru_hole oval (at 0 60.96 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /RDY))
    (pad 26 thru_hole oval (at 0 63.5 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SYNC))
    (pad 27 thru_hole oval (at 0 66.04 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D0))
    (pad 28 thru_hole oval (at 0 68.58 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D1))
    (pad 29 thru_hole oval (at 0 71.12 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D2))
    (pad 30 thru_hole oval (at 0 73.66 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D3))
    (pad 31 thru_hole oval (at 0 76.2 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /D4))
    (pad 32 thru_hole oval (at 0 78.74 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /D5))
    (pad 33 thru_hole oval (at 0 81.28 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /D6))
    (pad 34 thru_hole oval (at 0 83.82 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /D7))
    (pad 35 thru_hole oval (at 0 86.36 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /TX))
    (pad 36 thru_hole oval (at 0 88.9 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /RX))
    (pad 37 thru_hole oval (at 0 91.44 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /NMI))
    (pad 38 thru_hole oval (at 0 93.98 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /SPARE1))
    (pad 39 thru_hole oval (at 0 96.52 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /SPARE2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x39_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module mounting:Mounting (layer F.Cu) (tedit 594143BA) (tstamp 5C334B40)
    (at 69.85 153.67)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5C334F92)
    (fp_text reference J7 (at 0 -3.81) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Mounting (at 0 3.81) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask))
  )

  (module mounting:Mounting (layer F.Cu) (tedit 594143BA) (tstamp 5C334B45)
    (at 153.67 153.67)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5C3350AD)
    (fp_text reference J8 (at 0 -3.81) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Mounting (at 0 3.81) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask))
  )

  (module mounting:Mounting (layer F.Cu) (tedit 594143BA) (tstamp 5C334B4A)
    (at 153.67 62.23)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5C3350FF)
    (fp_text reference J9 (at 0 -3.81) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Mounting (at 0 3.81) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask))
  )

  (module mounting:Mounting (layer F.Cu) (tedit 594143BA) (tstamp 5C334B4F)
    (at 69.85 62.23)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (path /5C33514E)
    (fp_text reference J10 (at 0 -3.81) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Mounting (at 0 3.81) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2 0.8) (layer F.Fab) (width 0.1))
    (fp_circle (center 0 0) (end 2.6 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 0 -2.286) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.2) (layers *.Cu *.Mask))
  )

  (module TO_SOT_Packages_THT:TO-220-3_Horizontal (layer F.Cu) (tedit 5C61CE06) (tstamp 5C334B57)
    (at 147.32 77.47 180)
    (descr "TO-220-3, Horizontal, RM 2.54mm")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (path /5C2F5C17)
    (fp_text reference U1 (at 5.715 -5.08 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LM7805 (at 0.635 -5.08 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 5.715 -5.08 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.46 -13.06) (end -2.46 -19.46) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 -19.46) (end 7.54 -19.46) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 -19.46) (end 7.54 -13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 -13.06) (end -2.46 -13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 -3.81) (end -2.46 -13.06) (layer F.Fab) (width 0.1))
    (fp_line (start -2.46 -13.06) (end 7.54 -13.06) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 -13.06) (end 7.54 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 7.54 -3.81) (end -2.46 -3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -3.81) (end 0 0) (layer F.Fab) (width 0.1))
    (fp_line (start 2.54 -3.81) (end 2.54 0) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 -3.81) (end 5.08 0) (layer F.Fab) (width 0.1))
    (fp_line (start -2.58 -3.69) (end 7.66 -3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 -19.58) (end 7.66 -19.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.58 -19.58) (end -2.58 -3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.66 -19.58) (end 7.66 -3.69) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -3.69) (end 0 -1.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.54 -3.69) (end 2.54 -1.066) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.08 -3.69) (end 5.08 -1.066) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.71 -19.71) (end -2.71 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.71 1.15) (end 7.79 1.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 1.15) (end 7.79 -19.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.79 -19.71) (end -2.71 -19.71) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 2.54 -16.66) (end 4.39 -16.66) (layer F.Fab) (width 0.1))
    (pad 0 np_thru_hole oval (at 2.54 -16.66 180) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C61CE0C) (tstamp 5C335092)
    (at 146.05 85.725 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (path /5C2F5CB9)
    (fp_text reference JP1 (at 0 10.795 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value NO_REG (at 2.54 1.27 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 5.08 450) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5C61D2BF) (tstamp 5C61CD6D)
    (at 153.67 69.85 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (path /5C61CD3B)
    (fp_text reference D1 (at 1.27 9.525 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PWR_LED (at 1.27 12.065 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 1.27 0) (end -1.23 -1.469694) (angle 299.1) (layer F.Fab) (width 0.1))
    (fp_arc (start 1.27 0) (end -1.29 -1.54483) (angle 148.9) (layer F.SilkS) (width 0.12))
    (fp_arc (start 1.27 0) (end -1.29 1.54483) (angle -148.9) (layer F.SilkS) (width 0.12))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer F.Fab) (width 0.1))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.23 -1.469694) (end -1.23 1.469694) (layer F.Fab) (width 0.1))
    (fp_line (start -1.29 -1.545) (end -1.29 1.545) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.95 -3.25) (end -1.95 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 3.25) (end 4.5 3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 3.25) (end 4.5 -3.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.5 -3.25) (end -1.95 -3.25) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.27 9.525 180) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.2)))
    )
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C61D1EC) (tstamp 5C61CD73)
    (at 149.86 74.295 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (path /5C61D653)
    (fp_text reference R1 (at 6.985 0 360) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330 (at 3.81 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.93 0) (layer F.Fab) (width 0.1))
    (fp_line (start 10.16 0) (end 8.23 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.87 -1.31) (end 1.87 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.87 1.31) (end 8.29 1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 1.31) (end 8.29 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.29 -1.31) (end 1.87 -1.31) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.98 0) (end 1.87 0) (layer F.SilkS) (width 0.12))
    (fp_line (start 9.18 0) (end 8.29 0) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.05 -1.6) (end -1.05 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.05 1.6) (end 11.25 1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 1.6) (end 11.25 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 11.25 -1.6) (end -1.05 -1.6) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text "Center positive 7-12v\nCenter positive 5v (NO_REG)\n" (at 130.175 59.69 90) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify left mirror))
  )
  (gr_text PWR (at 153.67 72.39) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Revision B" (at 79.375 62.23) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text "RC6502 Computer Backplane\nhttps://hvetebolle.blogspot.com" (at 123.19 110.49 270) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "RC6502 Computer Backplane\nhttps://hvetebolle.blogspot.com" (at 99.695 110.49 90) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_line (start 149.225 155.2575) (end 149.098 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 149.225 156.5275) (end 149.098 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 144.78 156.5275) (end 144.907 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 144.78 155.2575) (end 144.907 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 125.73 156.5275) (end 125.603 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 125.73 155.2575) (end 125.603 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 121.285 156.5275) (end 121.412 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 121.285 155.2575) (end 121.412 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 102.235 155.2575) (end 102.108 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 102.235 156.5275) (end 102.108 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 97.79 156.5275) (end 97.917 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 97.79 155.2575) (end 97.917 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 78.74 156.5275) (end 78.613 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 78.74 155.2575) (end 78.613 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 74.295 156.5275) (end 74.422 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 74.295 155.2575) (end 74.422 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 62.1665 156.5275) (end 74.295 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 62.23 155.2575) (end 74.295 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 149.225 155.2575) (end 161.29 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 149.225 156.5275) (end 161.3535 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 125.73 156.5275) (end 144.78 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 125.73 155.2575) (end 144.78 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 121.285 156.5275) (end 102.235 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 102.235 155.2575) (end 121.285 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 78.74 156.5275) (end 97.79 156.5275) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 97.79 155.2575) (end 78.74 155.2575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 74.295 155.8925) (end 62.23 155.8925) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 97.79 155.8925) (end 78.74 155.8925) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 149.225 155.8925) (end 161.3535 155.8925) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 125.73 155.8925) (end 144.78 155.8925) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 102.235 155.8925) (end 121.285 155.8925) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 149.225 155.575) (end 149.225 156.21) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 144.78 156.21) (end 144.78 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 125.73 156.21) (end 125.73 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 121.285 156.21) (end 121.285 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 102.235 155.575) (end 102.235 156.21) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 97.79 156.21) (end 97.79 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 78.74 156.21) (end 78.74 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 74.295 156.21) (end 74.295 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 62.23 156.21) (end 74.295 156.21) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 74.295 155.575) (end 62.23 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 78.74 156.21) (end 97.79 156.21) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 97.79 155.575) (end 78.74 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 102.235 156.21) (end 121.285 156.21) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 121.285 155.575) (end 102.235 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 125.73 156.21) (end 144.78 156.21) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 144.78 155.575) (end 125.73 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 149.225 156.21) (end 161.29 156.21) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 161.29 155.575) (end 149.225 155.575) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_text "PIN 1" (at 147.066 155.956) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (gr_text "PIN 1" (at 76.454 155.956) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (gr_text "PIN 1" (at 123.444 155.956) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (gr_text "PIN 1" (at 100.076 155.956) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)))
  )
  (gr_text RX (at 67.31 67.31) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text TX (at 67.31 69.85) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text D7 (at 67.31 72.39) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text D6 (at 67.31 74.93) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text D5 (at 67.31 77.47) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text D4 (at 67.31 80.01) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text D3 (at 67.31 82.55) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text D2 (at 67.31 85.09) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text D1 (at 67.31 87.63) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text D0 (at 67.31 90.17) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text SYNC (at 67.31 92.71) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text RDY (at 67.31 95.25) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text R/~W (at 67.31 97.79) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text ~IRQ (at 67.31 102.87) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text Phi0 (at 67.31 105.41) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text RES (at 67.31 107.95) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A1 (at 67.31 120.65) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A2 (at 67.31 123.19) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A3 (at 67.31 125.73) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A4 (at 67.31 128.27) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A5 (at 67.31 130.81) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A6 (at 67.31 133.35) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A7 (at 67.31 135.89) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A9 (at 85.725 140.97) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A8 (at 67.31 138.43) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A10 (at 67.31 143.51) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A11 (at 67.31 146.05) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A12 (at 67.31 148.59) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A14 (at 85.725 153.67) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A13 (at 85.725 151.13) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A12 (at 85.725 148.59) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A11 (at 85.725 146.05) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A10 (at 85.725 143.51) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A9 (at 67.31 140.97) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify left))
  )
  (gr_text A8 (at 85.725 138.43) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A7 (at 85.725 135.89) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A6 (at 85.725 133.35) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A5 (at 85.725 130.81) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A4 (at 85.725 128.27) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A3 (at 85.725 125.73) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A2 (at 85.725 123.19) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A1 (at 85.725 120.65) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A0 (at 85.725 118.11) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text ~NMI (at 132.715 64.77) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RX (at 132.715 67.31) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text TX (at 132.715 69.85) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D7 (at 132.715 72.39) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D6 (at 132.715 74.93) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D5 (at 132.715 77.47) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D4 (at 132.715 80.01) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D3 (at 132.715 82.55) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D2 (at 132.715 85.09) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D1 (at 132.715 87.63) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D0 (at 132.715 90.17) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text SYNC (at 132.715 92.71) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RDY (at 156.21 95.25) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RDY (at 132.715 95.25) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text R/~W (at 156.21 97.79) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text R/~W (at 132.715 97.79) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text ~NMI (at 85.725 64.77) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RX (at 85.725 67.31) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text TX (at 85.725 69.85) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D7 (at 85.725 72.39) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D6 (at 85.725 74.93) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D5 (at 85.725 77.47) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D4 (at 85.725 80.01) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D3 (at 85.725 82.55) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D2 (at 85.725 85.09) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D1 (at 85.725 87.63) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D0 (at 85.725 90.17) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text SYNC (at 85.725 92.71) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RDY (at 85.725 95.25) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text R/~W (at 85.725 97.79) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text ~IRQ (at 85.725 102.87) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text Phi0 (at 85.725 105.41) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RES (at 85.725 107.95) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text Phi2 (at 85.725 110.49) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text GND (at 85.725 115.57) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text VCC (at 85.725 113.03) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text GND (at 132.715 115.57) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text VCC (at 132.715 113.03) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text Phi2 (at 132.715 110.49) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RES (at 156.21 107.95) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RES (at 132.715 107.95) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text Phi0 (at 156.21 105.41) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text Phi0 (at 132.715 105.41) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text ~IRQ (at 156.21 102.87) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text ~IRQ (at 132.715 102.87) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A14 (at 132.715 153.67) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A13 (at 156.21 150.495) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A13 (at 132.715 151.13) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A12 (at 156.21 148.59) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A12 (at 132.715 148.59) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A11 (at 156.21 146.05) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A11 (at 132.715 146.05) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A10 (at 156.21 143.51) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A10 (at 132.715 143.51) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A9 (at 156.21 140.97) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A9 (at 132.715 140.97) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A8 (at 156.21 138.43) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A8 (at 132.715 138.43) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A7 (at 156.21 135.89) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A7 (at 132.715 135.89) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A6 (at 156.21 133.35) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A6 (at 132.715 133.35) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A5 (at 156.21 130.81) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A5 (at 132.715 130.81) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A4 (at 156.21 128.27) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A4 (at 132.715 128.27) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A3 (at 156.21 125.73) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A3 (at 132.715 125.73) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A2 (at 156.21 123.19) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A2 (at 132.715 123.19) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A1 (at 156.21 120.65) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A1 (at 132.715 120.65) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A0 (at 132.715 118.11) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A14 (at 109.22 153.67) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A13 (at 109.22 151.13) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A12 (at 109.22 148.59) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A11 (at 109.22 146.05) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A10 (at 109.22 143.51) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A9 (at 109.22 140.97) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A8 (at 109.22 138.43) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A7 (at 109.22 135.89) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A6 (at 109.22 133.35) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A5 (at 109.22 130.81) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A4 (at 109.22 128.27) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A3 (at 109.22 125.73) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A2 (at 109.22 123.19) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A1 (at 109.22 120.65) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text A0 (at 109.22 118.11) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text GND (at 109.22 115.57) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text VCC (at 109.22 113.03) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text Phi2 (at 109.22 110.49) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RES (at 109.22 107.95) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text Phi0 (at 109.22 105.41) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text ~IRQ (at 109.22 102.87) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text R/~W (at 109.22 97.79) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RDY (at 109.22 95.25) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text SYNC (at 109.22 92.71) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D0 (at 109.22 90.17) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D1 (at 109.22 87.63) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D2 (at 109.22 85.09) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D3 (at 109.22 82.55) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D4 (at 109.22 80.01) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D5 (at 109.22 77.47) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D6 (at 109.22 74.93) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text D7 (at 109.22 72.39) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text TX (at 109.22 69.85) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text RX (at 109.22 67.31) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_text ~NMI (at 109.22 64.77) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.1)) (justify right))
  )
  (gr_line (start 62.23 156.845) (end 161.29 156.845) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 62.23 154.94) (end 161.29 154.94) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 62.23 59.69) (end 62.23 155.575) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.02 58.42) (end 63.5 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 156.21) (end 161.29 59.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.135 157.48) (end 160.02 157.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.02 156.21) (end 161.29 156.21) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 64.135 155.575) (end 64.135 157.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 63.5 59.69) (end 62.23 59.69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.02 59.69) (end 160.02 58.42) (angle 90) (layer Edge.Cuts) (width 0.15))

  (segment (start 144.145 95.25) (end 143.51 94.615) (width 0.25) (layer F.Cu) (net 0) (tstamp 5C335618))
  (segment (start 147.32 77.47) (end 147.32 84.455) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 147.32 84.455) (end 146.05 85.725) (width 0.25) (layer B.Cu) (net 1) (tstamp 5C61D19C))
  (segment (start 154.305 79.375) (end 154.305 78.105) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 153.67 77.47) (end 147.32 77.47) (width 0.25) (layer F.Cu) (net 1) (tstamp 5C61D132))
  (segment (start 154.305 78.105) (end 153.67 77.47) (width 0.25) (layer F.Cu) (net 1) (tstamp 5C61D131))
  (segment (start 145.415 68.58) (end 145.415 72.39) (width 0.25) (layer F.Cu) (net 1))
  (segment (start 147.32 73.66) (end 147.32 77.47) (width 0.25) (layer F.Cu) (net 1) (tstamp 5C61D124))
  (segment (start 146.685 73.025) (end 147.32 73.66) (width 0.25) (layer F.Cu) (net 1) (tstamp 5C61D123))
  (segment (start 146.05 73.025) (end 146.685 73.025) (width 0.25) (layer F.Cu) (net 1) (tstamp 5C61D122))
  (segment (start 145.415 72.39) (end 146.05 73.025) (width 0.25) (layer F.Cu) (net 1) (tstamp 5C61D121))
  (segment (start 151.67 85.09) (end 151.67 79.51) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 151.67 79.51) (end 151.805 79.375) (width 0.25) (layer B.Cu) (net 2) (tstamp 5C61D401))
  (segment (start 151.67 85.09) (end 151.67 88.885) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 151.67 88.885) (end 151.765 88.98) (width 0.25) (layer B.Cu) (net 2) (tstamp 5C61D3FE))
  (segment (start 151.67 79.51) (end 151.805 79.375) (width 0.25) (layer B.Cu) (net 2) (tstamp 5C61D3F8))
  (segment (start 145.415 62.58) (end 138.715 62.58) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 139.7 70.485) (end 139.7 74.295) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C61D12D))
  (segment (start 137.795 68.58) (end 139.7 70.485) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C61D12B))
  (segment (start 137.795 63.5) (end 137.795 68.58) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C61D12A))
  (segment (start 138.715 62.58) (end 137.795 63.5) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C61D129))
  (segment (start 151.805 79.375) (end 145.415 79.375) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 144.78 78.74) (end 145.415 79.375) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C61D0F4))
  (segment (start 144.78 78.74) (end 144.78 77.47) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 139.7 74.295) (end 144.145 74.295) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 144.145 74.295) (end 144.78 74.93) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C61D0F0))
  (segment (start 144.78 74.93) (end 144.78 77.47) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C61D0F1))
  (segment (start 149.86 116.84) (end 149.86 95.25) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 149.86 93.345) (end 149.86 95.25) (width 0.25) (layer B.Cu) (net 2) (tstamp 5C33556B))
  (segment (start 151.765 90.805) (end 151.765 88.98) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 149.86 92.71) (end 150.495 92.075) (width 0.25) (layer B.Cu) (net 2) (tstamp 5C33557D))
  (segment (start 149.86 93.345) (end 149.86 92.71) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 151.13 92.075) (end 151.765 91.44) (width 0.25) (layer B.Cu) (net 2) (tstamp 5C335585))
  (segment (start 151.765 91.44) (end 151.765 90.805) (width 0.25) (layer B.Cu) (net 2) (tstamp 5C335586))
  (segment (start 150.495 92.075) (end 151.13 92.075) (width 0.25) (layer B.Cu) (net 2))
  (via (at 149.86 116.84) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 2))
  (segment (start 149.86 116.84) (end 149.86 116.76) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C336140))
  (segment (start 149.86 116.76) (end 149.86 116.84) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C336141))
  (segment (start 149.86 116.84) (end 149.86 116.76) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C336143))
  (segment (start 139.065 116.76) (end 149.86 116.76) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 149.86 116.76) (end 154.94 116.76) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C336144))
  (segment (start 115.57 116.76) (end 132.16 116.76) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 133.35 115.57) (end 135.255 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C336126))
  (segment (start 132.16 116.76) (end 133.35 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C336124))
  (segment (start 92.075 116.76) (end 108.665 116.76) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 109.855 115.57) (end 111.76 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C336120))
  (segment (start 108.665 116.76) (end 109.855 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C33611E))
  (segment (start 68.58 116.76) (end 85.17 116.76) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 86.36 115.57) (end 88.265 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C336114))
  (segment (start 85.17 116.76) (end 86.36 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C336112))
  (segment (start 68.58 116.76) (end 68.5 116.76) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 68.5 116.76) (end 67.31 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C3360D8))
  (segment (start 67.31 115.57) (end 64.77 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C3360D9))
  (segment (start 92.075 116.76) (end 91.995 116.76) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 91.995 116.76) (end 90.805 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C3360CD))
  (segment (start 90.805 115.57) (end 88.265 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C3360CE))
  (segment (start 115.57 116.76) (end 115.49 116.76) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 115.49 116.76) (end 114.3 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C3360C8))
  (segment (start 114.3 115.57) (end 111.76 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C3360C9))
  (segment (start 139.065 116.76) (end 138.985 116.76) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 138.985 116.76) (end 137.795 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C3360C0))
  (segment (start 137.795 115.57) (end 135.255 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C3360C1))
  (segment (start 154.94 116.76) (end 155.02 116.76) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 155.02 116.76) (end 156.21 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C33605C))
  (segment (start 156.21 115.57) (end 158.75 115.57) (width 0.25) (layer F.Cu) (net 2) (tstamp 5C33605D))
  (segment (start 151.67 88.885) (end 151.765 88.98) (width 0.25) (layer B.Cu) (net 2) (tstamp 5C33555F))
  (segment (start 153.67 92.71) (end 153.67 85.09) (width 0.25) (layer B.Cu) (net 3) (tstamp 5C335565))
  (segment (start 152.4 83.82) (end 153.67 85.09) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C61D1BD))
  (segment (start 151.765 71.755) (end 151.765 72.39) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 142.875 73.025) (end 142.24 73.66) (width 0.25) (layer B.Cu) (net 3) (tstamp 5C61D27F))
  (segment (start 147.955 73.025) (end 142.875 73.025) (width 0.25) (layer B.Cu) (net 3) (tstamp 5C61D27E))
  (via (at 147.955 73.025) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 3))
  (segment (start 151.13 73.025) (end 147.955 73.025) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C61D27B))
  (segment (start 151.765 72.39) (end 151.13 73.025) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C61D279))
  (segment (start 153.67 67.31) (end 152.4 67.31) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 142.24 73.66) (end 142.24 77.47) (width 0.25) (layer B.Cu) (net 3) (tstamp 5C61D282))
  (segment (start 151.765 67.945) (end 151.765 71.755) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C61D24D))
  (segment (start 152.4 67.31) (end 151.765 67.945) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C61D24C))
  (via (at 144.145 83.82) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 3))
  (segment (start 142.24 77.47) (end 142.24 78.74) (width 0.25) (layer B.Cu) (net 3) (tstamp 5C61D1CB))
  (segment (start 144.145 80.645) (end 142.24 78.74) (width 0.25) (layer B.Cu) (net 3) (tstamp 5C61D1C8))
  (segment (start 144.145 80.645) (end 144.145 83.82) (width 0.25) (layer B.Cu) (net 3) (tstamp 5C61D1C7))
  (segment (start 143.51 85.725) (end 143.51 84.455) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 143.51 84.455) (end 144.145 83.82) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C61D1B9))
  (segment (start 144.145 83.82) (end 152.4 83.82) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C61D1BB))
  (segment (start 151.765 93.98) (end 151.765 111.76) (width 0.25) (layer B.Cu) (net 3))
  (via (at 151.765 111.76) (size 0.6) (drill 0.4) (layers F.Cu B.Cu) (net 3))
  (segment (start 139.065 111.76) (end 151.765 111.76) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 151.765 111.76) (end 154.94 111.76) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C33614A))
  (segment (start 115.57 111.76) (end 132.08 111.76) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 133.35 113.03) (end 135.255 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C33612C))
  (segment (start 132.08 111.76) (end 133.35 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C33612A))
  (segment (start 92.075 111.76) (end 108.585 111.76) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 109.855 113.03) (end 111.76 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C33611A))
  (segment (start 108.585 111.76) (end 109.855 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C336118))
  (segment (start 68.58 111.76) (end 85.09 111.76) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 86.36 113.03) (end 88.265 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C33610E))
  (segment (start 85.09 111.76) (end 86.36 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C33610C))
  (segment (start 68.58 111.76) (end 67.31 113.03) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 67.31 113.03) (end 64.77 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C3360D5))
  (segment (start 92.075 111.76) (end 90.805 113.03) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 90.805 113.03) (end 88.265 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C3360D2))
  (segment (start 115.57 111.76) (end 114.3 113.03) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 114.3 113.03) (end 111.76 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C3360C5))
  (segment (start 139.065 111.76) (end 137.795 113.03) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 137.795 113.03) (end 135.255 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C3360BD))
  (segment (start 154.94 111.76) (end 156.21 113.03) (width 0.25) (layer F.Cu) (net 3))
  (segment (start 156.21 113.03) (end 158.75 113.03) (width 0.25) (layer F.Cu) (net 3) (tstamp 5C336061))
  (segment (start 151.765 93.98) (end 152.4 93.98) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 152.4 93.98) (end 153.035 93.345) (width 0.25) (layer B.Cu) (net 3) (tstamp 5C335564))
  (segment (start 153.035 93.345) (end 153.67 92.71) (width 0.25) (layer B.Cu) (net 3) (tstamp 5C33557B))
  (segment (start 135.255 156.21) (end 135.89 156.21) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 135.89 156.21) (end 136.525 156.845) (width 0.25) (layer F.Cu) (net 4) (tstamp 5C334FB4))
  (segment (start 158.115 156.845) (end 158.75 156.21) (width 0.25) (layer F.Cu) (net 4) (tstamp 5C334FB6))
  (segment (start 136.525 156.845) (end 158.115 156.845) (width 0.25) (layer F.Cu) (net 4) (tstamp 5C334FB5))
  (segment (start 111.76 156.21) (end 135.255 156.21) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 88.265 156.21) (end 111.76 156.21) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 64.77 156.21) (end 65.405 156.21) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 65.405 156.21) (end 66.04 156.845) (width 0.25) (layer F.Cu) (net 4) (tstamp 5C334FAB))
  (segment (start 66.04 156.845) (end 87.63 156.845) (width 0.25) (layer F.Cu) (net 4) (tstamp 5C334FAC))
  (segment (start 87.63 156.845) (end 88.265 156.21) (width 0.25) (layer F.Cu) (net 4) (tstamp 5C334FAD))
  (segment (start 88.265 153.67) (end 111.76 153.67) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 111.76 153.67) (end 135.255 153.67) (width 0.25) (layer F.Cu) (net 5))
  (segment (start 158.75 153.67) (end 158.115 153.67) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 158.115 153.67) (end 156.845 154.94) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FC5))
  (segment (start 156.845 154.94) (end 156.845 156.21) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FC6))
  (segment (start 156.845 156.21) (end 156.21 156.845) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FC7))
  (segment (start 156.21 156.845) (end 137.795 156.845) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FC8))
  (segment (start 137.795 156.845) (end 137.16 156.21) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FC9))
  (segment (start 137.16 156.21) (end 137.16 154.94) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FCA))
  (segment (start 137.16 154.94) (end 135.89 153.67) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FCB))
  (segment (start 135.89 153.67) (end 135.255 153.67) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FCC))
  (segment (start 87.63 153.67) (end 86.36 154.94) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 86.36 156.21) (end 86.36 154.94) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FBF))
  (segment (start 85.725 156.845) (end 86.36 156.21) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FBE))
  (segment (start 67.31 156.845) (end 85.725 156.845) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FBD))
  (segment (start 66.675 156.21) (end 67.31 156.845) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FBC))
  (segment (start 66.675 154.94) (end 66.675 156.21) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FBA))
  (segment (start 66.675 154.94) (end 65.405 153.67) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FB9))
  (segment (start 87.63 153.67) (end 88.265 153.67) (width 0.25) (layer B.Cu) (net 5) (tstamp 5C334FC2))
  (segment (start 64.77 153.67) (end 65.405 153.67) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 111.76 151.13) (end 135.255 151.13) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 88.265 151.13) (end 111.76 151.13) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 156.845 150.495) (end 157.48 151.13) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 136.525 151.13) (end 135.255 151.13) (width 0.25) (layer F.Cu) (net 6) (tstamp 5C334FDC))
  (segment (start 137.16 150.495) (end 136.525 151.13) (width 0.25) (layer F.Cu) (net 6) (tstamp 5C334FDB))
  (segment (start 156.845 150.495) (end 137.16 150.495) (width 0.25) (layer F.Cu) (net 6) (tstamp 5C334FE4))
  (segment (start 157.48 151.13) (end 158.75 151.13) (width 0.25) (layer F.Cu) (net 6) (tstamp 5C334FE6))
  (segment (start 64.77 151.13) (end 66.04 151.13) (width 0.25) (layer F.Cu) (net 6))
  (segment (start 66.04 151.13) (end 66.675 150.495) (width 0.25) (layer F.Cu) (net 6) (tstamp 5C334FD3))
  (segment (start 66.675 150.495) (end 86.36 150.495) (width 0.25) (layer F.Cu) (net 6) (tstamp 5C334FD4))
  (segment (start 86.36 150.495) (end 86.995 151.13) (width 0.25) (layer F.Cu) (net 6) (tstamp 5C334FD5))
  (segment (start 86.995 151.13) (end 88.265 151.13) (width 0.25) (layer F.Cu) (net 6) (tstamp 5C334FD6))
  (segment (start 135.255 148.59) (end 158.75 148.59) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 111.76 148.59) (end 135.255 148.59) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 88.265 148.59) (end 111.76 148.59) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 64.77 148.59) (end 88.265 148.59) (width 0.25) (layer F.Cu) (net 7))
  (segment (start 135.255 146.05) (end 158.75 146.05) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 111.76 146.05) (end 135.255 146.05) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 88.265 146.05) (end 111.76 146.05) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 64.77 146.05) (end 88.265 146.05) (width 0.25) (layer F.Cu) (net 8))
  (segment (start 135.255 143.51) (end 158.75 143.51) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 135.255 143.51) (end 111.76 143.51) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 88.265 143.51) (end 111.76 143.51) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 88.265 143.51) (end 64.77 143.51) (width 0.25) (layer F.Cu) (net 9))
  (segment (start 135.255 140.97) (end 158.75 140.97) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 111.76 140.97) (end 135.255 140.97) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 88.265 140.97) (end 111.76 140.97) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 64.77 140.97) (end 88.265 140.97) (width 0.25) (layer F.Cu) (net 10))
  (segment (start 135.255 138.43) (end 158.75 138.43) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 111.76 138.43) (end 135.255 138.43) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 88.265 138.43) (end 111.76 138.43) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 64.77 138.43) (end 88.265 138.43) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 135.255 135.89) (end 158.75 135.89) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 135.255 135.89) (end 111.76 135.89) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 88.265 135.89) (end 111.76 135.89) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 64.77 135.89) (end 88.265 135.89) (width 0.25) (layer F.Cu) (net 12))
  (segment (start 135.255 133.35) (end 158.75 133.35) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 111.76 133.35) (end 135.255 133.35) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 88.265 133.35) (end 111.76 133.35) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 64.77 133.35) (end 88.265 133.35) (width 0.25) (layer F.Cu) (net 13))
  (segment (start 64.77 130.81) (end 88.265 130.81) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 88.265 130.81) (end 111.76 130.81) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 111.76 130.81) (end 135.255 130.81) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 135.255 130.81) (end 158.75 130.81) (width 0.25) (layer F.Cu) (net 14))
  (segment (start 88.265 128.27) (end 64.77 128.27) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 111.76 128.27) (end 88.265 128.27) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 135.255 128.27) (end 111.76 128.27) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 158.75 128.27) (end 135.255 128.27) (width 0.25) (layer F.Cu) (net 15))
  (segment (start 64.77 125.73) (end 88.265 125.73) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 88.265 125.73) (end 111.76 125.73) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 111.76 125.73) (end 135.255 125.73) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 135.255 125.73) (end 158.75 125.73) (width 0.25) (layer F.Cu) (net 16))
  (segment (start 88.265 123.19) (end 64.77 123.19) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 111.76 123.19) (end 88.265 123.19) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 111.76 123.19) (end 135.255 123.19) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 158.75 123.19) (end 135.255 123.19) (width 0.25) (layer F.Cu) (net 17))
  (segment (start 64.77 120.65) (end 88.265 120.65) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 88.265 120.65) (end 111.76 120.65) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 111.76 120.65) (end 135.255 120.65) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 135.255 120.65) (end 158.75 120.65) (width 0.25) (layer F.Cu) (net 18))
  (segment (start 88.265 118.11) (end 64.77 118.11) (width 0.25) (layer F.Cu) (net 19))
  (segment (start 111.76 118.11) (end 88.265 118.11) (width 0.25) (layer F.Cu) (net 19))
  (segment (start 135.255 118.11) (end 111.76 118.11) (width 0.25) (layer F.Cu) (net 19))
  (segment (start 158.75 118.11) (end 135.255 118.11) (width 0.25) (layer F.Cu) (net 19))
  (segment (start 111.76 110.49) (end 135.255 110.49) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 135.255 110.49) (end 158.75 110.49) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 88.265 110.49) (end 111.76 110.49) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 64.77 110.49) (end 88.265 110.49) (width 0.25) (layer F.Cu) (net 20))
  (segment (start 135.255 107.95) (end 158.75 107.95) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 111.76 107.95) (end 135.255 107.95) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 88.265 107.95) (end 111.76 107.95) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 64.77 107.95) (end 88.265 107.95) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 135.255 105.41) (end 158.75 105.41) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 135.255 105.41) (end 111.76 105.41) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 88.265 105.41) (end 111.76 105.41) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 88.265 105.41) (end 64.77 105.41) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 135.255 102.87) (end 158.75 102.87) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 111.76 102.87) (end 135.255 102.87) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 111.76 102.87) (end 88.265 102.87) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 64.77 102.87) (end 88.265 102.87) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 87.63 102.87) (end 88.265 102.87) (width 0.25) (layer F.Cu) (net 23) (tstamp 5C335416))
  (segment (start 135.255 100.33) (end 158.75 100.33) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 135.255 100.33) (end 111.76 100.33) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 88.265 100.33) (end 111.76 100.33) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 64.77 100.33) (end 88.265 100.33) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 87.47 100.33) (end 88.265 100.33) (width 0.25) (layer F.Cu) (net 24) (tstamp 5C33541A))
  (segment (start 141.605 99.695) (end 137.795 99.695) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 137.16 98.425) (end 136.525 97.79) (width 0.25) (layer F.Cu) (net 25) (tstamp 5C61D09E))
  (segment (start 137.16 99.06) (end 137.16 98.425) (width 0.25) (layer F.Cu) (net 25) (tstamp 5C61D09D))
  (segment (start 137.795 99.695) (end 137.16 99.06) (width 0.25) (layer F.Cu) (net 25) (tstamp 5C61D09C))
  (segment (start 153.035 98.425) (end 153.035 99.06) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 152.4 99.695) (end 141.605 99.695) (width 0.25) (layer F.Cu) (net 25) (tstamp 5C61D08A))
  (segment (start 153.035 99.06) (end 152.4 99.695) (width 0.25) (layer F.Cu) (net 25) (tstamp 5C61D089))
  (segment (start 135.255 97.79) (end 136.525 97.79) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 153.67 97.79) (end 153.035 98.425) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 153.67 97.79) (end 158.75 97.79) (width 0.25) (layer F.Cu) (net 25) (tstamp 5C335511))
  (segment (start 111.76 97.79) (end 135.255 97.79) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 88.265 97.79) (end 111.76 97.79) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 64.77 97.79) (end 88.265 97.79) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 142.24 99.06) (end 138.43 99.06) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 137.795 97.79) (end 137.16 97.155) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C61D0A5))
  (segment (start 137.795 98.425) (end 137.795 97.79) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C61D0A4))
  (segment (start 138.43 99.06) (end 137.795 98.425) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C61D0A3))
  (segment (start 152.4 98.609998) (end 152.4 97.79) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C61D092))
  (segment (start 151.949998 99.06) (end 152.4 98.609998) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C61D091))
  (segment (start 142.24 99.06) (end 151.949998 99.06) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C61D090))
  (segment (start 136.525 95.885) (end 135.89 95.25) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C335530))
  (segment (start 136.525 96.52) (end 136.525 95.885) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C33552F))
  (segment (start 137.16 97.155) (end 136.525 96.52) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C33552E))
  (segment (start 135.89 95.25) (end 135.255 95.25) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C335531))
  (segment (start 158.75 95.25) (end 158.115 95.25) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 158.115 95.25) (end 157.48 95.885) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C33551E))
  (segment (start 153.035 97.155) (end 152.4 97.79) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C335522))
  (segment (start 156.845 97.155) (end 153.035 97.155) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C335521))
  (segment (start 157.48 96.52) (end 156.845 97.155) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C335520))
  (segment (start 157.48 95.885) (end 157.48 96.52) (width 0.25) (layer F.Cu) (net 26) (tstamp 5C33551F))
  (segment (start 111.76 95.25) (end 135.255 95.25) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 111.76 95.25) (end 88.265 95.25) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 88.265 95.25) (end 64.77 95.25) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 151.13 98.425) (end 142.875 98.425) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 157.48 92.71) (end 156.845 93.345) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C33558B))
  (segment (start 156.845 93.345) (end 156.845 96.069998) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C33558C))
  (segment (start 156.845 96.069998) (end 156.394998 96.52) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C33558D))
  (segment (start 156.394998 96.52) (end 152.4 96.52) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C33558E))
  (segment (start 152.4 96.52) (end 151.765 97.155) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C33558F))
  (segment (start 137.16 93.345) (end 136.525 92.71) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C335595))
  (segment (start 137.16 95.885) (end 137.16 93.345) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C335594))
  (segment (start 137.795 96.52) (end 137.16 95.885) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C335593))
  (segment (start 135.255 92.71) (end 136.525 92.71) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C335596))
  (segment (start 157.48 92.71) (end 158.75 92.71) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 151.13 98.425) (end 151.765 97.79) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C61D098))
  (segment (start 151.765 97.79) (end 151.765 97.155) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C61D099))
  (segment (start 139.065 98.425) (end 138.43 97.79) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C61D0A8))
  (segment (start 138.43 97.79) (end 138.43 97.155) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C61D0A9))
  (segment (start 138.43 97.155) (end 137.795 96.52) (width 0.25) (layer F.Cu) (net 27) (tstamp 5C61D0AA))
  (segment (start 142.875 98.425) (end 139.065 98.425) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 111.76 92.71) (end 135.255 92.71) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 88.265 92.71) (end 111.76 92.71) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 64.77 92.71) (end 88.265 92.71) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 138.43 95.885) (end 139.065 96.52) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 151.13 97.155) (end 151.13 96.52) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C61D0B1))
  (segment (start 150.495 97.79) (end 151.13 97.155) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C61D0B0))
  (segment (start 139.7 97.79) (end 150.495 97.79) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C61D0AF))
  (segment (start 139.065 97.155) (end 139.7 97.79) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C61D0AE))
  (segment (start 139.065 96.52) (end 139.065 97.155) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C61D0AD))
  (segment (start 158.75 90.17) (end 156.845 90.17) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 137.16 90.17) (end 135.255 90.17) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C3355A4))
  (segment (start 137.795 90.805) (end 137.16 90.17) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C3355A3))
  (segment (start 137.795 95.25) (end 137.795 90.805) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C3355A2))
  (segment (start 138.43 95.885) (end 137.795 95.25) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C3355A1))
  (segment (start 151.765 95.885) (end 151.13 96.52) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C33559D))
  (segment (start 155.575 95.885) (end 151.765 95.885) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C33559C))
  (segment (start 156.21 95.25) (end 155.575 95.885) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C33559B))
  (segment (start 156.21 90.805) (end 156.21 95.25) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C33559A))
  (segment (start 156.845 90.17) (end 156.21 90.805) (width 0.25) (layer F.Cu) (net 28) (tstamp 5C335599))
  (segment (start 135.255 90.17) (end 111.76 90.17) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 111.76 90.17) (end 88.265 90.17) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 88.265 90.17) (end 64.77 90.17) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 154.94 95.25) (end 151.13 95.25) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 155.575 94.615) (end 154.94 95.25) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C3355E9))
  (segment (start 155.575 88.265) (end 155.575 94.615) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C3355E7))
  (segment (start 156.21 87.63) (end 155.575 88.265) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C3355E6))
  (segment (start 158.75 87.63) (end 156.21 87.63) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 149.86 97.155) (end 150.495 96.52) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C61D0C7))
  (segment (start 150.495 96.52) (end 150.495 95.885) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C61D0C8))
  (segment (start 150.495 95.885) (end 151.13 95.25) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C61D0C9))
  (segment (start 139.065 95.25) (end 139.7 95.885) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 139.7 96.52) (end 140.335 97.155) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C61D0B9))
  (segment (start 139.7 95.885) (end 139.7 96.52) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C61D0B8))
  (segment (start 137.795 87.63) (end 135.255 87.63) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C3355F8))
  (segment (start 138.43 88.265) (end 137.795 87.63) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C3355F5))
  (segment (start 138.43 94.615) (end 138.43 88.265) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C3355F3))
  (segment (start 139.065 95.25) (end 138.43 94.615) (width 0.25) (layer F.Cu) (net 29) (tstamp 5C3355F2))
  (segment (start 140.335 97.155) (end 149.86 97.155) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 111.76 87.63) (end 135.255 87.63) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 88.265 87.63) (end 111.76 87.63) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 64.77 87.63) (end 88.265 87.63) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 155.575 85.09) (end 154.94 85.725) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C335603))
  (segment (start 158.75 85.09) (end 155.575 85.09) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 154.94 85.725) (end 154.94 92.075) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C335606))
  (segment (start 139.7 94.615) (end 140.335 95.25) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 149.86 95.885) (end 149.86 94.615) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C61D0D3))
  (segment (start 149.225 96.52) (end 149.86 95.885) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C61D0D2))
  (segment (start 140.97 96.52) (end 149.225 96.52) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C61D0D1))
  (segment (start 140.335 95.885) (end 140.97 96.52) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C61D0D0))
  (segment (start 140.335 95.25) (end 140.335 95.885) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C61D0CF))
  (segment (start 154.94 92.075) (end 154.305 92.71) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C33560C))
  (segment (start 154.305 92.71) (end 150.495 92.71) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C33560E))
  (segment (start 150.495 92.71) (end 149.86 93.345) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C335612))
  (segment (start 149.86 93.345) (end 149.86 94.615) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C335614))
  (segment (start 138.43 85.09) (end 135.255 85.09) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C335623))
  (segment (start 139.065 85.725) (end 138.43 85.09) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C335621))
  (segment (start 139.065 93.98) (end 139.065 85.725) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C33561E))
  (segment (start 139.7 94.615) (end 139.065 93.98) (width 0.25) (layer F.Cu) (net 30) (tstamp 5C33561D))
  (segment (start 135.255 85.09) (end 111.76 85.09) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 111.76 85.09) (end 88.265 85.09) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 88.265 85.09) (end 64.77 85.09) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 137.16 83.185) (end 157.48 83.185) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 136.525 82.55) (end 137.16 83.185) (width 0.25) (layer F.Cu) (net 31) (tstamp 5C335697))
  (segment (start 135.255 82.55) (end 136.525 82.55) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 157.48 83.185) (end 158.115 83.185) (width 0.25) (layer F.Cu) (net 31) (tstamp 5C3356E4))
  (segment (start 158.115 83.185) (end 158.75 82.55) (width 0.25) (layer F.Cu) (net 31) (tstamp 5C3356E5))
  (segment (start 111.76 82.55) (end 135.255 82.55) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 88.265 82.55) (end 111.76 82.55) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 64.77 82.55) (end 88.265 82.55) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 156.845 81.915) (end 156.21 82.55) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 136.525 80.01) (end 137.16 80.645) (width 0.25) (layer F.Cu) (net 32) (tstamp 5C3356A9))
  (segment (start 137.16 80.645) (end 137.16 81.915) (width 0.25) (layer F.Cu) (net 32) (tstamp 5C3356AA))
  (segment (start 137.16 81.915) (end 137.795 82.55) (width 0.25) (layer F.Cu) (net 32) (tstamp 5C3356AB))
  (segment (start 158.75 80.01) (end 156.845 81.915) (width 0.25) (layer F.Cu) (net 32) (tstamp 5C3356EE))
  (segment (start 136.525 80.01) (end 135.255 80.01) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 156.21 82.55) (end 137.795 82.55) (width 0.25) (layer F.Cu) (net 32) (tstamp 5C61D17B))
  (segment (start 135.255 80.01) (end 111.76 80.01) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 111.76 80.01) (end 88.265 80.01) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 88.265 80.01) (end 64.77 80.01) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 138.43 81.915) (end 155.575 81.915) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 138.43 81.915) (end 137.795 81.28) (width 0.25) (layer F.Cu) (net 33) (tstamp 5C3356B2))
  (segment (start 137.795 81.28) (end 137.795 78.105) (width 0.25) (layer F.Cu) (net 33) (tstamp 5C3356B3))
  (segment (start 137.795 78.105) (end 137.16 77.47) (width 0.25) (layer F.Cu) (net 33) (tstamp 5C3356B4))
  (segment (start 135.255 77.47) (end 137.16 77.47) (width 0.25) (layer F.Cu) (net 33) (tstamp 5C3356B5))
  (segment (start 155.575 81.915) (end 156.21 81.28) (width 0.25) (layer F.Cu) (net 33) (tstamp 5C61D16E))
  (segment (start 157.48 77.47) (end 156.845 78.105) (width 0.25) (layer F.Cu) (net 33) (tstamp 5C335689))
  (segment (start 156.845 78.105) (end 156.845 80.645) (width 0.25) (layer F.Cu) (net 33) (tstamp 5C33568D))
  (segment (start 156.845 80.645) (end 156.21 81.28) (width 0.25) (layer F.Cu) (net 33) (tstamp 5C33568E))
  (segment (start 158.75 77.47) (end 157.48 77.47) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 111.76 77.47) (end 135.255 77.47) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 88.265 77.47) (end 111.76 77.47) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 64.77 77.47) (end 88.265 77.47) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 155.575 80.645) (end 154.94 81.28) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 139.065 81.28) (end 138.43 80.645) (width 0.25) (layer F.Cu) (net 34) (tstamp 5C3356D3))
  (segment (start 138.43 80.645) (end 138.43 75.565) (width 0.25) (layer F.Cu) (net 34) (tstamp 5C3356D4))
  (segment (start 138.43 75.565) (end 137.795 74.93) (width 0.25) (layer F.Cu) (net 34) (tstamp 5C3356D5))
  (segment (start 135.255 74.93) (end 137.795 74.93) (width 0.25) (layer F.Cu) (net 34) (tstamp 5C3356DA))
  (segment (start 156.21 76.2) (end 156.21 80.01) (width 0.25) (layer F.Cu) (net 34) (tstamp 5C3356C6))
  (segment (start 156.21 80.01) (end 155.575 80.645) (width 0.25) (layer F.Cu) (net 34) (tstamp 5C3356C8))
  (segment (start 157.48 74.93) (end 158.75 74.93) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 157.48 74.93) (end 156.21 76.2) (width 0.25) (layer F.Cu) (net 34) (tstamp 5C3356C4))
  (segment (start 154.94 81.28) (end 139.065 81.28) (width 0.25) (layer F.Cu) (net 34) (tstamp 5C61D168))
  (segment (start 135.255 74.93) (end 111.76 74.93) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 111.76 74.93) (end 88.265 74.93) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 88.265 74.93) (end 64.77 74.93) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 158.75 72.39) (end 135.255 72.39) (width 0.25) (layer B.Cu) (net 35))
  (segment (start 111.76 72.39) (end 135.255 72.39) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 88.265 72.39) (end 111.76 72.39) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 64.77 72.39) (end 88.265 72.39) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 148.59 71.755) (end 156.845 71.755) (width 0.25) (layer B.Cu) (net 36))
  (segment (start 156.845 71.755) (end 158.75 69.85) (width 0.25) (layer B.Cu) (net 36) (tstamp 5C61D111))
  (segment (start 136.525 69.85) (end 135.255 69.85) (width 0.25) (layer B.Cu) (net 36) (tstamp 5C3357A1))
  (segment (start 138.43 71.755) (end 136.525 69.85) (width 0.25) (layer B.Cu) (net 36) (tstamp 5C33579C))
  (segment (start 148.59 71.755) (end 138.43 71.755) (width 0.25) (layer B.Cu) (net 36) (tstamp 5C335799))
  (segment (start 135.255 69.85) (end 111.76 69.85) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 111.76 69.85) (end 88.265 69.85) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 88.265 69.85) (end 64.77 69.85) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 147.955 71.12) (end 156.21 71.12) (width 0.25) (layer B.Cu) (net 37))
  (segment (start 156.845 69.215) (end 158.75 67.31) (width 0.25) (layer B.Cu) (net 37) (tstamp 5C61D118))
  (segment (start 156.845 70.485) (end 156.845 69.215) (width 0.25) (layer B.Cu) (net 37) (tstamp 5C61D117))
  (segment (start 156.21 71.12) (end 156.845 70.485) (width 0.25) (layer B.Cu) (net 37) (tstamp 5C61D116))
  (segment (start 147.955 71.12) (end 139.065 71.12) (width 0.25) (layer B.Cu) (net 37) (tstamp 5C33577D))
  (segment (start 139.065 71.12) (end 137.16 69.215) (width 0.25) (layer B.Cu) (net 37) (tstamp 5C33577F))
  (segment (start 137.16 69.215) (end 137.16 67.945) (width 0.25) (layer B.Cu) (net 37) (tstamp 5C335786))
  (segment (start 137.16 67.945) (end 136.525 67.31) (width 0.25) (layer B.Cu) (net 37) (tstamp 5C335788))
  (segment (start 136.525 67.31) (end 135.255 67.31) (width 0.25) (layer B.Cu) (net 37) (tstamp 5C335789))
  (segment (start 111.76 67.31) (end 135.255 67.31) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 88.265 67.31) (end 111.76 67.31) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 64.77 67.31) (end 88.265 67.31) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 151.13 65.405) (end 149.225 65.405) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 148.59 60.325) (end 147.955 59.69) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C61CD8D))
  (segment (start 148.59 64.77) (end 148.59 60.325) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C61CD8C))
  (segment (start 149.225 65.405) (end 148.59 64.77) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C61CD8B))
  (segment (start 158.75 64.77) (end 157.48 64.77) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 136.525 64.77) (end 137.16 64.135) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C335743))
  (segment (start 136.525 64.77) (end 135.255 64.77) (width 0.25) (layer B.Cu) (net 38))
  (segment (start 138.43 59.69) (end 147.955 59.69) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C33574A))
  (segment (start 137.795 60.325) (end 138.43 59.69) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C335749))
  (segment (start 137.795 62.23) (end 137.795 60.325) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C335748))
  (segment (start 137.16 62.865) (end 137.795 62.23) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C335747))
  (segment (start 137.16 64.135) (end 137.16 62.865) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C335746))
  (segment (start 156.845 65.405) (end 151.13 65.405) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C335766))
  (segment (start 157.48 64.77) (end 156.845 65.405) (width 0.25) (layer B.Cu) (net 38) (tstamp 5C335765))
  (segment (start 111.76 64.77) (end 135.255 64.77) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 88.265 64.77) (end 111.76 64.77) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 64.77 64.77) (end 66.04 64.77) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 86.995 64.77) (end 88.265 64.77) (width 0.25) (layer F.Cu) (net 38) (tstamp 5C3354AB))
  (segment (start 86.36 65.405) (end 86.995 64.77) (width 0.25) (layer F.Cu) (net 38) (tstamp 5C3354AA))
  (segment (start 66.675 65.405) (end 86.36 65.405) (width 0.25) (layer F.Cu) (net 38) (tstamp 5C3354A9))
  (segment (start 66.04 64.77) (end 66.675 65.405) (width 0.25) (layer F.Cu) (net 38) (tstamp 5C3354A8))
  (segment (start 111.76 62.23) (end 88.265 62.23) (width 0.25) (layer F.Cu) (net 39))
  (segment (start 135.255 62.23) (end 111.76 62.23) (width 0.25) (layer F.Cu) (net 39))
  (segment (start 158.75 62.23) (end 157.48 62.23) (width 0.25) (layer B.Cu) (net 39))
  (segment (start 136.525 62.23) (end 135.255 62.23) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C33572B))
  (segment (start 137.16 61.595) (end 136.525 62.23) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C335726))
  (segment (start 137.16 59.69) (end 137.16 61.595) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C335725))
  (segment (start 137.795 59.055) (end 137.16 59.69) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C33571F))
  (segment (start 156.21 59.055) (end 137.795 59.055) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C33571E))
  (segment (start 156.845 59.69) (end 156.21 59.055) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C33571C))
  (segment (start 156.845 61.595) (end 156.845 59.69) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C335719))
  (segment (start 157.48 62.23) (end 156.845 61.595) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C335718))
  (segment (start 64.77 62.23) (end 65.405 62.23) (width 0.25) (layer B.Cu) (net 39))
  (segment (start 65.405 62.23) (end 66.675 60.96) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C335505))
  (segment (start 66.675 60.96) (end 66.675 59.69) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C335506))
  (segment (start 66.675 59.69) (end 67.31 59.055) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C335508))
  (segment (start 67.31 59.055) (end 85.725 59.055) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C335509))
  (segment (start 85.725 59.055) (end 86.36 59.69) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C33550A))
  (segment (start 86.36 59.69) (end 86.36 60.96) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C33550B))
  (segment (start 86.36 60.96) (end 87.63 62.23) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C33550C))
  (segment (start 87.63 62.23) (end 88.265 62.23) (width 0.25) (layer B.Cu) (net 39) (tstamp 5C33550E))
  (segment (start 88.265 59.69) (end 111.76 59.69) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 135.255 59.69) (end 111.76 59.69) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 135.255 59.69) (end 135.89 59.69) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 135.89 59.69) (end 136.525 59.055) (width 0.25) (layer F.Cu) (net 40) (tstamp 5C335499))
  (segment (start 158.75 59.69) (end 158.115 59.69) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 158.115 59.69) (end 157.48 59.055) (width 0.25) (layer F.Cu) (net 40) (tstamp 5C335494))
  (segment (start 157.48 59.055) (end 136.525 59.055) (width 0.25) (layer F.Cu) (net 40) (tstamp 5C335495))
  (segment (start 88.265 59.69) (end 87.63 59.69) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 87.63 59.69) (end 86.995 59.055) (width 0.25) (layer F.Cu) (net 40) (tstamp 5C33548E))
  (segment (start 86.995 59.055) (end 66.04 59.055) (width 0.25) (layer F.Cu) (net 40) (tstamp 5C33548F))
  (segment (start 66.04 59.055) (end 65.405 59.69) (width 0.25) (layer F.Cu) (net 40) (tstamp 5C335490))
  (segment (start 65.405 59.69) (end 64.77 59.69) (width 0.25) (layer F.Cu) (net 40) (tstamp 5C335491))
  (segment (start 153.67 69.85) (end 153.67 73.66) (width 0.25) (layer F.Cu) (net 41))
  (segment (start 153.035 74.295) (end 149.86 74.295) (width 0.25) (layer F.Cu) (net 41) (tstamp 5C61D11D))
  (segment (start 153.67 73.66) (end 153.035 74.295) (width 0.25) (layer F.Cu) (net 41) (tstamp 5C61D11C))
  (segment (start 153.67 69.85) (end 153.67 70.485) (width 0.25) (layer F.Cu) (net 41))

)
