(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")

  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 293)
    (zones 0)
    (modules 77)
    (nets 23)
  )

  (page A)
  (title_block
    (title "Unified Retro Keyboard Multi-adapter")
    (date 2021-02-13)
    (rev 1.0)
  )

  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8128)
    (via_drill 0.4064)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.27 0.7112)
    (user_via 1.5748 0.8128)
    (uvia_size 0.3048)
    (uvia_drill 0.1016)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 61.4172 179.1081)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "outputs"))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 /D7)
  (net 3 /D1)
  (net 4 /D2)
  (net 5 /D3)
  (net 6 /D4)
  (net 7 /D5)
  (net 8 /D6)
  (net 9 /D0)
  (net 10 /~STROBE)
  (net 11 "Net-(J1-Pad9)")
  (net 12 "Net-(J1-Pad4)")
  (net 13 "Net-(J1-Pad14)")
  (net 14 "Net-(J1-Pad15)")
  (net 15 "Net-(J1-Pad16)")
  (net 16 "Net-(J2-Pad10)")
  (net 17 "Net-(J2-Pad11)")
  (net 18 "Net-(J2-Pad13)")
  (net 19 VCC)
  (net 20 /~RESET)
  (net 21 /CLR-LOCAL)
  (net 22 /BREAK)

  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net /BREAK)
    (add_net /CLR-LOCAL)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /~RESET)
    (add_net /~STROBE)
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net VCC)
  )

  (net_class power1 ""
    (clearance 0.1524)
    (trace_width 1.27)
    (via_dia 1.27)
    (via_drill 0.7112)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net GND)
  )

  (net_class signal ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.3048)
    (uvia_drill 0.1016)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 60278C29)
    (at 112.018 78.828)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at -0.762 -1.016) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FF0D)
    (at 124.718 99.148)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FEED)
    (at 122.178 99.148)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FECD)
    (at 119.638 99.148)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FEAD)
    (at 117.098 99.148)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FE8D)
    (at 114.558 99.148)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FE6D)
    (at 112.018 99.148)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FE4D)
    (at 124.718 96.608)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FE2D)
    (at 122.178 96.608)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FE0D)
    (at 119.638 96.608)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FDED)
    (at 117.098 96.608)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FDCD)
    (at 114.558 96.608)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FDAD)
    (at 112.018 96.608)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FD8D)
    (at 124.718 94.068)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FD6D)
    (at 122.178 94.068)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FD4D)
    (at 119.638 94.068)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FD2D)
    (at 117.098 94.068)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FD0D)
    (at 114.558 94.068)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E554)
    (at 112.018 94.068)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FC44)
    (at 124.718 91.528)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FC24)
    (at 122.178 91.528)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FC04)
    (at 119.638 91.528)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FBE4)
    (at 117.098 91.528)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FBC4)
    (at 114.558 91.528)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FBA4)
    (at 112.018 91.528)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FB84)
    (at 124.718 88.988)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FB64)
    (at 122.178 88.988)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FB44)
    (at 119.638 88.988)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FB24)
    (at 117.098 88.988)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FB04)
    (at 114.558 88.988)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FAE4)
    (at 112.018 88.988)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FAC4)
    (at 124.718 86.448)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FAA4)
    (at 122.178 86.448)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FA84)
    (at 119.638 86.448)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FA64)
    (at 117.098 86.448)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027FA44)
    (at 114.558 86.448)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E554)
    (at 112.018 86.448)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F936)
    (at 124.718 106.768)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F916)
    (at 122.178 106.768)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F8F6)
    (at 119.638 106.768)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F8D6)
    (at 117.098 106.768)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F8B6)
    (at 114.558 106.768)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F896)
    (at 112.018 106.768)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F876)
    (at 124.718 104.228)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F856)
    (at 122.178 104.228)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F836)
    (at 119.638 104.228)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F816)
    (at 117.098 104.228)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F7F6)
    (at 114.558 104.228)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F7D6)
    (at 112.018 104.228)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F7B6)
    (at 124.718 101.688)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F796)
    (at 122.178 101.688)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F776)
    (at 119.638 101.688)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F756)
    (at 117.098 101.688)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027F736)
    (at 114.558 101.688)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E554)
    (at 112.018 101.688)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E1A8)
    (at 124.718 83.908)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E188)
    (at 122.178 83.908)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E168)
    (at 119.638 83.908)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E148)
    (at 117.098 83.908)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E128)
    (at 114.558 83.908)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E108)
    (at 112.018 83.908)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E0E8)
    (at 124.718 81.368)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E0C8)
    (at 122.178 81.368)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E0A8)
    (at 119.638 81.368)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E088)
    (at 117.098 81.368)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E068)
    (at 114.558 81.368)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E048)
    (at 112.018 81.368)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E028)
    (at 124.718 78.828)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027E008)
    (at 122.178 78.828)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027DFE8)
    (at 119.638 78.828)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027DFC8)
    (at 117.098 78.828)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module unikbd:proto_pad (layer F.Cu) (tedit 602746C3) (tstamp 6027DFA8)
    (at 114.558 78.828)
    (descr "solder Pin_ with flat with fork, hole diameter 1.4mm, length 8.5mm, width 2.8mm, e.g. Ettinger 13.13.890, https://katalog.ettinger.de/#p=434")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 1.016 0.762) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value . (at 0 -2.05) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user . (at -1.27 0.254) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.4 0.25) (end -1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 -0.25) (end 1.4 0.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.4 -0.25) (end 1.4 -0.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.4 0.25) (end -1.4 0.25) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module "" (layer F.Cu) (tedit 0) (tstamp 0)
    (at 15.61 3.18)
    (attr smd)
    (fp_text reference "" (at 225.275 102.77) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.15)))
    )
    (fp_text value "" (at 225.275 102.77) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.15)))
    )
  )

  (module unikbd:SOL20-header-vertical (layer F.Cu) (tedit 5E1E2018) (tstamp 6026E4D2)
    (at 142.598 80.748 90)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (path /5E5FA80F)
    (attr virtual)
    (fp_text reference J5 (at 4.04 -2.898 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SOL-20 (at 5.056 7.516 180) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.1524)))
    )
    (fp_line (start 0 -1.27) (end 3.81 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 -1.27) (end 3.81 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start 3.81 24.13) (end -1.27 24.13) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 24.13) (end -1.27 0) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 0) (end 0 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 24.19) (end 3.87 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.87 -1.33) (end 3.87 24.19) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 1.27) (end 1.27 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.27 -1.33) (end 3.87 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 24.65) (end 4.35 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 24.65) (end 4.35 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.35 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 1.27 11.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VCC))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VCC))
    (pad 18 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /D7))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /D3))
    (pad 17 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /D6))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /D2))
    (pad 16 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D5))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /D1))
    (pad 15 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /D4))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 14 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /BREAK))
    (pad 13 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /~STROBE))
    (pad 12 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VCC))
    (pad 11 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB) (tstamp 6026E8D6)
    (at 104.703 97.143 180)
    (descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x05 2.54mm single row")
    (path /5E83DEBE)
    (attr virtual)
    (fp_text reference J4 (at 4.385 -2.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Outputs (at 4.385 12.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.135 -1.27) (end 4.04 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -1.27) (end 4.04 11.43) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 11.43) (end 1.5 11.43) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 11.43) (end 1.5 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -0.635) (end 2.135 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end 1.5 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end 1.5 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -0.32) (end 10.04 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 -0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 0.32) (end 10.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end 1.5 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.86) (end 1.5 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.22) (end 10.04 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 2.22) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 2.86) (end 10.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end 1.5 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 5.4) (end 1.5 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 4.76) (end 10.04 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 4.76) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 5.4) (end 10.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end 1.5 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end -0.32 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.94) (end 1.5 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 7.3) (end 10.04 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 7.3) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 7.94) (end 10.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 9.84) (end 1.5 9.84) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 9.84) (end -0.32 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 10.48) (end 1.5 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 9.84) (end 10.04 9.84) (layer F.Fab) (width 0.1))
    (fp_line (start 10.04 9.84) (end 10.04 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 10.48) (end 10.04 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start 1.44 -1.33) (end 1.44 11.49) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 11.49) (end 4.1 11.49) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 11.49) (end 4.1 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -1.33) (end 1.44 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.38) (end 10.1 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 -0.38) (end 10.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 0.38) (end 4.1 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.32) (end 10.1 -0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.2) (end 10.1 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 -0.08) (end 10.1 -0.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.04) (end 10.1 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.16) (end 10.1 0.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 0.28) (end 10.1 0.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 -0.38) (end 1.44 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.38) (end 1.44 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 1.27) (end 4.1 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 2.16) (end 10.1 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.16) (end 10.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 2.92) (end 4.1 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.16) (end 1.44 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.92) (end 1.44 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 3.81) (end 4.1 3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 4.7) (end 10.1 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 4.7) (end 10.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 5.46) (end 4.1 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 4.7) (end 1.44 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 5.46) (end 1.44 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 6.35) (end 4.1 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 7.24) (end 10.1 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 7.24) (end 10.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 8) (end 4.1 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 7.24) (end 1.44 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 8) (end 1.44 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.44 8.89) (end 4.1 8.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 4.1 9.78) (end 10.1 9.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 9.78) (end 10.1 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.1 10.54) (end 4.1 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 9.78) (end 1.44 9.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 10.54) (end 1.44 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.27) (end 0 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 11.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 11.95) (end 10.55 11.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.55 11.95) (end 10.55 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.55 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at -1.765 4.595) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VCC))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /BREAK))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-16_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5) (tstamp 5E98D813)
    (at 158.038 99.228 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (path /5D9AB54A)
    (fp_text reference J1 (at 8.509 -2.335832 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Apple 2" (at -2.8818 2.998) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.15)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 19.11) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 19.11) (end 8.89 19.11) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 19.11) (end 8.89 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 19.11) (end 6.46 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 19.11) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.39) (end -1.33 19.17) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 19.17) (end 8.95 19.17) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.95 19.17) (end 8.95 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.95 -1.39) (end -1.33 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.6) (end -1.55 19.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 19.4) (end 9.15 19.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 19.4) (end 9.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VCC))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /~STROBE))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad4)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D5))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D1))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D4))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad14)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D6))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad15)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad16)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DIP:DIP-16_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5) (tstamp 5D0D78AD)
    (at 131.288 99.288 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (path /5BCB9E1D)
    (fp_text reference J2 (at 8.255 -2.549166 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "Apple 1" (at -2.82 2.316 180) (layer F.SilkS)
      (effects (font (size 1.27 1.27) (thickness 0.1524)))
    )
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -1.33) (end -1.27 19.11) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 19.11) (end 8.89 19.11) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 19.11) (end 8.89 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 8.89 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 -1.33) (end 1.16 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.16 19.11) (end 6.46 19.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 19.11) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.39) (end -1.33 19.17) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 19.17) (end 8.95 19.17) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.95 19.17) (end 8.95 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.95 -1.39) (end -1.33 -1.39) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.55 -1.6) (end -1.55 19.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.55 19.4) (end 9.15 19.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 19.4) (end 9.15 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.15 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 9.50214 -0.78486 180) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /~RESET))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /D3))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /D2))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad11)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /D1))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /CLR-LOCAL))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /D0))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad13)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /D4))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /~STROBE))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /D5))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /D6))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 VCC))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 107.95 82.296) (end 110.236 81.28) (layer F.SilkS) (width 0.12))
  (gr_line (start 107.95 85.852) (end 107.95 82.296) (layer F.SilkS) (width 0.12))
  (gr_line (start 110.236 96.774) (end 108.966 94.996) (layer F.SilkS) (width 0.12))
  (gr_line (start 108.204 89.154) (end 110.236 88.9) (layer F.SilkS) (width 0.12))
  (gr_line (start 107.696 102.87) (end 110.236 104.14) (layer F.SilkS) (width 0.12))
  (gr_line (start 107.696 97.79) (end 107.696 102.87) (layer F.SilkS) (width 0.12))
  (gr_line (start 110.236 107.188) (end 110.744 107.696) (layer F.SilkS) (width 0.12) (tstamp 602833B2))
  (gr_line (start 110.236 101.092) (end 110.744 100.584) (layer F.SilkS) (width 0.12) (tstamp 602833B1))
  (gr_line (start 110.236 101.092) (end 110.236 107.188) (layer F.SilkS) (width 0.12) (tstamp 602833B0))
  (gr_line (start 110.236 99.822) (end 110.744 100.33) (layer F.SilkS) (width 0.12) (tstamp 602833B2))
  (gr_line (start 110.236 93.726) (end 110.744 93.218) (layer F.SilkS) (width 0.12) (tstamp 602833B1))
  (gr_line (start 110.236 93.726) (end 110.236 99.822) (layer F.SilkS) (width 0.12) (tstamp 602833B0))
  (gr_line (start 110.236 84.582) (end 110.744 85.09) (layer F.SilkS) (width 0.12) (tstamp 602833B2))
  (gr_line (start 110.236 78.486) (end 110.744 77.978) (layer F.SilkS) (width 0.12) (tstamp 602833B1))
  (gr_line (start 110.236 78.486) (end 110.236 84.582) (layer F.SilkS) (width 0.12) (tstamp 602833B0))
  (gr_line (start 110.236 85.852) (end 110.744 85.344) (layer F.SilkS) (width 0.12))
  (gr_line (start 110.236 91.948) (end 110.744 92.456) (layer F.SilkS) (width 0.12))
  (gr_line (start 110.236 85.852) (end 110.236 91.948) (layer F.SilkS) (width 0.12))
  (gr_text "Multi-adapter\nRev 1.0" (at 168.91 74.168) (layer F.SilkS) (tstamp 6028148C)
    (effects (font (size 1.524 1.524) (thickness 0.2032)) (justify left))
  )
  (gr_text 1 (at 139.7 81.534) (layer F.SilkS) (tstamp 602807C8)
    (effects (font (size 1.016 1.016) (thickness 0.127)) (justify left))
  )
  (gr_text GND (at 105.918 97.028) (layer F.SilkS) (tstamp 602807C8)
    (effects (font (size 1.016 1.016) (thickness 0.127)) (justify left))
  )
  (gr_text RESET (at 105.918 94.488) (layer F.SilkS) (tstamp 602807C8)
    (effects (font (size 0.762 0.762) (thickness 0.127)) (justify left))
  )
  (gr_text BREAK (at 105.918 91.948) (layer F.SilkS) (tstamp 602807C8)
    (effects (font (size 0.762 0.762) (thickness 0.127)) (justify left))
  )
  (gr_text "CLR\nLOCAL" (at 105.918 89.408) (layer F.SilkS) (tstamp 602807C8)
    (effects (font (size 0.508 0.508) (thickness 0.0762)) (justify left))
  )
  (gr_text +5V (at 105.918 86.868) (layer F.SilkS)
    (effects (font (size 1.016 1.016) (thickness 0.127)) (justify left))
  )
  (gr_line (start 91.948 110.998) (end 91.948 70.358) (layer Edge.Cuts) (width 0.1) (tstamp 602800AC))
  (gr_line (start 185.928 110.998) (end 185.928 70.358) (layer Edge.Cuts) (width 0.1) (tstamp 602800AC))
  (gr_line (start 91.948 110.998) (end 185.928 110.998) (layer Edge.Cuts) (width 0.1) (tstamp 602800AC))
  (gr_text "OSIWeb.org 2021" (at 105.0568 72.8234) (layer F.SilkS) (tstamp 5EB92393)
    (effects (font (size 1.524 1.524) (thickness 0.2032)))
  )
  (gr_line (start 91.948 70.358) (end 185.928 70.358) (layer Edge.Cuts) (width 0.1) (tstamp 5E1EE823))

  (segment (start 124.718 106.768) (end 112.018 106.768) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 112.018 104.228) (end 124.718 104.228) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 124.718 101.688) (end 124.718 106.768) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 122.178 106.768) (end 122.178 101.688) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 119.638 106.768) (end 119.638 101.688) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 117.098 106.768) (end 117.098 101.688) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 114.558 106.768) (end 114.558 101.688) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 112.018 106.768) (end 112.018 101.688) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 112.018 101.688) (end 124.718 101.688) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 109.248 101.688) (end 104.703 97.143) (width 1.27) (layer B.Cu) (net 1))
  (segment (start 112.018 101.688) (end 109.248 101.688) (width 1.27) (layer B.Cu) (net 1))
  (segment (start 149.068 91.668) (end 150.938 91.668) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 150.938 91.668) (end 151.788 92.518) (width 1.27) (layer F.Cu) (net 1))
  (via (at 151.788 107.038) (size 1.27) (drill 0.7112) (layers F.Cu B.Cu) (net 1))
  (segment (start 151.788 92.518) (end 151.788 107.038) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 124.988 107.038) (end 124.718 106.768) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 151.788 107.038) (end 124.988 107.038) (width 1.27) (layer F.Cu) (net 1))
  (via (at 175.908 107.008) (size 1.27) (drill 0.7112) (layers F.Cu B.Cu) (net 1))
  (segment (start 175.818 99.228) (end 175.818 106.918) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 175.818 106.918) (end 175.908 107.008) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 151.788 107.038) (end 175.878 107.038) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 175.878 107.038) (end 175.908 107.008) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 165.458 78.208) (end 165.458 80.748) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 182.848 100.328) (end 176.168 107.008) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 182.848 87.558) (end 182.848 100.328) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 176.168 107.008) (end 175.908 107.008) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 176.038 80.748) (end 182.848 87.558) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 165.458 80.748) (end 176.038 80.748) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 142.598 80.748) (end 142.598 78.208) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 142.598 78.208) (end 142.598 75.568) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 142.598 75.568) (end 144.538 73.628) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 144.538 73.628) (end 163.858 73.628) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 165.458 75.228) (end 165.458 78.208) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 163.858 73.628) (end 165.458 75.228) (width 1.27) (layer F.Cu) (net 1))
  (segment (start 165.658 91.608) (end 165.658 96.56381) (width 0.254) (layer F.Cu) (net 3))
  (via (at 165.708 96.61381) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 3))
  (segment (start 165.658 96.56381) (end 165.708 96.61381) (width 0.254) (layer F.Cu) (net 3))
  (segment (start 138.908 99.288) (end 138.908 96.587996) (width 0.254) (layer F.Cu) (net 3))
  (via (at 138.908 96.587996) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 3))
  (segment (start 165.708 96.61381) (end 165.133264 96.61381) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 165.133264 96.61381) (end 164.827462 96.919612) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 164.827462 96.919612) (end 161.256127 96.919612) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 161.075526 97.100213) (end 142.314388 97.100213) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 161.256127 96.919612) (end 161.075526 97.100213) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 142.314388 97.100213) (end 142.148586 96.934411) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 142.148586 96.934411) (end 139.829151 96.934411) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 139.829151 96.934411) (end 139.482736 96.587996) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 139.482736 96.587996) (end 138.908 96.587996) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 155.298 80.748) (end 155.298 83.358) (width 0.254) (layer F.Cu) (net 3))
  (via (at 155.268 83.388) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 3))
  (segment (start 155.298 83.358) (end 155.268 83.388) (width 0.254) (layer F.Cu) (net 3))
  (via (at 165.638 83.768) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 3))
  (segment (start 165.258 83.388) (end 165.638 83.768) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 155.268 83.388) (end 165.258 83.388) (width 0.254) (layer B.Cu) (net 3))
  (segment (start 165.638 91.588) (end 165.658 91.608) (width 0.254) (layer F.Cu) (net 3))
  (segment (start 165.638 83.768) (end 165.638 91.588) (width 0.254) (layer F.Cu) (net 3))
  (via (at 173.108 96.328) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 4))
  (segment (start 173.278 96.158) (end 173.108 96.328) (width 0.254) (layer F.Cu) (net 4))
  (segment (start 173.278 91.608) (end 173.278 96.158) (width 0.254) (layer F.Cu) (net 4))
  (via (at 136.368 96.588) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 4))
  (segment (start 136.368 99.288) (end 136.368 96.588) (width 0.254) (layer F.Cu) (net 4))
  (segment (start 137.130212 97.350212) (end 136.774399 96.994399) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 142.146048 97.506624) (end 141.989636 97.350212) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 136.774399 96.994399) (end 136.368 96.588) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 173.108 96.328) (end 170.578 96.328) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 161.263864 97.506624) (end 142.146048 97.506624) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 161.420276 97.350212) (end 161.263864 97.506624) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 165.59695 97.299611) (end 165.546349 97.350212) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 169.606389 97.299611) (end 165.59695 97.299611) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 165.546349 97.350212) (end 161.420276 97.350212) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 170.578 96.328) (end 169.606389 97.299611) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 141.989636 97.350212) (end 137.130212 97.350212) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 157.838 84.108) (end 158.008 84.278) (width 0.254) (layer F.Cu) (net 4))
  (via (at 158.008 84.278) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 4))
  (segment (start 157.838 80.748) (end 157.838 84.108) (width 0.254) (layer F.Cu) (net 4))
  (via (at 173.018 84.948) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 4))
  (segment (start 158.678 84.948) (end 173.018 84.948) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 158.008 84.278) (end 158.678 84.948) (width 0.254) (layer B.Cu) (net 4))
  (segment (start 173.018 91.348) (end 173.278 91.608) (width 0.254) (layer F.Cu) (net 4))
  (segment (start 173.018 84.948) (end 173.018 91.348) (width 0.254) (layer F.Cu) (net 4))
  (via (at 133.828 97.378) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 5))
  (segment (start 133.828 99.288) (end 133.828 97.378) (width 0.254) (layer F.Cu) (net 5))
  (segment (start 170.738 91.608) (end 170.738 97.446022) (width 0.254) (layer F.Cu) (net 5))
  (via (at 170.828 97.536022) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 5))
  (segment (start 170.738 97.446022) (end 170.828 97.536022) (width 0.254) (layer F.Cu) (net 5))
  (segment (start 161.412205 97.933034) (end 161.56084 97.784399) (width 0.254) (layer B.Cu) (net 5))
  (segment (start 134.383034 97.933034) (end 161.412205 97.933034) (width 0.254) (layer B.Cu) (net 5))
  (segment (start 133.828 97.378) (end 134.383034 97.933034) (width 0.254) (layer B.Cu) (net 5))
  (segment (start 170.004887 97.784399) (end 170.253264 97.536022) (width 0.254) (layer B.Cu) (net 5))
  (segment (start 161.56084 97.784399) (end 170.004887 97.784399) (width 0.254) (layer B.Cu) (net 5))
  (segment (start 170.253264 97.536022) (end 170.828 97.536022) (width 0.254) (layer B.Cu) (net 5))
  (via (at 160.538 85.698) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 5))
  (segment (start 160.378 85.538) (end 160.538 85.698) (width 0.254) (layer F.Cu) (net 5))
  (segment (start 160.378 80.748) (end 160.378 85.538) (width 0.254) (layer F.Cu) (net 5))
  (via (at 170.518812 85.73219) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 5))
  (segment (start 170.484622 85.698) (end 170.518812 85.73219) (width 0.254) (layer B.Cu) (net 5))
  (segment (start 170.738 91.608) (end 170.738 85.951378) (width 0.254) (layer F.Cu) (net 5))
  (segment (start 160.538 85.698) (end 170.484622 85.698) (width 0.254) (layer B.Cu) (net 5))
  (segment (start 170.738 85.951378) (end 170.518812 85.73219) (width 0.254) (layer F.Cu) (net 5))
  (segment (start 143.988 99.288) (end 143.988 101.768) (width 0.254) (layer F.Cu) (net 6))
  (via (at 143.988 101.768) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 6))
  (segment (start 143.988 101.768) (end 170.538 101.768) (width 0.254) (layer B.Cu) (net 6))
  (segment (start 170.538 101.768) (end 170.738 101.568) (width 0.254) (layer B.Cu) (net 6))
  (segment (start 170.738 99.228) (end 170.738 101.568) (width 0.254) (layer F.Cu) (net 6))
  (via (at 170.738 101.568) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 6))
  (via (at 154.198 86.418) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 6))
  (segment (start 177.408 101.568) (end 178.425178 100.550822) (width 0.254) (layer B.Cu) (net 6))
  (segment (start 178.425178 90.284678) (end 175.684899 87.544399) (width 0.254) (layer B.Cu) (net 6))
  (segment (start 175.684899 87.544399) (end 155.324399 87.544399) (width 0.254) (layer B.Cu) (net 6))
  (segment (start 170.738 101.568) (end 177.408 101.568) (width 0.254) (layer B.Cu) (net 6))
  (segment (start 178.425178 100.550822) (end 178.425178 90.284678) (width 0.254) (layer B.Cu) (net 6))
  (segment (start 155.324399 87.544399) (end 154.198 86.418) (width 0.254) (layer B.Cu) (net 6))
  (segment (start 153.998 79.448) (end 153.998 86.218) (width 0.254) (layer F.Cu) (net 6))
  (segment (start 153.998 86.218) (end 154.198 86.418) (width 0.254) (layer F.Cu) (net 6))
  (segment (start 152.758 78.208) (end 153.998 79.448) (width 0.254) (layer F.Cu) (net 6))
  (segment (start 168.198 99.228) (end 168.198 102.578) (width 0.254) (layer F.Cu) (net 7))
  (segment (start 168.198 102.578) (end 168.248 102.628) (width 0.254) (layer F.Cu) (net 7))
  (via (at 168.248 102.628) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 7))
  (segment (start 146.528 102.608) (end 146.678 102.758) (width 0.254) (layer F.Cu) (net 7))
  (segment (start 168.248 102.628) (end 146.808 102.628) (width 0.254) (layer B.Cu) (net 7))
  (via (at 146.678 102.758) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 7))
  (segment (start 146.528 99.288) (end 146.528 102.608) (width 0.254) (layer F.Cu) (net 7))
  (segment (start 146.808 102.628) (end 146.678 102.758) (width 0.254) (layer B.Cu) (net 7))
  (via (at 156.553555 86.383555) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 7))
  (segment (start 155.298 78.208) (end 156.553555 79.463555) (width 0.254) (layer F.Cu) (net 7))
  (segment (start 156.553555 79.463555) (end 156.553555 86.383555) (width 0.254) (layer F.Cu) (net 7))
  (segment (start 178.831589 100.719162) (end 178.831589 90.116339) (width 0.254) (layer B.Cu) (net 7))
  (segment (start 168.248 102.628) (end 176.922751 102.628) (width 0.254) (layer B.Cu) (net 7))
  (segment (start 176.922751 102.628) (end 178.831589 100.719162) (width 0.254) (layer B.Cu) (net 7))
  (segment (start 178.831589 90.116339) (end 175.819649 87.104399) (width 0.254) (layer B.Cu) (net 7))
  (segment (start 175.819649 87.104399) (end 157.274399 87.104399) (width 0.254) (layer B.Cu) (net 7))
  (segment (start 157.274399 87.104399) (end 156.553555 86.383555) (width 0.254) (layer B.Cu) (net 7))
  (segment (start 149.068 103.488) (end 149.178 103.598) (width 0.254) (layer F.Cu) (net 8))
  (segment (start 149.068 99.288) (end 149.068 103.488) (width 0.254) (layer F.Cu) (net 8))
  (via (at 149.178 103.598) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 8))
  (segment (start 158.967401 79.337401) (end 158.967401 83.947401) (width 0.254) (layer F.Cu) (net 8))
  (segment (start 157.838 78.208) (end 158.967401 79.337401) (width 0.254) (layer F.Cu) (net 8))
  (via (at 158.838 86.418) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 8))
  (segment (start 158.838 84.076802) (end 158.838 86.418) (width 0.254) (layer F.Cu) (net 8))
  (segment (start 158.967401 83.947401) (end 158.838 84.076802) (width 0.254) (layer F.Cu) (net 8))
  (segment (start 149.178 103.598) (end 172.85955 103.598) (width 0.254) (layer B.Cu) (net 8))
  (segment (start 173.278 99.228) (end 173.278 103.17955) (width 0.254) (layer F.Cu) (net 8))
  (segment (start 172.85955 103.598) (end 173.14374 103.31381) (width 0.254) (layer B.Cu) (net 8))
  (segment (start 173.278 103.17955) (end 173.14374 103.31381) (width 0.254) (layer F.Cu) (net 8))
  (via (at 173.14374 103.31381) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 8))
  (segment (start 176.811692 103.31381) (end 173.14374 103.31381) (width 0.254) (layer B.Cu) (net 8))
  (segment (start 179.238 89.948) (end 179.238 100.887502) (width 0.254) (layer B.Cu) (net 8))
  (segment (start 175.708 86.418) (end 179.238 89.948) (width 0.254) (layer B.Cu) (net 8))
  (segment (start 158.838 86.418) (end 175.708 86.418) (width 0.254) (layer B.Cu) (net 8))
  (segment (start 179.238 100.887502) (end 176.811692 103.31381) (width 0.254) (layer B.Cu) (net 8))
  (segment (start 168.198 91.608) (end 168.198 96.068) (width 0.254) (layer F.Cu) (net 9))
  (segment (start 168.198 96.068) (end 168.278 96.148) (width 0.254) (layer F.Cu) (net 9))
  (via (at 168.278 96.148) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 9))
  (segment (start 141.448 99.288) (end 141.448 96.23381) (width 0.254) (layer F.Cu) (net 9))
  (via (at 141.448 96.23381) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 9))
  (segment (start 142.022736 96.23381) (end 141.448 96.23381) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 142.482728 96.693802) (end 142.022736 96.23381) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 160.907186 96.693802) (end 142.482728 96.693802) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 168.278 96.148) (end 167.871601 95.741601) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 161.092988 96.508) (end 160.907186 96.693802) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 165.364399 95.741601) (end 164.598 96.508) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 167.871601 95.741601) (end 165.364399 95.741601) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 164.598 96.508) (end 161.092988 96.508) (width 0.254) (layer B.Cu) (net 9))
  (via (at 152.818 82.898) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 9))
  (segment (start 152.758 82.838) (end 152.818 82.898) (width 0.254) (layer F.Cu) (net 9))
  (segment (start 152.758 80.748) (end 152.758 82.838) (width 0.254) (layer F.Cu) (net 9))
  (via (at 167.488 83.128) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 9))
  (segment (start 168.198 83.838) (end 168.198 91.608) (width 0.254) (layer F.Cu) (net 9))
  (segment (start 167.488 83.128) (end 168.198 83.838) (width 0.254) (layer F.Cu) (net 9))
  (segment (start 152.818 82.898) (end 153.224399 82.491601) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 153.224399 82.491601) (end 166.851601 82.491601) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 166.851601 82.491601) (end 167.081601 82.721601) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 167.081601 82.721601) (end 167.488 83.128) (width 0.254) (layer B.Cu) (net 9))
  (segment (start 160.578 99.228) (end 160.578 95.908) (width 0.254) (layer F.Cu) (net 10))
  (via (at 160.578 95.908) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 10))
  (via (at 136.858002 95.658002) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 10))
  (segment (start 136.368 95.168) (end 136.858002 95.658002) (width 0.254) (layer F.Cu) (net 10))
  (segment (start 136.368 91.668) (end 136.368 95.168) (width 0.254) (layer F.Cu) (net 10))
  (segment (start 160.171601 95.501601) (end 137.014403 95.501601) (width 0.254) (layer B.Cu) (net 10))
  (segment (start 160.578 95.908) (end 160.171601 95.501601) (width 0.254) (layer B.Cu) (net 10))
  (segment (start 137.014403 95.501601) (end 136.858002 95.658002) (width 0.254) (layer B.Cu) (net 10))
  (segment (start 147.678 80.748) (end 147.678 82.868) (width 0.254) (layer F.Cu) (net 10))
  (via (at 147.728 82.888) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 10))
  (segment (start 147.708 82.868) (end 147.728 82.888) (width 0.254) (layer F.Cu) (net 10))
  (segment (start 147.678 82.868) (end 147.708 82.868) (width 0.254) (layer F.Cu) (net 10))
  (via (at 136.538 82.938) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 10))
  (segment (start 136.588 82.888) (end 136.538 82.938) (width 0.254) (layer B.Cu) (net 10))
  (segment (start 147.728 82.888) (end 136.588 82.888) (width 0.254) (layer B.Cu) (net 10))
  (segment (start 136.538 91.498) (end 136.368 91.668) (width 0.254) (layer F.Cu) (net 10))
  (segment (start 136.538 82.938) (end 136.538 91.498) (width 0.254) (layer F.Cu) (net 10))
  (segment (start 112.018 86.448) (end 124.718 86.448) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 124.718 88.988) (end 112.018 88.988) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 112.018 91.528) (end 124.718 91.528) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 124.718 86.448) (end 124.718 91.528) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 122.178 86.448) (end 122.178 91.528) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 119.638 91.528) (end 119.638 86.448) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 117.098 86.448) (end 117.098 91.528) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 114.558 91.528) (end 114.558 86.448) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 112.018 86.448) (end 112.018 91.528) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 111.483 89.523) (end 112.018 88.988) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 104.703 89.523) (end 111.483 89.523) (width 1.27) (layer B.Cu) (net 21))
  (segment (start 141.448 91.668) (end 139.928 93.188) (width 0.254) (layer B.Cu) (net 21))
  (segment (start 126.378 93.188) (end 124.718 91.528) (width 0.254) (layer B.Cu) (net 21))
  (segment (start 139.928 93.188) (end 126.378 93.188) (width 0.254) (layer B.Cu) (net 21))
  (segment (start 141.448 91.668) (end 141.448 85.158) (width 0.254) (layer F.Cu) (net 21))
  (via (at 141.418 85.128) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 21))
  (segment (start 141.448 85.158) (end 141.418 85.128) (width 0.254) (layer F.Cu) (net 21))
  (segment (start 141.418 85.128) (end 148.728 85.128) (width 0.254) (layer B.Cu) (net 21))
  (segment (start 148.828 85.028) (end 148.828 84.928) (width 0.254) (layer B.Cu) (net 21))
  (via (at 148.828 84.928) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 21))
  (segment (start 148.728 85.128) (end 148.828 85.028) (width 0.254) (layer B.Cu) (net 21))
  (via (at 150.218 78.208) (size 1.27) (drill 0.7112) (layers F.Cu B.Cu) (net 21))
  (segment (start 148.928 79.498) (end 150.218 78.208) (width 0.254) (layer F.Cu) (net 21))
  (segment (start 148.928 84.828) (end 148.928 79.498) (width 0.254) (layer F.Cu) (net 21))
  (segment (start 148.828 84.928) (end 148.928 84.828) (width 0.254) (layer F.Cu) (net 21))
  (via (at 138.698 86.348) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 22))
  (via (at 150.438 86.278) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 22))
  (segment (start 138.698 86.348) (end 150.368 86.348) (width 0.254) (layer B.Cu) (net 22))
  (segment (start 150.368 86.348) (end 150.438 86.278) (width 0.254) (layer B.Cu) (net 22))
  (segment (start 150.218 80.748) (end 150.218 86.058) (width 0.254) (layer F.Cu) (net 22))
  (segment (start 150.218 86.058) (end 150.438 86.278) (width 0.254) (layer F.Cu) (net 22))
  (segment (start 102.362 91.186) (end 102.362 82.394) (width 0.254) (layer B.Cu) (net 22))
  (segment (start 109.448 75.308) (end 137.458 75.308) (width 0.254) (layer F.Cu) (net 22))
  (segment (start 137.458 75.308) (end 138.698 76.548) (width 0.254) (layer F.Cu) (net 22))
  (segment (start 102.362 82.394) (end 109.448 75.308) (width 0.254) (layer B.Cu) (net 22))
  (segment (start 138.698 76.548) (end 138.698 86.348) (width 0.254) (layer F.Cu) (net 22))
  (segment (start 103.239 92.063) (end 102.362 91.186) (width 0.254) (layer B.Cu) (net 22))
  (segment (start 104.703 92.063) (end 103.239 92.063) (width 0.254) (layer B.Cu) (net 22))
  (via (at 109.448 75.308) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 22))
  (segment (start 112.018 94.068) (end 124.718 94.068) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 124.718 94.068) (end 124.718 99.148) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 112.018 99.148) (end 124.718 99.148) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 112.018 99.148) (end 112.018 94.068) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 114.558 94.068) (end 114.558 99.148) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 117.098 99.148) (end 117.098 94.068) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 119.638 94.068) (end 119.638 99.148) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 122.178 99.148) (end 122.178 94.068) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 112.018 96.608) (end 124.718 96.608) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 111.483 94.603) (end 112.018 94.068) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 104.703 94.603) (end 111.483 94.603) (width 1.27) (layer B.Cu) (net 20))
  (segment (start 124.858 99.288) (end 124.718 99.148) (width 0.254) (layer B.Cu) (net 20))
  (segment (start 131.288 99.288) (end 124.858 99.288) (width 0.254) (layer B.Cu) (net 20))
  (via (at 131.678 94.788) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 20))
  (segment (start 131.288 95.178) (end 131.678 94.788) (width 0.254) (layer F.Cu) (net 20))
  (segment (start 131.288 99.288) (end 131.288 95.178) (width 0.254) (layer F.Cu) (net 20))
  (via (at 162.928 88.968) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 20))
  (segment (start 161.998 98.108) (end 161.998 89.898) (width 0.254) (layer F.Cu) (net 20))
  (segment (start 161.998 89.898) (end 162.928 88.968) (width 0.254) (layer F.Cu) (net 20))
  (segment (start 163.118 99.228) (end 161.998 98.108) (width 0.254) (layer F.Cu) (net 20))
  (via (at 161.998 94.138) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 20))
  (segment (start 161.348 94.788) (end 161.998 94.138) (width 0.254) (layer B.Cu) (net 20))
  (segment (start 131.678 94.788) (end 161.348 94.788) (width 0.254) (layer B.Cu) (net 20))
  (segment (start 147.678 78.208) (end 146.291601 79.594399) (width 0.254) (layer F.Cu) (net 20))
  (via (at 147.598 87.458) (size 0.8128) (drill 0.4064) (layers F.Cu B.Cu) (net 20))
  (segment (start 162.928 88.968) (end 149.108 88.968) (width 0.254) (layer B.Cu) (net 20))
  (segment (start 146.291601 79.594399) (end 146.291601 86.151601) (width 0.254) (layer F.Cu) (net 20))
  (segment (start 146.291601 86.151601) (end 147.598 87.458) (width 0.254) (layer F.Cu) (net 20))
  (segment (start 149.108 88.968) (end 147.598 87.458) (width 0.254) (layer B.Cu) (net 20))
  (segment (start 145.138 80.748) (end 145.138 78.208) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 112.018 78.828) (end 124.718 78.828) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 112.018 81.368) (end 124.718 81.368) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 112.018 83.908) (end 124.718 83.908) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 124.718 78.828) (end 124.718 83.908) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 122.178 83.908) (end 122.178 78.828) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 119.638 78.828) (end 119.638 83.908) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 117.098 83.908) (end 117.098 78.828) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 114.558 78.828) (end 114.558 83.908) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 112.018 78.828) (end 112.018 83.908) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 104.703 86.983) (end 108.068 83.618) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 111.728 83.618) (end 112.018 83.908) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 108.068 83.618) (end 111.728 83.618) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 133.828 91.668) (end 131.288 91.668) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 131.288 91.668) (end 131.288 86.798) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 128.398 83.908) (end 124.718 83.908) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 131.288 86.798) (end 128.398 83.908) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 162.918 80.748) (end 162.918 78.208) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 162.918 78.208) (end 162.918 74.788) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 162.918 74.788) (end 161.658 73.528) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 161.658 73.528) (end 145.538 73.528) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 145.138 73.928) (end 145.138 78.208) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 145.538 73.528) (end 145.138 73.928) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 135.268 73.528) (end 131.288 77.508) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 131.288 77.508) (end 131.288 91.668) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 145.538 73.528) (end 135.268 73.528) (width 1.27) (layer B.Cu) (net 19))
  (segment (start 158.038 99.228) (end 156.388 99.228) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 156.388 99.228) (end 154.648 97.488) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 154.648 92.648646) (end 154.688 92.608646) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 154.648 97.488) (end 154.648 92.648646) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 154.688 92.608646) (end 154.688 89.948) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 154.688 89.948) (end 155.948 88.688) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 155.948 88.688) (end 160.028 88.688) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 162.918 85.798) (end 162.918 80.748) (width 1.27) (layer F.Cu) (net 19))
  (segment (start 160.028 88.688) (end 162.918 85.798) (width 1.27) (layer F.Cu) (net 19))

)
