(module DIP-16_W7.62mm_Proto (layer F.Cu) (tedit 5E98D090)
  (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
  (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
  (fp_text reference REF** (at 3.81 -2.33) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value DIP-16_W7.62mm_Socket (at 3.81 20.11) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 3.81 8.89) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9.15 -1.6) (end -1.55 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 9.15 19.4) (end 9.15 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.55 19.4) (end 9.15 19.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.55 -1.6) (end -1.55 19.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 8.95 -1.39) (end -1.33 -1.39) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.95 19.17) (end 8.95 -1.39) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 19.17) (end 8.95 19.17) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 -1.39) (end -1.33 19.17) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start 6.46 19.11) (end 6.46 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.16 19.11) (end 6.46 19.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.16 -1.33) (end 1.16 19.11) (layer F.SilkS) (width 0.12))
  (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start 8.89 -1.33) (end -1.27 -1.33) (layer F.Fab) (width 0.1))
  (fp_line (start 8.89 19.11) (end 8.89 -1.33) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 19.11) (end 8.89 19.11) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 -1.33) (end -1.27 19.11) (layer F.Fab) (width 0.1))
  (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer F.Fab) (width 0.1))
  (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer F.Fab) (width 0.1))
  (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer F.Fab) (width 0.1))
  (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer F.Fab) (width 0.1))
  (fp_arc (start 3.81 -1.33) (end 2.81 -1.33) (angle -180) (layer F.SilkS) (width 0.12))
  (fp_line (start 0 17.78) (end -2.54 17.78) (layer F.Cu) (width 1.27))
  (fp_line (start 0 15.24) (end -2.54 15.24) (layer F.Cu) (width 1.27))
  (fp_line (start 0 12.7) (end -2.54 12.7) (layer F.Cu) (width 1.27))
  (fp_line (start 0 10.16) (end -2.54 10.16) (layer F.Cu) (width 1.27))
  (fp_line (start 0 7.62) (end -2.54 7.62) (layer F.Cu) (width 1.27))
  (fp_line (start 0 5.08) (end -2.54 5.08) (layer F.Cu) (width 1.27))
  (fp_line (start 0 2.54) (end -2.54 2.54) (layer F.Cu) (width 1.27))
  (fp_line (start 0 0) (end -2.54 0) (layer F.Cu) (width 1.27))
  (fp_line (start 10.16 0) (end 7.62 0) (layer F.Cu) (width 1.27))
  (fp_line (start 10.16 2.54) (end 7.62 2.54) (layer F.Cu) (width 1.27))
  (fp_line (start 10.16 5.08) (end 7.62 5.08) (layer F.Cu) (width 1.27))
  (fp_line (start 10.16 7.62) (end 7.62 7.62) (layer F.Cu) (width 1.27))
  (fp_line (start 10.16 10.16) (end 7.62 10.16) (layer F.Cu) (width 1.27))
  (fp_line (start 10.16 12.7) (end 7.62 12.7) (layer F.Cu) (width 1.27))
  (fp_line (start 10.16 15.24) (end 7.62 15.24) (layer F.Cu) (width 1.27))
  (fp_line (start 10.16 17.78) (end 7.62 17.78) (layer F.Cu) (width 1.27))
  (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 17 thru_hole oval (at -2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 18 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 21 thru_hole oval (at -2.54 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 22 thru_hole oval (at 10.16 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 25 thru_hole oval (at -2.54 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 26 thru_hole oval (at 10.16 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 29 thru_hole oval (at -2.54 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 30 thru_hole oval (at 10.16 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 33 thru_hole oval (at -2.54 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 34 thru_hole oval (at 10.16 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 37 thru_hole oval (at -2.54 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 38 thru_hole oval (at 10.16 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 41 thru_hole oval (at -2.54 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 42 thru_hole oval (at 10.16 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 45 thru_hole oval (at -2.54 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 46 thru_hole oval (at 10.16 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
