(module kbd_header_two_mounting_holes (layer F.Cu) (tedit 5EF168FC)
  (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
  (tags "Through hole pin header THT 2x20 2.54mm double row")
  (fp_text reference REF** (at 1.2954 -2.5078) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value PinHeader_2x20_P2.54mm_Vertical (at 1.27 50.59) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2.5654 -1.4478) (end -1.2446 -1.4478) (layer F.Fab) (width 0.1))
  (fp_line (start -1.2446 -1.4478) (end -1.2446 49.3522) (layer F.Fab) (width 0.1))
  (fp_line (start -1.2446 49.3522) (end 3.8354 49.3522) (layer F.Fab) (width 0.1))
  (fp_line (start 3.8354 49.3522) (end 3.8354 -0.1778) (layer F.Fab) (width 0.1))
  (fp_line (start 3.8354 -0.1778) (end 2.5654 -1.4478) (layer F.Fab) (width 0.1))
  (fp_line (start 3.8954 49.4122) (end -1.3046 49.4122) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.8954 1.0922) (end 3.8954 49.4122) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.3046 -1.5078) (end -1.3046 49.4122) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.8954 1.0922) (end 1.2954 1.0922) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.2954 1.0922) (end 1.2954 -1.5078) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.2954 -1.5078) (end -1.3046 -1.5078) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.8954 -0.1778) (end 3.8954 -1.5078) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.8954 -1.5078) (end 2.5654 -1.5078) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.3654 -1.9778) (end 4.3654 49.8722) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.3654 49.8722) (end -1.7846 49.8722) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.7846 49.8722) (end -1.7846 -1.9778) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.7846 -1.9778) (end 4.3654 -1.9778) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 1.2954 23.9522 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "" np_thru_hole circle (at 91.4924 50.4712) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 91.4924 -2.8688) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask))
  (pad 40 thru_hole oval (at 0.0254 48.0822) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 39 thru_hole oval (at 2.5654 48.0822) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 38 thru_hole oval (at 0.0254 45.5422) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 37 thru_hole oval (at 2.5654 45.5422) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 36 thru_hole oval (at 0.0254 43.0022) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 35 thru_hole oval (at 2.5654 43.0022) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 34 thru_hole oval (at 0.0254 40.4622) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 33 thru_hole oval (at 2.5654 40.4622) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 32 thru_hole oval (at 0.0254 37.9222) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 31 thru_hole oval (at 2.5654 37.9222) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 30 thru_hole oval (at 0.0254 35.3822) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 29 thru_hole oval (at 2.5654 35.3822) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 28 thru_hole oval (at 0.0254 32.8422) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 27 thru_hole oval (at 2.5654 32.8422) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 26 thru_hole oval (at 0.0254 30.3022) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 25 thru_hole oval (at 2.5654 30.3022) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 24 thru_hole oval (at 0.0254 27.7622) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 23 thru_hole oval (at 2.5654 27.7622) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 22 thru_hole oval (at 0.0254 25.2222) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 21 thru_hole oval (at 2.5654 25.2222) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 20 thru_hole oval (at 0.0254 22.6822) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 19 thru_hole oval (at 2.5654 22.6822) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 18 thru_hole oval (at 0.0254 20.1422) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 17 thru_hole oval (at 2.5654 20.1422) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 16 thru_hole oval (at 0.0254 17.6022) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 15 thru_hole oval (at 2.5654 17.6022) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 14 thru_hole oval (at 0.0254 15.0622) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 13 thru_hole oval (at 2.5654 15.0622) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 12 thru_hole oval (at 0.0254 12.5222) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at 2.5654 12.5222) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 0.0254 9.9822) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at 2.5654 9.9822) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole oval (at 0.0254 7.4422) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 2.5654 7.4422) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 0.0254 4.9022) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 2.5654 4.9022) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0.0254 2.3622) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 2.5654 2.3622) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0.0254 -0.1778) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 2.5654 -0.1778) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
    (offset (xyz 2.54 0 -1.8288))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 0))
  )
)
