(footprint "Capacitor" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 621265E2)
  (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
  (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
  (attr through_hole)
  (fp_text reference "C1" (at 1.25 2.54) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e8ef4bbd-32e2-4ac3-86d3-eb359b36bf42)
  )
  (fp_text value "C" (at 1.25 2.55) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ea4f7bd6-6821-448f-bbec-c40ded7426db)
  )
  (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
    (effects (font (size 0.76 0.76) (thickness 0.114)))
    (tstamp e52d9220-36a6-4a8e-857e-59c3f9659ebc)
  )
  (fp_line (start 3.302 0.762) (end 3.302 -0.762) (layer "F.CrtYd") (width 0.12) (tstamp 40b5ab29-6809-46de-9d87-b01ea9af4068))
  (fp_line (start 3.302 -0.762) (end -0.762 -0.762) (layer "F.CrtYd") (width 0.12) (tstamp 4b724a05-e8b8-4d3a-9ef8-416f22a37460))
  (fp_line (start -0.762 0.762) (end 3.302 0.762) (layer "F.CrtYd") (width 0.12) (tstamp 81c671aa-d366-46b3-8f86-ff2263cc045a))
  (fp_line (start -0.762 -0.762) (end -0.762 0.762) (layer "F.CrtYd") (width 0.12) (tstamp a4f1e7d6-84c2-4bf5-a525-5b5c5d3f8486))
  (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (tstamp 3e8745f8-3055-487c-98b3-0d559c2ad40a))
  (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (tstamp 13b54699-28a1-4e4e-a982-18a5d294cbbd))
  (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
