#PACE: Start of Constraints generated by PACE
NET "DATA<2>"  BUFG = DATA_GATE ;
NET "DATA<3>"  BUFG = DATA_GATE ;
NET "DATA<4>"  BUFG = DATA_GATE ;
#PACE: Start of PACE I/O Pin Assignments
NET "ADD_HIGH<11>"  LOC = "P44"  ;
NET "ADD_HIGH<10>"  LOC = "P38"  ;
NET "ADD_HIGH<8>"  LOC = "P36"  ;
NET "ADD_HIGH<9>"  LOC = "P37"  ;
NET "ADD_LOW<0>"  LOC = "P19"  ;
NET "ADD_LOW<1>"  LOC = "P18"  ;
NET "B<10>"  LOC = "P22"  ;
NET "B<8>"  LOC = "P26"  ;
NET "B<9>"  LOC = "P27"  ;
NET "CARD"  LOC = "P33"  ;
NET "DATA<0>"  LOC = "P3"  ;
NET "DATA<1>"  LOC = "P4"  ;
NET "DATA<2>"  LOC = "P5" ;
NET "DATA<3>"  LOC = "P6"  ;
NET "DATA<4>"  LOC = "P7"  ;
NET "DATA<5>"  LOC = "P9"  ;
NET "DATA<6>"  LOC = "P11"  ;
NET "DATA<7>"  LOC = "P13"  ;
NET "CLK"  LOC = "P43"  ;
NET "LED"  LOC = "P29"  ;
NET "NDEV_SEL"  LOC = "P24"  ;
NET "NG"  LOC = "P12"  ;
NET "NIO_SEL"  LOC = "P14"  ;
NET "NIO_STB"  LOC = "P42"  ;
NET "NOE"  LOC = "P25"  ;
NET "PHI0"  LOC = "P8"  ;
NET "NRESET"  LOC = "P20"  ;
NET "RNW"  LOC = "P1"  ;
NET "MISO"  LOC = "P40"  ;
NET "MOSI"  LOC = "P35"  ;
NET "NSEL"  LOC = "P28"  ;
NET "SCLK"  LOC = "P34"  ;
NET "WP"  LOC = "P39"  ;

#PACE: Start of PACE Area Constraints

#PACE: Start of PACE Prohibit Constraints

#PACE: End of Constraints generated by PACE
