# -------------------------------------------------------------------------- #
#
# Copyright (C) 1991-2013 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.
#
# -------------------------------------------------------------------------- #
#
# Quartus II 32-bit
# Version 13.0.1 Build 232 06/12/2013 Service Pack 1 SJ Web Edition
# Date created = 13:41:40  March 15, 2021
#
# -------------------------------------------------------------------------- #
#
# Notes:
#
# 1) The default values for assignments are stored in the file:
#		GR8RAM_assignment_defaults.qdf
#    If this file doesn't exist, see file:
#		assignment_defaults.qdf
#
# 2) Altera recommends that you do not modify this file. This
#    file is updated automatically by the Quartus II software
#    and any changes you make may be lost or overwritten.
#
# -------------------------------------------------------------------------- #


set_global_assignment -name FAMILY "MAX II"
set_global_assignment -name DEVICE EPM240T100C5
set_global_assignment -name TOP_LEVEL_ENTITY GR8RAM
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 22.1STD.0
set_global_assignment -name PROJECT_CREATION_TIME_DATE "11:15:44  FEBRUARY 28, 2023"
set_global_assignment -name LAST_QUARTUS_VERSION "22.1std.0 Lite Edition"
set_global_assignment -name PROJECT_OUTPUT_DIRECTORY output_files
set_global_assignment -name MIN_CORE_JUNCTION_TEMP 0
set_global_assignment -name MAX_CORE_JUNCTION_TEMP 85
set_global_assignment -name DEVICE_FILTER_PACKAGE TQFP
set_global_assignment -name DEVICE_FILTER_PIN_COUNT 100
set_global_assignment -name DEVICE_FILTER_SPEED_GRADE 5
set_global_assignment -name ERROR_CHECK_FREQUENCY_DIVISOR "-1"
set_global_assignment -name POWER_EXT_SUPPLY_VOLTAGE_TO_REGULATOR 3.3V
set_global_assignment -name EDA_SIMULATION_TOOL "Questa Intel FPGA (Verilog)"
set_global_assignment -name EDA_NETLIST_WRITER_OUTPUT_DIR simulation/questa -section_id eda_simulation
set_global_assignment -name EDA_TIME_SCALE "1 ps" -section_id eda_simulation
set_global_assignment -name EDA_OUTPUT_DATA_FORMAT "VERILOG HDL" -section_id eda_simulation
set_global_assignment -name EDA_GENERATE_FUNCTIONAL_NETLIST OFF -section_id eda_board_design_timing
set_global_assignment -name EDA_GENERATE_FUNCTIONAL_NETLIST OFF -section_id eda_board_design_symbol
set_global_assignment -name EDA_GENERATE_FUNCTIONAL_NETLIST OFF -section_id eda_board_design_signal_integrity
set_global_assignment -name EDA_GENERATE_FUNCTIONAL_NETLIST OFF -section_id eda_board_design_boundary_scan
set_location_assignment PIN_2 -to RA[5]
set_location_assignment PIN_3 -to RA[6]
set_location_assignment PIN_4 -to RA[3]
set_location_assignment PIN_5 -to nFCS
set_location_assignment PIN_6 -to RA[7]
set_location_assignment PIN_7 -to RA[8]
set_location_assignment PIN_8 -to RA[9]
set_location_assignment PIN_12 -to FCK
set_location_assignment PIN_14 -to RA[10]
set_location_assignment PIN_15 -to MOSI
set_location_assignment PIN_16 -to MISO
set_location_assignment PIN_30 -to nRESout
set_location_assignment PIN_34 -to RA[11]
set_location_assignment PIN_35 -to RA[12]
set_location_assignment PIN_36 -to RA[13]
set_location_assignment PIN_37 -to RA[14]
set_location_assignment PIN_38 -to RA[15]
set_location_assignment PIN_39 -to nIOSEL
set_location_assignment PIN_42 -to nIOSTRB
set_location_assignment PIN_40 -to nDEVSEL
set_location_assignment PIN_41 -to PHI0
set_location_assignment PIN_43 -to nWE
set_location_assignment PIN_44 -to nRES
set_location_assignment PIN_47 -to SD[1]
set_location_assignment PIN_50 -to SD[0]
set_location_assignment PIN_51 -to SD[4]
set_location_assignment PIN_100 -to RA[0]
set_location_assignment PIN_99 -to RD[7]
set_location_assignment PIN_52 -to SD[5]
set_location_assignment PIN_54 -to SD[7]
set_location_assignment PIN_55 -to SD[3]
set_location_assignment PIN_56 -to SD[2]
set_location_assignment PIN_53 -to SD[6]
set_location_assignment PIN_57 -to DQMH
set_location_assignment PIN_58 -to nSWE
set_location_assignment PIN_62 -to nRAS
set_location_assignment PIN_61 -to nCAS
set_location_assignment PIN_64 -to C25M
set_location_assignment PIN_66 -to RCKE
set_location_assignment PIN_67 -to nRCS
set_location_assignment PIN_68 -to SA[12]
set_location_assignment PIN_69 -to SBA[0]
set_location_assignment PIN_70 -to SA[11]
set_location_assignment PIN_71 -to SBA[1]
set_location_assignment PIN_72 -to SA[9]
set_location_assignment PIN_73 -to SA[10]
set_location_assignment PIN_74 -to SA[8]
set_location_assignment PIN_75 -to SA[0]
set_location_assignment PIN_76 -to SA[4]
set_location_assignment PIN_77 -to SA[6]
set_location_assignment PIN_78 -to SA[7]
set_location_assignment PIN_81 -to SA[1]
set_location_assignment PIN_82 -to SA[2]
set_location_assignment PIN_83 -to SA[5]
set_location_assignment PIN_84 -to SA[3]
set_location_assignment PIN_85 -to DQML
set_location_assignment PIN_86 -to RD[0]
set_location_assignment PIN_87 -to RD[1]
set_location_assignment PIN_88 -to RD[2]
set_location_assignment PIN_89 -to RD[3]
set_location_assignment PIN_90 -to RD[4]
set_location_assignment PIN_91 -to RD[5]
set_location_assignment PIN_92 -to RD[6]
set_location_assignment PIN_97 -to RA[2]
set_location_assignment PIN_98 -to RA[1]
set_location_assignment PIN_96 -to SetFW[0]
set_location_assignment PIN_95 -to SetFW[1]
set_global_assignment -name IOBANK_VCCIO 3.3V -section_id 1
set_global_assignment -name IOBANK_VCCIO 3.3V -section_id 2
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to nFCS
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nFCS
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to FCK
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY ON -to FCK
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to MOSI
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY ON -to MOSI
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to MISO
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY ON -to MISO
set_location_assignment PIN_21 -to nDMAout
set_location_assignment PIN_19 -to RAdir
set_location_assignment PIN_20 -to INTout
set_location_assignment PIN_26 -to nNMIout
set_location_assignment PIN_27 -to nINHout
set_location_assignment PIN_28 -to nRDYout
set_location_assignment PIN_29 -to nIRQout
set_location_assignment PIN_33 -to RWout
set_location_assignment PIN_48 -to DMAin
set_location_assignment PIN_49 -to INTin
set_location_assignment PIN_17 -to RDdir
set_location_assignment PIN_18 -to DMAout
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to RA
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to RA
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to RA
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to RD
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to RD
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY ON -to RD
set_instance_assignment -name SLOW_SLEW_RATE OFF -to RD
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to RD
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to RAdir
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to RAdir
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to RAdir
set_instance_assignment -name SLOW_SLEW_RATE ON -to RAdir
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to RAdir
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to RDdir
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to RDdir
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to RDdir
set_instance_assignment -name SLOW_SLEW_RATE ON -to RDdir
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to RDdir
set_instance_assignment -name IO_STANDARD "3.3V SCHMITT TRIGGER INPUT" -to PHI0
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to PHI0
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to PHI0
set_instance_assignment -name IO_STANDARD "3.3V SCHMITT TRIGGER INPUT" -to nWE
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to nWE
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nWE
set_instance_assignment -name IO_STANDARD "3.3V SCHMITT TRIGGER INPUT" -to nDEVSEL
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to nDEVSEL
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nDEVSEL
set_instance_assignment -name IO_STANDARD "3.3V SCHMITT TRIGGER INPUT" -to nIOSEL
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to nIOSEL
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nIOSEL
set_instance_assignment -name IO_STANDARD "3.3V SCHMITT TRIGGER INPUT" -to nIOSTRB
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to nIOSTRB
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nIOSTRB
set_instance_assignment -name IO_STANDARD "3.3V SCHMITT TRIGGER INPUT" -to nRES
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to nRES
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nRES
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to nRESout
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to nRESout
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nRESout
set_instance_assignment -name SLOW_SLEW_RATE ON -to nRESout
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to nRESout
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to nFCS
set_instance_assignment -name SLOW_SLEW_RATE ON -to nFCS
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to nFCS
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to FCK
set_instance_assignment -name SLOW_SLEW_RATE ON -to FCK
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to FCK
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to MOSI
set_instance_assignment -name SLOW_SLEW_RATE ON -to MOSI
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to MOSI
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to MISO
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to C25M
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to C25M
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to C25M
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to nRCS
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to nRCS
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nRCS
set_instance_assignment -name SLOW_SLEW_RATE ON -to nRCS
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to nRCS
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to nRAS
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to nRAS
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nRAS
set_instance_assignment -name SLOW_SLEW_RATE ON -to nRAS
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to nRAS
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to nCAS
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to nCAS
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nCAS
set_instance_assignment -name SLOW_SLEW_RATE ON -to nCAS
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to nCAS
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to nSWE
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to nSWE
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to nSWE
set_instance_assignment -name SLOW_SLEW_RATE ON -to nSWE
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to nSWE
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to RCKE
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to RCKE
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to RCKE
set_instance_assignment -name SLOW_SLEW_RATE ON -to RCKE
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to RCKE
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SBA
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to SBA
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to SBA
set_instance_assignment -name SLOW_SLEW_RATE ON -to SBA
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to SBA
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SA
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to SA
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to SA
set_instance_assignment -name SLOW_SLEW_RATE ON -to SA
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to SA
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DQMH
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to DQMH
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to DQMH
set_instance_assignment -name SLOW_SLEW_RATE ON -to DQMH
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to DQMH
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to DQML
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to DQML
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to DQML
set_instance_assignment -name SLOW_SLEW_RATE ON -to DQML
set_instance_assignment -name CURRENT_STRENGTH_NEW "MINIMUM CURRENT" -to DQML
set_instance_assignment -name IO_STANDARD "3.3V SCHMITT TRIGGER INPUT" -to SetFW
set_instance_assignment -name WEAK_PULL_UP_RESISTOR ON -to SetFW
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to SetFW
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to SD
set_instance_assignment -name WEAK_PULL_UP_RESISTOR OFF -to SD
set_instance_assignment -name ENABLE_BUS_HOLD_CIRCUITRY OFF -to SD
set_instance_assignment -name SLOW_SLEW_RATE ON -to SD
set_instance_assignment -name CURRENT_STRENGTH_NEW "MAXIMUM CURRENT" -to SD
set_global_assignment -name SDC_FILE GR8RAM.sdc