 -- Copyright (C) 2022  Intel Corporation. All rights reserved.
 -- Your use of Intel Corporation's design tools, logic functions 
 -- and other software and tools, and any partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Intel Program License 
 -- Subscription Agreement, the Intel Quartus Prime License Agreement,
 -- the Intel FPGA IP License Agreement, or other applicable license
 -- agreement, including, without limitation, that your use is for
 -- the sole purpose of programming logic devices manufactured by
 -- Intel and sold by Intel or its authorized distributors.  Please
 -- refer to the applicable agreement for further details, at
 -- https://fpgasoftware.intel.com/eula.
 -- 
 -- This is a Quartus Prime output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus Prime input file. This file cannot be used
 -- to make Quartus Prime pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus Prime help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCCINT        : Dedicated power pin, which MUST be connected to VCC  (2.5V/3.3V).
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 --                  Bank 1:       3.3V
 --                  Bank 2:       3.3V
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --                  It can also be used to report unused dedicated pins. The connection
 --                  on the board for unused dedicated pins depends on whether this will
 --                  be used in a future design. One example is device migration. When
 --                  using device migration, refer to the device pin-tables. If it is a
 --                  GND pin in the pin table or if it will not be used in a future design
 --                  for another purpose the it MUST be connected to GND. If it is an unused
 --                  dedicated pin, then it can be connected to a valid signal on the board
 --                  (low, high, or toggling) if that signal is required for a different
 --                  revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --                  This pin should be connected to GND. It may also be connected  to a
 --                  valid signal  on the board  (low, high, or toggling)  if that signal
 --                  is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin. Connect each pin marked GND* directly to GND
 --                  or leave it unconnected.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus Prime Version 22.1std.0 Build 915 10/25/2022 SC Lite Edition
CHIP  "GR8RAM"  ASSIGNED TO AN: EPM240T100C5

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
RA[4]                        : 1         : input  : 3.3-V LVTTL       :         : 2         : N              
RA[5]                        : 2         : input  : 3.3-V LVTTL       :         : 1         : Y              
RA[6]                        : 3         : input  : 3.3-V LVTTL       :         : 1         : Y              
RA[3]                        : 4         : input  : 3.3-V LVTTL       :         : 1         : Y              
nFCS                         : 5         : output : 3.3-V LVTTL       :         : 1         : Y              
RA[7]                        : 6         : input  : 3.3-V LVTTL       :         : 1         : Y              
RA[8]                        : 7         : input  : 3.3-V LVTTL       :         : 1         : Y              
RA[9]                        : 8         : input  : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : 9         : power  :                   : 3.3V    : 1         :                
GNDIO                        : 10        : gnd    :                   :         :           :                
GNDINT                       : 11        : gnd    :                   :         :           :                
FCK                          : 12        : output : 3.3-V LVTTL       :         : 1         : Y              
VCCINT                       : 13        : power  :                   : 2.5V/3.3V :           :                
RA[10]                       : 14        : input  : 3.3-V LVTTL       :         : 1         : Y              
MOSI                         : 15        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
MISO                         : 16        : input  : 3.3-V LVTTL       :         : 1         : Y              
RDdir                        : 17        : output : 3.3-V LVTTL       :         : 1         : Y              
DMAout                       : 18        : output : 3.3-V LVTTL       :         : 1         : Y              
RAdir                        : 19        : output : 3.3-V LVTTL       :         : 1         : Y              
INTout                       : 20        : output : 3.3-V LVTTL       :         : 1         : Y              
nDMAout                      : 21        : output : 3.3-V LVTTL       :         : 1         : Y              
TMS                          : 22        : input  :                   :         : 1         :                
TDI                          : 23        : input  :                   :         : 1         :                
TCK                          : 24        : input  :                   :         : 1         :                
TDO                          : 25        : output :                   :         : 1         :                
nNMIout                      : 26        : output : 3.3-V LVTTL       :         : 1         : Y              
nINHout                      : 27        : output : 3.3-V LVTTL       :         : 1         : Y              
nRDYout                      : 28        : output : 3.3-V LVTTL       :         : 1         : Y              
nIRQout                      : 29        : output : 3.3-V LVTTL       :         : 1         : Y              
nRESout                      : 30        : output : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : 31        : power  :                   : 3.3V    : 1         :                
GNDIO                        : 32        : gnd    :                   :         :           :                
RWout                        : 33        : output : 3.3-V LVTTL       :         : 1         : Y              
RA[11]                       : 34        : input  : 3.3-V LVTTL       :         : 1         : Y              
RA[12]                       : 35        : input  : 3.3-V LVTTL       :         : 1         : Y              
RA[13]                       : 36        : input  : 3.3-V LVTTL       :         : 1         : Y              
RA[14]                       : 37        : input  : 3.3-V LVTTL       :         : 1         : Y              
RA[15]                       : 38        : input  : 3.3-V LVTTL       :         : 1         : Y              
nIOSEL                       : 39        : input  : 3.3V Schmitt Trigger Input :         : 1         : Y              
nDEVSEL                      : 40        : input  : 3.3V Schmitt Trigger Input :         : 1         : Y              
PHI0                         : 41        : input  : 3.3V Schmitt Trigger Input :         : 1         : Y              
nIOSTRB                      : 42        : input  : 3.3V Schmitt Trigger Input :         : 1         : Y              
nWE                          : 43        : input  : 3.3V Schmitt Trigger Input :         : 1         : Y              
nRES                         : 44        : input  : 3.3V Schmitt Trigger Input :         : 1         : Y              
VCCIO1                       : 45        : power  :                   : 3.3V    : 1         :                
GNDIO                        : 46        : gnd    :                   :         :           :                
SD[1]                        : 47        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DMAin                        : 48        : input  : 3.3-V LVTTL       :         : 1         : Y              
INTin                        : 49        : input  : 3.3-V LVTTL       :         : 1         : Y              
SD[0]                        : 50        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
SD[4]                        : 51        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
SD[5]                        : 52        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
SD[6]                        : 53        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
SD[7]                        : 54        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
SD[3]                        : 55        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
SD[2]                        : 56        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
DQMH                         : 57        : output : 3.3-V LVTTL       :         : 2         : Y              
nSWE                         : 58        : output : 3.3-V LVTTL       :         : 2         : Y              
VCCIO2                       : 59        : power  :                   : 3.3V    : 2         :                
GNDIO                        : 60        : gnd    :                   :         :           :                
nCAS                         : 61        : output : 3.3-V LVTTL       :         : 2         : Y              
nRAS                         : 62        : output : 3.3-V LVTTL       :         : 2         : Y              
VCCINT                       : 63        : power  :                   : 2.5V/3.3V :           :                
C25M                         : 64        : input  : 3.3-V LVTTL       :         : 2         : Y              
GNDINT                       : 65        : gnd    :                   :         :           :                
RCKE                         : 66        : output : 3.3-V LVTTL       :         : 2         : Y              
nRCS                         : 67        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[12]                       : 68        : output : 3.3-V LVTTL       :         : 2         : Y              
SBA[0]                       : 69        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[11]                       : 70        : output : 3.3-V LVTTL       :         : 2         : Y              
SBA[1]                       : 71        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[9]                        : 72        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[10]                       : 73        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[8]                        : 74        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[0]                        : 75        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[4]                        : 76        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[6]                        : 77        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[7]                        : 78        : output : 3.3-V LVTTL       :         : 2         : Y              
GNDIO                        : 79        : gnd    :                   :         :           :                
VCCIO2                       : 80        : power  :                   : 3.3V    : 2         :                
SA[1]                        : 81        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[2]                        : 82        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[5]                        : 83        : output : 3.3-V LVTTL       :         : 2         : Y              
SA[3]                        : 84        : output : 3.3-V LVTTL       :         : 2         : Y              
DQML                         : 85        : output : 3.3-V LVTTL       :         : 2         : Y              
RD[0]                        : 86        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
RD[1]                        : 87        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
RD[2]                        : 88        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
RD[3]                        : 89        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
RD[4]                        : 90        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
RD[5]                        : 91        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
RD[6]                        : 92        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
GNDIO                        : 93        : gnd    :                   :         :           :                
VCCIO2                       : 94        : power  :                   : 3.3V    : 2         :                
SetFW[1]                     : 95        : input  : 3.3V Schmitt Trigger Input :         : 2         : Y              
SetFW[0]                     : 96        : input  : 3.3V Schmitt Trigger Input :         : 2         : Y              
RA[2]                        : 97        : input  : 3.3-V LVTTL       :         : 2         : Y              
RA[1]                        : 98        : input  : 3.3-V LVTTL       :         : 2         : Y              
RD[7]                        : 99        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
RA[0]                        : 100       : input  : 3.3-V LVTTL       :         : 2         : Y              
