{ "Info" "IQCU_PARALLEL_AUTODETECT_ONE_PROCESSOR" "" "Only one processor detected - disabling parallel compilation" {  } {  } 0 20029 "Only one processor detected - disabling parallel compilation" 0 0 "Fitter" 0 -1 1590959452243 ""}
{ "Info" "IMPP_MPP_USER_DEVICE" "RAM2E EPM240T100C5 " "Selected device EPM240T100C5 for design \"RAM2E\"" {  } {  } 0 119006 "Selected device %2!s! for design \"%1!s!\"" 0 0 "Fitter" 0 -1 1590959452274 ""}
{ "Info" "ICUT_CUT_USING_OPERATING_CONDITION" "Low junction temperature 0 degrees C " "Low junction temperature is 0 degrees C" {  } {  } 0 21077 "%1!s! is %2!s!" 0 0 "Fitter" 0 -1 1590959452540 ""}
{ "Info" "ICUT_CUT_USING_OPERATING_CONDITION" "High junction temperature 85 degrees C " "High junction temperature is 85 degrees C" {  } {  } 0 21077 "%1!s! is %2!s!" 0 0 "Fitter" 0 -1 1590959452540 ""}
{ "Info" "IFITCC_FITCC_INFO_STANDARD_FIT_COMPILATION_ON" "" "Fitter is performing a Standard Fit compilation using maximum Fitter effort to optimize design performance" {  } {  } 0 171004 "Fitter is performing a Standard Fit compilation using maximum Fitter effort to optimize design performance" 0 0 "Fitter" 0 -1 1590959452837 ""}
{ "Warning" "WCPT_FEATURE_DISABLED_POST" "LogicLock " "Feature LogicLock is only available with a valid subscription license. You can purchase a software subscription to gain full access to this feature." {  } {  } 0 292013 "Feature %1!s! is only available with a valid subscription license. You can purchase a software subscription to gain full access to this feature." 0 0 "Fitter" 0 -1 1590959452868 ""}
{ "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED" "" "Device migration not selected. If you intend to use device migration later, you may need to change the pin assignments as they may be incompatible with other devices" { { "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED_SUB" "EPM240T100I5 " "Device EPM240T100I5 is compatible" {  } {  } 2 176445 "Device %1!s! is compatible" 0 0 "Quartus II" 0 -1 1590959453087 ""} { "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED_SUB" "EPM240T100A5 " "Device EPM240T100A5 is compatible" {  } {  } 2 176445 "Device %1!s! is compatible" 0 0 "Quartus II" 0 -1 1590959453087 ""} { "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED_SUB" "EPM570T100C5 " "Device EPM570T100C5 is compatible" {  } {  } 2 176445 "Device %1!s! is compatible" 0 0 "Quartus II" 0 -1 1590959453087 ""} { "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED_SUB" "EPM570T100I5 " "Device EPM570T100I5 is compatible" {  } {  } 2 176445 "Device %1!s! is compatible" 0 0 "Quartus II" 0 -1 1590959453087 ""} { "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED_SUB" "EPM570T100A5 " "Device EPM570T100A5 is compatible" {  } {  } 2 176445 "Device %1!s! is compatible" 0 0 "Quartus II" 0 -1 1590959453087 ""}  } {  } 2 176444 "Device migration not selected. If you intend to use device migration later, you may need to change the pin assignments as they may be incompatible with other devices" 0 0 "Fitter" 0 -1 1590959453087 ""}
{ "Info" "ISTA_SDC_FOUND" "constraints.sdc " "Reading SDC File: 'constraints.sdc'" {  } {  } 0 332104 "Reading SDC File: '%1!s!'" 0 0 "Fitter" 0 -1 1590959453353 ""}
{ "Warning" "WSTA_NODE_FOUND_WITHOUT_CLOCK_ASSIGNMENT" "DRCLK " "Node: DRCLK was determined to be a clock but was found without an associated clock assignment." {  } {  } 0 332060 "Node: %1!s! was determined to be a clock but was found without an associated clock assignment." 0 0 "Fitter" 0 -1 1590959453399 "|RAM2E|DRCLK"}
{ "Warning" "WSTA_NODE_FOUND_WITHOUT_CLOCK_ASSIGNMENT" "ARCLK " "Node: ARCLK was determined to be a clock but was found without an associated clock assignment." {  } {  } 0 332060 "Node: %1!s! was determined to be a clock but was found without an associated clock assignment." 0 0 "Fitter" 0 -1 1590959453399 "|RAM2E|ARCLK"}
{ "Info" "ISTA_USER_TDC_OPTIMIZATION_GOALS" "" "Detected timing requirements -- optimizing circuit to achieve only the specified requirements" {  } {  } 0 332129 "Detected timing requirements -- optimizing circuit to achieve only the specified requirements" 0 0 "Fitter" 0 -1 1590959453415 ""}
{ "Info" "ISTA_REPORT_CLOCKS_INFO" "Found 1 clocks " "Found 1 clocks" { { "Info" "ISTA_REPORT_CLOCKS_INFO" "  Period   Clock Name " "  Period   Clock Name" {  } {  } 0 332111 "%1!s!" 0 0 "Quartus II" 0 -1 1590959453415 ""} { "Info" "ISTA_REPORT_CLOCKS_INFO" "======== ============ " "======== ============" {  } {  } 0 332111 "%1!s!" 0 0 "Quartus II" 0 -1 1590959453415 ""} { "Info" "ISTA_REPORT_CLOCKS_INFO" "  69.841         C14M " "  69.841         C14M" {  } {  } 0 332111 "%1!s!" 0 0 "Quartus II" 0 -1 1590959453415 ""}  } {  } 0 332111 "%1!s!" 0 0 "Fitter" 0 -1 1590959453415 ""}
{ "Extra Info" "IFSAC_FSAC_START_REG_LOCATION_PROCESSING" "" "Performing register packing on registers with non-logic cell location assignments" {  } {  } 1 176273 "Performing register packing on registers with non-logic cell location assignments" 1 0 "Fitter" 0 -1 1590959453415 ""}
{ "Extra Info" "IFSAC_FSAC_FINISH_REG_LOCATION_PROCESSING" "" "Completed register packing on registers with non-logic cell location assignments" {  } {  } 1 176274 "Completed register packing on registers with non-logic cell location assignments" 1 0 "Fitter" 0 -1 1590959453431 ""}
{ "Info" "IFYGR_FYGR_OPINFO_COMPLETED_OP" "User Assigned Global Signals Promotion Operation " "Completed User Assigned Global Signals Promotion Operation" {  } {  } 0 186079 "Completed %1!s!" 0 0 "Fitter" 0 -1 1590959453446 ""}
{ "Info" "IFYGR_FYGR_AUTO_GLOBAL_ASSIGNED_ALL_TO_GLOBAL" "C14M Global clock in PIN 12 " "Automatically promoted signal \"C14M\" to use Global clock in PIN 12" {  } { { "RAM2E.v" "" { Text "//vmware-host/Shared Folders/Repos/RAM2E/cpld/RAM2E.v" 9 -1 0 } }  } 0 186215 "Automatically promoted signal \"%1!s!\" to use %2!s!" 0 0 "Fitter" 0 -1 1590959453462 ""}
{ "Info" "IFYGR_FYGR_OPINFO_COMPLETED_OP" "Auto Global Promotion Operation " "Completed Auto Global Promotion Operation" {  } {  } 0 186079 "Completed %1!s!" 0 0 "Fitter" 0 -1 1590959453462 ""}
{ "Info" "IFSAC_FSAC_REGISTER_PACKING_START_FYGR_REGPACKING_INFO" "" "Starting register packing" {  } {  } 0 176234 "Starting register packing" 0 0 "Fitter" 0 -1 1590959453462 ""}
{ "Info" "IFYGR_FYGR_INFO_AUTO_MODE_REGISTER_PACKING" "Auto Normal " "Fitter is using Normal packing mode for logic elements with Auto setting for Auto Packed Registers logic option" {  } {  } 0 186391 "Fitter is using %2!s! packing mode for logic elements with %1!s! setting for Auto Packed Registers logic option" 0 0 "Fitter" 0 -1 1590959453540 ""}
{ "Extra Info" "IFSAC_FSAC_START_LUT_PACKING" "" "Moving registers into LUTs to improve timing and density" {  } {  } 1 176244 "Moving registers into LUTs to improve timing and density" 1 0 "Fitter" 0 -1 1590959453556 ""}
{ "Info" "IFYGR_FYGR_NO_REGS_IN_IOS_HEADER" "" "Started processing fast register assignments" {  } {  } 0 186468 "Started processing fast register assignments" 0 0 "Fitter" 0 -1 1590959453634 ""}
{ "Info" "IFYGR_FYGR_NO_REGS_IN_IOS_FOOTER" "" "Finished processing fast register assignments" {  } {  } 0 186469 "Finished processing fast register assignments" 0 0 "Fitter" 0 -1 1590959453649 ""}
{ "Extra Info" "IFSAC_FSAC_FINISH_LUT_PACKING" "00:00:00 " "Finished moving registers into LUTs: elapsed time is 00:00:00" {  } {  } 1 176245 "Finished moving registers into LUTs: elapsed time is %1!s!" 1 0 "Fitter" 0 -1 1590959453649 ""}
{ "Info" "IFSAC_FSAC_REGISTER_PACKING_FINISH_REGPACKING_INFO" "" "Finished register packing" {  } {  } 0 176235 "Finished register packing" 0 0 "Fitter" 0 -1 1590959453649 ""}
{ "Info" "IFITCC_FITTER_PREPARATION_END" "00:00:00 " "Fitter preparation operations ending: elapsed time is 00:00:00" {  } {  } 0 171121 "Fitter preparation operations ending: elapsed time is %1!s!" 0 0 "Fitter" 0 -1 1590959453728 ""}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_PLACEMENT_PREP_START" "" "Fitter placement preparation operations beginning" {  } {  } 0 170189 "Fitter placement preparation operations beginning" 0 0 "Fitter" 0 -1 1590959454024 ""}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_PLACEMENT_PREP_END" "00:00:00 " "Fitter placement preparation operations ending: elapsed time is 00:00:00" {  } {  } 0 170190 "Fitter placement preparation operations ending: elapsed time is %1!s!" 0 0 "Fitter" 0 -1 1590959454290 ""}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_PLACEMENT_START" "" "Fitter placement operations beginning" {  } {  } 0 170191 "Fitter placement operations beginning" 0 0 "Fitter" 0 -1 1590959454306 ""}
{ "Info" "IFITAPI_FITAPI_INFO_VPR_PLACEMENT_FINISH" "" "Fitter placement was successful" {  } {  } 0 170137 "Fitter placement was successful" 0 0 "Fitter" 0 -1 1590959454837 ""}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_PLACEMENT_END" "00:00:01 " "Fitter placement operations ending: elapsed time is 00:00:01" {  } {  } 0 170192 "Fitter placement operations ending: elapsed time is %1!s!" 0 0 "Fitter" 0 -1 1590959454837 ""}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_ROUTING_START" "" "Fitter routing operations beginning" {  } {  } 0 170193 "Fitter routing operations beginning" 0 0 "Fitter" 0 -1 1590959454946 ""}
{ "Info" "IFITAPI_FITAPI_VPR_STATUS_DELAY_ADDED_FOR_HOLD" "4e+01 ns 2.8% " "4e+01 ns of routing delay (approximately 2.8% of available device routing delay) has been added to meet hold timing. For more information, refer to the Estimated Delay Added for Hold Timing section in the Fitter report." {  } {  } 0 170089 "%1!s! of routing delay (approximately %2!s! of available device routing delay) has been added to meet hold timing. For more information, refer to the Estimated Delay Added for Hold Timing section in the Fitter report." 0 0 "Fitter" 0 -1 1590959455321 ""}
{ "Info" "IFITAPI_FITAPI_VPR_PERCENT_ROUTING_RESOURCE_USAGE" "18 " "Router estimated average interconnect usage is 18% of the available device resources" { { "Info" "IFITAPI_FITAPI_VPR_PEAK_ROUTING_REGION" "18 X0_Y0 X8_Y5 " "Router estimated peak interconnect usage is 18% of the available device resources in the region that extends from location X0_Y0 to location X8_Y5" {  } { { "loc" "" { Generic "//vmware-host/Shared Folders/Repos/RAM2E/cpld/" { { 1 { 0 "Router estimated peak interconnect usage is 18% of the available device resources in the region that extends from location X0_Y0 to location X8_Y5"} { { 11 { 0 "Router estimated peak interconnect usage is 18% of the available device resources in the region that extends from location X0_Y0 to location X8_Y5"} 0 0 9 6 }  }  }  }  } }  } 0 170196 "Router estimated peak interconnect usage is %1!d!%% of the available device resources in the region that extends from location %2!s! to location %3!s!" 0 0 "Quartus II" 0 -1 1590959455415 ""}  } {  } 0 170195 "Router estimated average interconnect usage is %1!d!%% of the available device resources" 0 0 "Fitter" 0 -1 1590959455415 ""}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_ROUTING_END" "00:00:01 " "Fitter routing operations ending: elapsed time is 00:00:01" {  } {  } 0 170194 "Fitter routing operations ending: elapsed time is %1!s!" 0 0 "Fitter" 0 -1 1590959455665 ""}
{ "Info" "IVPR20K_VPR_TIMING_ANALYSIS_TIME" "0.28 " "Total time spent on timing analysis during the Fitter is 0.28 seconds." {  } {  } 0 11888 "Total time spent on timing analysis during the Fitter is %1!s! seconds." 0 0 "Fitter" 0 -1 1590959455696 ""}
{ "Info" "IFITCC_FITTER_POST_OPERATION_END" "00:00:00 " "Fitter post-fit operations ending: elapsed time is 00:00:00" {  } {  } 0 11218 "Fitter post-fit operations ending: elapsed time is %1!s!" 0 0 "Fitter" 0 -1 1590959455712 ""}
{ "Warning" "WFITCC_FITCC_IGNORED_ASSIGNMENT" "" "Found invalid Fitter assignments. See the Ignored Assignments panel in the Fitter Compilation Report for more information." {  } {  } 0 171167 "Found invalid Fitter assignments. See the Ignored Assignments panel in the Fitter Compilation Report for more information." 0 0 "Fitter" 0 -1 1590959455728 ""}
{ "Warning" "WFIOMGR_RESERVE_ASSIGNMENT_FOR_UNUSED_PINS_IS_DEFAULT" "As output driving ground " "The Reserve All Unused Pins setting has not been specified, and will default to 'As output driving ground'." {  } {  } 0 169174 "The Reserve All Unused Pins setting has not been specified, and will default to '%1!s!'." 0 0 "Fitter" 0 -1 1590959455743 ""}
{ "Info" "IRDB_WROTE_SUPPRESSED_MSGS" "/Repos/RAM2E/cpld/output_files/RAM2E.fit.smsg " "Generated suppressed messages file /Repos/RAM2E/cpld/output_files/RAM2E.fit.smsg" {  } {  } 0 144001 "Generated suppressed messages file %1!s!" 0 0 "Fitter" 0 -1 1590959455946 ""}
{ "Info" "IQEXE_ERROR_COUNT" "Fitter 0 s 5 s Quartus II 32-bit " "Quartus II 32-bit Fitter was successful. 0 errors, 5 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "366 " "Peak virtual memory: 366 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "Quartus II" 0 -1 1590959457103 ""} { "Info" "IQEXE_END_BANNER_TIME" "Sun May 31 17:10:56 2020 " "Processing ended: Sun May 31 17:10:56 2020" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "Quartus II" 0 -1 1590959457103 ""} { "Info" "IQEXE_ELAPSED_TIME" "00:00:07 " "Elapsed time: 00:00:07" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "Quartus II" 0 -1 1590959457103 ""} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:06 " "Total CPU time (on all processors): 00:00:06" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "Quartus II" 0 -1 1590959457103 ""}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "Fitter" 0 -1 1590959457103 ""}
