
            Lattice Mapping Report File for Design Module 'RAM2E'


Design Information
------------------

Command line:   map -a MachXO2 -p LCMXO2-640HC -t TQFP100 -s 4 -oc Commercial
     RAM2E_LCMXO2_640HC_impl1.ngd -o RAM2E_LCMXO2_640HC_impl1_map.ncd -pr
     RAM2E_LCMXO2_640HC_impl1.prf -mp RAM2E_LCMXO2_640HC_impl1.mrp -lpf //Mac/iC
     loud/Repos/ram2e/CPLD/LCMXO2-640HC/impl1/RAM2E_LCMXO2_640HC_impl1_synplify.
     lpf -lpf //Mac/iCloud/Repos/ram2e/CPLD/RAM2E-LCMXO2.lpf -c 0 -gui -msgset
     //Mac/iCloud/Repos/ram2e/CPLD/LCMXO2-640HC/promote.xml 
Target Vendor:  LATTICE
Target Device:  LCMXO2-640HCTQFP100
Target Performance:   4
Mapper:  xo2c00,  version:  Diamond (64-bit) 3.12.1.454
Mapped on:  12/28/23  23:23:28

Design Summary
--------------

   Number of registers:    122 out of   877 (14%)
      PFU registers:           93 out of   640 (15%)
      PIO registers:           29 out of   237 (12%)
   Number of SLICEs:       148 out of   320 (46%)
      SLICEs as Logic/ROM:    148 out of   320 (46%)
      SLICEs as RAM:            0 out of   240 (0%)
      SLICEs as Carry:          9 out of   320 (3%)
   Number of LUT4s:        296 out of   640 (46%)
      Number used as logic LUTs:        278
      Number used as distributed RAM:     0
      Number used as ripple logic:       18
      Number used as shift registers:     0
   Number of PIO sites used: 69 + 4(JTAG) out of 79 (92%)
   Number of block RAMs:  0 out of 2 (0%)
   Number of GSRs:        0 out of 1 (0%)
   EFB used :        Yes
   JTAG used :       No
   Readback used :   No
   Oscillator used : No
   Startup used :    No
   POR :             On
   Bandgap :         On
   Number of Power Controller:  0 out of 1 (0%)
   Number of Dynamic Bank Controller (BCINRD):  0 out of 4 (0%)
   Number of DCCA:  0 out of 8 (0%)
   Number of DCMA:  0 out of 2 (0%)
   Notes:-
      1. Total number of LUT4s = (Number of logic LUT4s) + 2*(Number of
     distributed RAMs) + 2*(Number of ripple logic)
      2. Number of logic LUT4s does not include count of distributed RAM and
     ripple logic.
   Number of clocks:  1
     Net C14M_c: 89 loads, 73 rising, 16 falling (Driver: PIO C14M )
   Number of Clock Enables:  14
     Net N_225_i: 2 loads, 0 LSLICEs
     Net N_201_i: 2 loads, 0 LSLICEs
     Net N_187_i: 11 loads, 11 LSLICEs
     Net ram2e_ufm/wb_adr_0_sqmuxa_1_i: 1 loads, 1 LSLICEs
     Net RC12: 2 loads, 2 LSLICEs
     Net ram2e_ufm/CmdBitbangMXO2_RNINSM62: 8 loads, 8 LSLICEs

                                    Page 1




Design:  RAM2E                                         Date:  12/28/23  23:23:28

Design Summary (cont)
---------------------
     Net ram2e_ufm/wb_we_RNO_0: 1 loads, 1 LSLICEs
     Net N_185_i: 2 loads, 2 LSLICEs
     Net ram2e_ufm/un1_CmdSetRWBankFFChip13_1_i_0_0[0]: 1 loads, 1 LSLICEs
     Net ram2e_ufm/un1_RWMask_0_sqmuxa_1_i_0_0[0]: 4 loads, 4 LSLICEs
     Net ram2e_ufm/un1_LEDEN_0_sqmuxa_1_i_0_0[0]: 1 loads, 1 LSLICEs
     Net N_126: 6 loads, 6 LSLICEs
     Net un9_VOEEN_0_a2_0_a3_0_a3: 1 loads, 1 LSLICEs
     Net Vout3: 8 loads, 0 LSLICEs
   Number of LSRs:  7
     Net un1_CS_0_sqmuxa_i: 2 loads, 2 LSLICEs
     Net BA_0_sqmuxa: 2 loads, 0 LSLICEs
     Net S[2]: 1 loads, 1 LSLICEs
     Net ram2e_ufm/wb_rst: 1 loads, 0 LSLICEs
     Net ram2e_ufm/wb_rst16_i: 1 loads, 1 LSLICEs
     Net N_1080_0: 1 loads, 1 LSLICEs
     Net N_1078_0: 1 loads, 1 LSLICEs
   Number of nets driven by tri-state buffers:  0
   Top 10 highest fanout non-clock nets:
     Net S[2]: 50 loads
     Net S[3]: 45 loads
     Net S[0]: 37 loads
     Net S[1]: 34 loads
     Net FS[12]: 24 loads
     Net FS[11]: 22 loads
     Net FS[10]: 19 loads
     Net FS[13]: 19 loads
     Net FS[9]: 19 loads
     Net FS[8]: 18 loads




   Number of warnings:  3
   Number of errors:    0
     

Design Errors/Warnings
----------------------

WARNING - map: //Mac/iCloud/Repos/ram2e/CPLD/RAM2E-LCMXO2.lpf(93): Semantic
     error in "IOBUF PORT "nWE80" IO_TYPE=LVCMOS33 PULLMODE=NONE ;": Port
     "nWE80" does not exist in the design. This preference has been disabled.
WARNING - map: UFM was enabled in EFB: Enabling the configuration interface will
     temporarily disable certain features of the device including Power
     Controller, GSR, Hardened User SPI Port, Hardened Primary User I2C Port.
     Functionality is restored after the Flash Memory (UFM/Configuration)
     Interface is disabled using Disable Configuration Interface command 0x26
     followed by Bypass command 0xFF. 
WARNING - map: IO buffer missing for top level port nWE80...logic will be
     discarded.

IO (PIO) Attributes
-------------------

+---------------------+-----------+-----------+------------+
| IO Name             | Direction | Levelmode | IO         |

                                    Page 2




Design:  RAM2E                                         Date:  12/28/23  23:23:28

IO (PIO) Attributes (cont)
--------------------------
|                     |           |  IO_TYPE  | Register   |
+---------------------+-----------+-----------+------------+
| RD[0]               | BIDIR     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| LED                 | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| C14M                | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| RD[7]               | BIDIR     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| RD[6]               | BIDIR     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| RD[5]               | BIDIR     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| RD[4]               | BIDIR     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| RD[3]               | BIDIR     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| RD[2]               | BIDIR     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| RD[1]               | BIDIR     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| DQMH                | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| DQML                | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[11]           | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[10]           | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[9]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[8]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[7]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[6]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[5]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[4]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[3]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[2]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[1]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| RAout[0]            | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| BA[1]               | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| BA[0]               | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| nRWEout             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+

                                    Page 3




Design:  RAM2E                                         Date:  12/28/23  23:23:28

IO (PIO) Attributes (cont)
--------------------------
| nCASout             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| nRASout             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| nCSout              | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| CKEout              | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| nVOE                | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Vout[7]             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| Vout[6]             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| Vout[5]             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| Vout[4]             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| Vout[3]             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| Vout[2]             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| Vout[1]             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| Vout[0]             | OUTPUT    | LVCMOS33  | OUT        |
+---------------------+-----------+-----------+------------+
| nDOE                | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Dout[7]             | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Dout[6]             | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Dout[5]             | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Dout[4]             | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Dout[3]             | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Dout[2]             | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Dout[1]             | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Dout[0]             | OUTPUT    | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Din[7]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Din[6]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Din[5]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Din[4]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Din[3]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Din[2]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+

                                    Page 4




Design:  RAM2E                                         Date:  12/28/23  23:23:28

IO (PIO) Attributes (cont)
--------------------------
| Din[1]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Din[0]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Ain[7]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Ain[6]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Ain[5]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Ain[4]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Ain[3]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Ain[2]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Ain[1]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| Ain[0]              | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| nC07X               | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| nEN80               | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| nWE                 | INPUT     | LVCMOS33  |            |
+---------------------+-----------+-----------+------------+
| PHI1                | INPUT     | LVCMOS33  | IN         |
+---------------------+-----------+-----------+------------+

Removed logic
-------------

Block GSR_INST undriven or does not drive anything - clipped.
Block ram2e_ufm/VCC undriven or does not drive anything - clipped.
Block ram2e_ufm/GND undriven or does not drive anything - clipped.
Signal CKEout.CN was merged into signal C14M_c
Signal ram2e_ufm/ufmefb/VCC undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/GND undriven or does not drive anything - clipped.
Signal FS_s_0_S1[15] undriven or does not drive anything - clipped.
Signal FS_s_0_COUT[15] undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/CFGSTDBY undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/CFGWAKE undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/wbc_ufm_irq undriven or does not drive anything -
     clipped.
Signal ram2e_ufm/ufmefb/TCOC undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/TCINT undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIIRQO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPICSNEN undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIMCSN7 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIMCSN6 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIMCSN5 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIMCSN4 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIMCSN3 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIMCSN2 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIMCSN1 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIMCSN0 undriven or does not drive anything - clipped.

                                    Page 5




Design:  RAM2E                                         Date:  12/28/23  23:23:28

Removed logic (cont)
--------------------
Signal ram2e_ufm/ufmefb/SPIMOSIEN undriven or does not drive anything - clipped.
     
Signal ram2e_ufm/ufmefb/SPIMOSIO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPIMISOEN undriven or does not drive anything - clipped.
     
Signal ram2e_ufm/ufmefb/SPIMISOO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPISCKEN undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/SPISCKO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/I2C2IRQO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/I2C1IRQO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/I2C2SDAOEN undriven or does not drive anything -
     clipped.
Signal ram2e_ufm/ufmefb/I2C2SDAO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/I2C2SCLOEN undriven or does not drive anything -
     clipped.
Signal ram2e_ufm/ufmefb/I2C2SCLO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/I2C1SDAOEN undriven or does not drive anything -
     clipped.
Signal ram2e_ufm/ufmefb/I2C1SDAO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/I2C1SCLOEN undriven or does not drive anything -
     clipped.
Signal ram2e_ufm/ufmefb/I2C1SCLO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLDATO0 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLDATO1 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLDATO2 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLDATO3 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLDATO4 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLDATO5 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLDATO6 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLDATO7 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLADRO0 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLADRO1 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLADRO2 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLADRO3 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLADRO4 undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLWEO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLL1STBO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLL0STBO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLRSTO undriven or does not drive anything - clipped.
Signal ram2e_ufm/ufmefb/PLLCLKO undriven or does not drive anything - clipped.
Signal FS_cry_0_S0[0] undriven or does not drive anything - clipped.
Signal N_1 undriven or does not drive anything - clipped.
Block nCASout.CN was optimized away.
Block ram2e_ufm/ufmefb/VCC was optimized away.
Block ram2e_ufm/ufmefb/GND was optimized away.

     

Embedded Functional Block Connection Summary
--------------------------------------------

   Desired WISHBONE clock frequency: 14.4 MHz
   Clock source:                     C14M_c
   Reset source:                     ram2e_ufm/wb_rst
   Functions mode:
      I2C #1 (Primary) Function:     DISABLED

                                    Page 6




Design:  RAM2E                                         Date:  12/28/23  23:23:28

Embedded Functional Block Connection Summary (cont)
---------------------------------------------------
      I2C #2 (Secondary) Function:   DISABLED
      SPI Function:                  DISABLED
      Timer/Counter Function:        DISABLED
      Timer/Counter Mode:            WB
      UFM Connection:                ENABLED
      PLL0 Connection:               DISABLED
      PLL1 Connection:               DISABLED
   I2C Function Summary:
   --------------------
      None
   SPI Function Summary:
   --------------------
      None
   Timer/Counter Function Summary:
   ------------------------------
      None
   UFM Function Summary:
   --------------------
      UFM Utilization:        General Purpose Flash Memory
      Initialized UFM Pages:  1 Pages (1*128 Bits)
      Available General
      Purpose Flash Memory:   191 Pages (191*128 Bits)

           EBR Blocks with Unique
      Initialization Data:    0

           WID		EBR Instance
      ---		------------


ASIC Components
---------------

Instance Name: ram2e_ufm/ufmefb/EFBInst_0
         Type: EFB

Run Time and Memory Usage
-------------------------

   Total CPU Time: 0 secs  
   Total REAL Time: 0 secs  
   Peak Memory Usage: 59 MB
        














                                    Page 7


Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
     Copyright (c) 1995 AT&T Corp.   All rights reserved.
     Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
     Copyright (c) 2001 Agere Systems   All rights reserved.
     Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights
     reserved.
