Loading design for application iotiming from file ram2gs_lcmxo256c_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO256C
Package:     TQFP100
Performance: 4
Package Status:                     Final          Version 1.19.
Performance Hardware Data Status: Version 1.124.
Loading design for application iotiming from file ram2gs_lcmxo256c_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO256C
Package:     TQFP100
Performance: 5
Package Status:                     Final          Version 1.19.
Performance Hardware Data Status: Version 1.124.
Loading design for application iotiming from file ram2gs_lcmxo256c_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO256C
Package:     TQFP100
Performance: M
Package Status:                     Final          Version 1.19.
Performance Hardware Data Status: Version 1.124.
// Design: RAM2GS
// Package: TQFP100
// ncd File: ram2gs_lcmxo256c_impl1.ncd
// Version: Diamond (64-bit) 3.12.1.454
// Written on Sat Jan 06 06:25:13 2024
// M: Minimum Performance Grade
// iotiming RAM2GS_LCMXO256C_impl1.ncd RAM2GS_LCMXO256C_impl1.prf -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO256C/promote.xml

I/O Timing Report (All units are in ns)

Worst Case Results across Performance Grades (M, 5, 4, 3):

// Input Setup and Hold Times

Port    Clock Edge  Setup Performance_Grade  Hold Performance_Grade
----------------------------------------------------------------------
CROW[0] nCRAS F    -0.006      M       1.907     3
CROW[1] nCRAS F    -0.006      M       1.907     3
Din[0]  PHI2  F     4.304      3       2.935     3
Din[0]  nCCAS F     0.567      3       0.723     3
Din[1]  PHI2  F     4.920      3       3.034     3
Din[1]  nCCAS F     0.414      3       0.851     3
Din[2]  PHI2  F     3.171      3       3.327     3
Din[2]  nCCAS F     0.909      3       0.432     3
Din[3]  PHI2  F     4.332      3       2.525     3
Din[3]  nCCAS F     0.038      3       1.155     3
Din[4]  PHI2  F     5.624      3       2.635     3
Din[4]  nCCAS F     1.448      3      -0.041     M
Din[5]  PHI2  F     4.126      3       2.124     3
Din[5]  nCCAS F     1.046      3       0.159     3
Din[6]  PHI2  F     5.565      3       2.394     3
Din[6]  nCCAS F     0.563      3       0.729     3
Din[7]  PHI2  F     5.293      3       1.654     3
Din[7]  nCCAS F     0.719      3       0.583     3
MAin[0] PHI2  F     8.072      3      -0.164     M
MAin[0] nCRAS F    -0.128      M       2.331     3
MAin[1] PHI2  F     7.487      3      -0.178     M
MAin[1] nCRAS F    -0.129      M       2.331     3
MAin[2] PHI2  F     6.793      3      -0.034     M
MAin[2] nCRAS F    -0.129      M       2.331     3
MAin[3] PHI2  F     7.235      3      -0.226     M
MAin[3] nCRAS F    -0.035      M       2.023     3
MAin[4] PHI2  F     7.305      3      -0.207     M
MAin[4] nCRAS F     0.428      3       1.517     3
MAin[5] PHI2  F     7.672      3      -0.236     M
MAin[5] nCRAS F    -0.037      M       2.028     3
MAin[6] PHI2  F     9.015      3      -0.710     M
MAin[6] nCRAS F    -0.003      M       1.896     3
MAin[7] PHI2  F     7.764      3      -0.441     M
MAin[7] nCRAS F    -0.126      M       2.324     3
MAin[8] nCRAS F    -0.038      M       2.034     3
MAin[9] nCRAS F     0.206      3       1.728     3
PHI2    RCLK  R     2.769      3      -0.274     M
UFMSDO  RCLK  R     1.753      3      -0.052     M
nCCAS   RCLK  R     1.935      3      -0.108     M
nCCAS   nCRAS F     0.843      3       1.179     3
nCRAS   RCLK  R     1.093      3       0.277     3
nFWE    PHI2  F     4.435      3       0.640     3
nFWE    nCRAS F     1.163      3       0.894     3


// Clock to Output Delay

Port   Clock Edge  Max_Delay Performance_Grade  Min_Delay Performance_Grade
------------------------------------------------------------------------
LED    RCLK  R    15.407         3        4.713          M
LED    nCRAS F    17.685         3        5.215          M
RA[0]  RCLK  R    10.436         3        2.152          M
RA[0]  nCRAS F    11.488         3        2.330          M
RA[10] RCLK  R     8.093         3        1.668          M
RA[11] PHI2  R     9.420         3        1.925          M
RA[1]  RCLK  R    10.958         3        2.270          M
RA[1]  nCRAS F    12.371         3        2.529          M
RA[2]  RCLK  R    10.892         3        2.242          M
RA[2]  nCRAS F    11.786         3        2.402          M
RA[3]  RCLK  R    10.561         3        2.184          M
RA[3]  nCRAS F    12.541         3        2.560          M
RA[4]  RCLK  R    10.909         3        2.257          M
RA[4]  nCRAS F    12.060         3        2.456          M
RA[5]  RCLK  R     9.970         3        2.057          M
RA[5]  nCRAS F    12.271         3        2.508          M
RA[6]  RCLK  R     9.222         3        1.920          M
RA[6]  nCRAS F    10.844         3        2.210          M
RA[7]  RCLK  R     9.613         3        1.981          M
RA[7]  nCRAS F    11.686         3        2.379          M
RA[8]  RCLK  R     9.617         3        1.982          M
RA[8]  nCRAS F    11.487         3        2.339          M
RA[9]  RCLK  R     9.762         3        2.016          M
RA[9]  nCRAS F    11.488         3        2.337          M
RBA[0] nCRAS F     8.925         3        1.828          M
RBA[1] nCRAS F    10.608         3        2.153          M
RCKE   RCLK  R     7.609         3        1.570          M
RDQMH  RCLK  R    10.915         3        2.299          M
RDQML  RCLK  R    11.554         3        2.433          M
RD[0]  nCCAS F     8.539         3        1.899          M
RD[1]  nCCAS F     9.248         3        2.027          M
RD[2]  nCCAS F     9.706         3        2.118          M
RD[3]  nCCAS F     8.539         3        1.899          M
RD[4]  nCCAS F     9.228         3        2.015          M
RD[5]  nCCAS F     8.772         3        1.924          M
RD[6]  nCCAS F     8.539         3        1.899          M
RD[7]  nCCAS F     9.706         3        2.118          M
UFMCLK RCLK  R     8.007         3        1.714          M
UFMSDI RCLK  R     8.007         3        1.714          M
nRCAS  RCLK  R     8.120         3        1.681          M
nRCS   RCLK  R     6.854         3        1.431          M
nRRAS  RCLK  R     8.089         3        1.669          M
nRWE   RCLK  R     6.854         3        1.431          M
nUFMCS RCLK  R     8.732         3        1.846          M
WARNING: you must also run trce with hold speed: 3
WARNING: you must also run trce with setup speed: M
