PAD Specification File
***************************

PART TYPE:        LCMXO640C
Performance Grade:      3
PACKAGE:          TQFP100
Package Status:                     Final          Version 1.17

Sat Jan 06 06:25:19 2024

Pinout by Port Name:
+-----------+----------+---------------+-------+----------------------------------+
| Port Name | Pin/Bank | Buffer Type   | Site  | Properties                       |
+-----------+----------+---------------+-------+----------------------------------+
| CROW[0]   | 32/2     | LVCMOS33_IN   | PB4C  | SLEW:FAST                        |
| CROW[1]   | 34/2     | LVCMOS33_IN   | PB4E  | SLEW:FAST                        |
| Din[0]    | 21/3     | LVCMOS33_IN   | PL10C | SLEW:FAST                        |
| Din[1]    | 15/3     | LVCMOS33_IN   | PL7B  | SLEW:FAST                        |
| Din[2]    | 14/3     | LVCMOS33_IN   | PL5B  | SLEW:FAST                        |
| Din[3]    | 16/3     | LVCMOS33_IN   | PL8C  | SLEW:FAST                        |
| Din[4]    | 18/3     | LVCMOS33_IN   | PL9A  | SLEW:FAST                        |
| Din[5]    | 17/3     | LVCMOS33_IN   | PL8D  | SLEW:FAST                        |
| Din[6]    | 20/3     | LVCMOS33_IN   | PL10A | SLEW:FAST                        |
| Din[7]    | 19/3     | LVCMOS33_IN   | PL9C  | SLEW:FAST                        |
| Dout[0]   | 1/3      | LVCMOS33_OUT  | PL2A  | DRIVE:4mA SLEW:FAST              |
| Dout[1]   | 7/3      | LVCMOS33_OUT  | PL3C  | DRIVE:4mA SLEW:FAST              |
| Dout[2]   | 8/3      | LVCMOS33_OUT  | PL3D  | DRIVE:4mA SLEW:FAST              |
| Dout[3]   | 6/3      | LVCMOS33_OUT  | PL3B  | DRIVE:4mA SLEW:FAST              |
| Dout[4]   | 4/3      | LVCMOS33_OUT  | PL2D  | DRIVE:4mA SLEW:FAST              |
| Dout[5]   | 5/3      | LVCMOS33_OUT  | PL3A  | DRIVE:4mA SLEW:FAST              |
| Dout[6]   | 2/3      | LVCMOS33_OUT  | PL2C  | DRIVE:4mA SLEW:FAST              |
| Dout[7]   | 3/3      | LVCMOS33_OUT  | PL2B  | DRIVE:4mA SLEW:FAST              |
| LED       | 57/1     | LVCMOS33_OUT  | PR10B | DRIVE:14mA SLEW:SLOW             |
| MAin[0]   | 23/3     | LVCMOS33_IN   | PL11C | SLEW:FAST                        |
| MAin[1]   | 38/2     | LVCMOS33_IN   | PB6B  | SLEW:FAST                        |
| MAin[2]   | 37/2     | LVCMOS33_IN   | PB5D  | SLEW:FAST                        |
| MAin[3]   | 47/2     | LVCMOS33_IN   | PB9C  | SLEW:FAST                        |
| MAin[4]   | 46/2     | LVCMOS33_IN   | PB9A  | SLEW:FAST                        |
| MAin[5]   | 45/2     | LVCMOS33_IN   | PB8D  | SLEW:FAST                        |
| MAin[6]   | 49/2     | LVCMOS33_IN   | PB9D  | SLEW:FAST                        |
| MAin[7]   | 44/2     | LVCMOS33_IN   | PB8C  | SLEW:FAST                        |
| MAin[8]   | 50/2     | LVCMOS33_IN   | PB9F  | SLEW:FAST                        |
| MAin[9]   | 51/1     | LVCMOS33_IN   | PR11D | SLEW:FAST                        |
| PHI2      | 39/2     | LVCMOS33_IN   | PB6C  | SLEW:FAST                        |
| RA[0]     | 98/0     | LVCMOS33_OUT  | PT2B  | DRIVE:4mA SLEW:SLOW              |
| RA[10]    | 87/0     | LVCMOS33_OUT  | PT5A  | DRIVE:4mA SLEW:SLOW              |
| RA[11]    | 79/0     | LVCMOS33_OUT  | PT9A  | DRIVE:4mA SLEW:SLOW              |
| RA[1]     | 89/0     | LVCMOS33_OUT  | PT4F  | DRIVE:4mA SLEW:SLOW              |
| RA[2]     | 94/0     | LVCMOS33_OUT  | PT3B  | DRIVE:4mA SLEW:SLOW              |
| RA[3]     | 97/0     | LVCMOS33_OUT  | PT2E  | DRIVE:4mA SLEW:SLOW              |
| RA[4]     | 99/0     | LVCMOS33_OUT  | PT2C  | DRIVE:4mA SLEW:SLOW              |
| RA[5]     | 95/0     | LVCMOS33_OUT  | PT3A  | DRIVE:4mA SLEW:SLOW              |
| RA[6]     | 91/0     | LVCMOS33_OUT  | PT3F  | DRIVE:4mA SLEW:SLOW              |
| RA[7]     | 100/0    | LVCMOS33_OUT  | PT2A  | DRIVE:4mA SLEW:SLOW              |
| RA[8]     | 96/0     | LVCMOS33_OUT  | PT2F  | DRIVE:4mA SLEW:SLOW              |
| RA[9]     | 85/0     | LVCMOS33_OUT  | PT6B  | DRIVE:4mA SLEW:SLOW              |
| RBA[0]    | 63/1     | LVCMOS33_OUT  | PR7B  | DRIVE:4mA SLEW:SLOW              |
| RBA[1]    | 83/0     | LVCMOS33_OUT  | PT7A  | DRIVE:4mA SLEW:SLOW              |
| RCKE      | 82/0     | LVCMOS33_OUT  | PT7E  | DRIVE:4mA SLEW:SLOW              |
| RCLK      | 86/0     | LVCMOS33_IN   | PT5B  | SLEW:FAST                        |
| RDQMH     | 76/0     | LVCMOS33_OUT  | PT9F  | DRIVE:4mA SLEW:SLOW              |
| RDQML     | 61/1     | LVCMOS33_OUT  | PR9B  | DRIVE:4mA SLEW:SLOW              |
| RD[0]     | 64/1     | LVCMOS33_BIDI | PR6C  | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[1]     | 65/1     | LVCMOS33_BIDI | PR6B  | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[2]     | 66/1     | LVCMOS33_BIDI | PR5D  | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[3]     | 67/1     | LVCMOS33_BIDI | PR5B  | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[4]     | 68/1     | LVCMOS33_BIDI | PR4D  | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[5]     | 69/1     | LVCMOS33_BIDI | PR4B  | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[6]     | 70/1     | LVCMOS33_BIDI | PR3D  | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| RD[7]     | 71/1     | LVCMOS33_BIDI | PR3B  | DRIVE:4mA SLEW:SLOW PULL:KEEPER  |
| UFMCLK    | 58/1     | LVCMOS33_OUT  | PR10A | DRIVE:4mA SLEW:SLOW              |
| UFMSDI    | 56/1     | LVCMOS33_OUT  | PR10C | DRIVE:4mA SLEW:SLOW              |
| UFMSDO    | 55/1     | LVCMOS33_IN   | PR10D | SLEW:FAST                        |
| nCCAS     | 27/2     | LVCMOS33_IN   | PB2C  | SLEW:FAST                        |
| nCRAS     | 43/2     | LVCMOS33_IN   | PB8B  | SLEW:FAST                        |
| nFWE      | 22/3     | LVCMOS33_IN   | PL11A | SLEW:FAST                        |
| nRCAS     | 78/0     | LVCMOS33_OUT  | PT9C  | DRIVE:4mA SLEW:SLOW              |
| nRCS      | 77/0     | LVCMOS33_OUT  | PT9E  | DRIVE:4mA SLEW:SLOW              |
| nRRAS     | 73/1     | LVCMOS33_OUT  | PR2B  | DRIVE:4mA SLEW:SLOW              |
| nRWE      | 72/1     | LVCMOS33_OUT  | PR2D  | DRIVE:4mA SLEW:SLOW              |
| nUFMCS    | 53/1     | LVCMOS33_OUT  | PR11C | DRIVE:4mA SLEW:SLOW              |
+-----------+----------+---------------+-------+----------------------------------+

Vccio by Bank:
+------+-------+
| Bank | Vccio |
+------+-------+
| 0    | 3.3V  |
| 1    | 3.3V  |
| 2    |       |
| 3    | 3.3V  |
+------+-------+

Vref by Bank:
+------+-----+-----------------+---------+
| Vref | Pin | Bank # / Vref # | Load(s) |
+------+-----+-----------------+---------+
+------+-----+-----------------+---------+

Pinout by Pin Number:
+----------+---------------------+------------+---------------+-------+---------------+
| Pin/Bank | Pin Info            | Preference | Buffer Type   | Site  | Dual Function |
+----------+---------------------+------------+---------------+-------+---------------+
| 1/3      | Dout[0]             | LOCATED    | LVCMOS33_OUT  | PL2A  |               |
| 2/3      | Dout[6]             | LOCATED    | LVCMOS33_OUT  | PL2C  |               |
| 3/3      | Dout[7]             | LOCATED    | LVCMOS33_OUT  | PL2B  |               |
| 4/3      | Dout[4]             | LOCATED    | LVCMOS33_OUT  | PL2D  |               |
| 5/3      | Dout[5]             | LOCATED    | LVCMOS33_OUT  | PL3A  |               |
| 6/3      | Dout[3]             | LOCATED    | LVCMOS33_OUT  | PL3B  |               |
| 7/3      | Dout[1]             | LOCATED    | LVCMOS33_OUT  | PL3C  |               |
| 8/3      | Dout[2]             | LOCATED    | LVCMOS33_OUT  | PL3D  |               |
| 9/3      |     unused, PULL:UP |            |               | PL4A  |               |
| 11/3     |     unused, PULL:UP |            |               | PL4C  |               |
| 13/3     |     unused, PULL:UP |            |               | PL4D  |               |
| 14/3     | Din[2]              | LOCATED    | LVCMOS33_IN   | PL5B  | GSR_PADN      |
| 15/3     | Din[1]              | LOCATED    | LVCMOS33_IN   | PL7B  |               |
| 16/3     | Din[3]              | LOCATED    | LVCMOS33_IN   | PL8C  | TSALLPAD      |
| 17/3     | Din[5]              | LOCATED    | LVCMOS33_IN   | PL8D  |               |
| 18/3     | Din[4]              | LOCATED    | LVCMOS33_IN   | PL9A  |               |
| 19/3     | Din[7]              | LOCATED    | LVCMOS33_IN   | PL9C  |               |
| 20/3     | Din[6]              | LOCATED    | LVCMOS33_IN   | PL10A |               |
| 21/3     | Din[0]              | LOCATED    | LVCMOS33_IN   | PL10C |               |
| 22/3     | nFWE                | LOCATED    | LVCMOS33_IN   | PL11A |               |
| 23/3     | MAin[0]             | LOCATED    | LVCMOS33_IN   | PL11C |               |
| 27/2     | nCCAS               | LOCATED    | LVCMOS33_IN   | PB2C  |               |
| 32/2     | CROW[0]             | LOCATED    | LVCMOS33_IN   | PB4C  |               |
| 34/2     | CROW[1]             | LOCATED    | LVCMOS33_IN   | PB4E  |               |
| 36/2     |     unused, PULL:UP |            |               | PB5B  | PCLKT2_1      |
| 37/2     | MAin[2]             | LOCATED    | LVCMOS33_IN   | PB5D  |               |
| 38/2     | MAin[1]             | LOCATED    | LVCMOS33_IN   | PB6B  | PCLKT2_0      |
| 39/2     | PHI2                | LOCATED    | LVCMOS33_IN   | PB6C  |               |
| 43/2     | nCRAS               | LOCATED    | LVCMOS33_IN   | PB8B  |               |
| 44/2     | MAin[7]             | LOCATED    | LVCMOS33_IN   | PB8C  |               |
| 45/2     | MAin[5]             | LOCATED    | LVCMOS33_IN   | PB8D  |               |
| 46/2     | MAin[4]             | LOCATED    | LVCMOS33_IN   | PB9A  |               |
| 47/2     | MAin[3]             | LOCATED    | LVCMOS33_IN   | PB9C  |               |
| 49/2     | MAin[6]             | LOCATED    | LVCMOS33_IN   | PB9D  |               |
| 50/2     | MAin[8]             | LOCATED    | LVCMOS33_IN   | PB9F  |               |
| 51/1     | MAin[9]             | LOCATED    | LVCMOS33_IN   | PR11D |               |
| 52/1     |     unused, PULL:UP |            |               | PR11B |               |
| 53/1     | nUFMCS              | LOCATED    | LVCMOS33_OUT  | PR11C |               |
| 54/1     |     unused, PULL:UP |            |               | PR11A |               |
| 55/1     | UFMSDO              | LOCATED    | LVCMOS33_IN   | PR10D |               |
| 56/1     | UFMSDI              | LOCATED    | LVCMOS33_OUT  | PR10C |               |
| 57/1     | LED                 | LOCATED    | LVCMOS33_OUT  | PR10B |               |
| 58/1     | UFMCLK              | LOCATED    | LVCMOS33_OUT  | PR10A |               |
| 59/1     |     unused, PULL:UP |            |               | PR9D  |               |
| 61/1     | RDQML               | LOCATED    | LVCMOS33_OUT  | PR9B  |               |
| 63/1     | RBA[0]              | LOCATED    | LVCMOS33_OUT  | PR7B  |               |
| 64/1     | RD[0]               | LOCATED    | LVCMOS33_BIDI | PR6C  |               |
| 65/1     | RD[1]               | LOCATED    | LVCMOS33_BIDI | PR6B  |               |
| 66/1     | RD[2]               | LOCATED    | LVCMOS33_BIDI | PR5D  |               |
| 67/1     | RD[3]               | LOCATED    | LVCMOS33_BIDI | PR5B  |               |
| 68/1     | RD[4]               | LOCATED    | LVCMOS33_BIDI | PR4D  |               |
| 69/1     | RD[5]               | LOCATED    | LVCMOS33_BIDI | PR4B  |               |
| 70/1     | RD[6]               | LOCATED    | LVCMOS33_BIDI | PR3D  |               |
| 71/1     | RD[7]               | LOCATED    | LVCMOS33_BIDI | PR3B  |               |
| 72/1     | nRWE                | LOCATED    | LVCMOS33_OUT  | PR2D  |               |
| 73/1     | nRRAS               | LOCATED    | LVCMOS33_OUT  | PR2B  |               |
| 76/0     | RDQMH               | LOCATED    | LVCMOS33_OUT  | PT9F  |               |
| 77/0     | nRCS                | LOCATED    | LVCMOS33_OUT  | PT9E  |               |
| 78/0     | nRCAS               | LOCATED    | LVCMOS33_OUT  | PT9C  |               |
| 79/0     | RA[11]              | LOCATED    | LVCMOS33_OUT  | PT9A  |               |
| 82/0     | RCKE                | LOCATED    | LVCMOS33_OUT  | PT7E  | D7            |
| 83/0     | RBA[1]              | LOCATED    | LVCMOS33_OUT  | PT7A  | D6            |
| 85/0     | RA[9]               | LOCATED    | LVCMOS33_OUT  | PT6B  | PCLKT0_1      |
| 86/0     | RCLK                | LOCATED    | LVCMOS33_IN   | PT5B  | PCLKT0_0      |
| 87/0     | RA[10]              | LOCATED    | LVCMOS33_OUT  | PT5A  |               |
| 89/0     | RA[1]               | LOCATED    | LVCMOS33_OUT  | PT4F  |               |
| 91/0     | RA[6]               | LOCATED    | LVCMOS33_OUT  | PT3F  | D3            |
| 94/0     | RA[2]               | LOCATED    | LVCMOS33_OUT  | PT3B  |               |
| 95/0     | RA[5]               | LOCATED    | LVCMOS33_OUT  | PT3A  |               |
| 96/0     | RA[8]               | LOCATED    | LVCMOS33_OUT  | PT2F  | D2            |
| 97/0     | RA[3]               | LOCATED    | LVCMOS33_OUT  | PT2E  |               |
| 98/0     | RA[0]               | LOCATED    | LVCMOS33_OUT  | PT2B  | D1            |
| 99/0     | RA[4]               | LOCATED    | LVCMOS33_OUT  | PT2C  |               |
| 100/0    | RA[7]               | LOCATED    | LVCMOS33_OUT  | PT2A  |               |
| PB2A/2   |     unused, PULL:UP |            |               | PB2A  |               |
| PB2B/2   |     unused, PULL:UP |            |               | PB2B  |               |
| PB2D/2   |     unused, PULL:UP |            |               | PB2D  |               |
| PB3A/2   |     unused, PULL:UP |            |               | PB3A  |               |
| PB3B/2   |     unused, PULL:UP |            |               | PB3B  |               |
| PB3C/2   |     unused, PULL:UP |            |               | PB3C  |               |
| PB3D/2   |     unused, PULL:UP |            |               | PB3D  |               |
| PB4A/2   |     unused, PULL:UP |            |               | PB4A  |               |
| PB4B/2   |     unused, PULL:UP |            |               | PB4B  |               |
| PB4D/2   |     unused, PULL:UP |            |               | PB4D  |               |
| PB4F/2   |     unused, PULL:UP |            |               | PB4F  |               |
| PB5A/2   |     unused, PULL:UP |            |               | PB5A  |               |
| PB5C/2   |     unused, PULL:UP |            |               | PB5C  |               |
| PB6A/2   |     unused, PULL:UP |            |               | PB6A  |               |
| PB6D/2   |     unused, PULL:UP |            |               | PB6D  |               |
| PB7A/2   |     unused, PULL:UP |            |               | PB7A  |               |
| PB7B/2   |     unused, PULL:UP |            |               | PB7B  |               |
| PB7C/2   |     unused, PULL:UP |            |               | PB7C  |               |
| PB7D/2   |     unused, PULL:UP |            |               | PB7D  |               |
| PB7E/2   |     unused, PULL:UP |            |               | PB7E  |               |
| PB7F/2   |     unused, PULL:UP |            |               | PB7F  |               |
| PB8A/2   |     unused, PULL:UP |            |               | PB8A  |               |
| PB9B/2   |     unused, PULL:UP |            |               | PB9B  |               |
| PB9E/0   |     unused, PULL:UP |            |               | PB9E  |               |
| PL4B/3   |     unused, PULL:UP |            |               | PL4B  |               |
| PL5A/3   |     unused, PULL:UP |            |               | PL5A  |               |
| PL5C/3   |     unused, PULL:UP |            |               | PL5C  |               |
| PL5D/3   |     unused, PULL:UP |            |               | PL5D  |               |
| PL6A/3   |     unused, PULL:UP |            |               | PL6A  |               |
| PL6B/3   |     unused, PULL:UP |            |               | PL6B  |               |
| PL6C/3   |     unused, PULL:UP |            |               | PL6C  |               |
| PL6D/3   |     unused, PULL:UP |            |               | PL6D  |               |
| PL7A/3   |     unused, PULL:UP |            |               | PL7A  |               |
| PL7C/3   |     unused, PULL:UP |            |               | PL7C  |               |
| PL7D/3   |     unused, PULL:UP |            |               | PL7D  |               |
| PL8A/3   |     unused, PULL:UP |            |               | PL8A  |               |
| PL8B/3   |     unused, PULL:UP |            |               | PL8B  |               |
| PL9B/3   |     unused, PULL:UP |            |               | PL9B  |               |
| PL9D/3   |     unused, PULL:UP |            |               | PL9D  |               |
| PL10B/3  |     unused, PULL:UP |            |               | PL10B |               |
| PL10D/3  |     unused, PULL:UP |            |               | PL10D |               |
| PL11B/3  |     unused, PULL:UP |            |               | PL11B |               |
| PL11D/3  |     unused, PULL:UP |            |               | PL11D |               |
| PR2A/1   |     unused, PULL:UP |            |               | PR2A  |               |
| PR2C/1   |     unused, PULL:UP |            |               | PR2C  |               |
| PR3A/1   |     unused, PULL:UP |            |               | PR3A  |               |
| PR3C/1   |     unused, PULL:UP |            |               | PR3C  |               |
| PR4A/1   |     unused, PULL:UP |            |               | PR4A  |               |
| PR4C/1   |     unused, PULL:UP |            |               | PR4C  |               |
| PR5A/1   |     unused, PULL:UP |            |               | PR5A  |               |
| PR5C/1   |     unused, PULL:UP |            |               | PR5C  |               |
| PR6A/1   |     unused, PULL:UP |            |               | PR6A  |               |
| PR6D/1   |     unused, PULL:UP |            |               | PR6D  |               |
| PR7A/1   |     unused, PULL:UP |            |               | PR7A  |               |
| PR7C/1   |     unused, PULL:UP |            |               | PR7C  |               |
| PR7D/1   |     unused, PULL:UP |            |               | PR7D  |               |
| PR8A/1   |     unused, PULL:UP |            |               | PR8A  |               |
| PR8B/1   |     unused, PULL:UP |            |               | PR8B  |               |
| PR8C/1   |     unused, PULL:UP |            |               | PR8C  |               |
| PR8D/1   |     unused, PULL:UP |            |               | PR8D  |               |
| PR9A/1   |     unused, PULL:UP |            |               | PR9A  |               |
| PR9C/1   |     unused, PULL:UP |            |               | PR9C  |               |
| PT2D/0   |     unused, PULL:UP |            |               | PT2D  |               |
| PT3C/0   |     unused, PULL:UP |            |               | PT3C  |               |
| PT3D/0   |     unused, PULL:UP |            |               | PT3D  |               |
| PT3E/0   |     unused, PULL:UP |            |               | PT3E  |               |
| PT4A/0   |     unused, PULL:UP |            |               | PT4A  |               |
| PT4B/0   |     unused, PULL:UP |            |               | PT4B  |               |
| PT4C/0   |     unused, PULL:UP |            |               | PT4C  |               |
| PT4D/0   |     unused, PULL:UP |            |               | PT4D  |               |
| PT4E/0   |     unused, PULL:UP |            |               | PT4E  |               |
| PT5C/0   |     unused, PULL:UP |            |               | PT5C  |               |
| PT5D/0   |     unused, PULL:UP |            |               | PT5D  |               |
| PT6A/0   |     unused, PULL:UP |            |               | PT6A  |               |
| PT6C/0   |     unused, PULL:UP |            |               | PT6C  |               |
| PT6D/0   |     unused, PULL:UP |            |               | PT6D  |               |
| PT7B/0   |     unused, PULL:UP |            |               | PT7B  |               |
| PT7C/0   |     unused, PULL:UP |            |               | PT7C  |               |
| PT7D/0   |     unused, PULL:UP |            |               | PT7D  |               |
| PT7F/0   |     unused, PULL:UP |            |               | PT7F  |               |
| PT8A/0   |     unused, PULL:UP |            |               | PT8A  |               |
| PT8B/0   |     unused, PULL:UP |            |               | PT8B  |               |
| PT8C/0   |     unused, PULL:UP |            |               | PT8C  |               |
| PT8D/0   |     unused, PULL:UP |            |               | PT8D  |               |
| PT9B/0   |     unused, PULL:UP |            |               | PT9B  |               |
| PT9D/0   |     unused, PULL:UP |            |               | PT9D  |               |
| TCK/2    |                     |            |               | TCK   | TCK           |
| TDI/2    |                     |            |               | TDI   | TDID0         |
| TDO/2    |                     |            |               | TDO   | TDO           |
| TMS/2    |                     |            |               | TMS   | TMS           |
+----------+---------------------+------------+---------------+-------+---------------+


List of All Pins' Locate Preferences Based on Final Placement After PAR 
to Help Users Lock Down ALL the Pins Easily (by Simply Copy & Paste): 

LOCATE  COMP  "CROW[0]"  SITE  "32";
LOCATE  COMP  "CROW[1]"  SITE  "34";
LOCATE  COMP  "Din[0]"  SITE  "21";
LOCATE  COMP  "Din[1]"  SITE  "15";
LOCATE  COMP  "Din[2]"  SITE  "14";
LOCATE  COMP  "Din[3]"  SITE  "16";
LOCATE  COMP  "Din[4]"  SITE  "18";
LOCATE  COMP  "Din[5]"  SITE  "17";
LOCATE  COMP  "Din[6]"  SITE  "20";
LOCATE  COMP  "Din[7]"  SITE  "19";
LOCATE  COMP  "Dout[0]"  SITE  "1";
LOCATE  COMP  "Dout[1]"  SITE  "7";
LOCATE  COMP  "Dout[2]"  SITE  "8";
LOCATE  COMP  "Dout[3]"  SITE  "6";
LOCATE  COMP  "Dout[4]"  SITE  "4";
LOCATE  COMP  "Dout[5]"  SITE  "5";
LOCATE  COMP  "Dout[6]"  SITE  "2";
LOCATE  COMP  "Dout[7]"  SITE  "3";
LOCATE  COMP  "LED"  SITE  "57";
LOCATE  COMP  "MAin[0]"  SITE  "23";
LOCATE  COMP  "MAin[1]"  SITE  "38";
LOCATE  COMP  "MAin[2]"  SITE  "37";
LOCATE  COMP  "MAin[3]"  SITE  "47";
LOCATE  COMP  "MAin[4]"  SITE  "46";
LOCATE  COMP  "MAin[5]"  SITE  "45";
LOCATE  COMP  "MAin[6]"  SITE  "49";
LOCATE  COMP  "MAin[7]"  SITE  "44";
LOCATE  COMP  "MAin[8]"  SITE  "50";
LOCATE  COMP  "MAin[9]"  SITE  "51";
LOCATE  COMP  "PHI2"  SITE  "39";
LOCATE  COMP  "RA[0]"  SITE  "98";
LOCATE  COMP  "RA[10]"  SITE  "87";
LOCATE  COMP  "RA[11]"  SITE  "79";
LOCATE  COMP  "RA[1]"  SITE  "89";
LOCATE  COMP  "RA[2]"  SITE  "94";
LOCATE  COMP  "RA[3]"  SITE  "97";
LOCATE  COMP  "RA[4]"  SITE  "99";
LOCATE  COMP  "RA[5]"  SITE  "95";
LOCATE  COMP  "RA[6]"  SITE  "91";
LOCATE  COMP  "RA[7]"  SITE  "100";
LOCATE  COMP  "RA[8]"  SITE  "96";
LOCATE  COMP  "RA[9]"  SITE  "85";
LOCATE  COMP  "RBA[0]"  SITE  "63";
LOCATE  COMP  "RBA[1]"  SITE  "83";
LOCATE  COMP  "RCKE"  SITE  "82";
LOCATE  COMP  "RCLK"  SITE  "86";
LOCATE  COMP  "RDQMH"  SITE  "76";
LOCATE  COMP  "RDQML"  SITE  "61";
LOCATE  COMP  "RD[0]"  SITE  "64";
LOCATE  COMP  "RD[1]"  SITE  "65";
LOCATE  COMP  "RD[2]"  SITE  "66";
LOCATE  COMP  "RD[3]"  SITE  "67";
LOCATE  COMP  "RD[4]"  SITE  "68";
LOCATE  COMP  "RD[5]"  SITE  "69";
LOCATE  COMP  "RD[6]"  SITE  "70";
LOCATE  COMP  "RD[7]"  SITE  "71";
LOCATE  COMP  "UFMCLK"  SITE  "58";
LOCATE  COMP  "UFMSDI"  SITE  "56";
LOCATE  COMP  "UFMSDO"  SITE  "55";
LOCATE  COMP  "nCCAS"  SITE  "27";
LOCATE  COMP  "nCRAS"  SITE  "43";
LOCATE  COMP  "nFWE"  SITE  "22";
LOCATE  COMP  "nRCAS"  SITE  "78";
LOCATE  COMP  "nRCS"  SITE  "77";
LOCATE  COMP  "nRRAS"  SITE  "73";
LOCATE  COMP  "nRWE"  SITE  "72";
LOCATE  COMP  "nUFMCS"  SITE  "53";





PAR: Place And Route Diamond (64-bit) 3.12.1.454.
Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
Copyright (c) 1995 AT&T Corp.   All rights reserved.
Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
Copyright (c) 2001 Agere Systems   All rights reserved.
Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.
Sat Jan 06 06:25:19 2024

