Loading design for application iotiming from file ram2gs_lcmxo640c_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO640C
Package:     TQFP100
Performance: 4
Package Status:                     Final          Version 1.17.
Performance Hardware Data Status: Version 1.124.
Loading design for application iotiming from file ram2gs_lcmxo640c_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO640C
Package:     TQFP100
Performance: 5
Package Status:                     Final          Version 1.17.
Performance Hardware Data Status: Version 1.124.
Loading design for application iotiming from file ram2gs_lcmxo640c_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO640C
Package:     TQFP100
Performance: M
Package Status:                     Final          Version 1.17.
Performance Hardware Data Status: Version 1.124.
// Design: RAM2GS
// Package: TQFP100
// ncd File: ram2gs_lcmxo640c_impl1.ncd
// Version: Diamond (64-bit) 3.12.1.454
// Written on Sat Jan 06 06:25:22 2024
// M: Minimum Performance Grade
// iotiming RAM2GS_LCMXO640C_impl1.ncd RAM2GS_LCMXO640C_impl1.prf -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO640C/promote.xml

I/O Timing Report (All units are in ns)

Worst Case Results across Performance Grades (M, 5, 4, 3):

// Input Setup and Hold Times

Port    Clock Edge  Setup Performance_Grade  Hold Performance_Grade
----------------------------------------------------------------------
CROW[0] nCRAS F    -0.112      M       2.651     3
CROW[1] nCRAS F    -0.021      M       2.351     3
Din[0]  PHI2  F     4.317      3       1.888     3
Din[0]  nCCAS F     1.401      3      -0.032     M
Din[1]  PHI2  F     6.362      3       2.174     3
Din[1]  nCCAS F     0.920      3       0.293     3
Din[2]  PHI2  F     4.582      3       1.108     3
Din[2]  nCCAS F     1.367      3      -0.025     M
Din[3]  PHI2  F     6.558      3       2.698     3
Din[3]  nCCAS F     0.619      3       0.544     3
Din[4]  PHI2  F     7.083      3       0.535     3
Din[4]  nCCAS F     0.558      3       0.857     3
Din[5]  PHI2  F     6.015      3       2.171     3
Din[5]  nCCAS F     0.035      3       1.300     3
Din[6]  PHI2  F     6.445      3       1.417     3
Din[6]  nCCAS F     1.089      3       0.272     3
Din[7]  PHI2  F     6.645      3       2.275     3
Din[7]  nCCAS F     0.961      3       0.396     3
MAin[0] PHI2  F     7.871      3      -0.129     M
MAin[0] nCRAS F    -0.325      M       3.376     3
MAin[1] PHI2  F     8.822      3      -0.149     M
MAin[1] nCRAS F    -0.467      M       3.889     3
MAin[2] PHI2  F     7.393      3       0.809     3
MAin[2] nCRAS F    -0.468      M       3.890     3
MAin[3] PHI2  F     8.567      3      -0.143     M
MAin[3] nCRAS F    -0.148      M       2.780     3
MAin[4] PHI2  F     9.168      3      -0.113     M
MAin[4] nCRAS F     0.492      3       1.836     3
MAin[5] PHI2  F     7.300      3       0.076     3
MAin[5] nCRAS F    -0.108      M       2.641     3
MAin[6] PHI2  F     8.643      3      -0.385     M
MAin[6] nCRAS F    -0.216      M       2.988     3
MAin[7] PHI2  F     7.923      3      -0.224     M
MAin[7] nCRAS F    -0.325      M       3.376     3
MAin[8] nCRAS F    -0.328      M       3.387     3
MAin[9] nCRAS F    -0.352      M       3.481     3
PHI2    RCLK  R     2.024      3      -0.115     M
UFMSDO  RCLK  R     2.286      3      -0.106     M
nCCAS   RCLK  R     3.326      3      -0.370     M
nCCAS   nCRAS F     0.813      3       1.646     3
nCRAS   RCLK  R     5.235      3      -0.614     M
nFWE    PHI2  F     5.814      3       0.503     3
nFWE    nCRAS F     0.183      3       2.096     3


// Clock to Output Delay

Port   Clock Edge  Max_Delay Performance_Grade  Min_Delay Performance_Grade
------------------------------------------------------------------------
LED    RCLK  R    16.515         3        4.482          M
LED    nCRAS F    17.585         3        5.197          M
RA[0]  RCLK  R    11.366         3        2.326          M
RA[0]  nCRAS F    13.548         3        2.745          M
RA[10] RCLK  R     6.926         3        1.431          M
RA[11] PHI2  R     9.183         3        1.867          M
RA[1]  RCLK  R     9.283         3        1.909          M
RA[1]  nCRAS F    12.064         3        2.463          M
RA[2]  RCLK  R    11.466         3        2.345          M
RA[2]  nCRAS F    13.609         3        2.759          M
RA[3]  RCLK  R    10.239         3        2.114          M
RA[3]  nCRAS F    12.115         3        2.471          M
RA[4]  RCLK  R    10.462         3        2.158          M
RA[4]  nCRAS F    12.460         3        2.541          M
RA[5]  RCLK  R    11.714         3        2.410          M
RA[5]  nCRAS F    14.027         3        2.856          M
RA[6]  RCLK  R    10.222         3        2.111          M
RA[6]  nCRAS F    12.507         3        2.549          M
RA[7]  RCLK  R    10.118         3        2.066          M
RA[7]  nCRAS F    13.612         3        2.768          M
RA[8]  RCLK  R    11.860         3        2.450          M
RA[8]  nCRAS F    13.529         3        2.745          M
RA[9]  RCLK  R    11.723         3        2.414          M
RA[9]  nCRAS F    14.189         3        2.884          M
RBA[0] nCRAS F    12.165         3        2.476          M
RBA[1] nCRAS F    10.690         3        2.155          M
RCKE   RCLK  R     6.926         3        1.431          M
RDQMH  RCLK  R    12.309         3        2.582          M
RDQML  RCLK  R    11.893         3        2.496          M
RD[0]  nCCAS F     8.780         3        1.926          M
RD[1]  nCCAS F     8.780         3        1.926          M
RD[2]  nCCAS F     8.071         3        1.798          M
RD[3]  nCCAS F     9.242         3        2.016          M
RD[4]  nCCAS F    11.095         3        2.414          M
RD[5]  nCCAS F    10.651         3        2.326          M
RD[6]  nCCAS F     8.532         3        1.897          M
RD[7]  nCCAS F     9.699         3        2.116          M
UFMCLK RCLK  R     8.800         3        1.847          M
UFMSDI RCLK  R     8.079         3        1.714          M
nRCAS  RCLK  R     6.926         3        1.431          M
nRCS   RCLK  R     6.926         3        1.431          M
nRRAS  RCLK  R     8.147         3        1.667          M
nRWE   RCLK  R     9.027         3        1.858          M
nUFMCS RCLK  R     9.262         3        1.937          M
WARNING: you must also run trce with hold speed: 3
WARNING: you must also run trce with setup speed: M
