Loading design for application iotiming from file ram2gs_lcmxo2_640hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-640HC
Package:     TQFP100
Performance: 5
Package Status:                     Final          Version 1.39.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2gs_lcmxo2_640hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-640HC
Package:     TQFP100
Performance: 6
Package Status:                     Final          Version 1.39.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2gs_lcmxo2_640hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-640HC
Package:     TQFP100
Performance: M
Package Status:                     Final          Version 1.39.
Performance Hardware Data Status:   Final          Version 34.4.
// Design: RAM2GS
// Package: TQFP100
// ncd File: ram2gs_lcmxo2_640hc_impl1.ncd
// Version: Diamond (64-bit) 3.12.1.454
// Written on Sat Nov 18 02:06:14 2023
// M: Minimum Performance Grade
// iotiming RAM2GS_LCMXO2_640HC_impl1.ncd RAM2GS_LCMXO2_640HC_impl1.prf -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO2-640HC/promote.xml

I/O Timing Report (All units are in ns)

Worst Case Results across Performance Grades (M, 6, 5, 4):

// Input Setup and Hold Times

Port    Clock Edge  Setup Performance_Grade  Hold Performance_Grade
----------------------------------------------------------------------
CROW[0] nCRAS F     2.058      4      -0.092     M
CROW[1] nCRAS F     2.269      4      -0.117     M
Din[0]  PHI2  F     7.415      4       3.636     4
Din[0]  nCCAS F     2.760      4      -0.330     M
Din[1]  PHI2  F     6.384      4       3.516     4
Din[1]  nCCAS F     1.112      4       0.128     4
Din[2]  PHI2  F     6.717      4       3.516     4
Din[2]  nCCAS F     0.113      4       0.982     4
Din[3]  PHI2  F     5.806      4       3.516     4
Din[3]  nCCAS F     1.105      4       0.134     4
Din[4]  PHI2  F     6.853      4       3.516     4
Din[4]  nCCAS F     1.538      4      -0.010     M
Din[5]  PHI2  F     7.478      4       3.516     4
Din[5]  nCCAS F     0.714      4       0.460     4
Din[6]  PHI2  F     5.667      4       3.636     4
Din[6]  nCCAS F     1.504      4      -0.015     M
Din[7]  PHI2  F     5.567      4       3.636     4
Din[7]  nCCAS F     1.063      4       0.194     4
MAin[0] PHI2  F     4.483      4       0.742     4
MAin[0] nCRAS F     1.204      4       0.334     4
MAin[1] PHI2  F     4.440      4       0.520     4
MAin[1] nCRAS F     1.245      4       0.313     4
MAin[2] PHI2  F     9.497      4      -0.729     M
MAin[2] nCRAS F     0.758      4       0.714     4
MAin[3] PHI2  F     9.534      4      -0.752     M
MAin[3] nCRAS F     0.454      4       0.874     4
MAin[4] PHI2  F     7.882      4      -0.326     M
MAin[4] nCRAS F     0.832      4       0.632     4
MAin[5] PHI2  F    10.136      4      -0.894     M
MAin[5] nCRAS F     0.830      4       0.632     4
MAin[6] PHI2  F     8.759      4      -0.555     M
MAin[6] nCRAS F     1.259      4       0.268     4
MAin[7] PHI2  F     8.430      4      -0.434     M
MAin[7] nCRAS F     0.881      4       0.510     4
MAin[8] nCRAS F     1.066      4       0.422     4
MAin[9] nCRAS F     0.723      4       0.746     4
PHI2    RCLK  R    -0.005      M       2.116     4
nCCAS   RCLK  R     3.614      4      -0.637     M
nCCAS   nCRAS F     3.629      4      -0.447     M
nCRAS   RCLK  R     3.040      4      -0.485     M
nFWE    PHI2  F     8.830      4      -0.567     M
nFWE    nCRAS F     0.454      4       0.874     4


// Clock to Output Delay

Port    Clock Edge  Max_Delay Performance_Grade  Min_Delay Performance_Grade
------------------------------------------------------------------------
LED     RCLK  R    11.284         4        2.893          M
LED     nCRAS F    11.111         4        3.244          M
RA[0]   RCLK  R    10.888         4        3.313          M
RA[0]   nCRAS F    11.968         4        3.554          M
RA[10]  RCLK  R     7.578         4        2.578          M
RA[11]  PHI2  R     9.098         4        3.021          M
RA[1]   RCLK  R    11.272         4        3.408          M
RA[1]   nCRAS F    11.484         4        3.438          M
RA[2]   RCLK  R    11.749         4        3.528          M
RA[2]   nCRAS F    11.267         4        3.385          M
RA[3]   RCLK  R    11.291         4        3.431          M
RA[3]   nCRAS F    11.596         4        3.449          M
RA[4]   RCLK  R    10.696         4        3.276          M
RA[4]   nCRAS F    11.720         4        3.503          M
RA[5]   RCLK  R    11.228         4        3.401          M
RA[5]   nCRAS F    11.364         4        3.427          M
RA[6]   RCLK  R    10.132         4        3.112          M
RA[6]   nCRAS F    10.958         4        3.284          M
RA[7]   RCLK  R    11.404         4        3.446          M
RA[7]   nCRAS F    11.918         4        3.561          M
RA[8]   RCLK  R    10.488         4        3.236          M
RA[8]   nCRAS F    11.512         4        3.463          M
RA[9]   RCLK  R    10.941         4        3.329          M
RA[9]   nCRAS F    11.074         4        3.356          M
RBA[0]  nCRAS F     8.645         4        2.828          M
RBA[1]  nCRAS F     8.625         4        2.835          M
RCKE    RCLK  R     9.454         4        3.006          M
RCLKout RCLK  R     6.857         4        1.980          M
RDQMH   RCLK  R     9.846         4        3.033          M
RDQML   RCLK  R     9.741         4        3.008          M
RD[0]   nCCAS F     8.761         4        2.984          M
RD[1]   nCCAS F     8.761         4        2.984          M
RD[2]   nCCAS F     8.761         4        2.984          M
RD[3]   nCCAS F     8.761         4        2.984          M
RD[4]   nCCAS F     8.761         4        2.984          M
RD[5]   nCCAS F     8.761         4        2.984          M
RD[6]   nCCAS F     8.761         4        2.984          M
RD[7]   nCCAS F     8.761         4        2.984          M
nRCAS   RCLK  R     7.578         4        2.578          M
nRCS    RCLK  R     7.578         4        2.578          M
nRRAS   RCLK  R     7.578         4        2.578          M
nRWE    RCLK  R     7.558         4        2.585          M
WARNING: you must also run trce with hold speed: 4
WARNING: you must also run trce with setup speed: M
