
Loading design for application trce from file ram2gs_lcmxo640c_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO640C
Package:     TQFP100
Performance: 3
Loading device for application trce from file 'mj5g12x10.nph' in environment: C:/lscc/diamond/3.12/ispfpga.
Package Status:                     Final          Version 1.17.
Performance Hardware Data Status: Version 1.124.
Setup and Hold Report

--------------------------------------------------------------------------------
Lattice TRACE Report - Setup, Version Diamond (64-bit) 3.12.1.454
Sat Jan 06 06:25:20 2024

Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
Copyright (c) 1995 AT&T Corp.   All rights reserved.
Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
Copyright (c) 2001 Agere Systems   All rights reserved.
Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.

Report Information
------------------
Command line:    trce -v 10 -gt -sethld -sp 3 -sphld m -o RAM2GS_LCMXO640C_impl1.twr -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO640C/promote.xml RAM2GS_LCMXO640C_impl1.ncd RAM2GS_LCMXO640C_impl1.prf 
Design file:     ram2gs_lcmxo640c_impl1.ncd
Preference file: ram2gs_lcmxo640c_impl1.prf
Device,speed:    LCMXO640C,3
Report level:    verbose report, limited to 10 items per preference
--------------------------------------------------------------------------------

BLOCK ASYNCPATHS
BLOCK RESETPATHS
--------------------------------------------------------------------------------



================================================================================
Preference: FREQUENCY PORT "PHI2" 2.900000 MHz ;
            168 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 161.315ns (weighted slack = 322.630ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[4]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMSDI  (to PHI2_c -)

   Delay:              10.834ns  (22.3% logic, 77.7% route), 6 logic levels.

 Constraint Details:

     10.834ns physical path delay SLICE_93 to SLICE_88 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.265ns CE_SET requirement (totaling 172.149ns) by 161.315ns

 Physical Path Details:

      Data path SLICE_93 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R2C4C.CLK to       R2C4C.Q0 SLICE_93 (from PHI2_c)
ROUTE         1     2.104       R2C4C.Q0 to       R7C5A.B0 Bank[4]
CTOF_DEL    ---     0.371       R7C5A.B0 to       R7C5A.F0 SLICE_100
ROUTE         2     1.032       R7C5A.F0 to       R8C5C.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R8C5C.A0 to       R8C5C.F0 SLICE_79
ROUTE         2     1.503       R8C5C.F0 to       R7C6B.A1 C1WR_7
CTOF_DEL    ---     0.371       R7C6B.A1 to       R7C6B.F1 SLICE_70
ROUTE         2     0.710       R7C6B.F1 to       R9C6A.D0 CMDWR
CTOF_DEL    ---     0.371       R9C6A.D0 to       R9C6A.F0 SLICE_73
ROUTE         5     1.398       R9C6A.F0 to       R9C8C.C1 XOR8MEG18
CTOF_DEL    ---     0.371       R9C8C.C1 to       R9C8C.F1 SLICE_85
ROUTE         2     1.672       R9C8C.F1 to       R9C7A.CE CmdUFMCLK_1_sqmuxa (to PHI2_c)
                  --------
                   10.834   (22.3% logic, 77.7% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_93:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R2C4C.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R9C7A.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 161.760ns (weighted slack = 323.520ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[5]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMSDI  (to PHI2_c -)

   Delay:              10.389ns  (23.2% logic, 76.8% route), 6 logic levels.

 Constraint Details:

     10.389ns physical path delay SLICE_93 to SLICE_88 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.265ns CE_SET requirement (totaling 172.149ns) by 161.760ns

 Physical Path Details:

      Data path SLICE_93 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R2C4C.CLK to       R2C4C.Q1 SLICE_93 (from PHI2_c)
ROUTE         1     1.979       R2C4C.Q1 to       R8C5A.A1 Bank[5]
CTOF_DEL    ---     0.371       R8C5A.A1 to       R8C5A.F1 SLICE_77
ROUTE         2     0.712       R8C5A.F1 to       R8C5C.B0 un1_Bank_1_5
CTOF_DEL    ---     0.371       R8C5C.B0 to       R8C5C.F0 SLICE_79
ROUTE         2     1.503       R8C5C.F0 to       R7C6B.A1 C1WR_7
CTOF_DEL    ---     0.371       R7C6B.A1 to       R7C6B.F1 SLICE_70
ROUTE         2     0.710       R7C6B.F1 to       R9C6A.D0 CMDWR
CTOF_DEL    ---     0.371       R9C6A.D0 to       R9C6A.F0 SLICE_73
ROUTE         5     1.398       R9C6A.F0 to       R9C8C.C1 XOR8MEG18
CTOF_DEL    ---     0.371       R9C8C.C1 to       R9C8C.F1 SLICE_85
ROUTE         2     1.672       R9C8C.F1 to       R9C7A.CE CmdUFMCLK_1_sqmuxa (to PHI2_c)
                  --------
                   10.389   (23.2% logic, 76.8% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_93:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R2C4C.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R9C7A.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 161.922ns (weighted slack = 323.844ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[4]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:              10.318ns  (27.0% logic, 73.0% route), 7 logic levels.

 Constraint Details:

     10.318ns physical path delay SLICE_93 to SLICE_20 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 161.922ns

 Physical Path Details:

      Data path SLICE_93 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R2C4C.CLK to       R2C4C.Q0 SLICE_93 (from PHI2_c)
ROUTE         1     2.104       R2C4C.Q0 to       R7C5A.B0 Bank[4]
CTOF_DEL    ---     0.371       R7C5A.B0 to       R7C5A.F0 SLICE_100
ROUTE         2     1.032       R7C5A.F0 to       R8C5C.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R8C5C.A0 to       R8C5C.F0 SLICE_79
ROUTE         2     0.320       R8C5C.F0 to       R8C5B.D0 C1WR_7
CTOF_DEL    ---     0.371       R8C5B.D0 to       R8C5B.F0 SLICE_76
ROUTE         5     2.032       R8C5B.F0 to       R7C6B.B0 C1WR
CTOF_DEL    ---     0.371       R7C6B.B0 to       R7C6B.F0 SLICE_70
ROUTE         1     1.086       R7C6B.F0 to       R8C6C.B1 N_121
CTOF_DEL    ---     0.371       R8C6C.B1 to       R8C6C.F1 SLICE_14
ROUTE         1     0.958       R8C6C.F1 to       R8C6A.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.371       R8C6A.A0 to       R8C6A.F0 SLICE_20
ROUTE         1     0.000       R8C6A.F0 to      R8C6A.DI0 CmdEnable_s (to PHI2_c)
                  --------
                   10.318   (27.0% logic, 73.0% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_93:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R2C4C.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R8C6A.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.174ns (weighted slack = 324.348ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[3]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMSDI  (to PHI2_c -)

   Delay:               9.975ns  (24.2% logic, 75.8% route), 6 logic levels.

 Constraint Details:

      9.975ns physical path delay SLICE_79 to SLICE_88 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.265ns CE_SET requirement (totaling 172.149ns) by 162.174ns

 Physical Path Details:

      Data path SLICE_79 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C5C.CLK to       R8C5C.Q1 SLICE_79 (from PHI2_c)
ROUTE         1     1.245       R8C5C.Q1 to       R7C5A.C0 Bank[3]
CTOF_DEL    ---     0.371       R7C5A.C0 to       R7C5A.F0 SLICE_100
ROUTE         2     1.032       R7C5A.F0 to       R8C5C.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R8C5C.A0 to       R8C5C.F0 SLICE_79
ROUTE         2     1.503       R8C5C.F0 to       R7C6B.A1 C1WR_7
CTOF_DEL    ---     0.371       R7C6B.A1 to       R7C6B.F1 SLICE_70
ROUTE         2     0.710       R7C6B.F1 to       R9C6A.D0 CMDWR
CTOF_DEL    ---     0.371       R9C6A.D0 to       R9C6A.F0 SLICE_73
ROUTE         5     1.398       R9C6A.F0 to       R9C8C.C1 XOR8MEG18
CTOF_DEL    ---     0.371       R9C8C.C1 to       R9C8C.F1 SLICE_85
ROUTE         2     1.672       R9C8C.F1 to       R9C7A.CE CmdUFMCLK_1_sqmuxa (to PHI2_c)
                  --------
                    9.975   (24.2% logic, 75.8% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_79:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R8C5C.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R9C7A.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.258ns (weighted slack = 324.516ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[4]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               9.982ns  (27.9% logic, 72.1% route), 7 logic levels.

 Constraint Details:

      9.982ns physical path delay SLICE_93 to SLICE_20 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.258ns

 Physical Path Details:

      Data path SLICE_93 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R2C4C.CLK to       R2C4C.Q0 SLICE_93 (from PHI2_c)
ROUTE         1     2.104       R2C4C.Q0 to       R7C5A.B0 Bank[4]
CTOF_DEL    ---     0.371       R7C5A.B0 to       R7C5A.F0 SLICE_100
ROUTE         2     1.032       R7C5A.F0 to       R8C5C.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R8C5C.A0 to       R8C5C.F0 SLICE_79
ROUTE         2     1.503       R8C5C.F0 to       R7C6B.A1 C1WR_7
CTOF_DEL    ---     0.371       R7C6B.A1 to       R7C6B.F1 SLICE_70
ROUTE         2     0.513       R7C6B.F1 to       R7C6B.C0 CMDWR
CTOF_DEL    ---     0.371       R7C6B.C0 to       R7C6B.F0 SLICE_70
ROUTE         1     1.086       R7C6B.F0 to       R8C6C.B1 N_121
CTOF_DEL    ---     0.371       R8C6C.B1 to       R8C6C.F1 SLICE_14
ROUTE         1     0.958       R8C6C.F1 to       R8C6A.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.371       R8C6A.A0 to       R8C6A.F0 SLICE_20
ROUTE         1     0.000       R8C6A.F0 to      R8C6A.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    9.982   (27.9% logic, 72.1% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_93:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R2C4C.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R8C6A.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.324ns (weighted slack = 324.648ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[4]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMCS  (to PHI2_c -)
                   FF                        CmdUFMCLK

   Delay:               9.825ns  (24.6% logic, 75.4% route), 6 logic levels.

 Constraint Details:

      9.825ns physical path delay SLICE_93 to SLICE_85 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.265ns CE_SET requirement (totaling 172.149ns) by 162.324ns

 Physical Path Details:

      Data path SLICE_93 to SLICE_85:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R2C4C.CLK to       R2C4C.Q0 SLICE_93 (from PHI2_c)
ROUTE         1     2.104       R2C4C.Q0 to       R7C5A.B0 Bank[4]
CTOF_DEL    ---     0.371       R7C5A.B0 to       R7C5A.F0 SLICE_100
ROUTE         2     1.032       R7C5A.F0 to       R8C5C.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R8C5C.A0 to       R8C5C.F0 SLICE_79
ROUTE         2     1.503       R8C5C.F0 to       R7C6B.A1 C1WR_7
CTOF_DEL    ---     0.371       R7C6B.A1 to       R7C6B.F1 SLICE_70
ROUTE         2     0.710       R7C6B.F1 to       R9C6A.D0 CMDWR
CTOF_DEL    ---     0.371       R9C6A.D0 to       R9C6A.F0 SLICE_73
ROUTE         5     1.398       R9C6A.F0 to       R9C8C.C1 XOR8MEG18
CTOF_DEL    ---     0.371       R9C8C.C1 to       R9C8C.F1 SLICE_85
ROUTE         2     0.663       R9C8C.F1 to       R9C8C.CE CmdUFMCLK_1_sqmuxa (to PHI2_c)
                  --------
                    9.825   (24.6% logic, 75.4% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_93:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R2C4C.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_85:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R9C8C.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.367ns (weighted slack = 324.734ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[5]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               9.873ns  (28.2% logic, 71.8% route), 7 logic levels.

 Constraint Details:

      9.873ns physical path delay SLICE_93 to SLICE_20 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.367ns

 Physical Path Details:

      Data path SLICE_93 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R2C4C.CLK to       R2C4C.Q1 SLICE_93 (from PHI2_c)
ROUTE         1     1.979       R2C4C.Q1 to       R8C5A.A1 Bank[5]
CTOF_DEL    ---     0.371       R8C5A.A1 to       R8C5A.F1 SLICE_77
ROUTE         2     0.712       R8C5A.F1 to       R8C5C.B0 un1_Bank_1_5
CTOF_DEL    ---     0.371       R8C5C.B0 to       R8C5C.F0 SLICE_79
ROUTE         2     0.320       R8C5C.F0 to       R8C5B.D0 C1WR_7
CTOF_DEL    ---     0.371       R8C5B.D0 to       R8C5B.F0 SLICE_76
ROUTE         5     2.032       R8C5B.F0 to       R7C6B.B0 C1WR
CTOF_DEL    ---     0.371       R7C6B.B0 to       R7C6B.F0 SLICE_70
ROUTE         1     1.086       R7C6B.F0 to       R8C6C.B1 N_121
CTOF_DEL    ---     0.371       R8C6C.B1 to       R8C6C.F1 SLICE_14
ROUTE         1     0.958       R8C6C.F1 to       R8C6A.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.371       R8C6A.A0 to       R8C6A.F0 SLICE_20
ROUTE         1     0.000       R8C6A.F0 to      R8C6A.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    9.873   (28.2% logic, 71.8% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_93:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R2C4C.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R8C6A.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.387ns (weighted slack = 324.774ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[0]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMSDI  (to PHI2_c -)

   Delay:               9.762ns  (24.7% logic, 75.3% route), 6 logic levels.

 Constraint Details:

      9.762ns physical path delay SLICE_76 to SLICE_88 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.265ns CE_SET requirement (totaling 172.149ns) by 162.387ns

 Physical Path Details:

      Data path SLICE_76 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C5B.CLK to       R8C5B.Q0 SLICE_76 (from PHI2_c)
ROUTE         1     1.032       R8C5B.Q0 to       R7C5A.A0 Bank[0]
CTOF_DEL    ---     0.371       R7C5A.A0 to       R7C5A.F0 SLICE_100
ROUTE         2     1.032       R7C5A.F0 to       R8C5C.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R8C5C.A0 to       R8C5C.F0 SLICE_79
ROUTE         2     1.503       R8C5C.F0 to       R7C6B.A1 C1WR_7
CTOF_DEL    ---     0.371       R7C6B.A1 to       R7C6B.F1 SLICE_70
ROUTE         2     0.710       R7C6B.F1 to       R9C6A.D0 CMDWR
CTOF_DEL    ---     0.371       R9C6A.D0 to       R9C6A.F0 SLICE_73
ROUTE         5     1.398       R9C6A.F0 to       R9C8C.C1 XOR8MEG18
CTOF_DEL    ---     0.371       R9C8C.C1 to       R9C8C.F1 SLICE_85
ROUTE         2     1.672       R9C8C.F1 to       R9C7A.CE CmdUFMCLK_1_sqmuxa (to PHI2_c)
                  --------
                    9.762   (24.7% logic, 75.3% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_76:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R8C5B.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R9C7A.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.647ns (weighted slack = 325.294ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[7]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMSDI  (to PHI2_c -)

   Delay:               9.502ns  (25.4% logic, 74.6% route), 6 logic levels.

 Constraint Details:

      9.502ns physical path delay SLICE_75 to SLICE_88 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.265ns CE_SET requirement (totaling 172.149ns) by 162.647ns

 Physical Path Details:

      Data path SLICE_75 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C6D.CLK to       R8C6D.Q1 SLICE_75 (from PHI2_c)
ROUTE         1     1.092       R8C6D.Q1 to       R8C5A.B1 Bank[7]
CTOF_DEL    ---     0.371       R8C5A.B1 to       R8C5A.F1 SLICE_77
ROUTE         2     0.712       R8C5A.F1 to       R8C5C.B0 un1_Bank_1_5
CTOF_DEL    ---     0.371       R8C5C.B0 to       R8C5C.F0 SLICE_79
ROUTE         2     1.503       R8C5C.F0 to       R7C6B.A1 C1WR_7
CTOF_DEL    ---     0.371       R7C6B.A1 to       R7C6B.F1 SLICE_70
ROUTE         2     0.710       R7C6B.F1 to       R9C6A.D0 CMDWR
CTOF_DEL    ---     0.371       R9C6A.D0 to       R9C6A.F0 SLICE_73
ROUTE         5     1.398       R9C6A.F0 to       R9C8C.C1 XOR8MEG18
CTOF_DEL    ---     0.371       R9C8C.C1 to       R9C8C.F1 SLICE_85
ROUTE         2     1.672       R9C8C.F1 to       R9C7A.CE CmdUFMCLK_1_sqmuxa (to PHI2_c)
                  --------
                    9.502   (25.4% logic, 74.6% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_75:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R8C6D.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R9C7A.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.703ns (weighted slack = 325.406ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[5]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               9.537ns  (29.2% logic, 70.8% route), 7 logic levels.

 Constraint Details:

      9.537ns physical path delay SLICE_93 to SLICE_20 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.703ns

 Physical Path Details:

      Data path SLICE_93 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R2C4C.CLK to       R2C4C.Q1 SLICE_93 (from PHI2_c)
ROUTE         1     1.979       R2C4C.Q1 to       R8C5A.A1 Bank[5]
CTOF_DEL    ---     0.371       R8C5A.A1 to       R8C5A.F1 SLICE_77
ROUTE         2     0.712       R8C5A.F1 to       R8C5C.B0 un1_Bank_1_5
CTOF_DEL    ---     0.371       R8C5C.B0 to       R8C5C.F0 SLICE_79
ROUTE         2     1.503       R8C5C.F0 to       R7C6B.A1 C1WR_7
CTOF_DEL    ---     0.371       R7C6B.A1 to       R7C6B.F1 SLICE_70
ROUTE         2     0.513       R7C6B.F1 to       R7C6B.C0 CMDWR
CTOF_DEL    ---     0.371       R7C6B.C0 to       R7C6B.F0 SLICE_70
ROUTE         1     1.086       R7C6B.F0 to       R8C6C.B1 N_121
CTOF_DEL    ---     0.371       R8C6C.B1 to       R8C6C.F1 SLICE_14
ROUTE         1     0.958       R8C6C.F1 to       R8C6A.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.371       R8C6A.A0 to       R8C6A.F0 SLICE_20
ROUTE         1     0.000       R8C6A.F0 to      R8C6A.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    9.537   (29.2% logic, 70.8% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_93:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R2C4C.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.682       39.PADDI to      R8C6A.CLK PHI2_c
                  --------
                    3.682   (0.0% logic, 100.0% route), 0 logic levels.

Report:   45.049MHz is the maximum frequency for this preference.


================================================================================
Preference: FREQUENCY PORT "nCCAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed:  The following path meets requirements by 342.328ns
         The internal maximum frequency of the following component is 400.000 MHz

 Logical Details:  Cell type  Pin name       Component name

   Destination:    PIO        PAD            nCCAS

   Delay:               2.500ns -- based on Minimum Pulse Width

Report:  400.000MHz is the maximum frequency for this preference.


================================================================================
Preference: FREQUENCY PORT "nCRAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed:  The following path meets requirements by 342.328ns
         The internal maximum frequency of the following component is 400.000 MHz

 Logical Details:  Cell type  Pin name       Component name

   Destination:    PIO        PAD            nCRAS

   Delay:               2.500ns -- based on Minimum Pulse Width

Report:  400.000MHz is the maximum frequency for this preference.


================================================================================
Preference: FREQUENCY PORT "RCLK" 62.500000 MHz ;
            392 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 7.529ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[15]  (from RCLK_c +)
   Destination:    FF         Data in        UFMCLK  (to RCLK_c +)

   Delay:               8.290ns  (29.1% logic, 70.9% route), 6 logic levels.

 Constraint Details:

      8.290ns physical path delay SLICE_2 to SLICE_51 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.529ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_51:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C4D.CLK to      R10C4D.Q1 SLICE_2 (from RCLK_c)
ROUTE         3     1.116      R10C4D.Q1 to      R10C5C.B1 FS[15]
CTOF_DEL    ---     0.371      R10C5C.B1 to      R10C5C.F1 SLICE_86
ROUTE         1     1.026      R10C5C.F1 to      R10C6D.A1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371      R10C6D.A1 to      R10C6D.F1 SLICE_69
ROUTE         4     1.689      R10C6D.F1 to      R10C6D.B0 N_128
CTOF_DEL    ---     0.371      R10C6D.B0 to      R10C6D.F0 SLICE_69
ROUTE         1     1.547      R10C6D.F0 to      R10C9C.B1 N_129
CTOF_DEL    ---     0.371      R10C9C.B1 to      R10C9C.F1 SLICE_51
ROUTE         1     0.497      R10C9C.F1 to      R10C9C.C0 UFMCLK_r_i_m4_xx_mm_1
CTOF_DEL    ---     0.371      R10C9C.C0 to      R10C9C.F0 SLICE_51
ROUTE         1     0.000      R10C9C.F0 to     R10C9C.DI0 UFMCLK_RNO (to RCLK_c)
                  --------
                    8.290   (29.1% logic, 70.9% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C4D.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_51:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C9C.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.597ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[12]  (from RCLK_c +)
   Destination:    FF         Data in        UFMCLK  (to RCLK_c +)

   Delay:               8.222ns  (29.4% logic, 70.6% route), 6 logic levels.

 Constraint Details:

      8.222ns physical path delay SLICE_3 to SLICE_51 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.597ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_51:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C4C.CLK to      R10C4C.Q0 SLICE_3 (from RCLK_c)
ROUTE         3     1.048      R10C4C.Q0 to      R10C5C.A1 FS[12]
CTOF_DEL    ---     0.371      R10C5C.A1 to      R10C5C.F1 SLICE_86
ROUTE         1     1.026      R10C5C.F1 to      R10C6D.A1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371      R10C6D.A1 to      R10C6D.F1 SLICE_69
ROUTE         4     1.689      R10C6D.F1 to      R10C6D.B0 N_128
CTOF_DEL    ---     0.371      R10C6D.B0 to      R10C6D.F0 SLICE_69
ROUTE         1     1.547      R10C6D.F0 to      R10C9C.B1 N_129
CTOF_DEL    ---     0.371      R10C9C.B1 to      R10C9C.F1 SLICE_51
ROUTE         1     0.497      R10C9C.F1 to      R10C9C.C0 UFMCLK_r_i_m4_xx_mm_1
CTOF_DEL    ---     0.371      R10C9C.C0 to      R10C9C.F0 SLICE_51
ROUTE         1     0.000      R10C9C.F0 to     R10C9C.DI0 UFMCLK_RNO (to RCLK_c)
                  --------
                    8.222   (29.4% logic, 70.6% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C4C.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_51:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C9C.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.653ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[4]  (from RCLK_c +)
   Destination:    FF         Data in        LEDEN  (to RCLK_c +)

   Delay:               8.103ns  (20.6% logic, 79.4% route), 4 logic levels.

 Constraint Details:

      8.103ns physical path delay SLICE_7 to SLICE_33 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.244ns CE_SET requirement (totaling 15.756ns) by 7.653ns

 Physical Path Details:

      Data path SLICE_7 to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C3C.CLK to      R10C3C.Q0 SLICE_7 (from RCLK_c)
ROUTE         3     2.172      R10C3C.Q0 to       R4C9B.D1 FS[4]
CTOF_DEL    ---     0.371       R4C9B.D1 to       R4C9B.F1 SLICE_56
ROUTE         2     2.098       R4C9B.F1 to       R9C5A.D1 N_43
CTOF_DEL    ---     0.371       R9C5A.D1 to       R9C5A.F1 SLICE_72
ROUTE         1     0.626       R9C5A.F1 to       R9C5A.D0 un1_FS_13_i_a2_1
CTOF_DEL    ---     0.371       R9C5A.D0 to       R9C5A.F0 SLICE_72
ROUTE         1     1.534       R9C5A.F0 to       R9C9B.CE N_26 (to RCLK_c)
                  --------
                    8.103   (20.6% logic, 79.4% route), 4 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_7:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C3C.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to      R9C9B.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.721ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[14]  (from RCLK_c +)
   Destination:    FF         Data in        UFMCLK  (to RCLK_c +)

   Delay:               8.098ns  (29.8% logic, 70.2% route), 6 logic levels.

 Constraint Details:

      8.098ns physical path delay SLICE_2 to SLICE_51 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.721ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_51:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C4D.CLK to      R10C4D.Q0 SLICE_2 (from RCLK_c)
ROUTE         3     0.924      R10C4D.Q0 to      R10C5C.C1 FS[14]
CTOF_DEL    ---     0.371      R10C5C.C1 to      R10C5C.F1 SLICE_86
ROUTE         1     1.026      R10C5C.F1 to      R10C6D.A1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371      R10C6D.A1 to      R10C6D.F1 SLICE_69
ROUTE         4     1.689      R10C6D.F1 to      R10C6D.B0 N_128
CTOF_DEL    ---     0.371      R10C6D.B0 to      R10C6D.F0 SLICE_69
ROUTE         1     1.547      R10C6D.F0 to      R10C9C.B1 N_129
CTOF_DEL    ---     0.371      R10C9C.B1 to      R10C9C.F1 SLICE_51
ROUTE         1     0.497      R10C9C.F1 to      R10C9C.C0 UFMCLK_r_i_m4_xx_mm_1
CTOF_DEL    ---     0.371      R10C9C.C0 to      R10C9C.F0 SLICE_51
ROUTE         1     0.000      R10C9C.F0 to     R10C9C.DI0 UFMCLK_RNO (to RCLK_c)
                  --------
                    8.098   (29.8% logic, 70.2% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C4D.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_51:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C9C.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.727ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[15]  (from RCLK_c +)
   Destination:    FF         Data in        LEDEN  (to RCLK_c +)

   Delay:               8.029ns  (25.5% logic, 74.5% route), 5 logic levels.

 Constraint Details:

      8.029ns physical path delay SLICE_2 to SLICE_33 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.244ns CE_SET requirement (totaling 15.756ns) by 7.727ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C4D.CLK to      R10C4D.Q1 SLICE_2 (from RCLK_c)
ROUTE         3     1.116      R10C4D.Q1 to      R10C5C.B1 FS[15]
CTOF_DEL    ---     0.371      R10C5C.B1 to      R10C5C.F1 SLICE_86
ROUTE         1     1.026      R10C5C.F1 to      R10C6D.A1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371      R10C6D.A1 to      R10C6D.F1 SLICE_69
ROUTE         4     1.201      R10C6D.F1 to       R9C7B.D1 N_128
CTOF_DEL    ---     0.371       R9C7B.D1 to       R9C7B.F1 SLICE_58
ROUTE         3     1.108       R9C7B.F1 to       R9C5A.B0 N_94
CTOF_DEL    ---     0.371       R9C5A.B0 to       R9C5A.F0 SLICE_72
ROUTE         1     1.534       R9C5A.F0 to       R9C9B.CE N_26 (to RCLK_c)
                  --------
                    8.029   (25.5% logic, 74.5% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C4D.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to      R9C9B.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.795ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[12]  (from RCLK_c +)
   Destination:    FF         Data in        LEDEN  (to RCLK_c +)

   Delay:               7.961ns  (25.7% logic, 74.3% route), 5 logic levels.

 Constraint Details:

      7.961ns physical path delay SLICE_3 to SLICE_33 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.244ns CE_SET requirement (totaling 15.756ns) by 7.795ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C4C.CLK to      R10C4C.Q0 SLICE_3 (from RCLK_c)
ROUTE         3     1.048      R10C4C.Q0 to      R10C5C.A1 FS[12]
CTOF_DEL    ---     0.371      R10C5C.A1 to      R10C5C.F1 SLICE_86
ROUTE         1     1.026      R10C5C.F1 to      R10C6D.A1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371      R10C6D.A1 to      R10C6D.F1 SLICE_69
ROUTE         4     1.201      R10C6D.F1 to       R9C7B.D1 N_128
CTOF_DEL    ---     0.371       R9C7B.D1 to       R9C7B.F1 SLICE_58
ROUTE         3     1.108       R9C7B.F1 to       R9C5A.B0 N_94
CTOF_DEL    ---     0.371       R9C5A.B0 to       R9C5A.F0 SLICE_72
ROUTE         1     1.534       R9C5A.F0 to       R9C9B.CE N_26 (to RCLK_c)
                  --------
                    7.961   (25.7% logic, 74.3% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C4C.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to      R9C9B.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.823ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[11]  (from RCLK_c +)
   Destination:    FF         Data in        LEDEN  (to RCLK_c +)

   Delay:               7.933ns  (21.1% logic, 78.9% route), 4 logic levels.

 Constraint Details:

      7.933ns physical path delay SLICE_4 to SLICE_33 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.244ns CE_SET requirement (totaling 15.756ns) by 7.823ns

 Physical Path Details:

      Data path SLICE_4 to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C4B.CLK to      R10C4B.Q1 SLICE_4 (from RCLK_c)
ROUTE         6     2.002      R10C4B.Q1 to       R4C9B.C1 FS[11]
CTOF_DEL    ---     0.371       R4C9B.C1 to       R4C9B.F1 SLICE_56
ROUTE         2     2.098       R4C9B.F1 to       R9C5A.D1 N_43
CTOF_DEL    ---     0.371       R9C5A.D1 to       R9C5A.F1 SLICE_72
ROUTE         1     0.626       R9C5A.F1 to       R9C5A.D0 un1_FS_13_i_a2_1
CTOF_DEL    ---     0.371       R9C5A.D0 to       R9C5A.F0 SLICE_72
ROUTE         1     1.534       R9C5A.F0 to       R9C9B.CE N_26 (to RCLK_c)
                  --------
                    7.933   (21.1% logic, 78.9% route), 4 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_4:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C4B.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to      R9C9B.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.864ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[15]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               7.955ns  (30.4% logic, 69.6% route), 6 logic levels.

 Constraint Details:

      7.955ns physical path delay SLICE_2 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.864ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C4D.CLK to      R10C4D.Q1 SLICE_2 (from RCLK_c)
ROUTE         3     1.116      R10C4D.Q1 to      R10C5C.B1 FS[15]
CTOF_DEL    ---     0.371      R10C5C.B1 to      R10C5C.F1 SLICE_86
ROUTE         1     1.026      R10C5C.F1 to      R10C6D.A1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371      R10C6D.A1 to      R10C6D.F1 SLICE_69
ROUTE         4     1.201      R10C6D.F1 to       R9C7B.D1 N_128
CTOF_DEL    ---     0.371       R9C7B.D1 to       R9C7B.F1 SLICE_58
ROUTE         3     1.171       R9C7B.F1 to      R10C9A.D0 N_94
CTOF_DEL    ---     0.371      R10C9A.D0 to      R10C9A.F0 SLICE_55
ROUTE         1     1.026      R10C9A.F0 to       R9C9C.A0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R9C9C.A0 to       R9C9C.F0 SLICE_52
ROUTE         1     0.000       R9C9C.F0 to      R9C9C.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    7.955   (30.4% logic, 69.6% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C4D.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to      R9C9C.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.884ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[15]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               7.935ns  (30.4% logic, 69.6% route), 6 logic levels.

 Constraint Details:

      7.935ns physical path delay SLICE_2 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.884ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C4D.CLK to      R10C4D.Q1 SLICE_2 (from RCLK_c)
ROUTE         3     1.116      R10C4D.Q1 to      R10C5C.B1 FS[15]
CTOF_DEL    ---     0.371      R10C5C.B1 to      R10C5C.F1 SLICE_86
ROUTE         1     1.026      R10C5C.F1 to      R10C6D.A1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371      R10C6D.A1 to      R10C6D.F1 SLICE_69
ROUTE         4     0.865      R10C6D.F1 to      R10C6A.C1 N_128
CTOF_DEL    ---     0.371      R10C6A.C1 to      R10C6A.F1 SLICE_32
ROUTE         1     1.487      R10C6A.F1 to      R10C9A.A0 UFMSDI_ens2_i_a0
CTOF_DEL    ---     0.371      R10C9A.A0 to      R10C9A.F0 SLICE_55
ROUTE         1     1.026      R10C9A.F0 to       R9C9C.A0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R9C9C.A0 to       R9C9C.F0 SLICE_52
ROUTE         1     0.000       R9C9C.F0 to      R9C9C.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    7.935   (30.4% logic, 69.6% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C4D.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to      R9C9C.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.919ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[14]  (from RCLK_c +)
   Destination:    FF         Data in        LEDEN  (to RCLK_c +)

   Delay:               7.837ns  (26.1% logic, 73.9% route), 5 logic levels.

 Constraint Details:

      7.837ns physical path delay SLICE_2 to SLICE_33 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.244ns CE_SET requirement (totaling 15.756ns) by 7.919ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560     R10C4D.CLK to      R10C4D.Q0 SLICE_2 (from RCLK_c)
ROUTE         3     0.924      R10C4D.Q0 to      R10C5C.C1 FS[14]
CTOF_DEL    ---     0.371      R10C5C.C1 to      R10C5C.F1 SLICE_86
ROUTE         1     1.026      R10C5C.F1 to      R10C6D.A1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371      R10C6D.A1 to      R10C6D.F1 SLICE_69
ROUTE         4     1.201      R10C6D.F1 to       R9C7B.D1 N_128
CTOF_DEL    ---     0.371       R9C7B.D1 to       R9C7B.F1 SLICE_58
ROUTE         3     1.108       R9C7B.F1 to       R9C5A.B0 N_94
CTOF_DEL    ---     0.371       R9C5A.B0 to       R9C5A.F0 SLICE_72
ROUTE         1     1.534       R9C5A.F0 to       R9C9B.CE N_26 (to RCLK_c)
                  --------
                    7.837   (26.1% logic, 73.9% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to     R10C4D.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.425       86.PADDI to      R9C9B.CLK RCLK_c
                  --------
                    1.425   (0.0% logic, 100.0% route), 0 logic levels.

Report:  118.050MHz is the maximum frequency for this preference.

Report Summary
--------------
----------------------------------------------------------------------------
Preference                              |   Constraint|       Actual|Levels
----------------------------------------------------------------------------
                                        |             |             |
FREQUENCY PORT "PHI2" 2.900000 MHz ;    |    2.900 MHz|   45.049 MHz|   6  
                                        |             |             |
FREQUENCY PORT "nCCAS" 2.900000 MHz ;   |    2.900 MHz|  400.000 MHz|   0  
                                        |             |             |
FREQUENCY PORT "nCRAS" 2.900000 MHz ;   |    2.900 MHz|  400.000 MHz|   0  
                                        |             |             |
FREQUENCY PORT "RCLK" 62.500000 MHz ;   |   62.500 MHz|  118.050 MHz|   6  
                                        |             |             |
----------------------------------------------------------------------------


All preferences were met.


Clock Domains Analysis
------------------------

Found 4 clocks:

Clock Domain: nCRAS_c   Source: nCRAS.PAD   Loads: 10
   No transfer within this clock domain is found

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: nCCAS_c   Source: nCCAS.PAD   Loads: 8
   No transfer within this clock domain is found

Clock Domain: RCLK_c   Source: RCLK.PAD   Loads: 32
   Covered under: FREQUENCY PORT "RCLK" 62.500000 MHz ;

   Data transfers from:
   Clock Domain: nCRAS_c   Source: nCRAS.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

   Clock Domain: PHI2_c   Source: PHI2.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: PHI2_c   Source: PHI2.PAD   Loads: 15
   Covered under: FREQUENCY PORT "PHI2" 2.900000 MHz ;

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.


Timing summary (Setup):
---------------

Timing errors: 0  Score: 0
Cumulative negative slack: 0

Constraints cover 560 paths, 4 nets, and 450 connections (66.08% coverage)

--------------------------------------------------------------------------------
Lattice TRACE Report - Hold, Version Diamond (64-bit) 3.12.1.454
Sat Jan 06 06:25:20 2024

Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
Copyright (c) 1995 AT&T Corp.   All rights reserved.
Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
Copyright (c) 2001 Agere Systems   All rights reserved.
Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.

Report Information
------------------
Command line:    trce -v 10 -gt -sethld -sp 3 -sphld m -o RAM2GS_LCMXO640C_impl1.twr -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO640C/promote.xml RAM2GS_LCMXO640C_impl1.ncd RAM2GS_LCMXO640C_impl1.prf 
Design file:     ram2gs_lcmxo640c_impl1.ncd
Preference file: ram2gs_lcmxo640c_impl1.prf
Device,speed:    LCMXO640C,m
Report level:    verbose report, limited to 10 items per preference
--------------------------------------------------------------------------------

BLOCK ASYNCPATHS
BLOCK RESETPATHS
--------------------------------------------------------------------------------



================================================================================
Preference: FREQUENCY PORT "PHI2" 2.900000 MHz ;
            168 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 0.360ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdEnable  (from PHI2_c -)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               0.341ns  (61.9% logic, 38.1% route), 2 logic levels.

 Constraint Details:

      0.341ns physical path delay SLICE_20 to SLICE_20 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.360ns

 Physical Path Details:

      Data path SLICE_20 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R8C6A.CLK to       R8C6A.Q0 SLICE_20 (from PHI2_c)
ROUTE         2     0.130       R8C6A.Q0 to       R8C6A.D0 CmdEnable
CTOF_DEL    ---     0.074       R8C6A.D0 to       R8C6A.F0 SLICE_20
ROUTE         1     0.000       R8C6A.F0 to      R8C6A.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    0.341   (61.9% logic, 38.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6A.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6A.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.361ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              C1Submitted  (from PHI2_c -)
   Destination:    FF         Data in        C1Submitted  (to PHI2_c -)

   Delay:               0.342ns  (61.7% logic, 38.3% route), 2 logic levels.

 Constraint Details:

      0.342ns physical path delay SLICE_14 to SLICE_14 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.361ns

 Physical Path Details:

      Data path SLICE_14 to SLICE_14:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R8C6C.CLK to       R8C6C.Q0 SLICE_14 (from PHI2_c)
ROUTE         2     0.131       R8C6C.Q0 to       R8C6C.A0 C1Submitted
CTOF_DEL    ---     0.074       R8C6C.A0 to       R8C6C.F0 SLICE_14
ROUTE         1     0.000       R8C6C.F0 to      R8C6C.DI0 C1Submitted_RNO (to PHI2_c)
                  --------
                    0.342   (61.7% logic, 38.3% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_14:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6C.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_14:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6C.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.361ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              ADSubmitted  (from PHI2_c -)
   Destination:    FF         Data in        ADSubmitted  (to PHI2_c -)

   Delay:               0.342ns  (61.7% logic, 38.3% route), 2 logic levels.

 Constraint Details:

      0.342ns physical path delay SLICE_9 to SLICE_9 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.361ns

 Physical Path Details:

      Data path SLICE_9 to SLICE_9:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R8C6B.CLK to       R8C6B.Q0 SLICE_9 (from PHI2_c)
ROUTE         2     0.131       R8C6B.Q0 to       R8C6B.A0 ADSubmitted
CTOF_DEL    ---     0.074       R8C6B.A0 to       R8C6B.F0 SLICE_9
ROUTE         1     0.000       R8C6B.F0 to      R8C6B.DI0 ADSubmitted_r (to PHI2_c)
                  --------
                    0.342   (61.7% logic, 38.3% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_9:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6B.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_9:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6B.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.364ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdSubmitted  (from PHI2_c -)
   Destination:    FF         Data in        CmdSubmitted  (to PHI2_c -)

   Delay:               0.345ns  (61.2% logic, 38.8% route), 2 logic levels.

 Constraint Details:

      0.345ns physical path delay SLICE_22 to SLICE_22 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.364ns

 Physical Path Details:

      Data path SLICE_22 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R9C6B.CLK to       R9C6B.Q0 SLICE_22 (from PHI2_c)
ROUTE         3     0.134       R9C6B.Q0 to       R9C6B.A0 CmdSubmitted
CTOF_DEL    ---     0.074       R9C6B.A0 to       R9C6B.F0 SLICE_22
ROUTE         1     0.000       R9C6B.F0 to      R9C6B.DI0 N_428_0 (to PHI2_c)
                  --------
                    0.345   (61.2% logic, 38.8% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R9C6B.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R9C6B.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.572ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              ADSubmitted  (from PHI2_c -)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               0.553ns  (51.5% logic, 48.5% route), 3 logic levels.

 Constraint Details:

      0.553ns physical path delay SLICE_9 to SLICE_20 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.572ns

 Physical Path Details:

      Data path SLICE_9 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R8C6B.CLK to       R8C6B.Q0 SLICE_9 (from PHI2_c)
ROUTE         2     0.130       R8C6B.Q0 to       R8C6A.D1 ADSubmitted
CTOF_DEL    ---     0.074       R8C6A.D1 to       R8C6A.F1 SLICE_20
ROUTE         1     0.138       R8C6A.F1 to       R8C6A.B0 CmdEnable_0_sqmuxa
CTOF_DEL    ---     0.074       R8C6A.B0 to       R8C6A.F0 SLICE_20
ROUTE         1     0.000       R8C6A.F0 to      R8C6A.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    0.553   (51.5% logic, 48.5% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_9:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6B.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6A.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.597ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Cmdn8MEGEN  (from PHI2_c -)
   Destination:    FF         Data in        Cmdn8MEGEN  (to PHI2_c -)

   Delay:               0.578ns  (49.3% logic, 50.7% route), 3 logic levels.

 Constraint Details:

      0.578ns physical path delay SLICE_26 to SLICE_26 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.597ns

 Physical Path Details:

      Data path SLICE_26 to SLICE_26:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R9C7D.CLK to       R9C7D.Q0 SLICE_26 (from PHI2_c)
ROUTE         2     0.194       R9C7D.Q0 to       R9C7D.A1 Cmdn8MEGEN
CTOF_DEL    ---     0.074       R9C7D.A1 to       R9C7D.F1 SLICE_26
ROUTE         1     0.099       R9C7D.F1 to       R9C7D.C0 Cmdn8MEGEN_4_u_i_0
CTOF_DEL    ---     0.074       R9C7D.C0 to       R9C7D.F0 SLICE_26
ROUTE         1     0.000       R9C7D.F0 to      R9C7D.DI0 N_12_i (to PHI2_c)
                  --------
                    0.578   (49.3% logic, 50.7% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_26:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R9C7D.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_26:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R9C7D.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.599ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdLEDEN  (from PHI2_c -)
   Destination:    FF         Data in        CmdLEDEN  (to PHI2_c -)

   Delay:               0.580ns  (49.1% logic, 50.9% route), 3 logic levels.

 Constraint Details:

      0.580ns physical path delay SLICE_21 to SLICE_21 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.599ns

 Physical Path Details:

      Data path SLICE_21 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R9C8D.CLK to       R9C8D.Q0 SLICE_21 (from PHI2_c)
ROUTE         2     0.196       R9C8D.Q0 to       R9C8D.A1 CmdLEDEN
CTOF_DEL    ---     0.074       R9C8D.A1 to       R9C8D.F1 SLICE_21
ROUTE         1     0.099       R9C8D.F1 to       R9C8D.C0 CmdLEDEN_4_u_i_0
CTOF_DEL    ---     0.074       R9C8D.C0 to       R9C8D.F0 SLICE_21
ROUTE         1     0.000       R9C8D.F0 to      R9C8D.DI0 N_14_i (to PHI2_c)
                  --------
                    0.580   (49.1% logic, 50.9% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R9C8D.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R9C8D.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.626ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              C1Submitted  (from PHI2_c -)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               0.607ns  (47.0% logic, 53.0% route), 3 logic levels.

 Constraint Details:

      0.607ns physical path delay SLICE_14 to SLICE_20 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.626ns

 Physical Path Details:

      Data path SLICE_14 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R8C6C.CLK to       R8C6C.Q0 SLICE_14 (from PHI2_c)
ROUTE         2     0.130       R8C6C.Q0 to       R8C6C.D1 C1Submitted
CTOF_DEL    ---     0.074       R8C6C.D1 to       R8C6C.F1 SLICE_14
ROUTE         1     0.192       R8C6C.F1 to       R8C6A.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.074       R8C6A.A0 to       R8C6A.F0 SLICE_20
ROUTE         1     0.000       R8C6A.F0 to      R8C6A.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    0.607   (47.0% logic, 53.0% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_14:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6C.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6A.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.638ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              XOR8MEG  (from PHI2_c -)
   Destination:    FF         Data in        XOR8MEG  (to PHI2_c -)

   Delay:               0.619ns  (46.0% logic, 54.0% route), 3 logic levels.

 Constraint Details:

      0.619ns physical path delay SLICE_57 to SLICE_57 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.638ns

 Physical Path Details:

      Data path SLICE_57 to SLICE_57:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R9C8A.CLK to       R9C8A.Q0 SLICE_57 (from PHI2_c)
ROUTE         2     0.196       R9C8A.Q0 to       R9C8A.A1 XOR8MEG
CTOF_DEL    ---     0.074       R9C8A.A1 to       R9C8A.F1 SLICE_57
ROUTE         1     0.138       R9C8A.F1 to       R9C8A.B0 N_166
CTOF_DEL    ---     0.074       R9C8A.B0 to       R9C8A.F0 SLICE_57
ROUTE         1     0.000       R9C8A.F0 to      R9C8A.DI0 XOR8MEG_3 (to PHI2_c)
                  --------
                    0.619   (46.0% logic, 54.0% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_57:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R9C8A.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_57:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R9C8A.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.659ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdEnable  (from PHI2_c -)
   Destination:    FF         Data in        CmdLEDEN  (to PHI2_c -)

   Delay:               0.636ns  (33.2% logic, 66.8% route), 2 logic levels.

 Constraint Details:

      0.636ns physical path delay SLICE_20 to SLICE_21 meets
     -0.023ns CE_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.023ns) by 0.659ns

 Physical Path Details:

      Data path SLICE_20 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R8C6A.CLK to       R8C6A.Q0 SLICE_20 (from PHI2_c)
ROUTE         2     0.183       R8C6A.Q0 to       R9C6A.C0 CmdEnable
CTOF_DEL    ---     0.074       R9C6A.C0 to       R9C6A.F0 SLICE_73
ROUTE         5     0.242       R9C6A.F0 to       R9C8D.CE XOR8MEG18 (to PHI2_c)
                  --------
                    0.636   (33.2% logic, 66.8% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R8C6A.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.907       39.PADDI to      R9C8D.CLK PHI2_c
                  --------
                    0.907   (0.0% logic, 100.0% route), 0 logic levels.


================================================================================
Preference: FREQUENCY PORT "nCCAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


================================================================================
Preference: FREQUENCY PORT "nCRAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


================================================================================
Preference: FREQUENCY PORT "RCLK" 62.500000 MHz ;
            392 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 0.273ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CASr  (from RCLK_c +)
   Destination:    FF         Data in        CASr2  (to RCLK_c +)

   Delay:               0.256ns  (49.2% logic, 50.8% route), 1 logic levels.

 Constraint Details:

      0.256ns physical path delay SLICE_74 to SLICE_74 meets
     -0.017ns M_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.017ns) by 0.273ns

 Physical Path Details:

      Data path SLICE_74 to SLICE_74:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R8C7B.CLK to       R8C7B.Q0 SLICE_74 (from RCLK_c)
ROUTE         1     0.130       R8C7B.Q0 to       R8C7B.M1 CASr (to RCLK_c)
                  --------
                    0.256   (49.2% logic, 50.8% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_74:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to      R8C7B.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_74:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to      R8C7B.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.277ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              PHI2r2  (from RCLK_c +)
   Destination:    FF         Data in        PHI2r3  (to RCLK_c +)

   Delay:               0.260ns  (48.5% logic, 51.5% route), 1 logic levels.

 Constraint Details:

      0.260ns physical path delay SLICE_41 to SLICE_43 meets
     -0.017ns M_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.017ns) by 0.277ns

 Physical Path Details:

      Data path SLICE_41 to SLICE_43:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R4C6C.CLK to       R4C6C.Q1 SLICE_41 (from RCLK_c)
ROUTE         3     0.134       R4C6C.Q1 to       R4C6A.M1 PHI2r2 (to RCLK_c)
                  --------
                    0.260   (48.5% logic, 51.5% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_41:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to      R4C6C.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_43:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to      R4C6A.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.277ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              RASr  (from RCLK_c +)
   Destination:    FF         Data in        RASr2  (to RCLK_c +)

   Delay:               0.260ns  (48.5% logic, 51.5% route), 1 logic levels.

 Constraint Details:

      0.260ns physical path delay SLICE_95 to SLICE_95 meets
     -0.017ns M_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.017ns) by 0.277ns

 Physical Path Details:

      Data path SLICE_95 to SLICE_95:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R3C5D.CLK to       R3C5D.Q0 SLICE_95 (from RCLK_c)
ROUTE         2     0.134       R3C5D.Q0 to       R3C5D.M1 RASr (to RCLK_c)
                  --------
                    0.260   (48.5% logic, 51.5% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_95:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to      R3C5D.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_95:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to      R3C5D.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.284ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              RASr2  (from RCLK_c +)
   Destination:    FF         Data in        S[0]  (to RCLK_c +)

   Delay:               0.267ns  (47.2% logic, 52.8% route), 1 logic levels.

 Constraint Details:

      0.267ns physical path delay SLICE_95 to SLICE_68 meets
     -0.017ns M_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.017ns) by 0.284ns

 Physical Path Details:

      Data path SLICE_95 to SLICE_68:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R3C5D.CLK to       R3C5D.Q1 SLICE_95 (from RCLK_c)
ROUTE        13     0.141       R3C5D.Q1 to       R3C5C.M0 RASr2 (to RCLK_c)
                  --------
                    0.267   (47.2% logic, 52.8% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_95:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to      R3C5D.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_68:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to      R3C5C.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[15]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[14]  (to RCLK_c +)
                   FF                        FS[15]
                   FF                        FS[14]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_2 to SLICE_2 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126     R10C4D.CLK to      R10C4D.Q1 SLICE_2 (from RCLK_c)
ROUTE         3     0.131      R10C4D.Q1 to      R10C4D.A1 FS[15] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C4D.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C4D.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[13]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[12]  (to RCLK_c +)
                   FF                        FS[13]
                   FF                        FS[12]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_3 to SLICE_3 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126     R10C4C.CLK to      R10C4C.Q1 SLICE_3 (from RCLK_c)
ROUTE         4     0.131      R10C4C.Q1 to      R10C4C.A1 FS[13] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C4C.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C4C.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[9]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[8]  (to RCLK_c +)
                   FF                        FS[9]
                   FF                        FS[8]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_5 to SLICE_5 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_5 to SLICE_5:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126     R10C4A.CLK to      R10C4A.Q1 SLICE_5 (from RCLK_c)
ROUTE         3     0.131      R10C4A.Q1 to      R10C4A.A1 FS[9] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_5:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C4A.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_5:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C4A.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[7]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[6]  (to RCLK_c +)
                   FF                        FS[7]
                   FF                        FS[6]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_6 to SLICE_6 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_6 to SLICE_6:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126     R10C3D.CLK to      R10C3D.Q1 SLICE_6 (from RCLK_c)
ROUTE         3     0.131      R10C3D.Q1 to      R10C3D.A1 FS[7] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_6:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C3D.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_6:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C3D.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[5]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[4]  (to RCLK_c +)
                   FF                        FS[5]
                   FF                        FS[4]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_7 to SLICE_7 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_7 to SLICE_7:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126     R10C3C.CLK to      R10C3C.Q1 SLICE_7 (from RCLK_c)
ROUTE         4     0.131      R10C3C.Q1 to      R10C3C.A1 FS[5] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_7:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C3C.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_7:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C3C.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[3]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[2]  (to RCLK_c +)
                   FF                        FS[3]
                   FF                        FS[2]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_8 to SLICE_8 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_8 to SLICE_8:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126     R10C3B.CLK to      R10C3B.Q1 SLICE_8 (from RCLK_c)
ROUTE         2     0.131      R10C3B.Q1 to      R10C3B.A1 FS[3] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_8:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C3B.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_8:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.351       86.PADDI to     R10C3B.CLK RCLK_c
                  --------
                    0.351   (0.0% logic, 100.0% route), 0 logic levels.

Report Summary
--------------
----------------------------------------------------------------------------
Preference(MIN Delays)                  |   Constraint|       Actual|Levels
----------------------------------------------------------------------------
                                        |             |             |
FREQUENCY PORT "PHI2" 2.900000 MHz ;    |            -|            -|   2  
                                        |             |             |
FREQUENCY PORT "nCCAS" 2.900000 MHz ;   |            -|            -|   0  
                                        |             |             |
FREQUENCY PORT "nCRAS" 2.900000 MHz ;   |            -|            -|   0  
                                        |             |             |
FREQUENCY PORT "RCLK" 62.500000 MHz ;   |            -|            -|   1  
                                        |             |             |
----------------------------------------------------------------------------


All preferences were met.


Clock Domains Analysis
------------------------

Found 4 clocks:

Clock Domain: nCRAS_c   Source: nCRAS.PAD   Loads: 10
   No transfer within this clock domain is found

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: nCCAS_c   Source: nCCAS.PAD   Loads: 8
   No transfer within this clock domain is found

Clock Domain: RCLK_c   Source: RCLK.PAD   Loads: 32
   Covered under: FREQUENCY PORT "RCLK" 62.500000 MHz ;

   Data transfers from:
   Clock Domain: nCRAS_c   Source: nCRAS.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

   Clock Domain: PHI2_c   Source: PHI2.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: PHI2_c   Source: PHI2.PAD   Loads: 15
   Covered under: FREQUENCY PORT "PHI2" 2.900000 MHz ;

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.


Timing summary (Hold):
---------------

Timing errors: 0  Score: 0
Cumulative negative slack: 0

Constraints cover 560 paths, 4 nets, and 450 connections (66.08% coverage)



Timing summary (Setup and Hold):
---------------

Timing errors: 0 (setup), 0 (hold)
Score: 0 (setup), 0 (hold)
Cumulative negative slack: 0 (0+0)
--------------------------------------------------------------------------------

--------------------------------------------------------------------------------

