
Loading design for application trce from file ram2gs_lcmxo256c_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO256C
Package:     TQFP100
Performance: 3
Loading device for application trce from file 'mj5g10x6.nph' in environment: C:/lscc/diamond/3.12/ispfpga.
Package Status:                     Final          Version 1.19.
Performance Hardware Data Status: Version 1.124.
Setup and Hold Report

--------------------------------------------------------------------------------
Lattice TRACE Report - Setup, Version Diamond (64-bit) 3.12.1.454
Sat Jan 06 06:25:12 2024

Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
Copyright (c) 1995 AT&T Corp.   All rights reserved.
Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
Copyright (c) 2001 Agere Systems   All rights reserved.
Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.

Report Information
------------------
Command line:    trce -v 10 -gt -sethld -sp 3 -sphld m -o RAM2GS_LCMXO256C_impl1.twr -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO256C/promote.xml RAM2GS_LCMXO256C_impl1.ncd RAM2GS_LCMXO256C_impl1.prf 
Design file:     ram2gs_lcmxo256c_impl1.ncd
Preference file: ram2gs_lcmxo256c_impl1.prf
Device,speed:    LCMXO256C,3
Report level:    verbose report, limited to 10 items per preference
--------------------------------------------------------------------------------

BLOCK ASYNCPATHS
BLOCK RESETPATHS
--------------------------------------------------------------------------------



================================================================================
Preference: FREQUENCY PORT "PHI2" 2.900000 MHz ;
            168 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 161.825ns (weighted slack = 323.650ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[7]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:              10.415ns  (26.7% logic, 73.3% route), 7 logic levels.

 Constraint Details:

     10.415ns physical path delay SLICE_75 to SLICE_20 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 161.825ns

 Physical Path Details:

      Data path SLICE_75 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R5C3D.CLK to       R5C3D.Q1 SLICE_75 (from PHI2_c)
ROUTE         1     2.039       R5C3D.Q1 to       R5C2D.B1 Bank[7]
CTOF_DEL    ---     0.371       R5C2D.B1 to       R5C2D.F1 SLICE_77
ROUTE         2     0.835       R5C2D.F1 to       R5C2B.C0 un1_Bank_1_5
CTOF_DEL    ---     0.371       R5C2B.C0 to       R5C2B.F0 SLICE_79
ROUTE         2     1.092       R5C2B.F0 to       R6C2C.B0 C1WR_7
CTOF_DEL    ---     0.371       R6C2C.B0 to       R6C2C.F0 SLICE_76
ROUTE         5     1.529       R6C2C.F0 to       R5C3D.A0 C1WR
CTOF_DEL    ---     0.371       R5C3D.A0 to       R5C3D.F0 SLICE_75
ROUTE         3     1.108       R5C3D.F0 to       R6C3A.B1 CmdEnable16
CTOF_DEL    ---     0.371       R6C3A.B1 to       R6C3A.F1 SLICE_14
ROUTE         1     1.026       R6C3A.F1 to       R5C3C.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.371       R5C3C.A0 to       R5C3C.F0 SLICE_20
ROUTE         1     0.000       R5C3C.F0 to      R5C3C.DI0 CmdEnable_s (to PHI2_c)
                  --------
                   10.415   (26.7% logic, 73.3% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_75:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3D.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.064ns (weighted slack = 324.128ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[7]  (from PHI2_c +)
   Destination:    FF         Data in        CmdSubmitted  (to PHI2_c -)

   Delay:              10.176ns  (27.4% logic, 72.6% route), 7 logic levels.

 Constraint Details:

     10.176ns physical path delay SLICE_75 to SLICE_22 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.064ns

 Physical Path Details:

      Data path SLICE_75 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R5C3D.CLK to       R5C3D.Q1 SLICE_75 (from PHI2_c)
ROUTE         1     2.039       R5C3D.Q1 to       R5C2D.B1 Bank[7]
CTOF_DEL    ---     0.371       R5C2D.B1 to       R5C2D.F1 SLICE_77
ROUTE         2     0.835       R5C2D.F1 to       R5C2B.C0 un1_Bank_1_5
CTOF_DEL    ---     0.371       R5C2B.C0 to       R5C2B.F0 SLICE_79
ROUTE         2     0.893       R5C2B.F0 to       R6C2B.C1 C1WR_7
CTOF_DEL    ---     0.371       R6C2B.C1 to       R6C2B.F1 SLICE_70
ROUTE         2     1.563       R6C2B.F1 to       R5C3B.B0 CMDWR
CTOF_DEL    ---     0.371       R5C3B.B0 to       R5C3B.F0 SLICE_73
ROUTE         5     0.513       R5C3B.F0 to       R5C3B.C1 XOR8MEG18
CTOF_DEL    ---     0.371       R5C3B.C1 to       R5C3B.F1 SLICE_73
ROUTE         1     1.547       R5C3B.F1 to       R6C5C.B0 CmdSubmitted_1_sqmuxa
CTOF_DEL    ---     0.371       R6C5C.B0 to       R6C5C.F0 SLICE_22
ROUTE         1     0.000       R6C5C.F0 to      R6C5C.DI0 N_428_0 (to PHI2_c)
                  --------
                   10.176   (27.4% logic, 72.6% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_75:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3D.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R6C5C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.564ns (weighted slack = 325.128ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[7]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMCS  (to PHI2_c -)
                   FF                        CmdUFMCLK

   Delay:               9.585ns  (25.2% logic, 74.8% route), 6 logic levels.

 Constraint Details:

      9.585ns physical path delay SLICE_75 to SLICE_85 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.265ns CE_SET requirement (totaling 172.149ns) by 162.564ns

 Physical Path Details:

      Data path SLICE_75 to SLICE_85:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R5C3D.CLK to       R5C3D.Q1 SLICE_75 (from PHI2_c)
ROUTE         1     2.039       R5C3D.Q1 to       R5C2D.B1 Bank[7]
CTOF_DEL    ---     0.371       R5C2D.B1 to       R5C2D.F1 SLICE_77
ROUTE         2     0.835       R5C2D.F1 to       R5C2B.C0 un1_Bank_1_5
CTOF_DEL    ---     0.371       R5C2B.C0 to       R5C2B.F0 SLICE_79
ROUTE         2     0.893       R5C2B.F0 to       R6C2B.C1 C1WR_7
CTOF_DEL    ---     0.371       R6C2B.C1 to       R6C2B.F1 SLICE_70
ROUTE         2     1.563       R6C2B.F1 to       R5C3B.B0 CMDWR
CTOF_DEL    ---     0.371       R5C3B.B0 to       R5C3B.F0 SLICE_73
ROUTE         5     1.185       R5C3B.F0 to       R6C4A.D1 XOR8MEG18
CTOF_DEL    ---     0.371       R6C4A.D1 to       R6C4A.F1 SLICE_85
ROUTE         2     0.655       R6C4A.F1 to       R6C4A.CE CmdUFMCLK_1_sqmuxa (to PHI2_c)
                  --------
                    9.585   (25.2% logic, 74.8% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_75:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3D.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_85:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R6C4A.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.564ns (weighted slack = 325.128ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[7]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMSDI  (to PHI2_c -)

   Delay:               9.585ns  (25.2% logic, 74.8% route), 6 logic levels.

 Constraint Details:

      9.585ns physical path delay SLICE_75 to SLICE_88 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.265ns CE_SET requirement (totaling 172.149ns) by 162.564ns

 Physical Path Details:

      Data path SLICE_75 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R5C3D.CLK to       R5C3D.Q1 SLICE_75 (from PHI2_c)
ROUTE         1     2.039       R5C3D.Q1 to       R5C2D.B1 Bank[7]
CTOF_DEL    ---     0.371       R5C2D.B1 to       R5C2D.F1 SLICE_77
ROUTE         2     0.835       R5C2D.F1 to       R5C2B.C0 un1_Bank_1_5
CTOF_DEL    ---     0.371       R5C2B.C0 to       R5C2B.F0 SLICE_79
ROUTE         2     0.893       R5C2B.F0 to       R6C2B.C1 C1WR_7
CTOF_DEL    ---     0.371       R6C2B.C1 to       R6C2B.F1 SLICE_70
ROUTE         2     1.563       R6C2B.F1 to       R5C3B.B0 CMDWR
CTOF_DEL    ---     0.371       R5C3B.B0 to       R5C3B.F0 SLICE_73
ROUTE         5     1.185       R5C3B.F0 to       R6C4A.D1 XOR8MEG18
CTOF_DEL    ---     0.371       R6C4A.D1 to       R6C4A.F1 SLICE_85
ROUTE         2     0.655       R6C4A.F1 to       R6C4B.CE CmdUFMCLK_1_sqmuxa (to PHI2_c)
                  --------
                    9.585   (25.2% logic, 74.8% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_75:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3D.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_88:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R6C4B.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.699ns (weighted slack = 325.398ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[1]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               9.541ns  (29.2% logic, 70.8% route), 7 logic levels.

 Constraint Details:

      9.541ns physical path delay SLICE_76 to SLICE_20 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.699ns

 Physical Path Details:

      Data path SLICE_76 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R6C2C.CLK to       R6C2C.Q1 SLICE_76 (from PHI2_c)
ROUTE         1     1.026       R6C2C.Q1 to       R5C2A.A0 Bank[1]
CTOF_DEL    ---     0.371       R5C2A.A0 to       R5C2A.F0 SLICE_100
ROUTE         2     0.974       R5C2A.F0 to       R5C2B.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R5C2B.A0 to       R5C2B.F0 SLICE_79
ROUTE         2     1.092       R5C2B.F0 to       R6C2C.B0 C1WR_7
CTOF_DEL    ---     0.371       R6C2C.B0 to       R6C2C.F0 SLICE_76
ROUTE         5     1.529       R6C2C.F0 to       R5C3D.A0 C1WR
CTOF_DEL    ---     0.371       R5C3D.A0 to       R5C3D.F0 SLICE_75
ROUTE         3     1.108       R5C3D.F0 to       R6C3A.B1 CmdEnable16
CTOF_DEL    ---     0.371       R6C3A.B1 to       R6C3A.F1 SLICE_14
ROUTE         1     1.026       R6C3A.F1 to       R5C3C.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.371       R5C3C.A0 to       R5C3C.F0 SLICE_20
ROUTE         1     0.000       R5C3C.F0 to      R5C3C.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    9.541   (29.2% logic, 70.8% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_76:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R6C2C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.707ns (weighted slack = 325.414ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[3]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               9.533ns  (29.2% logic, 70.8% route), 7 logic levels.

 Constraint Details:

      9.533ns physical path delay SLICE_79 to SLICE_20 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.707ns

 Physical Path Details:

      Data path SLICE_79 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R5C2B.CLK to       R5C2B.Q1 SLICE_79 (from PHI2_c)
ROUTE         1     1.018       R5C2B.Q1 to       R5C2A.B0 Bank[3]
CTOF_DEL    ---     0.371       R5C2A.B0 to       R5C2A.F0 SLICE_100
ROUTE         2     0.974       R5C2A.F0 to       R5C2B.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R5C2B.A0 to       R5C2B.F0 SLICE_79
ROUTE         2     1.092       R5C2B.F0 to       R6C2C.B0 C1WR_7
CTOF_DEL    ---     0.371       R6C2C.B0 to       R6C2C.F0 SLICE_76
ROUTE         5     1.529       R6C2C.F0 to       R5C3D.A0 C1WR
CTOF_DEL    ---     0.371       R5C3D.A0 to       R5C3D.F0 SLICE_75
ROUTE         3     1.108       R5C3D.F0 to       R6C3A.B1 CmdEnable16
CTOF_DEL    ---     0.371       R6C3A.B1 to       R6C3A.F1 SLICE_14
ROUTE         1     1.026       R6C3A.F1 to       R5C3C.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.371       R5C3C.A0 to       R5C3C.F0 SLICE_20
ROUTE         1     0.000       R5C3C.F0 to      R5C3C.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    9.533   (29.2% logic, 70.8% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_79:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C2B.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.832ns (weighted slack = 325.664ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[6]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               9.408ns  (29.6% logic, 70.4% route), 7 logic levels.

 Constraint Details:

      9.408ns physical path delay SLICE_75 to SLICE_20 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.832ns

 Physical Path Details:

      Data path SLICE_75 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R5C3D.CLK to       R5C3D.Q0 SLICE_75 (from PHI2_c)
ROUTE         1     1.032       R5C3D.Q0 to       R5C2D.A1 Bank[6]
CTOF_DEL    ---     0.371       R5C2D.A1 to       R5C2D.F1 SLICE_77
ROUTE         2     0.835       R5C2D.F1 to       R5C2B.C0 un1_Bank_1_5
CTOF_DEL    ---     0.371       R5C2B.C0 to       R5C2B.F0 SLICE_79
ROUTE         2     1.092       R5C2B.F0 to       R6C2C.B0 C1WR_7
CTOF_DEL    ---     0.371       R6C2C.B0 to       R6C2C.F0 SLICE_76
ROUTE         5     1.529       R6C2C.F0 to       R5C3D.A0 C1WR
CTOF_DEL    ---     0.371       R5C3D.A0 to       R5C3D.F0 SLICE_75
ROUTE         3     1.108       R5C3D.F0 to       R6C3A.B1 CmdEnable16
CTOF_DEL    ---     0.371       R6C3A.B1 to       R6C3A.F1 SLICE_14
ROUTE         1     1.026       R6C3A.F1 to       R5C3C.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.371       R5C3C.A0 to       R5C3C.F0 SLICE_20
ROUTE         1     0.000       R5C3C.F0 to      R5C3C.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    9.408   (29.6% logic, 70.4% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_75:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3D.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.838ns (weighted slack = 325.676ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[4]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               9.402ns  (29.6% logic, 70.4% route), 7 logic levels.

 Constraint Details:

      9.402ns physical path delay SLICE_93 to SLICE_20 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.838ns

 Physical Path Details:

      Data path SLICE_93 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R6C2A.CLK to       R6C2A.Q0 SLICE_93 (from PHI2_c)
ROUTE         1     0.887       R6C2A.Q0 to       R5C2A.C0 Bank[4]
CTOF_DEL    ---     0.371       R5C2A.C0 to       R5C2A.F0 SLICE_100
ROUTE         2     0.974       R5C2A.F0 to       R5C2B.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R5C2B.A0 to       R5C2B.F0 SLICE_79
ROUTE         2     1.092       R5C2B.F0 to       R6C2C.B0 C1WR_7
CTOF_DEL    ---     0.371       R6C2C.B0 to       R6C2C.F0 SLICE_76
ROUTE         5     1.529       R6C2C.F0 to       R5C3D.A0 C1WR
CTOF_DEL    ---     0.371       R5C3D.A0 to       R5C3D.F0 SLICE_75
ROUTE         3     1.108       R5C3D.F0 to       R6C3A.B1 CmdEnable16
CTOF_DEL    ---     0.371       R6C3A.B1 to       R6C3A.F1 SLICE_14
ROUTE         1     1.026       R6C3A.F1 to       R5C3C.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.371       R5C3C.A0 to       R5C3C.F0 SLICE_20
ROUTE         1     0.000       R5C3C.F0 to      R5C3C.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    9.402   (29.6% logic, 70.4% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_93:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R6C2A.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.938ns (weighted slack = 325.876ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[1]  (from PHI2_c +)
   Destination:    FF         Data in        CmdSubmitted  (to PHI2_c -)

   Delay:               9.302ns  (30.0% logic, 70.0% route), 7 logic levels.

 Constraint Details:

      9.302ns physical path delay SLICE_76 to SLICE_22 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.938ns

 Physical Path Details:

      Data path SLICE_76 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R6C2C.CLK to       R6C2C.Q1 SLICE_76 (from PHI2_c)
ROUTE         1     1.026       R6C2C.Q1 to       R5C2A.A0 Bank[1]
CTOF_DEL    ---     0.371       R5C2A.A0 to       R5C2A.F0 SLICE_100
ROUTE         2     0.974       R5C2A.F0 to       R5C2B.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R5C2B.A0 to       R5C2B.F0 SLICE_79
ROUTE         2     0.893       R5C2B.F0 to       R6C2B.C1 C1WR_7
CTOF_DEL    ---     0.371       R6C2B.C1 to       R6C2B.F1 SLICE_70
ROUTE         2     1.563       R6C2B.F1 to       R5C3B.B0 CMDWR
CTOF_DEL    ---     0.371       R5C3B.B0 to       R5C3B.F0 SLICE_73
ROUTE         5     0.513       R5C3B.F0 to       R5C3B.C1 XOR8MEG18
CTOF_DEL    ---     0.371       R5C3B.C1 to       R5C3B.F1 SLICE_73
ROUTE         1     1.547       R5C3B.F1 to       R6C5C.B0 CmdSubmitted_1_sqmuxa
CTOF_DEL    ---     0.371       R6C5C.B0 to       R6C5C.F0 SLICE_22
ROUTE         1     0.000       R6C5C.F0 to      R6C5C.DI0 N_428_0 (to PHI2_c)
                  --------
                    9.302   (30.0% logic, 70.0% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_76:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R6C2C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R6C5C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.946ns (weighted slack = 325.892ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank[3]  (from PHI2_c +)
   Destination:    FF         Data in        CmdSubmitted  (to PHI2_c -)

   Delay:               9.294ns  (30.0% logic, 70.0% route), 7 logic levels.

 Constraint Details:

      9.294ns physical path delay SLICE_79 to SLICE_22 meets
    172.414ns delay constraint less
      0.000ns skew and
      0.174ns DIN_SET requirement (totaling 172.240ns) by 162.946ns

 Physical Path Details:

      Data path SLICE_79 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R5C2B.CLK to       R5C2B.Q1 SLICE_79 (from PHI2_c)
ROUTE         1     1.018       R5C2B.Q1 to       R5C2A.B0 Bank[3]
CTOF_DEL    ---     0.371       R5C2A.B0 to       R5C2A.F0 SLICE_100
ROUTE         2     0.974       R5C2A.F0 to       R5C2B.A0 un1_Bank_1_4
CTOF_DEL    ---     0.371       R5C2B.A0 to       R5C2B.F0 SLICE_79
ROUTE         2     0.893       R5C2B.F0 to       R6C2B.C1 C1WR_7
CTOF_DEL    ---     0.371       R6C2B.C1 to       R6C2B.F1 SLICE_70
ROUTE         2     1.563       R6C2B.F1 to       R5C3B.B0 CMDWR
CTOF_DEL    ---     0.371       R5C3B.B0 to       R5C3B.F0 SLICE_73
ROUTE         5     0.513       R5C3B.F0 to       R5C3B.C1 XOR8MEG18
CTOF_DEL    ---     0.371       R5C3B.C1 to       R5C3B.F1 SLICE_73
ROUTE         1     1.547       R5C3B.F1 to       R6C5C.B0 CmdSubmitted_1_sqmuxa
CTOF_DEL    ---     0.371       R6C5C.B0 to       R6C5C.F0 SLICE_22
ROUTE         1     0.000       R6C5C.F0 to      R6C5C.DI0 N_428_0 (to PHI2_c)
                  --------
                    9.294   (30.0% logic, 70.0% route), 7 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_79:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R5C2B.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     3.919       39.PADDI to      R6C5C.CLK PHI2_c
                  --------
                    3.919   (0.0% logic, 100.0% route), 0 logic levels.

Report:   47.219MHz is the maximum frequency for this preference.


================================================================================
Preference: FREQUENCY PORT "nCCAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed:  The following path meets requirements by 342.328ns
         The internal maximum frequency of the following component is 400.000 MHz

 Logical Details:  Cell type  Pin name       Component name

   Destination:    PIO        PAD            nCCAS

   Delay:               2.500ns -- based on Minimum Pulse Width

Report:  400.000MHz is the maximum frequency for this preference.


================================================================================
Preference: FREQUENCY PORT "nCRAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed:  The following path meets requirements by 342.328ns
         The internal maximum frequency of the following component is 400.000 MHz

 Logical Details:  Cell type  Pin name       Component name

   Destination:    PIO        PAD            nCRAS

   Delay:               2.500ns -- based on Minimum Pulse Width

Report:  400.000MHz is the maximum frequency for this preference.


================================================================================
Preference: FREQUENCY PORT "RCLK" 62.500000 MHz ;
            392 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 6.770ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[12]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               9.049ns  (26.7% logic, 73.3% route), 6 logic levels.

 Constraint Details:

      9.049ns physical path delay SLICE_3 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 6.770ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C3C.CLK to       R8C3C.Q0 SLICE_3 (from RCLK_c)
ROUTE         3     1.870       R8C3C.Q0 to       R8C4B.C1 FS[12]
CTOF_DEL    ---     0.371       R8C4B.C1 to       R8C4B.F1 SLICE_86
ROUTE         1     0.694       R8C4B.F1 to       R7C4A.D1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371       R7C4A.D1 to       R7C4A.F1 SLICE_69
ROUTE         4     1.192       R7C4A.F1 to       R6C5D.D1 N_128
CTOF_DEL    ---     0.371       R6C5D.D1 to       R6C5D.F1 SLICE_58
ROUTE         3     1.723       R6C5D.F1 to       R3C5A.C0 N_94
CTOF_DEL    ---     0.371       R3C5A.C0 to       R3C5A.F0 SLICE_55
ROUTE         1     1.155       R3C5A.F0 to       R7C5B.D0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R7C5B.D0 to       R7C5B.F0 SLICE_52
ROUTE         1     0.000       R7C5B.F0 to      R7C5B.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    9.049   (26.7% logic, 73.3% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C3C.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R7C5B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.278ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[10]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               8.541ns  (23.9% logic, 76.1% route), 5 logic levels.

 Constraint Details:

      8.541ns physical path delay SLICE_4 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.278ns

 Physical Path Details:

      Data path SLICE_4 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C3B.CLK to       R8C3B.Q0 SLICE_4 (from RCLK_c)
ROUTE         5     1.886       R8C3B.Q0 to       R7C3C.C1 FS[10]
CTOF_DEL    ---     0.371       R7C3C.C1 to       R7C3C.F1 SLICE_94
ROUTE         1     1.840       R7C3C.F1 to       R7C4B.C1 UFMSDI_ens2_i_a2_4_2
CTOF_DEL    ---     0.371       R7C4B.C1 to       R7C4B.F1 SLICE_32
ROUTE         1     1.616       R7C4B.F1 to       R3C5A.D0 UFMSDI_ens2_i_a0
CTOF_DEL    ---     0.371       R3C5A.D0 to       R3C5A.F0 SLICE_55
ROUTE         1     1.155       R3C5A.F0 to       R7C5B.D0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R7C5B.D0 to       R7C5B.F0 SLICE_52
ROUTE         1     0.000       R7C5B.F0 to      R7C5B.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    8.541   (23.9% logic, 76.1% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_4:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C3B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R7C5B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.584ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[15]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               8.235ns  (29.3% logic, 70.7% route), 6 logic levels.

 Constraint Details:

      8.235ns physical path delay SLICE_2 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.584ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C3D.CLK to       R8C3D.Q1 SLICE_2 (from RCLK_c)
ROUTE         3     1.056       R8C3D.Q1 to       R8C4B.A1 FS[15]
CTOF_DEL    ---     0.371       R8C4B.A1 to       R8C4B.F1 SLICE_86
ROUTE         1     0.694       R8C4B.F1 to       R7C4A.D1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371       R7C4A.D1 to       R7C4A.F1 SLICE_69
ROUTE         4     1.192       R7C4A.F1 to       R6C5D.D1 N_128
CTOF_DEL    ---     0.371       R6C5D.D1 to       R6C5D.F1 SLICE_58
ROUTE         3     1.723       R6C5D.F1 to       R3C5A.C0 N_94
CTOF_DEL    ---     0.371       R3C5A.C0 to       R3C5A.F0 SLICE_55
ROUTE         1     1.155       R3C5A.F0 to       R7C5B.D0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R7C5B.D0 to       R7C5B.F0 SLICE_52
ROUTE         1     0.000       R7C5B.F0 to      R7C5B.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    8.235   (29.3% logic, 70.7% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C3D.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R7C5B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.591ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[17]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               8.228ns  (29.4% logic, 70.6% route), 6 logic levels.

 Constraint Details:

      8.228ns physical path delay SLICE_1 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.591ns

 Physical Path Details:

      Data path SLICE_1 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C4A.CLK to       R8C4A.Q1 SLICE_1 (from RCLK_c)
ROUTE         3     1.049       R8C4A.Q1 to       R8C4B.B1 FS[17]
CTOF_DEL    ---     0.371       R8C4B.B1 to       R8C4B.F1 SLICE_86
ROUTE         1     0.694       R8C4B.F1 to       R7C4A.D1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371       R7C4A.D1 to       R7C4A.F1 SLICE_69
ROUTE         4     1.192       R7C4A.F1 to       R6C5D.D1 N_128
CTOF_DEL    ---     0.371       R6C5D.D1 to       R6C5D.F1 SLICE_58
ROUTE         3     1.723       R6C5D.F1 to       R3C5A.C0 N_94
CTOF_DEL    ---     0.371       R3C5A.C0 to       R3C5A.F0 SLICE_55
ROUTE         1     1.155       R3C5A.F0 to       R7C5B.D0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R7C5B.D0 to       R7C5B.F0 SLICE_52
ROUTE         1     0.000       R7C5B.F0 to      R7C5B.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    8.228   (29.4% logic, 70.6% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_1:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C4A.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R7C5B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.610ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[12]  (from RCLK_c +)
   Destination:    FF         Data in        n8MEGEN  (to RCLK_c +)

   Delay:               8.146ns  (25.1% logic, 74.9% route), 5 logic levels.

 Constraint Details:

      8.146ns physical path delay SLICE_3 to SLICE_58 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.244ns CE_SET requirement (totaling 15.756ns) by 7.610ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_58:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C3C.CLK to       R8C3C.Q0 SLICE_3 (from RCLK_c)
ROUTE         3     1.870       R8C3C.Q0 to       R8C4B.C1 FS[12]
CTOF_DEL    ---     0.371       R8C4B.C1 to       R8C4B.F1 SLICE_86
ROUTE         1     0.694       R8C4B.F1 to       R7C4A.D1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371       R7C4A.D1 to       R7C4A.F1 SLICE_69
ROUTE         4     1.192       R7C4A.F1 to       R6C5D.D1 N_128
CTOF_DEL    ---     0.371       R6C5D.D1 to       R6C5D.F1 SLICE_58
ROUTE         3     0.716       R6C5D.F1 to       R7C5C.D0 N_94
CTOF_DEL    ---     0.371       R7C5C.D0 to       R7C5C.F0 SLICE_71
ROUTE         1     1.630       R7C5C.F0 to       R6C5D.CE N_24 (to RCLK_c)
                  --------
                    8.146   (25.1% logic, 74.9% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C3C.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_58:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R6C5D.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.734ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[12]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               8.085ns  (29.9% logic, 70.1% route), 6 logic levels.

 Constraint Details:

      8.085ns physical path delay SLICE_3 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.734ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C3C.CLK to       R8C3C.Q0 SLICE_3 (from RCLK_c)
ROUTE         3     1.870       R8C3C.Q0 to       R8C4B.C1 FS[12]
CTOF_DEL    ---     0.371       R8C4B.C1 to       R8C4B.F1 SLICE_86
ROUTE         1     0.694       R8C4B.F1 to       R7C4A.D1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371       R7C4A.D1 to       R7C4A.F1 SLICE_69
ROUTE         4     0.335       R7C4A.F1 to       R7C4B.D1 N_128
CTOF_DEL    ---     0.371       R7C4B.D1 to       R7C4B.F1 SLICE_32
ROUTE         1     1.616       R7C4B.F1 to       R3C5A.D0 UFMSDI_ens2_i_a0
CTOF_DEL    ---     0.371       R3C5A.D0 to       R3C5A.F0 SLICE_55
ROUTE         1     1.155       R3C5A.F0 to       R7C5B.D0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R7C5B.D0 to       R7C5B.F0 SLICE_52
ROUTE         1     0.000       R7C5B.F0 to      R7C5B.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    8.085   (29.9% logic, 70.1% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C3C.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R7C5B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.924ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[14]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               7.895ns  (30.6% logic, 69.4% route), 6 logic levels.

 Constraint Details:

      7.895ns physical path delay SLICE_2 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.924ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C3D.CLK to       R8C3D.Q0 SLICE_2 (from RCLK_c)
ROUTE         3     0.716       R8C3D.Q0 to       R8C4B.D1 FS[14]
CTOF_DEL    ---     0.371       R8C4B.D1 to       R8C4B.F1 SLICE_86
ROUTE         1     0.694       R8C4B.F1 to       R7C4A.D1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371       R7C4A.D1 to       R7C4A.F1 SLICE_69
ROUTE         4     1.192       R7C4A.F1 to       R6C5D.D1 N_128
CTOF_DEL    ---     0.371       R6C5D.D1 to       R6C5D.F1 SLICE_58
ROUTE         3     1.723       R6C5D.F1 to       R3C5A.C0 N_94
CTOF_DEL    ---     0.371       R3C5A.C0 to       R3C5A.F0 SLICE_55
ROUTE         1     1.155       R3C5A.F0 to       R7C5B.D0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R7C5B.D0 to       R7C5B.F0 SLICE_52
ROUTE         1     0.000       R7C5B.F0 to      R7C5B.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    7.895   (30.6% logic, 69.4% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C3D.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R7C5B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.974ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[12]  (from RCLK_c +)
   Destination:    FF         Data in        LEDEN  (to RCLK_c +)

   Delay:               7.782ns  (26.3% logic, 73.7% route), 5 logic levels.

 Constraint Details:

      7.782ns physical path delay SLICE_3 to SLICE_33 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.244ns CE_SET requirement (totaling 15.756ns) by 7.974ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C3C.CLK to       R8C3C.Q0 SLICE_3 (from RCLK_c)
ROUTE         3     1.870       R8C3C.Q0 to       R8C4B.C1 FS[12]
CTOF_DEL    ---     0.371       R8C4B.C1 to       R8C4B.F1 SLICE_86
ROUTE         1     0.694       R8C4B.F1 to       R7C4A.D1 UFMSDI_ens2_i_o2_0_3
CTOF_DEL    ---     0.371       R7C4A.D1 to       R7C4A.F1 SLICE_69
ROUTE         4     1.192       R7C4A.F1 to       R6C5D.D1 N_128
CTOF_DEL    ---     0.371       R6C5D.D1 to       R6C5D.F1 SLICE_58
ROUTE         3     0.909       R6C5D.F1 to       R7C5D.C0 N_94
CTOF_DEL    ---     0.371       R7C5D.C0 to       R7C5D.F0 SLICE_72
ROUTE         1     1.073       R7C5D.F0 to       R6C5B.CE N_26 (to RCLK_c)
                  --------
                    7.782   (26.3% logic, 73.7% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C3C.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_33:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R6C5B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 7.985ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[6]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               7.834ns  (26.1% logic, 73.9% route), 5 logic levels.

 Constraint Details:

      7.834ns physical path delay SLICE_6 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 7.985ns

 Physical Path Details:

      Data path SLICE_6 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C2D.CLK to       R8C2D.Q0 SLICE_6 (from RCLK_c)
ROUTE         3     1.179       R8C2D.Q0 to       R7C3C.D1 FS[6]
CTOF_DEL    ---     0.371       R7C3C.D1 to       R7C3C.F1 SLICE_94
ROUTE         1     1.840       R7C3C.F1 to       R7C4B.C1 UFMSDI_ens2_i_a2_4_2
CTOF_DEL    ---     0.371       R7C4B.C1 to       R7C4B.F1 SLICE_32
ROUTE         1     1.616       R7C4B.F1 to       R3C5A.D0 UFMSDI_ens2_i_a0
CTOF_DEL    ---     0.371       R3C5A.D0 to       R3C5A.F0 SLICE_55
ROUTE         1     1.155       R3C5A.F0 to       R7C5B.D0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R7C5B.D0 to       R7C5B.F0 SLICE_52
ROUTE         1     0.000       R7C5B.F0 to      R7C5B.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    7.834   (26.1% logic, 73.9% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_6:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C2D.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R7C5B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 8.032ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[11]  (from RCLK_c +)
   Destination:    FF         Data in        UFMSDI  (to RCLK_c +)

   Delay:               7.787ns  (26.2% logic, 73.8% route), 5 logic levels.

 Constraint Details:

      7.787ns physical path delay SLICE_4 to SLICE_52 meets
     16.000ns delay constraint less
      0.000ns skew and
      0.181ns DIN_SET requirement (totaling 15.819ns) by 8.032ns

 Physical Path Details:

      Data path SLICE_4 to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.560      R8C3B.CLK to       R8C3B.Q1 SLICE_4 (from RCLK_c)
ROUTE         6     1.132       R8C3B.Q1 to       R7C3C.B1 FS[11]
CTOF_DEL    ---     0.371       R7C3C.B1 to       R7C3C.F1 SLICE_94
ROUTE         1     1.840       R7C3C.F1 to       R7C4B.C1 UFMSDI_ens2_i_a2_4_2
CTOF_DEL    ---     0.371       R7C4B.C1 to       R7C4B.F1 SLICE_32
ROUTE         1     1.616       R7C4B.F1 to       R3C5A.D0 UFMSDI_ens2_i_a0
CTOF_DEL    ---     0.371       R3C5A.D0 to       R3C5A.F0 SLICE_55
ROUTE         1     1.155       R3C5A.F0 to       R7C5B.D0 UFMSDI_r_xx_mm_1
CTOF_DEL    ---     0.371       R7C5B.D0 to       R7C5B.F0 SLICE_52
ROUTE         1     0.000       R7C5B.F0 to      R7C5B.DI0 UFMSDI_RNO (to RCLK_c)
                  --------
                    7.787   (26.2% logic, 73.8% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_4:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R8C3B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_52:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     1.353       86.PADDI to      R7C5B.CLK RCLK_c
                  --------
                    1.353   (0.0% logic, 100.0% route), 0 logic levels.

Report:  108.342MHz is the maximum frequency for this preference.

Report Summary
--------------
----------------------------------------------------------------------------
Preference                              |   Constraint|       Actual|Levels
----------------------------------------------------------------------------
                                        |             |             |
FREQUENCY PORT "PHI2" 2.900000 MHz ;    |    2.900 MHz|   47.219 MHz|   7  
                                        |             |             |
FREQUENCY PORT "nCCAS" 2.900000 MHz ;   |    2.900 MHz|  400.000 MHz|   0  
                                        |             |             |
FREQUENCY PORT "nCRAS" 2.900000 MHz ;   |    2.900 MHz|  400.000 MHz|   0  
                                        |             |             |
FREQUENCY PORT "RCLK" 62.500000 MHz ;   |   62.500 MHz|  108.342 MHz|   6  
                                        |             |             |
----------------------------------------------------------------------------


All preferences were met.


Clock Domains Analysis
------------------------

Found 4 clocks:

Clock Domain: nCRAS_c   Source: nCRAS.PAD   Loads: 10
   No transfer within this clock domain is found

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: nCCAS_c   Source: nCCAS.PAD   Loads: 8
   No transfer within this clock domain is found

Clock Domain: RCLK_c   Source: RCLK.PAD   Loads: 32
   Covered under: FREQUENCY PORT "RCLK" 62.500000 MHz ;

   Data transfers from:
   Clock Domain: nCRAS_c   Source: nCRAS.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

   Clock Domain: PHI2_c   Source: PHI2.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: PHI2_c   Source: PHI2.PAD   Loads: 15
   Covered under: FREQUENCY PORT "PHI2" 2.900000 MHz ;

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.


Timing summary (Setup):
---------------

Timing errors: 0  Score: 0
Cumulative negative slack: 0

Constraints cover 560 paths, 4 nets, and 447 connections (65.64% coverage)

--------------------------------------------------------------------------------
Lattice TRACE Report - Hold, Version Diamond (64-bit) 3.12.1.454
Sat Jan 06 06:25:12 2024

Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
Copyright (c) 1995 AT&T Corp.   All rights reserved.
Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
Copyright (c) 2001 Agere Systems   All rights reserved.
Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.

Report Information
------------------
Command line:    trce -v 10 -gt -sethld -sp 3 -sphld m -o RAM2GS_LCMXO256C_impl1.twr -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO256C/promote.xml RAM2GS_LCMXO256C_impl1.ncd RAM2GS_LCMXO256C_impl1.prf 
Design file:     ram2gs_lcmxo256c_impl1.ncd
Preference file: ram2gs_lcmxo256c_impl1.prf
Device,speed:    LCMXO256C,m
Report level:    verbose report, limited to 10 items per preference
--------------------------------------------------------------------------------

BLOCK ASYNCPATHS
BLOCK RESETPATHS
--------------------------------------------------------------------------------



================================================================================
Preference: FREQUENCY PORT "PHI2" 2.900000 MHz ;
            168 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 0.358ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              ADSubmitted  (from PHI2_c -)
   Destination:    FF         Data in        ADSubmitted  (to PHI2_c -)

   Delay:               0.339ns  (62.2% logic, 37.8% route), 2 logic levels.

 Constraint Details:

      0.339ns physical path delay SLICE_9 to SLICE_9 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.358ns

 Physical Path Details:

      Data path SLICE_9 to SLICE_9:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R5C3A.CLK to       R5C3A.Q0 SLICE_9 (from PHI2_c)
ROUTE         2     0.128       R5C3A.Q0 to       R5C3A.D0 ADSubmitted
CTOF_DEL    ---     0.074       R5C3A.D0 to       R5C3A.F0 SLICE_9
ROUTE         1     0.000       R5C3A.F0 to      R5C3A.DI0 ADSubmitted_r (to PHI2_c)
                  --------
                    0.339   (62.2% logic, 37.8% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_9:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C3A.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_9:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C3A.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.364ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdSubmitted  (from PHI2_c -)
   Destination:    FF         Data in        CmdSubmitted  (to PHI2_c -)

   Delay:               0.345ns  (61.2% logic, 38.8% route), 2 logic levels.

 Constraint Details:

      0.345ns physical path delay SLICE_22 to SLICE_22 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.364ns

 Physical Path Details:

      Data path SLICE_22 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R6C5C.CLK to       R6C5C.Q0 SLICE_22 (from PHI2_c)
ROUTE         3     0.134       R6C5C.Q0 to       R6C5C.A0 CmdSubmitted
CTOF_DEL    ---     0.074       R6C5C.A0 to       R6C5C.F0 SLICE_22
ROUTE         1     0.000       R6C5C.F0 to      R6C5C.DI0 N_428_0 (to PHI2_c)
                  --------
                    0.345   (61.2% logic, 38.8% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C5C.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_22:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C5C.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.399ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              C1Submitted  (from PHI2_c -)
   Destination:    FF         Data in        C1Submitted  (to PHI2_c -)

   Delay:               0.380ns  (55.5% logic, 44.5% route), 2 logic levels.

 Constraint Details:

      0.380ns physical path delay SLICE_14 to SLICE_14 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.399ns

 Physical Path Details:

      Data path SLICE_14 to SLICE_14:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R6C3A.CLK to       R6C3A.Q0 SLICE_14 (from PHI2_c)
ROUTE         2     0.169       R6C3A.Q0 to       R6C3A.C0 C1Submitted
CTOF_DEL    ---     0.074       R6C3A.C0 to       R6C3A.F0 SLICE_14
ROUTE         1     0.000       R6C3A.F0 to      R6C3A.DI0 C1Submitted_RNO (to PHI2_c)
                  --------
                    0.380   (55.5% logic, 44.5% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_14:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C3A.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_14:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C3A.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.438ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdEnable  (from PHI2_c -)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               0.419ns  (50.4% logic, 49.6% route), 2 logic levels.

 Constraint Details:

      0.419ns physical path delay SLICE_20 to SLICE_20 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.438ns

 Physical Path Details:

      Data path SLICE_20 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R5C3C.CLK to       R5C3C.Q0 SLICE_20 (from PHI2_c)
ROUTE         2     0.208       R5C3C.Q0 to       R5C3C.B0 CmdEnable
CTOF_DEL    ---     0.074       R5C3C.B0 to       R5C3C.F0 SLICE_20
ROUTE         1     0.000       R5C3C.F0 to      R5C3C.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    0.419   (50.4% logic, 49.6% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.572ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Cmdn8MEGEN  (from PHI2_c -)
   Destination:    FF         Data in        Cmdn8MEGEN  (to PHI2_c -)

   Delay:               0.553ns  (51.5% logic, 48.5% route), 3 logic levels.

 Constraint Details:

      0.553ns physical path delay SLICE_26 to SLICE_26 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.572ns

 Physical Path Details:

      Data path SLICE_26 to SLICE_26:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R6C4C.CLK to       R6C4C.Q0 SLICE_26 (from PHI2_c)
ROUTE         2     0.169       R6C4C.Q0 to       R6C4C.C1 Cmdn8MEGEN
CTOF_DEL    ---     0.074       R6C4C.C1 to       R6C4C.F1 SLICE_26
ROUTE         1     0.099       R6C4C.F1 to       R6C4C.C0 Cmdn8MEGEN_4_u_i_0
CTOF_DEL    ---     0.074       R6C4C.C0 to       R6C4C.F0 SLICE_26
ROUTE         1     0.000       R6C4C.F0 to      R6C4C.DI0 N_12_i (to PHI2_c)
                  --------
                    0.553   (51.5% logic, 48.5% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_26:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C4C.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_26:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C4C.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.599ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdLEDEN  (from PHI2_c -)
   Destination:    FF         Data in        CmdLEDEN  (to PHI2_c -)

   Delay:               0.580ns  (49.1% logic, 50.9% route), 3 logic levels.

 Constraint Details:

      0.580ns physical path delay SLICE_21 to SLICE_21 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.599ns

 Physical Path Details:

      Data path SLICE_21 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R6C4D.CLK to       R6C4D.Q0 SLICE_21 (from PHI2_c)
ROUTE         2     0.196       R6C4D.Q0 to       R6C4D.A1 CmdLEDEN
CTOF_DEL    ---     0.074       R6C4D.A1 to       R6C4D.F1 SLICE_21
ROUTE         1     0.099       R6C4D.F1 to       R6C4D.C0 CmdLEDEN_4_u_i_0
CTOF_DEL    ---     0.074       R6C4D.C0 to       R6C4D.F0 SLICE_21
ROUTE         1     0.000       R6C4D.F0 to      R6C4D.DI0 N_14_i (to PHI2_c)
                  --------
                    0.580   (49.1% logic, 50.9% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C4D.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C4D.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.609ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              ADSubmitted  (from PHI2_c -)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               0.590ns  (48.3% logic, 51.7% route), 3 logic levels.

 Constraint Details:

      0.590ns physical path delay SLICE_9 to SLICE_20 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.609ns

 Physical Path Details:

      Data path SLICE_9 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R5C3A.CLK to       R5C3A.Q0 SLICE_9 (from PHI2_c)
ROUTE         2     0.206       R5C3A.Q0 to       R5C3C.B1 ADSubmitted
CTOF_DEL    ---     0.074       R5C3C.B1 to       R5C3C.F1 SLICE_20
ROUTE         1     0.099       R5C3C.F1 to       R5C3C.C0 CmdEnable_0_sqmuxa
CTOF_DEL    ---     0.074       R5C3C.C0 to       R5C3C.F0 SLICE_20
ROUTE         1     0.000       R5C3C.F0 to      R5C3C.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    0.590   (48.3% logic, 51.7% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_9:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C3A.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.611ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              XOR8MEG  (from PHI2_c -)
   Destination:    FF         Data in        XOR8MEG  (to PHI2_c -)

   Delay:               0.592ns  (48.1% logic, 51.9% route), 3 logic levels.

 Constraint Details:

      0.592ns physical path delay SLICE_57 to SLICE_57 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.611ns

 Physical Path Details:

      Data path SLICE_57 to SLICE_57:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R5C4D.CLK to       R5C4D.Q0 SLICE_57 (from PHI2_c)
ROUTE         2     0.208       R5C4D.Q0 to       R5C4D.B1 XOR8MEG
CTOF_DEL    ---     0.074       R5C4D.B1 to       R5C4D.F1 SLICE_57
ROUTE         1     0.099       R5C4D.F1 to       R5C4D.C0 N_166
CTOF_DEL    ---     0.074       R5C4D.C0 to       R5C4D.F0 SLICE_57
ROUTE         1     0.000       R5C4D.F0 to      R5C4D.DI0 XOR8MEG_3 (to PHI2_c)
                  --------
                    0.592   (48.1% logic, 51.9% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_57:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C4D.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_57:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C4D.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.641ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              C1Submitted  (from PHI2_c -)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               0.622ns  (45.8% logic, 54.2% route), 3 logic levels.

 Constraint Details:

      0.622ns physical path delay SLICE_14 to SLICE_20 meets
     -0.019ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.641ns

 Physical Path Details:

      Data path SLICE_14 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R6C3A.CLK to       R6C3A.Q0 SLICE_14 (from PHI2_c)
ROUTE         2     0.130       R6C3A.Q0 to       R6C3A.D1 C1Submitted
CTOF_DEL    ---     0.074       R6C3A.D1 to       R6C3A.F1 SLICE_14
ROUTE         1     0.207       R6C3A.F1 to       R5C3C.A0 un1_CmdEnable20_i
CTOF_DEL    ---     0.074       R5C3C.A0 to       R5C3C.F0 SLICE_20
ROUTE         1     0.000       R5C3C.F0 to      R5C3C.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    0.622   (45.8% logic, 54.2% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_14:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C3A.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.687ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdEnable  (from PHI2_c -)
   Destination:    FF         Data in        CmdLEDEN  (to PHI2_c -)

   Delay:               0.664ns  (31.8% logic, 68.2% route), 2 logic levels.

 Constraint Details:

      0.664ns physical path delay SLICE_20 to SLICE_21 meets
     -0.023ns CE_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.023ns) by 0.687ns

 Physical Path Details:

      Data path SLICE_20 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.137      R5C3C.CLK to       R5C3C.Q0 SLICE_20 (from PHI2_c)
ROUTE         2     0.130       R5C3C.Q0 to       R5C3B.D0 CmdEnable
CTOF_DEL    ---     0.074       R5C3B.D0 to       R5C3B.F0 SLICE_73
ROUTE         5     0.323       R5C3B.F0 to       R6C4D.CE XOR8MEG18 (to PHI2_c)
                  --------
                    0.664   (31.8% logic, 68.2% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R5C3C.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        15     0.967       39.PADDI to      R6C4D.CLK PHI2_c
                  --------
                    0.967   (0.0% logic, 100.0% route), 0 logic levels.


================================================================================
Preference: FREQUENCY PORT "nCCAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


================================================================================
Preference: FREQUENCY PORT "nCRAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


================================================================================
Preference: FREQUENCY PORT "RCLK" 62.500000 MHz ;
            392 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 0.273ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CASr  (from RCLK_c +)
   Destination:    FF         Data in        CASr2  (to RCLK_c +)

   Delay:               0.256ns  (49.2% logic, 50.8% route), 1 logic levels.

 Constraint Details:

      0.256ns physical path delay SLICE_74 to SLICE_74 meets
     -0.017ns M_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.017ns) by 0.273ns

 Physical Path Details:

      Data path SLICE_74 to SLICE_74:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R6C3D.CLK to       R6C3D.Q0 SLICE_74 (from RCLK_c)
ROUTE         1     0.130       R6C3D.Q0 to       R6C3D.M1 CASr (to RCLK_c)
                  --------
                    0.256   (49.2% logic, 50.8% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_74:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R6C3D.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_74:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R6C3D.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.275ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              RASr  (from RCLK_c +)
   Destination:    FF         Data in        RASr2  (to RCLK_c +)

   Delay:               0.258ns  (48.8% logic, 51.2% route), 1 logic levels.

 Constraint Details:

      0.258ns physical path delay SLICE_95 to SLICE_95 meets
     -0.017ns M_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.017ns) by 0.275ns

 Physical Path Details:

      Data path SLICE_95 to SLICE_95:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R2C4A.CLK to       R2C4A.Q0 SLICE_95 (from RCLK_c)
ROUTE         2     0.132       R2C4A.Q0 to       R2C4A.M1 RASr (to RCLK_c)
                  --------
                    0.258   (48.8% logic, 51.2% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_95:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R2C4A.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_95:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R2C4A.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[15]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[14]  (to RCLK_c +)
                   FF                        FS[15]
                   FF                        FS[14]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_2 to SLICE_2 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R8C3D.CLK to       R8C3D.Q1 SLICE_2 (from RCLK_c)
ROUTE         3     0.131       R8C3D.Q1 to       R8C3D.A1 FS[15] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3D.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3D.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[13]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[12]  (to RCLK_c +)
                   FF                        FS[13]
                   FF                        FS[12]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_3 to SLICE_3 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R8C3C.CLK to       R8C3C.Q1 SLICE_3 (from RCLK_c)
ROUTE         4     0.131       R8C3C.Q1 to       R8C3C.A1 FS[13] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3C.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3C.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[9]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[8]  (to RCLK_c +)
                   FF                        FS[9]
                   FF                        FS[8]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_5 to SLICE_5 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_5 to SLICE_5:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R8C3A.CLK to       R8C3A.Q1 SLICE_5 (from RCLK_c)
ROUTE         3     0.131       R8C3A.Q1 to       R8C3A.A1 FS[9] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_5:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3A.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_5:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3A.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[7]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[6]  (to RCLK_c +)
                   FF                        FS[7]
                   FF                        FS[6]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_6 to SLICE_6 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_6 to SLICE_6:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R8C2D.CLK to       R8C2D.Q1 SLICE_6 (from RCLK_c)
ROUTE         3     0.131       R8C2D.Q1 to       R8C2D.A1 FS[7] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_6:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C2D.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_6:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C2D.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.301ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[3]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[2]  (to RCLK_c +)
                   FF                        FS[3]
                   FF                        FS[2]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_8 to SLICE_8 meets
     -0.044ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.044ns) by 0.301ns

 Physical Path Details:

      Data path SLICE_8 to SLICE_8:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R8C2B.CLK to       R8C2B.Q1 SLICE_8 (from RCLK_c)
ROUTE         2     0.131       R8C2B.Q1 to       R8C2B.A1 FS[3] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_8:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C2B.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_8:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C2B.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.302ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[0]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[0]  (to RCLK_c +)
                   FF                        FS[1]
                   FF                        FS[0]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_0 to SLICE_0 meets
     -0.045ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.045ns) by 0.302ns

 Physical Path Details:

      Data path SLICE_0 to SLICE_0:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R8C2A.CLK to       R8C2A.Q0 SLICE_0 (from RCLK_c)
ROUTE         2     0.131       R8C2A.Q0 to       R8C2A.A0 FS[0] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_0:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C2A.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_0:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C2A.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.302ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[14]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[14]  (to RCLK_c +)
                   FF                        FS[15]
                   FF                        FS[14]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_2 to SLICE_2 meets
     -0.045ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.045ns) by 0.302ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R8C3D.CLK to       R8C3D.Q0 SLICE_2 (from RCLK_c)
ROUTE         3     0.131       R8C3D.Q0 to       R8C3D.A0 FS[14] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3D.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3D.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.302ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[12]  (from RCLK_c +)
   Destination:    FF         Data in        FS_cry_0[12]  (to RCLK_c +)
                   FF                        FS[13]
                   FF                        FS[12]

   Delay:               0.257ns  (49.0% logic, 51.0% route), 1 logic levels.

 Constraint Details:

      0.257ns physical path delay SLICE_3 to SLICE_3 meets
     -0.045ns LUT_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.045ns) by 0.302ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.126      R8C3C.CLK to       R8C3C.Q0 SLICE_3 (from RCLK_c)
ROUTE         3     0.131       R8C3C.Q0 to       R8C3C.A0 FS[12] (to RCLK_c)
                  --------
                    0.257   (49.0% logic, 51.0% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3C.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        32     0.333       86.PADDI to      R8C3C.CLK RCLK_c
                  --------
                    0.333   (0.0% logic, 100.0% route), 0 logic levels.

Report Summary
--------------
----------------------------------------------------------------------------
Preference(MIN Delays)                  |   Constraint|       Actual|Levels
----------------------------------------------------------------------------
                                        |             |             |
FREQUENCY PORT "PHI2" 2.900000 MHz ;    |            -|            -|   2  
                                        |             |             |
FREQUENCY PORT "nCCAS" 2.900000 MHz ;   |            -|            -|   0  
                                        |             |             |
FREQUENCY PORT "nCRAS" 2.900000 MHz ;   |            -|            -|   0  
                                        |             |             |
FREQUENCY PORT "RCLK" 62.500000 MHz ;   |            -|            -|   1  
                                        |             |             |
----------------------------------------------------------------------------


All preferences were met.


Clock Domains Analysis
------------------------

Found 4 clocks:

Clock Domain: nCRAS_c   Source: nCRAS.PAD   Loads: 10
   No transfer within this clock domain is found

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: nCCAS_c   Source: nCCAS.PAD   Loads: 8
   No transfer within this clock domain is found

Clock Domain: RCLK_c   Source: RCLK.PAD   Loads: 32
   Covered under: FREQUENCY PORT "RCLK" 62.500000 MHz ;

   Data transfers from:
   Clock Domain: nCRAS_c   Source: nCRAS.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

   Clock Domain: PHI2_c   Source: PHI2.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: PHI2_c   Source: PHI2.PAD   Loads: 15
   Covered under: FREQUENCY PORT "PHI2" 2.900000 MHz ;

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.


Timing summary (Hold):
---------------

Timing errors: 0  Score: 0
Cumulative negative slack: 0

Constraints cover 560 paths, 4 nets, and 447 connections (65.64% coverage)



Timing summary (Setup and Hold):
---------------

Timing errors: 0 (setup), 0 (hold)
Score: 0 (setup), 0 (hold)
Cumulative negative slack: 0 (0+0)
--------------------------------------------------------------------------------

--------------------------------------------------------------------------------

