Loading design for application iotiming from file ram2gs_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: 5
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2gs_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: 6
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
Loading design for application iotiming from file ram2gs_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: M
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
// Design: RAM2GS
// Package: TQFP100
// ncd File: ram2gs_lcmxo2_1200hc_impl1.ncd
// Version: Diamond (64-bit) 3.12.1.454
// Written on Sat Nov 18 02:06:17 2023
// M: Minimum Performance Grade
// iotiming RAM2GS_LCMXO2_1200HC_impl1.ncd RAM2GS_LCMXO2_1200HC_impl1.prf -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO2-1200HC/promote.xml

I/O Timing Report (All units are in ns)

Worst Case Results across Performance Grades (M, 6, 5, 4):

// Input Setup and Hold Times

Port    Clock Edge  Setup Performance_Grade  Hold Performance_Grade
----------------------------------------------------------------------
CROW[0] nCRAS F     3.288      4      -0.390     M
CROW[1] nCRAS F     2.823      4      -0.285     M
Din[0]  PHI2  F     6.398      4       4.293     4
Din[0]  nCCAS F     1.411      4      -0.004     M
Din[1]  PHI2  F     3.916      4       4.173     4
Din[1]  nCCAS F     1.877      4      -0.123     M
Din[2]  PHI2  F     6.180      4       4.173     4
Din[2]  nCCAS F     1.548      4      -0.062     M
Din[3]  PHI2  F     5.536      4       4.173     4
Din[3]  nCCAS F     0.467      4       0.734     4
Din[4]  PHI2  F     3.611      4       4.173     4
Din[4]  nCCAS F     1.533      4      -0.043     M
Din[5]  PHI2  F     5.673      4       4.173     4
Din[5]  nCCAS F     1.663      4      -0.072     M
Din[6]  PHI2  F     5.355      4       4.293     4
Din[6]  nCCAS F     2.807      4      -0.352     M
Din[7]  PHI2  F     5.296      4       4.293     4
Din[7]  nCCAS F     1.914      4      -0.136     M
MAin[0] PHI2  F     4.091      4       1.414     4
MAin[0] nCRAS F     1.207      4       0.347     4
MAin[1] PHI2  F     3.273      4       1.759     4
MAin[1] nCRAS F     1.077      4       0.460     4
MAin[2] PHI2  F     8.126      4      -0.351     M
MAin[2] nCRAS F     0.671      4       0.850     4
MAin[3] PHI2  F     8.831      4      -0.579     M
MAin[3] nCRAS F     1.100      4       0.463     4
MAin[4] PHI2  F     8.415      4      -0.447     M
MAin[4] nCRAS F     1.390      4       0.207     4
MAin[5] PHI2  F     9.742      4      -0.803     M
MAin[5] nCRAS F     1.269      4       0.218     4
MAin[6] PHI2  F     7.970      4      -0.325     M
MAin[6] nCRAS F     1.165      4       0.337     4
MAin[7] PHI2  F     8.481      4      -0.438     M
MAin[7] nCRAS F     0.761      4       0.673     4
MAin[8] nCRAS F     1.261      4       0.223     4
MAin[9] nCRAS F     0.756      4       0.667     4
PHI2    RCLK  R    -0.133      M       2.360     4
nCCAS   RCLK  R     4.128      4      -0.675     M
nCCAS   nCRAS F     4.568      4      -0.666     M
nCRAS   RCLK  R     3.070      4      -0.412     M
nFWE    PHI2  F     8.979      4      -0.603     M
nFWE    nCRAS F     1.467      4       0.144     4


// Clock to Output Delay

Port    Clock Edge  Max_Delay Performance_Grade  Min_Delay Performance_Grade
------------------------------------------------------------------------
LED     RCLK  R    11.034         4        3.119          M
LED     nCRAS F    11.531         4        3.339          M
RA[0]   RCLK  R    11.682         4        3.586          M
RA[0]   nCRAS F    11.704         4        3.483          M
RA[10]  RCLK  R     7.888         4        2.711          M
RA[11]  PHI2  R     9.755         4        3.200          M
RA[1]   RCLK  R    11.454         4        3.535          M
RA[1]   nCRAS F    11.216         4        3.347          M
RA[2]   RCLK  R    12.084         4        3.693          M
RA[2]   nCRAS F    11.742         4        3.501          M
RA[3]   RCLK  R    12.131         4        3.715          M
RA[3]   nCRAS F    11.857         4        3.533          M
RA[4]   RCLK  R    11.966         4        3.684          M
RA[4]   nCRAS F    12.319         4        3.650          M
RA[5]   RCLK  R    11.928         4        3.670          M
RA[5]   nCRAS F    11.637         4        3.446          M
RA[6]   RCLK  R    11.419         4        3.523          M
RA[6]   nCRAS F    11.718         4        3.486          M
RA[7]   RCLK  R    11.988         4        3.651          M
RA[7]   nCRAS F    12.274         4        3.636          M
RA[8]   RCLK  R    11.660         4        3.582          M
RA[8]   nCRAS F    11.098         4        3.343          M
RA[9]   RCLK  R    11.454         4        3.547          M
RA[9]   nCRAS F    11.134         4        3.314          M
RBA[0]  nCRAS F     8.903         4        2.891          M
RBA[1]  nCRAS F     8.883         4        2.898          M
RCKE    RCLK  R     9.774         4        3.159          M
RCLKout RCLK  R     7.101         4        2.108          M
RDQMH   RCLK  R    10.733         4        3.351          M
RDQML   RCLK  R    10.683         4        3.364          M
RD[0]   nCCAS F     8.977         4        3.012          M
RD[1]   nCCAS F     8.977         4        3.012          M
RD[2]   nCCAS F     8.977         4        3.012          M
RD[3]   nCCAS F     8.977         4        3.012          M
RD[4]   nCCAS F     8.977         4        3.012          M
RD[5]   nCCAS F     8.977         4        3.012          M
RD[6]   nCCAS F     8.977         4        3.012          M
RD[7]   nCCAS F     8.977         4        3.012          M
nRCAS   RCLK  R     7.822         4        2.706          M
nRCS    RCLK  R     7.822         4        2.706          M
nRRAS   RCLK  R     7.822         4        2.706          M
nRWE    RCLK  R     7.803         4        2.713          M
WARNING: you must also run trce with hold speed: 4
WARNING: you must also run trce with setup speed: M
