
Loading design for application trce from file ram2gs_lcmxo2_1200hc_impl1.ncd.
Design name: RAM2GS
NCD version: 3.3
Vendor:      LATTICE
Device:      LCMXO2-1200HC
Package:     TQFP100
Performance: 4
Loading device for application trce from file 'xo2c1200.nph' in environment: C:/lscc/diamond/3.12/ispfpga.
Package Status:                     Final          Version 1.44.
Performance Hardware Data Status:   Final          Version 34.4.
Setup and Hold Report

--------------------------------------------------------------------------------
Lattice TRACE Report - Setup, Version Diamond (64-bit) 3.12.1.454
Sat Nov 18 02:06:13 2023

Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
Copyright (c) 1995 AT&T Corp.   All rights reserved.
Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
Copyright (c) 2001 Agere Systems   All rights reserved.
Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.

Report Information
------------------
Command line:    trce -v 10 -gt -sethld -sp 4 -sphld m -o RAM2GS_LCMXO2_1200HC_impl1.twr -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO2-1200HC/promote.xml RAM2GS_LCMXO2_1200HC_impl1.ncd RAM2GS_LCMXO2_1200HC_impl1.prf 
Design file:     ram2gs_lcmxo2_1200hc_impl1.ncd
Preference file: ram2gs_lcmxo2_1200hc_impl1.prf
Device,speed:    LCMXO2-1200HC,4
Report level:    verbose report, limited to 10 items per preference
--------------------------------------------------------------------------------

BLOCK ASYNCPATHS
BLOCK RESETPATHS
--------------------------------------------------------------------------------



================================================================================
Preference: FREQUENCY PORT "PHI2" 2.900000 MHz ;
            147 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 162.097ns (weighted slack = 324.194ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[7]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMData  (to PHI2_c -)

   Delay:               9.837ns  (26.0% logic, 74.0% route), 5 logic levels.

 Constraint Details:

      9.837ns physical path delay Din[7]_MGIOL to SLICE_19 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.307ns CE_SET requirement (totaling 171.934ns) by 162.097ns

 Physical Path Details:

      Data path Din[7]_MGIOL to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577    IOL_L2C.CLK to     IOL_L2C.IN Din[7]_MGIOL (from PHI2_c)
ROUTE         1     2.215     IOL_L2C.IN to      R4C10D.A0 Bank[7]
CTOF_DEL    ---     0.495      R4C10D.A0 to      R4C10D.F0 SLICE_90
ROUTE         1     0.958      R4C10D.F0 to       R2C9D.D0 un1_CmdEnable20_0_0_o2_10
CTOF_DEL    ---     0.495       R2C9D.D0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.104       R2C9D.F0 to       R5C9A.D1 N_367
CTOF_DEL    ---     0.495       R5C9A.D1 to       R5C9A.F1 SLICE_23
ROUTE         8     1.295       R5C9A.F1 to      R7C10B.C0 XOR8MEG18
CTOF_DEL    ---     0.495      R7C10B.C0 to      R7C10B.F0 SLICE_77
ROUTE         1     1.708      R7C10B.F0 to      R7C11B.CE CmdUFMData_1_sqmuxa (to PHI2_c)
                  --------
                    9.837   (26.0% logic, 74.0% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[7]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to    IOL_L2C.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to     R7C11B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 162.937ns (weighted slack = 325.874ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[1]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMData  (to PHI2_c -)

   Delay:               8.997ns  (28.4% logic, 71.6% route), 5 logic levels.

 Constraint Details:

      8.997ns physical path delay Din[1]_MGIOL to SLICE_19 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.307ns CE_SET requirement (totaling 171.934ns) by 162.937ns

 Physical Path Details:

      Data path Din[1]_MGIOL to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577   IOL_T10B.CLK to    IOL_T10B.IN Din[1]_MGIOL (from PHI2_c)
ROUTE         1     1.375    IOL_T10B.IN to      R4C10D.D0 Bank[1]
CTOF_DEL    ---     0.495      R4C10D.D0 to      R4C10D.F0 SLICE_90
ROUTE         1     0.958      R4C10D.F0 to       R2C9D.D0 un1_CmdEnable20_0_0_o2_10
CTOF_DEL    ---     0.495       R2C9D.D0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.104       R2C9D.F0 to       R5C9A.D1 N_367
CTOF_DEL    ---     0.495       R5C9A.D1 to       R5C9A.F1 SLICE_23
ROUTE         8     1.295       R5C9A.F1 to      R7C10B.C0 XOR8MEG18
CTOF_DEL    ---     0.495      R7C10B.C0 to      R7C10B.F0 SLICE_77
ROUTE         1     1.708      R7C10B.F0 to      R7C11B.CE CmdUFMData_1_sqmuxa (to PHI2_c)
                  --------
                    8.997   (28.4% logic, 71.6% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[1]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to   IOL_T10B.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to     R7C11B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 163.032ns (weighted slack = 326.064ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[6]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMData  (to PHI2_c -)

   Delay:               8.902ns  (28.7% logic, 71.3% route), 5 logic levels.

 Constraint Details:

      8.902ns physical path delay Din[6]_MGIOL to SLICE_19 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.307ns CE_SET requirement (totaling 171.934ns) by 163.032ns

 Physical Path Details:

      Data path Din[6]_MGIOL to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577    IOL_L2D.CLK to     IOL_L2D.IN Din[6]_MGIOL (from PHI2_c)
ROUTE         1     1.802     IOL_L2D.IN to       R2C9D.D1 Bank[6]
CTOF_DEL    ---     0.495       R2C9D.D1 to       R2C9D.F1 SLICE_80
ROUTE         1     0.436       R2C9D.F1 to       R2C9D.C0 un1_CmdEnable20_0_0_o2_11
CTOF_DEL    ---     0.495       R2C9D.C0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.104       R2C9D.F0 to       R5C9A.D1 N_367
CTOF_DEL    ---     0.495       R5C9A.D1 to       R5C9A.F1 SLICE_23
ROUTE         8     1.295       R5C9A.F1 to      R7C10B.C0 XOR8MEG18
CTOF_DEL    ---     0.495      R7C10B.C0 to      R7C10B.F0 SLICE_77
ROUTE         1     1.708      R7C10B.F0 to      R7C11B.CE CmdUFMData_1_sqmuxa (to PHI2_c)
                  --------
                    8.902   (28.7% logic, 71.3% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[6]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to    IOL_L2D.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to     R7C11B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 163.085ns (weighted slack = 326.170ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[7]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               8.990ns  (33.9% logic, 66.1% route), 6 logic levels.

 Constraint Details:

      8.990ns physical path delay Din[7]_MGIOL to SLICE_17 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.166ns DIN_SET requirement (totaling 172.075ns) by 163.085ns

 Physical Path Details:

      Data path Din[7]_MGIOL to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577    IOL_L2C.CLK to     IOL_L2C.IN Din[7]_MGIOL (from PHI2_c)
ROUTE         1     2.215     IOL_L2C.IN to      R4C10D.A0 Bank[7]
CTOF_DEL    ---     0.495      R4C10D.A0 to      R4C10D.F0 SLICE_90
ROUTE         1     0.958      R4C10D.F0 to       R2C9D.D0 un1_CmdEnable20_0_0_o2_10
CTOF_DEL    ---     0.495       R2C9D.D0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.048       R2C9D.F0 to       R4C9A.B1 N_367
CTOF_DEL    ---     0.495       R4C9A.B1 to       R4C9A.F1 SLICE_11
ROUTE         3     0.753       R4C9A.F1 to       R4C8A.C0 CmdEnable16
CTOF_DEL    ---     0.495       R4C8A.C0 to       R4C8A.F0 SLICE_33
ROUTE         1     0.964       R4C8A.F0 to       R4C9B.A0 CmdEnable_0_sqmuxa
CTOF_DEL    ---     0.495       R4C9B.A0 to       R4C9B.F0 SLICE_17
ROUTE         1     0.000       R4C9B.F0 to      R4C9B.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    8.990   (33.9% logic, 66.1% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[7]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to    IOL_L2C.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to      R4C9B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 163.118ns (weighted slack = 326.236ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[2]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMData  (to PHI2_c -)

   Delay:               8.816ns  (29.0% logic, 71.0% route), 5 logic levels.

 Constraint Details:

      8.816ns physical path delay Din[2]_MGIOL to SLICE_19 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.307ns CE_SET requirement (totaling 171.934ns) by 163.118ns

 Physical Path Details:

      Data path Din[2]_MGIOL to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577   IOL_T12A.CLK to    IOL_T12A.IN Din[2]_MGIOL (from PHI2_c)
ROUTE         1     1.716    IOL_T12A.IN to       R2C9D.A1 Bank[2]
CTOF_DEL    ---     0.495       R2C9D.A1 to       R2C9D.F1 SLICE_80
ROUTE         1     0.436       R2C9D.F1 to       R2C9D.C0 un1_CmdEnable20_0_0_o2_11
CTOF_DEL    ---     0.495       R2C9D.C0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.104       R2C9D.F0 to       R5C9A.D1 N_367
CTOF_DEL    ---     0.495       R5C9A.D1 to       R5C9A.F1 SLICE_23
ROUTE         8     1.295       R5C9A.F1 to      R7C10B.C0 XOR8MEG18
CTOF_DEL    ---     0.495      R7C10B.C0 to      R7C10B.F0 SLICE_77
ROUTE         1     1.708      R7C10B.F0 to      R7C11B.CE CmdUFMData_1_sqmuxa (to PHI2_c)
                  --------
                    8.816   (29.0% logic, 71.0% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[2]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to   IOL_T12A.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to     R7C11B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 163.196ns (weighted slack = 326.392ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[5]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMData  (to PHI2_c -)

   Delay:               8.738ns  (29.3% logic, 70.7% route), 5 logic levels.

 Constraint Details:

      8.738ns physical path delay Din[5]_MGIOL to SLICE_19 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.307ns CE_SET requirement (totaling 171.934ns) by 163.196ns

 Physical Path Details:

      Data path Din[5]_MGIOL to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577    IOL_T9B.CLK to     IOL_T9B.IN Din[5]_MGIOL (from PHI2_c)
ROUTE         1     1.638     IOL_T9B.IN to       R2C9D.B1 Bank[5]
CTOF_DEL    ---     0.495       R2C9D.B1 to       R2C9D.F1 SLICE_80
ROUTE         1     0.436       R2C9D.F1 to       R2C9D.C0 un1_CmdEnable20_0_0_o2_11
CTOF_DEL    ---     0.495       R2C9D.C0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.104       R2C9D.F0 to       R5C9A.D1 N_367
CTOF_DEL    ---     0.495       R5C9A.D1 to       R5C9A.F1 SLICE_23
ROUTE         8     1.295       R5C9A.F1 to      R7C10B.C0 XOR8MEG18
CTOF_DEL    ---     0.495      R7C10B.C0 to      R7C10B.F0 SLICE_77
ROUTE         1     1.708      R7C10B.F0 to      R7C11B.CE CmdUFMData_1_sqmuxa (to PHI2_c)
                  --------
                    8.738   (29.3% logic, 70.7% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[5]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to    IOL_T9B.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to     R7C11B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 163.537ns (weighted slack = 327.074ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[3]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMData  (to PHI2_c -)

   Delay:               8.397ns  (30.5% logic, 69.5% route), 5 logic levels.

 Constraint Details:

      8.397ns physical path delay Din[3]_MGIOL to SLICE_19 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.307ns CE_SET requirement (totaling 171.934ns) by 163.537ns

 Physical Path Details:

      Data path Din[3]_MGIOL to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577   IOL_T10A.CLK to    IOL_T10A.IN Din[3]_MGIOL (from PHI2_c)
ROUTE         1     1.297    IOL_T10A.IN to       R2C9D.C1 Bank[3]
CTOF_DEL    ---     0.495       R2C9D.C1 to       R2C9D.F1 SLICE_80
ROUTE         1     0.436       R2C9D.F1 to       R2C9D.C0 un1_CmdEnable20_0_0_o2_11
CTOF_DEL    ---     0.495       R2C9D.C0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.104       R2C9D.F0 to       R5C9A.D1 N_367
CTOF_DEL    ---     0.495       R5C9A.D1 to       R5C9A.F1 SLICE_23
ROUTE         8     1.295       R5C9A.F1 to      R7C10B.C0 XOR8MEG18
CTOF_DEL    ---     0.495      R7C10B.C0 to      R7C10B.F0 SLICE_77
ROUTE         1     1.708      R7C10B.F0 to      R7C11B.CE CmdUFMData_1_sqmuxa (to PHI2_c)
                  --------
                    8.397   (30.5% logic, 69.5% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[3]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to   IOL_T10A.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to     R7C11B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 163.622ns (weighted slack = 327.244ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[0]  (from PHI2_c +)
   Destination:    FF         Data in        CmdUFMData  (to PHI2_c -)

   Delay:               8.312ns  (24.8% logic, 75.2% route), 4 logic levels.

 Constraint Details:

      8.312ns physical path delay Din[0]_MGIOL to SLICE_19 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.307ns CE_SET requirement (totaling 171.934ns) by 163.622ns

 Physical Path Details:

      Data path Din[0]_MGIOL to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577    IOL_L3A.CLK to     IOL_L3A.IN Din[0]_MGIOL (from PHI2_c)
ROUTE         1     2.143     IOL_L3A.IN to       R2C9D.A0 Bank[0]
CTOF_DEL    ---     0.495       R2C9D.A0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.104       R2C9D.F0 to       R5C9A.D1 N_367
CTOF_DEL    ---     0.495       R5C9A.D1 to       R5C9A.F1 SLICE_23
ROUTE         8     1.295       R5C9A.F1 to      R7C10B.C0 XOR8MEG18
CTOF_DEL    ---     0.495      R7C10B.C0 to      R7C10B.F0 SLICE_77
ROUTE         1     1.708      R7C10B.F0 to      R7C11B.CE CmdUFMData_1_sqmuxa (to PHI2_c)
                  --------
                    8.312   (24.8% logic, 75.2% route), 4 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[0]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to    IOL_L3A.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_19:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to     R7C11B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 163.925ns (weighted slack = 327.850ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[1]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               8.150ns  (37.4% logic, 62.6% route), 6 logic levels.

 Constraint Details:

      8.150ns physical path delay Din[1]_MGIOL to SLICE_17 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.166ns DIN_SET requirement (totaling 172.075ns) by 163.925ns

 Physical Path Details:

      Data path Din[1]_MGIOL to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577   IOL_T10B.CLK to    IOL_T10B.IN Din[1]_MGIOL (from PHI2_c)
ROUTE         1     1.375    IOL_T10B.IN to      R4C10D.D0 Bank[1]
CTOF_DEL    ---     0.495      R4C10D.D0 to      R4C10D.F0 SLICE_90
ROUTE         1     0.958      R4C10D.F0 to       R2C9D.D0 un1_CmdEnable20_0_0_o2_10
CTOF_DEL    ---     0.495       R2C9D.D0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.048       R2C9D.F0 to       R4C9A.B1 N_367
CTOF_DEL    ---     0.495       R4C9A.B1 to       R4C9A.F1 SLICE_11
ROUTE         3     0.753       R4C9A.F1 to       R4C8A.C0 CmdEnable16
CTOF_DEL    ---     0.495       R4C8A.C0 to       R4C8A.F0 SLICE_33
ROUTE         1     0.964       R4C8A.F0 to       R4C9B.A0 CmdEnable_0_sqmuxa
CTOF_DEL    ---     0.495       R4C9B.A0 to       R4C9B.F0 SLICE_17
ROUTE         1     0.000       R4C9B.F0 to      R4C9B.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    8.150   (37.4% logic, 62.6% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[1]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to   IOL_T10B.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to      R4C9B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 164.020ns (weighted slack = 328.040ns)

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Bank_0io[6]  (from PHI2_c +)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               8.055ns  (37.9% logic, 62.1% route), 6 logic levels.

 Constraint Details:

      8.055ns physical path delay Din[6]_MGIOL to SLICE_17 meets
    172.414ns delay constraint less
      0.173ns skew and
      0.166ns DIN_SET requirement (totaling 172.075ns) by 164.020ns

 Physical Path Details:

      Data path Din[6]_MGIOL to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
C2INP_DEL   ---     0.577    IOL_L2D.CLK to     IOL_L2D.IN Din[6]_MGIOL (from PHI2_c)
ROUTE         1     1.802     IOL_L2D.IN to       R2C9D.D1 Bank[6]
CTOF_DEL    ---     0.495       R2C9D.D1 to       R2C9D.F1 SLICE_80
ROUTE         1     0.436       R2C9D.F1 to       R2C9D.C0 un1_CmdEnable20_0_0_o2_11
CTOF_DEL    ---     0.495       R2C9D.C0 to       R2C9D.F0 SLICE_80
ROUTE         6     1.048       R2C9D.F0 to       R4C9A.B1 N_367
CTOF_DEL    ---     0.495       R4C9A.B1 to       R4C9A.F1 SLICE_11
ROUTE         3     0.753       R4C9A.F1 to       R4C8A.C0 CmdEnable16
CTOF_DEL    ---     0.495       R4C8A.C0 to       R4C8A.F0 SLICE_33
ROUTE         1     0.964       R4C8A.F0 to       R4C9B.A0 CmdEnable_0_sqmuxa
CTOF_DEL    ---     0.495       R4C9B.A0 to       R4C9B.F0 SLICE_17
ROUTE         1     0.000       R4C9B.F0 to      R4C9B.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    8.055   (37.9% logic, 62.1% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to Din[6]_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.369        8.PADDI to    IOL_L2D.CLK PHI2_c
                  --------
                    4.369   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     4.196        8.PADDI to      R4C9B.CLK PHI2_c
                  --------
                    4.196   (0.0% logic, 100.0% route), 0 logic levels.

Report:   48.464MHz is the maximum frequency for this preference.


================================================================================
Preference: FREQUENCY PORT "nCCAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed:  The following path meets requirements by 338.168ns
         The internal maximum frequency of the following component is 150.150 MHz

 Logical Details:  Cell type  Pin name       Component name

   Destination:    PIO        PAD            nCCAS

   Delay:               6.660ns -- based on Minimum Pulse Width

Report:  150.150MHz is the maximum frequency for this preference.


================================================================================
Preference: FREQUENCY PORT "nCRAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed:  The following path meets requirements by 338.168ns
         The internal maximum frequency of the following component is 150.150 MHz

 Logical Details:  Cell type  Pin name       Component name

   Destination:    PIO        PAD            nCRAS

   Delay:               6.660ns -- based on Minimum Pulse Width

Report:  150.150MHz is the maximum frequency for this preference.


================================================================================
Preference: FREQUENCY PORT "RCLK" 62.500000 MHz ;
            891 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 6.215ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              RASr2  (from RCLK_c +)
   Destination:    FF         Data in        nRWE_0io  (to RCLK_c +)

   Delay:               9.805ns  (29.9% logic, 70.1% route), 6 logic levels.

 Constraint Details:

      9.805ns physical path delay SLICE_32 to nRWE_MGIOL meets
     16.000ns delay constraint less
     -0.173ns skew and
      0.153ns DO_SET requirement (totaling 16.020ns) by 6.215ns

 Physical Path Details:

      Data path SLICE_32 to nRWE_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.452     R4C12C.CLK to      R4C12C.Q1 SLICE_32 (from RCLK_c)
ROUTE        10     1.963      R4C12C.Q1 to      R8C11B.A1 RASr2
CTOF_DEL    ---     0.495      R8C11B.A1 to      R8C11B.F1 SLICE_62
ROUTE         6     1.078      R8C11B.F1 to      R7C12C.D1 IS_0_sqmuxa_0_o2
CTOF_DEL    ---     0.495      R7C12C.D1 to      R7C12C.F1 SLICE_79
ROUTE         2     0.635      R7C12C.F1 to      R7C12A.D1 IS_0_sqmuxa_0_o3
CTOF_DEL    ---     0.495      R7C12A.D1 to      R7C12A.F1 SLICE_28
ROUTE         1     0.744      R7C12A.F1 to      R8C12B.C1 nRWE_s_i_a2_1_0
CTOF_DEL    ---     0.495      R8C12B.C1 to      R8C12B.F1 SLICE_68
ROUTE         1     0.744      R8C12B.F1 to      R9C12D.C0 nRWE_s_i_tz_0
CTOF_DEL    ---     0.495      R9C12D.C0 to      R9C12D.F0 SLICE_75
ROUTE         1     1.714      R9C12D.F0 to  IOL_B20D.OPOS N_252_i (to RCLK_c)
                  --------
                    9.805   (29.9% logic, 70.1% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_32:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to     R4C12C.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to nRWE_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.437       63.PADDI to   IOL_B20D.CLK RCLK_c
                  --------
                    2.437   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 6.236ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         EFB        Port           ufmefb/EFBInst_0(ASIC)  (from RCLK_c +)
   Destination:    FF         Data in        n8MEGEN  (to RCLK_c +)

   Delay:               9.425ns  (77.1% logic, 22.9% route), 3 logic levels.

 Constraint Details:

      9.425ns physical path delay ufmefb/EFBInst_0 to SLICE_45 meets
     16.000ns delay constraint less
      0.173ns skew and
      0.166ns DIN_SET requirement (totaling 15.661ns) by 6.236ns

 Physical Path Details:

      Data path ufmefb/EFBInst_0 to SLICE_45:

   Name    Fanout   Delay (ns)          Site               Resource
WCLKI2WBDA  ---     6.278     EFB.WBCLKI to    EFB.WBDATO0 ufmefb/EFBInst_0 (from RCLK_c)
ROUTE         1     1.512    EFB.WBDATO0 to       R4C5C.C1 wb_dato[0]
CTOF_DEL    ---     0.495       R4C5C.C1 to       R4C5C.F1 SLICE_111
ROUTE         1     0.645       R4C5C.F1 to       R5C5B.D0 n8MEGENe_1_0
CTOF_DEL    ---     0.495       R5C5B.D0 to       R5C5B.F0 SLICE_45
ROUTE         1     0.000       R5C5B.F0 to      R5C5B.DI0 n8MEGENe_0 (to RCLK_c)
                  --------
                    9.425   (77.1% logic, 22.9% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to ufmefb/EFBInst_0:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.437       63.PADDI to     EFB.WBCLKI RCLK_c
                  --------
                    2.437   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_45:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to      R5C5B.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 6.365ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         EFB        Port           ufmefb/EFBInst_0(ASIC)  (from RCLK_c +)
   Destination:    FF         Data in        LEDEN  (to RCLK_c +)

   Delay:               9.296ns  (69.4% logic, 30.6% route), 3 logic levels.

 Constraint Details:

      9.296ns physical path delay ufmefb/EFBInst_0 to SLICE_30 meets
     16.000ns delay constraint less
      0.173ns skew and
      0.166ns DIN_SET requirement (totaling 15.661ns) by 6.365ns

 Physical Path Details:

      Data path ufmefb/EFBInst_0 to SLICE_30:

   Name    Fanout   Delay (ns)          Site               Resource
WCLKI2WBDA  ---     5.461     EFB.WBCLKI to    EFB.WBDATO1 ufmefb/EFBInst_0 (from RCLK_c)
ROUTE         1     2.152    EFB.WBDATO1 to       R7C5A.A1 wb_dato[1]
CTOF_DEL    ---     0.495       R7C5A.A1 to       R7C5A.F1 SLICE_30
ROUTE         1     0.693       R7C5A.F1 to       R7C5A.B0 LEDEN_6
CTOF_DEL    ---     0.495       R7C5A.B0 to       R7C5A.F0 SLICE_30
ROUTE         1     0.000       R7C5A.F0 to      R7C5A.DI0 LEDENe_0 (to RCLK_c)
                  --------
                    9.296   (69.4% logic, 30.6% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to ufmefb/EFBInst_0:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.437       63.PADDI to     EFB.WBCLKI RCLK_c
                  --------
                    2.437   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_30:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to      R7C5A.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 6.454ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              InitReady  (from RCLK_c +)
   Destination:    FF         Data in        nRWE_0io  (to RCLK_c +)

   Delay:               9.566ns  (30.6% logic, 69.4% route), 6 logic levels.

 Constraint Details:

      9.566ns physical path delay SLICE_29 to nRWE_MGIOL meets
     16.000ns delay constraint less
     -0.173ns skew and
      0.153ns DO_SET requirement (totaling 16.020ns) by 6.454ns

 Physical Path Details:

      Data path SLICE_29 to nRWE_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.452      R4C8D.CLK to       R4C8D.Q0 SLICE_29 (from RCLK_c)
ROUTE        40     1.724       R4C8D.Q0 to      R8C11B.D1 InitReady
CTOF_DEL    ---     0.495      R8C11B.D1 to      R8C11B.F1 SLICE_62
ROUTE         6     1.078      R8C11B.F1 to      R7C12C.D1 IS_0_sqmuxa_0_o2
CTOF_DEL    ---     0.495      R7C12C.D1 to      R7C12C.F1 SLICE_79
ROUTE         2     0.635      R7C12C.F1 to      R7C12A.D1 IS_0_sqmuxa_0_o3
CTOF_DEL    ---     0.495      R7C12A.D1 to      R7C12A.F1 SLICE_28
ROUTE         1     0.744      R7C12A.F1 to      R8C12B.C1 nRWE_s_i_a2_1_0
CTOF_DEL    ---     0.495      R8C12B.C1 to      R8C12B.F1 SLICE_68
ROUTE         1     0.744      R8C12B.F1 to      R9C12D.C0 nRWE_s_i_tz_0
CTOF_DEL    ---     0.495      R9C12D.C0 to      R9C12D.F0 SLICE_75
ROUTE         1     1.714      R9C12D.F0 to  IOL_B20D.OPOS N_252_i (to RCLK_c)
                  --------
                    9.566   (30.6% logic, 69.4% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_29:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to      R4C8D.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to nRWE_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.437       63.PADDI to   IOL_B20D.CLK RCLK_c
                  --------
                    2.437   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 6.646ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              IS[1]  (from RCLK_c +)
   Destination:    FF         Data in        nRCAS_0io  (to RCLK_c +)

   Delay:               9.373ns  (31.2% logic, 68.8% route), 6 logic levels.

 Constraint Details:

      9.373ns physical path delay SLICE_27 to nRCAS_MGIOL meets
     16.000ns delay constraint less
     -0.172ns skew and
      0.153ns DO_SET requirement (totaling 16.019ns) by 6.646ns

 Physical Path Details:

      Data path SLICE_27 to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.452     R7C11C.CLK to      R7C11C.Q0 SLICE_27 (from RCLK_c)
ROUTE         7     1.445      R7C11C.Q0 to      R8C12A.A1 IS[1]
CTOF_DEL    ---     0.495      R8C12A.A1 to      R8C12A.F1 SLICE_83
ROUTE         3     0.973      R8C12A.F1 to      R8C11B.A0 un1_nRCAS_6_sqmuxa_i_o2
CTOF_DEL    ---     0.495      R8C11B.A0 to      R8C11B.F0 SLICE_62
ROUTE         2     0.632      R8C11B.F0 to      R9C11A.D0 N_48
CTOF_DEL    ---     0.495      R9C11A.D0 to      R9C11A.F0 SLICE_69
ROUTE         1     0.626      R9C11A.F0 to      R9C11A.D1 nRCS_9_u_i_o3_0_0
CTOF_DEL    ---     0.495      R9C11A.D1 to      R9C11A.F1 SLICE_69
ROUTE         1     0.744      R9C11A.F1 to      R9C12C.C1 nRCS_9_u_i_o3_0_2
CTOF_DEL    ---     0.495      R9C12C.C1 to      R9C12C.F1 SLICE_101
ROUTE         1     2.026      R9C12C.F1 to  IOL_R10C.OPOS N_251_i (to RCLK_c)
                  --------
                    9.373   (31.2% logic, 68.8% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_27:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to     R7C11C.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.436       63.PADDI to   IOL_R10C.CLK RCLK_c
                  --------
                    2.436   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 6.656ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              RASr2  (from RCLK_c +)
   Destination:    FF         Data in        nRCAS_0io  (to RCLK_c +)

   Delay:               9.363ns  (31.3% logic, 68.7% route), 6 logic levels.

 Constraint Details:

      9.363ns physical path delay SLICE_32 to nRCAS_MGIOL meets
     16.000ns delay constraint less
     -0.172ns skew and
      0.153ns DO_SET requirement (totaling 16.019ns) by 6.656ns

 Physical Path Details:

      Data path SLICE_32 to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.452     R4C12C.CLK to      R4C12C.Q1 SLICE_32 (from RCLK_c)
ROUTE        10     1.963      R4C12C.Q1 to      R8C11B.A1 RASr2
CTOF_DEL    ---     0.495      R8C11B.A1 to      R8C11B.F1 SLICE_62
ROUTE         6     0.445      R8C11B.F1 to      R8C11B.C0 IS_0_sqmuxa_0_o2
CTOF_DEL    ---     0.495      R8C11B.C0 to      R8C11B.F0 SLICE_62
ROUTE         2     0.632      R8C11B.F0 to      R9C11A.D0 N_48
CTOF_DEL    ---     0.495      R9C11A.D0 to      R9C11A.F0 SLICE_69
ROUTE         1     0.626      R9C11A.F0 to      R9C11A.D1 nRCS_9_u_i_o3_0_0
CTOF_DEL    ---     0.495      R9C11A.D1 to      R9C11A.F1 SLICE_69
ROUTE         1     0.744      R9C11A.F1 to      R9C12C.C1 nRCS_9_u_i_o3_0_2
CTOF_DEL    ---     0.495      R9C12C.C1 to      R9C12C.F1 SLICE_101
ROUTE         1     2.026      R9C12C.F1 to  IOL_R10C.OPOS N_251_i (to RCLK_c)
                  --------
                    9.363   (31.3% logic, 68.7% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_32:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to     R4C12C.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.436       63.PADDI to   IOL_R10C.CLK RCLK_c
                  --------
                    2.436   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 6.868ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              IS[1]  (from RCLK_c +)
   Destination:    FF         Data in        nRCAS_0io  (to RCLK_c +)

   Delay:               9.151ns  (26.6% logic, 73.4% route), 5 logic levels.

 Constraint Details:

      9.151ns physical path delay SLICE_27 to nRCAS_MGIOL meets
     16.000ns delay constraint less
     -0.172ns skew and
      0.153ns DO_SET requirement (totaling 16.019ns) by 6.868ns

 Physical Path Details:

      Data path SLICE_27 to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.452     R7C11C.CLK to      R7C11C.Q0 SLICE_27 (from RCLK_c)
ROUTE         7     1.445      R7C11C.Q0 to      R8C12A.A1 IS[1]
CTOF_DEL    ---     0.495      R8C12A.A1 to      R8C12A.F1 SLICE_83
ROUTE         3     0.973      R8C12A.F1 to      R8C11B.A0 un1_nRCAS_6_sqmuxa_i_o2
CTOF_DEL    ---     0.495      R8C11B.A0 to      R8C11B.F0 SLICE_62
ROUTE         2     1.308      R8C11B.F0 to      R9C12C.A0 N_48
CTOF_DEL    ---     0.495      R9C12C.A0 to      R9C12C.F0 SLICE_101
ROUTE         1     0.967      R9C12C.F0 to      R9C12C.A1 N_251_i_sx
CTOF_DEL    ---     0.495      R9C12C.A1 to      R9C12C.F1 SLICE_101
ROUTE         1     2.026      R9C12C.F1 to  IOL_R10C.OPOS N_251_i (to RCLK_c)
                  --------
                    9.151   (26.6% logic, 73.4% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_27:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to     R7C11C.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.436       63.PADDI to   IOL_R10C.CLK RCLK_c
                  --------
                    2.436   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 6.878ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              RASr2  (from RCLK_c +)
   Destination:    FF         Data in        nRCAS_0io  (to RCLK_c +)

   Delay:               9.141ns  (26.6% logic, 73.4% route), 5 logic levels.

 Constraint Details:

      9.141ns physical path delay SLICE_32 to nRCAS_MGIOL meets
     16.000ns delay constraint less
     -0.172ns skew and
      0.153ns DO_SET requirement (totaling 16.019ns) by 6.878ns

 Physical Path Details:

      Data path SLICE_32 to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.452     R4C12C.CLK to      R4C12C.Q1 SLICE_32 (from RCLK_c)
ROUTE        10     1.963      R4C12C.Q1 to      R8C11B.A1 RASr2
CTOF_DEL    ---     0.495      R8C11B.A1 to      R8C11B.F1 SLICE_62
ROUTE         6     0.445      R8C11B.F1 to      R8C11B.C0 IS_0_sqmuxa_0_o2
CTOF_DEL    ---     0.495      R8C11B.C0 to      R8C11B.F0 SLICE_62
ROUTE         2     1.308      R8C11B.F0 to      R9C12C.A0 N_48
CTOF_DEL    ---     0.495      R9C12C.A0 to      R9C12C.F0 SLICE_101
ROUTE         1     0.967      R9C12C.F0 to      R9C12C.A1 N_251_i_sx
CTOF_DEL    ---     0.495      R9C12C.A1 to      R9C12C.F1 SLICE_101
ROUTE         1     2.026      R9C12C.F1 to  IOL_R10C.OPOS N_251_i (to RCLK_c)
                  --------
                    9.141   (26.6% logic, 73.4% route), 5 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_32:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to     R4C12C.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.436       63.PADDI to   IOL_R10C.CLK RCLK_c
                  --------
                    2.436   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 6.895ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              InitReady  (from RCLK_c +)
   Destination:    FF         Data in        nRCAS_0io  (to RCLK_c +)

   Delay:               9.124ns  (32.1% logic, 67.9% route), 6 logic levels.

 Constraint Details:

      9.124ns physical path delay SLICE_29 to nRCAS_MGIOL meets
     16.000ns delay constraint less
     -0.172ns skew and
      0.153ns DO_SET requirement (totaling 16.019ns) by 6.895ns

 Physical Path Details:

      Data path SLICE_29 to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.452      R4C8D.CLK to       R4C8D.Q0 SLICE_29 (from RCLK_c)
ROUTE        40     1.724       R4C8D.Q0 to      R8C11B.D1 InitReady
CTOF_DEL    ---     0.495      R8C11B.D1 to      R8C11B.F1 SLICE_62
ROUTE         6     0.445      R8C11B.F1 to      R8C11B.C0 IS_0_sqmuxa_0_o2
CTOF_DEL    ---     0.495      R8C11B.C0 to      R8C11B.F0 SLICE_62
ROUTE         2     0.632      R8C11B.F0 to      R9C11A.D0 N_48
CTOF_DEL    ---     0.495      R9C11A.D0 to      R9C11A.F0 SLICE_69
ROUTE         1     0.626      R9C11A.F0 to      R9C11A.D1 nRCS_9_u_i_o3_0_0
CTOF_DEL    ---     0.495      R9C11A.D1 to      R9C11A.F1 SLICE_69
ROUTE         1     0.744      R9C11A.F1 to      R9C12C.C1 nRCS_9_u_i_o3_0_2
CTOF_DEL    ---     0.495      R9C12C.C1 to      R9C12C.F1 SLICE_101
ROUTE         1     2.026      R9C12C.F1 to  IOL_R10C.OPOS N_251_i (to RCLK_c)
                  --------
                    9.124   (32.1% logic, 67.9% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_29:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to      R4C8D.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.436       63.PADDI to   IOL_R10C.CLK RCLK_c
                  --------
                    2.436   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 6.966ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              IS[2]  (from RCLK_c +)
   Destination:    FF         Data in        nRCAS_0io  (to RCLK_c +)

   Delay:               9.053ns  (32.3% logic, 67.7% route), 6 logic levels.

 Constraint Details:

      9.053ns physical path delay SLICE_27 to nRCAS_MGIOL meets
     16.000ns delay constraint less
     -0.172ns skew and
      0.153ns DO_SET requirement (totaling 16.019ns) by 6.966ns

 Physical Path Details:

      Data path SLICE_27 to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.452     R7C11C.CLK to      R7C11C.Q1 SLICE_27 (from RCLK_c)
ROUTE         6     1.125      R7C11C.Q1 to      R8C12A.C1 IS[2]
CTOF_DEL    ---     0.495      R8C12A.C1 to      R8C12A.F1 SLICE_83
ROUTE         3     0.973      R8C12A.F1 to      R8C11B.A0 un1_nRCAS_6_sqmuxa_i_o2
CTOF_DEL    ---     0.495      R8C11B.A0 to      R8C11B.F0 SLICE_62
ROUTE         2     0.632      R8C11B.F0 to      R9C11A.D0 N_48
CTOF_DEL    ---     0.495      R9C11A.D0 to      R9C11A.F0 SLICE_69
ROUTE         1     0.626      R9C11A.F0 to      R9C11A.D1 nRCS_9_u_i_o3_0_0
CTOF_DEL    ---     0.495      R9C11A.D1 to      R9C11A.F1 SLICE_69
ROUTE         1     0.744      R9C11A.F1 to      R9C12C.C1 nRCS_9_u_i_o3_0_2
CTOF_DEL    ---     0.495      R9C12C.C1 to      R9C12C.F1 SLICE_101
ROUTE         1     2.026      R9C12C.F1 to  IOL_R10C.OPOS N_251_i (to RCLK_c)
                  --------
                    9.053   (32.3% logic, 67.7% route), 6 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_27:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.264       63.PADDI to     R7C11C.CLK RCLK_c
                  --------
                    2.264   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to nRCAS_MGIOL:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     2.436       63.PADDI to   IOL_R10C.CLK RCLK_c
                  --------
                    2.436   (0.0% logic, 100.0% route), 0 logic levels.

Report:  102.197MHz is the maximum frequency for this preference.

Report Summary
--------------
----------------------------------------------------------------------------
Preference                              |   Constraint|       Actual|Levels
----------------------------------------------------------------------------
                                        |             |             |
FREQUENCY PORT "PHI2" 2.900000 MHz ;    |    2.900 MHz|   48.464 MHz|   5  
                                        |             |             |
FREQUENCY PORT "nCCAS" 2.900000 MHz ;   |    2.900 MHz|  150.150 MHz|   0  
                                        |             |             |
FREQUENCY PORT "nCRAS" 2.900000 MHz ;   |    2.900 MHz|  150.150 MHz|   0  
                                        |             |             |
FREQUENCY PORT "RCLK" 62.500000 MHz ;   |   62.500 MHz|  102.197 MHz|   6  
                                        |             |             |
----------------------------------------------------------------------------


All preferences were met.


Clock Domains Analysis
------------------------

Found 4 clocks:

Clock Domain: nCRAS_c   Source: nCRAS.PAD   Loads: 11
   No transfer within this clock domain is found

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: nCCAS_c   Source: nCCAS.PAD   Loads: 10
   No transfer within this clock domain is found

Clock Domain: RCLK_c   Source: RCLK.PAD   Loads: 48
   Covered under: FREQUENCY PORT "RCLK" 62.500000 MHz ;

   Data transfers from:
   Clock Domain: nCRAS_c   Source: nCRAS.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

   Clock Domain: PHI2_c   Source: PHI2.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: PHI2_c   Source: PHI2.PAD   Loads: 21
   Covered under: FREQUENCY PORT "PHI2" 2.900000 MHz ;

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.


Timing summary (Setup):
---------------

Timing errors: 0  Score: 0
Cumulative negative slack: 0

Constraints cover 1038 paths, 4 nets, and 750 connections (74.18% coverage)

--------------------------------------------------------------------------------
Lattice TRACE Report - Hold, Version Diamond (64-bit) 3.12.1.454
Sat Nov 18 02:06:13 2023

Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
Copyright (c) 1995 AT&T Corp.   All rights reserved.
Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
Copyright (c) 2001 Agere Systems   All rights reserved.
Copyright (c) 2002-2020 Lattice Semiconductor Corporation,  All rights reserved.

Report Information
------------------
Command line:    trce -v 10 -gt -sethld -sp 4 -sphld m -o RAM2GS_LCMXO2_1200HC_impl1.twr -gui -msgset //Mac/iCloud/Repos/RAM2GS/CPLD/LCMXO2-1200HC/promote.xml RAM2GS_LCMXO2_1200HC_impl1.ncd RAM2GS_LCMXO2_1200HC_impl1.prf 
Design file:     ram2gs_lcmxo2_1200hc_impl1.ncd
Preference file: ram2gs_lcmxo2_1200hc_impl1.prf
Device,speed:    LCMXO2-1200HC,m
Report level:    verbose report, limited to 10 items per preference
--------------------------------------------------------------------------------

BLOCK ASYNCPATHS
BLOCK RESETPATHS
--------------------------------------------------------------------------------



================================================================================
Preference: FREQUENCY PORT "PHI2" 2.900000 MHz ;
            147 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 0.379ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              ADSubmitted  (from PHI2_c -)
   Destination:    FF         Data in        ADSubmitted  (to PHI2_c -)

   Delay:               0.366ns  (63.9% logic, 36.1% route), 2 logic levels.

 Constraint Details:

      0.366ns physical path delay SLICE_10 to SLICE_10 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.379ns

 Physical Path Details:

      Data path SLICE_10 to SLICE_10:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R4C9D.CLK to       R4C9D.Q0 SLICE_10 (from PHI2_c)
ROUTE         2     0.132       R4C9D.Q0 to       R4C9D.A0 ADSubmitted
CTOF_DEL    ---     0.101       R4C9D.A0 to       R4C9D.F0 SLICE_10
ROUTE         1     0.000       R4C9D.F0 to      R4C9D.DI0 ADSubmitted_r_0_0 (to PHI2_c)
                  --------
                    0.366   (63.9% logic, 36.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_10:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9D.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_10:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9D.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.379ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdUFMShift  (from PHI2_c -)
   Destination:    FF         Data in        CmdUFMShift  (to PHI2_c -)

   Delay:               0.366ns  (63.9% logic, 36.1% route), 2 logic levels.

 Constraint Details:

      0.366ns physical path delay SLICE_20 to SLICE_20 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.379ns

 Physical Path Details:

      Data path SLICE_20 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R7C9A.CLK to       R7C9A.Q0 SLICE_20 (from PHI2_c)
ROUTE         2     0.132       R7C9A.Q0 to       R7C9A.A0 CmdUFMShift
CTOF_DEL    ---     0.101       R7C9A.A0 to       R7C9A.F0 SLICE_20
ROUTE         1     0.000       R7C9A.F0 to      R7C9A.DI0 CmdUFMShift_3 (to PHI2_c)
                  --------
                    0.366   (63.9% logic, 36.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R7C9A.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R7C9A.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.385ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              C1Submitted  (from PHI2_c -)
   Destination:    FF         Data in        C1Submitted  (to PHI2_c -)

   Delay:               0.372ns  (62.9% logic, 37.1% route), 2 logic levels.

 Constraint Details:

      0.372ns physical path delay SLICE_11 to SLICE_11 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.385ns

 Physical Path Details:

      Data path SLICE_11 to SLICE_11:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R4C9A.CLK to       R4C9A.Q0 SLICE_11 (from PHI2_c)
ROUTE         2     0.138       R4C9A.Q0 to       R4C9A.C0 C1Submitted
CTOF_DEL    ---     0.101       R4C9A.C0 to       R4C9A.F0 SLICE_11
ROUTE         1     0.000       R4C9A.F0 to      R4C9A.DI0 C1Submitted_RNO (to PHI2_c)
                  --------
                    0.372   (62.9% logic, 37.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_11:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9A.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_11:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9A.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.471ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdEnable  (from PHI2_c -)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               0.458ns  (51.1% logic, 48.9% route), 2 logic levels.

 Constraint Details:

      0.458ns physical path delay SLICE_17 to SLICE_17 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.471ns

 Physical Path Details:

      Data path SLICE_17 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R4C9B.CLK to       R4C9B.Q0 SLICE_17 (from PHI2_c)
ROUTE         2     0.224       R4C9B.Q0 to       R4C9B.B0 CmdEnable
CTOF_DEL    ---     0.101       R4C9B.B0 to       R4C9B.F0 SLICE_17
ROUTE         1     0.000       R4C9B.F0 to      R4C9B.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    0.458   (51.1% logic, 48.9% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9B.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9B.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.616ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdLEDEN  (from PHI2_c -)
   Destination:    FF         Data in        CmdLEDEN  (to PHI2_c -)

   Delay:               0.603ns  (55.6% logic, 44.4% route), 3 logic levels.

 Constraint Details:

      0.603ns physical path delay SLICE_18 to SLICE_18 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.616ns

 Physical Path Details:

      Data path SLICE_18 to SLICE_18:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R7C8C.CLK to       R7C8C.Q0 SLICE_18 (from PHI2_c)
ROUTE         2     0.212       R7C8C.Q0 to       R7C8C.A1 CmdLEDEN
CTOF_DEL    ---     0.101       R7C8C.A1 to       R7C8C.F1 SLICE_18
ROUTE         1     0.056       R7C8C.F1 to       R7C8C.C0 CmdLEDEN_4_u_i_m2_i_0
CTOF_DEL    ---     0.101       R7C8C.C0 to       R7C8C.F0 SLICE_18
ROUTE         1     0.000       R7C8C.F0 to      R7C8C.DI0 N_17_i (to PHI2_c)
                  --------
                    0.603   (55.6% logic, 44.4% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_18:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R7C8C.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_18:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R7C8C.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.622ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              C1Submitted  (from PHI2_c -)
   Destination:    FF         Data in        CmdEnable  (to PHI2_c -)

   Delay:               0.609ns  (55.0% logic, 45.0% route), 3 logic levels.

 Constraint Details:

      0.609ns physical path delay SLICE_11 to SLICE_17 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.622ns

 Physical Path Details:

      Data path SLICE_11 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R4C9A.CLK to       R4C9A.Q0 SLICE_11 (from PHI2_c)
ROUTE         2     0.137       R4C9A.Q0 to       R5C9D.D0 C1Submitted
CTOF_DEL    ---     0.101       R5C9D.D0 to       R5C9D.F0 SLICE_76
ROUTE         1     0.137       R5C9D.F0 to       R4C9B.C0 un1_CmdEnable20_i
CTOF_DEL    ---     0.101       R4C9B.C0 to       R4C9B.F0 SLICE_17
ROUTE         1     0.000       R4C9B.F0 to      R4C9B.DI0 CmdEnable_s (to PHI2_c)
                  --------
                    0.609   (55.0% logic, 45.0% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_11:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9A.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9B.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.705ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              Cmdn8MEGEN  (from PHI2_c -)
   Destination:    FF         Data in        Cmdn8MEGEN  (to PHI2_c -)

   Delay:               0.692ns  (48.4% logic, 51.6% route), 3 logic levels.

 Constraint Details:

      0.692ns physical path delay SLICE_24 to SLICE_24 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.705ns

 Physical Path Details:

      Data path SLICE_24 to SLICE_24:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R7C8B.CLK to       R7C8B.Q0 SLICE_24 (from PHI2_c)
ROUTE         2     0.135       R7C8B.Q0 to       R7C8B.D1 Cmdn8MEGEN
CTOF_DEL    ---     0.101       R7C8B.D1 to       R7C8B.F1 SLICE_24
ROUTE         1     0.222       R7C8B.F1 to       R7C8B.B0 Cmdn8MEGEN_4_u_i_m2_i_0
CTOF_DEL    ---     0.101       R7C8B.B0 to       R7C8B.F0 SLICE_24
ROUTE         1     0.000       R7C8B.F0 to      R7C8B.DI0 N_15_i (to PHI2_c)
                  --------
                    0.692   (48.4% logic, 51.6% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_24:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R7C8B.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_24:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R7C8B.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.728ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdEnable  (from PHI2_c -)
   Destination:    FF         Data in        CmdUFMShift  (to PHI2_c -)

   Delay:               0.700ns  (33.4% logic, 66.6% route), 2 logic levels.

 Constraint Details:

      0.700ns physical path delay SLICE_17 to SLICE_20 meets
     -0.028ns CE_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.028ns) by 0.728ns

 Physical Path Details:

      Data path SLICE_17 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R4C9B.CLK to       R4C9B.Q0 SLICE_17 (from PHI2_c)
ROUTE         2     0.277       R4C9B.Q0 to       R5C9A.C1 CmdEnable
CTOF_DEL    ---     0.101       R5C9A.C1 to       R5C9A.F1 SLICE_23
ROUTE         8     0.189       R5C9A.F1 to       R7C9A.CE XOR8MEG18 (to PHI2_c)
                  --------
                    0.700   (33.4% logic, 66.6% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9B.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_20:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R7C9A.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.770ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdEnable  (from PHI2_c -)
   Destination:    FF         Data in        CmdValid_fast  (to PHI2_c -)

   Delay:               0.757ns  (44.3% logic, 55.7% route), 3 logic levels.

 Constraint Details:

      0.757ns physical path delay SLICE_17 to SLICE_23 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.770ns

 Physical Path Details:

      Data path SLICE_17 to SLICE_23:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R4C9B.CLK to       R4C9B.Q0 SLICE_17 (from PHI2_c)
ROUTE         2     0.277       R4C9B.Q0 to       R5C9A.C1 CmdEnable
CTOF_DEL    ---     0.101       R5C9A.C1 to       R5C9A.F1 SLICE_23
ROUTE         8     0.145       R5C9A.F1 to       R5C9A.B0 XOR8MEG18
CTOF_DEL    ---     0.101       R5C9A.B0 to       R5C9A.F0 SLICE_23
ROUTE         1     0.000       R5C9A.F0 to      R5C9A.DI0 N_34_fast (to PHI2_c)
                  --------
                    0.757   (44.3% logic, 55.7% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_17:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R4C9B.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_23:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R5C9A.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.782ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CmdUFMWrite  (from PHI2_c -)
   Destination:    FF         Data in        CmdUFMWrite  (to PHI2_c -)

   Delay:               0.769ns  (43.6% logic, 56.4% route), 3 logic levels.

 Constraint Details:

      0.769ns physical path delay SLICE_21 to SLICE_21 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.782ns

 Physical Path Details:

      Data path SLICE_21 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R7C8D.CLK to       R7C8D.Q0 SLICE_21 (from PHI2_c)
ROUTE         2     0.224       R7C8D.Q0 to       R7C8D.B1 CmdUFMWrite
CTOF_DEL    ---     0.101       R7C8D.B1 to       R7C8D.F1 SLICE_21
ROUTE         1     0.210       R7C8D.F1 to       R7C8D.A0 N_415
CTOF_DEL    ---     0.101       R7C8D.A0 to       R7C8D.F0 SLICE_21
ROUTE         1     0.000       R7C8D.F0 to      R7C8D.DI0 CmdUFMWrite_3 (to PHI2_c)
                  --------
                    0.769   (43.6% logic, 56.4% route), 3 logic levels.

 Clock Skew Details: 

      Source Clock Path PHI2 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R7C8D.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path PHI2 to SLICE_21:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        21     1.423        8.PADDI to      R7C8D.CLK PHI2_c
                  --------
                    1.423   (0.0% logic, 100.0% route), 0 logic levels.


================================================================================
Preference: FREQUENCY PORT "nCCAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


================================================================================
Preference: FREQUENCY PORT "nCRAS" 2.900000 MHz ;
            0 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


================================================================================
Preference: FREQUENCY PORT "RCLK" 62.500000 MHz ;
            891 items scored, 0 timing errors detected.
--------------------------------------------------------------------------------


Passed: The following path meets requirements by 0.304ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              CASr  (from RCLK_c +)
   Destination:    FF         Data in        CASr2  (to RCLK_c +)

   Delay:               0.285ns  (46.7% logic, 53.3% route), 1 logic levels.

 Constraint Details:

      0.285ns physical path delay SLICE_12 to SLICE_12 meets
     -0.019ns M_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.304ns

 Physical Path Details:

      Data path SLICE_12 to SLICE_12:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133     R5C10B.CLK to      R5C10B.Q0 SLICE_12 (from RCLK_c)
ROUTE         1     0.152      R5C10B.Q0 to      R5C10B.M1 CASr (to RCLK_c)
                  --------
                    0.285   (46.7% logic, 53.3% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_12:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to     R5C10B.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_12:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to     R5C10B.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.306ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              RASr  (from RCLK_c +)
   Destination:    FF         Data in        RASr2  (to RCLK_c +)

   Delay:               0.287ns  (46.3% logic, 53.7% route), 1 logic levels.

 Constraint Details:

      0.287ns physical path delay SLICE_32 to SLICE_32 meets
     -0.019ns M_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.306ns

 Physical Path Details:

      Data path SLICE_32 to SLICE_32:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133     R4C12C.CLK to      R4C12C.Q0 SLICE_32 (from RCLK_c)
ROUTE         2     0.154      R4C12C.Q0 to      R4C12C.M1 RASr (to RCLK_c)
                  --------
                    0.287   (46.3% logic, 53.7% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_32:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to     R4C12C.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_32:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to     R4C12C.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.322ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              PHI2r2  (from RCLK_c +)
   Destination:    FF         Data in        PHI2r3  (to RCLK_c +)

   Delay:               0.303ns  (43.9% logic, 56.1% route), 1 logic levels.

 Constraint Details:

      0.303ns physical path delay SLICE_31 to SLICE_31 meets
     -0.019ns M_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.019ns) by 0.322ns

 Physical Path Details:

      Data path SLICE_31 to SLICE_31:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R5C8B.CLK to       R5C8B.Q0 SLICE_31 (from RCLK_c)
ROUTE         5     0.170       R5C8B.Q0 to       R5C8B.M1 PHI2r2 (to RCLK_c)
                  --------
                    0.303   (43.9% logic, 56.1% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_31:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R5C8B.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_31:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R5C8B.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.326ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              wb_dati[7]  (from RCLK_c +)
   Destination:    EFB        Port           ufmefb/EFBInst_0(ASIC)  (to RCLK_c +)

   Delay:               0.307ns  (43.3% logic, 56.7% route), 1 logic levels.

 Constraint Details:

      0.307ns physical path delay SLICE_55 to ufmefb/EFBInst_0 meets
     -0.073ns WBDATI_HLD and
      0.000ns delay constraint less
     -0.054ns skew requirement (totaling -0.019ns) by 0.326ns

 Physical Path Details:

      Data path SLICE_55 to ufmefb/EFBInst_0:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R3C6C.CLK to       R3C6C.Q1 SLICE_55 (from RCLK_c)
ROUTE         2     0.174       R3C6C.Q1 to    EFB.WBDATI7 wb_dati[7] (to RCLK_c)
                  --------
                    0.307   (43.3% logic, 56.7% route), 1 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_55:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R3C6C.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to ufmefb/EFBInst_0:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.842       63.PADDI to     EFB.WBCLKI RCLK_c
                  --------
                    0.842   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.379ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[0]  (from RCLK_c +)
   Destination:    FF         Data in        FS[0]  (to RCLK_c +)

   Delay:               0.366ns  (63.9% logic, 36.1% route), 2 logic levels.

 Constraint Details:

      0.366ns physical path delay SLICE_0 to SLICE_0 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.379ns

 Physical Path Details:

      Data path SLICE_0 to SLICE_0:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R2C7A.CLK to       R2C7A.Q1 SLICE_0 (from RCLK_c)
ROUTE         3     0.132       R2C7A.Q1 to       R2C7A.A1 FS[0]
CTOF_DEL    ---     0.101       R2C7A.A1 to       R2C7A.F1 SLICE_0
ROUTE         1     0.000       R2C7A.F1 to      R2C7A.DI1 FS_s[0] (to RCLK_c)
                  --------
                    0.366   (63.9% logic, 36.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_0:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R2C7A.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_0:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R2C7A.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.379ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[17]  (from RCLK_c +)
   Destination:    FF         Data in        FS[17]  (to RCLK_c +)

   Delay:               0.366ns  (63.9% logic, 36.1% route), 2 logic levels.

 Constraint Details:

      0.366ns physical path delay SLICE_1 to SLICE_1 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.379ns

 Physical Path Details:

      Data path SLICE_1 to SLICE_1:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R2C9B.CLK to       R2C9B.Q0 SLICE_1 (from RCLK_c)
ROUTE         7     0.132       R2C9B.Q0 to       R2C9B.A0 FS[17]
CTOF_DEL    ---     0.101       R2C9B.A0 to       R2C9B.F0 SLICE_1
ROUTE         1     0.000       R2C9B.F0 to      R2C9B.DI0 FS_s[17] (to RCLK_c)
                  --------
                    0.366   (63.9% logic, 36.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_1:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R2C9B.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_1:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R2C9B.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.379ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[15]  (from RCLK_c +)
   Destination:    FF         Data in        FS[15]  (to RCLK_c +)

   Delay:               0.366ns  (63.9% logic, 36.1% route), 2 logic levels.

 Constraint Details:

      0.366ns physical path delay SLICE_2 to SLICE_2 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.379ns

 Physical Path Details:

      Data path SLICE_2 to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R2C9A.CLK to       R2C9A.Q0 SLICE_2 (from RCLK_c)
ROUTE         6     0.132       R2C9A.Q0 to       R2C9A.A0 FS[15]
CTOF_DEL    ---     0.101       R2C9A.A0 to       R2C9A.F0 SLICE_2
ROUTE         1     0.000       R2C9A.F0 to      R2C9A.DI0 FS_s[15] (to RCLK_c)
                  --------
                    0.366   (63.9% logic, 36.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R2C9A.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_2:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R2C9A.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.379ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              FS[14]  (from RCLK_c +)
   Destination:    FF         Data in        FS[14]  (to RCLK_c +)

   Delay:               0.366ns  (63.9% logic, 36.1% route), 2 logic levels.

 Constraint Details:

      0.366ns physical path delay SLICE_3 to SLICE_3 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.379ns

 Physical Path Details:

      Data path SLICE_3 to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R2C8D.CLK to       R2C8D.Q1 SLICE_3 (from RCLK_c)
ROUTE        19     0.132       R2C8D.Q1 to       R2C8D.A1 FS[14]
CTOF_DEL    ---     0.101       R2C8D.A1 to       R2C8D.F1 SLICE_3
ROUTE         1     0.000       R2C8D.F1 to      R2C8D.DI1 FS_s[14] (to RCLK_c)
                  --------
                    0.366   (63.9% logic, 36.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R2C8D.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_3:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R2C8D.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.379ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              LEDEN  (from RCLK_c +)
   Destination:    FF         Data in        LEDEN  (to RCLK_c +)

   Delay:               0.366ns  (63.9% logic, 36.1% route), 2 logic levels.

 Constraint Details:

      0.366ns physical path delay SLICE_30 to SLICE_30 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.379ns

 Physical Path Details:

      Data path SLICE_30 to SLICE_30:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R7C5A.CLK to       R7C5A.Q0 SLICE_30 (from RCLK_c)
ROUTE         4     0.132       R7C5A.Q0 to       R7C5A.A0 LEDEN
CTOF_DEL    ---     0.101       R7C5A.A0 to       R7C5A.F0 SLICE_30
ROUTE         1     0.000       R7C5A.F0 to      R7C5A.DI0 LEDENe_0 (to RCLK_c)
                  --------
                    0.366   (63.9% logic, 36.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_30:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R7C5A.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_30:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R7C5A.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.


Passed: The following path meets requirements by 0.379ns

 Logical Details:  Cell type  Pin type       Cell/ASIC name  (clock net +/-)

   Source:         FF         Q              n8MEGEN  (from RCLK_c +)
   Destination:    FF         Data in        n8MEGEN  (to RCLK_c +)

   Delay:               0.366ns  (63.9% logic, 36.1% route), 2 logic levels.

 Constraint Details:

      0.366ns physical path delay SLICE_45 to SLICE_45 meets
     -0.013ns DIN_HLD and
      0.000ns delay constraint less
      0.000ns skew requirement (totaling -0.013ns) by 0.379ns

 Physical Path Details:

      Data path SLICE_45 to SLICE_45:

   Name    Fanout   Delay (ns)          Site               Resource
REG_DEL     ---     0.133      R5C5B.CLK to       R5C5B.Q0 SLICE_45 (from RCLK_c)
ROUTE         3     0.132       R5C5B.Q0 to       R5C5B.A0 n8MEGEN
CTOF_DEL    ---     0.101       R5C5B.A0 to       R5C5B.F0 SLICE_45
ROUTE         1     0.000       R5C5B.F0 to      R5C5B.DI0 n8MEGENe_0 (to RCLK_c)
                  --------
                    0.366   (63.9% logic, 36.1% route), 2 logic levels.

 Clock Skew Details: 

      Source Clock Path RCLK to SLICE_45:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R5C5B.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

      Destination Clock Path RCLK to SLICE_45:

   Name    Fanout   Delay (ns)          Site               Resource
ROUTE        48     0.788       63.PADDI to      R5C5B.CLK RCLK_c
                  --------
                    0.788   (0.0% logic, 100.0% route), 0 logic levels.

Report Summary
--------------
----------------------------------------------------------------------------
Preference(MIN Delays)                  |   Constraint|       Actual|Levels
----------------------------------------------------------------------------
                                        |             |             |
FREQUENCY PORT "PHI2" 2.900000 MHz ;    |            -|            -|   2  
                                        |             |             |
FREQUENCY PORT "nCCAS" 2.900000 MHz ;   |            -|            -|   0  
                                        |             |             |
FREQUENCY PORT "nCRAS" 2.900000 MHz ;   |            -|            -|   0  
                                        |             |             |
FREQUENCY PORT "RCLK" 62.500000 MHz ;   |            -|            -|   1  
                                        |             |             |
----------------------------------------------------------------------------


All preferences were met.


Clock Domains Analysis
------------------------

Found 4 clocks:

Clock Domain: nCRAS_c   Source: nCRAS.PAD   Loads: 11
   No transfer within this clock domain is found

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: nCCAS_c   Source: nCCAS.PAD   Loads: 10
   No transfer within this clock domain is found

Clock Domain: RCLK_c   Source: RCLK.PAD   Loads: 48
   Covered under: FREQUENCY PORT "RCLK" 62.500000 MHz ;

   Data transfers from:
   Clock Domain: nCRAS_c   Source: nCRAS.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

   Clock Domain: PHI2_c   Source: PHI2.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.

Clock Domain: PHI2_c   Source: PHI2.PAD   Loads: 21
   Covered under: FREQUENCY PORT "PHI2" 2.900000 MHz ;

   Data transfers from:
   Clock Domain: RCLK_c   Source: RCLK.PAD
      Not reported because source and destination domains are unrelated.
      To report these transfers please refer to preference CLKSKEWDIFF to define
      external clock skew between clock ports.


Timing summary (Hold):
---------------

Timing errors: 0  Score: 0
Cumulative negative slack: 0

Constraints cover 1038 paths, 4 nets, and 750 connections (74.18% coverage)



Timing summary (Setup and Hold):
---------------

Timing errors: 0 (setup), 0 (hold)
Score: 0 (setup), 0 (hold)
Cumulative negative slack: 0 (0+0)
--------------------------------------------------------------------------------

--------------------------------------------------------------------------------

