(kicad_pcb (version 20171130) (host pcbnew "(5.1.8-0-10_14)")

  (general
    (thickness 1.6)
    (drawings 67)
    (tracks 32)
    (zones 0)
    (modules 4)
    (nets 33)
  )

  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./edge-card-32v2"))
  )

  (net 0 "")
  (net 1 "Net-(J1-Pad16)")
  (net 2 "Net-(J1-Pad15)")
  (net 3 "Net-(J1-Pad14)")
  (net 4 "Net-(J1-Pad13)")
  (net 5 "Net-(J1-Pad12)")
  (net 6 "Net-(J1-Pad11)")
  (net 7 "Net-(J1-Pad10)")
  (net 8 "Net-(J1-Pad9)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad7)")
  (net 11 "Net-(J1-Pad6)")
  (net 12 "Net-(J1-Pad5)")
  (net 13 "Net-(J1-Pad4)")
  (net 14 "Net-(J1-Pad3)")
  (net 15 "Net-(J1-Pad2)")
  (net 16 "Net-(J1-Pad1)")
  (net 17 "Net-(J2-Pad16)")
  (net 18 "Net-(J2-Pad15)")
  (net 19 "Net-(J2-Pad14)")
  (net 20 "Net-(J2-Pad13)")
  (net 21 "Net-(J2-Pad12)")
  (net 22 "Net-(J2-Pad11)")
  (net 23 "Net-(J2-Pad10)")
  (net 24 "Net-(J2-Pad9)")
  (net 25 "Net-(J2-Pad8)")
  (net 26 "Net-(J2-Pad7)")
  (net 27 "Net-(J2-Pad6)")
  (net 28 "Net-(J2-Pad5)")
  (net 29 "Net-(J2-Pad4)")
  (net 30 "Net-(J2-Pad3)")
  (net 31 "Net-(J2-Pad2)")
  (net 32 "Net-(J2-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x16_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 662941FD)
    (at 94.3864 101.5492 180)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (path /66297E5E)
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value card (at 0 40.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 39.37) (end -1.27 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 39.37) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 39.43) (end 1.33 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 39.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 39.9) (end 1.8 39.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 39.9) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 19.05 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad15)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x16_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 6629412A)
    (at 79.1422 63.4492)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (path /6629981F)
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value card (at 0 40.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 39.37) (end -1.27 39.37) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 39.37) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 39.43) (end 1.33 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 39.43) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 39.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 39.9) (end 1.8 39.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 39.9) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 19.05 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x16_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC) (tstamp 619BAD22)
    (at 84.2264 63.4492 180)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (path /61AFC6D5)
    (fp_text reference J1 (at 0 2.33) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value card (at 0 -40.43) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 -39.9) (end 1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -39.9) (end 1.8 -39.9) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end -1.8 -39.9) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.27) (end 1.33 -39.43) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end -1.33 -39.43) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -39.43) (end 1.33 -39.43) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 -39.37) (end -1.27 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 -39.37) (end -1.27 -39.37) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end 1.27 -39.37) (layer B.Fab) (width 0.1))
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 -19.05 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x16_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC) (tstamp 6621ACE3)
    (at 89.3064 101.5492)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (path /66251E72)
    (fp_text reference J2 (at 0 2.33) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value card (at 0 -40.43) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 -39.9) (end 1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -39.9) (end 1.8 -39.9) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end -1.8 -39.9) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.27) (end 1.33 -39.43) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end -1.33 -39.43) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -39.43) (end 1.33 -39.43) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 -39.37) (end -1.27 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 -39.37) (end -1.27 -39.37) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end 1.27 -39.37) (layer B.Fab) (width 0.1))
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer B.Fab) (width 0.1))
    (fp_text user %R (at 0 -19.05 -90) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad 16 thru_hole oval (at 0 -38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 -35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad15)"))
    (pad 14 thru_hole oval (at 0 -33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad14)"))
    (pad 13 thru_hole oval (at 0 -30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text "24 pin edge card to DIP" (at 86.7 85 90) (layer B.SilkS) (tstamp 662A6CF3)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text "30 pin edge card to DIP" (at 86.7 85 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_line (start 80.2 72.3392) (end 93.3 72.4) (layer B.SilkS) (width 0.15))
  (gr_line (start 84.1502 102.9208) (end 84.1502 64.7192) (layer F.SilkS) (width 0.15) (tstamp 6621C390))
  (gr_line (start 89.3318 102.9208) (end 84.1502 102.9208) (layer F.SilkS) (width 0.15))
  (gr_line (start 89.3318 64.7192) (end 89.3318 102.9208) (layer F.SilkS) (width 0.15))
  (gr_line (start 80.5 64.7192) (end 93.1 64.7) (layer F.SilkS) (width 0.15))
  (gr_text 16 (at 92 101.5492) (layer F.SilkS) (tstamp 6621C38E)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 17 (at 92 99) (layer F.SilkS) (tstamp 6621C023)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 18 (at 92 96.4692) (layer F.SilkS) (tstamp 6621C020)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 19 (at 92 93.9292) (layer F.SilkS) (tstamp 6621C01D)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 20 (at 92 91.3892) (layer F.SilkS) (tstamp 6621C01A)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 21 (at 92 88.8492) (layer F.SilkS) (tstamp 6621C017)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 22 (at 92 86.3092) (layer F.SilkS) (tstamp 6621C014)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 23 (at 92 83.7692) (layer F.SilkS) (tstamp 6621C011)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 24 (at 92 81.2292) (layer F.SilkS) (tstamp 6621C00E)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 25 (at 92 78.6892) (layer F.SilkS) (tstamp 6621C00B)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 26 (at 92 76.1492) (layer F.SilkS) (tstamp 6621C008)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 27 (at 92 73.6092) (layer F.SilkS) (tstamp 6621C005)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 15 (at 81.5 101.5492) (layer F.SilkS) (tstamp 6621BF0D)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 14 (at 81.5 99) (layer F.SilkS) (tstamp 6621BF0A)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 13 (at 81.5 96.4692) (layer F.SilkS) (tstamp 6621BF07)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 12 (at 81.5 93.9292) (layer F.SilkS) (tstamp 6621BF04)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 11 (at 81.5 91.3892) (layer F.SilkS) (tstamp 6621BF01)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 10 (at 81.5 88.8492) (layer F.SilkS) (tstamp 6621BEFE)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 9 (at 81.5 86.3092) (layer F.SilkS) (tstamp 6621BE07)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 8 (at 81.5 83.7692) (layer F.SilkS) (tstamp 6621BE04)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 7 (at 81.5 81.2546) (layer F.SilkS) (tstamp 6621BE01)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 6 (at 81.5 78.74) (layer F.SilkS) (tstamp 6621BDFE)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 5 (at 81.5 76.1492) (layer F.SilkS) (tstamp 6621BDFB)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 4 (at 81.5 73.6346) (layer F.SilkS) (tstamp 6621BDF8)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 3 (at 81.5 71.0692) (layer F.SilkS) (tstamp 6621BD01)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 2 (at 81.5 68.5292) (layer F.SilkS) (tstamp 6621BCFE)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 28 (at 92 71.0692) (layer F.SilkS) (tstamp 6621BCFA)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 29 (at 92 68.5292) (layer F.SilkS) (tstamp 6621BCF7)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 30 (at 92 65.9892) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_line (start 91.2 62.1538) (end 91.2 102.7176) (layer Dwgs.User) (width 0.15))
  (gr_line (start 82.2198 62.5094) (end 82.2198 102.5144) (layer Dwgs.User) (width 0.15) (tstamp 6621B8DA))
  (gr_text 1 (at 81.5 65.9892) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 24 (at 81.28 73.5838) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 23 (at 81.28 76.1492) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 22 (at 81.28 78.6892) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 21 (at 81.28 81.2292) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 20 (at 81.28 83.7438) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 19 (at 81.28 86.3092) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 18 (at 81.28 88.8492) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 17 (at 81.28 91.3892) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 16 (at 81.28 93.9292) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 15 (at 81.28 96.4692) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 14 (at 81.28 99.0092) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 13 (at 81.28 101.5492) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 12 (at 92.3 101.5492) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 11 (at 92.3 99.0092) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 10 (at 92.3 96.4) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 9 (at 92.3 93.9292) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 8 (at 92.3 91.4146) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 7 (at 92.3 88.8492) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 6 (at 92.3 86.3092) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 5 (at 92.3 83.7692) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 4 (at 92.3 81.2292) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 3 (at 92.3 78.6892) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 2 (at 92.3 76.1492) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_text 1 (at 92.3 73.6) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (gr_line (start 76.0922 104.5334) (end 76.0922 60.5334) (layer Edge.Cuts) (width 0.05) (tstamp 619B151C))
  (gr_line (start 97.0922 104.5334) (end 76.0922 104.5334) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.0922 60.5334) (end 97.0922 104.5334) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.0922 60.5334) (end 97.0922 60.5334) (layer Edge.Cuts) (width 0.05))

  (segment (start 79.1422 101.5492) (end 84.2264 101.5492) (width 0.25) (layer B.Cu) (net 1))
  (segment (start 79.1422 99.0092) (end 84.2264 99.0092) (width 0.25) (layer B.Cu) (net 2))
  (segment (start 79.1422 96.4692) (end 84.2264 96.4692) (width 0.25) (layer B.Cu) (net 3))
  (segment (start 79.1422 93.9292) (end 84.2264 93.9292) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 79.1422 91.3892) (end 84.2264 91.3892) (width 0.25) (layer B.Cu) (net 5))
  (segment (start 79.1422 88.8492) (end 84.2264 88.8492) (width 0.25) (layer B.Cu) (net 6))
  (segment (start 79.1422 86.3092) (end 84.2264 86.3092) (width 0.25) (layer B.Cu) (net 7))
  (segment (start 79.1422 83.7692) (end 84.2264 83.7692) (width 0.25) (layer B.Cu) (net 8))
  (segment (start 79.1422 81.2292) (end 84.2264 81.2292) (width 0.25) (layer B.Cu) (net 9))
  (segment (start 79.1422 78.6892) (end 84.2264 78.6892) (width 0.25) (layer B.Cu) (net 10))
  (segment (start 79.1422 76.1492) (end 84.2264 76.1492) (width 0.25) (layer B.Cu) (net 11))
  (segment (start 79.1422 73.6092) (end 84.2264 73.6092) (width 0.25) (layer B.Cu) (net 12))
  (segment (start 79.1422 71.0692) (end 84.2264 71.0692) (width 0.25) (layer B.Cu) (net 13))
  (segment (start 79.1422 68.5292) (end 84.2264 68.5292) (width 0.25) (layer B.Cu) (net 14))
  (segment (start 79.1422 65.9892) (end 84.2264 65.9892) (width 0.25) (layer B.Cu) (net 15))
  (segment (start 79.1422 63.4492) (end 84.2264 63.4492) (width 0.25) (layer B.Cu) (net 16))
  (segment (start 89.3064 63.4492) (end 94.3822 63.4492) (width 0.25) (layer B.Cu) (net 17))
  (segment (start 89.3064 65.9892) (end 94.3822 65.9892) (width 0.25) (layer B.Cu) (net 18))
  (segment (start 89.3064 68.5292) (end 94.3822 68.5292) (width 0.25) (layer B.Cu) (net 19))
  (segment (start 89.3064 71.0692) (end 94.3822 71.0692) (width 0.25) (layer B.Cu) (net 20))
  (segment (start 89.3064 73.6092) (end 94.3822 73.6092) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 89.3064 76.1492) (end 94.3822 76.1492) (width 0.25) (layer B.Cu) (net 22))
  (segment (start 89.3064 78.6892) (end 94.3822 78.6892) (width 0.25) (layer B.Cu) (net 23))
  (segment (start 89.3064 81.2292) (end 94.3822 81.2292) (width 0.25) (layer B.Cu) (net 24))
  (segment (start 89.3064 83.7692) (end 94.3822 83.7692) (width 0.25) (layer B.Cu) (net 25))
  (segment (start 89.3064 86.3092) (end 94.3822 86.3092) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 89.3064 88.8492) (end 94.3822 88.8492) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 89.3064 91.3892) (end 94.3822 91.3892) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 89.3064 93.9292) (end 94.3822 93.9292) (width 0.25) (layer B.Cu) (net 29))
  (segment (start 89.3064 96.4692) (end 94.3822 96.4692) (width 0.25) (layer B.Cu) (net 30))
  (segment (start 89.3064 99.0092) (end 94.3822 99.0092) (width 0.25) (layer B.Cu) (net 31))
  (segment (start 89.3064 101.5492) (end 94.3822 101.5492) (width 0.25) (layer B.Cu) (net 32))

)
