(module AppleII (layer F.Cu) (tedit 629162E1)
  (descr "surface-mounted straight pin header, 2x25, 2.54mm pitch, double rows")
  (tags "Surface mounted pin header SMD 2x25 2.54mm double row")
  (attr smd)
  (fp_text reference J1 (at 4.7625 30.1625 270 unlocked) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "Apple II" (at 4.7625 -28.575 270 unlocked) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.5875 -32.7) (end -5.9 -32.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.5875 32.7) (end 1.5875 -32.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.9 32.7) (end 1.5875 32.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.9 -32.7) (end -5.9 32.7) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.6 -30.16) (end -2.54 -30.16) (layer F.Fab) (width 0.1))
  (fp_line (start -3.6 -30.8) (end -3.6 -30.16) (layer F.Fab) (width 0.1))
  (fp_line (start -2.54 -30.8) (end -3.6 -30.8) (layer F.Fab) (width 0.1))
  (pad 50 smd rect (at -1.5875 -30.48) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 49 smd rect (at -1.5875 -27.94) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 48 smd rect (at -1.5875 -25.4) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 47 smd rect (at -1.5875 -22.86) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 46 smd rect (at -1.5875 -20.32) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 45 smd rect (at -1.5875 -17.78) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 44 smd rect (at -1.5875 -15.24) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 43 smd rect (at -1.5875 -12.7) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 42 smd rect (at -1.5875 -10.16) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 41 smd rect (at -1.5875 -7.62) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 40 smd rect (at -1.5875 -5.08) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 39 smd rect (at -1.5875 -2.54) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 38 smd rect (at -1.5875 0) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 37 smd rect (at -1.5875 2.54) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 36 smd rect (at -1.5875 5.08) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 35 smd rect (at -1.5875 7.62) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 34 smd rect (at -1.5875 10.16) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 33 smd rect (at -1.5875 12.7) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 32 smd rect (at -1.5875 15.24) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 31 smd rect (at -1.5875 17.78) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 30 smd rect (at -1.5875 20.32) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 29 smd rect (at -1.5875 22.86) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 28 smd rect (at -1.5875 25.4) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 27 smd rect (at -1.5875 27.94) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 26 smd rect (at -1.5875 30.48) (size 8 1.4) (layers B.Cu B.Paste B.Mask))
  (pad 25 smd rect (at -1.5875 30.48) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at -1.5875 27.94) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at -1.5875 25.4) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at -1.5875 22.86) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at -1.5875 20.32) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -1.5875 17.78) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -1.5875 15.24) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -1.5875 12.7) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -1.5875 10.16) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -1.5875 7.62) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -1.5875 5.08) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -1.5875 2.54) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -1.5875 0) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -1.5875 -2.54) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -1.5875 -5.08) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -1.5875 -7.62) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.5875 -10.16) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -1.5875 -12.7) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -1.5875 -15.24) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.5875 -17.78) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.5875 -20.32) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.5875 -22.86) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.5875 -25.4) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.5875 -27.94) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.5875 -30.48) (size 8 1.4) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x25_P2.54mm_Vertical_SMD.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
