(export (version D)
  (design
    (source C:\Users\Grizzly\Documents\DasUberTerm\PCB\DasUberTerm.sch)
    (date "5/27/2022 7:48:33 PM")
    (tool "Eeschema (5.1.10)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source DasUberTerm.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J2)
      (value "MKR VIDOR 4000")
      (footprint Connector_PCBEdge:BUS_PCI_Express_Mini_Half)
      (datasheet ~)
      (libsource (lib Connector) (part Bus_PCI_Express_Mini) (description "Mini-PCI Express bus connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6291A584))
    (comp (ref J1)
      (value "Apple II")
      (footprint STDBUS:AppleII)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x25_Counter_Clockwise) (description "Generic connector, double row, 02x25, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 629381EB))
    (comp (ref J3)
      (value "MKR VIDOR 4000")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x14) (description "Generic connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 629D1345))
    (comp (ref J4)
      (value "MKR VIDOR 4000")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x14) (description "Generic connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 629D29DB))
    (comp (ref U1)
      (value SN74LVC8T245DGVR)
      (footprint Package_SO:TSSOP-24_4.4x5mm_P0.4mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x12_Counter_Clockwise) (description "Generic connector, double row, 02x12, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62A8607A))
    (comp (ref U2)
      (value SN74LVC8T245DGVR)
      (footprint Package_SO:TSSOP-24_4.4x5mm_P0.4mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x12_Counter_Clockwise) (description "Generic connector, double row, 02x12, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62A87454))
    (comp (ref U3)
      (value SN74LVC8T245DGVR)
      (footprint Package_SO:TSSOP-24_4.4x5mm_P0.4mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x12_Counter_Clockwise) (description "Generic connector, double row, 02x12, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62A887EA))
    (comp (ref U4)
      (value SN74LVC8T245DGVR)
      (footprint Package_SO:TSSOP-24_4.4x5mm_P0.4mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x12_Counter_Clockwise) (description "Generic connector, double row, 02x12, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62A898B8))
    (comp (ref R3)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B78737))
    (comp (ref R6)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B81CAC))
    (comp (ref R7)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B8B68F))
    (comp (ref R5)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62B95325))
    (comp (ref R1)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62BA8CC7))
    (comp (ref R4)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62BB2E94))
    (comp (ref U5)
      (value SN74LVC2T45DCUT)
      (footprint Package_SO:VSSOP-8_2.3x2mm_P0.5mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x04_Counter_Clockwise) (description "Generic connector, double row, 02x04, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62DB7B52))
    (comp (ref Q1)
      (value 2N3904)
      (footprint Package_TO_SOT_THT:TO-92_HandSolder)
      (datasheet https://www.onsemi.com/pub/Collateral/2N3903-D.PDF)
      (libsource (lib Transistor_BJT) (part 2N3904) (description "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"))
      (sheetpath (names /) (tstamps /))
      (tstamp 62EAF7EA))
    (comp (ref R2)
      (value R)
      (footprint Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 62EE8D3D)))
  (libparts
    (libpart (lib Connector) (part Bus_PCI_Express_Mini)
      (description "Mini-PCI Express bus connector")
      (docs ~)
      (footprints
        (fp *PCI*Express*Mini*))
      (fields
        (field (name Reference) J)
        (field (name Value) Bus_PCI_Express_Mini))
      (pins
        (pin (num 1) (name ~WAKE) (type openCol))
        (pin (num 2) (name +3V3AUX) (type power_in))
        (pin (num 3) (name COEX1) (type passive))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name COEX2) (type passive))
        (pin (num 6) (name +1V5) (type power_in))
        (pin (num 7) (name ~CLKREQ) (type openCol))
        (pin (num 8) (name UIM_PWR) (type power_out))
        (pin (num 9) (name GND) (type passive))
        (pin (num 10) (name UIM_DATA) (type BiDi))
        (pin (num 11) (name REFCLK-) (type input))
        (pin (num 12) (name UIM_CLK) (type output))
        (pin (num 13) (name REFCLK+) (type input))
        (pin (num 14) (name ~UIM_RESET) (type output))
        (pin (num 15) (name GND) (type passive))
        (pin (num 16) (name UIM_VPP) (type power_out))
        (pin (num 17) (name UIM_C8) (type passive))
        (pin (num 18) (name GND) (type passive))
        (pin (num 19) (name UIM_C4) (type passive))
        (pin (num 20) (name ~W_DISABLE) (type input))
        (pin (num 21) (name GND) (type passive))
        (pin (num 22) (name ~PERST) (type input))
        (pin (num 23) (name PERn0) (type output))
        (pin (num 24) (name +3V3AUX) (type power_in))
        (pin (num 25) (name PERp0) (type output))
        (pin (num 26) (name GND) (type passive))
        (pin (num 27) (name GND) (type passive))
        (pin (num 28) (name +1V5) (type power_in))
        (pin (num 29) (name GND) (type passive))
        (pin (num 30) (name SMB_CLK) (type input))
        (pin (num 31) (name PETn0) (type input))
        (pin (num 32) (name SMB_DATA) (type BiDi))
        (pin (num 33) (name PETp0) (type input))
        (pin (num 34) (name GND) (type passive))
        (pin (num 35) (name GND) (type passive))
        (pin (num 36) (name USB_D-) (type BiDi))
        (pin (num 37) (name GND) (type passive))
        (pin (num 38) (name USB_D+) (type BiDi))
        (pin (num 39) (name +3V3AUX) (type power_in))
        (pin (num 40) (name GND) (type passive))
        (pin (num 41) (name +3V3AUX) (type power_in))
        (pin (num 42) (name ~LED_WWAN) (type openCol))
        (pin (num 43) (name GND) (type passive))
        (pin (num 44) (name ~LED_WLAN) (type openCol))
        (pin (num 45) (name Reserved) (type passive))
        (pin (num 46) (name ~LED_WPAN) (type openCol))
        (pin (num 47) (name Reserved) (type passive))
        (pin (num 48) (name +1V5) (type power_in))
        (pin (num 49) (name Reserved) (type passive))
        (pin (num 50) (name GND) (type passive))
        (pin (num 51) (name Reserved) (type passive))
        (pin (num 52) (name +3V3AUX) (type power_in))
        (pin (num MP) (name MP) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x14)
      (description "Generic connector, single row, 01x14, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x14))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x04_Counter_Clockwise)
      (description "Generic connector, double row, 02x04, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x04_Counter_Clockwise))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x12_Counter_Clockwise)
      (description "Generic connector, double row, 02x12, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x12_Counter_Clockwise))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x25_Counter_Clockwise)
      (description "Generic connector, double row, 02x25, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x25_Counter_Clockwise))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))
        (pin (num 25) (name Pin_25) (type passive))
        (pin (num 26) (name Pin_26) (type passive))
        (pin (num 27) (name Pin_27) (type passive))
        (pin (num 28) (name Pin_28) (type passive))
        (pin (num 29) (name Pin_29) (type passive))
        (pin (num 30) (name Pin_30) (type passive))
        (pin (num 31) (name Pin_31) (type passive))
        (pin (num 32) (name Pin_32) (type passive))
        (pin (num 33) (name Pin_33) (type passive))
        (pin (num 34) (name Pin_34) (type passive))
        (pin (num 35) (name Pin_35) (type passive))
        (pin (num 36) (name Pin_36) (type passive))
        (pin (num 37) (name Pin_37) (type passive))
        (pin (num 38) (name Pin_38) (type passive))
        (pin (num 39) (name Pin_39) (type passive))
        (pin (num 40) (name Pin_40) (type passive))
        (pin (num 41) (name Pin_41) (type passive))
        (pin (num 42) (name Pin_42) (type passive))
        (pin (num 43) (name Pin_43) (type passive))
        (pin (num 44) (name Pin_44) (type passive))
        (pin (num 45) (name Pin_45) (type passive))
        (pin (num 46) (name Pin_46) (type passive))
        (pin (num 47) (name Pin_47) (type passive))
        (pin (num 48) (name Pin_48) (type passive))
        (pin (num 49) (name Pin_49) (type passive))
        (pin (num 50) (name Pin_50) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Transistor_BJT) (part 2N3904)
      (description "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
      (docs https://www.onsemi.com/pub/Collateral/2N3903-D.PDF)
      (footprints
        (fp TO?92*))
      (fields
        (field (name Reference) Q)
        (field (name Value) 2N3904)
        (field (name Footprint) Package_TO_SOT_THT:TO-92_Inline))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Connector_Generic)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical Transistor_BJT)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Transistor_BJT.lib")))
  (nets
    (net (code 1) (name LD3)
      (node (ref J4) (pin 12))
      (node (ref U1) (pin 18)))
    (net (code 2) (name LD2)
      (node (ref J4) (pin 11))
      (node (ref U1) (pin 19)))
    (net (code 3) (name LD1)
      (node (ref J4) (pin 10))
      (node (ref U1) (pin 20)))
    (net (code 4) (name LD0)
      (node (ref J4) (pin 9))
      (node (ref U1) (pin 21)))
    (net (code 5) (name 3V3)
      (node (ref J2) (pin 2))
      (node (ref U3) (pin 24))
      (node (ref J2) (pin 39))
      (node (ref U2) (pin 23))
      (node (ref J2) (pin 24))
      (node (ref J2) (pin 52))
      (node (ref J2) (pin 41))
      (node (ref U3) (pin 23))
      (node (ref U2) (pin 24))
      (node (ref J3) (pin 3))
      (node (ref U4) (pin 23))
      (node (ref U4) (pin 24))
      (node (ref U1) (pin 24))
      (node (ref U1) (pin 23))
      (node (ref U5) (pin 8)))
    (net (code 6) (name nACTIVE)
      (node (ref U1) (pin 22))
      (node (ref U5) (pin 2)))
    (net (code 7) (name D3)
      (node (ref J1) (pin 46))
      (node (ref U1) (pin 6)))
    (net (code 8) (name D0)
      (node (ref J1) (pin 49))
      (node (ref U1) (pin 3)))
    (net (code 9) (name GND)
      (node (ref U5) (pin 4))
      (node (ref U5) (pin 5))
      (node (ref Q1) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref J2) (pin 18))
      (node (ref U1) (pin 11))
      (node (ref U4) (pin 11))
      (node (ref U4) (pin 12))
      (node (ref U4) (pin 13))
      (node (ref J3) (pin 4))
      (node (ref J1) (pin 26))
      (node (ref U1) (pin 13))
      (node (ref U1) (pin 12))
      (node (ref J2) (pin 21))
      (node (ref J2) (pin 50))
      (node (ref J2) (pin 43))
      (node (ref J2) (pin 40))
      (node (ref J2) (pin 9))
      (node (ref J2) (pin 26))
      (node (ref J2) (pin 27))
      (node (ref J2) (pin 29))
      (node (ref J2) (pin 4))
      (node (ref J2) (pin 34))
      (node (ref J2) (pin 35))
      (node (ref J2) (pin 37))
      (node (ref R3) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref J2) (pin 15))
      (node (ref U2) (pin 13))
      (node (ref U2) (pin 12))
      (node (ref U2) (pin 11))
      (node (ref U3) (pin 13))
      (node (ref U3) (pin 12))
      (node (ref U3) (pin 11)))
    (net (code 10) (name nLACTIVE)
      (node (ref U5) (pin 7))
      (node (ref J2) (pin 33)))
    (net (code 11) (name D2)
      (node (ref U1) (pin 5))
      (node (ref J1) (pin 47)))
    (net (code 12) (name D5)
      (node (ref U1) (pin 8))
      (node (ref J1) (pin 44)))
    (net (code 13) (name LD5)
      (node (ref U1) (pin 16))
      (node (ref J4) (pin 14)))
    (net (code 14) (name LD4)
      (node (ref J4) (pin 13))
      (node (ref U1) (pin 17)))
    (net (code 15) (name LD7)
      (node (ref J3) (pin 13))
      (node (ref U1) (pin 14)))
    (net (code 16) (name LD6)
      (node (ref J3) (pin 14))
      (node (ref U1) (pin 15)))
    (net (code 17) (name D7)
      (node (ref U1) (pin 10))
      (node (ref J1) (pin 42)))
    (net (code 18) (name D6)
      (node (ref U1) (pin 9))
      (node (ref J1) (pin 43)))
    (net (code 19) (name D4)
      (node (ref U1) (pin 7))
      (node (ref J1) (pin 45)))
    (net (code 20) (name D1)
      (node (ref U1) (pin 4))
      (node (ref J1) (pin 48)))
    (net (code 21) (name LA12)
      (node (ref J2) (pin 45))
      (node (ref U3) (pin 17)))
    (net (code 22) (name A5)
      (node (ref J1) (pin 7))
      (node (ref U2) (pin 8)))
    (net (code 23) (name A6)
      (node (ref U2) (pin 9))
      (node (ref J1) (pin 8)))
    (net (code 24) (name LA15)
      (node (ref U3) (pin 14))
      (node (ref J2) (pin 51)))
    (net (code 25) (name LA14)
      (node (ref U3) (pin 15))
      (node (ref J2) (pin 49)))
    (net (code 26) (name A4)
      (node (ref J1) (pin 6))
      (node (ref U2) (pin 7)))
    (net (code 27) (name LA11)
      (node (ref J2) (pin 48))
      (node (ref U3) (pin 18)))
    (net (code 28) (name "Net-(R6-Pad2)")
      (node (ref U3) (pin 22))
      (node (ref R6) (pin 2)))
    (net (code 29) (name A8)
      (node (ref U3) (pin 3))
      (node (ref J1) (pin 10)))
    (net (code 30) (name A9)
      (node (ref U3) (pin 4))
      (node (ref J1) (pin 11)))
    (net (code 31) (name LA2)
      (node (ref J2) (pin 10))
      (node (ref U2) (pin 19)))
    (net (code 32) (name A7)
      (node (ref J1) (pin 9))
      (node (ref U2) (pin 10)))
    (net (code 33) (name LA4)
      (node (ref U2) (pin 17))
      (node (ref J2) (pin 14)))
    (net (code 34) (name LA3)
      (node (ref J2) (pin 12))
      (node (ref U2) (pin 18)))
    (net (code 35) (name A10)
      (node (ref U3) (pin 5))
      (node (ref J1) (pin 12)))
    (net (code 36) (name LA1)
      (node (ref U2) (pin 20))
      (node (ref J2) (pin 8)))
    (net (code 37) (name LA0)
      (node (ref U2) (pin 21))
      (node (ref J2) (pin 6)))
    (net (code 38) (name A0)
      (node (ref J1) (pin 2))
      (node (ref U2) (pin 3)))
    (net (code 39) (name A1)
      (node (ref J1) (pin 3))
      (node (ref U2) (pin 4)))
    (net (code 40) (name A2)
      (node (ref J1) (pin 4))
      (node (ref U2) (pin 5)))
    (net (code 41) (name A3)
      (node (ref J1) (pin 5))
      (node (ref U2) (pin 6)))
    (net (code 42) (name "Net-(U4-Pad6)")
      (node (ref U4) (pin 6)))
    (net (code 43) (name "Net-(U4-Pad7)")
      (node (ref U4) (pin 7)))
    (net (code 44) (name "Net-(U4-Pad8)")
      (node (ref U4) (pin 8)))
    (net (code 45) (name "Net-(U4-Pad9)")
      (node (ref U4) (pin 9)))
    (net (code 46) (name +5V)
      (node (ref U5) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref J1) (pin 25))
      (node (ref J3) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref U4) (pin 1)))
    (net (code 47) (name "Net-(U4-Pad15)")
      (node (ref U4) (pin 15)))
    (net (code 48) (name A11)
      (node (ref U3) (pin 6))
      (node (ref J1) (pin 13)))
    (net (code 49) (name A12)
      (node (ref U3) (pin 7))
      (node (ref J1) (pin 14)))
    (net (code 50) (name "Net-(U4-Pad10)")
      (node (ref U4) (pin 10)))
    (net (code 51) (name "Net-(U4-Pad14)")
      (node (ref U4) (pin 14)))
    (net (code 52) (name LPHI0)
      (node (ref U4) (pin 17))
      (node (ref J2) (pin 11)))
    (net (code 53) (name LA7)
      (node (ref J2) (pin 28))
      (node (ref U2) (pin 14)))
    (net (code 54) (name LA6)
      (node (ref U2) (pin 15))
      (node (ref J2) (pin 20)))
    (net (code 55) (name LR\W)
      (node (ref J2) (pin 13))
      (node (ref U4) (pin 16)))
    (net (code 56) (name nLRESET)
      (node (ref U4) (pin 18)))
    (net (code 57) (name nROMINHIBIT)
      (node (ref J1) (pin 32))
      (node (ref Q1) (pin 3)))
    (net (code 58) (name nLROMINHIBIT)
      (node (ref R2) (pin 2)))
    (net (code 59) (name LA5)
      (node (ref U2) (pin 16))
      (node (ref J2) (pin 16)))
    (net (code 60) (name LA13)
      (node (ref U3) (pin 16))
      (node (ref J2) (pin 47)))
    (net (code 61) (name nROMRQ)
      (node (ref J1) (pin 1))
      (node (ref U4) (pin 5)))
    (net (code 62) (name LA10)
      (node (ref U3) (pin 19))
      (node (ref J2) (pin 46)))
    (net (code 63) (name LA9)
      (node (ref U3) (pin 20))
      (node (ref J2) (pin 44)))
    (net (code 64) (name LA8)
      (node (ref J2) (pin 42))
      (node (ref U3) (pin 21)))
    (net (code 65) (name nDDIR)
      (node (ref U1) (pin 2))
      (node (ref U5) (pin 3)))
    (net (code 66) (name "Net-(Q1-Pad2)")
      (node (ref Q1) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 67) (name nIORQ)
      (node (ref J1) (pin 41))
      (node (ref U4) (pin 4)))
    (net (code 68) (name nEXMEMRQ)
      (node (ref J1) (pin 20))
      (node (ref U4) (pin 3)))
    (net (code 69) (name nLDDIR)
      (node (ref U5) (pin 6)))
    (net (code 70) (name "Net-(R1-Pad1)")
      (node (ref U2) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 71) (name "Net-(R7-Pad2)")
      (node (ref R7) (pin 2))
      (node (ref U4) (pin 22)))
    (net (code 72) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1))
      (node (ref U4) (pin 2)))
    (net (code 73) (name "Net-(R4-Pad1)")
      (node (ref R4) (pin 1))
      (node (ref U3) (pin 2)))
    (net (code 74) (name nLEXMEMRQ)
      (node (ref U4) (pin 21))
      (node (ref J2) (pin 31)))
    (net (code 75) (name nLIORQ)
      (node (ref J2) (pin 25))
      (node (ref U4) (pin 20)))
    (net (code 76) (name nLROMRQ)
      (node (ref J2) (pin 23))
      (node (ref U4) (pin 19)))
    (net (code 77) (name "Net-(R3-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref U2) (pin 22)))
    (net (code 78) (name A13)
      (node (ref U3) (pin 8))
      (node (ref J1) (pin 15)))
    (net (code 79) (name A14)
      (node (ref U3) (pin 9))
      (node (ref J1) (pin 16)))
    (net (code 80) (name A15)
      (node (ref U3) (pin 10))
      (node (ref J1) (pin 17)))
    (net (code 81) (name "Net-(J2-Pad5)")
      (node (ref J2) (pin 5)))
    (net (code 82) (name "Net-(J2-Pad7)")
      (node (ref J2) (pin 7)))
    (net (code 83) (name "Net-(J2-PadMP)")
      (node (ref J2) (pin MP)))
    (net (code 84) (name "Net-(J2-Pad30)")
      (node (ref J2) (pin 30)))
    (net (code 85) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3)))
    (net (code 86) (name "Net-(J2-Pad32)")
      (node (ref J2) (pin 32)))
    (net (code 87) (name "Net-(J2-Pad36)")
      (node (ref J2) (pin 36)))
    (net (code 88) (name "Net-(J2-Pad38)")
      (node (ref J2) (pin 38)))
    (net (code 89) (name "Net-(J2-Pad19)")
      (node (ref J2) (pin 19)))
    (net (code 90) (name nLRST)
      (node (ref J2) (pin 22)))
    (net (code 91) (name "Net-(J2-Pad17)")
      (node (ref J2) (pin 17)))
    (net (code 92) (name "Net-(J2-Pad1)")
      (node (ref J2) (pin 1)))
    (net (code 93) (name nNMI)
      (node (ref J1) (pin 29)))
    (net (code 94) (name nIRQ)
      (node (ref J1) (pin 30)))
    (net (code 95) (name nDMA)
      (node (ref J1) (pin 22)))
    (net (code 96) (name nSYNC)
      (node (ref J1) (pin 19)))
    (net (code 97) (name -12V)
      (node (ref J1) (pin 33)))
    (net (code 98) (name nWR)
      (node (ref J1) (pin 18)))
    (net (code 99) (name nSYSRESET)
      (node (ref J1) (pin 31)))
    (net (code 100) (name +12V)
      (node (ref J1) (pin 50)))
    (net (code 101) (name FPGARESET)
      (node (ref J3) (pin 5)))
    (net (code 102) (name UARTRX)
      (node (ref J3) (pin 7)))
    (net (code 103) (name SCL)
      (node (ref J3) (pin 8)))
    (net (code 104) (name SDA)
      (node (ref J3) (pin 9)))
    (net (code 105) (name "Net-(J4-Pad7)")
      (node (ref J4) (pin 7)))
    (net (code 106) (name "Net-(J4-Pad2)")
      (node (ref J4) (pin 2)))
    (net (code 107) (name "Net-(J4-Pad3)")
      (node (ref J4) (pin 3)))
    (net (code 108) (name "Net-(J4-Pad4)")
      (node (ref J4) (pin 4)))
    (net (code 109) (name "Net-(J4-Pad5)")
      (node (ref J4) (pin 5)))
    (net (code 110) (name "Net-(J4-Pad6)")
      (node (ref J4) (pin 6)))
    (net (code 111) (name "Net-(J4-Pad8)")
      (node (ref J4) (pin 8)))
    (net (code 112) (name UARTTX)
      (node (ref J3) (pin 6)))
    (net (code 113) (name "Net-(J4-Pad1)")
      (node (ref J4) (pin 1)))
    (net (code 114) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1)))
    (net (code 115) (name "Net-(J1-Pad35)")
      (node (ref J1) (pin 35)))
    (net (code 116) (name 2MHz)
      (node (ref J1) (pin 37)))
    (net (code 117) (name nRDY)
      (node (ref J1) (pin 21)))
    (net (code 118) (name "Net-(J1-Pad23)")
      (node (ref J1) (pin 23))
      (node (ref J1) (pin 28)))
    (net (code 119) (name "Net-(J1-Pad24)")
      (node (ref J1) (pin 24))
      (node (ref J1) (pin 27)))
    (net (code 120) (name "Net-(J3-Pad12)")
      (node (ref J3) (pin 12)))
    (net (code 121) (name PHI1)
      (node (ref J1) (pin 38)))
    (net (code 122) (name PHI0)
      (node (ref J1) (pin 40)))
    (net (code 123) (name USER1)
      (node (ref J1) (pin 39)))
    (net (code 124) (name "Net-(J3-Pad10)")
      (node (ref J3) (pin 10)))
    (net (code 125) (name "Net-(J3-Pad11)")
      (node (ref J3) (pin 11)))
    (net (code 126) (name -5V)
      (node (ref J1) (pin 34)))
    (net (code 127) (name 7MHz)
      (node (ref J1) (pin 36)))))