(module kbd_mounting_holes_only (layer F.Cu) (tedit 5EF57261)
  (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
  (tags "Through hole pin header THT 2x20 2.54mm double row")
  (fp_text reference REF** (at 1.2954 -2.5078) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "Interface mount" (at 1.27 50.59) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "" np_thru_hole circle (at 91.4924 50.4712) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 91.4924 -2.8688) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 1.2954 -8.8124) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 1.2954 54.5606) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
    (offset (xyz 2.54 0 -1.8288))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 0))
  )
)
