;------------------------------------------------------------------------------
; @file regs.ddf
; @brief Device Description File for use with IAR's C-SPY
;
; To see all registers defined in Embedded Workbench's C-SPY Register window,
; this file must be pointed to under
;   Project > Options > Debugger > Device description file
;
; Please Note: This file is automatically generated, and should not
;       be directly edited
;
; COPYRIGHT 2010 STMicroelectronics. All rights reserved. 
;------------------------------------------------------------------------------


; Start of SFR definition.
[Sfr]
;     Name                                              Zone       Address      Bytesize  Displaybase  Bitrange
;     ----                                              ----       -------      --------  -----------  --------

sfr = "INT_TIM1FLAG",                                   "Memory",  0x4000A800,  4,        base=16
sfr = "INT_TIM1FLAG.INT_TIMRSVD",                       "Memory",  0x4000A800,  4,        base=16,     bitMask=0x00001E00
sfr = "INT_TIM1FLAG.INT_TIMTIF",                        "Memory",  0x4000A800,  4,        base=16,     bitMask=0x00000040
sfr = "INT_TIM1FLAG.INT_TIMCC4IF",                      "Memory",  0x4000A800,  4,        base=16,     bitMask=0x00000010
sfr = "INT_TIM1FLAG.INT_TIMCC3IF",                      "Memory",  0x4000A800,  4,        base=16,     bitMask=0x00000008
sfr = "INT_TIM1FLAG.INT_TIMCC2IF",                      "Memory",  0x4000A800,  4,        base=16,     bitMask=0x00000004
sfr = "INT_TIM1FLAG.INT_TIMCC1IF",                      "Memory",  0x4000A800,  4,        base=16,     bitMask=0x00000002
sfr = "INT_TIM1FLAG.INT_TIMUIF",                        "Memory",  0x4000A800,  4,        base=16,     bitMask=0x00000001

sfr = "INT_TIM2FLAG",                                   "Memory",  0x4000A804,  4,        base=16
sfr = "INT_TIM2FLAG.INT_TIMRSVD",                       "Memory",  0x4000A804,  4,        base=16,     bitMask=0x00001E00
sfr = "INT_TIM2FLAG.INT_TIMTIF",                        "Memory",  0x4000A804,  4,        base=16,     bitMask=0x00000040
sfr = "INT_TIM2FLAG.INT_TIMCC4IF",                      "Memory",  0x4000A804,  4,        base=16,     bitMask=0x00000010
sfr = "INT_TIM2FLAG.INT_TIMCC3IF",                      "Memory",  0x4000A804,  4,        base=16,     bitMask=0x00000008
sfr = "INT_TIM2FLAG.INT_TIMCC2IF",                      "Memory",  0x4000A804,  4,        base=16,     bitMask=0x00000004
sfr = "INT_TIM2FLAG.INT_TIMCC1IF",                      "Memory",  0x4000A804,  4,        base=16,     bitMask=0x00000002
sfr = "INT_TIM2FLAG.INT_TIMUIF",                        "Memory",  0x4000A804,  4,        base=16,     bitMask=0x00000001

sfr = "INT_SC1FLAG",                                    "Memory",  0x4000A808,  4,        base=16
sfr = "INT_SC1FLAG.INT_SC1PARERR",                      "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00004000
sfr = "INT_SC1FLAG.INT_SC1FRMERR",                      "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00002000
sfr = "INT_SC1FLAG.INT_SCTXULDB",                       "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00001000
sfr = "INT_SC1FLAG.INT_SCTXULDA",                       "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000800
sfr = "INT_SC1FLAG.INT_SCRXULDB",                       "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000400
sfr = "INT_SC1FLAG.INT_SCRXULDA",                       "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000200
sfr = "INT_SC1FLAG.INT_SCNAK",                          "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000100
sfr = "INT_SC1FLAG.INT_SCCMDFIN",                       "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000080
sfr = "INT_SC1FLAG.INT_SCTXFIN",                        "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000040
sfr = "INT_SC1FLAG.INT_SCRXFIN",                        "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000020
sfr = "INT_SC1FLAG.INT_SCTXUND",                        "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000010
sfr = "INT_SC1FLAG.INT_SCRXOVF",                        "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000008
sfr = "INT_SC1FLAG.INT_SCTXIDLE",                       "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000004
sfr = "INT_SC1FLAG.INT_SCTXFREE",                       "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000002
sfr = "INT_SC1FLAG.INT_SCRXVAL",                        "Memory",  0x4000A808,  4,        base=16,     bitMask=0x00000001

sfr = "INT_SC2FLAG",                                    "Memory",  0x4000A80C,  4,        base=16
sfr = "INT_SC2FLAG.INT_SCTXULDB",                       "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00001000
sfr = "INT_SC2FLAG.INT_SCTXULDA",                       "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000800
sfr = "INT_SC2FLAG.INT_SCRXULDB",                       "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000400
sfr = "INT_SC2FLAG.INT_SCRXULDA",                       "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000200
sfr = "INT_SC2FLAG.INT_SCNAK",                          "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000100
sfr = "INT_SC2FLAG.INT_SCCMDFIN",                       "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000080
sfr = "INT_SC2FLAG.INT_SCTXFIN",                        "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000040
sfr = "INT_SC2FLAG.INT_SCRXFIN",                        "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000020
sfr = "INT_SC2FLAG.INT_SCTXUND",                        "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000010
sfr = "INT_SC2FLAG.INT_SCRXOVF",                        "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000008
sfr = "INT_SC2FLAG.INT_SCTXIDLE",                       "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000004
sfr = "INT_SC2FLAG.INT_SCTXFREE",                       "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000002
sfr = "INT_SC2FLAG.INT_SCRXVAL",                        "Memory",  0x4000A80C,  4,        base=16,     bitMask=0x00000001

sfr = "INT_ADCFLAG",                                    "Memory",  0x4000A810,  4,        base=16
sfr = "INT_ADCFLAG.INT_ADCOVF",                         "Memory",  0x4000A810,  4,        base=16,     bitMask=0x00000010
sfr = "INT_ADCFLAG.INT_ADCSAT",                         "Memory",  0x4000A810,  4,        base=16,     bitMask=0x00000008
sfr = "INT_ADCFLAG.INT_ADCULDFULL",                     "Memory",  0x4000A810,  4,        base=16,     bitMask=0x00000004
sfr = "INT_ADCFLAG.INT_ADCULDHALF",                     "Memory",  0x4000A810,  4,        base=16,     bitMask=0x00000002
sfr = "INT_ADCFLAG.INT_ADCFLAGRSVD",                    "Memory",  0x4000A810,  4,        base=16,     bitMask=0x00000001

sfr = "INT_GPIOFLAG",                                   "Memory",  0x4000A814,  4,        base=16
sfr = "INT_GPIOFLAG.INT_IRQDFLAG",                      "Memory",  0x4000A814,  4,        base=16,     bitMask=0x00000008
sfr = "INT_GPIOFLAG.INT_IRQCFLAG",                      "Memory",  0x4000A814,  4,        base=16,     bitMask=0x00000004
sfr = "INT_GPIOFLAG.INT_IRQBFLAG",                      "Memory",  0x4000A814,  4,        base=16,     bitMask=0x00000002
sfr = "INT_GPIOFLAG.INT_IRQAFLAG",                      "Memory",  0x4000A814,  4,        base=16,     bitMask=0x00000001

sfr = "INT_TIM1MISS",                                   "Memory",  0x4000A818,  4,        base=16
sfr = "INT_TIM1MISS.INT_TIMMISSCC4IF",                  "Memory",  0x4000A818,  4,        base=16,     bitMask=0x00001000
sfr = "INT_TIM1MISS.INT_TIMMISSCC3IF",                  "Memory",  0x4000A818,  4,        base=16,     bitMask=0x00000800
sfr = "INT_TIM1MISS.INT_TIMMISSCC2IF",                  "Memory",  0x4000A818,  4,        base=16,     bitMask=0x00000400
sfr = "INT_TIM1MISS.INT_TIMMISSCC1IF",                  "Memory",  0x4000A818,  4,        base=16,     bitMask=0x00000200
sfr = "INT_TIM1MISS.INT_TIMMISSRSVD",                   "Memory",  0x4000A818,  4,        base=16,     bitMask=0x0000007F

sfr = "INT_TIM2MISS",                                   "Memory",  0x4000A81C,  4,        base=16
sfr = "INT_TIM2MISS.INT_TIMMISSCC4IF",                  "Memory",  0x4000A81C,  4,        base=16,     bitMask=0x00001000
sfr = "INT_TIM2MISS.INT_TIMMISSCC3IF",                  "Memory",  0x4000A81C,  4,        base=16,     bitMask=0x00000800
sfr = "INT_TIM2MISS.INT_TIMMISSCC2IF",                  "Memory",  0x4000A81C,  4,        base=16,     bitMask=0x00000400
sfr = "INT_TIM2MISS.INT_TIMMISSCC1IF",                  "Memory",  0x4000A81C,  4,        base=16,     bitMask=0x00000200
sfr = "INT_TIM2MISS.INT_TIMMISSRSVD",                   "Memory",  0x4000A81C,  4,        base=16,     bitMask=0x0000007F

sfr = "INT_MISS",                                       "Memory",  0x4000A820,  4,        base=16
sfr = "INT_MISS.INT_MISSIRQD",                          "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00008000
sfr = "INT_MISS.INT_MISSIRQC",                          "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00004000
sfr = "INT_MISS.INT_MISSIRQB",                          "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00002000
sfr = "INT_MISS.INT_MISSIRQA",                          "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00001000
sfr = "INT_MISS.INT_MISSADC",                           "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000800
sfr = "INT_MISS.INT_MISSMACRX",                         "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000400
sfr = "INT_MISS.INT_MISSMACTX",                         "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000200
sfr = "INT_MISS.INT_MISSMACTMR",                        "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000100
sfr = "INT_MISS.INT_MISSSEC",                           "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000080
sfr = "INT_MISS.INT_MISSSC2",                           "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000040
sfr = "INT_MISS.INT_MISSSC1",                           "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000020
sfr = "INT_MISS.INT_MISSSLEEP",                         "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000010
sfr = "INT_MISS.INT_MISSBB",                            "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000008
sfr = "INT_MISS.INT_MISSMGMT",                          "Memory",  0x4000A820,  4,        base=16,     bitMask=0x00000004

sfr = "INT_TIM1CFG",                                    "Memory",  0x4000A840,  4,        base=16
sfr = "INT_TIM1CFG.INT_TIMTIF",                         "Memory",  0x4000A840,  4,        base=16,     bitMask=0x00000040
sfr = "INT_TIM1CFG.INT_TIMCC4IF",                       "Memory",  0x4000A840,  4,        base=16,     bitMask=0x00000010
sfr = "INT_TIM1CFG.INT_TIMCC3IF",                       "Memory",  0x4000A840,  4,        base=16,     bitMask=0x00000008
sfr = "INT_TIM1CFG.INT_TIMCC2IF",                       "Memory",  0x4000A840,  4,        base=16,     bitMask=0x00000004
sfr = "INT_TIM1CFG.INT_TIMCC1IF",                       "Memory",  0x4000A840,  4,        base=16,     bitMask=0x00000002
sfr = "INT_TIM1CFG.INT_TIMUIF",                         "Memory",  0x4000A840,  4,        base=16,     bitMask=0x00000001

sfr = "INT_TIM2CFG",                                    "Memory",  0x4000A844,  4,        base=16
sfr = "INT_TIM2CFG.INT_TIMTIF",                         "Memory",  0x4000A844,  4,        base=16,     bitMask=0x00000040
sfr = "INT_TIM2CFG.INT_TIMCC4IF",                       "Memory",  0x4000A844,  4,        base=16,     bitMask=0x00000010
sfr = "INT_TIM2CFG.INT_TIMCC3IF",                       "Memory",  0x4000A844,  4,        base=16,     bitMask=0x00000008
sfr = "INT_TIM2CFG.INT_TIMCC2IF",                       "Memory",  0x4000A844,  4,        base=16,     bitMask=0x00000004
sfr = "INT_TIM2CFG.INT_TIMCC1IF",                       "Memory",  0x4000A844,  4,        base=16,     bitMask=0x00000002
sfr = "INT_TIM2CFG.INT_TIMUIF",                         "Memory",  0x4000A844,  4,        base=16,     bitMask=0x00000001

sfr = "INT_SC1CFG",                                     "Memory",  0x4000A848,  4,        base=16
sfr = "INT_SC1CFG.INT_SC1PARERR",                       "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00004000
sfr = "INT_SC1CFG.INT_SC1FRMERR",                       "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00002000
sfr = "INT_SC1CFG.INT_SCTXULDB",                        "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00001000
sfr = "INT_SC1CFG.INT_SCTXULDA",                        "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000800
sfr = "INT_SC1CFG.INT_SCRXULDB",                        "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000400
sfr = "INT_SC1CFG.INT_SCRXULDA",                        "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000200
sfr = "INT_SC1CFG.INT_SCNAK",                           "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000100
sfr = "INT_SC1CFG.INT_SCCMDFIN",                        "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000080
sfr = "INT_SC1CFG.INT_SCTXFIN",                         "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000040
sfr = "INT_SC1CFG.INT_SCRXFIN",                         "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000020
sfr = "INT_SC1CFG.INT_SCTXUND",                         "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000010
sfr = "INT_SC1CFG.INT_SCRXOVF",                         "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000008
sfr = "INT_SC1CFG.INT_SCTXIDLE",                        "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000004
sfr = "INT_SC1CFG.INT_SCTXFREE",                        "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000002
sfr = "INT_SC1CFG.INT_SCRXVAL",                         "Memory",  0x4000A848,  4,        base=16,     bitMask=0x00000001

sfr = "INT_SC2CFG",                                     "Memory",  0x4000A84C,  4,        base=16
sfr = "INT_SC2CFG.INT_SCTXULDB",                        "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00001000
sfr = "INT_SC2CFG.INT_SCTXULDA",                        "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000800
sfr = "INT_SC2CFG.INT_SCRXULDB",                        "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000400
sfr = "INT_SC2CFG.INT_SCRXULDA",                        "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000200
sfr = "INT_SC2CFG.INT_SCNAK",                           "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000100
sfr = "INT_SC2CFG.INT_SCCMDFIN",                        "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000080
sfr = "INT_SC2CFG.INT_SCTXFIN",                         "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000040
sfr = "INT_SC2CFG.INT_SCRXFIN",                         "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000020
sfr = "INT_SC2CFG.INT_SCTXUND",                         "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000010
sfr = "INT_SC2CFG.INT_SCRXOVF",                         "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000008
sfr = "INT_SC2CFG.INT_SCTXIDLE",                        "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000004
sfr = "INT_SC2CFG.INT_SCTXFREE",                        "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000002
sfr = "INT_SC2CFG.INT_SCRXVAL",                         "Memory",  0x4000A84C,  4,        base=16,     bitMask=0x00000001

sfr = "INT_ADCCFG",                                     "Memory",  0x4000A850,  4,        base=16
sfr = "INT_ADCCFG.INT_ADCOVF",                          "Memory",  0x4000A850,  4,        base=16,     bitMask=0x00000010
sfr = "INT_ADCCFG.INT_ADCSAT",                          "Memory",  0x4000A850,  4,        base=16,     bitMask=0x00000008
sfr = "INT_ADCCFG.INT_ADCULDFULL",                      "Memory",  0x4000A850,  4,        base=16,     bitMask=0x00000004
sfr = "INT_ADCCFG.INT_ADCULDHALF",                      "Memory",  0x4000A850,  4,        base=16,     bitMask=0x00000002
sfr = "INT_ADCCFG.INT_ADCCFGRSVD",                      "Memory",  0x4000A850,  4,        base=16,     bitMask=0x00000001

sfr = "SC1_INTMODE",                                    "Memory",  0x4000A854,  4,        base=16
sfr = "SC1_INTMODE.SC_TXIDLELEVEL",                     "Memory",  0x4000A854,  4,        base=16,     bitMask=0x00000004
sfr = "SC1_INTMODE.SC_TXFREELEVEL",                     "Memory",  0x4000A854,  4,        base=16,     bitMask=0x00000002
sfr = "SC1_INTMODE.SC_RXVALLEVEL",                      "Memory",  0x4000A854,  4,        base=16,     bitMask=0x00000001

sfr = "SC2_INTMODE",                                    "Memory",  0x4000A858,  4,        base=16
sfr = "SC2_INTMODE.SC_TXIDLELEVEL",                     "Memory",  0x4000A858,  4,        base=16,     bitMask=0x00000004
sfr = "SC2_INTMODE.SC_TXFREELEVEL",                     "Memory",  0x4000A858,  4,        base=16,     bitMask=0x00000002
sfr = "SC2_INTMODE.SC_RXVALLEVEL",                      "Memory",  0x4000A858,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_INTCFGA",                                   "Memory",  0x4000A860,  4,        base=16
sfr = "GPIO_INTCFGA.GPIO_INTFILT",                      "Memory",  0x4000A860,  4,        base=16,     bitMask=0x00000100
sfr = "GPIO_INTCFGA.GPIO_INTMOD",                       "Memory",  0x4000A860,  4,        base=16,     bitMask=0x000000E0

sfr = "GPIO_INTCFGB",                                   "Memory",  0x4000A864,  4,        base=16
sfr = "GPIO_INTCFGB.GPIO_INTFILT",                      "Memory",  0x4000A864,  4,        base=16,     bitMask=0x00000100
sfr = "GPIO_INTCFGB.GPIO_INTMOD",                       "Memory",  0x4000A864,  4,        base=16,     bitMask=0x000000E0

sfr = "GPIO_INTCFGC",                                   "Memory",  0x4000A868,  4,        base=16
sfr = "GPIO_INTCFGC.GPIO_INTFILT",                      "Memory",  0x4000A868,  4,        base=16,     bitMask=0x00000100
sfr = "GPIO_INTCFGC.GPIO_INTMOD",                       "Memory",  0x4000A868,  4,        base=16,     bitMask=0x000000E0

sfr = "GPIO_INTCFGD",                                   "Memory",  0x4000A86C,  4,        base=16
sfr = "GPIO_INTCFGD.GPIO_INTFILT",                      "Memory",  0x4000A86C,  4,        base=16,     bitMask=0x00000100
sfr = "GPIO_INTCFGD.GPIO_INTMOD",                       "Memory",  0x4000A86C,  4,        base=16,     bitMask=0x000000E0

sfr = "GPIO_PACFGL",                                    "Memory",  0x4000B000,  4,        base=16
sfr = "GPIO_PACFGL.PA3_CFG",                            "Memory",  0x4000B000,  4,        base=16,     bitMask=0x0000F000
sfr = "GPIO_PACFGL.PA2_CFG",                            "Memory",  0x4000B000,  4,        base=16,     bitMask=0x00000F00
sfr = "GPIO_PACFGL.PA1_CFG",                            "Memory",  0x4000B000,  4,        base=16,     bitMask=0x000000F0
sfr = "GPIO_PACFGL.PA0_CFG",                            "Memory",  0x4000B000,  4,        base=16,     bitMask=0x0000000F

sfr = "GPIO_PACFGH",                                    "Memory",  0x4000B004,  4,        base=16
sfr = "GPIO_PACFGH.PA7_CFG",                            "Memory",  0x4000B004,  4,        base=16,     bitMask=0x0000F000
sfr = "GPIO_PACFGH.PA6_CFG",                            "Memory",  0x4000B004,  4,        base=16,     bitMask=0x00000F00
sfr = "GPIO_PACFGH.PA5_CFG",                            "Memory",  0x4000B004,  4,        base=16,     bitMask=0x000000F0
sfr = "GPIO_PACFGH.PA4_CFG",                            "Memory",  0x4000B004,  4,        base=16,     bitMask=0x0000000F

sfr = "GPIO_PAIN",                                      "Memory",  0x4000B008,  4,        base=16
sfr = "GPIO_PAIN.PA7",                                  "Memory",  0x4000B008,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PAIN.PA6",                                  "Memory",  0x4000B008,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PAIN.PA5",                                  "Memory",  0x4000B008,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PAIN.PA4",                                  "Memory",  0x4000B008,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PAIN.PA3",                                  "Memory",  0x4000B008,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PAIN.PA2",                                  "Memory",  0x4000B008,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PAIN.PA1",                                  "Memory",  0x4000B008,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PAIN.PA0",                                  "Memory",  0x4000B008,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PAOUT",                                     "Memory",  0x4000B00C,  4,        base=16
sfr = "GPIO_PAOUT.PA7",                                 "Memory",  0x4000B00C,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PAOUT.PA6",                                 "Memory",  0x4000B00C,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PAOUT.PA5",                                 "Memory",  0x4000B00C,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PAOUT.PA4",                                 "Memory",  0x4000B00C,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PAOUT.PA3",                                 "Memory",  0x4000B00C,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PAOUT.PA2",                                 "Memory",  0x4000B00C,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PAOUT.PA1",                                 "Memory",  0x4000B00C,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PAOUT.PA0",                                 "Memory",  0x4000B00C,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PASET",                                     "Memory",  0x4000B010,  4,        base=16
sfr = "GPIO_PASET.GPIO_PXSETRSVD",                      "Memory",  0x4000B010,  4,        base=16,     bitMask=0x0000FF00
sfr = "GPIO_PASET.PA7",                                 "Memory",  0x4000B010,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PASET.PA6",                                 "Memory",  0x4000B010,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PASET.PA5",                                 "Memory",  0x4000B010,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PASET.PA4",                                 "Memory",  0x4000B010,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PASET.PA3",                                 "Memory",  0x4000B010,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PASET.PA2",                                 "Memory",  0x4000B010,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PASET.PA1",                                 "Memory",  0x4000B010,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PASET.PA0",                                 "Memory",  0x4000B010,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PACLR",                                     "Memory",  0x4000B014,  4,        base=16
sfr = "GPIO_PACLR.PA7",                                 "Memory",  0x4000B014,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PACLR.PA6",                                 "Memory",  0x4000B014,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PACLR.PA5",                                 "Memory",  0x4000B014,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PACLR.PA4",                                 "Memory",  0x4000B014,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PACLR.PA3",                                 "Memory",  0x4000B014,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PACLR.PA2",                                 "Memory",  0x4000B014,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PACLR.PA1",                                 "Memory",  0x4000B014,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PACLR.PA0",                                 "Memory",  0x4000B014,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PBCFGL",                                    "Memory",  0x4000B400,  4,        base=16
sfr = "GPIO_PBCFGL.PB3_CFG",                            "Memory",  0x4000B400,  4,        base=16,     bitMask=0x0000F000
sfr = "GPIO_PBCFGL.PB2_CFG",                            "Memory",  0x4000B400,  4,        base=16,     bitMask=0x00000F00
sfr = "GPIO_PBCFGL.PB1_CFG",                            "Memory",  0x4000B400,  4,        base=16,     bitMask=0x000000F0
sfr = "GPIO_PBCFGL.PB0_CFG",                            "Memory",  0x4000B400,  4,        base=16,     bitMask=0x0000000F

sfr = "GPIO_PBCFGH",                                    "Memory",  0x4000B404,  4,        base=16
sfr = "GPIO_PBCFGH.PB7_CFG",                            "Memory",  0x4000B404,  4,        base=16,     bitMask=0x0000F000
sfr = "GPIO_PBCFGH.PB6_CFG",                            "Memory",  0x4000B404,  4,        base=16,     bitMask=0x00000F00
sfr = "GPIO_PBCFGH.PB5_CFG",                            "Memory",  0x4000B404,  4,        base=16,     bitMask=0x000000F0
sfr = "GPIO_PBCFGH.PB4_CFG",                            "Memory",  0x4000B404,  4,        base=16,     bitMask=0x0000000F

sfr = "GPIO_PBIN",                                      "Memory",  0x4000B408,  4,        base=16
sfr = "GPIO_PBIN.PB7",                                  "Memory",  0x4000B408,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PBIN.PB6",                                  "Memory",  0x4000B408,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PBIN.PB5",                                  "Memory",  0x4000B408,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PBIN.PB4",                                  "Memory",  0x4000B408,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PBIN.PB3",                                  "Memory",  0x4000B408,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PBIN.PB2",                                  "Memory",  0x4000B408,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PBIN.PB1",                                  "Memory",  0x4000B408,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PBIN.PB0",                                  "Memory",  0x4000B408,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PBOUT",                                     "Memory",  0x4000B40C,  4,        base=16
sfr = "GPIO_PBOUT.PB7",                                 "Memory",  0x4000B40C,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PBOUT.PB6",                                 "Memory",  0x4000B40C,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PBOUT.PB5",                                 "Memory",  0x4000B40C,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PBOUT.PB4",                                 "Memory",  0x4000B40C,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PBOUT.PB3",                                 "Memory",  0x4000B40C,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PBOUT.PB2",                                 "Memory",  0x4000B40C,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PBOUT.PB1",                                 "Memory",  0x4000B40C,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PBOUT.PB0",                                 "Memory",  0x4000B40C,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PBSET",                                     "Memory",  0x4000B410,  4,        base=16
sfr = "GPIO_PBSET.GPIO_PXSETRSVD",                      "Memory",  0x4000B410,  4,        base=16,     bitMask=0x0000FF00
sfr = "GPIO_PBSET.PB7",                                 "Memory",  0x4000B410,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PBSET.PB6",                                 "Memory",  0x4000B410,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PBSET.PB5",                                 "Memory",  0x4000B410,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PBSET.PB4",                                 "Memory",  0x4000B410,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PBSET.PB3",                                 "Memory",  0x4000B410,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PBSET.PB2",                                 "Memory",  0x4000B410,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PBSET.PB1",                                 "Memory",  0x4000B410,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PBSET.PB0",                                 "Memory",  0x4000B410,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PBCLR",                                     "Memory",  0x4000B414,  4,        base=16
sfr = "GPIO_PBCLR.PB7",                                 "Memory",  0x4000B414,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PBCLR.PB6",                                 "Memory",  0x4000B414,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PBCLR.PB5",                                 "Memory",  0x4000B414,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PBCLR.PB4",                                 "Memory",  0x4000B414,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PBCLR.PB3",                                 "Memory",  0x4000B414,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PBCLR.PB2",                                 "Memory",  0x4000B414,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PBCLR.PB1",                                 "Memory",  0x4000B414,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PBCLR.PB0",                                 "Memory",  0x4000B414,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PCCFGL",                                    "Memory",  0x4000B800,  4,        base=16
sfr = "GPIO_PCCFGL.PC3_CFG",                            "Memory",  0x4000B800,  4,        base=16,     bitMask=0x0000F000
sfr = "GPIO_PCCFGL.PC2_CFG",                            "Memory",  0x4000B800,  4,        base=16,     bitMask=0x00000F00
sfr = "GPIO_PCCFGL.PC1_CFG",                            "Memory",  0x4000B800,  4,        base=16,     bitMask=0x000000F0
sfr = "GPIO_PCCFGL.PC0_CFG",                            "Memory",  0x4000B800,  4,        base=16,     bitMask=0x0000000F

sfr = "GPIO_PCCFGH",                                    "Memory",  0x4000B804,  4,        base=16
sfr = "GPIO_PCCFGH.PC7_CFG",                            "Memory",  0x4000B804,  4,        base=16,     bitMask=0x0000F000
sfr = "GPIO_PCCFGH.PC6_CFG",                            "Memory",  0x4000B804,  4,        base=16,     bitMask=0x00000F00
sfr = "GPIO_PCCFGH.PC5_CFG",                            "Memory",  0x4000B804,  4,        base=16,     bitMask=0x000000F0
sfr = "GPIO_PCCFGH.PC4_CFG",                            "Memory",  0x4000B804,  4,        base=16,     bitMask=0x0000000F

sfr = "GPIO_PCIN",                                      "Memory",  0x4000B808,  4,        base=16
sfr = "GPIO_PCIN.PC7",                                  "Memory",  0x4000B808,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PCIN.PC6",                                  "Memory",  0x4000B808,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PCIN.PC5",                                  "Memory",  0x4000B808,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PCIN.PC4",                                  "Memory",  0x4000B808,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PCIN.PC3",                                  "Memory",  0x4000B808,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PCIN.PC2",                                  "Memory",  0x4000B808,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PCIN.PC1",                                  "Memory",  0x4000B808,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PCIN.PC0",                                  "Memory",  0x4000B808,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PCOUT",                                     "Memory",  0x4000B80C,  4,        base=16
sfr = "GPIO_PCOUT.PC7",                                 "Memory",  0x4000B80C,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PCOUT.PC6",                                 "Memory",  0x4000B80C,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PCOUT.PC5",                                 "Memory",  0x4000B80C,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PCOUT.PC4",                                 "Memory",  0x4000B80C,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PCOUT.PC3",                                 "Memory",  0x4000B80C,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PCOUT.PC2",                                 "Memory",  0x4000B80C,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PCOUT.PC1",                                 "Memory",  0x4000B80C,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PCOUT.PC0",                                 "Memory",  0x4000B80C,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PCSET",                                     "Memory",  0x4000B810,  4,        base=16
sfr = "GPIO_PCSET.GPIO_PXSETRSVD",                      "Memory",  0x4000B810,  4,        base=16,     bitMask=0x0000FF00
sfr = "GPIO_PCSET.PC7",                                 "Memory",  0x4000B810,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PCSET.PC6",                                 "Memory",  0x4000B810,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PCSET.PC5",                                 "Memory",  0x4000B810,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PCSET.PC4",                                 "Memory",  0x4000B810,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PCSET.PC3",                                 "Memory",  0x4000B810,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PCSET.PC2",                                 "Memory",  0x4000B810,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PCSET.PC1",                                 "Memory",  0x4000B810,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PCSET.PC0",                                 "Memory",  0x4000B810,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PCCLR",                                     "Memory",  0x4000B814,  4,        base=16
sfr = "GPIO_PCCLR.PC7",                                 "Memory",  0x4000B814,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PCCLR.PC6",                                 "Memory",  0x4000B814,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PCCLR.PC5",                                 "Memory",  0x4000B814,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PCCLR.PC4",                                 "Memory",  0x4000B814,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PCCLR.PC3",                                 "Memory",  0x4000B814,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PCCLR.PC2",                                 "Memory",  0x4000B814,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PCCLR.PC1",                                 "Memory",  0x4000B814,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PCCLR.PC0",                                 "Memory",  0x4000B814,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_DBGCFG",                                    "Memory",  0x4000BC00,  4,        base=16
sfr = "GPIO_DBGCFG.GPIO_DEBUGDIS",                      "Memory",  0x4000BC00,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_DBGCFG.GPIO_EXTREGEN",                      "Memory",  0x4000BC00,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_DBGCFG.GPIO_DBGCFGRSVD",                    "Memory",  0x4000BC00,  4,        base=16,     bitMask=0x00000008

sfr = "GPIO_DBGSTAT",                                   "Memory",  0x4000BC04,  4,        base=16
sfr = "GPIO_DBGSTAT.GPIO_BOOTMODE",                     "Memory",  0x4000BC04,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_DBGSTAT.GPIO_FORCEDBG",                     "Memory",  0x4000BC04,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_DBGSTAT.GPIO_SWEN",                         "Memory",  0x4000BC04,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PAWAKE",                                    "Memory",  0x4000BC08,  4,        base=16
sfr = "GPIO_PAWAKE.PA7",                                "Memory",  0x4000BC08,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PAWAKE.PA6",                                "Memory",  0x4000BC08,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PAWAKE.PA5",                                "Memory",  0x4000BC08,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PAWAKE.PA4",                                "Memory",  0x4000BC08,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PAWAKE.PA3",                                "Memory",  0x4000BC08,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PAWAKE.PA2",                                "Memory",  0x4000BC08,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PAWAKE.PA1",                                "Memory",  0x4000BC08,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PAWAKE.PA0",                                "Memory",  0x4000BC08,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PBWAKE",                                    "Memory",  0x4000BC0C,  4,        base=16
sfr = "GPIO_PBWAKE.PB7",                                "Memory",  0x4000BC0C,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PBWAKE.PB6",                                "Memory",  0x4000BC0C,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PBWAKE.PB5",                                "Memory",  0x4000BC0C,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PBWAKE.PB4",                                "Memory",  0x4000BC0C,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PBWAKE.PB3",                                "Memory",  0x4000BC0C,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PBWAKE.PB2",                                "Memory",  0x4000BC0C,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PBWAKE.PB1",                                "Memory",  0x4000BC0C,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PBWAKE.PB0",                                "Memory",  0x4000BC0C,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_PCWAKE",                                    "Memory",  0x4000BC10,  4,        base=16
sfr = "GPIO_PCWAKE.PC7",                                "Memory",  0x4000BC10,  4,        base=16,     bitMask=0x00000080
sfr = "GPIO_PCWAKE.PC6",                                "Memory",  0x4000BC10,  4,        base=16,     bitMask=0x00000040
sfr = "GPIO_PCWAKE.PC5",                                "Memory",  0x4000BC10,  4,        base=16,     bitMask=0x00000020
sfr = "GPIO_PCWAKE.PC4",                                "Memory",  0x4000BC10,  4,        base=16,     bitMask=0x00000010
sfr = "GPIO_PCWAKE.PC3",                                "Memory",  0x4000BC10,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_PCWAKE.PC2",                                "Memory",  0x4000BC10,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_PCWAKE.PC1",                                "Memory",  0x4000BC10,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_PCWAKE.PC0",                                "Memory",  0x4000BC10,  4,        base=16,     bitMask=0x00000001

sfr = "GPIO_IRQCSEL",                                   "Memory",  0x4000BC14,  4,        base=16

sfr = "GPIO_IRQDSEL",                                   "Memory",  0x4000BC18,  4,        base=16

sfr = "GPIO_WAKEFILT",                                  "Memory",  0x4000BC1C,  4,        base=16
sfr = "GPIO_WAKEFILT.IRQD_WAKE_FILTER",                 "Memory",  0x4000BC1C,  4,        base=16,     bitMask=0x00000008
sfr = "GPIO_WAKEFILT.SC2_WAKE_FILTER",                  "Memory",  0x4000BC1C,  4,        base=16,     bitMask=0x00000004
sfr = "GPIO_WAKEFILT.SC1_WAKE_FILTER",                  "Memory",  0x4000BC1C,  4,        base=16,     bitMask=0x00000002
sfr = "GPIO_WAKEFILT.GPIO_WAKE_FILTER",                 "Memory",  0x4000BC1C,  4,        base=16,     bitMask=0x00000001

sfr = "SC2_RXBEGA",                                     "Memory",  0x4000C000,  4,        base=16

sfr = "SC2_RXENDA",                                     "Memory",  0x4000C004,  4,        base=16

sfr = "SC2_RXBEGB",                                     "Memory",  0x4000C008,  4,        base=16

sfr = "SC2_RXENDB",                                     "Memory",  0x4000C00C,  4,        base=16

sfr = "SC2_TXBEGA",                                     "Memory",  0x4000C010,  4,        base=16

sfr = "SC2_TXENDA",                                     "Memory",  0x4000C014,  4,        base=16

sfr = "SC2_TXBEGB",                                     "Memory",  0x4000C018,  4,        base=16

sfr = "SC2_TXENDB",                                     "Memory",  0x4000C01C,  4,        base=16

sfr = "SC2_RXCNTA",                                     "Memory",  0x4000C020,  4,        base=16

sfr = "SC2_RXCNTB",                                     "Memory",  0x4000C024,  4,        base=16

sfr = "SC2_TXCNT",                                      "Memory",  0x4000C028,  4,        base=16

sfr = "SC2_DMASTAT",                                    "Memory",  0x4000C02C,  4,        base=16
sfr = "SC2_DMASTAT.SC_RXSSEL",                          "Memory",  0x4000C02C,  4,        base=16,     bitMask=0x00001C00
sfr = "SC2_DMASTAT.SC_RXOVFB",                          "Memory",  0x4000C02C,  4,        base=16,     bitMask=0x00000020
sfr = "SC2_DMASTAT.SC_RXOVFA",                          "Memory",  0x4000C02C,  4,        base=16,     bitMask=0x00000010
sfr = "SC2_DMASTAT.SC_TXACTB",                          "Memory",  0x4000C02C,  4,        base=16,     bitMask=0x00000008
sfr = "SC2_DMASTAT.SC_TXACTA",                          "Memory",  0x4000C02C,  4,        base=16,     bitMask=0x00000004
sfr = "SC2_DMASTAT.SC_RXACTB",                          "Memory",  0x4000C02C,  4,        base=16,     bitMask=0x00000002
sfr = "SC2_DMASTAT.SC_RXACTA",                          "Memory",  0x4000C02C,  4,        base=16,     bitMask=0x00000001

sfr = "SC2_DMACTRL",                                    "Memory",  0x4000C030,  4,        base=16
sfr = "SC2_DMACTRL.SC_TXDMARST",                        "Memory",  0x4000C030,  4,        base=16,     bitMask=0x00000020
sfr = "SC2_DMACTRL.SC_RXDMARST",                        "Memory",  0x4000C030,  4,        base=16,     bitMask=0x00000010
sfr = "SC2_DMACTRL.SC_TXLODB",                          "Memory",  0x4000C030,  4,        base=16,     bitMask=0x00000008
sfr = "SC2_DMACTRL.SC_TXLODA",                          "Memory",  0x4000C030,  4,        base=16,     bitMask=0x00000004
sfr = "SC2_DMACTRL.SC_RXLODB",                          "Memory",  0x4000C030,  4,        base=16,     bitMask=0x00000002
sfr = "SC2_DMACTRL.SC_RXLODA",                          "Memory",  0x4000C030,  4,        base=16,     bitMask=0x00000001

sfr = "SC2_RXERRA",                                     "Memory",  0x4000C034,  4,        base=16

sfr = "SC2_RXERRB",                                     "Memory",  0x4000C038,  4,        base=16

sfr = "SC2_DATA",                                       "Memory",  0x4000C03C,  4,        base=16

sfr = "SC2_SPISTAT",                                    "Memory",  0x4000C040,  4,        base=16
sfr = "SC2_SPISTAT.SC_SPITXIDLE",                       "Memory",  0x4000C040,  4,        base=16,     bitMask=0x00000008
sfr = "SC2_SPISTAT.SC_SPITXFREE",                       "Memory",  0x4000C040,  4,        base=16,     bitMask=0x00000004
sfr = "SC2_SPISTAT.SC_SPIRXVAL",                        "Memory",  0x4000C040,  4,        base=16,     bitMask=0x00000002
sfr = "SC2_SPISTAT.SC_SPIRXOVF",                        "Memory",  0x4000C040,  4,        base=16,     bitMask=0x00000001

sfr = "SC2_TWISTAT",                                    "Memory",  0x4000C044,  4,        base=16
sfr = "SC2_TWISTAT.SC_TWICMDFIN",                       "Memory",  0x4000C044,  4,        base=16,     bitMask=0x00000008
sfr = "SC2_TWISTAT.SC_TWIRXFIN",                        "Memory",  0x4000C044,  4,        base=16,     bitMask=0x00000004
sfr = "SC2_TWISTAT.SC_TWITXFIN",                        "Memory",  0x4000C044,  4,        base=16,     bitMask=0x00000002
sfr = "SC2_TWISTAT.SC_TWIRXNAK",                        "Memory",  0x4000C044,  4,        base=16,     bitMask=0x00000001

sfr = "SC2_TWICTRL1",                                   "Memory",  0x4000C04C,  4,        base=16
sfr = "SC2_TWICTRL1.SC_TWISTOP",                        "Memory",  0x4000C04C,  4,        base=16,     bitMask=0x00000008
sfr = "SC2_TWICTRL1.SC_TWISTART",                       "Memory",  0x4000C04C,  4,        base=16,     bitMask=0x00000004
sfr = "SC2_TWICTRL1.SC_TWISEND",                        "Memory",  0x4000C04C,  4,        base=16,     bitMask=0x00000002
sfr = "SC2_TWICTRL1.SC_TWIRECV",                        "Memory",  0x4000C04C,  4,        base=16,     bitMask=0x00000001

sfr = "SC2_TWICTRL2",                                   "Memory",  0x4000C050,  4,        base=16

sfr = "SC2_MODE",                                       "Memory",  0x4000C054,  4,        base=16

sfr = "SC2_SPICFG",                                     "Memory",  0x4000C058,  4,        base=16
sfr = "SC2_SPICFG.SC_SPIRXDRV",                         "Memory",  0x4000C058,  4,        base=16,     bitMask=0x00000020
sfr = "SC2_SPICFG.SC_SPIMST",                           "Memory",  0x4000C058,  4,        base=16,     bitMask=0x00000010
sfr = "SC2_SPICFG.SC_SPIRPT",                           "Memory",  0x4000C058,  4,        base=16,     bitMask=0x00000008
sfr = "SC2_SPICFG.SC_SPIORD",                           "Memory",  0x4000C058,  4,        base=16,     bitMask=0x00000004
sfr = "SC2_SPICFG.SC_SPIPHA",                           "Memory",  0x4000C058,  4,        base=16,     bitMask=0x00000002
sfr = "SC2_SPICFG.SC_SPIPOL",                           "Memory",  0x4000C058,  4,        base=16,     bitMask=0x00000001

sfr = "SC2_RATELIN",                                    "Memory",  0x4000C060,  4,        base=16
sfr = "SC2_RATELIN.SC_RATELIN",                         "Memory",  0x4000C060,  4,        base=16,     bitMask=0x0000000F

sfr = "SC2_RATEEXP",                                    "Memory",  0x4000C064,  4,        base=16
sfr = "SC2_RATEEXP.SC_RATEEXP",                         "Memory",  0x4000C064,  4,        base=16,     bitMask=0x0000000F

sfr = "SC2_RXCNTSAVED",                                 "Memory",  0x4000C070,  4,        base=16

sfr = "SC1_RXBEGA",                                     "Memory",  0x4000C800,  4,        base=16

sfr = "SC1_RXENDA",                                     "Memory",  0x4000C804,  4,        base=16

sfr = "SC1_RXBEGB",                                     "Memory",  0x4000C808,  4,        base=16

sfr = "SC1_RXENDB",                                     "Memory",  0x4000C80C,  4,        base=16

sfr = "SC1_TXBEGA",                                     "Memory",  0x4000C810,  4,        base=16

sfr = "SC1_TXENDA",                                     "Memory",  0x4000C814,  4,        base=16

sfr = "SC1_TXBEGB",                                     "Memory",  0x4000C818,  4,        base=16

sfr = "SC1_TXENDB",                                     "Memory",  0x4000C81C,  4,        base=16

sfr = "SC1_RXCNTA",                                     "Memory",  0x4000C820,  4,        base=16

sfr = "SC1_RXCNTB",                                     "Memory",  0x4000C824,  4,        base=16

sfr = "SC1_TXCNT",                                      "Memory",  0x4000C828,  4,        base=16

sfr = "SC1_DMASTAT",                                    "Memory",  0x4000C82C,  4,        base=16
sfr = "SC1_DMASTAT.SC_RXSSEL",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00001C00
sfr = "SC1_DMASTAT.SC_RXFRMB",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000200
sfr = "SC1_DMASTAT.SC_RXFRMA",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000100
sfr = "SC1_DMASTAT.SC_RXPARB",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000080
sfr = "SC1_DMASTAT.SC_RXPARA",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000040
sfr = "SC1_DMASTAT.SC_RXOVFB",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000020
sfr = "SC1_DMASTAT.SC_RXOVFA",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000010
sfr = "SC1_DMASTAT.SC_TXACTB",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000008
sfr = "SC1_DMASTAT.SC_TXACTA",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000004
sfr = "SC1_DMASTAT.SC_RXACTB",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000002
sfr = "SC1_DMASTAT.SC_RXACTA",                          "Memory",  0x4000C82C,  4,        base=16,     bitMask=0x00000001

sfr = "SC1_DMACTRL",                                    "Memory",  0x4000C830,  4,        base=16
sfr = "SC1_DMACTRL.SC_TXDMARST",                        "Memory",  0x4000C830,  4,        base=16,     bitMask=0x00000020
sfr = "SC1_DMACTRL.SC_RXDMARST",                        "Memory",  0x4000C830,  4,        base=16,     bitMask=0x00000010
sfr = "SC1_DMACTRL.SC_TXLODB",                          "Memory",  0x4000C830,  4,        base=16,     bitMask=0x00000008
sfr = "SC1_DMACTRL.SC_TXLODA",                          "Memory",  0x4000C830,  4,        base=16,     bitMask=0x00000004
sfr = "SC1_DMACTRL.SC_RXLODB",                          "Memory",  0x4000C830,  4,        base=16,     bitMask=0x00000002
sfr = "SC1_DMACTRL.SC_RXLODA",                          "Memory",  0x4000C830,  4,        base=16,     bitMask=0x00000001

sfr = "SC1_RXERRA",                                     "Memory",  0x4000C834,  4,        base=16

sfr = "SC1_RXERRB",                                     "Memory",  0x4000C838,  4,        base=16

sfr = "SC1_DATA",                                       "Memory",  0x4000C83C,  4,        base=16

sfr = "SC1_SPISTAT",                                    "Memory",  0x4000C840,  4,        base=16
sfr = "SC1_SPISTAT.SC_SPITXIDLE",                       "Memory",  0x4000C840,  4,        base=16,     bitMask=0x00000008
sfr = "SC1_SPISTAT.SC_SPITXFREE",                       "Memory",  0x4000C840,  4,        base=16,     bitMask=0x00000004
sfr = "SC1_SPISTAT.SC_SPIRXVAL",                        "Memory",  0x4000C840,  4,        base=16,     bitMask=0x00000002
sfr = "SC1_SPISTAT.SC_SPIRXOVF",                        "Memory",  0x4000C840,  4,        base=16,     bitMask=0x00000001

sfr = "SC1_TWISTAT",                                    "Memory",  0x4000C844,  4,        base=16
sfr = "SC1_TWISTAT.SC_TWICMDFIN",                       "Memory",  0x4000C844,  4,        base=16,     bitMask=0x00000008
sfr = "SC1_TWISTAT.SC_TWIRXFIN",                        "Memory",  0x4000C844,  4,        base=16,     bitMask=0x00000004
sfr = "SC1_TWISTAT.SC_TWITXFIN",                        "Memory",  0x4000C844,  4,        base=16,     bitMask=0x00000002
sfr = "SC1_TWISTAT.SC_TWIRXNAK",                        "Memory",  0x4000C844,  4,        base=16,     bitMask=0x00000001

sfr = "SC1_UARTSTAT",                                   "Memory",  0x4000C848,  4,        base=16
sfr = "SC1_UARTSTAT.SC_UARTTXIDLE",                     "Memory",  0x4000C848,  4,        base=16,     bitMask=0x00000040
sfr = "SC1_UARTSTAT.SC_UARTPARERR",                     "Memory",  0x4000C848,  4,        base=16,     bitMask=0x00000020
sfr = "SC1_UARTSTAT.SC_UARTFRMERR",                     "Memory",  0x4000C848,  4,        base=16,     bitMask=0x00000010
sfr = "SC1_UARTSTAT.SC_UARTRXOVF",                      "Memory",  0x4000C848,  4,        base=16,     bitMask=0x00000008
sfr = "SC1_UARTSTAT.SC_UARTTXFREE",                     "Memory",  0x4000C848,  4,        base=16,     bitMask=0x00000004
sfr = "SC1_UARTSTAT.SC_UARTRXVAL",                      "Memory",  0x4000C848,  4,        base=16,     bitMask=0x00000002
sfr = "SC1_UARTSTAT.SC_UARTCTS",                        "Memory",  0x4000C848,  4,        base=16,     bitMask=0x00000001

sfr = "SC1_TWICTRL1",                                   "Memory",  0x4000C84C,  4,        base=16
sfr = "SC1_TWICTRL1.SC_TWISTOP",                        "Memory",  0x4000C84C,  4,        base=16,     bitMask=0x00000008
sfr = "SC1_TWICTRL1.SC_TWISTART",                       "Memory",  0x4000C84C,  4,        base=16,     bitMask=0x00000004
sfr = "SC1_TWICTRL1.SC_TWISEND",                        "Memory",  0x4000C84C,  4,        base=16,     bitMask=0x00000002
sfr = "SC1_TWICTRL1.SC_TWIRECV",                        "Memory",  0x4000C84C,  4,        base=16,     bitMask=0x00000001

sfr = "SC1_TWICTRL2",                                   "Memory",  0x4000C850,  4,        base=16

sfr = "SC1_MODE",                                       "Memory",  0x4000C854,  4,        base=16

sfr = "SC1_SPICFG",                                     "Memory",  0x4000C858,  4,        base=16
sfr = "SC1_SPICFG.SC_SPIRXDRV",                         "Memory",  0x4000C858,  4,        base=16,     bitMask=0x00000020
sfr = "SC1_SPICFG.SC_SPIMST",                           "Memory",  0x4000C858,  4,        base=16,     bitMask=0x00000010
sfr = "SC1_SPICFG.SC_SPIRPT",                           "Memory",  0x4000C858,  4,        base=16,     bitMask=0x00000008
sfr = "SC1_SPICFG.SC_SPIORD",                           "Memory",  0x4000C858,  4,        base=16,     bitMask=0x00000004
sfr = "SC1_SPICFG.SC_SPIPHA",                           "Memory",  0x4000C858,  4,        base=16,     bitMask=0x00000002
sfr = "SC1_SPICFG.SC_SPIPOL",                           "Memory",  0x4000C858,  4,        base=16,     bitMask=0x00000001

sfr = "SC1_UARTCFG",                                    "Memory",  0x4000C85C,  4,        base=16
sfr = "SC1_UARTCFG.SC_UARTAUTO",                        "Memory",  0x4000C85C,  4,        base=16,     bitMask=0x00000040
sfr = "SC1_UARTCFG.SC_UARTFLOW",                        "Memory",  0x4000C85C,  4,        base=16,     bitMask=0x00000020
sfr = "SC1_UARTCFG.SC_UARTODD",                         "Memory",  0x4000C85C,  4,        base=16,     bitMask=0x00000010
sfr = "SC1_UARTCFG.SC_UARTPAR",                         "Memory",  0x4000C85C,  4,        base=16,     bitMask=0x00000008
sfr = "SC1_UARTCFG.SC_UART2STP",                        "Memory",  0x4000C85C,  4,        base=16,     bitMask=0x00000004
sfr = "SC1_UARTCFG.SC_UART8BIT",                        "Memory",  0x4000C85C,  4,        base=16,     bitMask=0x00000002
sfr = "SC1_UARTCFG.SC_UARTRTS",                         "Memory",  0x4000C85C,  4,        base=16,     bitMask=0x00000001

sfr = "SC1_RATELIN",                                    "Memory",  0x4000C860,  4,        base=16

sfr = "SC1_RATEEXP",                                    "Memory",  0x4000C864,  4,        base=16

sfr = "SC1_UARTPER",                                    "Memory",  0x4000C868,  4,        base=16

sfr = "SC1_UARTFRAC",                                   "Memory",  0x4000C86C,  4,        base=16

sfr = "SC1_RXCNTSAVED",                                 "Memory",  0x4000C870,  4,        base=16

sfr = "ADC_CFG",                                        "Memory",  0x4000D004,  4,        base=16
sfr = "ADC_CFG.ADC_PERIOD",                             "Memory",  0x4000D004,  4,        base=16,     bitMask=0x0000E000
sfr = "ADC_CFG.ADC_HVSELP",                             "Memory",  0x4000D004,  4,        base=16,     bitMask=0x00001000
sfr = "ADC_CFG.ADC_HVSELN",                             "Memory",  0x4000D004,  4,        base=16,     bitMask=0x00000800
sfr = "ADC_CFG.ADC_MUXP",                               "Memory",  0x4000D004,  4,        base=16,     bitMask=0x00000780
sfr = "ADC_CFG.ADC_MUXN",                               "Memory",  0x4000D004,  4,        base=16,     bitMask=0x00000078
sfr = "ADC_CFG.ADC_1MHZCLK",                            "Memory",  0x4000D004,  4,        base=16,     bitMask=0x00000004
sfr = "ADC_CFG.ADC_CFGRSVD",                            "Memory",  0x4000D004,  4,        base=16,     bitMask=0x00000002
sfr = "ADC_CFG.ADC_ENABLE",                             "Memory",  0x4000D004,  4,        base=16,     bitMask=0x00000001

sfr = "ADC_OFFSET",                                     "Memory",  0x4000D008,  4,        base=16

sfr = "ADC_GAIN",                                       "Memory",  0x4000D00C,  4,        base=16

sfr = "ADC_DMACFG",                                     "Memory",  0x4000D010,  4,        base=16
sfr = "ADC_DMACFG.ADC_DMARST",                          "Memory",  0x4000D010,  4,        base=16,     bitMask=0x00000010
sfr = "ADC_DMACFG.ADC_DMAAUTOWRAP",                     "Memory",  0x4000D010,  4,        base=16,     bitMask=0x00000002
sfr = "ADC_DMACFG.ADC_DMALOAD",                         "Memory",  0x4000D010,  4,        base=16,     bitMask=0x00000001

sfr = "ADC_DMASTAT",                                    "Memory",  0x4000D014,  4,        base=16
sfr = "ADC_DMASTAT.ADC_DMAOVF",                         "Memory",  0x4000D014,  4,        base=16,     bitMask=0x00000002
sfr = "ADC_DMASTAT.ADC_DMAACT",                         "Memory",  0x4000D014,  4,        base=16,     bitMask=0x00000001

sfr = "ADC_DMABEG",                                     "Memory",  0x4000D018,  4,        base=16

sfr = "ADC_DMASIZE",                                    "Memory",  0x4000D01C,  4,        base=16

sfr = "ADC_DMACUR",                                     "Memory",  0x4000D020,  4,        base=16

sfr = "ADC_DMACNT",                                     "Memory",  0x4000D024,  4,        base=16

sfr = "TIM1_CR1",                                       "Memory",  0x4000E000,  4,        base=16
sfr = "TIM1_CR1.TIM_ARBE",                              "Memory",  0x4000E000,  4,        base=16,     bitMask=0x00000080
sfr = "TIM1_CR1.TIM_CMS",                               "Memory",  0x4000E000,  4,        base=16,     bitMask=0x00000060
sfr = "TIM1_CR1.TIM_DIR",                               "Memory",  0x4000E000,  4,        base=16,     bitMask=0x00000010
sfr = "TIM1_CR1.TIM_OPM",                               "Memory",  0x4000E000,  4,        base=16,     bitMask=0x00000008
sfr = "TIM1_CR1.TIM_URS",                               "Memory",  0x4000E000,  4,        base=16,     bitMask=0x00000004
sfr = "TIM1_CR1.TIM_UDIS",                              "Memory",  0x4000E000,  4,        base=16,     bitMask=0x00000002
sfr = "TIM1_CR1.TIM_CEN",                               "Memory",  0x4000E000,  4,        base=16,     bitMask=0x00000001

sfr = "TIM1_CR2",                                       "Memory",  0x4000E004,  4,        base=16
sfr = "TIM1_CR2.TIM_TI1S",                              "Memory",  0x4000E004,  4,        base=16,     bitMask=0x00000080
sfr = "TIM1_CR2.TIM_MMS",                               "Memory",  0x4000E004,  4,        base=16,     bitMask=0x00000070

sfr = "TIM1_SMCR",                                      "Memory",  0x4000E008,  4,        base=16
sfr = "TIM1_SMCR.TIM_ETP",                              "Memory",  0x4000E008,  4,        base=16,     bitMask=0x00008000
sfr = "TIM1_SMCR.TIM_ECE",                              "Memory",  0x4000E008,  4,        base=16,     bitMask=0x00004000
sfr = "TIM1_SMCR.TIM_ETPS",                             "Memory",  0x4000E008,  4,        base=16,     bitMask=0x00003000
sfr = "TIM1_SMCR.TIM_ETF",                              "Memory",  0x4000E008,  4,        base=16,     bitMask=0x00000F00
sfr = "TIM1_SMCR.TIM_MSM",                              "Memory",  0x4000E008,  4,        base=16,     bitMask=0x00000080
sfr = "TIM1_SMCR.TIM_TS",                               "Memory",  0x4000E008,  4,        base=16,     bitMask=0x00000070
sfr = "TIM1_SMCR.TIM_SMS",                              "Memory",  0x4000E008,  4,        base=16,     bitMask=0x00000007

sfr = "TIM1_EGR",                                       "Memory",  0x4000E014,  4,        base=16
sfr = "TIM1_EGR.TIM_TG",                                "Memory",  0x4000E014,  4,        base=16,     bitMask=0x00000040
sfr = "TIM1_EGR.TIM_CC4G",                              "Memory",  0x4000E014,  4,        base=16,     bitMask=0x00000010
sfr = "TIM1_EGR.TIM_CC3G",                              "Memory",  0x4000E014,  4,        base=16,     bitMask=0x00000008
sfr = "TIM1_EGR.TIM_CC2G",                              "Memory",  0x4000E014,  4,        base=16,     bitMask=0x00000004
sfr = "TIM1_EGR.TIM_CC1G",                              "Memory",  0x4000E014,  4,        base=16,     bitMask=0x00000002
sfr = "TIM1_EGR.TIM_UG",                                "Memory",  0x4000E014,  4,        base=16,     bitMask=0x00000001

sfr = "TIM1_CCMR1",                                     "Memory",  0x4000E018,  4,        base=16
sfr = "TIM1_CCMR1.TIM_IC2F",                            "Memory",  0x4000E018,  4,        base=16,     bitMask=0x0000F000
sfr = "TIM1_CCMR1.TIM_IC2PSC",                          "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00000C00
sfr = "TIM1_CCMR1.TIM_IC1F",                            "Memory",  0x4000E018,  4,        base=16,     bitMask=0x000000F0
sfr = "TIM1_CCMR1.TIM_IC1PSC",                          "Memory",  0x4000E018,  4,        base=16,     bitMask=0x0000000C
sfr = "TIM1_CCMR1.TIM_OC2CE",                           "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00008000
sfr = "TIM1_CCMR1.TIM_OC2M",                            "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00007000
sfr = "TIM1_CCMR1.TIM_OC2BE",                           "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00000800
sfr = "TIM1_CCMR1.TIM_OC2FE",                           "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00000400
sfr = "TIM1_CCMR1.TIM_CC2S",                            "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00000300
sfr = "TIM1_CCMR1.TIM_OC1CE",                           "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00000080
sfr = "TIM1_CCMR1.TIM_OC1M",                            "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00000070
sfr = "TIM1_CCMR1.TIM_OC1PE",                           "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00000008
sfr = "TIM1_CCMR1.TIM_OC1FE",                           "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00000004
sfr = "TIM1_CCMR1.TIM_CC1S",                            "Memory",  0x4000E018,  4,        base=16,     bitMask=0x00000003

sfr = "TIM1_CCMR2",                                     "Memory",  0x4000E01C,  4,        base=16
sfr = "TIM1_CCMR2.TIM_IC4F",                            "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x0000F000
sfr = "TIM1_CCMR2.TIM_IC4PSC",                          "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00000C00
sfr = "TIM1_CCMR2.TIM_IC3F",                            "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x000000F0
sfr = "TIM1_CCMR2.TIM_IC3PSC",                          "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x0000000C
sfr = "TIM1_CCMR2.TIM_OC4CE",                           "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00008000
sfr = "TIM1_CCMR2.TIM_OC4M",                            "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00007000
sfr = "TIM1_CCMR2.TIM_OC4BE",                           "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00000800
sfr = "TIM1_CCMR2.TIM_OC4FE",                           "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00000400
sfr = "TIM1_CCMR2.TIM_CC4S",                            "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00000300
sfr = "TIM1_CCMR2.TIM_OC3CE",                           "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00000080
sfr = "TIM1_CCMR2.TIM_OC3M",                            "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00000070
sfr = "TIM1_CCMR2.TIM_OC3BE",                           "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00000008
sfr = "TIM1_CCMR2.TIM_OC3FE",                           "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00000004
sfr = "TIM1_CCMR2.TIM_CC3S",                            "Memory",  0x4000E01C,  4,        base=16,     bitMask=0x00000003

sfr = "TIM1_CCER",                                      "Memory",  0x4000E020,  4,        base=16
sfr = "TIM1_CCER.TIM_CC4P",                             "Memory",  0x4000E020,  4,        base=16,     bitMask=0x00002000
sfr = "TIM1_CCER.TIM_CC4E",                             "Memory",  0x4000E020,  4,        base=16,     bitMask=0x00001000
sfr = "TIM1_CCER.TIM_CC3P",                             "Memory",  0x4000E020,  4,        base=16,     bitMask=0x00000200
sfr = "TIM1_CCER.TIM_CC3E",                             "Memory",  0x4000E020,  4,        base=16,     bitMask=0x00000100
sfr = "TIM1_CCER.TIM_CC2P",                             "Memory",  0x4000E020,  4,        base=16,     bitMask=0x00000020
sfr = "TIM1_CCER.TIM_CC2E",                             "Memory",  0x4000E020,  4,        base=16,     bitMask=0x00000010
sfr = "TIM1_CCER.TIM_CC1P",                             "Memory",  0x4000E020,  4,        base=16,     bitMask=0x00000002
sfr = "TIM1_CCER.TIM_CC1E",                             "Memory",  0x4000E020,  4,        base=16,     bitMask=0x00000001

sfr = "TIM1_CNT",                                       "Memory",  0x4000E024,  4,        base=16

sfr = "TIM1_PSC",                                       "Memory",  0x4000E028,  4,        base=16

sfr = "TIM1_ARR",                                       "Memory",  0x4000E02C,  4,        base=16

sfr = "TIM1_CCR1",                                      "Memory",  0x4000E034,  4,        base=16

sfr = "TIM1_CCR2",                                      "Memory",  0x4000E038,  4,        base=16

sfr = "TIM1_CCR3",                                      "Memory",  0x4000E03C,  4,        base=16

sfr = "TIM1_CCR4",                                      "Memory",  0x4000E040,  4,        base=16

sfr = "TIM1_OR",                                        "Memory",  0x4000E050,  4,        base=16
sfr = "TIM1_OR.TIM_ORRSVD",                             "Memory",  0x4000E050,  4,        base=16,     bitMask=0x00000008
sfr = "TIM1_OR.TIM_CLKMSKEN",                           "Memory",  0x4000E050,  4,        base=16,     bitMask=0x00000004
sfr = "TIM1_OR.TIM1_EXTRIGSEL",                         "Memory",  0x4000E050,  4,        base=16,     bitMask=0x00000003

sfr = "TIM2_CR1",                                       "Memory",  0x4000F000,  4,        base=16
sfr = "TIM2_CR1.TIM_ARBE",                              "Memory",  0x4000F000,  4,        base=16,     bitMask=0x00000080
sfr = "TIM2_CR1.TIM_CMS",                               "Memory",  0x4000F000,  4,        base=16,     bitMask=0x00000060
sfr = "TIM2_CR1.TIM_DIR",                               "Memory",  0x4000F000,  4,        base=16,     bitMask=0x00000010
sfr = "TIM2_CR1.TIM_OPM",                               "Memory",  0x4000F000,  4,        base=16,     bitMask=0x00000008
sfr = "TIM2_CR1.TIM_URS",                               "Memory",  0x4000F000,  4,        base=16,     bitMask=0x00000004
sfr = "TIM2_CR1.TIM_UDIS",                              "Memory",  0x4000F000,  4,        base=16,     bitMask=0x00000002
sfr = "TIM2_CR1.TIM_CEN",                               "Memory",  0x4000F000,  4,        base=16,     bitMask=0x00000001

sfr = "TIM2_CR2",                                       "Memory",  0x4000F004,  4,        base=16
sfr = "TIM2_CR2.TIM_TI1S",                              "Memory",  0x4000F004,  4,        base=16,     bitMask=0x00000080
sfr = "TIM2_CR2.TIM_MMS",                               "Memory",  0x4000F004,  4,        base=16,     bitMask=0x00000070

sfr = "TIM2_SMCR",                                      "Memory",  0x4000F008,  4,        base=16
sfr = "TIM2_SMCR.TIM_ETP",                              "Memory",  0x4000F008,  4,        base=16,     bitMask=0x00008000
sfr = "TIM2_SMCR.TIM_ECE",                              "Memory",  0x4000F008,  4,        base=16,     bitMask=0x00004000
sfr = "TIM2_SMCR.TIM_ETPS",                             "Memory",  0x4000F008,  4,        base=16,     bitMask=0x00003000
sfr = "TIM2_SMCR.TIM_ETF",                              "Memory",  0x4000F008,  4,        base=16,     bitMask=0x00000F00
sfr = "TIM2_SMCR.TIM_MSM",                              "Memory",  0x4000F008,  4,        base=16,     bitMask=0x00000080
sfr = "TIM2_SMCR.TIM_TS",                               "Memory",  0x4000F008,  4,        base=16,     bitMask=0x00000070
sfr = "TIM2_SMCR.TIM_SMS",                              "Memory",  0x4000F008,  4,        base=16,     bitMask=0x00000007

sfr = "TIM2_EGR",                                       "Memory",  0x4000F014,  4,        base=16
sfr = "TIM2_EGR.TIM_TG",                                "Memory",  0x4000F014,  4,        base=16,     bitMask=0x00000040
sfr = "TIM2_EGR.TIM_CC4G",                              "Memory",  0x4000F014,  4,        base=16,     bitMask=0x00000010
sfr = "TIM2_EGR.TIM_CC3G",                              "Memory",  0x4000F014,  4,        base=16,     bitMask=0x00000008
sfr = "TIM2_EGR.TIM_CC2G",                              "Memory",  0x4000F014,  4,        base=16,     bitMask=0x00000004
sfr = "TIM2_EGR.TIM_CC1G",                              "Memory",  0x4000F014,  4,        base=16,     bitMask=0x00000002
sfr = "TIM2_EGR.TIM_UG",                                "Memory",  0x4000F014,  4,        base=16,     bitMask=0x00000001

sfr = "TIM2_CCMR1",                                     "Memory",  0x4000F018,  4,        base=16
sfr = "TIM2_CCMR1.TIM_IC2F",                            "Memory",  0x4000F018,  4,        base=16,     bitMask=0x0000F000
sfr = "TIM2_CCMR1.TIM_IC2PSC",                          "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00000C00
sfr = "TIM2_CCMR1.TIM_IC1F",                            "Memory",  0x4000F018,  4,        base=16,     bitMask=0x000000F0
sfr = "TIM2_CCMR1.TIM_IC1PSC",                          "Memory",  0x4000F018,  4,        base=16,     bitMask=0x0000000C
sfr = "TIM2_CCMR1.TIM_OC2CE",                           "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00008000
sfr = "TIM2_CCMR1.TIM_OC2M",                            "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00007000
sfr = "TIM2_CCMR1.TIM_OC2BE",                           "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00000800
sfr = "TIM2_CCMR1.TIM_OC2FE",                           "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00000400
sfr = "TIM2_CCMR1.TIM_CC2S",                            "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00000300
sfr = "TIM2_CCMR1.TIM_OC1CE",                           "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00000080
sfr = "TIM2_CCMR1.TIM_OC1M",                            "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00000070
sfr = "TIM2_CCMR1.TIM_OC1PE",                           "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00000008
sfr = "TIM2_CCMR1.TIM_OC1FE",                           "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00000004
sfr = "TIM2_CCMR1.TIM_CC1S",                            "Memory",  0x4000F018,  4,        base=16,     bitMask=0x00000003

sfr = "TIM2_CCMR2",                                     "Memory",  0x4000F01C,  4,        base=16
sfr = "TIM2_CCMR2.TIM_IC4F",                            "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x0000F000
sfr = "TIM2_CCMR2.TIM_IC4PSC",                          "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00000C00
sfr = "TIM2_CCMR2.TIM_IC3F",                            "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x000000F0
sfr = "TIM2_CCMR2.TIM_IC3PSC",                          "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x0000000C
sfr = "TIM2_CCMR2.TIM_OC4CE",                           "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00008000
sfr = "TIM2_CCMR2.TIM_OC4M",                            "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00007000
sfr = "TIM2_CCMR2.TIM_OC4BE",                           "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00000800
sfr = "TIM2_CCMR2.TIM_OC4FE",                           "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00000400
sfr = "TIM2_CCMR2.TIM_CC4S",                            "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00000300
sfr = "TIM2_CCMR2.TIM_OC3CE",                           "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00000080
sfr = "TIM2_CCMR2.TIM_OC3M",                            "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00000070
sfr = "TIM2_CCMR2.TIM_OC3BE",                           "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00000008
sfr = "TIM2_CCMR2.TIM_OC3FE",                           "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00000004
sfr = "TIM2_CCMR2.TIM_CC3S",                            "Memory",  0x4000F01C,  4,        base=16,     bitMask=0x00000003

sfr = "TIM2_CCER",                                      "Memory",  0x4000F020,  4,        base=16
sfr = "TIM2_CCER.TIM_CC4P",                             "Memory",  0x4000F020,  4,        base=16,     bitMask=0x00002000
sfr = "TIM2_CCER.TIM_CC4E",                             "Memory",  0x4000F020,  4,        base=16,     bitMask=0x00001000
sfr = "TIM2_CCER.TIM_CC3P",                             "Memory",  0x4000F020,  4,        base=16,     bitMask=0x00000200
sfr = "TIM2_CCER.TIM_CC3E",                             "Memory",  0x4000F020,  4,        base=16,     bitMask=0x00000100
sfr = "TIM2_CCER.TIM_CC2P",                             "Memory",  0x4000F020,  4,        base=16,     bitMask=0x00000020
sfr = "TIM2_CCER.TIM_CC2E",                             "Memory",  0x4000F020,  4,        base=16,     bitMask=0x00000010
sfr = "TIM2_CCER.TIM_CC1P",                             "Memory",  0x4000F020,  4,        base=16,     bitMask=0x00000002
sfr = "TIM2_CCER.TIM_CC1E",                             "Memory",  0x4000F020,  4,        base=16,     bitMask=0x00000001

sfr = "TIM2_CNT",                                       "Memory",  0x4000F024,  4,        base=16

sfr = "TIM2_PSC",                                       "Memory",  0x4000F028,  4,        base=16

sfr = "TIM2_ARR",                                       "Memory",  0x4000F02C,  4,        base=16

sfr = "TIM2_CCR1",                                      "Memory",  0x4000F034,  4,        base=16

sfr = "TIM2_CCR2",                                      "Memory",  0x4000F038,  4,        base=16

sfr = "TIM2_CCR3",                                      "Memory",  0x4000F03C,  4,        base=16

sfr = "TIM2_CCR4",                                      "Memory",  0x4000F040,  4,        base=16

sfr = "TIM2_OR",                                        "Memory",  0x4000F050,  4,        base=16
sfr = "TIM2_OR.TIM_REMAPC4",                            "Memory",  0x4000F050,  4,        base=16,     bitMask=0x00000080
sfr = "TIM2_OR.TIM_REMAPC3",                            "Memory",  0x4000F050,  4,        base=16,     bitMask=0x00000040
sfr = "TIM2_OR.TIM_REMAPC2",                            "Memory",  0x4000F050,  4,        base=16,     bitMask=0x00000020
sfr = "TIM2_OR.TIM_REMAPC1",                            "Memory",  0x4000F050,  4,        base=16,     bitMask=0x00000010
sfr = "TIM2_OR.TIM_ORRSVD",                             "Memory",  0x4000F050,  4,        base=16,     bitMask=0x00000008
sfr = "TIM2_OR.TIM_CLKMSKEN",                           "Memory",  0x4000F050,  4,        base=16,     bitMask=0x00000004
sfr = "TIM2_OR.TIM1_EXTRIGSEL",                         "Memory",  0x4000F050,  4,        base=16,     bitMask=0x00000003

sfr = "INT_CFGSET",                                     "Memory",  0xE000E100,  4,        base=16
sfr = "INT_CFGSET.INT_DEBUG",                           "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00010000
sfr = "INT_CFGSET.INT_IRQD",                            "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00008000
sfr = "INT_CFGSET.INT_IRQC",                            "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00004000
sfr = "INT_CFGSET.INT_IRQB",                            "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00002000
sfr = "INT_CFGSET.INT_IRQA",                            "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00001000
sfr = "INT_CFGSET.INT_ADC",                             "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000800
sfr = "INT_CFGSET.INT_MACRX",                           "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000400
sfr = "INT_CFGSET.INT_MACTX",                           "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000200
sfr = "INT_CFGSET.INT_MACTMR",                          "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000100
sfr = "INT_CFGSET.INT_SEC",                             "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000080
sfr = "INT_CFGSET.INT_SC2",                             "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000040
sfr = "INT_CFGSET.INT_SC1",                             "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000020
sfr = "INT_CFGSET.INT_SLEEPTMR",                        "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000010
sfr = "INT_CFGSET.INT_BB",                              "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000008
sfr = "INT_CFGSET.INT_MGMT",                            "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000004
sfr = "INT_CFGSET.INT_TIM2",                            "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000002
sfr = "INT_CFGSET.INT_TIM1",                            "Memory",  0xE000E100,  4,        base=16,     bitMask=0x00000001

sfr = "INT_CFGCLR",                                     "Memory",  0xE000E180,  4,        base=16
sfr = "INT_CFGCLR.INT_DEBUG",                           "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00010000
sfr = "INT_CFGCLR.INT_IRQD",                            "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00008000
sfr = "INT_CFGCLR.INT_IRQC",                            "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00004000
sfr = "INT_CFGCLR.INT_IRQB",                            "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00002000
sfr = "INT_CFGCLR.INT_IRQA",                            "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00001000
sfr = "INT_CFGCLR.INT_ADC",                             "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000800
sfr = "INT_CFGCLR.INT_MACRX",                           "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000400
sfr = "INT_CFGCLR.INT_MACTX",                           "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000200
sfr = "INT_CFGCLR.INT_MACTMR",                          "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000100
sfr = "INT_CFGCLR.INT_SEC",                             "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000080
sfr = "INT_CFGCLR.INT_SC2",                             "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000040
sfr = "INT_CFGCLR.INT_SC1",                             "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000020
sfr = "INT_CFGCLR.INT_SLEEPTMR",                        "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000010
sfr = "INT_CFGCLR.INT_BB",                              "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000008
sfr = "INT_CFGCLR.INT_MGMT",                            "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000004
sfr = "INT_CFGCLR.INT_TIM2",                            "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000002
sfr = "INT_CFGCLR.INT_TIM1",                            "Memory",  0xE000E180,  4,        base=16,     bitMask=0x00000001

sfr = "INT_PENDSET",                                    "Memory",  0xE000E200,  4,        base=16
sfr = "INT_PENDSET.INT_DEBUG",                          "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00010000
sfr = "INT_PENDSET.INT_IRQD",                           "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00008000
sfr = "INT_PENDSET.INT_IRQC",                           "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00004000
sfr = "INT_PENDSET.INT_IRQB",                           "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00002000
sfr = "INT_PENDSET.INT_IRQA",                           "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00001000
sfr = "INT_PENDSET.INT_ADC",                            "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000800
sfr = "INT_PENDSET.INT_MACRX",                          "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000400
sfr = "INT_PENDSET.INT_MACTX",                          "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000200
sfr = "INT_PENDSET.INT_MACTMR",                         "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000100
sfr = "INT_PENDSET.INT_SEC",                            "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000080
sfr = "INT_PENDSET.INT_SC2",                            "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000040
sfr = "INT_PENDSET.INT_SC1",                            "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000020
sfr = "INT_PENDSET.INT_SLEEPTMR",                       "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000010
sfr = "INT_PENDSET.INT_BB",                             "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000008
sfr = "INT_PENDSET.INT_MGMT",                           "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000004
sfr = "INT_PENDSET.INT_TIM2",                           "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000002
sfr = "INT_PENDSET.INT_TIM1",                           "Memory",  0xE000E200,  4,        base=16,     bitMask=0x00000001

sfr = "INT_PENDCLR",                                    "Memory",  0xE000E280,  4,        base=16
sfr = "INT_PENDCLR.INT_DEBUG",                          "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00010000
sfr = "INT_PENDCLR.INT_IRQD",                           "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00008000
sfr = "INT_PENDCLR.INT_IRQC",                           "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00004000
sfr = "INT_PENDCLR.INT_IRQB",                           "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00002000
sfr = "INT_PENDCLR.INT_IRQA",                           "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00001000
sfr = "INT_PENDCLR.INT_ADC",                            "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000800
sfr = "INT_PENDCLR.INT_MACRX",                          "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000400
sfr = "INT_PENDCLR.INT_MACTX",                          "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000200
sfr = "INT_PENDCLR.INT_MACTMR",                         "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000100
sfr = "INT_PENDCLR.INT_SEC",                            "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000080
sfr = "INT_PENDCLR.INT_SC2",                            "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000040
sfr = "INT_PENDCLR.INT_SC1",                            "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000020
sfr = "INT_PENDCLR.INT_SLEEPTMR",                       "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000010
sfr = "INT_PENDCLR.INT_BB",                             "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000008
sfr = "INT_PENDCLR.INT_MGMT",                           "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000004
sfr = "INT_PENDCLR.INT_TIM2",                           "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000002
sfr = "INT_PENDCLR.INT_TIM1",                           "Memory",  0xE000E280,  4,        base=16,     bitMask=0x00000001

sfr = "INT_ACTIVE",                                     "Memory",  0xE000E300,  4,        base=16
sfr = "INT_ACTIVE.INT_DEBUG",                           "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00010000
sfr = "INT_ACTIVE.INT_IRQD",                            "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00008000
sfr = "INT_ACTIVE.INT_IRQC",                            "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00004000
sfr = "INT_ACTIVE.INT_IRQB",                            "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00002000
sfr = "INT_ACTIVE.INT_IRQA",                            "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00001000
sfr = "INT_ACTIVE.INT_ADC",                             "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000800
sfr = "INT_ACTIVE.INT_MACRX",                           "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000400
sfr = "INT_ACTIVE.INT_MACTX",                           "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000200
sfr = "INT_ACTIVE.INT_MACTMR",                          "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000100
sfr = "INT_ACTIVE.INT_SEC",                             "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000080
sfr = "INT_ACTIVE.INT_SC2",                             "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000040
sfr = "INT_ACTIVE.INT_SC1",                             "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000020
sfr = "INT_ACTIVE.INT_SLEEPTMR",                        "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000010
sfr = "INT_ACTIVE.INT_BB",                              "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000008
sfr = "INT_ACTIVE.INT_MGMT",                            "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000004
sfr = "INT_ACTIVE.INT_TIM2",                            "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000002
sfr = "INT_ACTIVE.INT_TIM1",                            "Memory",  0xE000E300,  4,        base=16,     bitMask=0x00000001

sfr = "SCS_AFSR",                                       "Memory",  0xE000ED3C,  4,        base=16
sfr = "SCS_AFSR.WRONGSIZE",                             "Memory",  0xE000ED3C,  4,        base=16,     bitMask=0x00000008
sfr = "SCS_AFSR.PROTECTED",                             "Memory",  0xE000ED3C,  4,        base=16,     bitMask=0x00000004
sfr = "SCS_AFSR.RESERVED",                              "Memory",  0xE000ED3C,  4,        base=16,     bitMask=0x00000002
sfr = "SCS_AFSR.MISSED",                                "Memory",  0xE000ED3C,  4,        base=16,     bitMask=0x00000001



; Group info for SFR Window.
[SfrGroupInfo]
group = "GPIO" , "GPIO_PACFGL" , "GPIO_PACFGH" , "GPIO_PAIN" , "GPIO_PAOUT" , "GPIO_PASET" , "GPIO_PACLR" , "GPIO_PBCFGL" , "GPIO_PBCFGH" , "GPIO_PBIN" , "GPIO_PBOUT" , "GPIO_PBSET" , "GPIO_PBCLR" , "GPIO_PCCFGL" , "GPIO_PCCFGH" , "GPIO_PCIN" , "GPIO_PCOUT" , "GPIO_PCSET" , "GPIO_PCCLR" , "GPIO_DBGCFG" , "GPIO_DBGSTAT"
group = "Top-level Interrupts" , "INT_CFGSET" , "INT_CFGCLR" , "INT_PENDSET" , "INT_PENDCLR" , "INT_MISS" , "INT_ACTIVE" , "SCS_AFSR"
group = "External Interrupts" ,  "GPIO_IRQCSEL" , "GPIO_IRQDSEL" , "GPIO_INTCFGA" , "GPIO_INTCFGB" , "GPIO_INTCFGC" , "GPIO_INTCFGD" , "INT_GPIOFLAG"
group = "Serial Controller 1" , "INT_SC1CFG" , "SC1_INTMODE" , "INT_SC1FLAG" , "SC1_RXBEGA" , "SC1_RXENDA" , "SC1_RXBEGB" , "SC1_RXENDB" , "SC1_TXBEGA" , "SC1_TXENDA" , "SC1_TXBEGB" , "SC1_TXENDB" , "SC1_RXCNTA" , "SC1_RXCNTB" , "SC1_TXCNT" , "SC1_DMASTAT" , "SC1_DMACTRL" , "SC1_RXERRA" , "SC1_RXERRB" , "SC1_DATA" , "SC1_SPISTAT" , "SC1_TWISTAT" , "SC1_UARTSTAT" , "SC1_TWICTRL1" , "SC1_TWICTRL2" , "SC1_MODE" , "SC1_SPICFG" , "SC1_UARTCFG" , "SC1_RATELIN" , "SC1_RATEEXP" , "SC1_UARTPER" , "SC1_UARTFRAC" , "SC1_RXCNTSAVED"
group = "Serial Controller 2" , "INT_SC2CFG" , "SC2_INTMODE" , "INT_SC2FLAG" , "SC2_RXBEGA" , "SC2_RXENDA" , "SC2_RXBEGB" , "SC2_RXENDB" , "SC2_TXBEGA" , "SC2_TXENDA" , "SC2_TXBEGB" , "SC2_TXENDB" , "SC2_RXCNTA" , "SC2_RXCNTB" , "SC2_TXCNT" , "SC2_DMASTAT" , "SC2_DMACTRL" , "SC2_RXERRA" , "SC2_RXERRB" , "SC2_DATA" , "SC2_SPISTAT" , "SC2_TWISTAT" , "SC2_TWICTRL1" , "SC2_TWICTRL2" , "SC2_MODE" , "SC2_SPICFG" , "SC2_RATELIN" , "SC2_RATEEXP" , "SC2_RXCNTSAVED"
group = "ADC" , "INT_ADCCFG" , "INT_ADCFLAG" , "ADC_CFG" , "ADC_OFFSET" , "ADC_GAIN" , "ADC_DMACFG" , "ADC_DMASTAT" , "ADC_DMABEG" , "ADC_DMASIZE" , "ADC_DMACUR" , "ADC_DMACNT"
group = "Timer 1" , "INT_TIM1CFG" , "INT_TIM1FLAG" , "INT_TIM1MISS" , "TIM1_CR1" , "TIM1_CR2" , "TIM1_SMCR" , "TIM1_EGR" , "TIM1_CCMR1" , "TIM1_CCMR2" , "TIM1_CCER" , "TIM1_CNT" , "TIM1_PSC" , "TIM1_ARR" , "TIM1_CCR1" , "TIM1_CCR2" , "TIM1_CCR3" , "TIM1_CCR4" , "TIM1_OR"
group = "Timer 2" , "INT_TIM2CFG" ,  "INT_TIM2FLAG" , "INT_TIM2MISS" ,"TIM2_CR1" , "TIM2_CR2" , "TIM2_SMCR" , "TIM2_EGR" , "TIM2_CCMR1" , "TIM2_CCMR2" , "TIM2_CCER" , "TIM2_CNT" , "TIM2_PSC" , "TIM2_ARR" , "TIM2_CCR1" , "TIM2_CCR2" , "TIM2_CCR3" , "TIM2_CCR4" , "TIM2_OR"
group = "Wake-Up Controls" , "GPIO_PAWAKE" , "GPIO_PBWAKE" , "GPIO_PCWAKE" , "GPIO_WAKEFILT"
