40COL
%c%Linpack Results

10x10 Matrix-matrix multiply
START
STOP
HOW MANY SECONDS? 15
133.333333 FLOP/s

Yes I know using BASIC is unfair
But I am too lazy to code up a
6502 FP implementation in assembler
