(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")

  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 4066)
    (zones 0)
    (modules 165)
    (nets 561)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (user_trace_width 0.55)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.27)
    (user_trace_width 1.524)
    (trace_clearance 0.15)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.15)
    (via_size 0.5)
    (via_drill 0.2)
    (via_min_size 0.5)
    (via_min_drill 0.2)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (user_via 1 0.5)
    (user_via 1.524 0.762)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.1524)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.7 0.95)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1)
    (pad_to_paste_clearance -0.0381)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 /MC68k/A0)
  (net 5 /MC68k/A1)
  (net 6 /MC68k/A31)
  (net 7 /MC68k/A30)
  (net 8 /MC68k/A29)
  (net 9 /MC68k/A28)
  (net 10 /MC68k/A27)
  (net 11 /MC68k/A26)
  (net 12 /MC68k/A25)
  (net 13 /MC68k/A24)
  (net 14 /MC68k/A23)
  (net 15 /MC68k/A22)
  (net 16 /MC68k/A21)
  (net 17 /MC68k/A20)
  (net 18 /MC68k/A19)
  (net 19 /MC68k/A18)
  (net 20 /MC68k/A17)
  (net 21 /MC68k/A16)
  (net 22 /MC68k/A15)
  (net 23 /MC68k/A14)
  (net 24 /MC68k/A13)
  (net 25 /MC68k/A12)
  (net 26 /MC68k/A11)
  (net 27 /MC68k/A10)
  (net 28 /CPUBuf.sch/CPU_D15)
  (net 29 /MC68k/A9)
  (net 30 /MC68k/A8)
  (net 31 /MC68k/A7)
  (net 32 /MC68k/A6)
  (net 33 /MC68k/A5)
  (net 34 /MC68k/A4)
  (net 35 /MC68k/A3)
  (net 36 /MC68k/A2)
  (net 37 "Net-(U1-Pad62)")
  (net 38 /PDSBuf/IOB_~RESET~)
  (net 39 /MC68k/~IPL~2)
  (net 40 /MC68k/~IPL~1)
  (net 41 /MC68k/~IPL~0)
  (net 42 "Net-(U1-Pad73)")
  (net 43 "Net-(U1-Pad74)")
  (net 44 /CPUBuf.sch/CPU_D0)
  (net 45 "Net-(U1-Pad121)")
  (net 46 /Control/CPU_~CIIN~)
  (net 47 /Control/CPU_~CBACK~)
  (net 48 /Control/CPU_~HALT~)
  (net 49 /Control/CPU_~BERR~)
  (net 50 /Control/CPU_~STERM~)
  (net 51 /Control/CPUCLK)
  (net 52 "Net-(U1-Pad14)")
  (net 53 "Net-(U1-Pad16)")
  (net 54 /Control/FPU~CS~)
  (net 55 "Net-(U2-Pad15)")
  (net 56 /Control/FPUCLK)
  (net 57 "Net-(U2-Pad4)")
  (net 58 "Net-(U3-PadA2)")
  (net 59 "Net-(U3-PadA3)")
  (net 60 "Net-(U3-PadA4)")
  (net 61 "Net-(U3-PadA5)")
  (net 62 "Net-(U3-PadA6)")
  (net 63 "Net-(U3-PadA7)")
  (net 64 "Net-(U3-PadA8)")
  (net 65 "Net-(U3-PadA9)")
  (net 66 "Net-(U3-PadA10)")
  (net 67 "Net-(U3-PadA11)")
  (net 68 "Net-(U3-PadA12)")
  (net 69 "Net-(U3-PadA13)")
  (net 70 "Net-(U3-PadA14)")
  (net 71 "Net-(U3-PadA15)")
  (net 72 "Net-(U3-PadB1)")
  (net 73 "Net-(U3-PadC1)")
  (net 74 "Net-(U3-PadD1)")
  (net 75 "Net-(U3-PadE1)")
  (net 76 "Net-(U3-PadF1)")
  (net 77 "Net-(U3-PadG1)")
  (net 78 "Net-(U3-PadH1)")
  (net 79 "Net-(U3-PadJ1)")
  (net 80 "Net-(U3-PadB16)")
  (net 81 "Net-(U3-PadB15)")
  (net 82 "Net-(U3-PadB14)")
  (net 83 "Net-(U3-PadB12)")
  (net 84 "Net-(U3-PadB10)")
  (net 85 "Net-(U3-PadB8)")
  (net 86 "Net-(U3-PadB6)")
  (net 87 "Net-(U3-PadB5)")
  (net 88 "Net-(U3-PadB2)")
  (net 89 "Net-(U3-PadB3)")
  (net 90 "Net-(U3-PadC2)")
  (net 91 "Net-(U3-PadC3)")
  (net 92 "Net-(U3-PadC5)")
  (net 93 "Net-(U3-PadC6)")
  (net 94 "Net-(U3-PadC7)")
  (net 95 "Net-(U3-PadC8)")
  (net 96 "Net-(U3-PadC9)")
  (net 97 "Net-(U3-PadD3)")
  (net 98 "Net-(U3-PadD5)")
  (net 99 "Net-(U3-PadD6)")
  (net 100 "Net-(U3-PadD8)")
  (net 101 "Net-(U3-PadD9)")
  (net 102 "Net-(U3-PadE2)")
  (net 103 "Net-(U3-PadE3)")
  (net 104 "Net-(U3-PadE4)")
  (net 105 "Net-(U3-PadC10)")
  (net 106 "Net-(U3-PadC11)")
  (net 107 "Net-(U3-PadD11)")
  (net 108 "Net-(U3-PadD12)")
  (net 109 "Net-(U3-PadC12)")
  (net 110 "Net-(U3-PadC13)")
  (net 111 "Net-(U3-PadC14)")
  (net 112 "Net-(U3-PadD14)")
  (net 113 "Net-(U3-PadC15)")
  (net 114 "Net-(U3-PadD16)")
  (net 115 "Net-(U3-PadC16)")
  (net 116 "Net-(U3-PadE13)")
  (net 117 "Net-(U3-PadF13)")
  (net 118 "Net-(U3-PadG14)")
  (net 119 "Net-(U3-PadF14)")
  (net 120 "Net-(U3-PadE14)")
  (net 121 "Net-(U3-PadE15)")
  (net 122 "Net-(U3-PadF15)")
  (net 123 "Net-(U3-PadG16)")
  (net 124 "Net-(U3-PadF16)")
  (net 125 "Net-(U3-PadE16)")
  (net 126 "Net-(U3-PadF2)")
  (net 127 "Net-(U3-PadF3)")
  (net 128 "Net-(U3-PadF4)")
  (net 129 "Net-(U3-PadG3)")
  (net 130 "Net-(U3-PadH2)")
  (net 131 "Net-(U3-PadH3)")
  (net 132 "Net-(U3-PadH4)")
  (net 133 "Net-(U3-PadJ4)")
  (net 134 "Net-(U3-PadJ3)")
  (net 135 "Net-(U3-PadK1)")
  (net 136 "Net-(U3-PadK2)")
  (net 137 "Net-(U3-PadK3)")
  (net 138 "Net-(U3-PadL4)")
  (net 139 "Net-(U3-PadL3)")
  (net 140 "Net-(U3-PadL1)")
  (net 141 "Net-(U3-PadM1)")
  (net 142 "Net-(U3-PadM2)")
  (net 143 "Net-(U3-PadM3)")
  (net 144 "Net-(U3-PadM4)")
  (net 145 "Net-(U3-PadN4)")
  (net 146 "Net-(U3-PadP4)")
  (net 147 "Net-(U3-PadN3)")
  (net 148 "Net-(U3-PadP2)")
  (net 149 "Net-(U3-PadR2)")
  (net 150 "Net-(U3-PadN1)")
  (net 151 "Net-(U3-PadP1)")
  (net 152 "Net-(U3-PadR1)")
  (net 153 "Net-(U3-PadT4)")
  (net 154 "Net-(U3-PadE8)")
  (net 155 "Net-(U3-PadE7)")
  (net 156 "Net-(U3-PadE6)")
  (net 157 "Net-(U3-PadF5)")
  (net 158 "Net-(U3-PadF6)")
  (net 159 "Net-(U3-PadF7)")
  (net 160 "Net-(U3-PadG5)")
  (net 161 "Net-(U3-PadG6)")
  (net 162 "Net-(U3-PadH5)")
  (net 163 "Net-(U3-PadJ6)")
  (net 164 "Net-(U3-PadK5)")
  (net 165 "Net-(U3-PadK6)")
  (net 166 "Net-(U3-PadL5)")
  (net 167 "Net-(U3-PadL7)")
  (net 168 "Net-(U3-PadL8)")
  (net 169 "Net-(U3-PadM5)")
  (net 170 "Net-(U3-PadM6)")
  (net 171 "Net-(U3-PadM7)")
  (net 172 "Net-(U3-PadP5)")
  (net 173 "Net-(U3-PadP6)")
  (net 174 "Net-(U3-PadR5)")
  (net 175 "Net-(U3-PadT5)")
  (net 176 "Net-(U3-PadT6)")
  (net 177 "Net-(U3-PadN5)")
  (net 178 "Net-(U3-PadN6)")
  (net 179 "Net-(U3-PadP11)")
  (net 180 "Net-(U3-PadP9)")
  (net 181 "Net-(U3-PadP8)")
  (net 182 "Net-(U3-PadP7)")
  (net 183 "Net-(U3-PadR7)")
  (net 184 "Net-(U3-PadR9)")
  (net 185 "Net-(U3-PadT7)")
  (net 186 "Net-(U3-PadT8)")
  (net 187 "Net-(U3-PadT9)")
  (net 188 "Net-(U3-PadN8)")
  (net 189 "Net-(U3-PadE10)")
  (net 190 "Net-(U3-PadE11)")
  (net 191 "Net-(U3-PadE12)")
  (net 192 "Net-(U3-PadF9)")
  (net 193 "Net-(U3-PadF10)")
  (net 194 "Net-(U3-PadF12)")
  (net 195 "Net-(U3-PadG12)")
  (net 196 "Net-(U3-PadG11)")
  (net 197 "Net-(U3-PadR12)")
  (net 198 "Net-(U3-PadT12)")
  (net 199 "Net-(U3-PadH11)")
  (net 200 "Net-(U3-PadJ11)")
  (net 201 "Net-(U3-PadJ12)")
  (net 202 "Net-(U3-PadH13)")
  (net 203 "Net-(U3-PadJ13)")
  (net 204 "Net-(U3-PadL13)")
  (net 205 "Net-(U3-PadM13)")
  (net 206 "Net-(U3-PadT13)")
  (net 207 "Net-(U3-PadN9)")
  (net 208 "Net-(U3-PadM9)")
  (net 209 "Net-(U3-PadL10)")
  (net 210 "Net-(U3-PadM10)")
  (net 211 "Net-(U3-PadT14)")
  (net 212 "Net-(U3-PadR14)")
  (net 213 "Net-(U3-PadP14)")
  (net 214 "Net-(U3-PadN14)")
  (net 215 "Net-(U3-PadM14)")
  (net 216 "Net-(U3-PadL14)")
  (net 217 "Net-(U3-PadK14)")
  (net 218 "Net-(U3-PadJ14)")
  (net 219 "Net-(U3-PadH14)")
  (net 220 "Net-(U3-PadH15)")
  (net 221 "Net-(U3-PadK15)")
  (net 222 "Net-(U3-PadM15)")
  (net 223 "Net-(U3-PadP15)")
  (net 224 "Net-(U3-PadR15)")
  (net 225 "Net-(U3-PadT15)")
  (net 226 "Net-(U3-PadM11)")
  (net 227 "Net-(U3-PadL11)")
  (net 228 "Net-(U3-PadK11)")
  (net 229 "Net-(U3-PadK12)")
  (net 230 "Net-(U3-PadL12)")
  (net 231 "Net-(U3-PadM12)")
  (net 232 "Net-(U3-PadR16)")
  (net 233 "Net-(U3-PadP16)")
  (net 234 "Net-(U3-PadN16)")
  (net 235 "Net-(U3-PadM16)")
  (net 236 "Net-(U3-PadL16)")
  (net 237 "Net-(U3-PadK16)")
  (net 238 "Net-(U3-PadJ16)")
  (net 239 "Net-(U3-PadH16)")
  (net 240 /RAM/D15)
  (net 241 /RAM/D14)
  (net 242 /RAM/D13)
  (net 243 /RAM/D12)
  (net 244 /RAM/D11)
  (net 245 /RAM/D10)
  (net 246 /RAM/D9)
  (net 247 /RAM/D8)
  (net 248 /RAM/DQM1)
  (net 249 /RAM/CLK01)
  (net 250 /RAM/CKE)
  (net 251 /RAM/RA12)
  (net 252 /RAM/RA11)
  (net 253 /RAM/RA9)
  (net 254 /RAM/RA8)
  (net 255 /RAM/RA7)
  (net 256 /RAM/RA6)
  (net 257 /RAM/RA5)
  (net 258 /RAM/RA4)
  (net 259 /RAM/RA3)
  (net 260 /RAM/RA2)
  (net 261 /RAM/RA1)
  (net 262 /RAM/RA0)
  (net 263 /RAM/RA10)
  (net 264 /RAM/BA1)
  (net 265 /RAM/BA0)
  (net 266 /Control/RAM_~CS~)
  (net 267 /Control/RAM_~RAS~)
  (net 268 /Control/RAM_~CAS~)
  (net 269 /Control/RAM_~WE~)
  (net 270 /RAM/DQM0)
  (net 271 /RAM/D7)
  (net 272 /RAM/D6)
  (net 273 /RAM/D5)
  (net 274 /RAM/D4)
  (net 275 /RAM/D3)
  (net 276 /RAM/D2)
  (net 277 /RAM/D1)
  (net 278 /RAM/D0)
  (net 279 /RAM/D16)
  (net 280 /RAM/D17)
  (net 281 /RAM/D18)
  (net 282 /RAM/D19)
  (net 283 /RAM/D20)
  (net 284 /RAM/D21)
  (net 285 /RAM/D22)
  (net 286 /RAM/D23)
  (net 287 /RAM/DQM2)
  (net 288 /RAM/CLK23)
  (net 289 /RAM/DQM3)
  (net 290 /RAM/D24)
  (net 291 /RAM/D25)
  (net 292 /RAM/D26)
  (net 293 /RAM/D27)
  (net 294 /RAM/D28)
  (net 295 /RAM/D29)
  (net 296 /RAM/D30)
  (net 297 /RAM/D31)
  (net 298 /PDSBuf/IOB_SIZ1)
  (net 299 /PDSBuf/IOB_SIZ0)
  (net 300 /PDS/A3)
  (net 301 /PDS/A2)
  (net 302 /PDS/A1)
  (net 303 /PDS/A0)
  (net 304 /PDSBuf/IOB_~AS~)
  (net 305 /PDSBuf/IOB_~DS~)
  (net 306 /Control/IOC_~DS~)
  (net 307 /Control/IOC_~AS~)
  (net 308 /PDSBuf/IOC_A0)
  (net 309 /PDSBuf/IOC_A1)
  (net 310 /PDSBuf/IOC_A2)
  (net 311 /PDSBuf/IOC_A3)
  (net 312 /PDSBuf/IOC_SIZ0)
  (net 313 /PDSBuf/IOC_SIZ1)
  (net 314 /PDSBuf/A~OE~)
  (net 315 /PDSBuf/ADoutLE)
  (net 316 /PDS/A24)
  (net 317 /PDS/A25)
  (net 318 /PDS/A26)
  (net 319 /PDS/A27)
  (net 320 /PDS/A30)
  (net 321 /PDS/A31)
  (net 322 /PDSBuf/IOB_R~W~)
  (net 323 "Net-(U9-Pad19)")
  (net 324 /PDS/A16)
  (net 325 /PDS/A17)
  (net 326 /PDS/A18)
  (net 327 /PDS/A19)
  (net 328 /PDS/A20)
  (net 329 /PDS/A21)
  (net 330 /PDS/A22)
  (net 331 /PDS/A23)
  (net 332 /PDS/A8)
  (net 333 /PDS/A9)
  (net 334 /PDS/A10)
  (net 335 /PDS/A11)
  (net 336 /PDS/A12)
  (net 337 /PDS/A13)
  (net 338 /PDS/A14)
  (net 339 /PDS/A15)
  (net 340 /PDS/A7)
  (net 341 /PDS/A6)
  (net 342 /PDS/A5)
  (net 343 /PDS/A4)
  (net 344 /PDSBuf/IOB_~RMC~)
  (net 345 /PDSBuf/IOB_FC2)
  (net 346 /PDSBuf/IOB_FC1)
  (net 347 /PDSBuf/IOB_FC0)
  (net 348 /Control/IOB_~DSACK~0)
  (net 349 /PDSBuf/IOB_~DSACK~1)
  (net 350 /Control/IOB_~HALT~)
  (net 351 /PDS/C16M)
  (net 352 /Control/IOB_~BERR~)
  (net 353 /PDSBuf/FSB_~RESET~)
  (net 354 "Net-(U13-Pad9)")
  (net 355 /PDSBuf/IOB_~DSACK~0)
  (net 356 "Net-(U13-Pad7)")
  (net 357 /PDSBuf/IOB_~HALT~)
  (net 358 /Control/IOB_C16M)
  (net 359 /PDSBuf/IOB_~BERR~)
  (net 360 /Control/IOB_~DSACK~1)
  (net 361 /Control/CPU_~DSACK~1)
  (net 362 /Control/CPU_~DSACK~0)
  (net 363 "Net-(U22-Pad4)")
  (net 364 "Net-(U22-Pad5)")
  (net 365 "Net-(U22-Pad6)")
  (net 366 "Net-(U22-Pad7)")
  (net 367 "Net-(U22-Pad8)")
  (net 368 "Net-(U22-Pad9)")
  (net 369 "Net-(U22-Pad12)")
  (net 370 "Net-(U22-Pad13)")
  (net 371 "Net-(U22-Pad14)")
  (net 372 "Net-(U22-Pad15)")
  (net 373 "Net-(U22-Pad16)")
  (net 374 "Net-(U22-Pad17)")
  (net 375 "Net-(U23-Pad9)")
  (net 376 "Net-(U24-Pad5)")
  (net 377 "Net-(U24-Pad7)")
  (net 378 "Net-(U24-Pad9)")
  (net 379 /PDSBuf/DDIR)
  (net 380 /PDSBuf/IOC_D0)
  (net 381 /PDSBuf/IOC_D1)
  (net 382 /PDSBuf/IOC_D2)
  (net 383 /PDSBuf/IOC_D3)
  (net 384 /PDSBuf/IOC_D4)
  (net 385 /PDSBuf/IOC_D5)
  (net 386 /PDSBuf/IOC_D6)
  (net 387 /PDSBuf/IOC_D7)
  (net 388 /PDS/D7)
  (net 389 /PDS/D6)
  (net 390 /PDS/D5)
  (net 391 /PDS/D4)
  (net 392 /PDS/D3)
  (net 393 /PDS/D2)
  (net 394 /PDS/D1)
  (net 395 /PDS/D0)
  (net 396 /PDSBuf/D~OE~)
  (net 397 /PDSBuf/IOC_D8)
  (net 398 /PDSBuf/IOC_D9)
  (net 399 /PDSBuf/IOC_D10)
  (net 400 /PDSBuf/IOC_D11)
  (net 401 /PDSBuf/IOC_D12)
  (net 402 /PDSBuf/IOC_D13)
  (net 403 /PDSBuf/IOC_D14)
  (net 404 /PDSBuf/IOC_D15)
  (net 405 /PDS/D15)
  (net 406 /PDS/D14)
  (net 407 /PDS/D13)
  (net 408 /PDS/D12)
  (net 409 /PDS/D11)
  (net 410 /PDS/D10)
  (net 411 /PDS/D9)
  (net 412 /PDS/D8)
  (net 413 /PDS/D16)
  (net 414 /PDS/D17)
  (net 415 /PDS/D18)
  (net 416 /PDS/D19)
  (net 417 /PDS/D20)
  (net 418 /PDS/D21)
  (net 419 /PDS/D22)
  (net 420 /PDS/D23)
  (net 421 /PDSBuf/IOC_D23)
  (net 422 /PDSBuf/IOC_D22)
  (net 423 /PDSBuf/IOC_D21)
  (net 424 /PDSBuf/IOC_D20)
  (net 425 /PDSBuf/IOC_D19)
  (net 426 /PDSBuf/IOC_D18)
  (net 427 /PDSBuf/IOC_D17)
  (net 428 /PDSBuf/IOC_D16)
  (net 429 /PDS/D24)
  (net 430 /PDS/D25)
  (net 431 /PDS/D26)
  (net 432 /PDS/D27)
  (net 433 /PDS/D28)
  (net 434 /PDS/D29)
  (net 435 /PDS/D30)
  (net 436 /PDS/D31)
  (net 437 /PDSBuf/IOC_D31)
  (net 438 /PDSBuf/IOC_D30)
  (net 439 /PDSBuf/IOC_D29)
  (net 440 /PDSBuf/IOC_D28)
  (net 441 /PDSBuf/IOC_D27)
  (net 442 /PDSBuf/IOC_D26)
  (net 443 /PDSBuf/IOC_D25)
  (net 444 /PDSBuf/IOC_D24)
  (net 445 /Control/CPU_D~OE~)
  (net 446 /Control/CPU_DDIR)
  (net 447 +1V2)
  (net 448 "Net-(U6-Pad4)")
  (net 449 "Net-(U6-Pad3)")
  (net 450 "Net-(U6-Pad2)")
  (net 451 "Net-(U6-Pad1)")
  (net 452 -5V)
  (net 453 +12V)
  (net 454 -12V)
  (net 455 /Control/HSWAPEN)
  (net 456 /Control/~INIT~)
  (net 457 /Control/~PROG~)
  (net 458 /Control/M0)
  (net 459 /Control/DONE)
  (net 460 /Control/M1)
  (net 461 /Control/RESET~OE~)
  (net 462 "Net-(R1-Pad1)")
  (net 463 /CPUBuf/CPU_D8)
  (net 464 /CPUBuf/CPU_D9)
  (net 465 /CPUBuf/CPU_D10)
  (net 466 /CPUBuf/CPU_D11)
  (net 467 /CPUBuf/CPU_D12)
  (net 468 /CPUBuf/CPU_D13)
  (net 469 /CPUBuf/CPU_D14)
  (net 470 /CPUBuf/CPU_D15)
  (net 471 /CPUBuf/CPU_D16)
  (net 472 /CPUBuf/CPU_D17)
  (net 473 /CPUBuf/CPU_D18)
  (net 474 /CPUBuf/CPU_D19)
  (net 475 /CPUBuf/CPU_D20)
  (net 476 /CPUBuf/CPU_D21)
  (net 477 /CPUBuf/CPU_D22)
  (net 478 /CPUBuf/CPU_D23)
  (net 479 /CPUBuf/CPU_D24)
  (net 480 /CPUBuf/CPU_D25)
  (net 481 /CPUBuf/CPU_D26)
  (net 482 /CPUBuf/CPU_D27)
  (net 483 /CPUBuf/CPU_D28)
  (net 484 /CPUBuf/CPU_D29)
  (net 485 /CPUBuf/CPU_D30)
  (net 486 /CPUBuf/CPU_D31)
  (net 487 /CPUBuf/CPU_D0)
  (net 488 /CPUBuf/CPU_D1)
  (net 489 /CPUBuf/CPU_D2)
  (net 490 /CPUBuf/CPU_D3)
  (net 491 /CPUBuf/CPU_D4)
  (net 492 /CPUBuf/CPU_D5)
  (net 493 /CPUBuf/CPU_D6)
  (net 494 /CPUBuf/CPU_D7)
  (net 495 /CPUBuf/CPU_R~W~)
  (net 496 /CPUBuf/CPU_~ECS~)
  (net 497 /CPUBuf/CPU_SIZ1)
  (net 498 /CPUBuf/CPU_SIZ0)
  (net 499 /CPUBuf/CPU_~DS~)
  (net 500 /CPUBuf/CPU_~AS~)
  (net 501 /CPUBuf/CPU_~CBREQ~)
  (net 502 /CPUBuf/CPU_~DSACK~1)
  (net 503 /CPUBuf/CPU_~DSACK~0)
  (net 504 /CPUBuf/CPU_FC2)
  (net 505 /CPUBuf/CPU_FC1)
  (net 506 /CPUBuf/CPU_FC0)
  (net 507 /CPUBuf/CPU_~RMC~)
  (net 508 /CPUBuf/CPU_~CIOUT~)
  (net 509 "Net-(U3-PadT3)")
  (net 510 /Control/MOSI_DIN)
  (net 511 /Control/CCLK_SCK)
  (net 512 "Net-(U3-PadT10)")
  (net 513 "Net-(U3-PadP12)")
  (net 514 "Net-(U3-PadN12)")
  (net 515 /CPUBuf/FSB_A24)
  (net 516 /CPUBuf/FSB_A25)
  (net 517 /CPUBuf/FSB_A26)
  (net 518 /CPUBuf/FSB_A27)
  (net 519 /CPUBuf/FSB_A30)
  (net 520 /CPUBuf/FSB_A31)
  (net 521 /CPUBuf/FSB_R~W~)
  (net 522 /CPUBuf/FSB_A23)
  (net 523 /CPUBuf/FSB_A22)
  (net 524 /CPUBuf/FSB_A21)
  (net 525 /CPUBuf/FSB_A20)
  (net 526 /CPUBuf/FSB_A19)
  (net 527 /CPUBuf/FSB_A18)
  (net 528 /CPUBuf/FSB_A17)
  (net 529 /CPUBuf/FSB_A16)
  (net 530 /CPUBuf/FSB_A8)
  (net 531 /CPUBuf/FSB_A9)
  (net 532 /CPUBuf/FSB_A10)
  (net 533 /CPUBuf/FSB_A11)
  (net 534 /CPUBuf/FSB_A12)
  (net 535 /CPUBuf/FSB_A13)
  (net 536 /CPUBuf/FSB_A14)
  (net 537 /CPUBuf/FSB_A15)
  (net 538 /CPUBuf/FSB_FC0)
  (net 539 /CPUBuf/FSB_FC1)
  (net 540 /CPUBuf/FSB_FC2)
  (net 541 /CPUBuf/FSB_A4)
  (net 542 /CPUBuf/FSB_A5)
  (net 543 /CPUBuf/FSB_A6)
  (net 544 /CPUBuf/FSB_A7)
  (net 545 /CPUBuf/A~OE~)
  (net 546 /CPUBuf/FSB_A3)
  (net 547 /CPUBuf/FSB_A2)
  (net 548 /CPUBuf/FSB_A1)
  (net 549 /CPUBuf/FSB_A0)
  (net 550 /CPUBuf/FSB_A28)
  (net 551 /CPUBuf/FSB_A29)
  (net 552 /CPUBuf/DSACK~OE~)
  (net 553 /CPUBuf/FSB_~CIOUT~)
  (net 554 /CPUBuf/FSB_SIZ0)
  (net 555 /CPUBuf/FSB_SIZ1)
  (net 556 /CPUBuf/FSB_~AS~)
  (net 557 /CPUBuf/FSB_~CBREQ~)
  (net 558 /CPUBuf/FSB_~DS~)
  (net 559 /CPUBuf/FSB_~ECS~)
  (net 560 /CPUBuf/FSB_~RMC~)

  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.15)
    (via_dia 0.5)
    (via_drill 0.2)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +1V2)
    (add_net +3V3)
    (add_net +5V)
    (add_net -12V)
    (add_net -5V)
    (add_net /CPUBuf.sch/CPU_D0)
    (add_net /CPUBuf.sch/CPU_D15)
    (add_net /CPUBuf/A~OE~)
    (add_net /CPUBuf/CPU_D0)
    (add_net /CPUBuf/CPU_D1)
    (add_net /CPUBuf/CPU_D10)
    (add_net /CPUBuf/CPU_D11)
    (add_net /CPUBuf/CPU_D12)
    (add_net /CPUBuf/CPU_D13)
    (add_net /CPUBuf/CPU_D14)
    (add_net /CPUBuf/CPU_D15)
    (add_net /CPUBuf/CPU_D16)
    (add_net /CPUBuf/CPU_D17)
    (add_net /CPUBuf/CPU_D18)
    (add_net /CPUBuf/CPU_D19)
    (add_net /CPUBuf/CPU_D2)
    (add_net /CPUBuf/CPU_D20)
    (add_net /CPUBuf/CPU_D21)
    (add_net /CPUBuf/CPU_D22)
    (add_net /CPUBuf/CPU_D23)
    (add_net /CPUBuf/CPU_D24)
    (add_net /CPUBuf/CPU_D25)
    (add_net /CPUBuf/CPU_D26)
    (add_net /CPUBuf/CPU_D27)
    (add_net /CPUBuf/CPU_D28)
    (add_net /CPUBuf/CPU_D29)
    (add_net /CPUBuf/CPU_D3)
    (add_net /CPUBuf/CPU_D30)
    (add_net /CPUBuf/CPU_D31)
    (add_net /CPUBuf/CPU_D4)
    (add_net /CPUBuf/CPU_D5)
    (add_net /CPUBuf/CPU_D6)
    (add_net /CPUBuf/CPU_D7)
    (add_net /CPUBuf/CPU_D8)
    (add_net /CPUBuf/CPU_D9)
    (add_net /CPUBuf/CPU_FC0)
    (add_net /CPUBuf/CPU_FC1)
    (add_net /CPUBuf/CPU_FC2)
    (add_net /CPUBuf/CPU_R~W~)
    (add_net /CPUBuf/CPU_SIZ0)
    (add_net /CPUBuf/CPU_SIZ1)
    (add_net /CPUBuf/CPU_~AS~)
    (add_net /CPUBuf/CPU_~CBREQ~)
    (add_net /CPUBuf/CPU_~CIOUT~)
    (add_net /CPUBuf/CPU_~DSACK~0)
    (add_net /CPUBuf/CPU_~DSACK~1)
    (add_net /CPUBuf/CPU_~DS~)
    (add_net /CPUBuf/CPU_~ECS~)
    (add_net /CPUBuf/CPU_~RMC~)
    (add_net /CPUBuf/DSACK~OE~)
    (add_net /CPUBuf/FSB_A0)
    (add_net /CPUBuf/FSB_A1)
    (add_net /CPUBuf/FSB_A10)
    (add_net /CPUBuf/FSB_A11)
    (add_net /CPUBuf/FSB_A12)
    (add_net /CPUBuf/FSB_A13)
    (add_net /CPUBuf/FSB_A14)
    (add_net /CPUBuf/FSB_A15)
    (add_net /CPUBuf/FSB_A16)
    (add_net /CPUBuf/FSB_A17)
    (add_net /CPUBuf/FSB_A18)
    (add_net /CPUBuf/FSB_A19)
    (add_net /CPUBuf/FSB_A2)
    (add_net /CPUBuf/FSB_A20)
    (add_net /CPUBuf/FSB_A21)
    (add_net /CPUBuf/FSB_A22)
    (add_net /CPUBuf/FSB_A23)
    (add_net /CPUBuf/FSB_A24)
    (add_net /CPUBuf/FSB_A25)
    (add_net /CPUBuf/FSB_A26)
    (add_net /CPUBuf/FSB_A27)
    (add_net /CPUBuf/FSB_A28)
    (add_net /CPUBuf/FSB_A29)
    (add_net /CPUBuf/FSB_A3)
    (add_net /CPUBuf/FSB_A30)
    (add_net /CPUBuf/FSB_A31)
    (add_net /CPUBuf/FSB_A4)
    (add_net /CPUBuf/FSB_A5)
    (add_net /CPUBuf/FSB_A6)
    (add_net /CPUBuf/FSB_A7)
    (add_net /CPUBuf/FSB_A8)
    (add_net /CPUBuf/FSB_A9)
    (add_net /CPUBuf/FSB_FC0)
    (add_net /CPUBuf/FSB_FC1)
    (add_net /CPUBuf/FSB_FC2)
    (add_net /CPUBuf/FSB_R~W~)
    (add_net /CPUBuf/FSB_SIZ0)
    (add_net /CPUBuf/FSB_SIZ1)
    (add_net /CPUBuf/FSB_~AS~)
    (add_net /CPUBuf/FSB_~CBREQ~)
    (add_net /CPUBuf/FSB_~CIOUT~)
    (add_net /CPUBuf/FSB_~DS~)
    (add_net /CPUBuf/FSB_~ECS~)
    (add_net /CPUBuf/FSB_~RMC~)
    (add_net /Control/CCLK_SCK)
    (add_net /Control/CPUCLK)
    (add_net /Control/CPU_DDIR)
    (add_net /Control/CPU_D~OE~)
    (add_net /Control/CPU_~BERR~)
    (add_net /Control/CPU_~CBACK~)
    (add_net /Control/CPU_~CIIN~)
    (add_net /Control/CPU_~DSACK~0)
    (add_net /Control/CPU_~DSACK~1)
    (add_net /Control/CPU_~HALT~)
    (add_net /Control/CPU_~STERM~)
    (add_net /Control/DONE)
    (add_net /Control/FPUCLK)
    (add_net /Control/FPU~CS~)
    (add_net /Control/HSWAPEN)
    (add_net /Control/IOB_C16M)
    (add_net /Control/IOB_~BERR~)
    (add_net /Control/IOB_~DSACK~0)
    (add_net /Control/IOB_~DSACK~1)
    (add_net /Control/IOB_~HALT~)
    (add_net /Control/IOC_~AS~)
    (add_net /Control/IOC_~DS~)
    (add_net /Control/M0)
    (add_net /Control/M1)
    (add_net /Control/MOSI_DIN)
    (add_net /Control/RAM_~CAS~)
    (add_net /Control/RAM_~CS~)
    (add_net /Control/RAM_~RAS~)
    (add_net /Control/RAM_~WE~)
    (add_net /Control/RESET~OE~)
    (add_net /Control/~INIT~)
    (add_net /Control/~PROG~)
    (add_net /MC68k/A0)
    (add_net /MC68k/A1)
    (add_net /MC68k/A10)
    (add_net /MC68k/A11)
    (add_net /MC68k/A12)
    (add_net /MC68k/A13)
    (add_net /MC68k/A14)
    (add_net /MC68k/A15)
    (add_net /MC68k/A16)
    (add_net /MC68k/A17)
    (add_net /MC68k/A18)
    (add_net /MC68k/A19)
    (add_net /MC68k/A2)
    (add_net /MC68k/A20)
    (add_net /MC68k/A21)
    (add_net /MC68k/A22)
    (add_net /MC68k/A23)
    (add_net /MC68k/A24)
    (add_net /MC68k/A25)
    (add_net /MC68k/A26)
    (add_net /MC68k/A27)
    (add_net /MC68k/A28)
    (add_net /MC68k/A29)
    (add_net /MC68k/A3)
    (add_net /MC68k/A30)
    (add_net /MC68k/A31)
    (add_net /MC68k/A4)
    (add_net /MC68k/A5)
    (add_net /MC68k/A6)
    (add_net /MC68k/A7)
    (add_net /MC68k/A8)
    (add_net /MC68k/A9)
    (add_net /MC68k/~IPL~0)
    (add_net /MC68k/~IPL~1)
    (add_net /MC68k/~IPL~2)
    (add_net /PDS/A0)
    (add_net /PDS/A1)
    (add_net /PDS/A10)
    (add_net /PDS/A11)
    (add_net /PDS/A12)
    (add_net /PDS/A13)
    (add_net /PDS/A14)
    (add_net /PDS/A15)
    (add_net /PDS/A16)
    (add_net /PDS/A17)
    (add_net /PDS/A18)
    (add_net /PDS/A19)
    (add_net /PDS/A2)
    (add_net /PDS/A20)
    (add_net /PDS/A21)
    (add_net /PDS/A22)
    (add_net /PDS/A23)
    (add_net /PDS/A24)
    (add_net /PDS/A25)
    (add_net /PDS/A26)
    (add_net /PDS/A27)
    (add_net /PDS/A3)
    (add_net /PDS/A30)
    (add_net /PDS/A31)
    (add_net /PDS/A4)
    (add_net /PDS/A5)
    (add_net /PDS/A6)
    (add_net /PDS/A7)
    (add_net /PDS/A8)
    (add_net /PDS/A9)
    (add_net /PDS/C16M)
    (add_net /PDS/D0)
    (add_net /PDS/D1)
    (add_net /PDS/D10)
    (add_net /PDS/D11)
    (add_net /PDS/D12)
    (add_net /PDS/D13)
    (add_net /PDS/D14)
    (add_net /PDS/D15)
    (add_net /PDS/D16)
    (add_net /PDS/D17)
    (add_net /PDS/D18)
    (add_net /PDS/D19)
    (add_net /PDS/D2)
    (add_net /PDS/D20)
    (add_net /PDS/D21)
    (add_net /PDS/D22)
    (add_net /PDS/D23)
    (add_net /PDS/D24)
    (add_net /PDS/D25)
    (add_net /PDS/D26)
    (add_net /PDS/D27)
    (add_net /PDS/D28)
    (add_net /PDS/D29)
    (add_net /PDS/D3)
    (add_net /PDS/D30)
    (add_net /PDS/D31)
    (add_net /PDS/D4)
    (add_net /PDS/D5)
    (add_net /PDS/D6)
    (add_net /PDS/D7)
    (add_net /PDS/D8)
    (add_net /PDS/D9)
    (add_net /PDSBuf/ADoutLE)
    (add_net /PDSBuf/A~OE~)
    (add_net /PDSBuf/DDIR)
    (add_net /PDSBuf/D~OE~)
    (add_net /PDSBuf/FSB_~RESET~)
    (add_net /PDSBuf/IOB_FC0)
    (add_net /PDSBuf/IOB_FC1)
    (add_net /PDSBuf/IOB_FC2)
    (add_net /PDSBuf/IOB_R~W~)
    (add_net /PDSBuf/IOB_SIZ0)
    (add_net /PDSBuf/IOB_SIZ1)
    (add_net /PDSBuf/IOB_~AS~)
    (add_net /PDSBuf/IOB_~BERR~)
    (add_net /PDSBuf/IOB_~DSACK~0)
    (add_net /PDSBuf/IOB_~DSACK~1)
    (add_net /PDSBuf/IOB_~DS~)
    (add_net /PDSBuf/IOB_~HALT~)
    (add_net /PDSBuf/IOB_~RESET~)
    (add_net /PDSBuf/IOB_~RMC~)
    (add_net /PDSBuf/IOC_A0)
    (add_net /PDSBuf/IOC_A1)
    (add_net /PDSBuf/IOC_A2)
    (add_net /PDSBuf/IOC_A3)
    (add_net /PDSBuf/IOC_D0)
    (add_net /PDSBuf/IOC_D1)
    (add_net /PDSBuf/IOC_D10)
    (add_net /PDSBuf/IOC_D11)
    (add_net /PDSBuf/IOC_D12)
    (add_net /PDSBuf/IOC_D13)
    (add_net /PDSBuf/IOC_D14)
    (add_net /PDSBuf/IOC_D15)
    (add_net /PDSBuf/IOC_D16)
    (add_net /PDSBuf/IOC_D17)
    (add_net /PDSBuf/IOC_D18)
    (add_net /PDSBuf/IOC_D19)
    (add_net /PDSBuf/IOC_D2)
    (add_net /PDSBuf/IOC_D20)
    (add_net /PDSBuf/IOC_D21)
    (add_net /PDSBuf/IOC_D22)
    (add_net /PDSBuf/IOC_D23)
    (add_net /PDSBuf/IOC_D24)
    (add_net /PDSBuf/IOC_D25)
    (add_net /PDSBuf/IOC_D26)
    (add_net /PDSBuf/IOC_D27)
    (add_net /PDSBuf/IOC_D28)
    (add_net /PDSBuf/IOC_D29)
    (add_net /PDSBuf/IOC_D3)
    (add_net /PDSBuf/IOC_D30)
    (add_net /PDSBuf/IOC_D31)
    (add_net /PDSBuf/IOC_D4)
    (add_net /PDSBuf/IOC_D5)
    (add_net /PDSBuf/IOC_D6)
    (add_net /PDSBuf/IOC_D7)
    (add_net /PDSBuf/IOC_D8)
    (add_net /PDSBuf/IOC_D9)
    (add_net /PDSBuf/IOC_SIZ0)
    (add_net /PDSBuf/IOC_SIZ1)
    (add_net /RAM/BA0)
    (add_net /RAM/BA1)
    (add_net /RAM/CKE)
    (add_net /RAM/CLK01)
    (add_net /RAM/CLK23)
    (add_net /RAM/D0)
    (add_net /RAM/D1)
    (add_net /RAM/D10)
    (add_net /RAM/D11)
    (add_net /RAM/D12)
    (add_net /RAM/D13)
    (add_net /RAM/D14)
    (add_net /RAM/D15)
    (add_net /RAM/D16)
    (add_net /RAM/D17)
    (add_net /RAM/D18)
    (add_net /RAM/D19)
    (add_net /RAM/D2)
    (add_net /RAM/D20)
    (add_net /RAM/D21)
    (add_net /RAM/D22)
    (add_net /RAM/D23)
    (add_net /RAM/D24)
    (add_net /RAM/D25)
    (add_net /RAM/D26)
    (add_net /RAM/D27)
    (add_net /RAM/D28)
    (add_net /RAM/D29)
    (add_net /RAM/D3)
    (add_net /RAM/D30)
    (add_net /RAM/D31)
    (add_net /RAM/D4)
    (add_net /RAM/D5)
    (add_net /RAM/D6)
    (add_net /RAM/D7)
    (add_net /RAM/D8)
    (add_net /RAM/D9)
    (add_net /RAM/DQM0)
    (add_net /RAM/DQM1)
    (add_net /RAM/DQM2)
    (add_net /RAM/DQM3)
    (add_net /RAM/RA0)
    (add_net /RAM/RA1)
    (add_net /RAM/RA10)
    (add_net /RAM/RA11)
    (add_net /RAM/RA12)
    (add_net /RAM/RA2)
    (add_net /RAM/RA3)
    (add_net /RAM/RA4)
    (add_net /RAM/RA5)
    (add_net /RAM/RA6)
    (add_net /RAM/RA7)
    (add_net /RAM/RA8)
    (add_net /RAM/RA9)
    (add_net GND)
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad121)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad62)")
    (add_net "Net-(U1-Pad73)")
    (add_net "Net-(U1-Pad74)")
    (add_net "Net-(U13-Pad7)")
    (add_net "Net-(U13-Pad9)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U22-Pad12)")
    (add_net "Net-(U22-Pad13)")
    (add_net "Net-(U22-Pad14)")
    (add_net "Net-(U22-Pad15)")
    (add_net "Net-(U22-Pad16)")
    (add_net "Net-(U22-Pad17)")
    (add_net "Net-(U22-Pad4)")
    (add_net "Net-(U22-Pad5)")
    (add_net "Net-(U22-Pad6)")
    (add_net "Net-(U22-Pad7)")
    (add_net "Net-(U22-Pad8)")
    (add_net "Net-(U22-Pad9)")
    (add_net "Net-(U23-Pad9)")
    (add_net "Net-(U24-Pad5)")
    (add_net "Net-(U24-Pad7)")
    (add_net "Net-(U24-Pad9)")
    (add_net "Net-(U3-PadA10)")
    (add_net "Net-(U3-PadA11)")
    (add_net "Net-(U3-PadA12)")
    (add_net "Net-(U3-PadA13)")
    (add_net "Net-(U3-PadA14)")
    (add_net "Net-(U3-PadA15)")
    (add_net "Net-(U3-PadA2)")
    (add_net "Net-(U3-PadA3)")
    (add_net "Net-(U3-PadA4)")
    (add_net "Net-(U3-PadA5)")
    (add_net "Net-(U3-PadA6)")
    (add_net "Net-(U3-PadA7)")
    (add_net "Net-(U3-PadA8)")
    (add_net "Net-(U3-PadA9)")
    (add_net "Net-(U3-PadB1)")
    (add_net "Net-(U3-PadB10)")
    (add_net "Net-(U3-PadB12)")
    (add_net "Net-(U3-PadB14)")
    (add_net "Net-(U3-PadB15)")
    (add_net "Net-(U3-PadB16)")
    (add_net "Net-(U3-PadB2)")
    (add_net "Net-(U3-PadB3)")
    (add_net "Net-(U3-PadB5)")
    (add_net "Net-(U3-PadB6)")
    (add_net "Net-(U3-PadB8)")
    (add_net "Net-(U3-PadC1)")
    (add_net "Net-(U3-PadC10)")
    (add_net "Net-(U3-PadC11)")
    (add_net "Net-(U3-PadC12)")
    (add_net "Net-(U3-PadC13)")
    (add_net "Net-(U3-PadC14)")
    (add_net "Net-(U3-PadC15)")
    (add_net "Net-(U3-PadC16)")
    (add_net "Net-(U3-PadC2)")
    (add_net "Net-(U3-PadC3)")
    (add_net "Net-(U3-PadC5)")
    (add_net "Net-(U3-PadC6)")
    (add_net "Net-(U3-PadC7)")
    (add_net "Net-(U3-PadC8)")
    (add_net "Net-(U3-PadC9)")
    (add_net "Net-(U3-PadD1)")
    (add_net "Net-(U3-PadD11)")
    (add_net "Net-(U3-PadD12)")
    (add_net "Net-(U3-PadD14)")
    (add_net "Net-(U3-PadD16)")
    (add_net "Net-(U3-PadD3)")
    (add_net "Net-(U3-PadD5)")
    (add_net "Net-(U3-PadD6)")
    (add_net "Net-(U3-PadD8)")
    (add_net "Net-(U3-PadD9)")
    (add_net "Net-(U3-PadE1)")
    (add_net "Net-(U3-PadE10)")
    (add_net "Net-(U3-PadE11)")
    (add_net "Net-(U3-PadE12)")
    (add_net "Net-(U3-PadE13)")
    (add_net "Net-(U3-PadE14)")
    (add_net "Net-(U3-PadE15)")
    (add_net "Net-(U3-PadE16)")
    (add_net "Net-(U3-PadE2)")
    (add_net "Net-(U3-PadE3)")
    (add_net "Net-(U3-PadE4)")
    (add_net "Net-(U3-PadE6)")
    (add_net "Net-(U3-PadE7)")
    (add_net "Net-(U3-PadE8)")
    (add_net "Net-(U3-PadF1)")
    (add_net "Net-(U3-PadF10)")
    (add_net "Net-(U3-PadF12)")
    (add_net "Net-(U3-PadF13)")
    (add_net "Net-(U3-PadF14)")
    (add_net "Net-(U3-PadF15)")
    (add_net "Net-(U3-PadF16)")
    (add_net "Net-(U3-PadF2)")
    (add_net "Net-(U3-PadF3)")
    (add_net "Net-(U3-PadF4)")
    (add_net "Net-(U3-PadF5)")
    (add_net "Net-(U3-PadF6)")
    (add_net "Net-(U3-PadF7)")
    (add_net "Net-(U3-PadF9)")
    (add_net "Net-(U3-PadG1)")
    (add_net "Net-(U3-PadG11)")
    (add_net "Net-(U3-PadG12)")
    (add_net "Net-(U3-PadG14)")
    (add_net "Net-(U3-PadG16)")
    (add_net "Net-(U3-PadG3)")
    (add_net "Net-(U3-PadG5)")
    (add_net "Net-(U3-PadG6)")
    (add_net "Net-(U3-PadH1)")
    (add_net "Net-(U3-PadH11)")
    (add_net "Net-(U3-PadH13)")
    (add_net "Net-(U3-PadH14)")
    (add_net "Net-(U3-PadH15)")
    (add_net "Net-(U3-PadH16)")
    (add_net "Net-(U3-PadH2)")
    (add_net "Net-(U3-PadH3)")
    (add_net "Net-(U3-PadH4)")
    (add_net "Net-(U3-PadH5)")
    (add_net "Net-(U3-PadJ1)")
    (add_net "Net-(U3-PadJ11)")
    (add_net "Net-(U3-PadJ12)")
    (add_net "Net-(U3-PadJ13)")
    (add_net "Net-(U3-PadJ14)")
    (add_net "Net-(U3-PadJ16)")
    (add_net "Net-(U3-PadJ3)")
    (add_net "Net-(U3-PadJ4)")
    (add_net "Net-(U3-PadJ6)")
    (add_net "Net-(U3-PadK1)")
    (add_net "Net-(U3-PadK11)")
    (add_net "Net-(U3-PadK12)")
    (add_net "Net-(U3-PadK14)")
    (add_net "Net-(U3-PadK15)")
    (add_net "Net-(U3-PadK16)")
    (add_net "Net-(U3-PadK2)")
    (add_net "Net-(U3-PadK3)")
    (add_net "Net-(U3-PadK5)")
    (add_net "Net-(U3-PadK6)")
    (add_net "Net-(U3-PadL1)")
    (add_net "Net-(U3-PadL10)")
    (add_net "Net-(U3-PadL11)")
    (add_net "Net-(U3-PadL12)")
    (add_net "Net-(U3-PadL13)")
    (add_net "Net-(U3-PadL14)")
    (add_net "Net-(U3-PadL16)")
    (add_net "Net-(U3-PadL3)")
    (add_net "Net-(U3-PadL4)")
    (add_net "Net-(U3-PadL5)")
    (add_net "Net-(U3-PadL7)")
    (add_net "Net-(U3-PadL8)")
    (add_net "Net-(U3-PadM1)")
    (add_net "Net-(U3-PadM10)")
    (add_net "Net-(U3-PadM11)")
    (add_net "Net-(U3-PadM12)")
    (add_net "Net-(U3-PadM13)")
    (add_net "Net-(U3-PadM14)")
    (add_net "Net-(U3-PadM15)")
    (add_net "Net-(U3-PadM16)")
    (add_net "Net-(U3-PadM2)")
    (add_net "Net-(U3-PadM3)")
    (add_net "Net-(U3-PadM4)")
    (add_net "Net-(U3-PadM5)")
    (add_net "Net-(U3-PadM6)")
    (add_net "Net-(U3-PadM7)")
    (add_net "Net-(U3-PadM9)")
    (add_net "Net-(U3-PadN1)")
    (add_net "Net-(U3-PadN12)")
    (add_net "Net-(U3-PadN14)")
    (add_net "Net-(U3-PadN16)")
    (add_net "Net-(U3-PadN3)")
    (add_net "Net-(U3-PadN4)")
    (add_net "Net-(U3-PadN5)")
    (add_net "Net-(U3-PadN6)")
    (add_net "Net-(U3-PadN8)")
    (add_net "Net-(U3-PadN9)")
    (add_net "Net-(U3-PadP1)")
    (add_net "Net-(U3-PadP11)")
    (add_net "Net-(U3-PadP12)")
    (add_net "Net-(U3-PadP14)")
    (add_net "Net-(U3-PadP15)")
    (add_net "Net-(U3-PadP16)")
    (add_net "Net-(U3-PadP2)")
    (add_net "Net-(U3-PadP4)")
    (add_net "Net-(U3-PadP5)")
    (add_net "Net-(U3-PadP6)")
    (add_net "Net-(U3-PadP7)")
    (add_net "Net-(U3-PadP8)")
    (add_net "Net-(U3-PadP9)")
    (add_net "Net-(U3-PadR1)")
    (add_net "Net-(U3-PadR12)")
    (add_net "Net-(U3-PadR14)")
    (add_net "Net-(U3-PadR15)")
    (add_net "Net-(U3-PadR16)")
    (add_net "Net-(U3-PadR2)")
    (add_net "Net-(U3-PadR5)")
    (add_net "Net-(U3-PadR7)")
    (add_net "Net-(U3-PadR9)")
    (add_net "Net-(U3-PadT10)")
    (add_net "Net-(U3-PadT12)")
    (add_net "Net-(U3-PadT13)")
    (add_net "Net-(U3-PadT14)")
    (add_net "Net-(U3-PadT15)")
    (add_net "Net-(U3-PadT3)")
    (add_net "Net-(U3-PadT4)")
    (add_net "Net-(U3-PadT5)")
    (add_net "Net-(U3-PadT6)")
    (add_net "Net-(U3-PadT7)")
    (add_net "Net-(U3-PadT8)")
    (add_net "Net-(U3-PadT9)")
    (add_net "Net-(U6-Pad1)")
    (add_net "Net-(U6-Pad2)")
    (add_net "Net-(U6-Pad3)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U9-Pad19)")
  )

  (module stdpads:TQFP-100_14x14mm_P0.5mm (layer F.Cu) (tedit 608E5AA2) (tstamp 61BA4157)
    (at 243.6 174)
    (descr "TQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TQFP QFP")
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.035)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value TQFP-100_14x14mm_P0.5mm (at 1.05 0 90) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start 6.4 -8.65) (end 0 -8.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.4 -7.25) (end 6.4 -8.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.25 -7.25) (end 6.4 -7.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.25 -6.4) (end 7.25 -7.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.65 -6.4) (end 7.25 -6.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.65 0) (end 8.65 -6.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.4 8.65) (end 0 8.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.4 7.25) (end 6.4 8.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.25 7.25) (end 6.4 7.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 7.25 6.4) (end 7.25 7.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.65 6.4) (end 7.25 6.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.65 0) (end 8.65 6.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.4 -8.65) (end 0 -8.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.4 -7.25) (end -6.4 -8.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -7.25 -7.25) (end -6.4 -7.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -7.25 -6.4) (end -7.25 -7.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.65 -6.4) (end -7.25 -6.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.65 0) (end -8.65 -6.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.4 8.65) (end 0 8.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.4 7.25) (end -6.4 8.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -7.25 7.25) (end -6.4 7.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -7.25 6.4) (end -7.25 7.25) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.65 6.4) (end -7.25 6.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.65 0) (end -8.65 6.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6 7) (end -7 6) (layer F.Fab) (width 0.1))
    (fp_line (start 7 7) (end -6 7) (layer F.Fab) (width 0.1))
    (fp_line (start 7 -7) (end 7 7) (layer F.Fab) (width 0.1))
    (fp_line (start -7 -7) (end 7 -7) (layer F.Fab) (width 0.1))
    (fp_line (start -7 6) (end -7 -7) (layer F.Fab) (width 0.1))
    (fp_line (start -6.41 7.11) (end -6.41 8.4) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.11 7.11) (end -6.41 7.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.11 6.41) (end -7.11 7.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.11 -7.11) (end -6.41 -7.11) (layer F.SilkS) (width 0.12))
    (fp_line (start -7.11 -6.41) (end -7.11 -7.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 7.11) (end 6.41 7.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 6.41) (end 7.11 7.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -7.11) (end 6.41 -7.11) (layer F.SilkS) (width 0.12))
    (fp_line (start 7.11 -6.41) (end 7.11 -7.11) (layer F.SilkS) (width 0.12))
    (pad 1 smd roundrect (at -6 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -5.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -4.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -4 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -3.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -2.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -2 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at -1.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at -1 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at -0.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at 0 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 14 smd roundrect (at 0.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at 1 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 16 smd roundrect (at 1.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 17 smd roundrect (at 2 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 18 smd roundrect (at 2.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 19 smd roundrect (at 3 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 20 smd roundrect (at 3.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 21 smd roundrect (at 4 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 22 smd roundrect (at 4.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 23 smd roundrect (at 5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 24 smd roundrect (at 5.5 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 25 smd roundrect (at 6 7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 26 smd roundrect (at 7.6625 6 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 27 smd roundrect (at 7.6625 5.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 28 smd roundrect (at 7.6625 5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 29 smd roundrect (at 7.6625 4.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 30 smd roundrect (at 7.6625 4 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 31 smd roundrect (at 7.6625 3.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 7.6625 3 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 7.6625 2.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 7.6625 2 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 7.6625 1.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 36 smd roundrect (at 7.6625 1 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 37 smd roundrect (at 7.6625 0.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 38 smd roundrect (at 7.6625 0 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 39 smd roundrect (at 7.6625 -0.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 40 smd roundrect (at 7.6625 -1 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 41 smd roundrect (at 7.6625 -1.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 42 smd roundrect (at 7.6625 -2 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 43 smd roundrect (at 7.6625 -2.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 44 smd roundrect (at 7.6625 -3 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 45 smd roundrect (at 7.6625 -3.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 46 smd roundrect (at 7.6625 -4 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 47 smd roundrect (at 7.6625 -4.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 48 smd roundrect (at 7.6625 -5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 49 smd roundrect (at 7.6625 -5.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 50 smd roundrect (at 7.6625 -6 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 51 smd roundrect (at 6 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 52 smd roundrect (at 5.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 53 smd roundrect (at 5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 54 smd roundrect (at 4.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 55 smd roundrect (at 4 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 56 smd roundrect (at 3.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 57 smd roundrect (at 3 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 58 smd roundrect (at 2.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 59 smd roundrect (at 2 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 60 smd roundrect (at 1.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 61 smd roundrect (at 1 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 62 smd roundrect (at 0.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 63 smd roundrect (at 0 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 64 smd roundrect (at -0.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 65 smd roundrect (at -1 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 66 smd roundrect (at -1.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 67 smd roundrect (at -2 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 68 smd roundrect (at -2.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 69 smd roundrect (at -3 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 70 smd roundrect (at -3.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 71 smd roundrect (at -4 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 72 smd roundrect (at -4.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 73 smd roundrect (at -5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 74 smd roundrect (at -5.5 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 75 smd roundrect (at -6 -7.6625 90) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 76 smd roundrect (at -7.6625 -6 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 77 smd roundrect (at -7.6625 -5.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 78 smd roundrect (at -7.6625 -5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 79 smd roundrect (at -7.6625 -4.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 80 smd roundrect (at -7.6625 -4 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 81 smd roundrect (at -7.6625 -3.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 82 smd roundrect (at -7.6625 -3 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 83 smd roundrect (at -7.6625 -2.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 84 smd roundrect (at -7.6625 -2 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 85 smd roundrect (at -7.6625 -1.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 86 smd roundrect (at -7.6625 -1 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 87 smd roundrect (at -7.6625 -0.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 88 smd roundrect (at -7.6625 0 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 89 smd roundrect (at -7.6625 0.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 90 smd roundrect (at -7.6625 1 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 91 smd roundrect (at -7.6625 1.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 92 smd roundrect (at -7.6625 2 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 93 smd roundrect (at -7.6625 2.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 94 smd roundrect (at -7.6625 3 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 95 smd roundrect (at -7.6625 3.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 96 smd roundrect (at -7.6625 4 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 97 smd roundrect (at -7.6625 4.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 98 smd roundrect (at -7.6625 5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 99 smd roundrect (at -7.6625 5.5 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 100 smd roundrect (at -7.6625 6 90) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-100_14x14mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:PLCC-68_SMDSocket (layer F.Cu) (tedit 616FF780) (tstamp 617CEACC)
    (at 207.5815 113.792 90)
    (descr "PLCC, 68 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_plcc_jLead_generator.py")
    (tags "PLCC LCC")
    (path /5F72F108/63A841DD)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference U2 (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value MC68882FN (at 0 1.27 90) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start -12.9 -10.71) (end -12.9 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -12.37 -10.71) (end -12.9 -10.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start -12.37 -11.08) (end -12.37 -10.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start -11.08 -12.37) (end -12.37 -11.08) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.71 -12.37) (end -11.08 -12.37) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.71 -12.9) (end -10.71 -12.37) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 -12.9) (end -10.71 -12.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.9 10.71) (end 12.9 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.37 10.71) (end 12.9 10.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.37 12.37) (end 12.37 10.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.71 12.37) (end 12.37 12.37) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.71 12.9) (end 10.71 12.37) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 12.9) (end 10.71 12.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -12.9 10.71) (end -12.9 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start -12.37 10.71) (end -12.9 10.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start -12.37 12.37) (end -12.37 10.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.71 12.37) (end -12.37 12.37) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.71 12.9) (end -10.71 12.37) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 12.9) (end -10.71 12.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.9 -10.71) (end 12.9 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.37 -10.71) (end 12.9 -10.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start 12.37 -12.37) (end 12.37 -10.71) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.71 -12.37) (end 12.37 -12.37) (layer F.CrtYd) (width 0.05))
    (fp_line (start 10.71 -12.9) (end 10.71 -12.37) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 -12.9) (end 10.71 -12.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 -12.1158) (end 0 -11.408693) (layer F.Fab) (width 0.1))
    (fp_line (start -10.9728 -12.1158) (end -0.5 -12.1158) (layer F.Fab) (width 0.1))
    (fp_line (start -12.1158 -10.9728) (end -10.9728 -12.1158) (layer F.Fab) (width 0.1))
    (fp_line (start -12.1158 12.1158) (end -12.1158 -10.9728) (layer F.Fab) (width 0.1))
    (fp_line (start 12.1158 12.1158) (end -12.1158 12.1158) (layer F.Fab) (width 0.1))
    (fp_line (start 12.1158 -12.1158) (end 12.1158 12.1158) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -12.1158) (end 12.1158 -12.1158) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -11.408693) (end 0.5 -12.1158) (layer F.Fab) (width 0.1))
    (fp_line (start -12.2258 -11.050582) (end -12.2258 -10.72) (layer F.SilkS) (width 0.12))
    (fp_line (start -11.050582 -12.2258) (end -12.2258 -11.050582) (layer F.SilkS) (width 0.12))
    (fp_line (start -10.72 -12.2258) (end -11.050582 -12.2258) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.2258 12.2258) (end 12.2258 10.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.72 12.2258) (end 12.2258 12.2258) (layer F.SilkS) (width 0.12))
    (fp_line (start -12.2258 12.2258) (end -12.2258 10.72) (layer F.SilkS) (width 0.12))
    (fp_line (start -10.72 12.2258) (end -12.2258 12.2258) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.2258 -12.2258) (end 12.2258 -10.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.72 -12.2258) (end 12.2258 -12.2258) (layer F.SilkS) (width 0.12))
    (fp_line (start 15.625 -15.625) (end 1 -15.625) (layer F.SilkS) (width 0.12))
    (fp_line (start 15.625 15.625) (end 15.625 -15.625) (layer F.SilkS) (width 0.12))
    (fp_line (start -15.625 15.625) (end 15.625 15.625) (layer F.SilkS) (width 0.12))
    (fp_line (start -15.625 -14.625) (end -15.625 15.625) (layer F.SilkS) (width 0.12))
    (fp_line (start -14.625 -15.625) (end -15.625 -14.625) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -15.625) (end -14.625 -15.625) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -14.475) (end 0.5 -15.475) (layer F.Fab) (width 0.1))
    (fp_line (start -0.5 -15.475) (end 0 -14.475) (layer F.Fab) (width 0.1))
    (fp_line (start 14.205 -14.205) (end -14.205 -14.205) (layer F.Fab) (width 0.1))
    (fp_line (start 14.205 14.205) (end 14.205 -14.205) (layer F.Fab) (width 0.1))
    (fp_line (start -14.205 14.205) (end 14.205 14.205) (layer F.Fab) (width 0.1))
    (fp_line (start -14.205 -14.205) (end -14.205 14.205) (layer F.Fab) (width 0.1))
    (fp_line (start 15.95 -15.95) (end -15.95 -15.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 15.95 15.95) (end 15.95 -15.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -15.95 15.95) (end 15.95 15.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -15.95 -15.95) (end -15.95 15.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 15.475 -15.475) (end -14.475 -15.475) (layer F.Fab) (width 0.1))
    (fp_line (start 15.475 15.475) (end 15.475 -15.475) (layer F.Fab) (width 0.1))
    (fp_line (start -15.475 15.475) (end 15.475 15.475) (layer F.Fab) (width 0.1))
    (fp_line (start -15.475 -14.475) (end -15.475 15.475) (layer F.Fab) (width 0.1))
    (fp_line (start -14.475 -15.475) (end -15.475 -14.475) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 66 smd roundrect (at 3.81 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 492 /CPUBuf/CPU_D5))
    (pad 65 smd roundrect (at 5.08 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 493 /CPUBuf/CPU_D6))
    (pad 64 smd roundrect (at 6.35 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 494 /CPUBuf/CPU_D7))
    (pad 63 smd roundrect (at 7.62 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 62 smd roundrect (at 8.89 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 463 /CPUBuf/CPU_D8))
    (pad 61 smd roundrect (at 10.16 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 60 smd roundrect (at 11.8 -10.16 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 464 /CPUBuf/CPU_D9))
    (pad 40 smd roundrect (at 6.35 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 479 /CPUBuf/CPU_D24))
    (pad 39 smd roundrect (at 5.08 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 480 /CPUBuf/CPU_D25))
    (pad 38 smd roundrect (at 3.81 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 481 /CPUBuf/CPU_D26))
    (pad 37 smd roundrect (at 2.54 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 482 /CPUBuf/CPU_D27))
    (pad 36 smd roundrect (at 1.27 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 483 /CPUBuf/CPU_D28))
    (pad 35 smd roundrect (at 0 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 484 /CPUBuf/CPU_D29))
    (pad 34 smd roundrect (at -1.27 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 485 /CPUBuf/CPU_D30))
    (pad 33 smd roundrect (at -2.54 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 486 /CPUBuf/CPU_D31))
    (pad 32 smd roundrect (at -3.81 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 502 /CPUBuf/CPU_~DSACK~1))
    (pad 31 smd roundrect (at -5.08 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 503 /CPUBuf/CPU_~DSACK~0))
    (pad 30 smd roundrect (at -6.35 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 29 smd roundrect (at -7.62 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /Control/FPU~CS~))
    (pad 28 smd roundrect (at -8.89 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 495 /CPUBuf/CPU_R~W~))
    (pad 27 smd roundrect (at -10.16 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 26 smd roundrect (at -11.8 10.16 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 25 smd roundrect (at -11.8 8.89 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /MC68k/A1))
    (pad 24 smd roundrect (at -11.8 7.62 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /MC68k/A2))
    (pad 23 smd roundrect (at -11.8 6.35 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /MC68k/A3))
    (pad 22 smd roundrect (at -11.8 5.08 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /MC68k/A4))
    (pad 21 smd roundrect (at -11.8 3.81 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 500 /CPUBuf/CPU_~AS~))
    (pad 20 smd roundrect (at -11.8 2.54 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 499 /CPUBuf/CPU_~DS~))
    (pad 19 smd roundrect (at -11.8 1.27 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 18 smd roundrect (at -11.8 0 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 17 smd roundrect (at -11.8 -1.27 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 16 smd roundrect (at -11.8 -2.54 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 15 smd roundrect (at -11.8 -3.81 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(U2-Pad15)"))
    (pad 14 smd roundrect (at -11.8 -5.08 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 13 smd roundrect (at -11.8 -6.35 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /PDSBuf/IOB_~RESET~))
    (pad 12 smd roundrect (at -11.8 -7.62 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at -11.8 -8.89 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /Control/FPUCLK))
    (pad 10 smd roundrect (at -11.8 -10.16 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 9 smd roundrect (at -10.16 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at -8.89 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 55 smd roundrect (at 11.8 -3.81 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 469 /CPUBuf/CPU_D14))
    (pad 54 smd roundrect (at 11.8 -2.54 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 470 /CPUBuf/CPU_D15))
    (pad 53 smd roundrect (at 11.8 -1.27 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 52 smd roundrect (at 11.8 0 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 51 smd roundrect (at 11.8 1.27 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 50 smd roundrect (at 11.8 2.54 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 471 /CPUBuf/CPU_D16))
    (pad 49 smd roundrect (at 11.8 3.81 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 472 /CPUBuf/CPU_D17))
    (pad 48 smd roundrect (at 11.8 5.08 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 473 /CPUBuf/CPU_D18))
    (pad 47 smd roundrect (at 11.8 6.35 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 474 /CPUBuf/CPU_D19))
    (pad 46 smd roundrect (at 11.8 7.62 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 475 /CPUBuf/CPU_D20))
    (pad 45 smd roundrect (at 11.8 8.89 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 476 /CPUBuf/CPU_D21))
    (pad 44 smd roundrect (at 11.8 10.16 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 477 /CPUBuf/CPU_D22))
    (pad 43 smd roundrect (at 10.16 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 42 smd roundrect (at 8.89 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 478 /CPUBuf/CPU_D23))
    (pad 41 smd roundrect (at 7.62 11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 59 smd roundrect (at 11.8 -8.89 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 465 /CPUBuf/CPU_D10))
    (pad 58 smd roundrect (at 11.8 -7.62 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 466 /CPUBuf/CPU_D11))
    (pad 57 smd roundrect (at 11.8 -6.35 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 467 /CPUBuf/CPU_D12))
    (pad 56 smd roundrect (at 11.8 -5.08 90) (size 1.7 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 468 /CPUBuf/CPU_D13))
    (pad 67 smd roundrect (at 2.54 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 491 /CPUBuf/CPU_D4))
    (pad 68 smd roundrect (at 1.27 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 490 /CPUBuf/CPU_D3))
    (pad 7 smd roundrect (at -7.62 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at -6.35 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 5 smd roundrect (at -5.08 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at -3.81 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(U2-Pad4)"))
    (pad 3 smd roundrect (at -2.54 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 487 /CPUBuf/CPU_D0))
    (pad 2 smd roundrect (at -1.27 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 488 /CPUBuf/CPU_D1))
    (pad 1 smd roundrect (at 0 -11.8 90) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 489 /CPUBuf/CPU_D2))
    (model ${KIPRJMOD}/../../stdpads.3dshapes/PLCC-68_PTHSocket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.5))
      (rotate (xyz 0 0 180))
    )
    (model ${KIPRJMOD}/../../stdpads.3dshapes/PLCC-68.wrl
      (offset (xyz 0 0 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AB4A40)
    (at 209.65 38.8)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 447 +1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AB4B1D)
    (at 197.35 49 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 447 +1V2))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AB4B0F)
    (at 197.35 51.1 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 447 +1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AB4A4E)
    (at 207.55 38.8 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 447 +1V2))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_BGA:BGA-256_17.0x17.0mm_Layout16x16_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD (layer F.Cu) (tedit 5A058D74) (tstamp 6178601D)
    (at 208.6 50.05 90)
    (descr "BGA-256, dimensions: https://www.xilinx.com/support/documentation/package_specs/ft256.pdf, design rules: https://www.xilinx.com/support/documentation/user_guides/ug1099-bga-device-design-rules.pdf")
    (tags BGA-256)
    (path /5F723173/63B6D9FE)
    (attr smd)
    (fp_text reference U3 (at 0 -9.6 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value XC6SLX9-FTG256 (at 0 9.7 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 9.5 9.5) (end -9.5 9.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9.5 9.5) (end 9.5 -9.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -9.5 -9.5) (end -9.5 9.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -9.5 -9.5) (end 9.5 -9.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.5 -8) (end -8.5 8.5) (layer F.Fab) (width 0.1))
    (fp_line (start -8 -8.5) (end -8.5 -8) (layer F.Fab) (width 0.1))
    (fp_line (start 8.5 -8.5) (end -8 -8.5) (layer F.Fab) (width 0.1))
    (fp_line (start 8.5 8.5) (end 8.5 -8.5) (layer F.Fab) (width 0.1))
    (fp_line (start -8.5 8.5) (end 8.5 8.5) (layer F.Fab) (width 0.1))
    (fp_line (start 8.6 8.6) (end 8.6 -8.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -8.6 8.6) (end 8.6 8.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -8.6 -8.6) (end -8.6 8.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.6 -8.6) (end -8.6 -8.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -8.8 -8.8) (end -8.8 -8.1) (layer F.SilkS) (width 0.12))
    (fp_line (start -8.1 -8.8) (end -8.8 -8.8) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad A1 smd circle (at -7.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad A2 smd circle (at -6.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U3-PadA2)"))
    (pad A3 smd circle (at -5.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U3-PadA3)"))
    (pad A4 smd circle (at -4.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U3-PadA4)"))
    (pad A5 smd circle (at -3.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U3-PadA5)"))
    (pad A6 smd circle (at -2.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U3-PadA6)"))
    (pad A7 smd circle (at -1.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U3-PadA7)"))
    (pad A8 smd circle (at -0.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U3-PadA8)"))
    (pad A9 smd circle (at 0.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U3-PadA9)"))
    (pad A10 smd circle (at 1.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U3-PadA10)"))
    (pad A11 smd circle (at 2.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U3-PadA11)"))
    (pad A12 smd circle (at 3.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U3-PadA12)"))
    (pad A13 smd circle (at 4.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U3-PadA13)"))
    (pad A14 smd circle (at 5.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U3-PadA14)"))
    (pad A15 smd circle (at 6.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U3-PadA15)"))
    (pad A16 smd circle (at 7.5 -7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad B1 smd circle (at -7.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U3-PadB1)"))
    (pad C1 smd circle (at -7.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U3-PadC1)"))
    (pad D1 smd circle (at -7.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U3-PadD1)"))
    (pad E1 smd circle (at -7.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U3-PadE1)"))
    (pad F1 smd circle (at -7.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U3-PadF1)"))
    (pad G1 smd circle (at -7.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U3-PadG1)"))
    (pad H1 smd circle (at -7.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U3-PadH1)"))
    (pad J1 smd circle (at -7.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U3-PadJ1)"))
    (pad B16 smd circle (at 7.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U3-PadB16)"))
    (pad B15 smd circle (at 6.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U3-PadB15)"))
    (pad B14 smd circle (at 5.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U3-PadB14)"))
    (pad B13 smd circle (at 4.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad B12 smd circle (at 3.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U3-PadB12)"))
    (pad B11 smd circle (at 2.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad B10 smd circle (at 1.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U3-PadB10)"))
    (pad B9 smd circle (at 0.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad B8 smd circle (at -0.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U3-PadB8)"))
    (pad B7 smd circle (at -1.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad B6 smd circle (at -2.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U3-PadB6)"))
    (pad B5 smd circle (at -3.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U3-PadB5)"))
    (pad B2 smd circle (at -6.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U3-PadB2)"))
    (pad B3 smd circle (at -5.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U3-PadB3)"))
    (pad B4 smd circle (at -4.5 -6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad C2 smd circle (at -6.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U3-PadC2)"))
    (pad C3 smd circle (at -5.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U3-PadC3)"))
    (pad C4 smd circle (at -4.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 455 /Control/HSWAPEN))
    (pad C5 smd circle (at -3.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U3-PadC5)"))
    (pad C6 smd circle (at -2.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U3-PadC6)"))
    (pad C7 smd circle (at -1.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U3-PadC7)"))
    (pad C8 smd circle (at -0.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U3-PadC8)"))
    (pad C9 smd circle (at 0.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U3-PadC9)"))
    (pad D2 smd circle (at -6.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad D3 smd circle (at -5.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U3-PadD3)"))
    (pad D4 smd circle (at -4.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad D5 smd circle (at -3.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(U3-PadD5)"))
    (pad D6 smd circle (at -2.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(U3-PadD6)"))
    (pad D7 smd circle (at -1.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad D8 smd circle (at -0.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(U3-PadD8)"))
    (pad D9 smd circle (at 0.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(U3-PadD9)"))
    (pad E2 smd circle (at -6.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(U3-PadE2)"))
    (pad E3 smd circle (at -5.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(U3-PadE3)"))
    (pad E4 smd circle (at -4.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(U3-PadE4)"))
    (pad C10 smd circle (at 1.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(U3-PadC10)"))
    (pad D10 smd circle (at 1.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad C11 smd circle (at 2.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U3-PadC11)"))
    (pad D11 smd circle (at 2.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U3-PadD11)"))
    (pad D12 smd circle (at 3.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(U3-PadD12)"))
    (pad C12 smd circle (at 3.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(U3-PadC12)"))
    (pad C13 smd circle (at 4.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(U3-PadC13)"))
    (pad C14 smd circle (at 5.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(U3-PadC14)"))
    (pad D14 smd circle (at 5.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(U3-PadD14)"))
    (pad D13 smd circle (at 4.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad C15 smd circle (at 6.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(U3-PadC15)"))
    (pad D15 smd circle (at 6.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad D16 smd circle (at 7.5 -4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(U3-PadD16)"))
    (pad C16 smd circle (at 7.5 -5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(U3-PadC16)"))
    (pad E13 smd circle (at 4.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(U3-PadE13)"))
    (pad F13 smd circle (at 4.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(U3-PadF13)"))
    (pad G13 smd circle (at 4.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad G14 smd circle (at 5.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(U3-PadG14)"))
    (pad F14 smd circle (at 5.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(U3-PadF14)"))
    (pad E14 smd circle (at 5.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(U3-PadE14)"))
    (pad E15 smd circle (at 6.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(U3-PadE15)"))
    (pad F15 smd circle (at 6.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(U3-PadF15)"))
    (pad G15 smd circle (at 6.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad G16 smd circle (at 7.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(U3-PadG16)"))
    (pad F16 smd circle (at 7.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(U3-PadF16)"))
    (pad E16 smd circle (at 7.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U3-PadE16)"))
    (pad F2 smd circle (at -6.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U3-PadF2)"))
    (pad F3 smd circle (at -5.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(U3-PadF3)"))
    (pad F4 smd circle (at -4.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(U3-PadF4)"))
    (pad G4 smd circle (at -4.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad G3 smd circle (at -5.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(U3-PadG3)"))
    (pad G2 smd circle (at -6.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad H2 smd circle (at -6.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(U3-PadH2)"))
    (pad H3 smd circle (at -5.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(U3-PadH3)"))
    (pad H4 smd circle (at -4.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(U3-PadH4)"))
    (pad J4 smd circle (at -4.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(U3-PadJ4)"))
    (pad J3 smd circle (at -5.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(U3-PadJ3)"))
    (pad J2 smd circle (at -6.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad K1 smd circle (at -7.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(U3-PadK1)"))
    (pad K2 smd circle (at -6.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(U3-PadK2)"))
    (pad K3 smd circle (at -5.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(U3-PadK3)"))
    (pad K4 smd circle (at -4.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad L4 smd circle (at -4.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(U3-PadL4)"))
    (pad L3 smd circle (at -5.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(U3-PadL3)"))
    (pad L2 smd circle (at -6.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad L1 smd circle (at -7.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(U3-PadL1)"))
    (pad M1 smd circle (at -7.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(U3-PadM1)"))
    (pad M2 smd circle (at -6.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(U3-PadM2)"))
    (pad M3 smd circle (at -5.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(U3-PadM3)"))
    (pad M4 smd circle (at -4.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(U3-PadM4)"))
    (pad N4 smd circle (at -4.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(U3-PadN4)"))
    (pad P4 smd circle (at -4.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(U3-PadP4)"))
    (pad R4 smd circle (at -4.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad R3 smd circle (at -5.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 456 /Control/~INIT~))
    (pad P3 smd circle (at -5.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad N3 smd circle (at -5.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(U3-PadN3)"))
    (pad N2 smd circle (at -6.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad P2 smd circle (at -6.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(U3-PadP2)"))
    (pad R2 smd circle (at -6.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(U3-PadR2)"))
    (pad N1 smd circle (at -7.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(U3-PadN1)"))
    (pad P1 smd circle (at -7.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(U3-PadP1)"))
    (pad R1 smd circle (at -7.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(U3-PadR1)"))
    (pad T1 smd circle (at -7.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad T2 smd circle (at -6.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 457 /Control/~PROG~))
    (pad T3 smd circle (at -5.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 509 "Net-(U3-PadT3)"))
    (pad T4 smd circle (at -4.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(U3-PadT4)"))
    (pad E8 smd circle (at -0.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(U3-PadE8)"))
    (pad E7 smd circle (at -1.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(U3-PadE7)"))
    (pad E6 smd circle (at -2.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(U3-PadE6)"))
    (pad E5 smd circle (at -3.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad F5 smd circle (at -3.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(U3-PadF5)"))
    (pad F6 smd circle (at -2.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(U3-PadF6)"))
    (pad F7 smd circle (at -1.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(U3-PadF7)"))
    (pad F8 smd circle (at -0.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad G5 smd circle (at -3.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(U3-PadG5)"))
    (pad G6 smd circle (at -2.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(U3-PadG6)"))
    (pad G7 smd circle (at -1.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 447 +1V2))
    (pad G8 smd circle (at -0.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad H5 smd circle (at -3.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(U3-PadH5)"))
    (pad H6 smd circle (at -2.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad H7 smd circle (at -1.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad H8 smd circle (at -0.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 447 +1V2))
    (pad J5 smd circle (at -3.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad J6 smd circle (at -2.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U3-PadJ6)"))
    (pad J7 smd circle (at -1.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 447 +1V2))
    (pad J8 smd circle (at -0.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad K5 smd circle (at -3.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(U3-PadK5)"))
    (pad K6 smd circle (at -2.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(U3-PadK6)"))
    (pad K7 smd circle (at -1.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad K8 smd circle (at -0.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 447 +1V2))
    (pad L5 smd circle (at -3.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(U3-PadL5)"))
    (pad L6 smd circle (at -2.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad L7 smd circle (at -1.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(U3-PadL7)"))
    (pad L8 smd circle (at -0.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(U3-PadL8)"))
    (pad M5 smd circle (at -3.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(U3-PadM5)"))
    (pad M6 smd circle (at -2.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 170 "Net-(U3-PadM6)"))
    (pad M7 smd circle (at -1.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(U3-PadM7)"))
    (pad P5 smd circle (at -3.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(U3-PadP5)"))
    (pad P6 smd circle (at -2.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(U3-PadP6)"))
    (pad R5 smd circle (at -3.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(U3-PadR5)"))
    (pad R6 smd circle (at -2.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad T5 smd circle (at -3.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(U3-PadT5)"))
    (pad T6 smd circle (at -2.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(U3-PadT6)"))
    (pad M8 smd circle (at -0.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad N5 smd circle (at -3.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(U3-PadN5)"))
    (pad N6 smd circle (at -2.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(U3-PadN6)"))
    (pad N7 smd circle (at -1.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad P11 smd circle (at 2.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(U3-PadP11)"))
    (pad P10 smd circle (at 1.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 510 /Control/MOSI_DIN))
    (pad P9 smd circle (at 0.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(U3-PadP9)"))
    (pad P8 smd circle (at -0.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(U3-PadP8)"))
    (pad P7 smd circle (at -1.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(U3-PadP7)"))
    (pad R7 smd circle (at -1.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 183 "Net-(U3-PadR7)"))
    (pad R8 smd circle (at -0.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad R9 smd circle (at 0.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 184 "Net-(U3-PadR9)"))
    (pad R10 smd circle (at 1.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad R11 smd circle (at 2.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 511 /Control/CCLK_SCK))
    (pad T7 smd circle (at -1.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 185 "Net-(U3-PadT7)"))
    (pad T8 smd circle (at -0.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(U3-PadT8)"))
    (pad T9 smd circle (at 0.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(U3-PadT9)"))
    (pad T10 smd circle (at 1.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 512 "Net-(U3-PadT10)"))
    (pad T11 smd circle (at 2.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 458 /Control/M0))
    (pad N8 smd circle (at -0.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 188 "Net-(U3-PadN8)"))
    (pad E9 smd circle (at 0.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad E10 smd circle (at 1.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(U3-PadE10)"))
    (pad E11 smd circle (at 2.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(U3-PadE11)"))
    (pad E12 smd circle (at 3.5 -3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 191 "Net-(U3-PadE12)"))
    (pad P12 smd circle (at 3.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 513 "Net-(U3-PadP12)"))
    (pad F9 smd circle (at 0.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 192 "Net-(U3-PadF9)"))
    (pad F10 smd circle (at 1.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 193 "Net-(U3-PadF10)"))
    (pad F11 smd circle (at 2.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad F12 smd circle (at 3.5 -2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 194 "Net-(U3-PadF12)"))
    (pad J9 smd circle (at 0.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 447 +1V2))
    (pad G12 smd circle (at 3.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(U3-PadG12)"))
    (pad G11 smd circle (at 2.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(U3-PadG11)"))
    (pad G10 smd circle (at 1.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad G9 smd circle (at 0.5 -1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 447 +1V2))
    (pad R12 smd circle (at 3.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 197 "Net-(U3-PadR12)"))
    (pad T12 smd circle (at 3.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 198 "Net-(U3-PadT12)"))
    (pad H9 smd circle (at 0.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad H10 smd circle (at 1.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 447 +1V2))
    (pad H11 smd circle (at 2.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 199 "Net-(U3-PadH11)"))
    (pad H12 smd circle (at 3.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad J10 smd circle (at 1.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad J11 smd circle (at 2.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 200 "Net-(U3-PadJ11)"))
    (pad J12 smd circle (at 3.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 201 "Net-(U3-PadJ12)"))
    (pad H13 smd circle (at 4.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 202 "Net-(U3-PadH13)"))
    (pad J13 smd circle (at 4.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 203 "Net-(U3-PadJ13)"))
    (pad K13 smd circle (at 4.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad L13 smd circle (at 4.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 204 "Net-(U3-PadL13)"))
    (pad M13 smd circle (at 4.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 205 "Net-(U3-PadM13)"))
    (pad N13 smd circle (at 4.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad P13 smd circle (at 4.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 459 /Control/DONE))
    (pad R13 smd circle (at 4.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad T13 smd circle (at 4.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 206 "Net-(U3-PadT13)"))
    (pad N9 smd circle (at 0.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 207 "Net-(U3-PadN9)"))
    (pad M9 smd circle (at 0.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 208 "Net-(U3-PadM9)"))
    (pad L9 smd circle (at 0.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad K9 smd circle (at 0.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad K10 smd circle (at 1.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 447 +1V2))
    (pad L10 smd circle (at 1.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 209 "Net-(U3-PadL10)"))
    (pad M10 smd circle (at 1.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 210 "Net-(U3-PadM10)"))
    (pad N10 smd circle (at 1.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad T14 smd circle (at 5.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 211 "Net-(U3-PadT14)"))
    (pad R14 smd circle (at 5.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 212 "Net-(U3-PadR14)"))
    (pad P14 smd circle (at 5.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 213 "Net-(U3-PadP14)"))
    (pad N14 smd circle (at 5.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 214 "Net-(U3-PadN14)"))
    (pad M14 smd circle (at 5.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 215 "Net-(U3-PadM14)"))
    (pad L14 smd circle (at 5.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 216 "Net-(U3-PadL14)"))
    (pad K14 smd circle (at 5.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 217 "Net-(U3-PadK14)"))
    (pad J14 smd circle (at 5.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 218 "Net-(U3-PadJ14)"))
    (pad H14 smd circle (at 5.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 219 "Net-(U3-PadH14)"))
    (pad H15 smd circle (at 6.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 220 "Net-(U3-PadH15)"))
    (pad J15 smd circle (at 6.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad K15 smd circle (at 6.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 221 "Net-(U3-PadK15)"))
    (pad L15 smd circle (at 6.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad M15 smd circle (at 6.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 222 "Net-(U3-PadM15)"))
    (pad N15 smd circle (at 6.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad P15 smd circle (at 6.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 223 "Net-(U3-PadP15)"))
    (pad R15 smd circle (at 6.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 224 "Net-(U3-PadR15)"))
    (pad T15 smd circle (at 6.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 225 "Net-(U3-PadT15)"))
    (pad N11 smd circle (at 2.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 460 /Control/M1))
    (pad M11 smd circle (at 2.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 226 "Net-(U3-PadM11)"))
    (pad L11 smd circle (at 2.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 227 "Net-(U3-PadL11)"))
    (pad K11 smd circle (at 2.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 228 "Net-(U3-PadK11)"))
    (pad K12 smd circle (at 3.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 229 "Net-(U3-PadK12)"))
    (pad L12 smd circle (at 3.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 230 "Net-(U3-PadL12)"))
    (pad M12 smd circle (at 3.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 231 "Net-(U3-PadM12)"))
    (pad N12 smd circle (at 3.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 514 "Net-(U3-PadN12)"))
    (pad T16 smd circle (at 7.5 7.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad R16 smd circle (at 7.5 6.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 232 "Net-(U3-PadR16)"))
    (pad P16 smd circle (at 7.5 5.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 233 "Net-(U3-PadP16)"))
    (pad N16 smd circle (at 7.5 4.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 234 "Net-(U3-PadN16)"))
    (pad M16 smd circle (at 7.5 3.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 235 "Net-(U3-PadM16)"))
    (pad L16 smd circle (at 7.5 2.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 236 "Net-(U3-PadL16)"))
    (pad K16 smd circle (at 7.5 1.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 237 "Net-(U3-PadK16)"))
    (pad J16 smd circle (at 7.5 0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 238 "Net-(U3-PadJ16)"))
    (pad H16 smd circle (at 7.5 -0.5 90) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 239 "Net-(U3-PadH16)"))
    (model ${KISYS3DMOD}/Package_BGA.3dshapes/BGA-256_17.0x17.0mm_Layout16x16_P1.0mm_Ball0.5mm_Pad0.4mm_NSMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AA5A66)
    (at 219.85 51.1 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 447 +1V2))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AA5A58)
    (at 219.85 49 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 447 +1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:PQFP-132_24x24mm_P0.635mm_MC68030 (layer F.Cu) (tedit 616BE190) (tstamp 61867E43)
    (at 207.5815 145.669 180)
    (descr "PQFP, 132 pins, 24mm sq body, 0.635mm pitch (https://www.intel.com/content/dam/www/public/us/en/documents/packaging-databooks/packaging-chapter-02-databook.pdf, http://www.nxp.com/docs/en/application-note/AN4388.pdf)")
    (tags "PQFP 132")
    (path /5F72F108/627CB7E6)
    (autoplace_cost180 5)
    (solder_mask_margin 0.03)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value MC68030FE (at 0 1.27) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start 12.12 -12.12) (end 12.12 -10.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 -12.12) (end 12.12 -12.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -11 -12) (end -12 -11) (layer F.Fab) (width 0.1))
    (fp_line (start -14.47 -14.47) (end -14.47 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.47 -14.47) (end -14.47 -14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start -11 -12) (end 12 -12) (layer F.Fab) (width 0.1))
    (fp_line (start 12 -12) (end 12 12) (layer F.Fab) (width 0.1))
    (fp_line (start 12 12) (end -12 12) (layer F.Fab) (width 0.1))
    (fp_line (start -12 12) (end -12 -11) (layer F.Fab) (width 0.1))
    (fp_line (start 14.47 -14.47) (end 14.47 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start 14.47 14.47) (end -14.47 14.47) (layer F.CrtYd) (width 0.05))
    (fp_line (start -10.6 -12.12) (end -12.12 -12.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -12.12 -12.12) (end -12.12 -10.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 10.6 12.12) (end 12.12 12.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.12 12.12) (end 12.12 10.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -12.12 12.12) (end -12.12 10.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -10.6 12.12) (end -12.12 12.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -14.1 -10.6) (end -12.12 -10.6) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 18 smd roundrect (at -13.4 -10.16 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 19 smd roundrect (at -13.4 -9.525 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 20 smd roundrect (at -13.4 -8.89 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 21 smd roundrect (at -13.4 -8.255 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /MC68k/A0))
    (pad 22 smd roundrect (at -13.4 -7.62 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /MC68k/A1))
    (pad 23 smd roundrect (at -13.4 -6.985 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /MC68k/A31))
    (pad 24 smd roundrect (at -13.4 -6.35 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /MC68k/A30))
    (pad 25 smd roundrect (at -13.4 -5.715 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 26 smd roundrect (at -13.4 -5.08 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /MC68k/A29))
    (pad 27 smd roundrect (at -13.4 -4.445 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /MC68k/A28))
    (pad 28 smd roundrect (at -13.4 -3.81 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /MC68k/A27))
    (pad 29 smd roundrect (at -13.4 -3.175 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /MC68k/A26))
    (pad 30 smd roundrect (at -13.4 -2.54 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 31 smd roundrect (at -13.4 -1.905 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /MC68k/A25))
    (pad 32 smd roundrect (at -13.4 -1.27 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /MC68k/A24))
    (pad 33 smd roundrect (at -13.4 -0.635 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /MC68k/A23))
    (pad 34 smd roundrect (at -13.4 0 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /MC68k/A22))
    (pad 35 smd roundrect (at -13.4 0.635 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 36 smd roundrect (at -13.4 1.27 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /MC68k/A21))
    (pad 37 smd roundrect (at -13.4 1.905 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /MC68k/A20))
    (pad 38 smd roundrect (at -13.4 2.54 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /MC68k/A19))
    (pad 39 smd roundrect (at -13.4 3.175 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /MC68k/A18))
    (pad 40 smd roundrect (at -13.4 3.81 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /MC68k/A17))
    (pad 41 smd roundrect (at -13.4 4.445 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /MC68k/A16))
    (pad 42 smd roundrect (at -13.4 5.08 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /MC68k/A15))
    (pad 43 smd roundrect (at -13.4 5.715 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /MC68k/A14))
    (pad 44 smd roundrect (at -13.4 6.35 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 45 smd roundrect (at -13.4 6.985 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /MC68k/A13))
    (pad 46 smd roundrect (at -13.4 7.62 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /MC68k/A12))
    (pad 47 smd roundrect (at -13.4 8.255 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /MC68k/A11))
    (pad 48 smd roundrect (at -13.4 8.89 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /MC68k/A10))
    (pad 49 smd roundrect (at -13.4 9.525 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 50 smd roundrect (at -13.4 10.16 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 84 smd roundrect (at 13.4 10.16 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 85 smd roundrect (at 13.4 9.525 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 86 smd roundrect (at 13.4 8.89 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 463 /CPUBuf/CPU_D8))
    (pad 87 smd roundrect (at 13.4 8.255 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 464 /CPUBuf/CPU_D9))
    (pad 88 smd roundrect (at 13.4 7.62 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 465 /CPUBuf/CPU_D10))
    (pad 89 smd roundrect (at 13.4 6.985 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 466 /CPUBuf/CPU_D11))
    (pad 90 smd roundrect (at 13.4 6.35 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 91 smd roundrect (at 13.4 5.715 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 467 /CPUBuf/CPU_D12))
    (pad 92 smd roundrect (at 13.4 5.08 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 468 /CPUBuf/CPU_D13))
    (pad 93 smd roundrect (at 13.4 4.445 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 469 /CPUBuf/CPU_D14))
    (pad 94 smd roundrect (at 13.4 3.81 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 470 /CPUBuf/CPU_D15))
    (pad 95 smd roundrect (at 13.4 3.175 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 96 smd roundrect (at 13.4 2.54 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 471 /CPUBuf/CPU_D16))
    (pad 97 smd roundrect (at 13.4 1.905 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 472 /CPUBuf/CPU_D17))
    (pad 98 smd roundrect (at 13.4 1.27 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 473 /CPUBuf/CPU_D18))
    (pad 99 smd roundrect (at 13.4 0.635 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 474 /CPUBuf/CPU_D19))
    (pad 100 smd roundrect (at 13.4 0 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 101 smd roundrect (at 13.4 -0.635 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 475 /CPUBuf/CPU_D20))
    (pad 102 smd roundrect (at 13.4 -1.27 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 476 /CPUBuf/CPU_D21))
    (pad 103 smd roundrect (at 13.4 -1.905 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 477 /CPUBuf/CPU_D22))
    (pad 104 smd roundrect (at 13.4 -2.54 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 478 /CPUBuf/CPU_D23))
    (pad 105 smd roundrect (at 13.4 -3.175 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 106 smd roundrect (at 13.4 -3.81 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 479 /CPUBuf/CPU_D24))
    (pad 107 smd roundrect (at 13.4 -4.445 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 480 /CPUBuf/CPU_D25))
    (pad 108 smd roundrect (at 13.4 -5.08 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 481 /CPUBuf/CPU_D26))
    (pad 109 smd roundrect (at 13.4 -5.715 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 482 /CPUBuf/CPU_D27))
    (pad 110 smd roundrect (at 13.4 -6.35 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 111 smd roundrect (at 13.4 -6.985 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 483 /CPUBuf/CPU_D28))
    (pad 112 smd roundrect (at 13.4 -7.62 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 484 /CPUBuf/CPU_D29))
    (pad 113 smd roundrect (at 13.4 -8.255 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 485 /CPUBuf/CPU_D30))
    (pad 114 smd roundrect (at 13.4 -8.89 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 486 /CPUBuf/CPU_D31))
    (pad 115 smd roundrect (at 13.4 -9.525 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 116 smd roundrect (at 13.4 -10.16 180) (size 1.635 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 51 smd roundrect (at -10.16 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /MC68k/A9))
    (pad 52 smd roundrect (at -9.525 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /MC68k/A8))
    (pad 53 smd roundrect (at -8.89 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /MC68k/A7))
    (pad 54 smd roundrect (at -8.255 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /MC68k/A6))
    (pad 55 smd roundrect (at -7.62 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /MC68k/A5))
    (pad 56 smd roundrect (at -6.985 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /MC68k/A4))
    (pad 57 smd roundrect (at -6.35 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 58 smd roundrect (at -5.715 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /MC68k/A3))
    (pad 59 smd roundrect (at -5.08 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /MC68k/A2))
    (pad 60 smd roundrect (at -4.445 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 61 smd roundrect (at -3.81 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 62 smd roundrect (at -3.175 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(U1-Pad62)"))
    (pad 63 smd roundrect (at -2.54 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 64 smd roundrect (at -1.905 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /PDSBuf/IOB_~RESET~))
    (pad 65 smd roundrect (at -1.27 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 66 smd roundrect (at -0.635 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 67 smd roundrect (at 0 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 68 smd roundrect (at 0.635 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /MC68k/~IPL~2))
    (pad 69 smd roundrect (at 1.27 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /MC68k/~IPL~1))
    (pad 70 smd roundrect (at 1.905 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /MC68k/~IPL~0))
    (pad 71 smd roundrect (at 2.54 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 72 smd roundrect (at 3.175 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 73 smd roundrect (at 3.81 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(U1-Pad73)"))
    (pad 74 smd roundrect (at 4.445 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(U1-Pad74)"))
    (pad 75 smd roundrect (at 5.08 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 487 /CPUBuf/CPU_D0))
    (pad 76 smd roundrect (at 5.715 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 488 /CPUBuf/CPU_D1))
    (pad 77 smd roundrect (at 6.35 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 78 smd roundrect (at 6.985 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 489 /CPUBuf/CPU_D2))
    (pad 79 smd roundrect (at 7.62 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 490 /CPUBuf/CPU_D3))
    (pad 80 smd roundrect (at 8.255 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 491 /CPUBuf/CPU_D4))
    (pad 81 smd roundrect (at 8.89 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 492 /CPUBuf/CPU_D5))
    (pad 82 smd roundrect (at 9.525 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 493 /CPUBuf/CPU_D6))
    (pad 83 smd roundrect (at 10.16 13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 494 /CPUBuf/CPU_D7))
    (pad 117 smd roundrect (at 10.16 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 495 /CPUBuf/CPU_R~W~))
    (pad 118 smd roundrect (at 9.525 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 496 /CPUBuf/CPU_~ECS~))
    (pad 119 smd roundrect (at 8.89 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 497 /CPUBuf/CPU_SIZ1))
    (pad 120 smd roundrect (at 8.255 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 498 /CPUBuf/CPU_SIZ0))
    (pad 121 smd roundrect (at 7.62 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(U1-Pad121)"))
    (pad 122 smd roundrect (at 6.985 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /Control/CPU_~CIIN~))
    (pad 123 smd roundrect (at 6.35 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 124 smd roundrect (at 5.715 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 499 /CPUBuf/CPU_~DS~))
    (pad 125 smd roundrect (at 5.08 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 500 /CPUBuf/CPU_~AS~))
    (pad 126 smd roundrect (at 4.445 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 501 /CPUBuf/CPU_~CBREQ~))
    (pad 127 smd roundrect (at 3.81 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /Control/CPU_~CBACK~))
    (pad 128 smd roundrect (at 3.175 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 129 smd roundrect (at 2.54 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /Control/CPU_~HALT~))
    (pad 130 smd roundrect (at 1.905 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /Control/CPU_~BERR~))
    (pad 131 smd roundrect (at 1.27 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /Control/CPU_~STERM~))
    (pad 132 smd roundrect (at 0.635 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 502 /CPUBuf/CPU_~DSACK~1))
    (pad 1 smd roundrect (at 0 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at -0.635 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 3 smd roundrect (at -1.27 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 503 /CPUBuf/CPU_~DSACK~0))
    (pad 4 smd roundrect (at -1.905 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 5 smd roundrect (at -2.54 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at -3.175 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /Control/CPUCLK))
    (pad 7 smd roundrect (at -3.81 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 8 smd roundrect (at -4.445 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 9 smd roundrect (at -5.08 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 504 /CPUBuf/CPU_FC2))
    (pad 10 smd roundrect (at -5.715 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 505 /CPUBuf/CPU_FC1))
    (pad 11 smd roundrect (at -6.35 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 12 smd roundrect (at -6.985 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 506 /CPUBuf/CPU_FC0))
    (pad 13 smd roundrect (at -7.62 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 507 /CPUBuf/CPU_~RMC~))
    (pad 14 smd roundrect (at -8.255 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(U1-Pad14)"))
    (pad 15 smd roundrect (at -8.89 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 508 /CPUBuf/CPU_~CIOUT~))
    (pad 16 smd roundrect (at -9.525 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(U1-Pad16)"))
    (pad 17 smd roundrect (at -10.16 -13.4 180) (size 0.4 1.635) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/PQFP-132_24x24mm_P0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSOP-II-54_22.2x10.16mm_P0.8mm (layer F.Cu) (tedit 616CEBAA) (tstamp 61736EA1)
    (at 218.55 74.9 180)
    (descr "54-lead TSOP typ II package")
    (tags "TSOPII TSOP2")
    (path /63261D60/6327223F)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.03)
    (attr smd)
    (fp_text reference U5 (at 0 0) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value W9825G6KH-6 (at 0 0.95) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -4.08 -11.11) (end 5.08 -11.11) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 -11.11) (end 5.08 11.11) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 11.11) (end -5.08 11.11) (layer F.Fab) (width 0.1))
    (fp_line (start -5.08 11.11) (end -5.08 -10.11) (layer F.Fab) (width 0.1))
    (fp_line (start -4.08 -11.11) (end -5.08 -10.11) (layer F.Fab) (width 0.1))
    (fp_line (start -6.5 -10.9) (end -5.3 -10.9) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.3 -10.9) (end -5.3 -11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.3 -11.3) (end 5.3 -11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.3 11.3) (end 5.3 11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.3 -11.3) (end 5.3 -10.9) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.3 10.9) (end 5.3 11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.3 10.9) (end -5.3 11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.76 -11.36) (end 6.76 -11.36) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.76 -11.36) (end 6.76 11.36) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.76 11.36) (end -6.76 11.36) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.76 -11.36) (end -6.76 11.36) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -5.75 -10.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at -5.75 -9.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 279 /RAM/D16))
    (pad 3 smd roundrect (at -5.75 -8.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 4 smd roundrect (at -5.75 -8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 280 /RAM/D17))
    (pad 5 smd roundrect (at -5.75 -7.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 281 /RAM/D18))
    (pad 6 smd roundrect (at -5.75 -6.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 7 smd roundrect (at -5.75 -5.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 282 /RAM/D19))
    (pad 8 smd roundrect (at -5.75 -4.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 283 /RAM/D20))
    (pad 9 smd roundrect (at -5.75 -4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 10 smd roundrect (at -5.75 -3.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 284 /RAM/D21))
    (pad 11 smd roundrect (at -5.75 -2.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 285 /RAM/D22))
    (pad 12 smd roundrect (at -5.75 -1.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 13 smd roundrect (at -5.75 -0.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 286 /RAM/D23))
    (pad 14 smd roundrect (at -5.75 0 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 15 smd roundrect (at -5.75 0.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 287 /RAM/DQM2))
    (pad 16 smd roundrect (at -5.75 1.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 269 /Control/RAM_~WE~))
    (pad 17 smd roundrect (at -5.75 2.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 268 /Control/RAM_~CAS~))
    (pad 18 smd roundrect (at -5.75 3.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 267 /Control/RAM_~RAS~))
    (pad 19 smd roundrect (at -5.75 4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 266 /Control/RAM_~CS~))
    (pad 20 smd roundrect (at -5.75 4.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 265 /RAM/BA0))
    (pad 21 smd roundrect (at -5.75 5.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 264 /RAM/BA1))
    (pad 22 smd roundrect (at -5.75 6.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 263 /RAM/RA10))
    (pad 23 smd roundrect (at -5.75 7.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 262 /RAM/RA0))
    (pad 24 smd roundrect (at -5.75 8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 261 /RAM/RA1))
    (pad 25 smd roundrect (at -5.75 8.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 260 /RAM/RA2))
    (pad 26 smd roundrect (at -5.75 9.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 259 /RAM/RA3))
    (pad 27 smd roundrect (at -5.75 10.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 28 smd roundrect (at 5.75 10.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 29 smd roundrect (at 5.75 9.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 258 /RAM/RA4))
    (pad 30 smd roundrect (at 5.75 8.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 257 /RAM/RA5))
    (pad 31 smd roundrect (at 5.75 8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 256 /RAM/RA6))
    (pad 32 smd roundrect (at 5.75 7.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 255 /RAM/RA7))
    (pad 33 smd roundrect (at 5.75 6.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 254 /RAM/RA8))
    (pad 34 smd roundrect (at 5.75 5.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 253 /RAM/RA9))
    (pad 35 smd roundrect (at 5.75 4.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 252 /RAM/RA11))
    (pad 36 smd roundrect (at 5.75 4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 251 /RAM/RA12))
    (pad 37 smd roundrect (at 5.75 3.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 250 /RAM/CKE))
    (pad 38 smd roundrect (at 5.75 2.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 288 /RAM/CLK23))
    (pad 39 smd roundrect (at 5.75 1.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 289 /RAM/DQM3))
    (pad 40 smd roundrect (at 5.75 0.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 41 smd roundrect (at 5.75 0 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 42 smd roundrect (at 5.75 -0.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 290 /RAM/D24))
    (pad 43 smd roundrect (at 5.75 -1.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 44 smd roundrect (at 5.75 -2.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 291 /RAM/D25))
    (pad 45 smd roundrect (at 5.75 -3.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 292 /RAM/D26))
    (pad 46 smd roundrect (at 5.75 -4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 47 smd roundrect (at 5.75 -4.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 293 /RAM/D27))
    (pad 48 smd roundrect (at 5.75 -5.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 294 /RAM/D28))
    (pad 49 smd roundrect (at 5.75 -6.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 50 smd roundrect (at 5.75 -7.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 295 /RAM/D29))
    (pad 51 smd roundrect (at 5.75 -8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 296 /RAM/D30))
    (pad 52 smd roundrect (at 5.75 -8.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 53 smd roundrect (at 5.75 -9.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 297 /RAM/D31))
    (pad 54 smd roundrect (at 5.75 -10.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-II-54_22.2x10.16mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:R_0603 (layer F.Cu) (tedit 617287CD) (tstamp 619A2E13)
    (at 194.05 45 180)
    (tags resistor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value R_0603 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.8 0 180) (size 0.7 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /Control/CPUCLK))
    (pad 1 smd roundrect (at -0.8 0 180) (size 0.7 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /Control/CPUCLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:R_0603 (layer F.Cu) (tedit 617287D0) (tstamp 619A2E43)
    (at 194.05 43.5 180)
    (tags resistor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value R_0603 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.8 0 180) (size 0.7 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /Control/FPUCLK))
    (pad 2 smd roundrect (at 0.8 0 180) (size 0.7 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /Control/FPUCLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AE5030)
    (at 197.35 44.05 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 61ABC93F)
    (at 231.35 104.225 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/6372B95C)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U22 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHCT573PW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 502 /CPUBuf/CPU_~DSACK~1))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 503 /CPUBuf/CPU_~DSACK~0))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 374 "Net-(U22-Pad17)"))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 373 "Net-(U22-Pad16)"))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 372 "Net-(U22-Pad15)"))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 371 "Net-(U22-Pad14)"))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 370 "Net-(U22-Pad13)"))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 369 "Net-(U22-Pad12)"))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 368 "Net-(U22-Pad9)"))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 367 "Net-(U22-Pad8)"))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 366 "Net-(U22-Pad7)"))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 365 "Net-(U22-Pad6)"))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 364 "Net-(U22-Pad5)"))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 363 "Net-(U22-Pad4)"))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 362 /Control/CPU_~DSACK~0))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 361 /Control/CPU_~DSACK~1))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 552 /CPUBuf/DSACK~OE~))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61ABC931)
    (at 233.8 100 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC31C6)
    (at 202.6 38.8)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC321A)
    (at 217.85 38.8)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC3244)
    (at 199.35 38.8)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC319C)
    (at 214.6 38.8)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC30A0)
    (at 219.85 40.8 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC2C32)
    (at 219.85 59.3 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC32EC)
    (at 219.85 56.05 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC2BDE)
    (at 219.85 44.05 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC30CA)
    (at 217.75 61.3 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 6178EECF)
    (at 209.65 61.3)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 447 +1V2))
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC311E)
    (at 199.45 61.3 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 6178EEA5)
    (at 207.55 61.3 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 447 +1V2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61795B84)
    (at 203.35 61.3 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AC326E)
    (at 213.55 61.3)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AE5084)
    (at 197.35 40.8 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AE505A)
    (at 197.35 59.4 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 61AE4FB2)
    (at 197.35 56.05 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer F.Cu) (tedit 5F326081) (tstamp 61AC3042)
    (at 229.2 54.85 90)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (path /5F723173/63C6B24E)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference U6 (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_text value 50M (at 0 0.75 90) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -1.6 -1.25) (end -1.6 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 1.25) (end 1.6 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 1.25) (end 1.6 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start 1.6 -1.25) (end -1.6 -1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.6 0.25) (end -0.6 1.25) (layer F.Fab) (width 0.1))
    (fp_line (start -2.15 -0.85) (end -2.15 1.75) (layer F.SilkS) (width 0.1524))
    (fp_line (start -2.15 1.75) (end 1.1 1.75) (layer F.SilkS) (width 0.1524))
    (fp_line (start -2.1 -1.7) (end -2.1 1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.1 1.7) (end 2.1 1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.1 1.7) (end 2.1 -1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.1 -1.7) (end -2.1 -1.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 -2.25 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 4 smd roundrect (at -1.1 -0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 448 "Net-(U6-Pad4)"))
    (pad 3 smd roundrect (at 1.1 -0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 449 "Net-(U6-Pad3)"))
    (pad 2 smd roundrect (at 1.1 0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 450 "Net-(U6-Pad2)"))
    (pad 1 smd roundrect (at -1.1 0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 451 "Net-(U6-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:SOIC-16_3.9mm (layer F.Cu) (tedit 5FDA018C) (tstamp 61AB1A60)
    (at 251.3965 55.5625 270)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference REF** (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value SOIC-16_3.9mm (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -5.2 -3.7) (end -5.2 3.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.2 -3.7) (end -5.2 -3.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.2 3.7) (end 5.2 -3.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.2 3.7) (end 5.2 3.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.975 1.95) (end -4.95 0.975) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 1.95) (end -3.975 1.95) (layer F.Fab) (width 0.1))
    (fp_line (start 4.95 -1.95) (end 4.95 1.95) (layer F.Fab) (width 0.1))
    (fp_line (start -4.95 -1.95) (end 4.95 -1.95) (layer F.Fab) (width 0.1))
    (fp_line (start -4.95 0.975) (end -4.95 -1.95) (layer F.Fab) (width 0.1))
    (fp_line (start -5.06 0) (end -5.06 3.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.06 0) (end -5.06 -1.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.06 0) (end 5.06 1.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.06 0) (end 5.06 -1.95) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 270) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -4.445 2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.175 2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -1.905 2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -0.635 2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at 0.635 2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at 1.905 2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 3.175 2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at 4.445 2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 4.445 -2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 3.175 -2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 1.905 -2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at 0.635 -2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at -0.635 -2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 14 smd roundrect (at -1.905 -2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at -3.175 -2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 16 smd roundrect (at -4.445 -2.475) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:USB_Micro-B_ShouHan_MicroXNJ (layer F.Cu) (tedit 602BA043) (tstamp 61AC0867)
    (at 232.75 30 90)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference REF** (at -0.45 0) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value USB_Micro-B_ShouHan_MicroXNJ (at -4.4 0) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start -2.4225 1.1) (end -2.2125 1.1) (layer F.Fab) (width 0.1))
    (fp_line (start -2.4225 1.5) (end -2.2125 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.4225 1.5) (end -2.4225 1.1) (layer F.Fab) (width 0.1))
    (fp_line (start -2.2125 1.1) (end -2.0125 1.3) (layer F.Fab) (width 0.1))
    (fp_line (start -2.0125 1.3) (end -2.2125 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.6125 1.7) (end -2.1625 1.7) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6125 1.7) (end -2.6125 1.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6125 -3.9) (end -2.6125 -3.45) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.25 -3.9) (end -2.6125 -3.9) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 3.9) (end 1.9875 3.9) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.989204 3.75) (end -2.4625 3.75) (layer F.Fab) (width 0.1))
    (fp_line (start -2.4625 3.75) (end -2.4625 -3.75) (layer F.Fab) (width 0.1))
    (fp_line (start 2.989204 3.75) (end 2.989204 -3.75) (layer F.Fab) (width 0.1))
    (fp_line (start 2.6 3) (end 2.6 -3) (layer F.Fab) (width 0.1))
    (fp_line (start 2.989204 -3.75) (end -2.4625 -3.75) (layer F.Fab) (width 0.1))
    (fp_line (start 2.35 -3.9) (end 1.9875 -3.9) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.25 3.9) (end -2.6125 3.9) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.6125 3.9) (end -2.6125 3.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.24 4.4) (end -2.86 4.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.86 4.4) (end -2.86 -4.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.86 -4.4) (end 3.24 -4.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.24 4.4) (end 3.24 -4.4) (layer F.CrtYd) (width 0.05))
    (fp_text user "PCB Edge" (at 2.05 0) (layer Dwgs.User)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (fp_text user %R (at -3.5 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 6 smd roundrect (at 0.875 -0.8 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 thru_hole circle (at -1.8 2.425 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 smd roundrect (at -1.775 0.65 180) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (solder_mask_margin 0.04) (solder_paste_margin -0.05))
    (pad 1 smd roundrect (at -1.775 1.3 180) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (solder_mask_margin 0.04) (solder_paste_margin -0.05))
    (pad 5 smd roundrect (at -1.775 -1.3 180) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (solder_mask_margin 0.04) (solder_paste_margin -0.05))
    (pad 4 smd roundrect (at -1.775 -0.65 180) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (solder_mask_margin 0.04) (solder_paste_margin -0.05))
    (pad 3 smd roundrect (at -1.775 0 180) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (solder_mask_margin 0.04) (solder_paste_margin -0.05))
    (pad 6 thru_hole circle (at -1.8 -2.425 180) (size 1.3 1.3) (drill 0.7) (layers *.Cu *.Mask))
    (pad 6 smd roundrect (at 0.875 0.8 180) (size 0.6 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 thru_hole oval (at 0.85 3.6) (size 1.07 1.9) (drill oval 0.5 1.3) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0.85 -3.6 180) (size 1.07 1.9) (drill oval 0.5 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (offset (xyz -0.6 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:DIN41612_R_3x32_Male_Vertical_THT (layer B.Cu) (tedit 5EAFCB80) (tstamp 61882B84)
    (at 268.432 73.872 180)
    (descr "DIN41612 connector, type R, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
    (tags "DIN 41612 IEC 60603 R")
    (fp_text reference REF** (at 2.54 9.13) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value DIN41612_R_3x32_Male_Vertical_THT (at 2.54 -87.87) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -1.81 3.13) (end 4.39 3.13) (layer B.Fab) (width 0.1))
    (fp_line (start 4.39 3.13) (end 4.39 2.13) (layer B.Fab) (width 0.1))
    (fp_line (start 4.39 2.13) (end 6.89 2.13) (layer B.Fab) (width 0.1))
    (fp_line (start 6.89 2.13) (end 6.89 -80.87) (layer B.Fab) (width 0.1))
    (fp_line (start 6.89 -80.87) (end 4.39 -80.87) (layer B.Fab) (width 0.1))
    (fp_line (start 4.39 -80.87) (end 4.39 -81.87) (layer B.Fab) (width 0.1))
    (fp_line (start 4.39 -81.87) (end -1.81 -81.87) (layer B.Fab) (width 0.1))
    (fp_line (start -1.81 -81.87) (end -1.81 3.13) (layer B.Fab) (width 0.1))
    (fp_line (start -3.01 -83.37) (end -0.76 -83.37) (layer B.Fab) (width 0.1))
    (fp_line (start -0.76 -83.37) (end -0.76 -81.87) (layer B.Fab) (width 0.1))
    (fp_line (start 4.39 -81.87) (end 5.24 -81.87) (layer B.Fab) (width 0.1))
    (fp_line (start 5.24 -81.87) (end 5.24 -83.37) (layer B.Fab) (width 0.1))
    (fp_line (start 5.24 -83.37) (end 8.09 -83.37) (layer B.Fab) (width 0.1))
    (fp_line (start -3.01 4.63) (end -0.76 4.63) (layer B.Fab) (width 0.1))
    (fp_line (start -0.76 4.63) (end -0.76 3.13) (layer B.Fab) (width 0.1))
    (fp_line (start 4.39 3.13) (end 5.24 3.13) (layer B.Fab) (width 0.1))
    (fp_line (start 5.24 3.13) (end 5.24 4.63) (layer B.Fab) (width 0.1))
    (fp_line (start 5.24 4.63) (end 8.09 4.63) (layer B.Fab) (width 0.1))
    (fp_line (start -3.01 8.13) (end 8.09 8.13) (layer B.Fab) (width 0.1))
    (fp_line (start 8.09 8.13) (end 8.09 -86.87) (layer B.Fab) (width 0.1))
    (fp_line (start 8.09 -86.87) (end -3.01 -86.87) (layer B.Fab) (width 0.1))
    (fp_line (start -3.01 -86.87) (end -3.01 8.13) (layer B.Fab) (width 0.1))
    (fp_line (start -3.12 8.24) (end 8.2 8.24) (layer B.SilkS) (width 0.12))
    (fp_line (start 8.2 8.24) (end 8.2 -86.98) (layer B.SilkS) (width 0.12))
    (fp_line (start 8.2 -86.98) (end -3.12 -86.98) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.12 -86.98) (end -3.12 8.24) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.5 8.63) (end 8.59 8.63) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.59 8.63) (end 8.59 -87.37) (layer B.CrtYd) (width 0.05))
    (fp_line (start 8.59 -87.37) (end -3.5 -87.37) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.5 -87.37) (end -3.5 8.63) (layer B.CrtYd) (width 0.05))
    (fp_line (start -3.31 0) (end -3.99 0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.99 0.3) (end -3.99 -0.3) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.99 -0.3) (end -3.31 0) (layer B.SilkS) (width 0.12))
    (fp_line (start -3.01 0.5) (end -2.31 0) (layer B.Fab) (width 0.1))
    (fp_line (start -2.31 0) (end -3.01 -0.5) (layer B.Fab) (width 0.1))
    (fp_line (start -1.81 3.131) (end 4.39 3.131) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.39 3.131) (end 4.39 2.131) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.39 2.131) (end 6.89 2.131) (layer B.SilkS) (width 0.12))
    (fp_line (start 6.89 2.131) (end 6.89 -80.87) (layer B.SilkS) (width 0.12))
    (fp_line (start 6.89 -80.87) (end 4.39 -80.87) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.39 -80.87) (end 4.39 -81.87) (layer B.SilkS) (width 0.12))
    (fp_line (start 4.39 -81.87) (end -1.81 -81.87) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.81 -81.87) (end -1.81 3.131) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 2.54 -39.37) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (pad "" np_thru_hole circle (at 2.24 -84.37 180) (size 2.85 2.85) (drill 2.85) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.24 5.63 180) (size 2.85 2.85) (drill 2.85) (layers *.Cu *.Mask))
    (pad C32 thru_hole circle (at 5.08 -78.74 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C31 thru_hole circle (at 5.08 -76.2 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C30 thru_hole circle (at 5.08 -73.66 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C29 thru_hole circle (at 5.08 -71.12 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C28 thru_hole circle (at 5.08 -68.58 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C27 thru_hole circle (at 5.08 -66.04 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C26 thru_hole circle (at 5.08 -63.5 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C25 thru_hole circle (at 5.08 -60.96 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C24 thru_hole circle (at 5.08 -58.42 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C23 thru_hole circle (at 5.08 -55.88 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C22 thru_hole circle (at 5.08 -53.34 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C21 thru_hole circle (at 5.08 -50.8 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C20 thru_hole circle (at 5.08 -48.26 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C19 thru_hole circle (at 5.08 -45.72 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C18 thru_hole circle (at 5.08 -43.18 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C17 thru_hole circle (at 5.08 -40.64 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C16 thru_hole circle (at 5.08 -38.1 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C15 thru_hole circle (at 5.08 -35.56 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C14 thru_hole circle (at 5.08 -33.02 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C13 thru_hole circle (at 5.08 -30.48 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C12 thru_hole circle (at 5.08 -27.94 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C11 thru_hole circle (at 5.08 -25.4 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C10 thru_hole circle (at 5.08 -22.86 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C9 thru_hole circle (at 5.08 -20.32 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C8 thru_hole circle (at 5.08 -17.78 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C7 thru_hole circle (at 5.08 -15.24 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C6 thru_hole circle (at 5.08 -12.7 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C5 thru_hole circle (at 5.08 -10.16 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C4 thru_hole circle (at 5.08 -7.62 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C3 thru_hole circle (at 5.08 -5.08 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C2 thru_hole circle (at 5.08 -2.54 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad C1 thru_hole circle (at 5.08 0 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B32 thru_hole circle (at 2.54 -78.74 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B31 thru_hole circle (at 2.54 -76.2 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B30 thru_hole circle (at 2.54 -73.66 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B29 thru_hole circle (at 2.54 -71.12 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B28 thru_hole circle (at 2.54 -68.58 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B27 thru_hole circle (at 2.54 -66.04 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B26 thru_hole circle (at 2.54 -63.5 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B25 thru_hole circle (at 2.54 -60.96 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B24 thru_hole circle (at 2.54 -58.42 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B23 thru_hole circle (at 2.54 -55.88 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B22 thru_hole circle (at 2.54 -53.34 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B21 thru_hole circle (at 2.54 -50.8 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B20 thru_hole circle (at 2.54 -48.26 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B19 thru_hole circle (at 2.54 -45.72 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B18 thru_hole circle (at 2.54 -43.18 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B17 thru_hole circle (at 2.54 -40.64 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B16 thru_hole circle (at 2.54 -38.1 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B15 thru_hole circle (at 2.54 -35.56 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B14 thru_hole circle (at 2.54 -33.02 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B13 thru_hole circle (at 2.54 -30.48 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B12 thru_hole circle (at 2.54 -27.94 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B11 thru_hole circle (at 2.54 -25.4 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B10 thru_hole circle (at 2.54 -22.86 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B9 thru_hole circle (at 2.54 -20.32 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B8 thru_hole circle (at 2.54 -17.78 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B7 thru_hole circle (at 2.54 -15.24 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B6 thru_hole circle (at 2.54 -12.7 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B5 thru_hole circle (at 2.54 -10.16 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B4 thru_hole circle (at 2.54 -7.62 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B3 thru_hole circle (at 2.54 -5.08 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B2 thru_hole circle (at 2.54 -2.54 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad B1 thru_hole circle (at 2.54 0 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A32 thru_hole circle (at 0 -78.74 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A31 thru_hole circle (at 0 -76.2 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A30 thru_hole circle (at 0 -73.66 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A29 thru_hole circle (at 0 -71.12 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A28 thru_hole circle (at 0 -68.58 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A27 thru_hole circle (at 0 -66.04 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A26 thru_hole circle (at 0 -63.5 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A25 thru_hole circle (at 0 -60.96 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A24 thru_hole circle (at 0 -58.42 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A23 thru_hole circle (at 0 -55.88 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A22 thru_hole circle (at 0 -53.34 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A21 thru_hole circle (at 0 -50.8 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A20 thru_hole circle (at 0 -48.26 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A19 thru_hole circle (at 0 -45.72 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A18 thru_hole circle (at 0 -43.18 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A17 thru_hole circle (at 0 -40.64 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A16 thru_hole circle (at 0 -38.1 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A15 thru_hole circle (at 0 -35.56 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A14 thru_hole circle (at 0 -33.02 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A13 thru_hole circle (at 0 -30.48 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A12 thru_hole circle (at 0 -27.94 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A11 thru_hole circle (at 0 -25.4 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A10 thru_hole circle (at 0 -22.86 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A9 thru_hole circle (at 0 -20.32 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A8 thru_hole circle (at 0 -17.78 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A7 thru_hole circle (at 0 -15.24 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A6 thru_hole circle (at 0 -12.7 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A5 thru_hole circle (at 0 -10.16 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A4 thru_hole circle (at 0 -7.62 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A3 thru_hole circle (at 0 -5.08 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A2 thru_hole circle (at 0 -2.54 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask))
    (pad A1 thru_hole roundrect (at 0 0 180) (size 1.55 1.55) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.16129))
    (model ${KISYS3DMOD}/Connector_DIN.3dshapes/DIN41612_R_3x32_Male_Vertical_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:Xunpu_TF-115_microSD (layer F.Cu) (tedit 606CA97D) (tstamp 61A9D25C)
    (at 265.6 56.55)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at -2.55 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value Xunpu_TF-115_microSD (at -1.65 0 90) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -8.25 7.6) (end 6.15 7.6) (layer F.SilkS) (width 0.127))
    (fp_line (start 5.45 -0.9) (end 5.45 7.4) (layer F.Fab) (width 0.127))
    (fp_line (start 6.45 -4.6) (end 5.45 -0.9) (layer F.Fab) (width 0.127))
    (fp_line (start 6.45 -7.35) (end 6.45 -4.6) (layer F.Fab) (width 0.127))
    (fp_line (start -8.05 -7.35) (end 6.45 -7.35) (layer F.Fab) (width 0.127))
    (fp_line (start -8.05 7.4) (end -8.05 -7.35) (layer F.Fab) (width 0.127))
    (fp_line (start -8.25 7.6) (end -8.25 -7.55) (layer F.SilkS) (width 0.127))
    (fp_line (start -8.25 -7.55) (end 6.15 -7.55) (layer F.SilkS) (width 0.127))
    (fp_line (start -8.05 7.4) (end 5.45 7.4) (layer F.Fab) (width 0.127))
    (fp_line (start -8.85 8.55) (end 6.9 8.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.9 8.55) (end 6.9 -8.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.85 -8.55) (end 6.9 -8.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -8.85 -8.55) (end -8.85 8.55) (layer F.CrtYd) (width 0.05))
    (pad 10 smd roundrect (at 2.75 7.75 90) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at -6.85 7.8 90) (size 1.2 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -7.85 6.6 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at -6.85 -6.85 90) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 2.75 -7.75 90) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -7.85 -2.2 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -7.85 -1.1 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -7.85 0 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -7.85 1.1 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -7.85 2.2 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -7.85 3.3 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -7.85 4.4 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -7.85 5.5 90) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad "" np_thru_hole circle (at 3.15 4.95 90) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.15 -3.05 90) (size 1 1) (drill 1) (layers *.Cu *.Mask))
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 6182787D)
    (at 209.9 88.35 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSOP-II-54_22.2x10.16mm_P0.8mm (layer F.Cu) (tedit 616CEBAA) (tstamp 61736BBB)
    (at 200.85 74.9 180)
    (descr "54-lead TSOP typ II package")
    (tags "TSOPII TSOP2")
    (path /63261D60/6326A531)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.03)
    (attr smd)
    (fp_text reference U4 (at 0 0) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value W9825G6KH-6 (at 0 0.95) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -6.76 -11.36) (end -6.76 11.36) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.76 11.36) (end -6.76 11.36) (layer F.CrtYd) (width 0.05))
    (fp_line (start 6.76 -11.36) (end 6.76 11.36) (layer F.CrtYd) (width 0.05))
    (fp_line (start -6.76 -11.36) (end 6.76 -11.36) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.3 10.9) (end -5.3 11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.3 10.9) (end 5.3 11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.3 -11.3) (end 5.3 -10.9) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.3 11.3) (end 5.3 11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.3 -11.3) (end 5.3 -11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.3 -10.9) (end -5.3 -11.3) (layer F.SilkS) (width 0.12))
    (fp_line (start -6.5 -10.9) (end -5.3 -10.9) (layer F.SilkS) (width 0.12))
    (fp_line (start -4.08 -11.11) (end -5.08 -10.11) (layer F.Fab) (width 0.1))
    (fp_line (start -5.08 11.11) (end -5.08 -10.11) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 11.11) (end -5.08 11.11) (layer F.Fab) (width 0.1))
    (fp_line (start 5.08 -11.11) (end 5.08 11.11) (layer F.Fab) (width 0.1))
    (fp_line (start -4.08 -11.11) (end 5.08 -11.11) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 54 smd roundrect (at 5.75 -10.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 53 smd roundrect (at 5.75 -9.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 240 /RAM/D15))
    (pad 52 smd roundrect (at 5.75 -8.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 51 smd roundrect (at 5.75 -8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 241 /RAM/D14))
    (pad 50 smd roundrect (at 5.75 -7.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 242 /RAM/D13))
    (pad 49 smd roundrect (at 5.75 -6.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 48 smd roundrect (at 5.75 -5.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 243 /RAM/D12))
    (pad 47 smd roundrect (at 5.75 -4.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 244 /RAM/D11))
    (pad 46 smd roundrect (at 5.75 -4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 45 smd roundrect (at 5.75 -3.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 245 /RAM/D10))
    (pad 44 smd roundrect (at 5.75 -2.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 246 /RAM/D9))
    (pad 43 smd roundrect (at 5.75 -1.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 42 smd roundrect (at 5.75 -0.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 247 /RAM/D8))
    (pad 41 smd roundrect (at 5.75 0 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 40 smd roundrect (at 5.75 0.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 39 smd roundrect (at 5.75 1.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 248 /RAM/DQM1))
    (pad 38 smd roundrect (at 5.75 2.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 249 /RAM/CLK01))
    (pad 37 smd roundrect (at 5.75 3.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 250 /RAM/CKE))
    (pad 36 smd roundrect (at 5.75 4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 251 /RAM/RA12))
    (pad 35 smd roundrect (at 5.75 4.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 252 /RAM/RA11))
    (pad 34 smd roundrect (at 5.75 5.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 253 /RAM/RA9))
    (pad 33 smd roundrect (at 5.75 6.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 254 /RAM/RA8))
    (pad 32 smd roundrect (at 5.75 7.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 255 /RAM/RA7))
    (pad 31 smd roundrect (at 5.75 8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 256 /RAM/RA6))
    (pad 30 smd roundrect (at 5.75 8.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 257 /RAM/RA5))
    (pad 29 smd roundrect (at 5.75 9.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 258 /RAM/RA4))
    (pad 28 smd roundrect (at 5.75 10.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 27 smd roundrect (at -5.75 10.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 26 smd roundrect (at -5.75 9.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 259 /RAM/RA3))
    (pad 25 smd roundrect (at -5.75 8.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 260 /RAM/RA2))
    (pad 24 smd roundrect (at -5.75 8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 261 /RAM/RA1))
    (pad 23 smd roundrect (at -5.75 7.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 262 /RAM/RA0))
    (pad 22 smd roundrect (at -5.75 6.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 263 /RAM/RA10))
    (pad 21 smd roundrect (at -5.75 5.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 264 /RAM/BA1))
    (pad 20 smd roundrect (at -5.75 4.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 265 /RAM/BA0))
    (pad 19 smd roundrect (at -5.75 4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 266 /Control/RAM_~CS~))
    (pad 18 smd roundrect (at -5.75 3.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 267 /Control/RAM_~RAS~))
    (pad 17 smd roundrect (at -5.75 2.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 268 /Control/RAM_~CAS~))
    (pad 16 smd roundrect (at -5.75 1.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 269 /Control/RAM_~WE~))
    (pad 15 smd roundrect (at -5.75 0.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 270 /RAM/DQM0))
    (pad 14 smd roundrect (at -5.75 0 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 13 smd roundrect (at -5.75 -0.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 271 /RAM/D7))
    (pad 12 smd roundrect (at -5.75 -1.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at -5.75 -2.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 272 /RAM/D6))
    (pad 10 smd roundrect (at -5.75 -3.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 273 /RAM/D5))
    (pad 9 smd roundrect (at -5.75 -4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 8 smd roundrect (at -5.75 -4.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 274 /RAM/D4))
    (pad 7 smd roundrect (at -5.75 -5.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 275 /RAM/D3))
    (pad 6 smd roundrect (at -5.75 -6.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 5 smd roundrect (at -5.75 -7.2 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 276 /RAM/D2))
    (pad 4 smd roundrect (at -5.75 -8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 277 /RAM/D1))
    (pad 3 smd roundrect (at -5.75 -8.8 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at -5.75 -9.6 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 278 /RAM/D0))
    (pad 1 smd roundrect (at -5.75 -10.4 180) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-II-54_22.2x10.16mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 6188EED4)
    (at 222.975 90.8)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/63262F0F)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U28 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHC245APW (at 0 1.016 180) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 19 smd roundrect (at -2.275 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 445 /Control/CPU_D~OE~))
    (pad 18 smd roundrect (at -1.625 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 290 /RAM/D24))
    (pad 17 smd roundrect (at -0.975 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 291 /RAM/D25))
    (pad 16 smd roundrect (at -0.325 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 292 /RAM/D26))
    (pad 15 smd roundrect (at 0.325 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 293 /RAM/D27))
    (pad 14 smd roundrect (at 0.975 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 294 /RAM/D28))
    (pad 13 smd roundrect (at 1.625 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 295 /RAM/D29))
    (pad 12 smd roundrect (at 2.275 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 296 /RAM/D30))
    (pad 11 smd roundrect (at 2.925 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 297 /RAM/D31))
    (pad 10 smd roundrect (at 2.925 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 486 /CPUBuf/CPU_D31))
    (pad 8 smd roundrect (at 1.625 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 485 /CPUBuf/CPU_D30))
    (pad 7 smd roundrect (at 0.975 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 484 /CPUBuf/CPU_D29))
    (pad 6 smd roundrect (at 0.325 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 483 /CPUBuf/CPU_D28))
    (pad 5 smd roundrect (at -0.325 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 482 /CPUBuf/CPU_D27))
    (pad 4 smd roundrect (at -0.975 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 481 /CPUBuf/CPU_D26))
    (pad 3 smd roundrect (at -1.625 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 480 /CPUBuf/CPU_D25))
    (pad 2 smd roundrect (at -2.275 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 479 /CPUBuf/CPU_D24))
    (pad 1 smd roundrect (at -2.925 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 446 /Control/CPU_DDIR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618DDCA1)
    (at 226.2 85.8 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618DDC93)
    (at 226.2 65 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618DDC85)
    (at 226.2 75.7 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618DDC77)
    (at 226.2 83.2 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618DDC69)
    (at 226.2 79.4 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618A2E3B)
    (at 193.2 77 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618A2E2D)
    (at 193.2 81.8 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618A1429)
    (at 210.9 81.8 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618A13E3)
    (at 210.9 77 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 618F11FE)
    (at 208.5 65 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 6189FEEB)
    (at 208.5 75.7 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 6189FEDD)
    (at 208.5 85.8 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 6189FE85)
    (at 208.5 79.4 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616CEBED) (tstamp 6189FE77)
    (at 208.5 83.2 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61891CD1)
    (at 206.8115 130.302)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 61882E22)
    (at 255.2 75.575 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/622CABC7)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U17 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHC245APW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 396 /PDSBuf/D~OE~))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 429 /PDS/D24))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 430 /PDS/D25))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 431 /PDS/D26))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 432 /PDS/D27))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 433 /PDS/D28))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 434 /PDS/D29))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 435 /PDS/D30))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 436 /PDS/D31))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 437 /PDSBuf/IOC_D31))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 438 /PDSBuf/IOC_D30))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 439 /PDSBuf/IOC_D29))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 440 /PDSBuf/IOC_D28))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 441 /PDSBuf/IOC_D27))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 442 /PDSBuf/IOC_D26))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 443 /PDSBuf/IOC_D25))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 444 /PDSBuf/IOC_D24))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 379 /PDSBuf/DDIR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61882E14)
    (at 257.65 71.35 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 6188172E)
    (at 231.35 132.225 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/629FA6C8)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U21 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74LVC244 (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /MC68k/A24))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 550 /CPUBuf/FSB_A28))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /MC68k/A25))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 551 /CPUBuf/FSB_A29))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /MC68k/A26))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 519 /CPUBuf/FSB_A30))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /MC68k/A27))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 520 /CPUBuf/FSB_A31))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /MC68k/A31))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 515 /CPUBuf/FSB_A24))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /MC68k/A30))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 516 /CPUBuf/FSB_A25))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /MC68k/A29))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 517 /CPUBuf/FSB_A26))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /MC68k/A28))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 518 /CPUBuf/FSB_A27))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61881720)
    (at 233.8 137 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61881712)
    (at 233.8 146 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61881704)
    (at 233.8 155 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 618816F6)
    (at 233.8 128 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 618816D3)
    (at 231.35 141.225 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/629F220F)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U20 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74LVC244 (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 526 /CPUBuf/FSB_A19))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /MC68k/A20))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 527 /CPUBuf/FSB_A18))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /MC68k/A21))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 528 /CPUBuf/FSB_A17))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /MC68k/A22))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 529 /CPUBuf/FSB_A16))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /MC68k/A23))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 522 /CPUBuf/FSB_A23))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /MC68k/A19))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 523 /CPUBuf/FSB_A22))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /MC68k/A18))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 524 /CPUBuf/FSB_A21))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /MC68k/A17))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 525 /CPUBuf/FSB_A20))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /MC68k/A16))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 618816B0)
    (at 231.35 150.225 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/629E6572)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U19 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74LVC244 (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /MC68k/A8))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 534 /CPUBuf/FSB_A12))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /MC68k/A9))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 535 /CPUBuf/FSB_A13))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /MC68k/A10))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 536 /CPUBuf/FSB_A14))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /MC68k/A11))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 537 /CPUBuf/FSB_A15))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /MC68k/A15))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 530 /CPUBuf/FSB_A8))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /MC68k/A14))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 531 /CPUBuf/FSB_A9))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /MC68k/A13))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 532 /CPUBuf/FSB_A10))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /MC68k/A12))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 533 /CPUBuf/FSB_A11))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 6188168D)
    (at 231.35 159.225 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/629FEFBA)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U18 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74LVC244 (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 546 /CPUBuf/FSB_A3))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /MC68k/A4))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 547 /CPUBuf/FSB_A2))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /MC68k/A5))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 548 /CPUBuf/FSB_A1))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /MC68k/A6))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 549 /CPUBuf/FSB_A0))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /MC68k/A7))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 544 /CPUBuf/FSB_A7))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /MC68k/A3))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 543 /CPUBuf/FSB_A6))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /MC68k/A2))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 542 /CPUBuf/FSB_A5))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /MC68k/A1))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 541 /CPUBuf/FSB_A4))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /MC68k/A0))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 6188167F)
    (at 233.8 119 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 61ABC89D)
    (at 231.35 114.225 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/62A2CF45)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U24 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74LVC244APW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 507 /CPUBuf/CPU_~RMC~))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 538 /CPUBuf/FSB_FC0))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 495 /CPUBuf/CPU_R~W~))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 376 "Net-(U24-Pad5)"))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 504 /CPUBuf/CPU_FC2))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 377 "Net-(U24-Pad7)"))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 505 /CPUBuf/CPU_FC1))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 378 "Net-(U24-Pad9)"))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 560 /CPUBuf/FSB_~RMC~))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 521 /CPUBuf/FSB_R~W~))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 540 /CPUBuf/FSB_FC2))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 506 /CPUBuf/CPU_FC0))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 539 /CPUBuf/FSB_FC1))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 545 /CPUBuf/A~OE~))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61ABC8F1)
    (at 233.8 110 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 61ABC7FA)
    (at 231.35 123.225 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/62A56F1A)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U23 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74LVC244APW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 500 /CPUBuf/CPU_~AS~))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 553 /CPUBuf/FSB_~CIOUT~))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 501 /CPUBuf/CPU_~CBREQ~))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 554 /CPUBuf/FSB_SIZ0))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 499 /CPUBuf/CPU_~DS~))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 555 /CPUBuf/FSB_SIZ1))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 496 /CPUBuf/CPU_~ECS~))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 375 "Net-(U23-Pad9)"))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 556 /CPUBuf/FSB_~AS~))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 497 /CPUBuf/CPU_SIZ1))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 557 /CPUBuf/FSB_~CBREQ~))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 498 /CPUBuf/CPU_SIZ0))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 558 /CPUBuf/FSB_~DS~))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 508 /CPUBuf/CPU_~CIOUT~))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 559 /CPUBuf/FSB_~ECS~))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61871312)
    (at 196.9215 130.302 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 618712BE)
    (at 224.2185 123.452 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61871294)
    (at 218.8925 97.282 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61871240)
    (at 208.0815 97.282)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61871081)
    (at 205.8115 97.282 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 617C1B28)
    (at 197.731 97.282)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867D0F)
    (at 209.804 161.036)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867CE5)
    (at 212.5345 161.036)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867CBB)
    (at 204.9065 161.036)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867C91)
    (at 192.2145 156.0115 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867C67)
    (at 210.6215 130.302)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867D8D)
    (at 203.9065 130.302 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867D63)
    (at 192.2145 149.344 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867D39)
    (at 192.2145 135.644 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867C3D)
    (at 222.9485 155.5115 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867F85)
    (at 222.9485 148.709 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 616BDDCB) (tstamp 61867FAF)
    (at 223.012 135.644 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:ESP32-WROOM-32 (layer F.Cu) (tedit 601CCBE5) (tstamp 61ABAACE)
    (at 258.953 28.575)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value ESP32-WROOM-32 (at 0 1.5) (layer F.Fab) hide
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_line (start -11.55 20.55) (end -11.55 -10.05) (layer F.CrtYd) (width 0.12))
    (fp_line (start 11.55 20.55) (end -11.55 20.55) (layer F.CrtYd) (width 0.12))
    (fp_line (start 11.55 -10.05) (end 11.55 20.55) (layer F.CrtYd) (width 0.12))
    (fp_line (start -11.55 -10.05) (end 11.55 -10.05) (layer F.CrtYd) (width 0.12))
    (fp_line (start 9.1 18.11) (end 6.4 18.11) (layer F.SilkS) (width 0.2032))
    (fp_line (start 9 -7.49) (end -9 -7.49) (layer F.Fab) (width 0.05))
    (fp_line (start 9 18.01) (end 9 -7.49) (layer F.Fab) (width 0.05))
    (fp_line (start -9 18.01) (end 9 18.01) (layer F.Fab) (width 0.05))
    (fp_line (start -9 -7.49) (end -9 18.01) (layer F.Fab) (width 0.05))
    (fp_line (start -9.1 -1.14) (end 9.1 -1.14) (layer F.SilkS) (width 0.2032))
    (fp_line (start -9.1 18.11) (end -9.1 17.19) (layer F.SilkS) (width 0.2032))
    (fp_line (start -9.1 -0.65) (end -9.1 -7.49) (layer F.SilkS) (width 0.2032))
    (fp_line (start 9.1 -0.65) (end 9.1 -7.49) (layer F.SilkS) (width 0.2032))
    (fp_line (start -9 -1.14) (end 9 -1.14) (layer F.Fab) (width 0.05))
    (fp_line (start 9.1 18.11) (end 9.1 17.19) (layer F.SilkS) (width 0.2032))
    (fp_line (start -6.4 18.11) (end -9.1 18.11) (layer F.SilkS) (width 0.2032))
    (fp_text user %R (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 39 smd rect (at -1 7.53) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 39 smd rect (at 1.159 7.53) (size 0.5 3) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 39 smd rect (at -1 9.562) (size 3 0.5) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 39 smd rect (at -3.032 7.53) (size 0.5 3) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 39 smd rect (at -1 5.498) (size 3 0.5) (layers F.Cu F.Paste F.Mask)
      (zone_connect 2))
    (pad 39 thru_hole circle (at -1 6.403) (size 0.8 0.8) (drill 0.3) (layers *.Cu F.Mask)
      (zone_connect 2))
    (pad 39 thru_hole circle (at -1 8.657) (size 0.8 0.8) (drill 0.3) (layers *.Cu F.Mask)
      (zone_connect 2))
    (pad 39 thru_hole circle (at 0.127 8.657) (size 0.8 0.8) (drill 0.3) (layers *.Cu F.Mask)
      (zone_connect 2))
    (pad 39 thru_hole circle (at 0.127 7.53) (size 0.8 0.8) (drill 0.3) (layers *.Cu F.Mask)
      (zone_connect 2))
    (pad 39 thru_hole circle (at 0.127 6.403) (size 0.8 0.8) (drill 0.3) (layers *.Cu F.Mask)
      (zone_connect 2))
    (pad 39 thru_hole circle (at -2.127 6.403) (size 0.8 0.8) (drill 0.3) (layers *.Cu F.Mask)
      (zone_connect 2))
    (pad 39 thru_hole circle (at -2.127 7.53) (size 0.8 0.8) (drill 0.3) (layers *.Cu F.Mask)
      (zone_connect 2))
    (pad 39 thru_hole circle (at -2.127 8.657) (size 0.8 0.8) (drill 0.3) (layers *.Cu F.Mask)
      (zone_connect 2))
    (pad 39 smd rect (at -1 7.53) (size 5 5) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 1 smd oval (at -8.75 0) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd oval (at -8.75 1.27) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd oval (at -8.75 2.54) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd oval (at -8.75 3.81) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd oval (at -8.75 5.08) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd oval (at -8.75 6.35) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd oval (at -8.75 7.62) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd oval (at -8.75 8.89) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd oval (at -8.75 10.16) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd oval (at -8.75 11.43) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd oval (at -8.75 12.7) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd oval (at -8.75 13.97) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd oval (at -8.75 15.24) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd oval (at -8.75 16.51) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd oval (at 8.75 16.51) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd oval (at 8.75 15.24) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd oval (at 8.75 13.97) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd oval (at 8.75 12.7) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd oval (at 8.75 11.43) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd oval (at 8.75 10.16) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd oval (at 8.75 8.89) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd oval (at 8.75 7.62) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd oval (at 8.75 6.35) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd oval (at 8.75 5.08) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd oval (at 8.75 3.81) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd oval (at 8.75 2.54) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd oval (at 8.75 1.27) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd oval (at 8.75 0) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd oval (at -0.635 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd oval (at -1.905 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd oval (at -3.175 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd oval (at -4.445 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd oval (at -5.715 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd oval (at 0.635 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd oval (at 1.905 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd oval (at 3.175 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd oval (at 4.445 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd oval (at 5.715 17.79 90) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP32-WROOM-32.wrl
      (offset (xyz 0 -8.210000000000001 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 6188EF84)
    (at 214.125 90.8)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/63262F0C)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U27 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHC245APW (at 0 1.016 180) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 446 /Control/CPU_DDIR))
    (pad 2 smd roundrect (at -2.275 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 471 /CPUBuf/CPU_D16))
    (pad 3 smd roundrect (at -1.625 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 472 /CPUBuf/CPU_D17))
    (pad 4 smd roundrect (at -0.975 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 473 /CPUBuf/CPU_D18))
    (pad 5 smd roundrect (at -0.325 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 474 /CPUBuf/CPU_D19))
    (pad 6 smd roundrect (at 0.325 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 475 /CPUBuf/CPU_D20))
    (pad 7 smd roundrect (at 0.975 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 476 /CPUBuf/CPU_D21))
    (pad 8 smd roundrect (at 1.625 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 478 /CPUBuf/CPU_D23))
    (pad 9 smd roundrect (at 2.275 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 477 /CPUBuf/CPU_D22))
    (pad 10 smd roundrect (at 2.925 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 285 /RAM/D22))
    (pad 12 smd roundrect (at 2.275 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 286 /RAM/D23))
    (pad 13 smd roundrect (at 1.625 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 284 /RAM/D21))
    (pad 14 smd roundrect (at 0.975 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 283 /RAM/D20))
    (pad 15 smd roundrect (at 0.325 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 282 /RAM/D19))
    (pad 16 smd roundrect (at -0.325 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 281 /RAM/D18))
    (pad 17 smd roundrect (at -0.975 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 280 /RAM/D17))
    (pad 18 smd roundrect (at -1.625 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 279 /RAM/D16))
    (pad 19 smd roundrect (at -2.275 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 445 /Control/CPU_D~OE~))
    (pad 20 smd roundrect (at -2.925 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61827853)
    (at 218.75 88.35 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 6188F23C)
    (at 205.275 90.8)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/622AE852)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U26 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHC245APW (at 0 1.016 180) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 446 /Control/CPU_DDIR))
    (pad 2 smd roundrect (at -2.275 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 464 /CPUBuf/CPU_D9))
    (pad 3 smd roundrect (at -1.625 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 463 /CPUBuf/CPU_D8))
    (pad 4 smd roundrect (at -0.975 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 465 /CPUBuf/CPU_D10))
    (pad 5 smd roundrect (at -0.325 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 466 /CPUBuf/CPU_D11))
    (pad 6 smd roundrect (at 0.325 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 467 /CPUBuf/CPU_D12))
    (pad 7 smd roundrect (at 0.975 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 468 /CPUBuf/CPU_D13))
    (pad 8 smd roundrect (at 1.625 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 469 /CPUBuf/CPU_D14))
    (pad 9 smd roundrect (at 2.275 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 470 /CPUBuf/CPU_D15))
    (pad 10 smd roundrect (at 2.925 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 240 /RAM/D15))
    (pad 12 smd roundrect (at 2.275 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 241 /RAM/D14))
    (pad 13 smd roundrect (at 1.625 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 242 /RAM/D13))
    (pad 14 smd roundrect (at 0.975 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 243 /RAM/D12))
    (pad 15 smd roundrect (at 0.325 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 244 /RAM/D11))
    (pad 16 smd roundrect (at -0.325 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 245 /RAM/D10))
    (pad 17 smd roundrect (at -0.975 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 247 /RAM/D8))
    (pad 18 smd roundrect (at -1.625 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 246 /RAM/D9))
    (pad 19 smd roundrect (at -2.275 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 445 /Control/CPU_D~OE~))
    (pad 20 smd roundrect (at -2.925 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 618279A3)
    (at 201.05 88.35 270)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 270) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 6188F2EC)
    (at 196.425 90.8)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /629B918A/6226E539)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U25 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHC245APW (at 0 1.016 180) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 19 smd roundrect (at -2.275 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 445 /Control/CPU_D~OE~))
    (pad 18 smd roundrect (at -1.625 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 274 /RAM/D4))
    (pad 17 smd roundrect (at -0.975 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 273 /RAM/D5))
    (pad 16 smd roundrect (at -0.325 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 275 /RAM/D3))
    (pad 15 smd roundrect (at 0.325 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 272 /RAM/D6))
    (pad 14 smd roundrect (at 0.975 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 276 /RAM/D2))
    (pad 13 smd roundrect (at 1.625 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 271 /RAM/D7))
    (pad 12 smd roundrect (at 2.275 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 277 /RAM/D1))
    (pad 11 smd roundrect (at 2.925 -2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 278 /RAM/D0))
    (pad 10 smd roundrect (at 2.925 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 487 /CPUBuf/CPU_D0))
    (pad 8 smd roundrect (at 1.625 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 488 /CPUBuf/CPU_D1))
    (pad 7 smd roundrect (at 0.975 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 494 /CPUBuf/CPU_D7))
    (pad 6 smd roundrect (at 0.325 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 489 /CPUBuf/CPU_D2))
    (pad 5 smd roundrect (at -0.325 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 493 /CPUBuf/CPU_D6))
    (pad 4 smd roundrect (at -0.975 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 490 /CPUBuf/CPU_D3))
    (pad 3 smd roundrect (at -1.625 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 492 /CPUBuf/CPU_D5))
    (pad 2 smd roundrect (at -2.275 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 491 /CPUBuf/CPU_D4))
    (pad 1 smd roundrect (at -2.925 2.95 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 446 /Control/CPU_DDIR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61A01B2E)
    (at 193.2 85.6 90)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4 90) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 61815AF6)
    (at 255.2 119.825 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/60941F85)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U12 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHCT573PW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 340 /PDS/A7))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 341 /PDS/A6))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 342 /PDS/A5))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 343 /PDS/A4))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 344 /PDSBuf/IOB_~RMC~))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 345 /PDSBuf/IOB_FC2))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 346 /PDSBuf/IOB_FC1))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 347 /PDSBuf/IOB_FC0))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 315 /PDSBuf/ADoutLE))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 538 /CPUBuf/FSB_FC0))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 539 /CPUBuf/FSB_FC1))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 540 /CPUBuf/FSB_FC2))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 541 /CPUBuf/FSB_A4))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 542 /CPUBuf/FSB_A5))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 543 /CPUBuf/FSB_A6))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 544 /CPUBuf/FSB_A7))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 314 /PDSBuf/A~OE~))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61815AE8)
    (at 257.65 115.6 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 61815A3F)
    (at 255.2 110.975 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/62A8E938)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U13 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74LVC244APW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 348 /Control/IOB_~DSACK~0))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 349 /PDSBuf/IOB_~DSACK~1))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 350 /Control/IOB_~HALT~))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 351 /PDS/C16M))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 352 /Control/IOB_~BERR~))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 353 /PDSBuf/FSB_~RESET~))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 354 "Net-(U13-Pad9)"))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 355 /PDSBuf/IOB_~DSACK~0))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 356 "Net-(U13-Pad7)"))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 357 /PDSBuf/IOB_~HALT~))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 358 /Control/IOB_C16M))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 359 /PDSBuf/IOB_~BERR~))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 360 /Control/IOB_~DSACK~1))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /PDSBuf/IOB_~RESET~))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61815A31)
    (at 257.65 106.75 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 6188298A)
    (at 255.2 102.125 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/63262F04)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U14 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHC245APW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 379 /PDSBuf/DDIR))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 380 /PDSBuf/IOC_D0))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 381 /PDSBuf/IOC_D1))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 382 /PDSBuf/IOC_D2))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 383 /PDSBuf/IOC_D3))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 384 /PDSBuf/IOC_D4))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 385 /PDSBuf/IOC_D5))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 386 /PDSBuf/IOC_D6))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 387 /PDSBuf/IOC_D7))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 388 /PDS/D7))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 389 /PDS/D6))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 390 /PDS/D5))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 391 /PDS/D4))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 392 /PDS/D3))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 393 /PDS/D2))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 394 /PDS/D1))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 395 /PDS/D0))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 396 /PDSBuf/D~OE~))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61815A00)
    (at 257.65 97.9 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 6181596C)
    (at 257.65 89.05 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 61882870)
    (at 255.2 93.275 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/63262F09)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U15 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHC245APW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 379 /PDSBuf/DDIR))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 397 /PDSBuf/IOC_D8))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 398 /PDSBuf/IOC_D9))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 399 /PDSBuf/IOC_D10))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 400 /PDSBuf/IOC_D11))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 401 /PDSBuf/IOC_D12))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 402 /PDSBuf/IOC_D13))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 403 /PDSBuf/IOC_D14))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 404 /PDSBuf/IOC_D15))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 405 /PDS/D15))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 406 /PDS/D14))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 407 /PDS/D13))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 408 /PDS/D12))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 409 /PDS/D11))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 410 /PDS/D10))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 411 /PDS/D9))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 412 /PDS/D8))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 396 /PDSBuf/D~OE~))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 618828FD)
    (at 255.2 84.425 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/622CABB5)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U16 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHC245APW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 396 /PDSBuf/D~OE~))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 413 /PDS/D16))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 414 /PDS/D17))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 415 /PDS/D18))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 416 /PDS/D19))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 417 /PDS/D20))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 418 /PDS/D21))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 419 /PDS/D22))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 420 /PDS/D23))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 421 /PDSBuf/IOC_D23))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 422 /PDSBuf/IOC_D22))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 423 /PDSBuf/IOC_D21))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 424 /PDSBuf/IOC_D20))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 425 /PDSBuf/IOC_D19))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 426 /PDSBuf/IOC_D18))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 427 /PDSBuf/IOC_D17))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 428 /PDSBuf/IOC_D16))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 379 /PDSBuf/DDIR))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61815918)
    (at 257.65 80.2 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61815884)
    (at 257.65 133.3 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 61822CBA)
    (at 255.2 128.675 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/6094447D)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U11 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHCT573PW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 339 /PDS/A15))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 338 /PDS/A14))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 337 /PDS/A13))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 336 /PDS/A12))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 335 /PDS/A11))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 334 /PDS/A10))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 333 /PDS/A9))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 332 /PDS/A8))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 315 /PDSBuf/ADoutLE))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 530 /CPUBuf/FSB_A8))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 531 /CPUBuf/FSB_A9))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 532 /CPUBuf/FSB_A10))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 533 /CPUBuf/FSB_A11))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 534 /CPUBuf/FSB_A12))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 535 /CPUBuf/FSB_A13))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 536 /CPUBuf/FSB_A14))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 537 /CPUBuf/FSB_A15))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 314 /PDSBuf/A~OE~))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 6181583E)
    (at 255.2 137.525 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/61398C8D)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U10 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHCT573PW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 314 /PDSBuf/A~OE~))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 522 /CPUBuf/FSB_A23))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 523 /CPUBuf/FSB_A22))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 524 /CPUBuf/FSB_A21))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 525 /CPUBuf/FSB_A20))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 526 /CPUBuf/FSB_A19))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 527 /CPUBuf/FSB_A18))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 528 /CPUBuf/FSB_A17))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 529 /CPUBuf/FSB_A16))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 315 /PDSBuf/ADoutLE))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 324 /PDS/A16))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 325 /PDS/A17))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 326 /PDS/A18))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 327 /PDS/A19))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 328 /PDS/A20))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 329 /PDS/A21))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 330 /PDS/A22))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 331 /PDS/A23))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61815830)
    (at 257.65 124.45 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 618157F9)
    (at 257.65 151 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0402 (layer F.Cu) (tedit 5EE29C3C) (tstamp 61814E9B)
    (at 257.65 142.15 180)
    (tags capacitor)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.05)
    (attr smd)
    (fp_text reference REF** (at 0 0) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_text value C_0402 (at 0 0.4) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.5 0.25) (end -0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -0.5 -0.25) (end 0.5 -0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 -0.25) (end 0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start 0.5 0.25) (end -0.5 0.25) (layer F.Fab) (width 0.05))
    (fp_line (start -1 0.5) (end -1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1 -0.5) (end 1 -0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 -0.5) (end 1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1 0.5) (end -1 0.5) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (pad 1 smd roundrect (at -0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.5 0 180) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 6181573F)
    (at 255.2 146.375 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/61DF380D)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U9 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHCT573PW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 323 "Net-(U9-Pad19)"))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 322 /PDSBuf/IOB_R~W~))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 321 /PDS/A31))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 320 /PDS/A30))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 319 /PDS/A27))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 318 /PDS/A26))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 317 /PDS/A25))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 316 /PDS/A24))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 315 /PDSBuf/ADoutLE))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 515 /CPUBuf/FSB_A24))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 516 /CPUBuf/FSB_A25))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 517 /CPUBuf/FSB_A26))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 518 /CPUBuf/FSB_A27))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 519 /CPUBuf/FSB_A30))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 520 /CPUBuf/FSB_A31))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 521 /CPUBuf/FSB_R~W~))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 314 /PDSBuf/A~OE~))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:TSSOP-20_4.4x6.5mm_P0.65mm (layer F.Cu) (tedit 5F27C9F6) (tstamp 61724302)
    (at 255.2 155.225 270)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (path /60941922/61ED1513)
    (solder_mask_margin 0.024)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U8 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (fp_text value 74AHCT573PW (at 0 1.016 270) (layer F.Fab)
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_line (start -3.45 3.75) (end -3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.45 2.225) (end 3.45 -2.225) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.55 3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end -3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 -3.95) (end 3.55 -3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.55 3.95) (end 3.55 3.95) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 2.2) (end -3.25 1.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 2.2) (end -2.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start 3.25 -2.2) (end 3.25 2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 -2.2) (end 3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_line (start -3.25 1.2) (end -3.25 -2.2) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 90) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 1 smd roundrect (at -2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 314 /PDSBuf/A~OE~))
    (pad 2 smd roundrect (at -2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 313 /PDSBuf/IOC_SIZ1))
    (pad 3 smd roundrect (at -1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 312 /PDSBuf/IOC_SIZ0))
    (pad 4 smd roundrect (at -0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 311 /PDSBuf/IOC_A3))
    (pad 5 smd roundrect (at -0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 310 /PDSBuf/IOC_A2))
    (pad 6 smd roundrect (at 0.325 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 309 /PDSBuf/IOC_A1))
    (pad 7 smd roundrect (at 0.975 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 308 /PDSBuf/IOC_A0))
    (pad 8 smd roundrect (at 1.625 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 307 /Control/IOC_~AS~))
    (pad 9 smd roundrect (at 2.275 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 306 /Control/IOC_~DS~))
    (pad 10 smd roundrect (at 2.925 2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 11 smd roundrect (at 2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 12 smd roundrect (at 2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 305 /PDSBuf/IOB_~DS~))
    (pad 13 smd roundrect (at 1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 304 /PDSBuf/IOB_~AS~))
    (pad 14 smd roundrect (at 0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 303 /PDS/A0))
    (pad 15 smd roundrect (at 0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 302 /PDS/A1))
    (pad 16 smd roundrect (at -0.325 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 301 /PDS/A2))
    (pad 17 smd roundrect (at -0.975 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 300 /PDS/A3))
    (pad 18 smd roundrect (at -1.625 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 299 /PDSBuf/IOB_SIZ0))
    (pad 19 smd roundrect (at -2.275 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 298 /PDSBuf/IOB_SIZ1))
    (pad 20 smd roundrect (at -2.925 -2.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9AEB5)
    (at 118.396001 184.020501)
    (tags capacitor)
    (path /5F6DA71D/616DE7E8)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C4 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9AE85)
    (at 118.396001 187.070501)
    (tags capacitor)
    (path /5F6DA71D/616DE7D1)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C5 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9AE55)
    (at 122.846001 184.020501)
    (tags capacitor)
    (path /5F6DA71D/616DE7BE)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C6 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 452 -5V))
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 616FF043)
    (at 118.396001 190.120501)
    (tags capacitor)
    (path /5F6DA71D/616DE7F4)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C7 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 452 -5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9AE25)
    (at 122.846001 187.070501)
    (tags capacitor)
    (path /5F6DA71D/616DE7DB)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C8 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 453 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9ADF5)
    (at 127.296001 184.020501)
    (tags capacitor)
    (path /5F6DA71D/616DE7C5)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C9 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 453 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 616FF076)
    (at 122.846001 190.120501)
    (tags capacitor)
    (path /5F6DA71D/616F27B1)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C10 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 454 -12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9ADC5)
    (at 127.296001 187.070501)
    (tags capacitor)
    (path /5F6DA71D/616F27A7)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C11 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 454 -12V))
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9AD95)
    (at 156.806001 183.010501)
    (tags capacitor)
    (path /5F72F108/6161ACA7)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C12 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9AD65)
    (at 156.806001 186.060501)
    (tags capacitor)
    (path /5F72F108/6161ACA0)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C13 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9AD35)
    (at 161.256001 183.010501)
    (tags capacitor)
    (path /5F72F108/613F0B6D)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C14 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0805 (layer F.Cu) (tedit 5F02840E) (tstamp 61B9AD05)
    (at 161.256001 186.060501)
    (tags capacitor)
    (path /5F72F108/613F0B66)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.025)
    (attr smd)
    (fp_text reference C15 (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 10u (at 0 0.35) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_line (start 1.7 1) (end -1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.7 -1) (end 1.7 1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 -1) (end 1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.7 1) (end -1.7 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.4064 0.8) (end 0.4064 0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start -0.4064 -0.8) (end 0.4064 -0.8) (layer F.SilkS) (width 0.1524))
    (fp_line (start 1 0.625) (end -1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer F.Fab) (width 0.15))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0 180) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.85 0) (size 1.05 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B4EE)
    (at 130.046001 170.420501)
    (tags capacitor)
    (path /60941922/63262F00)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C16 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B4BE)
    (at 125.796001 172.870501)
    (tags capacitor)
    (path /60941922/63262EF8)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C17 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B1BE)
    (at 121.946001 176.520501)
    (tags capacitor)
    (path /60941922/63262EFC)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C18 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B18E)
    (at 126.196001 170.420501)
    (tags capacitor)
    (path /60941922/63262EF4)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C19 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B15E)
    (at 121.946001 174.070501)
    (tags capacitor)
    (path /60941922/63262EFD)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C20 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B12E)
    (at 118.096001 174.070501)
    (tags capacitor)
    (path /60941922/63262EF5)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C21 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B24E)
    (at 129.646001 175.320501)
    (tags capacitor)
    (path /60941922/63262EFE)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C22 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B21E)
    (at 125.796001 177.770501)
    (tags capacitor)
    (path /60941922/63262EF6)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C23 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B1EE)
    (at 129.646001 172.870501)
    (tags capacitor)
    (path /60941922/61D73237)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C24 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B48E)
    (at 125.796001 175.320501)
    (tags capacitor)
    (path /60941922/63262EFA)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C25 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B45E)
    (at 118.096001 176.520501)
    (tags capacitor)
    (path /60941922/63262F01)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C26 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B42E)
    (at 122.346001 170.420501)
    (tags capacitor)
    (path /60941922/63262EF9)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C27 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B3FE)
    (at 158.926001 175.320501)
    (tags capacitor)
    (path /5F723173/616131FC)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C28 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B3CE)
    (at 162.776001 172.870501)
    (tags capacitor)
    (path /5F723173/616131D5)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C29 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B39E)
    (at 158.926001 170.420501)
    (tags capacitor)
    (path /5F723173/616131E1)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C30 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B36E)
    (at 162.776001 175.320501)
    (tags capacitor)
    (path /5F723173/616131EB)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C31 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B0FE)
    (at 166.626001 170.420501)
    (tags capacitor)
    (path /5F723173/6161320E)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C32 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B0CE)
    (at 162.776001 170.420501)
    (tags capacitor)
    (path /5F723173/61613208)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C33 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B09E)
    (at 158.926001 172.870501)
    (tags capacitor)
    (path /5F723173/616151AF)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C34 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B06E)
    (at 137.906001 183.720501)
    (tags capacitor)
    (path /629B918A/61D7322B)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C35 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B03E)
    (at 137.906001 186.170501)
    (tags capacitor)
    (path /629B918A/616280AF)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C36 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B00E)
    (at 141.756001 183.720501)
    (tags capacitor)
    (path /629B918A/61D73204)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C37 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B33E)
    (at 137.906001 188.620501)
    (tags capacitor)
    (path /629B918A/61628088)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C38 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B30E)
    (at 149.456001 188.620501)
    (tags capacitor)
    (path /629B918A/61D73210)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C39 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B2DE)
    (at 141.756001 186.170501)
    (tags capacitor)
    (path /629B918A/61628094)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C40 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B2AE)
    (at 145.606001 183.720501)
    (tags capacitor)
    (path /629B918A/61D7321A)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C41 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9B27E)
    (at 141.756001 188.620501)
    (tags capacitor)
    (path /629B918A/6162809E)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C42 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9AFDE)
    (at 145.606001 186.170501)
    (tags capacitor)
    (path /629B918A/63262F02)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C43 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9AFAE)
    (at 149.456001 183.720501)
    (tags capacitor)
    (path /629B918A/616280BB)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C44 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9AEE5)
    (at 145.606001 188.620501)
    (tags capacitor)
    (path /629B918A/61D73231)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C45 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:C_0603 (layer F.Cu) (tedit 5EE29C36) (tstamp 61B9AF15)
    (at 149.456001 186.170501)
    (tags capacitor)
    (path /629B918A/616280B5)
    (solder_mask_margin 0.05)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference C46 (at 0 0) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 2u2 (at 0 0.25) (layer F.Fab)
      (effects (font (size 0.127 0.127) (thickness 0.03175)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.162779 -0.51) (end 0.162779 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.162779 0.51) (end 0.162779 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.4 0.7) (end -1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.4 -0.7) (end 1.4 -0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 -0.7) (end 1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.4 0.7) (end -1.4 0.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.SilkS) hide
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (pad 2 smd roundrect (at 0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.75 0) (size 0.85 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module stdpads:Fiducial (layer F.Cu) (tedit 5F1BCA76) (tstamp 61B9AF58)
    (at 151.431001 170.745501)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5CC47A28)
    (attr smd)
    (fp_text reference FID1 (at 0 0.05) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_text value Fiducial (at 0 1.651) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.575))
  )

  (module stdpads:Fiducial (layer F.Cu) (tedit 5F1BCA76) (tstamp 61B9AF49)
    (at 148.331001 173.845501)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5CC4DBD8)
    (attr smd)
    (fp_text reference FID2 (at 0 0.05) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_text value Fiducial (at 0 1.651) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.575))
  )

  (module stdpads:Fiducial (layer F.Cu) (tedit 5F1BCA76) (tstamp 61B9AF3A)
    (at 148.331001 170.745501)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5CC4921D)
    (attr smd)
    (fp_text reference FID3 (at 0 0.05) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_text value Fiducial (at 0 1.651) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.575))
  )

  (module stdpads:Fiducial (layer F.Cu) (tedit 5F1BCA76) (tstamp 61B9AF67)
    (at 145.231001 173.845501)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5CC4DBDF)
    (attr smd)
    (fp_text reference FID4 (at 0 0.05) (layer F.Fab)
      (effects (font (size 0.381 0.381) (thickness 0.09525)))
    )
    (fp_text value Fiducial (at 0 1.651) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.575))
  )

  (module stdpads:PasteHole_1.1mm_PTH (layer F.Cu) (tedit 5E892B4B) (tstamp 61B9AF76)
    (at 145.231001 170.745501)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5CC53461)
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H1 (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )

  (module stdpads:PasteHole_1.1mm_PTH (layer F.Cu) (tedit 5E892B4B) (tstamp 61B9AF94)
    (at 142.131001 173.845501)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5CC795A2)
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H2 (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )

  (module stdpads:PasteHole_1.1mm_PTH (layer F.Cu) (tedit 5E892B4B) (tstamp 61B9AF85)
    (at 142.131001 170.745501)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5CC7E0B9)
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H3 (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )

  (module stdpads:PasteHole_1.1mm_PTH (layer F.Cu) (tedit 5E892B4B) (tstamp 61B9ACEB)
    (at 139.031001 173.845501)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5CC7E0C0)
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H4 (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )

  (module stdpads:PasteHole_1.1mm_PTH (layer F.Cu) (tedit 5E892B4B) (tstamp 61B9ACDC)
    (at 139.031001 170.745501)
    (descr "Circular Fiducial, 1mm bare copper top; 2mm keepout (Level A)")
    (tags marker)
    (path /5ED15A93)
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H5 (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.1)))
    )
    (fp_text value " " (at 0 2) (layer F.Fab) hide
      (effects (font (size 0.508 0.508) (thickness 0.127)))
    )
    (fp_circle (center 0 0) (end 1 0) (layer F.Fab) (width 0.1))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )

  (module stdpads:SOT-353 (layer F.Cu) (tedit 5F739FE4) (tstamp 61B9ACAF)
    (at 118.296001 171.020501)
    (tags "SOT-353 SC-70-5")
    (path /60941922/6178B34B)
    (solder_mask_margin 0.04)
    (solder_paste_margin -0.04)
    (attr smd)
    (fp_text reference U29 (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.254 0.254) (thickness 0.0635)))
    )
    (fp_text value 74LVC1G125GW (at -0.35 0 270) (layer F.Fab)
      (effects (font (size 0.1905 0.1905) (thickness 0.047625)))
    )
    (fp_line (start -1.6 -1.3) (end 1.6 -1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.6 1.3) (end -1.6 -1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.6 1.3) (end -1.6 1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.6 -1.3) (end 1.6 1.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.73 1.16) (end 1.3 1.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.68 -1.16) (end -0.73 -1.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.67 1.1) (end 0.18 1.1) (layer F.Fab) (width 0.1))
    (fp_line (start 0.68 0.6) (end 0.68 -1.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.67 1.1) (end -0.67 -1.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.67 -1.1) (end 0.68 -1.1) (layer F.Fab) (width 0.1))
    (fp_line (start 0.18 1.1) (end 0.68 0.6) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 1.9) (layer F.SilkS)
      (effects (font (size 0.8128 0.8128) (thickness 0.2032)))
    )
    (pad 3 smd roundrect (at 0.85 -0.65 180) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at 0.85 0.65 180) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 461 /Control/RESET~OE~))
    (pad 2 smd roundrect (at 0.85 0 180) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at -0.85 -0.65 180) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 462 "Net-(R1-Pad1)"))
    (pad 5 smd roundrect (at -0.85 0.65 180) (size 1 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )

  (gr_arc (start 191.389 29.464) (end 191.389 27.432) (angle -90) (layer Edge.Cuts) (width 0.15) (tstamp 6185F845))
  (gr_arc (start 270.002 29.464) (end 272.034 29.464) (angle -90) (layer Edge.Cuts) (width 0.15) (tstamp 6185F8D4))
  (gr_arc (start 270.002 161.925) (end 270.002 163.957) (angle -90) (layer Edge.Cuts) (width 0.15) (tstamp 6185F8CD))
  (gr_arc (start 191.389 161.925) (end 189.357 161.925) (angle -90) (layer Edge.Cuts) (width 0.15) (tstamp 61867BD9))
  (gr_line (start 272.034 29.464) (end 272.034 161.925) (layer Edge.Cuts) (width 0.15) (tstamp 618069C5))
  (gr_line (start 191.389 27.432) (end 270.002 27.432) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.357 161.925) (end 189.357 29.464) (layer Edge.Cuts) (width 0.15) (tstamp 61887A9B))
  (gr_line (start 270.002 163.957) (end 191.389 163.957) (layer Edge.Cuts) (width 0.15))

  (segment (start 258.15 143.45) (end 258.15 142.85) (width 0.45) (layer F.Cu) (net 0) (tstamp 61814E93))
  (segment (start 258.15 142.15) (end 258.15 141.45) (width 0.5) (layer F.Cu) (net 0) (tstamp 61814E94))
  (segment (start 257.15 142.15) (end 257.15 142.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61814E95))
  (segment (start 257.15 142.15) (end 257.15 141.45) (width 0.5) (layer F.Cu) (net 0) (tstamp 61814E96))
  (via (at 258.15 142.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61814E97))
  (via (at 257.15 141.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61814E98))
  (via (at 257.15 142.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61814E99))
  (via (at 258.15 141.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61814E9A))
  (segment (start 258.15 142.85) (end 258.15 142.15) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 258.15 151.7) (end 258.15 151) (width 0.5) (layer F.Cu) (net 0) (tstamp 618157F0))
  (via (at 258.15 150.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618157F1))
  (via (at 257.15 150.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618157F2))
  (segment (start 257.15 151) (end 257.15 151.7) (width 0.5) (layer F.Cu) (net 0) (tstamp 618157F3))
  (segment (start 258.15 152.3) (end 258.15 151.7) (width 0.45) (layer F.Cu) (net 0) (tstamp 618157F4))
  (via (at 257.15 151.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618157F5))
  (via (at 258.15 151.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618157F6))
  (segment (start 258.15 151) (end 258.15 150.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 618157F7))
  (segment (start 257.15 151) (end 257.15 150.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 618157F8))
  (segment (start 258.15 134) (end 258.15 133.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 6181581E))
  (via (at 258.15 132.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6181581F))
  (via (at 257.15 132.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815820))
  (segment (start 257.15 133.3) (end 257.15 134) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815821))
  (segment (start 258.15 134.6) (end 258.15 134) (width 0.45) (layer F.Cu) (net 0) (tstamp 61815822))
  (via (at 257.15 134) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815823))
  (via (at 258.15 134) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815824))
  (segment (start 258.15 133.3) (end 258.15 132.6) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815825))
  (segment (start 257.15 133.3) (end 257.15 132.6) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815826))
  (via (at 257.15 125.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815827))
  (segment (start 257.15 124.45) (end 257.15 125.15) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815828))
  (via (at 258.15 123.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815829))
  (segment (start 258.15 124.45) (end 258.15 123.75) (width 0.5) (layer F.Cu) (net 0) (tstamp 6181582A))
  (segment (start 257.15 124.45) (end 257.15 123.75) (width 0.5) (layer F.Cu) (net 0) (tstamp 6181582B))
  (segment (start 258.15 125.75) (end 258.15 125.15) (width 0.45) (layer F.Cu) (net 0) (tstamp 6181582C))
  (segment (start 258.15 125.15) (end 258.15 124.45) (width 0.5) (layer F.Cu) (net 0) (tstamp 6181582D))
  (via (at 257.15 123.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6181582E))
  (via (at 258.15 125.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6181582F))
  (segment (start 258.15 80.9) (end 258.15 80.2) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815906))
  (segment (start 258.15 81.5) (end 258.15 80.9) (width 0.45) (layer F.Cu) (net 0) (tstamp 61815907))
  (via (at 257.15 79.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815908))
  (via (at 258.15 79.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815909))
  (segment (start 257.15 80.2) (end 257.15 80.9) (width 0.5) (layer F.Cu) (net 0) (tstamp 6181590A))
  (segment (start 258.15 89.75) (end 258.15 89.05) (width 0.5) (layer F.Cu) (net 0) (tstamp 6181590B))
  (via (at 258.15 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6181590C))
  (via (at 257.15 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6181590D))
  (via (at 257.15 80.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6181590E))
  (segment (start 257.15 80.2) (end 257.15 79.5) (width 0.5) (layer F.Cu) (net 0) (tstamp 6181590F))
  (segment (start 258.15 89.05) (end 258.15 88.35) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815910))
  (segment (start 257.15 89.05) (end 257.15 89.75) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815911))
  (via (at 258.15 80.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815912))
  (segment (start 258.15 80.2) (end 258.15 79.5) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815913))
  (via (at 258.15 88.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815914))
  (segment (start 258.15 90.35) (end 258.15 89.75) (width 0.45) (layer F.Cu) (net 0) (tstamp 61815915))
  (segment (start 257.15 89.05) (end 257.15 88.35) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815916))
  (via (at 257.15 88.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815917))
  (via (at 258.15 97.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618159EE))
  (segment (start 258.15 106.75) (end 258.15 106.05) (width 0.5) (layer F.Cu) (net 0) (tstamp 618159EF))
  (via (at 258.15 98.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618159F0))
  (segment (start 257.15 106.75) (end 257.15 107.45) (width 0.5) (layer F.Cu) (net 0) (tstamp 618159F1))
  (via (at 257.15 107.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618159F2))
  (segment (start 257.15 97.9) (end 257.15 98.6) (width 0.5) (layer F.Cu) (net 0) (tstamp 618159F3))
  (via (at 258.15 106.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618159F4))
  (segment (start 258.15 97.9) (end 258.15 97.2) (width 0.5) (layer F.Cu) (net 0) (tstamp 618159F5))
  (segment (start 258.15 99.2) (end 258.15 98.6) (width 0.45) (layer F.Cu) (net 0) (tstamp 618159F6))
  (via (at 258.15 107.45) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618159F7))
  (segment (start 258.15 107.45) (end 258.15 106.75) (width 0.5) (layer F.Cu) (net 0) (tstamp 618159F8))
  (segment (start 257.15 106.75) (end 257.15 106.05) (width 0.5) (layer F.Cu) (net 0) (tstamp 618159F9))
  (segment (start 258.15 98.6) (end 258.15 97.9) (width 0.5) (layer F.Cu) (net 0) (tstamp 618159FA))
  (segment (start 258.15 108.05) (end 258.15 107.45) (width 0.45) (layer F.Cu) (net 0) (tstamp 618159FB))
  (via (at 257.15 106.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618159FC))
  (segment (start 257.15 97.9) (end 257.15 97.2) (width 0.5) (layer F.Cu) (net 0) (tstamp 618159FD))
  (via (at 257.15 97.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618159FE))
  (via (at 257.15 98.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618159FF))
  (segment (start 258.15 116.3) (end 258.15 115.6) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815AD7))
  (segment (start 258.15 115.6) (end 258.15 114.9) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815ADA))
  (via (at 257.15 116.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815ADB))
  (segment (start 257.15 115.6) (end 257.15 114.9) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815ADE))
  (segment (start 258.15 116.9) (end 258.15 116.3) (width 0.45) (layer F.Cu) (net 0) (tstamp 61815ADF))
  (via (at 258.15 116.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815AE0))
  (segment (start 257.15 115.6) (end 257.15 116.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 61815AE1))
  (via (at 258.15 114.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815AE4))
  (via (at 257.15 114.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61815AE5))
  (segment (start 201.05 88.85) (end 200.35 88.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A92))
  (segment (start 201.05 87.85) (end 200.35 87.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A8C))
  (via (at 200.35 88.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A8F))
  (segment (start 201.75 87.85) (end 201.05 87.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A80))
  (via (at 201.75 88.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A7D))
  (segment (start 193.5 87.85) (end 192.9 87.85) (width 0.45) (layer F.Cu) (net 0) (tstamp 61827A77))
  (via (at 192.9 87.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A74))
  (segment (start 202.35 87.85) (end 201.75 87.85) (width 0.45) (layer F.Cu) (net 0) (tstamp 61827A6E))
  (via (at 201.75 87.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A6B))
  (segment (start 201.05 88.85) (end 201.75 88.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A62))
  (via (at 200.35 87.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A5F))
  (via (at 210.6 87.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A5C))
  (via (at 219.45 87.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A59))
  (segment (start 211.2 87.85) (end 210.6 87.85) (width 0.45) (layer F.Cu) (net 0) (tstamp 61827A56))
  (via (at 219.45 88.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A53))
  (segment (start 219.45 87.85) (end 218.75 87.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A50))
  (segment (start 218.75 88.85) (end 219.45 88.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A4D))
  (segment (start 218.75 88.85) (end 218.05 88.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A4A))
  (segment (start 220.05 87.85) (end 219.45 87.85) (width 0.45) (layer F.Cu) (net 0) (tstamp 61827A44))
  (segment (start 209.9 88.85) (end 209.2 88.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A41))
  (via (at 210.6 88.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A3E))
  (via (at 218.05 87.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A3B))
  (via (at 218.05 88.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A38))
  (segment (start 210.6 87.85) (end 209.9 87.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A35))
  (via (at 209.2 88.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A32))
  (segment (start 218.75 87.85) (end 218.05 87.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A2F))
  (segment (start 209.9 88.85) (end 210.6 88.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A29))
  (via (at 233.3 128.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618815F5))
  (segment (start 234.3 129.3) (end 234.3 128.7) (width 0.45) (layer F.Cu) (net 0) (tstamp 618815F7))
  (via (at 234.3 109.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61ABC926))
  (segment (start 234.3 137.7) (end 234.3 137) (width 0.5) (layer F.Cu) (net 0) (tstamp 618815F9))
  (via (at 233.3 146.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618815FA))
  (segment (start 233.3 137) (end 233.3 137.7) (width 0.5) (layer F.Cu) (net 0) (tstamp 618815FB))
  (via (at 233.3 119.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618815FC))
  (segment (start 233.3 146) (end 233.3 145.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 618815FE))
  (segment (start 234.3 128) (end 234.3 127.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 618815FF))
  (via (at 233.3 145.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881600))
  (via (at 233.3 127.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881601))
  (segment (start 234.3 138.3) (end 234.3 137.7) (width 0.45) (layer F.Cu) (net 0) (tstamp 61881602))
  (segment (start 233.3 110) (end 233.3 110.7) (width 0.5) (layer F.Cu) (net 0) (tstamp 61ABC920))
  (segment (start 234.3 111.3) (end 234.3 110.7) (width 0.45) (layer F.Cu) (net 0) (tstamp 61ABC91D))
  (via (at 234.3 128.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881607))
  (via (at 234.3 145.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881608))
  (segment (start 234.3 110) (end 234.3 109.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 61ABC923))
  (segment (start 233.3 128) (end 233.3 128.7) (width 0.5) (layer F.Cu) (net 0) (tstamp 6188160B))
  (segment (start 234.3 146.7) (end 234.3 146) (width 0.5) (layer F.Cu) (net 0) (tstamp 6188160C))
  (segment (start 233.3 146) (end 233.3 146.7) (width 0.5) (layer F.Cu) (net 0) (tstamp 6188160E))
  (via (at 234.3 146.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6188160F))
  (via (at 233.3 136.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881610))
  (segment (start 234.3 110.7) (end 234.3 110) (width 0.5) (layer F.Cu) (net 0) (tstamp 61ABC91A))
  (via (at 233.3 110.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61ABC917))
  (segment (start 234.3 146) (end 234.3 145.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 61881614))
  (segment (start 233.3 128) (end 233.3 127.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 61881615))
  (via (at 234.3 127.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881616))
  (via (at 234.3 136.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881617))
  (segment (start 234.3 128.7) (end 234.3 128) (width 0.5) (layer F.Cu) (net 0) (tstamp 61881618))
  (via (at 233.3 137.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881619))
  (via (at 234.3 137.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6188161A))
  (segment (start 234.3 137) (end 234.3 136.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 6188161B))
  (segment (start 234.3 147.3) (end 234.3 146.7) (width 0.45) (layer F.Cu) (net 0) (tstamp 6188161D))
  (segment (start 233.3 137) (end 233.3 136.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 6188161E))
  (segment (start 234.3 119.7) (end 234.3 119) (width 0.5) (layer F.Cu) (net 0) (tstamp 61881620))
  (segment (start 234.3 119) (end 234.3 118.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 61881621))
  (via (at 234.3 110.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61ABC90E))
  (segment (start 233.3 110) (end 233.3 109.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 61ABC914))
  (via (at 233.3 109.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61ABC911))
  (segment (start 234.3 120.3) (end 234.3 119.7) (width 0.45) (layer F.Cu) (net 0) (tstamp 61881625))
  (via (at 234.3 119.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881626))
  (segment (start 233.3 119) (end 233.3 119.7) (width 0.5) (layer F.Cu) (net 0) (tstamp 61881627))
  (via (at 233.3 118.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881628))
  (via (at 234.3 118.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61881629))
  (segment (start 233.3 119) (end 233.3 118.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 6188162A))
  (segment (start 258.15 80.9) (end 258.15 80.2) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882DF7))
  (via (at 258.15 80.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882DF1))
  (via (at 257.15 79.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882DFA))
  (segment (start 257.15 80.2) (end 257.15 80.9) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882DEB))
  (via (at 258.15 79.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882E00))
  (segment (start 258.15 80.2) (end 258.15 79.5) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882DFD))
  (segment (start 258.15 81.5) (end 258.15 80.9) (width 0.45) (layer F.Cu) (net 0) (tstamp 61882DF4))
  (via (at 257.15 80.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882DEE))
  (segment (start 257.15 80.2) (end 257.15 79.5) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882DE8))
  (segment (start 258.15 72.05) (end 258.15 71.35) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882E02))
  (via (at 258.15 72.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882E03))
  (via (at 257.15 70.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882E04))
  (segment (start 257.15 71.35) (end 257.15 72.05) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882E05))
  (via (at 258.15 70.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882E06))
  (segment (start 258.15 71.35) (end 258.15 70.65) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882E07))
  (segment (start 258.15 72.65) (end 258.15 72.05) (width 0.45) (layer F.Cu) (net 0) (tstamp 61882E08))
  (via (at 257.15 72.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882E09))
  (segment (start 257.15 71.35) (end 257.15 70.65) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882E0A))
  (via (at 258.15 70.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882E0B))
  (segment (start 258.15 71.35) (end 258.15 70.65) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882E0C))
  (via (at 257.15 70.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882E0D))
  (segment (start 258.15 72.05) (end 258.15 71.35) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882E0E))
  (segment (start 258.15 72.65) (end 258.15 72.05) (width 0.45) (layer F.Cu) (net 0) (tstamp 61882E0F))
  (via (at 258.15 72.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882E10))
  (via (at 257.15 72.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61882E11))
  (segment (start 257.15 71.35) (end 257.15 72.05) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882E12))
  (segment (start 257.15 71.35) (end 257.15 70.65) (width 0.5) (layer F.Cu) (net 0) (tstamp 61882E13))
  (via (at 196.85 84.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 195.1 84.5) (end 196.85 84.5) (width 0.15) (layer F.Cu) (net 0))
  (via (at 197 83) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D5270))
  (via (at 197 82) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 196.9 82.1) (end 197 82) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 195.1 82.1) (end 196.9 82.1) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 196.9 82.9) (end 197 83) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 195.1 82.9) (end 196.9 82.9) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 195.1 79.7) (end 196.9 79.7) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6478))
  (segment (start 196.9 79.7) (end 197 79.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6479))
  (via (at 197 79.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D647A))
  (via (at 197 80.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D647B))
  (segment (start 195.1 80.5) (end 196.9 80.5) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D647C))
  (segment (start 196.9 80.5) (end 197 80.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D647D))
  (segment (start 195.1 77.3) (end 196.9 77.3) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6484))
  (via (at 197 77.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6485))
  (via (at 197 78.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6486))
  (segment (start 195.1 78.1) (end 196.9 78.1) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6487))
  (segment (start 196.9 78.1) (end 197 78.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6488))
  (segment (start 196.9 77.3) (end 197 77.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6489))
  (segment (start 212.8 84.5) (end 214.55 84.5) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B6B))
  (via (at 214.55 84.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6B6C))
  (segment (start 212.8 82.1) (end 214.6 82.1) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B6D))
  (segment (start 214.6 82.1) (end 214.7 82) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B6E))
  (via (at 214.7 82) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6B6F))
  (via (at 214.7 83) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6B70))
  (segment (start 212.8 82.9) (end 214.6 82.9) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B71))
  (segment (start 214.6 82.9) (end 214.7 83) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B72))
  (segment (start 212.8 79.7) (end 214.6 79.7) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B73))
  (via (at 214.7 79.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6B74))
  (via (at 214.7 80.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6B75))
  (segment (start 212.8 80.5) (end 214.6 80.5) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B76))
  (segment (start 214.6 80.5) (end 214.7 80.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B77))
  (segment (start 214.6 79.7) (end 214.7 79.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B78))
  (via (at 214.55 75.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6B79))
  (segment (start 212.8 75.7) (end 214.55 75.7) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B7A))
  (segment (start 214.6 77.3) (end 214.7 77.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B7B))
  (segment (start 212.8 78.1) (end 214.6 78.1) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B7C))
  (segment (start 212.8 77.3) (end 214.6 77.3) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B7D))
  (segment (start 214.6 78.1) (end 214.7 78.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D6B7E))
  (via (at 214.7 78.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6B7F))
  (via (at 214.7 77.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D6B80))
  (via (at 204.85 75.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 206.6 75.7) (end 204.85 75.7) (width 0.15) (layer F.Cu) (net 0))
  (via (at 204.7 77.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 204.8 77.3) (end 204.7 77.2) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 206.6 77.3) (end 204.8 77.3) (width 0.15) (layer F.Cu) (net 0))
  (via (at 204.7 78.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 204.8 78.1) (end 204.7 78.2) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 206.6 78.1) (end 204.8 78.1) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 204.8 80.5) (end 204.7 80.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D75E0))
  (via (at 204.7 80.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D75E1))
  (segment (start 206.6 80.5) (end 204.8 80.5) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D75E2))
  (segment (start 206.6 79.7) (end 204.8 79.7) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D75E3))
  (via (at 204.7 79.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D75E4))
  (segment (start 204.8 79.7) (end 204.7 79.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D75E5))
  (via (at 204.7 83) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D75EC))
  (segment (start 204.8 82.9) (end 204.7 83) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D75ED))
  (segment (start 204.8 82.1) (end 204.7 82) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D75EE))
  (via (at 204.7 82) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618D75EF))
  (segment (start 206.6 82.1) (end 204.8 82.1) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D75F0))
  (segment (start 206.6 82.9) (end 204.8 82.9) (width 0.15) (layer F.Cu) (net 0) (tstamp 618D75F1))
  (via (at 204.85 84.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 206.6 84.5) (end 204.85 84.5) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 222.5 78.1) (end 222.4 78.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDBF4))
  (via (at 222.4 78.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618DDBF5))
  (segment (start 224.3 78.1) (end 222.5 78.1) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDBF6))
  (segment (start 222.5 82.1) (end 222.4 82) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDBF7))
  (via (at 222.4 80.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618DDBF8))
  (segment (start 222.5 80.5) (end 222.4 80.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDBF9))
  (segment (start 224.3 77.3) (end 222.5 77.3) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDBFA))
  (via (at 222.4 77.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618DDBFB))
  (segment (start 222.5 79.7) (end 222.4 79.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDBFC))
  (via (at 222.4 82) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618DDBFD))
  (segment (start 224.3 82.9) (end 222.5 82.9) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDBFE))
  (via (at 222.4 83) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618DDBFF))
  (segment (start 222.5 82.9) (end 222.4 83) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDC00))
  (via (at 222.4 79.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618DDC01))
  (segment (start 224.3 79.7) (end 222.5 79.7) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDC02))
  (segment (start 224.3 80.5) (end 222.5 80.5) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDC03))
  (segment (start 222.5 77.3) (end 222.4 77.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDC04))
  (segment (start 224.3 82.1) (end 222.5 82.1) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDC05))
  (via (at 222.55 84.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618DDC13))
  (segment (start 224.3 84.5) (end 222.55 84.5) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDC14))
  (via (at 222.55 75.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 618DDC24))
  (segment (start 224.3 75.7) (end 222.55 75.7) (width 0.15) (layer F.Cu) (net 0) (tstamp 618DDC25))
  (via (at 194.8 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 194.8 87.85) (end 194.8 88.95) (width 0.15) (layer F.Cu) (net 0))
  (via (at 195.45 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 195.45 87.85) (end 195.45 89.75) (width 0.15) (layer F.Cu) (net 0))
  (via (at 196.75 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FC9))
  (segment (start 196.75 87.85) (end 196.75 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FCA))
  (segment (start 196.1 87.85) (end 196.1 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FCB))
  (via (at 196.1 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FCC))
  (via (at 198.05 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FD1))
  (segment (start 198.05 87.85) (end 198.05 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FD2))
  (segment (start 198.7 87.85) (end 198.7 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FD4))
  (via (at 198.7 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FD5))
  (segment (start 197.4 87.85) (end 197.4 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FD7))
  (via (at 197.4 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FD8))
  (via (at 204.3 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FE1))
  (segment (start 204.3 87.85) (end 204.3 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FE2))
  (segment (start 205.6 87.85) (end 205.6 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FE3))
  (segment (start 204.95 87.85) (end 204.95 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FE4))
  (via (at 204.95 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FE5))
  (via (at 205.6 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FE6))
  (segment (start 203.65 87.85) (end 203.65 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FE7))
  (via (at 203.65 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FE8))
  (via (at 206.9 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FE9))
  (via (at 208.2 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FEA))
  (segment (start 207.55 87.85) (end 207.55 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FEB))
  (via (at 207.55 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FEC))
  (segment (start 206.9 87.85) (end 206.9 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FED))
  (segment (start 206.25 87.85) (end 206.25 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FEE))
  (via (at 206.25 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61903FEF))
  (segment (start 208.2 87.85) (end 208.2 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61903FF0))
  (via (at 215.1 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904021))
  (segment (start 217.05 87.85) (end 217.05 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61904022))
  (via (at 217.05 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904023))
  (segment (start 216.4 87.85) (end 216.4 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61904024))
  (segment (start 215.75 87.85) (end 215.75 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61904025))
  (segment (start 215.1 87.85) (end 215.1 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61904026))
  (via (at 216.4 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904027))
  (via (at 213.8 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904028))
  (via (at 213.15 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904029))
  (segment (start 213.8 87.85) (end 213.8 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 6190402A))
  (segment (start 213.15 87.85) (end 213.15 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 6190402B))
  (segment (start 214.45 87.85) (end 214.45 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 6190402C))
  (via (at 215.75 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6190402D))
  (via (at 212.5 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6190402E))
  (segment (start 212.5 87.85) (end 212.5 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 6190402F))
  (via (at 214.45 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904030))
  (via (at 225.25 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904051))
  (via (at 223.3 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904052))
  (via (at 221.35 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904053))
  (via (at 222 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904054))
  (segment (start 222.65 87.85) (end 222.65 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61904055))
  (segment (start 221.35 87.85) (end 221.35 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61904056))
  (segment (start 222 87.85) (end 222 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61904057))
  (via (at 224.6 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61904058))
  (segment (start 223.3 87.85) (end 223.3 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 61904059))
  (via (at 222.65 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6190405A))
  (segment (start 225.25 87.85) (end 225.25 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 6190405B))
  (segment (start 224.6 87.85) (end 224.6 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 6190405C))
  (segment (start 225.9 87.85) (end 225.9 89.75) (width 0.15) (layer F.Cu) (net 0) (tstamp 6190405D))
  (via (at 223.95 88.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6190405E))
  (via (at 225.9 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6190405F))
  (segment (start 223.95 87.85) (end 223.95 88.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 61904060))
  (via (at 202.35 86.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 202.35 87.85) (end 202.35 86.75) (width 0.45) (layer F.Cu) (net 0))
  (via (at 202.35 89.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0))
  (segment (start 202.35 87.85) (end 202.35 89.65) (width 0.45) (layer F.Cu) (net 0))
  (segment (start 193.5 87.85) (end 193.5 89.65) (width 0.45) (layer F.Cu) (net 0) (tstamp 6192C148))
  (via (at 193.5 89.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6192C14B))
  (via (at 193.5 86.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6192C14C))
  (segment (start 193.5 87.85) (end 193.5 86.75) (width 0.45) (layer F.Cu) (net 0) (tstamp 6192C14D))
  (segment (start 220.05 87.85) (end 220.05 89.65) (width 0.45) (layer F.Cu) (net 0) (tstamp 6192C154))
  (via (at 220.05 89.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6192C157))
  (segment (start 211.2 87.85) (end 211.2 89.65) (width 0.45) (layer F.Cu) (net 0) (tstamp 6192C158))
  (via (at 211.2 86.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6192C159))
  (via (at 211.2 89.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6192C15C))
  (segment (start 211.2 87.85) (end 211.2 86.75) (width 0.45) (layer F.Cu) (net 0) (tstamp 6192C15D))
  (via (at 220.05 86.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 6192C15E))
  (segment (start 220.05 87.85) (end 220.05 86.75) (width 0.45) (layer F.Cu) (net 0) (tstamp 6192C15F))
  (segment (start 225.9 89.75) (end 225.9 88.75) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 222.55 85.4) (end 222.55 84.5) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 225.9 88.75) (end 222.55 85.4) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 222.05 83.35) (end 222.4 83) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 222.05 85.35) (end 222.05 83.35) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 225.25 88.55) (end 222.05 85.35) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 225.25 88.95) (end 225.25 88.55) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 221.75 82.65) (end 222.4 82) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 221.75 85.5) (end 221.75 82.65) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 224.6 88.35) (end 221.75 85.5) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 224.6 89.75) (end 224.6 88.35) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 223.95 88.15) (end 221.45 85.65) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 221.45 81.55) (end 222.4 80.6) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 221.45 85.65) (end 221.45 81.55) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 223.95 88.95) (end 223.95 88.15) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 221.15 85.8) (end 221.15 80.85) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 223.3 87.95) (end 221.15 85.8) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 221.15 80.85) (end 222.4 79.6) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 223.3 89.75) (end 223.3 87.95) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 220.85 79.75) (end 222.4 78.2) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 220.85 85.95) (end 220.85 79.75) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 222.65 87.75) (end 220.85 85.95) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 222.65 88.95) (end 222.65 87.75) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 220.55 79.05) (end 222.4 77.2) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 220.55 86.1) (end 220.55 79.05) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 222 87.55) (end 220.55 86.1) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 222 89.75) (end 222 87.55) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 220.25 78) (end 222.55 75.7) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 220.25 86.25) (end 220.25 78) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 221.35 87.35) (end 220.25 86.25) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 221.35 88.95) (end 221.35 87.35) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 202.85 79.05) (end 204.7 77.2) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB94))
  (segment (start 202.85 86.1) (end 202.85 79.05) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB95))
  (segment (start 204.3 87.55) (end 202.85 86.1) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB96))
  (segment (start 204.3 89.75) (end 204.3 87.55) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB97))
  (segment (start 203.65 88.95) (end 203.65 87.35) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB98))
  (segment (start 202.55 78) (end 204.85 75.7) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB99))
  (segment (start 203.65 87.35) (end 202.55 86.25) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB9A))
  (segment (start 202.55 86.25) (end 202.55 78) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB9B))
  (segment (start 203.15 79.75) (end 204.7 78.2) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB9C))
  (segment (start 204.95 87.75) (end 203.15 85.95) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB9D))
  (segment (start 204.95 88.95) (end 204.95 87.75) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB9E))
  (segment (start 203.15 85.95) (end 203.15 79.75) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195AB9F))
  (segment (start 203.45 80.85) (end 204.7 79.6) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA0))
  (segment (start 203.45 85.8) (end 203.45 80.85) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA1))
  (segment (start 205.6 87.95) (end 203.45 85.8) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA2))
  (segment (start 205.6 89.75) (end 205.6 87.95) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA3))
  (segment (start 208.2 88.75) (end 204.85 85.4) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA4))
  (segment (start 204.85 85.4) (end 204.85 84.5) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA5))
  (segment (start 207.55 88.95) (end 207.55 88.55) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA6))
  (segment (start 204.35 85.35) (end 204.35 83.35) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA7))
  (segment (start 207.55 88.55) (end 204.35 85.35) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA8))
  (segment (start 204.35 83.35) (end 204.7 83) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABA9))
  (segment (start 208.2 89.75) (end 208.2 88.75) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABAA))
  (segment (start 204.05 82.65) (end 204.7 82) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABAB))
  (segment (start 206.9 88.35) (end 204.05 85.5) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABAC))
  (segment (start 206.9 89.75) (end 206.9 88.35) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABAD))
  (segment (start 204.05 85.5) (end 204.05 82.65) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABAE))
  (segment (start 206.25 88.15) (end 203.75 85.65) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABAF))
  (segment (start 203.75 81.55) (end 204.7 80.6) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABB0))
  (segment (start 206.25 88.95) (end 206.25 88.15) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABB1))
  (segment (start 203.75 85.65) (end 203.75 81.55) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195ABB2))
  (segment (start 198.7 88.95) (end 199.05 88.6) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 199.05 79.25) (end 197 77.2) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 199.05 88.6) (end 199.05 79.25) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 197 78.2) (end 198.75 79.95) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 198.75 79.95) (end 198.75 88.2) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 198.05 88.9) (end 198.05 89.75) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 198.75 88.2) (end 198.05 88.9) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 197.4 88.95) (end 198.45 87.9) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 198.45 81.05) (end 198.45 87.9) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 197 79.6) (end 198.45 81.05) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 196.75 89.75) (end 196.75 88.9) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 196.75 88.9) (end 198.15 87.5) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 198.15 81.75) (end 197 80.6) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 198.15 87.5) (end 198.15 81.75) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 197 82) (end 197.85 82.85) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 197.85 87.2) (end 196.1 88.95) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 197.85 82.85) (end 197.85 87.2) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 196.85 86.9) (end 194.8 88.95) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 196.85 84.5) (end 196.85 86.9) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 197.55 86.8) (end 197.55 83.55) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 197.55 83.55) (end 197 83) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 195.45 88.9) (end 197.55 86.8) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 195.45 89.75) (end 195.45 88.9) (width 0.15) (layer B.Cu) (net 0))
  (segment (start 216.45 79.95) (end 216.45 88.2) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFDE))
  (segment (start 215.55 87.2) (end 213.8 88.95) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFDF))
  (segment (start 215.55 82.85) (end 215.55 87.2) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE0))
  (segment (start 214.45 88.9) (end 215.85 87.5) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE1))
  (segment (start 216.75 79.25) (end 214.7 77.2) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE2))
  (segment (start 216.75 88.6) (end 216.75 79.25) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE3))
  (segment (start 217.05 89.75) (end 217.05 78.2) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE4))
  (segment (start 217.05 78.2) (end 214.55 75.7) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE5))
  (segment (start 215.1 88.95) (end 216.15 87.9) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE6))
  (segment (start 214.7 82) (end 215.55 82.85) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE7))
  (segment (start 215.25 83.55) (end 214.7 83) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE8))
  (segment (start 213.15 89.75) (end 213.15 88.9) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFE9))
  (segment (start 213.15 88.9) (end 215.25 86.8) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFEA))
  (segment (start 215.25 86.8) (end 215.25 83.55) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFEB))
  (segment (start 214.55 86.9) (end 212.5 88.95) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFEC))
  (segment (start 214.7 78.2) (end 216.45 79.95) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFED))
  (segment (start 214.55 84.5) (end 214.55 86.9) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFEE))
  (segment (start 214.45 89.75) (end 214.45 88.9) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFEF))
  (segment (start 215.85 81.75) (end 214.7 80.6) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFF0))
  (segment (start 215.85 87.5) (end 215.85 81.75) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFF1))
  (segment (start 216.4 88.95) (end 216.75 88.6) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFF2))
  (segment (start 214.7 79.6) (end 216.15 81.05) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFF3))
  (segment (start 216.15 81.05) (end 216.15 87.9) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFF4))
  (segment (start 215.75 88.9) (end 215.75 89.75) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFF5))
  (segment (start 216.45 88.2) (end 215.75 88.9) (width 0.15) (layer B.Cu) (net 0) (tstamp 6195DFF6))
  (segment (start 203.1 73.95) (end 204.85 75.7) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 203.1 64.15) (end 203.1 73.95) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 202.8 75.3) (end 204.7 77.2) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 202.8 64.15) (end 202.8 75.3) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 202.5 76) (end 204.7 78.2) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 202.5 64.15) (end 202.5 76) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 202.2 77.1) (end 204.7 79.6) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 202.2 64.15) (end 202.2 77.1) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 201.9 77.8) (end 204.7 80.6) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 201.9 64.15) (end 201.9 77.8) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 204.7 82) (end 201.6 78.9) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 201.6 64.15) (end 201.6 78.9) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 201.3 79.6) (end 204.7 83) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 201.3 64.15) (end 201.3 79.6) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 201 80.65) (end 204.85 84.5) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 201 64.15) (end 201 80.65) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 200.7 80.65) (end 196.85 84.5) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 200.7 64.15) (end 200.7 80.65) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 200.4 79.6) (end 197 83) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 200.4 64.15) (end 200.4 79.6) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 200.1 78.9) (end 197 82) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 200.1 64.15) (end 200.1 78.9) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 199.8 77.8) (end 197 80.6) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 199.8 64.15) (end 199.8 77.8) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 199.5 77.1) (end 197 79.6) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 199.5 64.15) (end 199.5 77.1) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 199.2 76) (end 197 78.2) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 199.2 64.15) (end 199.2 76) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 198.9 75.3) (end 197 77.2) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 198.9 64.15) (end 198.9 75.3) (width 0.15) (layer F.Cu) (net 0))
  (segment (start 218.4 80.65) (end 214.55 84.5) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE44))
  (segment (start 218.4 64.15) (end 218.4 80.65) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE45))
  (segment (start 216.6 75.3) (end 214.7 77.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE46))
  (segment (start 216.6 64.15) (end 216.6 75.3) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE47))
  (segment (start 222.4 82) (end 219.3 78.9) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE48))
  (segment (start 216.9 76) (end 214.7 78.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE49))
  (segment (start 216.9 64.15) (end 216.9 76) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE4A))
  (segment (start 218.1 64.15) (end 218.1 79.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE4B))
  (segment (start 219.6 64.15) (end 219.6 77.8) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE4C))
  (segment (start 219.6 77.8) (end 222.4 80.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE4D))
  (segment (start 217.8 64.15) (end 217.8 78.9) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE4E))
  (segment (start 217.8 78.9) (end 214.7 82) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE4F))
  (segment (start 218.1 79.6) (end 214.7 83) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE50))
  (segment (start 220.5 75.3) (end 222.4 77.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE51))
  (segment (start 220.5 64.15) (end 220.5 75.3) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE52))
  (segment (start 220.8 64.15) (end 220.8 73.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE53))
  (segment (start 220.8 73.95) (end 222.55 75.7) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE54))
  (segment (start 219 79.6) (end 222.4 83) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE55))
  (segment (start 219 64.15) (end 219 79.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE56))
  (segment (start 216.3 73.95) (end 214.55 75.7) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE57))
  (segment (start 216.3 64.15) (end 216.3 73.95) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE58))
  (segment (start 219.3 64.15) (end 219.3 78.9) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE59))
  (segment (start 220.2 76) (end 222.4 78.2) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE5A))
  (segment (start 220.2 64.15) (end 220.2 76) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE5B))
  (segment (start 217.2 77.1) (end 214.7 79.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE5C))
  (segment (start 217.5 77.8) (end 214.7 80.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE5D))
  (segment (start 217.5 64.15) (end 217.5 77.8) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE5E))
  (segment (start 217.2 64.15) (end 217.2 77.1) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE5F))
  (segment (start 218.7 80.65) (end 222.55 84.5) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE60))
  (segment (start 218.7 64.15) (end 218.7 80.65) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE61))
  (segment (start 219.9 77.1) (end 222.4 79.6) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE62))
  (segment (start 219.9 64.15) (end 219.9 77.1) (width 0.15) (layer F.Cu) (net 0) (tstamp 6196EE63))
  (via (at 192.5 86.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61A01B51))
  (segment (start 193.2 86.1) (end 192.5 86.1) (width 0.5) (layer F.Cu) (net 0))
  (via (at 192.5 85.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61A01B4B))
  (segment (start 193.2 85.1) (end 192.5 85.1) (width 0.5) (layer F.Cu) (net 0) (tstamp 61A01B4E))
  (segment (start 193.2 86.1) (end 193.2 86.6) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 193.5 86.9) (end 193.5 87.85) (width 0.5) (layer F.Cu) (net 0))
  (segment (start 193.2 86.6) (end 193.5 86.9) (width 0.5) (layer F.Cu) (net 0))
  (via (at 209.2 87.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61827A2C))
  (segment (start 209.9 87.85) (end 209.2 87.85) (width 0.5) (layer F.Cu) (net 0) (tstamp 61827A47))
  (via (at 269.494 28.575) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 0) (tstamp 61A9F784))
  (segment (start 267.703 28.575) (end 269.494 28.575) (width 0.8) (layer F.Cu) (net 0) (tstamp 61A9F781))
  (via (at 248.412 28.575) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 0) (tstamp 61A9F77E))
  (segment (start 250.203 28.575) (end 248.412 28.575) (width 0.8) (layer F.Cu) (net 0) (tstamp 61A9F77B))
  (via (at 248.412 29.845) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 0))
  (segment (start 250.203 29.845) (end 248.412 29.845) (width 0.8) (layer F.Cu) (net 0))
  (via (at 234.3 99.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61ABC928))
  (segment (start 234.3 100) (end 234.3 99.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 61ABC929))
  (segment (start 233.3 100) (end 233.3 100.7) (width 0.5) (layer F.Cu) (net 0) (tstamp 61ABC92A))
  (segment (start 234.3 101.3) (end 234.3 100.7) (width 0.45) (layer F.Cu) (net 0) (tstamp 61ABC92B))
  (segment (start 234.3 100.7) (end 234.3 100) (width 0.5) (layer F.Cu) (net 0) (tstamp 61ABC92C))
  (via (at 233.3 100.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61ABC92D))
  (segment (start 233.3 100) (end 233.3 99.3) (width 0.5) (layer F.Cu) (net 0) (tstamp 61ABC92E))
  (via (at 233.3 99.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61ABC92F))
  (via (at 234.3 100.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 0) (tstamp 61ABC930))
  (via (at 207.5815 126.8095) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 207.5815 125.592) (end 207.5815 126.8095) (width 0.15) (layer F.Cu) (net 1))
  (via (at 222.25 136.144) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6186835F))
  (segment (start 223.012 136.144) (end 222.25 136.144) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868368))
  (segment (start 220.9815 148.209) (end 222.1865 148.209) (width 0.4) (layer F.Cu) (net 1) (tstamp 6186839B))
  (via (at 222.1865 148.209) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61868380))
  (segment (start 222.9485 148.209) (end 222.1865 148.209) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683B0))
  (via (at 222.25 156.083) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618683A4))
  (segment (start 221.996 155.829) (end 222.25 156.083) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683C2))
  (segment (start 220.9815 155.829) (end 221.996 155.829) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868386))
  (segment (start 222.3215 156.0115) (end 222.25 156.083) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683B6))
  (segment (start 222.9485 156.0115) (end 222.3215 156.0115) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868356))
  (via (at 212.0265 160.274) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61868374))
  (segment (start 212.0265 159.069) (end 212.0265 160.274) (width 0.4) (layer F.Cu) (net 1) (tstamp 6186837D))
  (via (at 212.0265 157.861) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6186835C))
  (segment (start 212.0265 159.069) (end 212.0265 157.861) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683B3))
  (via (at 204.4065 160.274) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61868362))
  (segment (start 204.4065 159.069) (end 204.4065 160.274) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868389))
  (via (at 204.4065 157.861) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618683C5))
  (segment (start 204.4065 159.069) (end 204.4065 157.861) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683D4))
  (segment (start 194.1815 155.829) (end 195.199 155.829) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683AD))
  (via (at 195.3895 155.5115) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6186834D))
  (segment (start 195.3895 155.6385) (end 195.3895 155.5115) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683D7))
  (segment (start 195.199 155.829) (end 195.3895 155.6385) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868350))
  (segment (start 194.1815 155.194) (end 195.199 155.194) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868395))
  (segment (start 195.3895 155.3845) (end 195.3895 155.5115) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683DD))
  (segment (start 195.199 155.194) (end 195.3895 155.3845) (width 0.4) (layer F.Cu) (net 1) (tstamp 6186839E))
  (segment (start 194.1815 155.829) (end 193.167 155.829) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683DA))
  (via (at 192.9765 155.5115) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618683AA))
  (segment (start 192.9765 155.6385) (end 192.9765 155.5115) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868398))
  (segment (start 193.167 155.829) (end 192.9765 155.6385) (width 0.4) (layer F.Cu) (net 1) (tstamp 6186834A))
  (segment (start 194.1815 155.194) (end 193.167 155.194) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868365))
  (segment (start 192.9765 155.3845) (end 192.9765 155.5115) (width 0.4) (layer F.Cu) (net 1) (tstamp 6186838F))
  (segment (start 193.167 155.194) (end 192.9765 155.3845) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683BF))
  (via (at 195.3895 148.844) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61868383))
  (segment (start 194.1815 148.844) (end 195.3895 148.844) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868392))
  (via (at 192.9765 148.844) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618683C8))
  (segment (start 194.1815 148.844) (end 192.9765 148.844) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683CB))
  (via (at 195.3895 136.144) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618683D1))
  (segment (start 194.1815 136.144) (end 195.3895 136.144) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683A7))
  (via (at 192.9765 136.144) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6186837A))
  (segment (start 194.1815 136.144) (end 192.9765 136.144) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683CE))
  (segment (start 192.2145 136.144) (end 192.9765 136.144) (width 0.5) (layer F.Cu) (net 1) (tstamp 61868353))
  (segment (start 192.2145 148.844) (end 192.9765 148.844) (width 0.5) (layer F.Cu) (net 1) (tstamp 618683B9))
  (segment (start 220.9815 155.829) (end 219.964 155.829) (width 0.4) (layer F.Cu) (net 1) (tstamp 6186836E))
  (via (at 219.71 156.083) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61868359))
  (segment (start 219.964 155.829) (end 219.71 156.083) (width 0.4) (layer F.Cu) (net 1) (tstamp 618683A1))
  (via (at 204.4065 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 619E7C82))
  (via (at 204.4065 131.064) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61868377))
  (segment (start 204.4065 132.269) (end 204.4065 131.064) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868371))
  (segment (start 204.4065 130.302) (end 204.4065 131.064) (width 0.5) (layer F.Cu) (net 1) (tstamp 61868164))
  (via (at 210.1215 131.064) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61868140))
  (via (at 210.1215 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6186819D))
  (segment (start 210.1215 130.302) (end 210.1215 131.064) (width 0.5) (layer F.Cu) (net 1) (tstamp 61868101))
  (segment (start 192.9765 155.5115) (end 192.2145 155.5115) (width 0.5) (layer F.Cu) (net 1) (tstamp 6186818E))
  (segment (start 204.4065 161.036) (end 204.4065 160.274) (width 0.5) (layer F.Cu) (net 1) (tstamp 61868161))
  (via (at 209.2325 160.3375) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618680D1))
  (segment (start 209.4865 160.0835) (end 209.2325 160.3375) (width 0.4) (layer F.Cu) (net 1) (tstamp 618680C2))
  (segment (start 209.4865 159.069) (end 209.4865 160.0835) (width 0.4) (layer F.Cu) (net 1) (tstamp 618681F4))
  (segment (start 212.0345 160.282) (end 212.0265 160.274) (width 0.5) (layer F.Cu) (net 1) (tstamp 618681E5))
  (segment (start 212.0345 161.036) (end 212.0345 160.282) (width 0.5) (layer F.Cu) (net 1) (tstamp 61868116))
  (segment (start 209.304 160.409) (end 209.2325 160.3375) (width 0.5) (layer F.Cu) (net 1) (tstamp 6186813A))
  (segment (start 209.304 161.036) (end 209.304 160.409) (width 0.5) (layer F.Cu) (net 1) (tstamp 618681A0))
  (via (at 209.2325 157.7975) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618680DD))
  (segment (start 209.4865 158.0515) (end 209.2325 157.7975) (width 0.4) (layer F.Cu) (net 1) (tstamp 61868197))
  (segment (start 209.4865 159.069) (end 209.4865 158.0515) (width 0.4) (layer F.Cu) (net 1) (tstamp 6186816D))
  (via (at 196.723 125.603) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6187135F))
  (segment (start 197.4105 125.603) (end 196.723 125.603) (width 0.5) (layer F.Cu) (net 1) (tstamp 61871374))
  (segment (start 197.4215 125.592) (end 197.4105 125.603) (width 0.5) (layer F.Cu) (net 1) (tstamp 61871362))
  (via (at 197.4215 126.8095) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618713A7))
  (segment (start 197.4215 125.592) (end 197.4215 126.8095) (width 0.5) (layer F.Cu) (net 1) (tstamp 61871368))
  (via (at 207.5815 100.7745) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61871398))
  (segment (start 207.5815 101.992) (end 207.5815 100.7745) (width 0.5) (layer F.Cu) (net 1) (tstamp 6187139B))
  (via (at 206.3115 100.7745) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61871347))
  (segment (start 206.3115 101.992) (end 206.3115 100.7745) (width 0.5) (layer F.Cu) (net 1) (tstamp 61871380))
  (via (at 207.5815 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6187134A))
  (segment (start 207.5815 101.992) (end 207.5815 103.1875) (width 0.5) (layer F.Cu) (net 1) (tstamp 6187138C))
  (via (at 206.3115 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618713A4))
  (segment (start 206.3115 101.992) (end 206.3115 103.1875) (width 0.5) (layer F.Cu) (net 1) (tstamp 6187135C))
  (via (at 205.0415 124.3965) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61871377))
  (segment (start 205.0415 125.592) (end 205.0415 124.3965) (width 0.5) (layer F.Cu) (net 1) (tstamp 61871359))
  (via (at 206.3115 124.3965) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618713A1))
  (segment (start 206.3115 125.592) (end 206.3115 124.3965) (width 0.5) (layer F.Cu) (net 1) (tstamp 618713AD))
  (via (at 206.3115 126.8095) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61871392))
  (segment (start 206.3115 125.592) (end 206.3115 126.8095) (width 0.5) (layer F.Cu) (net 1) (tstamp 61871350))
  (via (at 205.0415 126.8095) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61871386))
  (segment (start 205.0415 125.592) (end 205.0415 126.8095) (width 0.5) (layer F.Cu) (net 1) (tstamp 6187137A))
  (via (at 218.186 123.952) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61871395))
  (segment (start 219.3815 123.952) (end 218.186 123.952) (width 0.5) (layer F.Cu) (net 1) (tstamp 61871365))
  (via (at 220.7895 123.952) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6187136E))
  (via (at 219.3925 102.997) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61871356))
  (segment (start 219.3815 103.008) (end 219.3925 102.997) (width 0.5) (layer F.Cu) (net 1) (tstamp 61871353))
  (segment (start 219.3815 103.632) (end 219.3815 103.008) (width 0.5) (layer F.Cu) (net 1) (tstamp 61871383))
  (via (at 220.599 103.632) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618713AA))
  (segment (start 219.3815 103.632) (end 220.599 103.632) (width 0.5) (layer F.Cu) (net 1) (tstamp 6187138F))
  (via (at 223.647 156.0195) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6186808F))
  (segment (start 223.639 156.0115) (end 223.647 156.0195) (width 0.5) (layer F.Cu) (net 1) (tstamp 61868092))
  (segment (start 222.9485 156.0115) (end 223.639 156.0115) (width 0.5) (layer F.Cu) (net 1) (tstamp 6186808C))
  (via (at 223.647 148.209) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618683E0))
  (segment (start 222.9485 148.209) (end 223.647 148.209) (width 0.5) (layer F.Cu) (net 1) (tstamp 618683E3))
  (via (at 223.7105 136.144) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618683E6))
  (segment (start 223.012 136.144) (end 223.7105 136.144) (width 0.5) (layer F.Cu) (net 1) (tstamp 618683E9))
  (via (at 204.4065 129.6035) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6186804A))
  (segment (start 204.4065 130.302) (end 204.4065 129.6035) (width 0.5) (layer F.Cu) (net 1) (tstamp 61868050))
  (via (at 210.1215 129.6035) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618680A1))
  (segment (start 210.1215 130.302) (end 210.1215 129.6035) (width 0.5) (layer F.Cu) (net 1) (tstamp 6186809B))
  (via (at 204.4065 161.7345) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 619141D1))
  (segment (start 204.4065 161.036) (end 204.4065 161.7345) (width 0.5) (layer F.Cu) (net 1))
  (via (at 191.516 148.844) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 192.2145 148.844) (end 191.516 148.844) (width 0.5) (layer F.Cu) (net 1))
  (via (at 197.4215 129.6035) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 197.4215 130.302) (end 197.4215 129.6035) (width 0.5) (layer F.Cu) (net 1))
  (via (at 206.3115 129.6035) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 206.3115 130.302) (end 206.3115 129.6035) (width 0.5) (layer F.Cu) (net 1))
  (via (at 207.75 74.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE35))
  (segment (start 206.6 74.9) (end 207.75 74.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE36))
  (segment (start 206.6 74.9) (end 205.45 74.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE37))
  (via (at 205.45 74.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE38))
  (segment (start 207.95 75.2) (end 207.75 75) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE3C))
  (via (at 205.45 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE3D))
  (segment (start 207.75 75) (end 207.75 74.9) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE3E))
  (segment (start 206.6 78.9) (end 205.45 78.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE3F))
  (segment (start 208.5 83.7) (end 207.75 83.7) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE41))
  (segment (start 208.5 78.9) (end 209.2 78.9) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE42))
  (via (at 209.2 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE43))
  (via (at 207.75 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE4C))
  (segment (start 206.6 83.7) (end 207.75 83.7) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE4D))
  (segment (start 206.6 85.3) (end 205.45 85.3) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE4E))
  (via (at 209.2 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE4F))
  (segment (start 208.5 83.7) (end 209.2 83.7) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE50))
  (via (at 205.45 85.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE51))
  (via (at 206.6 63.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE52))
  (segment (start 206.6 64.5) (end 206.6 63.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE53))
  (via (at 209.2 85.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE54))
  (segment (start 208.5 85.3) (end 209.2 85.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE55))
  (segment (start 206.6 64.5) (end 207.75 64.5) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE56))
  (via (at 205.45 64.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE57))
  (via (at 207.75 64.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE58))
  (segment (start 206.6 64.5) (end 205.45 64.5) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE59))
  (segment (start 208.5 85.3) (end 207.75 85.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE5C))
  (segment (start 208.5 75.2) (end 207.95 75.2) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE5F))
  (segment (start 208.5 64.5) (end 209.2 64.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 618F1224))
  (segment (start 208.5 75.2) (end 209.2 75.2) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE67))
  (via (at 209.2 75.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE68))
  (via (at 209.2 64.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618F121B))
  (via (at 207.75 85.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE6F))
  (via (at 205.45 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE70))
  (segment (start 206.6 85.3) (end 207.75 85.3) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE71))
  (segment (start 206.6 78.9) (end 207.75 78.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE72))
  (segment (start 208.5 64.5) (end 207.75 64.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 6189FE73))
  (segment (start 208.5 78.9) (end 207.75 78.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE74))
  (segment (start 206.6 83.7) (end 205.45 83.7) (width 0.45) (layer F.Cu) (net 1) (tstamp 6189FE75))
  (via (at 207.75 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 6189FE76))
  (via (at 213.95 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A06DE))
  (segment (start 212.8 76.5) (end 213.95 76.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A06DF))
  (segment (start 212.8 76.5) (end 211.65 76.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A06E0))
  (via (at 211.65 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A06E1))
  (segment (start 212.8 81.3) (end 213.95 81.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A06F6))
  (via (at 211.65 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A06F7))
  (via (at 213.95 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A06F8))
  (segment (start 212.8 81.3) (end 211.65 81.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A06F9))
  (segment (start 210.9 76.5) (end 211.65 76.5) (width 0.5) (layer F.Cu) (net 1))
  (via (at 210.2 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 210.9 76.5) (end 210.2 76.5) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 210.9 81.3) (end 211.65 81.3) (width 0.5) (layer F.Cu) (net 1))
  (via (at 210.2 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 210.9 81.3) (end 210.2 81.3) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 193.2 81.3) (end 192.5 81.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A2E03))
  (via (at 192.5 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A2E04))
  (segment (start 195.1 81.3) (end 193.95 81.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A2E08))
  (via (at 196.25 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A2E09))
  (via (at 193.95 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A2E0A))
  (segment (start 195.1 81.3) (end 196.25 81.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A2E13))
  (segment (start 193.2 81.3) (end 193.95 81.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A2E17))
  (segment (start 193.2 76.5) (end 193.95 76.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A2E1A))
  (via (at 193.95 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A2E1B))
  (segment (start 195.1 76.5) (end 193.95 76.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A2E1C))
  (via (at 196.25 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A2E1D))
  (segment (start 195.1 76.5) (end 196.25 76.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A2E1F))
  (segment (start 193.2 76.5) (end 192.5 76.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 618A2E27))
  (via (at 192.5 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618A2E28))
  (via (at 225.45 85.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC2A))
  (via (at 223.15 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC2B))
  (segment (start 224.3 85.3) (end 225.45 85.3) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC2C))
  (segment (start 224.3 78.9) (end 225.45 78.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC2D))
  (segment (start 226.2 64.5) (end 225.45 64.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC2E))
  (segment (start 226.2 78.9) (end 225.45 78.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC2F))
  (segment (start 224.3 83.7) (end 223.15 83.7) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC30))
  (via (at 225.45 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC31))
  (segment (start 224.3 74.9) (end 225.45 74.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC32))
  (via (at 225.45 74.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC35))
  (segment (start 224.3 74.9) (end 223.15 74.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC36))
  (via (at 223.15 74.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC37))
  (segment (start 225.65 75.2) (end 225.45 75) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC3B))
  (via (at 223.15 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC3C))
  (segment (start 225.45 75) (end 225.45 74.9) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC3D))
  (segment (start 224.3 78.9) (end 223.15 78.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC3E))
  (segment (start 226.2 83.7) (end 225.45 83.7) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC40))
  (segment (start 226.2 78.9) (end 226.9 78.9) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC41))
  (via (at 226.9 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC42))
  (via (at 225.45 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC4B))
  (segment (start 224.3 83.7) (end 225.45 83.7) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC4C))
  (segment (start 224.3 85.3) (end 223.15 85.3) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC4D))
  (via (at 226.9 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC4E))
  (segment (start 226.2 83.7) (end 226.9 83.7) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC4F))
  (via (at 223.15 85.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC50))
  (via (at 224.3 63.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC51))
  (segment (start 224.3 64.5) (end 224.3 63.9) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC52))
  (via (at 226.9 85.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC53))
  (segment (start 226.2 85.3) (end 226.9 85.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC54))
  (segment (start 224.3 64.5) (end 225.45 64.5) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC55))
  (via (at 223.15 64.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC56))
  (via (at 225.45 64.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC57))
  (segment (start 224.3 64.5) (end 223.15 64.5) (width 0.45) (layer F.Cu) (net 1) (tstamp 618DDC58))
  (segment (start 226.2 85.3) (end 225.45 85.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC5B))
  (segment (start 226.2 75.2) (end 225.65 75.2) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC5E))
  (segment (start 226.2 75.2) (end 226.9 75.2) (width 0.5) (layer F.Cu) (net 1) (tstamp 618DDC63))
  (via (at 226.9 75.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 618DDC64))
  (via (at 226.9 64.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 226.2 64.5) (end 226.9 64.5) (width 0.5) (layer F.Cu) (net 1))
  (via (at 195.7705 102.9335) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 195.7815 102.9445) (end 195.7705 102.9335) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 195.7815 103.632) (end 195.7815 102.9445) (width 0.5) (layer F.Cu) (net 1))
  (via (at 223.52 123.952) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61907078))
  (segment (start 224.2185 123.952) (end 223.52 123.952) (width 0.5) (layer F.Cu) (net 1))
  (via (at 196.65 56.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AE50E6))
  (segment (start 197.35 56.55) (end 196.65 56.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AE50E3))
  (via (at 198.05 56.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AE50DD))
  (segment (start 197.35 44.55) (end 196.65 44.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AE50C2))
  (via (at 198.05 44.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AE50BF))
  (segment (start 197.35 44.55) (end 198.05 44.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AE50BC))
  (via (at 196.65 44.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AE50B9))
  (via (at 198.05 59.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AE50B0))
  (segment (start 197.35 59.9) (end 198.05 59.9) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AE50AD))
  (segment (start 197.35 41.3) (end 196.65 41.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AE50AA))
  (via (at 198.05 41.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AE50A7))
  (segment (start 197.35 41.3) (end 198.05 41.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AE50A4))
  (via (at 196.65 41.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AE50A1))
  (via (at 199.95 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC350A))
  (segment (start 218.25 61.3) (end 218.25 62) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC3501))
  (segment (start 199.95 61.3) (end 199.95 62) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC34B9))
  (via (at 218.25 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC349E))
  (via (at 218.25 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC34A7))
  (segment (start 199.95 61.3) (end 199.95 60.6) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC3510))
  (segment (start 218.25 61.3) (end 218.25 60.6) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC34BC))
  (via (at 199.95 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC34FE))
  (segment (start 219.85 58.8) (end 219.15 58.8) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC331E))
  (via (at 220.55 58.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC3327))
  (segment (start 219.85 43.55) (end 219.15 43.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC332A))
  (segment (start 219.85 40.3) (end 220.55 40.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC3330))
  (via (at 219.15 58.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC3333))
  (via (at 219.15 55.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC333F))
  (segment (start 219.85 43.55) (end 220.55 43.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC334E))
  (segment (start 219.85 55.55) (end 220.55 55.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC335D))
  (via (at 220.55 43.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC3360))
  (via (at 219.15 43.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC3366))
  (segment (start 219.85 40.3) (end 219.15 40.3) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC336C))
  (segment (start 219.85 58.8) (end 220.55 58.8) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC336F))
  (via (at 220.55 55.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC337E))
  (via (at 219.15 40.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC3384))
  (segment (start 219.85 55.55) (end 219.15 55.55) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC3387))
  (via (at 220.55 40.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC338A))
  (via (at 198.85 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC3513))
  (segment (start 214.1 38.8) (end 214.1 39.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC342F))
  (via (at 198.85 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC340E))
  (via (at 214.1 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC33E4))
  (segment (start 217.35 38.8) (end 217.35 38.1) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC3438))
  (segment (start 198.85 38.8) (end 198.85 39.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC3435))
  (via (at 202.1 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC33FF))
  (via (at 202.1 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC340B))
  (segment (start 214.1 38.8) (end 214.1 38.1) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC33F3))
  (segment (start 202.1 38.8) (end 202.1 38.1) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC341A))
  (via (at 214.1 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC343E))
  (via (at 217.35 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC3432))
  (segment (start 198.85 38.8) (end 198.85 38.1) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC33E1))
  (segment (start 202.1 38.8) (end 202.1 39.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC3411))
  (via (at 217.35 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 61AC3441))
  (segment (start 217.35 38.8) (end 217.35 39.5) (width 0.5) (layer F.Cu) (net 1) (tstamp 61AC3453))
  (via (at 197.35 60.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 197.35 59.9) (end 197.35 60.65) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 197.9 56.55) (end 198.05 56.4) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 197.35 56.55) (end 197.9 56.55) (width 0.5) (layer F.Cu) (net 1))
  (via (at 207.5815 97.9805) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 207.5815 97.282) (end 207.5815 97.9805) (width 0.5) (layer F.Cu) (net 1))
  (via (at 206.3115 97.9805) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 206.3115 97.282) (end 206.3115 97.9805) (width 0.5) (layer F.Cu) (net 1))
  (via (at 207.5815 96.5835) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 207.5815 97.282) (end 207.5815 96.5835) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 206.3115 100.7745) (end 206.3115 97.9805) (width 0.6) (layer F.Cu) (net 1))
  (segment (start 207.5815 97.9805) (end 207.5815 100.7745) (width 0.6) (layer F.Cu) (net 1))
  (via (at 206.3115 96.5835) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 206.3115 97.282) (end 206.3115 96.5835) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 197.231 97.282) (end 197.231 96.5835) (width 0.5) (layer F.Cu) (net 1) (tstamp 617C1B4B))
  (via (at 197.231 96.5835) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 617C1B4E))
  (via (at 197.231 97.9805) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1) (tstamp 617C1B45))
  (segment (start 197.231 97.282) (end 197.231 97.9805) (width 0.5) (layer F.Cu) (net 1) (tstamp 617C1B48))
  (via (at 219.3925 97.9805) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 219.3925 97.282) (end 219.3925 97.9805) (width 0.5) (layer F.Cu) (net 1))
  (via (at 219.3925 96.5835) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 219.3925 97.282) (end 219.3925 96.5835) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 219.3925 97.9805) (end 219.3925 102.997) (width 0.6) (layer F.Cu) (net 1))
  (via (at 217.7415 157.861) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 217.7415 159.069) (end 217.7415 157.861) (width 0.4) (layer F.Cu) (net 1))
  (via (at 217.7415 160.274) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 217.7415 159.069) (end 217.7415 160.274) (width 0.4) (layer F.Cu) (net 1))
  (via (at 218.3765 159.0675) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (via (at 212.0265 161.7345) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 212.0345 161.7265) (end 212.0265 161.7345) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 212.0345 161.036) (end 212.0345 161.7265) (width 0.5) (layer F.Cu) (net 1))
  (via (at 209.296 161.7345) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 209.304 161.7265) (end 209.296 161.7345) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 209.304 161.036) (end 209.304 161.7265) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 218.375 159.069) (end 218.3765 159.0675) (width 0.4) (layer F.Cu) (net 1))
  (segment (start 217.7415 159.069) (end 218.375 159.069) (width 0.4) (layer F.Cu) (net 1))
  (via (at 224.917 123.952) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 224.2185 123.952) (end 224.917 123.952) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 220.9815 136.144) (end 222.25 136.144) (width 0.4) (layer F.Cu) (net 1))
  (via (at 196.977 103.632) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 195.7815 103.632) (end 196.977 103.632) (width 0.5) (layer F.Cu) (net 1))
  (via (at 191.516 155.5115) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 192.2145 155.5115) (end 191.516 155.5115) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 197.231 99.06) (end 197.231 97.9805) (width 0.6) (layer F.Cu) (net 1))
  (segment (start 195.7705 100.5205) (end 197.231 99.06) (width 0.6) (layer F.Cu) (net 1))
  (segment (start 195.7705 102.9335) (end 195.7705 100.5205) (width 0.6) (layer F.Cu) (net 1))
  (segment (start 204.4065 132.269) (end 204.4065 133.477) (width 0.4) (layer F.Cu) (net 1) (tstamp 6186836B))
  (segment (start 210.1215 132.269) (end 210.1215 131.064) (width 0.4) (layer F.Cu) (net 1) (tstamp 618681AC))
  (segment (start 210.1215 132.269) (end 210.1215 133.477) (width 0.4) (layer F.Cu) (net 1))
  (via (at 218.186 128.27) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 217.424 127) (end 217.7415 126.6825) (width 0.15) (layer F.Cu) (net 1))
  (segment (start 217.7415 126.6825) (end 217.7415 125.592) (width 0.15) (layer F.Cu) (net 1))
  (segment (start 218.186 128.27) (end 217.424 127.508) (width 0.15) (layer F.Cu) (net 1))
  (segment (start 217.424 127.508) (end 217.424 127) (width 0.15) (layer F.Cu) (net 1))
  (segment (start 220.7895 123.952) (end 223.52 123.952) (width 0.6) (layer F.Cu) (net 1))
  (segment (start 219.3815 123.952) (end 220.7895 123.952) (width 0.5) (layer F.Cu) (net 1))
  (via (at 198.12 130.302) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 1))
  (segment (start 197.4215 130.302) (end 198.12 130.302) (width 0.5) (layer F.Cu) (net 1))
  (segment (start 233.3 155) (end 233.3 154.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 618815F6))
  (via (at 233.3 154.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61881603))
  (via (at 190.119 51.435) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61737E0E))
  (via (at 214.05 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC34CB))
  (segment (start 214.05 61.3) (end 214.05 62) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC34DD))
  (via (at 214.05 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC34C5))
  (segment (start 214.05 61.3) (end 214.05 60.6) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3507))
  (via (at 210.15 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6178EF13))
  (via (at 210.15 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6178EF0D))
  (segment (start 210.15 61.3) (end 210.15 60.6) (width 0.5) (layer F.Cu) (net 2) (tstamp 6178EF07))
  (segment (start 210.15 61.3) (end 210.15 62) (width 0.5) (layer F.Cu) (net 2) (tstamp 6178EF01))
  (via (at 199.35 92.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 199.35 93.75) (end 199.35 92.65) (width 0.45) (layer F.Cu) (net 2))
  (via (at 199.35 94.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 199.35 93.75) (end 199.35 94.85) (width 0.45) (layer F.Cu) (net 2))
  (via (at 199.95 93.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 199.35 93.75) (end 199.95 93.75) (width 0.45) (layer F.Cu) (net 2))
  (segment (start 208.2 93.75) (end 208.8 93.75) (width 0.45) (layer F.Cu) (net 2) (tstamp 61931A88))
  (via (at 208.8 93.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61931A8B))
  (segment (start 208.2 93.75) (end 208.2 92.65) (width 0.45) (layer F.Cu) (net 2) (tstamp 61931A8C))
  (via (at 208.2 92.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61931A8D))
  (segment (start 217.05 93.75) (end 217.65 93.75) (width 0.45) (layer F.Cu) (net 2) (tstamp 61931A94))
  (segment (start 217.05 93.75) (end 217.05 92.65) (width 0.45) (layer F.Cu) (net 2) (tstamp 61931A95))
  (segment (start 217.05 93.75) (end 217.05 94.85) (width 0.45) (layer F.Cu) (net 2) (tstamp 61931A96))
  (via (at 217.05 92.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61931A97))
  (via (at 217.65 93.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61931A98))
  (via (at 225.9 92.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61931AA0))
  (segment (start 225.9 93.75) (end 225.9 94.85) (width 0.45) (layer F.Cu) (net 2) (tstamp 61931AA1))
  (via (at 226.5 93.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61931AA2))
  (segment (start 225.9 93.75) (end 225.9 92.65) (width 0.45) (layer F.Cu) (net 2) (tstamp 61931AA3))
  (segment (start 225.9 93.75) (end 226.5 93.75) (width 0.45) (layer F.Cu) (net 2) (tstamp 61931AA4))
  (via (at 225.9 94.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61931AA5))
  (segment (start 222.9485 149.209) (end 222.266 149.209) (width 0.4) (layer F.Cu) (net 2) (tstamp 618681CA))
  (via (at 222.25 149.225) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618680EF))
  (segment (start 222.266 149.209) (end 222.25 149.225) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868125))
  (via (at 222.25 154.94) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868158))
  (segment (start 221.996 155.194) (end 222.25 154.94) (width 0.4) (layer F.Cu) (net 2) (tstamp 618681EB))
  (segment (start 220.9815 155.194) (end 221.996 155.194) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868119))
  (segment (start 222.3215 155.0115) (end 222.25 154.94) (width 0.4) (layer F.Cu) (net 2) (tstamp 618681EE))
  (segment (start 222.9485 155.0115) (end 222.3215 155.0115) (width 0.4) (layer F.Cu) (net 2) (tstamp 618681A6))
  (segment (start 208.2165 159.069) (end 208.2165 160.0835) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868191))
  (via (at 207.899 160.274) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618680CB))
  (segment (start 208.026 160.274) (end 207.899 160.274) (width 0.4) (layer F.Cu) (net 2) (tstamp 618680CE))
  (segment (start 208.2165 160.0835) (end 208.026 160.274) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868104))
  (segment (start 207.5815 159.069) (end 207.5815 160.0835) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868131))
  (segment (start 207.772 160.274) (end 207.899 160.274) (width 0.4) (layer F.Cu) (net 2) (tstamp 618680E0))
  (segment (start 207.5815 160.0835) (end 207.772 160.274) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186814F))
  (segment (start 208.2165 159.069) (end 208.2165 158.0515) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186812B))
  (via (at 207.899 157.861) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868146))
  (segment (start 208.026 157.861) (end 207.899 157.861) (width 0.4) (layer F.Cu) (net 2) (tstamp 618681E2))
  (segment (start 208.2165 158.0515) (end 208.026 157.861) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186811C))
  (segment (start 207.5815 159.069) (end 207.5815 158.0515) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186810A))
  (segment (start 207.772 157.861) (end 207.899 157.861) (width 0.4) (layer F.Cu) (net 2) (tstamp 618680FB))
  (segment (start 207.5815 158.0515) (end 207.772 157.861) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186818B))
  (segment (start 207.5815 132.269) (end 207.5815 133.2865) (width 0.4) (layer F.Cu) (net 2) (tstamp 618681DF))
  (via (at 207.8355 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868170))
  (segment (start 208.2165 132.269) (end 208.2165 133.2865) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868263))
  (segment (start 208.2165 132.269) (end 208.2165 131.2545) (width 0.4) (layer F.Cu) (net 2) (tstamp 618682BA))
  (via (at 207.8355 131.064) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868236))
  (via (at 192.913 135.128) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868257))
  (segment (start 192.897 135.144) (end 192.913 135.128) (width 0.5) (layer F.Cu) (net 2) (tstamp 618682C9))
  (segment (start 192.2145 135.144) (end 192.897 135.144) (width 0.5) (layer F.Cu) (net 2) (tstamp 618682B1))
  (via (at 192.913 149.86) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618681FA))
  (segment (start 192.897 149.844) (end 192.913 149.86) (width 0.5) (layer F.Cu) (net 2) (tstamp 6186822D))
  (segment (start 192.2145 149.844) (end 192.897 149.844) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868302))
  (via (at 222.3135 135.128) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868299))
  (segment (start 222.3295 135.144) (end 222.3135 135.128) (width 0.5) (layer F.Cu) (net 2) (tstamp 618682BD))
  (segment (start 223.012 135.144) (end 222.3295 135.144) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868293))
  (via (at 219.71 154.94) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868215))
  (segment (start 219.964 155.194) (end 219.71 154.94) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868287))
  (segment (start 220.9815 155.194) (end 219.964 155.194) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868251))
  (via (at 203.3905 131.0005) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868218))
  (segment (start 203.4065 130.9845) (end 203.3905 131.0005) (width 0.5) (layer F.Cu) (net 2) (tstamp 6186825A))
  (segment (start 203.4065 130.302) (end 203.4065 130.9845) (width 0.5) (layer F.Cu) (net 2) (tstamp 618682FC))
  (via (at 211.1375 131.0005) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6186828A))
  (segment (start 211.1215 130.9845) (end 211.1375 131.0005) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868209))
  (segment (start 211.1215 130.302) (end 211.1215 130.9845) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186833B))
  (via (at 192.913 156.5275) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6186826C))
  (segment (start 192.897 156.5115) (end 192.913 156.5275) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868326))
  (segment (start 192.2145 156.5115) (end 192.897 156.5115) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868248))
  (via (at 205.4225 160.3375) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618682D5))
  (segment (start 205.4065 160.3535) (end 205.4225 160.3375) (width 0.5) (layer F.Cu) (net 2) (tstamp 618682D2))
  (segment (start 205.4065 161.036) (end 205.4065 160.3535) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868317))
  (via (at 210.3755 160.3375) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618682AE))
  (segment (start 210.1215 160.0835) (end 210.3755 160.3375) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186821E))
  (segment (start 210.1215 159.069) (end 210.1215 160.0835) (width 0.4) (layer F.Cu) (net 2) (tstamp 618682FF))
  (segment (start 210.304 160.409) (end 210.3755 160.3375) (width 0.5) (layer F.Cu) (net 2) (tstamp 6186823C))
  (segment (start 210.304 161.036) (end 210.304 160.409) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868206))
  (via (at 213.0425 160.3375) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6186820F))
  (segment (start 213.0345 160.3455) (end 213.0425 160.3375) (width 0.5) (layer F.Cu) (net 2) (tstamp 6186832F))
  (segment (start 213.0345 161.036) (end 213.0345 160.3455) (width 0.5) (layer F.Cu) (net 2) (tstamp 618682A8))
  (via (at 210.3755 157.7975) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868269))
  (segment (start 210.1215 158.0515) (end 210.3755 157.7975) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868278))
  (segment (start 210.1215 159.069) (end 210.1215 158.0515) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186820C))
  (via (at 196.977 122.682) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61871416))
  (segment (start 195.7815 122.682) (end 196.977 122.682) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713B6))
  (via (at 196.977 123.952) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713EF))
  (segment (start 195.7815 123.952) (end 196.977 123.952) (width 0.5) (layer F.Cu) (net 2) (tstamp 6187141F))
  (via (at 196.977 121.412) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713E0))
  (segment (start 195.7815 121.412) (end 196.977 121.412) (width 0.5) (layer F.Cu) (net 2) (tstamp 6187140D))
  (via (at 196.977 120.142) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713B3))
  (segment (start 195.7815 120.142) (end 196.977 120.142) (width 0.5) (layer F.Cu) (net 2) (tstamp 61871401))
  (via (at 196.977 118.872) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713FB))
  (segment (start 195.7815 118.872) (end 196.977 118.872) (width 0.5) (layer F.Cu) (net 2) (tstamp 61871422))
  (via (at 194.564 118.872) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713F8))
  (segment (start 195.7815 118.872) (end 194.564 118.872) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713D4))
  (via (at 194.564 120.142) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6187142B))
  (segment (start 195.7815 120.142) (end 194.564 120.142) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713DD))
  (via (at 194.564 121.412) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713CB))
  (segment (start 195.7815 121.412) (end 194.564 121.412) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713E9))
  (via (at 194.564 122.682) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713E3))
  (segment (start 195.7815 122.682) (end 194.564 122.682) (width 0.5) (layer F.Cu) (net 2) (tstamp 61871413))
  (via (at 194.564 123.952) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61871425))
  (segment (start 195.7815 123.952) (end 194.564 123.952) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713F5))
  (segment (start 195.7705 123.963) (end 195.7705 124.6505) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713B9))
  (via (at 195.7705 124.6505) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713FE))
  (segment (start 195.7815 123.952) (end 195.7705 123.963) (width 0.5) (layer F.Cu) (net 2) (tstamp 61871419))
  (via (at 196.977 106.172) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713CE))
  (segment (start 195.7815 106.172) (end 196.977 106.172) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713EC))
  (via (at 194.564 106.172) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713E6))
  (segment (start 195.7815 106.172) (end 194.564 106.172) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713C2))
  (via (at 208.8515 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713C5))
  (segment (start 208.8515 101.992) (end 208.8515 103.1875) (width 0.5) (layer F.Cu) (net 2) (tstamp 61871407))
  (via (at 208.8515 100.7745) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6187142E))
  (segment (start 208.8515 101.992) (end 208.8515 100.7745) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713BC))
  (via (at 199.9615 124.3965) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713D7))
  (segment (start 199.9615 125.592) (end 199.9615 124.3965) (width 0.5) (layer F.Cu) (net 2) (tstamp 61871428))
  (via (at 199.9615 126.8095) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61871410))
  (segment (start 199.9615 125.592) (end 199.9615 126.8095) (width 0.5) (layer F.Cu) (net 2) (tstamp 6187140A))
  (via (at 202.5015 124.3965) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713C8))
  (segment (start 202.5015 125.592) (end 202.5015 124.3965) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713F2))
  (via (at 202.5015 126.8095) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61871431))
  (segment (start 202.5015 125.592) (end 202.5015 126.8095) (width 0.5) (layer F.Cu) (net 2) (tstamp 6187141C))
  (via (at 208.8515 124.3965) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618713BF))
  (segment (start 208.8515 125.592) (end 208.8515 124.3965) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713DA))
  (via (at 208.8515 126.8095) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61871404))
  (segment (start 208.8515 125.592) (end 208.8515 126.8095) (width 0.5) (layer F.Cu) (net 2) (tstamp 618713D1))
  (via (at 220.599 120.142) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6187133E))
  (segment (start 219.3815 120.142) (end 220.599 120.142) (width 0.5) (layer F.Cu) (net 2) (tstamp 61871335))
  (via (at 218.186 120.142) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61871338))
  (segment (start 219.3815 120.142) (end 218.186 120.142) (width 0.5) (layer F.Cu) (net 2) (tstamp 6187132F))
  (via (at 220.599 106.172) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6187133B))
  (segment (start 219.3815 106.172) (end 220.599 106.172) (width 0.5) (layer F.Cu) (net 2) (tstamp 61871344))
  (via (at 218.186 106.172) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61871332))
  (segment (start 219.3815 106.172) (end 218.186 106.172) (width 0.5) (layer F.Cu) (net 2) (tstamp 61871341))
  (segment (start 223.639 155.0115) (end 223.647 155.0035) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868083))
  (via (at 223.647 155.0035) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868089))
  (segment (start 222.9485 155.0115) (end 223.639 155.0115) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868086))
  (via (at 223.647 149.225) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868068))
  (segment (start 223.631 149.209) (end 223.647 149.225) (width 0.5) (layer F.Cu) (net 2) (tstamp 6186804D))
  (segment (start 222.9485 149.209) (end 223.631 149.209) (width 0.5) (layer F.Cu) (net 2) (tstamp 6186805F))
  (via (at 223.7105 135.128) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868062))
  (segment (start 223.6945 135.144) (end 223.7105 135.128) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868065))
  (segment (start 223.012 135.144) (end 223.6945 135.144) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868056))
  (via (at 203.3905 129.6035) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868095))
  (segment (start 203.4065 129.6195) (end 203.3905 129.6035) (width 0.5) (layer F.Cu) (net 2) (tstamp 6186809E))
  (segment (start 203.4065 130.302) (end 203.4065 129.6195) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868098))
  (segment (start 211.1215 129.6195) (end 211.1375 129.6035) (width 0.5) (layer F.Cu) (net 2) (tstamp 6186805C))
  (via (at 211.1375 129.6035) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868059))
  (segment (start 211.1215 130.302) (end 211.1215 129.6195) (width 0.5) (layer F.Cu) (net 2) (tstamp 61868053))
  (via (at 205.4225 161.7345) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 205.4065 161.7185) (end 205.4225 161.7345) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 205.4065 161.036) (end 205.4065 161.7185) (width 0.5) (layer F.Cu) (net 2))
  (via (at 191.516 149.86) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 191.532 149.844) (end 191.516 149.86) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 192.2145 149.844) (end 191.532 149.844) (width 0.5) (layer F.Cu) (net 2))
  (via (at 198.247 96.5835) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617C1B60))
  (segment (start 198.231 96.5995) (end 198.247 96.5835) (width 0.5) (layer F.Cu) (net 2) (tstamp 617C1B5D))
  (segment (start 198.231 97.282) (end 198.231 96.5995) (width 0.5) (layer F.Cu) (net 2) (tstamp 617C1B5A))
  (via (at 207.3275 129.6035) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 207.3115 129.6195) (end 207.3275 129.6035) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 207.3115 130.302) (end 207.3115 129.6195) (width 0.5) (layer F.Cu) (net 2))
  (via (at 207.8 82.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE33))
  (segment (start 208.5 82.7) (end 207.8 82.7) (width 0.5) (layer F.Cu) (net 2) (tstamp 6189FE34))
  (segment (start 208.5 79.9) (end 207.8 79.9) (width 0.45) (layer F.Cu) (net 2) (tstamp 6189FE39))
  (via (at 207.8 79.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE3A))
  (segment (start 207.95 76.2) (end 207.75 76.4) (width 0.5) (layer F.Cu) (net 2) (tstamp 6189FE3B))
  (segment (start 207.75 76.4) (end 207.75 76.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 6189FE40))
  (via (at 207.75 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE44))
  (segment (start 206.6 81.3) (end 207.75 81.3) (width 0.45) (layer F.Cu) (net 2) (tstamp 6189FE45))
  (segment (start 206.6 81.3) (end 205.45 81.3) (width 0.45) (layer F.Cu) (net 2) (tstamp 6189FE46))
  (via (at 205.45 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE47))
  (segment (start 208.5 86.3) (end 207.8 86.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 6189FE48))
  (via (at 209.2 86.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE49))
  (segment (start 208.5 86.3) (end 209.2 86.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 6189FE4A))
  (via (at 207.8 86.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE4B))
  (segment (start 208.5 82.7) (end 209.2 82.7) (width 0.5) (layer F.Cu) (net 2) (tstamp 6189FE5A))
  (via (at 209.2 82.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE5B))
  (via (at 207.8 65.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618F122A))
  (segment (start 208.5 65.5) (end 207.8 65.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 618F1227))
  (via (at 209.2 79.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE61))
  (via (at 209.2 76.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE62))
  (segment (start 208.5 79.9) (end 209.2 79.9) (width 0.5) (layer F.Cu) (net 2) (tstamp 6189FE63))
  (segment (start 208.5 65.5) (end 209.2 65.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 618F1221))
  (via (at 209.2 65.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618F121E))
  (segment (start 208.5 76.2) (end 209.2 76.2) (width 0.5) (layer F.Cu) (net 2) (tstamp 6189FE66))
  (segment (start 208.5 76.2) (end 207.95 76.2) (width 0.5) (layer F.Cu) (net 2) (tstamp 6189FE6A))
  (via (at 207.75 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE6B))
  (via (at 205.45 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6189FE6C))
  (segment (start 206.6 76.5) (end 207.75 76.5) (width 0.45) (layer F.Cu) (net 2) (tstamp 6189FE6D))
  (segment (start 206.6 76.5) (end 205.45 76.5) (width 0.45) (layer F.Cu) (net 2) (tstamp 6189FE6E))
  (via (at 211.65 74.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 212.8 74.9) (end 211.65 74.9) (width 0.5) (layer F.Cu) (net 2))
  (via (at 213.95 74.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 212.8 74.9) (end 213.95 74.9) (width 0.5) (layer F.Cu) (net 2))
  (via (at 211.65 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A06EA))
  (segment (start 212.8 78.9) (end 211.65 78.9) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A06EB))
  (via (at 213.95 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A06EC))
  (segment (start 212.8 78.9) (end 213.95 78.9) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A06ED))
  (segment (start 212.8 83.7) (end 211.65 83.7) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A0702))
  (via (at 213.95 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A0703))
  (via (at 211.65 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A0704))
  (segment (start 212.8 83.7) (end 213.95 83.7) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A0705))
  (via (at 213.95 85.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A070E))
  (segment (start 212.8 85.3) (end 213.95 85.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A070F))
  (via (at 211.65 85.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A0710))
  (segment (start 212.8 85.3) (end 211.65 85.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A0711))
  (segment (start 212.8 64.5) (end 213.95 64.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A0716))
  (via (at 213.95 64.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A0719))
  (via (at 211.6 77.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 210.9 77.5) (end 211.6 77.5) (width 0.5) (layer F.Cu) (net 2))
  (via (at 210.2 77.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 210.9 77.5) (end 210.2 77.5) (width 0.5) (layer F.Cu) (net 2))
  (via (at 211.6 82.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 210.9 82.3) (end 211.6 82.3) (width 0.5) (layer F.Cu) (net 2))
  (via (at 210.2 82.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 210.9 82.3) (end 210.2 82.3) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 195.1 78.9) (end 196.25 78.9) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E05))
  (via (at 193.95 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E06))
  (segment (start 195.1 64.5) (end 193.95 64.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E07))
  (via (at 196.25 78.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E0B))
  (segment (start 195.1 85.3) (end 196.25 85.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E0C))
  (segment (start 195.1 78.9) (end 193.95 78.9) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E0F))
  (via (at 196.25 85.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E10))
  (segment (start 195.1 64.5) (end 196.25 64.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E11))
  (via (at 196.25 64.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E12))
  (via (at 193.95 64.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E14))
  (segment (start 193.2 82.3) (end 193.9 82.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E15))
  (via (at 193.9 82.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E16))
  (via (at 192.5 77.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E18))
  (segment (start 193.2 77.5) (end 192.5 77.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E19))
  (via (at 196.25 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E1E))
  (segment (start 195.1 83.7) (end 196.25 83.7) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E20))
  (via (at 196.25 74.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E21))
  (segment (start 195.1 74.9) (end 196.25 74.9) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E22))
  (via (at 193.95 83.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E23))
  (segment (start 195.1 74.9) (end 193.95 74.9) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E24))
  (via (at 193.95 74.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E25))
  (segment (start 195.1 83.7) (end 193.95 83.7) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E26))
  (via (at 193.9 77.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E29))
  (segment (start 193.2 82.3) (end 192.5 82.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E2A))
  (via (at 192.5 82.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618A2E2B))
  (segment (start 193.2 77.5) (end 193.9 77.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 618A2E2C))
  (via (at 225.45 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC26))
  (via (at 223.15 76.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC27))
  (segment (start 224.3 76.5) (end 225.45 76.5) (width 0.45) (layer F.Cu) (net 2) (tstamp 618DDC28))
  (segment (start 224.3 76.5) (end 223.15 76.5) (width 0.45) (layer F.Cu) (net 2) (tstamp 618DDC29))
  (segment (start 226.2 82.7) (end 225.5 82.7) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC33))
  (via (at 225.5 82.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC34))
  (segment (start 226.2 79.9) (end 225.5 79.9) (width 0.45) (layer F.Cu) (net 2) (tstamp 618DDC38))
  (via (at 225.5 79.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC39))
  (segment (start 225.65 76.2) (end 225.45 76.4) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC3A))
  (segment (start 225.45 76.4) (end 225.45 76.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC3F))
  (via (at 225.45 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC43))
  (segment (start 224.3 81.3) (end 225.45 81.3) (width 0.45) (layer F.Cu) (net 2) (tstamp 618DDC44))
  (segment (start 224.3 81.3) (end 223.15 81.3) (width 0.45) (layer F.Cu) (net 2) (tstamp 618DDC45))
  (via (at 223.15 81.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC46))
  (segment (start 226.2 86.3) (end 225.5 86.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC47))
  (via (at 226.9 86.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC48))
  (segment (start 226.2 86.3) (end 226.9 86.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC49))
  (via (at 225.5 86.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC4A))
  (segment (start 226.2 82.7) (end 226.9 82.7) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC59))
  (via (at 226.9 82.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC5A))
  (via (at 225.5 65.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC5C))
  (segment (start 226.2 65.5) (end 225.5 65.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC5D))
  (via (at 226.9 79.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC5F))
  (via (at 226.9 76.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618DDC60))
  (segment (start 226.2 79.9) (end 226.9 79.9) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC61))
  (segment (start 226.2 76.2) (end 226.9 76.2) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC62))
  (segment (start 226.2 76.2) (end 225.65 76.2) (width 0.5) (layer F.Cu) (net 2) (tstamp 618DDC65))
  (via (at 226.9 65.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 226.2 65.5) (end 226.9 65.5) (width 0.5) (layer F.Cu) (net 2))
  (via (at 212.8 63.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 212.8 64.5) (end 212.8 63.9) (width 0.45) (layer F.Cu) (net 2))
  (via (at 223.52 122.936) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 223.536 122.952) (end 223.52 122.936) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 224.2185 122.952) (end 223.536 122.952) (width 0.5) (layer F.Cu) (net 2))
  (via (at 195.1 85.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 195.1 85.3) (end 195.1 85.9) (width 0.5) (layer F.Cu) (net 2))
  (via (at 193.95 85.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 194.05 85.3) (end 193.95 85.2) (width 0.45) (layer F.Cu) (net 2))
  (segment (start 195.1 85.3) (end 194.05 85.3) (width 0.45) (layer F.Cu) (net 2))
  (via (at 218.186 127.254) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61A75103))
  (via (at 196.65 55.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AE510A))
  (segment (start 197.35 55.55) (end 196.65 55.55) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AE5122))
  (via (at 198.05 55.4) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AE5104))
  (segment (start 197.35 58.9) (end 198.05 58.9) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AE5110))
  (via (at 198.05 58.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AE511C))
  (segment (start 197.35 40.3) (end 198.05 40.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AE50E9))
  (via (at 198.05 40.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AE512B))
  (segment (start 197.35 40.3) (end 196.65 40.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AE5128))
  (via (at 196.65 40.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AE50F8))
  (segment (start 207.05 61.3) (end 207.05 60.6) (width 0.5) (layer F.Cu) (net 2) (tstamp 6178EF19))
  (via (at 207.05 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6178EF1F))
  (via (at 207.05 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6178EF25))
  (segment (start 207.05 61.3) (end 207.05 62) (width 0.5) (layer F.Cu) (net 2) (tstamp 6178EF22))
  (segment (start 202.85 61.3) (end 202.85 60.6) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3495))
  (via (at 202.85 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC34D4))
  (segment (start 202.85 61.3) (end 202.85 62) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3492))
  (via (at 202.85 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC34C8))
  (segment (start 198.95 61.3) (end 198.95 62) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC34A4))
  (via (at 198.95 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC34EF))
  (via (at 217.25 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC34D1))
  (via (at 198.95 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC352B))
  (segment (start 198.95 61.3) (end 198.95 60.6) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC34C2))
  (via (at 217.25 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC3516))
  (segment (start 217.25 61.3) (end 217.25 62) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3522))
  (segment (start 217.25 61.3) (end 217.25 60.6) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC34B6))
  (via (at 220.55 59.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC3309))
  (segment (start 219.85 41.3) (end 220.55 41.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3315))
  (via (at 220.55 41.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC331B))
  (segment (start 219.85 44.55) (end 220.55 44.55) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC333C))
  (via (at 219.15 59.8) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC3342))
  (segment (start 219.85 44.55) (end 219.15 44.55) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3348))
  (via (at 219.15 56.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC3357))
  (via (at 219.15 41.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC335A))
  (via (at 220.55 56.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC3363))
  (segment (start 219.85 59.8) (end 219.15 59.8) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3369))
  (segment (start 219.85 41.3) (end 219.15 41.3) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3372))
  (via (at 219.15 44.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC3378))
  (segment (start 219.85 59.8) (end 220.55 59.8) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3381))
  (via (at 220.55 44.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC3390))
  (segment (start 219.85 56.55) (end 219.15 56.55) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3393))
  (segment (start 219.85 56.55) (end 220.55 56.55) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3396))
  (segment (start 215.1 38.8) (end 215.1 38.1) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC34E3))
  (segment (start 215.1 38.8) (end 215.1 39.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC34BF))
  (via (at 203.1 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC34E0))
  (segment (start 218.35 38.8) (end 218.35 38.1) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC33E7))
  (via (at 203.1 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC341D))
  (segment (start 199.85 38.8) (end 199.85 39.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3408))
  (segment (start 218.35 38.8) (end 218.35 39.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC343B))
  (via (at 215.1 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC33F0))
  (via (at 199.85 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC342C))
  (via (at 215.1 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC3426))
  (segment (start 203.1 38.8) (end 203.1 39.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC33ED))
  (via (at 218.35 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC3402))
  (segment (start 203.1 38.8) (end 203.1 38.1) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC33F9))
  (via (at 199.85 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC345C))
  (segment (start 199.85 38.8) (end 199.85 38.1) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AC3459))
  (via (at 218.35 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AC344A))
  (via (at 200.6 42.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 201.1 42.55) (end 200.6 42.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 206.6 43.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 207.1 43.55) (end 206.6 43.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 211.6 43.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 211.1 43.55) (end 211.6 43.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 216.6 42.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 216.1 42.55) (end 216.6 42.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 213.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 213.1 45.55) (end 213.6 45.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 203.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 204.1 45.55) (end 203.6 45.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 201.6 47.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 202.1 47.55) (end 201.6 47.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 207.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 208.1 46.55) (end 207.6 46.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 204.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 205.1 49.55) (end 204.6 49.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 207.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 208.1 49.55) (end 207.6 49.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 210.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 210.1 49.55) (end 210.6 49.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 209.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 209.1 50.55) (end 209.6 51.05) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 212.1 50.55) (end 212.6 51.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 212.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (via (at 210.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AD3517))
  (segment (start 210.1 51.55) (end 210.6 52.05) (width 0.4) (layer F.Cu) (net 2) (tstamp 61AD3518))
  (via (at 215.6 53.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AD351B))
  (segment (start 215.1 52.55) (end 215.6 53.05) (width 0.4) (layer F.Cu) (net 2) (tstamp 61AD351C))
  (via (at 214.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AD351F))
  (segment (start 214.1 55.55) (end 214.6 56.05) (width 0.4) (layer F.Cu) (net 2) (tstamp 61AD3520))
  (segment (start 216.1 57.55) (end 216.6 58.05) (width 0.4) (layer F.Cu) (net 2) (tstamp 61AD3523))
  (via (at 216.6 58.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AD3524))
  (segment (start 211.1 56.55) (end 211.6 57.05) (width 0.4) (layer F.Cu) (net 2) (tstamp 61AD3527))
  (via (at 211.6 57.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AD3528))
  (segment (start 207.1 56.55) (end 206.6 57.05) (width 0.4) (layer F.Cu) (net 2) (tstamp 61AD3872))
  (via (at 206.6 57.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AD3873))
  (via (at 203.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AD3880))
  (segment (start 204.1 54.55) (end 203.6 55.05) (width 0.4) (layer F.Cu) (net 2) (tstamp 61AD3881))
  (segment (start 201.1 57.55) (end 200.6 58.05) (width 0.4) (layer F.Cu) (net 2) (tstamp 61AD3884))
  (via (at 200.6 58.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AD3885))
  (segment (start 202.1 51.55) (end 201.6 52.05) (width 0.4) (layer F.Cu) (net 2) (tstamp 61AD3888))
  (via (at 201.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AD3889))
  (segment (start 207.1 50.55) (end 206.6 51.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 206.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (via (at 215.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 215.1 48.55) (end 215.6 48.05) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 209.1 53.55) (end 209.6 54.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 209.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (via (at 207.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 208.1 51.55) (end 207.6 52.05) (width 0.4) (layer F.Cu) (net 2))
  (via (at 198.05 43.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AE5113))
  (segment (start 197.35 43.55) (end 198.05 43.55) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AE50F2))
  (segment (start 197.35 43.55) (end 196.65 43.55) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AE5116))
  (via (at 196.65 43.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AE50FE))
  (via (at 190.119 69.246) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61737E08))
  (via (at 197.35 58.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 197.35 58.9) (end 197.35 58.15) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 197.9 55.55) (end 198.05 55.4) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 197.35 55.55) (end 197.9 55.55) (width 0.5) (layer F.Cu) (net 2))
  (via (at 208.6 59.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61792938))
  (via (at 205.2955 96.5835) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 205.3115 96.5995) (end 205.2955 96.5835) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 205.3115 97.282) (end 205.3115 96.5995) (width 0.5) (layer F.Cu) (net 2))
  (via (at 205.2955 97.9805) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 205.3115 97.9645) (end 205.2955 97.9805) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 205.3115 97.282) (end 205.3115 97.9645) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 208.5815 96.5995) (end 208.5975 96.5835) (width 0.5) (layer F.Cu) (net 2))
  (via (at 208.5975 96.5835) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 208.5815 97.282) (end 208.5815 96.5995) (width 0.5) (layer F.Cu) (net 2))
  (via (at 208.5975 97.9805) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 208.5815 97.9645) (end 208.5975 97.9805) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 208.5815 97.282) (end 208.5815 97.9645) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 198.231 97.282) (end 198.231 97.9645) (width 0.5) (layer F.Cu) (net 2) (tstamp 617C1B51))
  (segment (start 198.231 97.9645) (end 198.247 97.9805) (width 0.5) (layer F.Cu) (net 2) (tstamp 617C1B54))
  (via (at 198.247 97.9805) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617C1B57))
  (via (at 218.3765 97.9805) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 218.3925 97.9645) (end 218.3765 97.9805) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 218.3925 97.282) (end 218.3925 97.9645) (width 0.5) (layer F.Cu) (net 2))
  (via (at 218.3765 96.5835) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 218.3925 96.5995) (end 218.3765 96.5835) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 218.3925 97.282) (end 218.3925 96.5995) (width 0.5) (layer F.Cu) (net 2))
  (via (at 220.599 108.077) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617D599E))
  (via (at 220.599 109.347) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617D5E3E))
  (via (at 220.599 110.617) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617D5E40))
  (via (at 220.599 111.887) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617D5E42))
  (via (at 220.599 113.157) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617D5E44))
  (via (at 220.599 114.427) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617D5E46))
  (via (at 220.599 115.697) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617D5E48))
  (via (at 220.599 116.967) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617D5E4A))
  (via (at 220.599 118.237) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 617E4793))
  (via (at 222.1865 151.384) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6186829F))
  (segment (start 220.9815 151.384) (end 222.1865 151.384) (width 0.4) (layer F.Cu) (net 2) (tstamp 618682AB))
  (via (at 219.7735 151.384) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868224))
  (segment (start 220.9815 151.384) (end 219.7735 151.384) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868242))
  (via (at 222.1865 145.034) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618682E1))
  (segment (start 220.9815 145.034) (end 222.1865 145.034) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868200))
  (via (at 219.7735 145.034) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6186824E))
  (segment (start 220.9815 145.034) (end 219.7735 145.034) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186828D))
  (via (at 222.1865 139.319) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868281))
  (segment (start 220.9815 139.319) (end 222.1865 139.319) (width 0.4) (layer F.Cu) (net 2) (tstamp 618681FD))
  (via (at 219.7735 139.319) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618682E7))
  (segment (start 220.9815 139.319) (end 219.7735 139.319) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868230))
  (via (at 195.3895 139.319) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868128))
  (segment (start 194.1815 139.319) (end 195.3895 139.319) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868176))
  (via (at 192.9765 139.319) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618681B8))
  (segment (start 194.1815 139.319) (end 192.9765 139.319) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186817C))
  (via (at 195.3895 142.494) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618681F7))
  (segment (start 194.1815 142.494) (end 195.3895 142.494) (width 0.4) (layer F.Cu) (net 2) (tstamp 618681C4))
  (via (at 192.9765 142.494) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868122))
  (segment (start 194.1815 142.494) (end 192.9765 142.494) (width 0.4) (layer F.Cu) (net 2) (tstamp 618680D4))
  (via (at 195.3895 145.669) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618681F1))
  (segment (start 194.1815 145.669) (end 195.3895 145.669) (width 0.4) (layer F.Cu) (net 2) (tstamp 618680E9))
  (via (at 192.9765 145.669) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868149))
  (segment (start 194.1815 145.669) (end 192.9765 145.669) (width 0.4) (layer F.Cu) (net 2) (tstamp 618680F5))
  (via (at 195.3895 152.019) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618680BF))
  (segment (start 194.1815 152.019) (end 195.3895 152.019) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868173))
  (via (at 192.9765 152.019) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868167))
  (segment (start 194.1815 152.019) (end 192.9765 152.019) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868110))
  (via (at 214.0585 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618682C3))
  (via (at 214.0585 131.064) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61868329))
  (via (at 201.2315 131.064) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618681CD))
  (segment (start 201.2315 132.269) (end 201.2315 131.064) (width 0.4) (layer F.Cu) (net 2) (tstamp 618681DC))
  (segment (start 201.2315 132.269) (end 201.2315 133.477) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868113))
  (via (at 201.2315 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6186811F))
  (via (at 201.2315 160.274) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618681A9))
  (segment (start 201.2315 159.069) (end 201.2315 160.274) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868137))
  (via (at 201.2315 157.861) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6186819A))
  (segment (start 201.2315 159.069) (end 201.2315 157.861) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186815B))
  (via (at 214.0585 160.274) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618681B5))
  (via (at 213.9315 157.861) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 618680C8))
  (segment (start 213.9315 159.069) (end 213.9315 157.861) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868134))
  (segment (start 213.9315 160.147) (end 214.0585 160.274) (width 0.4) (layer F.Cu) (net 2) (tstamp 6186827B))
  (segment (start 213.9315 159.069) (end 213.9315 160.147) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868335))
  (via (at 213.0425 161.7345) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 213.0345 161.7265) (end 213.0425 161.7345) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 213.0345 161.036) (end 213.0345 161.7265) (width 0.5) (layer F.Cu) (net 2))
  (via (at 210.312 161.7345) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 210.304 161.7265) (end 210.312 161.7345) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 210.304 161.036) (end 210.304 161.7265) (width 0.5) (layer F.Cu) (net 2))
  (via (at 216.154 163.195) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 6196822F))
  (via (at 229.5 162.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 228.4 162.15) (end 229.5 162.15) (width 0.45) (layer F.Cu) (net 2))
  (via (at 227.3 162.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 228.4 162.15) (end 227.3 162.15) (width 0.45) (layer F.Cu) (net 2))
  (via (at 228.4 162.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 228.4 162.15) (end 228.4 162.75) (width 0.45) (layer F.Cu) (net 2))
  (via (at 232.65 155) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 233.3 155) (end 232.65 155) (width 0.45) (layer F.Cu) (net 2))
  (via (at 224.917 122.936) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 224.901 122.952) (end 224.917 122.936) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 224.2185 122.952) (end 224.901 122.952) (width 0.5) (layer F.Cu) (net 2))
  (via (at 211.3915 157.0355) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 211.3915 159.069) (end 211.3915 157.0355) (width 0.15) (layer F.Cu) (net 2))
  (via (at 191.516 156.5275) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 191.532 156.5115) (end 191.516 156.5275) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 192.2145 156.5115) (end 191.532 156.5115) (width 0.5) (layer F.Cu) (net 2))
  (via (at 190.119 155.194) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61963B19))
  (via (at 208.28 163.195) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61968234))
  (via (at 217.05 94.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61931A99))
  (via (at 210.55 72.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 619DDFA6))
  (segment (start 207.5815 132.269) (end 207.5815 131.2545) (width 0.4) (layer F.Cu) (net 2) (tstamp 61868296))
  (segment (start 207.772 131.064) (end 207.8355 131.064) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 207.5815 131.2545) (end 207.772 131.064) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 208.026 131.064) (end 208.2165 131.2545) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 207.8355 131.064) (end 208.026 131.064) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 207.772 133.477) (end 207.8355 133.477) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 207.5815 133.2865) (end 207.772 133.477) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 208.026 133.477) (end 207.8355 133.477) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 208.2165 133.2865) (end 208.026 133.477) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 213.9315 133.35) (end 214.0585 133.477) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 213.9315 132.269) (end 213.9315 133.35) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 213.9315 131.191) (end 214.0585 131.064) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 213.9315 132.269) (end 213.9315 131.191) (width 0.4) (layer F.Cu) (net 2))
  (via (at 212.09 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (via (at 208.915 135.9535) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61A40B55))
  (segment (start 212.0265 133.4135) (end 212.0265 132.269) (width 0.4) (layer F.Cu) (net 2))
  (segment (start 212.09 133.477) (end 212.0265 133.4135) (width 0.4) (layer F.Cu) (net 2))
  (via (at 219.15 51.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AA5A3E))
  (via (at 220.55 51.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AA5A40))
  (via (at 218.3 50.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AA5A43))
  (via (at 220.55 48.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AA5A44))
  (segment (start 219.85 48.5) (end 220.55 48.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AA5A45))
  (via (at 219.15 48.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AA5A46))
  (segment (start 219.85 48.5) (end 219.15 48.5) (width 0.5) (layer F.Cu) (net 2) (tstamp 61AA5A4A))
  (segment (start 219.15 51.6) (end 219.85 51.6) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 219.85 51.6) (end 220.55 51.6) (width 0.5) (layer F.Cu) (net 2))
  (via (at 208.6 40.35) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AB4A32))
  (via (at 198.9 50.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2) (tstamp 61AB4AEB))
  (via (at 210.15 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 210.15 38.8) (end 210.15 39.5) (width 0.5) (layer F.Cu) (net 2))
  (via (at 210.15 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 210.15 38.8) (end 210.15 38.1) (width 0.5) (layer F.Cu) (net 2))
  (via (at 207.05 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 207.05 38.8) (end 207.05 38.1) (width 0.5) (layer F.Cu) (net 2))
  (via (at 207.05 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 207.05 38.8) (end 207.05 39.5) (width 0.5) (layer F.Cu) (net 2))
  (via (at 196.65 51.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 197.35 51.6) (end 196.65 51.6) (width 0.5) (layer F.Cu) (net 2))
  (via (at 198.05 51.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 197.35 51.6) (end 198.05 51.6) (width 0.5) (layer F.Cu) (net 2))
  (via (at 196.65 48.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 197.35 48.5) (end 196.65 48.5) (width 0.5) (layer F.Cu) (net 2))
  (via (at 198.05 48.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 197.35 48.5) (end 198.05 48.5) (width 0.5) (layer F.Cu) (net 2))
  (via (at 196.4055 129.6035) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 196.4215 129.6195) (end 196.4055 129.6035) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 196.4215 130.302) (end 196.4215 129.6195) (width 0.5) (layer F.Cu) (net 2))
  (via (at 196.4055 131.0005) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 196.4215 130.9845) (end 196.4055 131.0005) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 196.4215 130.302) (end 196.4215 130.9845) (width 0.5) (layer F.Cu) (net 2))
  (via (at 195.7705 130.302) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 2))
  (segment (start 196.4215 130.302) (end 195.7705 130.302) (width 0.5) (layer F.Cu) (net 2))
  (segment (start 234.3 155) (end 234.3 154.3) (width 0.5) (layer F.Cu) (net 3) (tstamp 618815FD))
  (via (at 234.3 154.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61881604))
  (via (at 234.3 155.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 6188160A))
  (segment (start 234.3 155.7) (end 234.3 155) (width 0.5) (layer F.Cu) (net 3) (tstamp 6188160D))
  (segment (start 234.3 156.3) (end 234.3 155.7) (width 0.45) (layer F.Cu) (net 3) (tstamp 6188161F))
  (segment (start 203.85 61.3) (end 203.85 62) (width 0.5) (layer F.Cu) (net 3) (tstamp 61AC34CE))
  (via (at 203.85 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AC34AA))
  (segment (start 213.05 61.3) (end 213.05 60.6) (width 0.5) (layer F.Cu) (net 3) (tstamp 61AC34E9))
  (via (at 213.05 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AC3498))
  (segment (start 213.05 61.3) (end 213.05 62) (width 0.5) (layer F.Cu) (net 3) (tstamp 61AC34F5))
  (via (at 213.05 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AC34B0))
  (via (at 209.6 43.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3))
  (segment (start 209.1 43.55) (end 209.6 43.05) (width 0.4) (layer F.Cu) (net 3))
  (via (at 210.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD4885))
  (segment (start 210.1 45.55) (end 210.6 45.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD4886))
  (segment (start 213.1 43.55) (end 213.6 43.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD4889))
  (via (at 213.6 43.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD488A))
  (segment (start 215.1 45.55) (end 215.6 45.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD488D))
  (via (at 215.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD488E))
  (via (at 203.6 43.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD4891))
  (segment (start 204.1 43.55) (end 203.6 43.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD4892))
  (segment (start 207.1 45.55) (end 206.6 45.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD4897))
  (via (at 206.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD4898))
  (segment (start 202.1 45.55) (end 201.6 45.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD489B))
  (via (at 201.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD489C))
  (via (at 205.6 47.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD489F))
  (segment (start 206.1 47.55) (end 205.6 47.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48A0))
  (via (at 201.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48A3))
  (segment (start 202.1 49.55) (end 201.6 49.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48A4))
  (segment (start 213.1 48.55) (end 213.6 48.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48A7))
  (via (at 213.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48A8))
  (via (at 211.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48B1))
  (segment (start 211.1 49.55) (end 211.6 49.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48B2))
  (segment (start 209.1 48.55) (end 209.6 48.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48B5))
  (via (at 209.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48B6))
  (segment (start 207.1 48.55) (end 206.6 48.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48B9))
  (via (at 206.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48BA))
  (via (at 203.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48BF))
  (segment (start 204.1 48.55) (end 203.6 48.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48C0))
  (via (at 205.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48C3))
  (segment (start 206.1 50.55) (end 205.6 51.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48C4))
  (segment (start 204.1 51.55) (end 203.6 52.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48C9))
  (via (at 203.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48CA))
  (via (at 207.6 53.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48CD))
  (segment (start 208.1 52.55) (end 207.6 53.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48CE))
  (segment (start 211.1 52.55) (end 211.6 53.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48D1))
  (via (at 211.6 53.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48D2))
  (segment (start 213.1 51.55) (end 213.6 52.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48D7))
  (via (at 213.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48D8))
  (via (at 215.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48DB))
  (segment (start 215.1 50.55) (end 215.6 51.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48DC))
  (segment (start 215.1 54.55) (end 215.6 55.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48DF))
  (via (at 215.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48E0))
  (via (at 213.6 57.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48E3))
  (segment (start 213.1 56.55) (end 213.6 57.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48E4))
  (via (at 210.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48E7))
  (segment (start 210.1 54.55) (end 210.6 55.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48E8))
  (via (at 209.6 57.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48EB))
  (segment (start 209.1 56.55) (end 209.6 57.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48EC))
  (segment (start 207.1 54.55) (end 206.6 55.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48EF))
  (via (at 206.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48F0))
  (via (at 204.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48FD))
  (segment (start 205.1 53.55) (end 204.6 54.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48FE))
  (via (at 201.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD4901))
  (segment (start 202.1 54.55) (end 201.6 55.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD4902))
  (segment (start 213.6 60.05) (end 213.05 60.6) (width 0.3) (layer F.Cu) (net 3))
  (segment (start 213.6 57.05) (end 213.6 60.05) (width 0.3) (layer F.Cu) (net 3))
  (segment (start 203.85 61.3) (end 203.85 60.6) (width 0.5) (layer F.Cu) (net 3) (tstamp 61AC34A1))
  (via (at 203.85 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AC34F2))
  (segment (start 204.1 56.55) (end 203.6 57.05) (width 0.4) (layer F.Cu) (net 3) (tstamp 61AD48FA))
  (via (at 203.6 57.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3) (tstamp 61AD48F9))
  (segment (start 203.6 60.35) (end 203.85 60.6) (width 0.3) (layer F.Cu) (net 3))
  (segment (start 203.6 57.05) (end 203.6 60.35) (width 0.3) (layer F.Cu) (net 3))
  (via (at 233.2 156.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3))
  (segment (start 234.3 156.3) (end 233.2 156.3) (width 0.45) (layer F.Cu) (net 3))
  (via (at 235.4 156.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 3))
  (segment (start 234.3 156.3) (end 235.4 156.3) (width 0.45) (layer F.Cu) (net 3))
  (via (at 229.5 156.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 4) (tstamp 618BEEEE))
  (segment (start 228.4 156.95) (end 229.5 156.95) (width 0.15) (layer F.Cu) (net 4) (tstamp 618BEEED))
  (segment (start 213.0425 122.428) (end 216.9795 122.428) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 212.0265 127.762) (end 212.0265 123.444) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 212.9155 128.016) (end 212.2805 128.016) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 213.2965 127.635) (end 212.9155 128.016) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 214.0585 123.19) (end 213.2965 123.952) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 212.0265 123.444) (end 213.0425 122.428) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 212.2805 128.016) (end 212.0265 127.762) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 216.4715 124.079) (end 215.5825 123.19) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 213.2965 123.952) (end 213.2965 127.635) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 215.5825 123.19) (end 214.0585 123.19) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 216.4715 125.592) (end 216.4715 124.079) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 216.9795 122.428) (end 217.8685 123.317) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 217.8685 123.317) (end 221.4245 123.317) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 221.4245 123.317) (end 223.2025 121.539) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 223.2025 121.539) (end 223.9645 121.539) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 228.4 158.25) (end 229.5 158.25) (width 0.15) (layer F.Cu) (net 5) (tstamp 618BEEEC))
  (via (at 229.5 158.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 5) (tstamp 618BEEEB))
  (via (at 206.4385 151.0665) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 5))
  (segment (start 208.661 153.289) (end 206.4385 151.0665) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 220.9815 153.289) (end 208.661 153.289) (width 0.15) (layer F.Cu) (net 5))
  (segment (start 213.614 146.6215) (end 221.6785 138.557) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 221.6785 138.557) (end 221.6785 130.302) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 210.8835 146.6215) (end 213.614 146.6215) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 206.4385 151.0665) (end 210.8835 146.6215) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 221.6785 130.302) (end 221.6785 128.2065) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 221.6785 128.2065) (end 222.3135 127.5715) (width 0.15) (layer B.Cu) (net 5))
  (segment (start 222.3135 127.5715) (end 222.3135 120.65) (width 0.15) (layer B.Cu) (net 5))
  (via (at 207.55 91.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 28))
  (segment (start 217.7415 132.269) (end 217.7415 131.318) (width 0.15) (layer F.Cu) (net 29))
  (segment (start 217.7415 131.318) (end 218.5035 130.556) (width 0.15) (layer F.Cu) (net 29))
  (segment (start 218.5035 130.556) (end 222.6945 130.556) (width 0.15) (layer F.Cu) (net 29))
  (segment (start 217.1065 132.269) (end 217.1065 131.318) (width 0.15) (layer F.Cu) (net 30))
  (segment (start 217.1065 131.318) (end 218.186 130.2385) (width 0.15) (layer F.Cu) (net 30))
  (segment (start 218.186 130.2385) (end 222.3135 130.2385) (width 0.15) (layer F.Cu) (net 30))
  (segment (start 216.4715 132.269) (end 216.4715 131.318) (width 0.15) (layer F.Cu) (net 31))
  (segment (start 216.4715 131.318) (end 217.8685 129.921) (width 0.15) (layer F.Cu) (net 31))
  (segment (start 217.8685 129.921) (end 222.25 129.921) (width 0.15) (layer F.Cu) (net 31))
  (via (at 232.4 162.15) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 31))
  (segment (start 234.3 162.15) (end 232.4 162.15) (width 0.15) (layer F.Cu) (net 31))
  (segment (start 230.25 162.15) (end 229.7 161.6) (width 0.15) (layer B.Cu) (net 31))
  (segment (start 229.7 161.6) (end 225.6 161.6) (width 0.15) (layer B.Cu) (net 31))
  (segment (start 232.4 162.15) (end 230.25 162.15) (width 0.15) (layer B.Cu) (net 31))
  (segment (start 234.3 160.85) (end 232.4 160.85) (width 0.15) (layer F.Cu) (net 32) (tstamp 618C2B8D))
  (via (at 232.4 160.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 32) (tstamp 618C2B8E))
  (segment (start 215.8365 132.269) (end 215.8365 131.318) (width 0.15) (layer F.Cu) (net 32))
  (segment (start 215.8365 131.318) (end 217.551 129.6035) (width 0.15) (layer F.Cu) (net 32))
  (segment (start 217.551 129.6035) (end 222.25 129.6035) (width 0.15) (layer F.Cu) (net 32))
  (segment (start 229.75 160.35) (end 226.1 160.35) (width 0.15) (layer B.Cu) (net 32))
  (segment (start 230.25 160.85) (end 229.75 160.35) (width 0.15) (layer B.Cu) (net 32))
  (segment (start 232.4 160.85) (end 230.25 160.85) (width 0.15) (layer B.Cu) (net 32))
  (segment (start 234.3 159.55) (end 232.4 159.55) (width 0.15) (layer F.Cu) (net 33) (tstamp 618C2B93))
  (via (at 232.4 159.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 33) (tstamp 618C2B94))
  (segment (start 217.2335 129.286) (end 222.25 129.286) (width 0.15) (layer F.Cu) (net 33))
  (segment (start 215.2015 131.318) (end 217.2335 129.286) (width 0.15) (layer F.Cu) (net 33))
  (segment (start 215.2015 132.269) (end 215.2015 131.318) (width 0.15) (layer F.Cu) (net 33))
  (segment (start 229.75 159.05) (end 226.95 159.05) (width 0.15) (layer B.Cu) (net 33))
  (segment (start 230.25 159.55) (end 229.75 159.05) (width 0.15) (layer B.Cu) (net 33))
  (segment (start 232.4 159.55) (end 230.25 159.55) (width 0.15) (layer B.Cu) (net 33))
  (segment (start 234.3 158.25) (end 232.4 158.25) (width 0.15) (layer F.Cu) (net 34) (tstamp 618C2B99))
  (via (at 232.4 158.25) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 34) (tstamp 618C2B9A))
  (segment (start 214.5665 132.269) (end 214.5665 129.794) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 214.5665 129.794) (end 217.1065 127.254) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 217.1065 127.254) (end 217.1065 124.079) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 217.1065 124.079) (end 215.8365 122.809) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 215.8365 122.809) (end 213.5505 122.809) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 212.6615 123.698) (end 212.6615 125.592) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 213.5505 122.809) (end 212.6615 123.698) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 214.8205 133.858) (end 218.186 133.858) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 218.186 133.858) (end 220.091 131.953) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 214.5665 133.604) (end 214.8205 133.858) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 214.5665 132.269) (end 214.5665 133.604) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 220.091 131.953) (end 220.472 131.572) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 220.472 131.572) (end 222.5675 131.572) (width 0.15) (layer F.Cu) (net 34))
  (segment (start 229.75 157.75) (end 228.15 157.75) (width 0.15) (layer B.Cu) (net 34))
  (segment (start 230.25 158.25) (end 229.75 157.75) (width 0.15) (layer B.Cu) (net 34))
  (segment (start 232.4 158.25) (end 230.25 158.25) (width 0.15) (layer B.Cu) (net 34))
  (segment (start 228.15 157.75) (end 227.8 157.75) (width 0.15) (layer B.Cu) (net 34))
  (segment (start 213.9315 123.952) (end 213.9315 125.592) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 214.3125 123.571) (end 213.9315 123.952) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 215.4555 123.571) (end 214.3125 123.571) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 215.8365 123.952) (end 215.4555 123.571) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 213.2965 130.556) (end 215.8365 128.016) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 215.8365 128.016) (end 215.8365 123.952) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 213.2965 132.269) (end 213.2965 130.556) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 213.2965 132.269) (end 213.2965 133.5405) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 213.2965 133.5405) (end 213.9315 134.1755) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 213.9315 134.1755) (end 218.313 134.1755) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 218.313 134.1755) (end 220.4085 132.08) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 220.4085 132.08) (end 220.599 131.8895) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 220.599 131.8895) (end 222.377 131.8895) (width 0.15) (layer F.Cu) (net 35))
  (segment (start 228.4 160.85) (end 229.5 160.85) (width 0.15) (layer F.Cu) (net 35))
  (via (at 229.5 160.85) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 35))
  (segment (start 212.6615 132.269) (end 212.6615 130.683) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 215.2015 128.143) (end 215.2015 125.592) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 212.6615 130.683) (end 215.2015 128.143) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 220.726 132.207) (end 222.377 132.207) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 212.6615 132.269) (end 212.6615 133.35) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 218.44 134.493) (end 220.726 132.207) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 213.8045 134.493) (end 218.44 134.493) (width 0.15) (layer F.Cu) (net 36))
  (segment (start 212.6615 133.35) (end 213.8045 134.493) (width 0.15) (layer F.Cu) (net 36))
  (via (at 229.5 159.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 36) (tstamp 618BEEE5))
  (segment (start 228.4 159.55) (end 229.5 159.55) (width 0.15) (layer F.Cu) (net 36) (tstamp 618BEEE6))
  (segment (start 209.4865 129.794) (end 209.4865 132.269) (width 0.15) (layer F.Cu) (net 38))
  (segment (start 208.28 128.5875) (end 209.4865 129.794) (width 0.15) (layer F.Cu) (net 38))
  (segment (start 201.803 128.5875) (end 208.28 128.5875) (width 0.15) (layer F.Cu) (net 38))
  (segment (start 201.2315 128.016) (end 201.803 128.5875) (width 0.15) (layer F.Cu) (net 38))
  (segment (start 201.2315 125.592) (end 201.2315 128.016) (width 0.15) (layer F.Cu) (net 38))
  (segment (start 200.66 128.5875) (end 201.2315 128.016) (width 0.15) (layer F.Cu) (net 38))
  (segment (start 196.9135 128.5875) (end 200.66 128.5875) (width 0.15) (layer F.Cu) (net 38))
  (via (at 196.9135 128.5875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 38))
  (via (at 206.9465 134.3025) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 39))
  (segment (start 206.9465 132.269) (end 206.9465 134.3025) (width 0.15) (layer F.Cu) (net 39))
  (segment (start 205.486 131.953) (end 200.5965 131.953) (width 0.15) (layer B.Cu) (net 39))
  (segment (start 206.9465 133.4135) (end 205.486 131.953) (width 0.15) (layer B.Cu) (net 39))
  (segment (start 206.9465 134.3025) (end 206.9465 133.4135) (width 0.15) (layer B.Cu) (net 39))
  (via (at 206.3115 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 40))
  (segment (start 206.3115 132.269) (end 206.3115 133.477) (width 0.15) (layer F.Cu) (net 40))
  (segment (start 205.359 132.2705) (end 200.5965 132.2705) (width 0.15) (layer B.Cu) (net 40))
  (segment (start 206.3115 133.223) (end 205.359 132.2705) (width 0.15) (layer B.Cu) (net 40))
  (segment (start 206.3115 133.477) (end 206.3115 133.223) (width 0.15) (layer B.Cu) (net 40))
  (via (at 205.6765 134.3025) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 41))
  (segment (start 205.6765 132.269) (end 205.6765 134.3025) (width 0.15) (layer F.Cu) (net 41))
  (segment (start 205.232 132.588) (end 200.5965 132.588) (width 0.15) (layer B.Cu) (net 41))
  (segment (start 205.6765 133.0325) (end 205.232 132.588) (width 0.15) (layer B.Cu) (net 41))
  (segment (start 205.6765 134.3025) (end 205.6765 133.0325) (width 0.15) (layer B.Cu) (net 41))
  (via (at 194.15 92.65) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 44) (tstamp 61935598))
  (segment (start 200.5965 156.9085) (end 198.882 155.194) (width 0.15) (layer F.Cu) (net 46))
  (segment (start 200.5965 159.069) (end 200.5965 156.9085) (width 0.15) (layer F.Cu) (net 46))
  (via (at 198.882 155.194) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 46))
  (segment (start 190.627 156.7815) (end 190.627 154.1145) (width 0.15) (layer B.Cu) (net 46))
  (segment (start 191.897 158.0515) (end 190.627 156.7815) (width 0.15) (layer B.Cu) (net 46))
  (segment (start 196.0245 158.0515) (end 191.897 158.0515) (width 0.15) (layer B.Cu) (net 46))
  (segment (start 198.882 155.194) (end 196.0245 158.0515) (width 0.15) (layer B.Cu) (net 46))
  (segment (start 203.7715 159.069) (end 203.7715 156.2735) (width 0.15) (layer F.Cu) (net 47))
  (via (at 200.025 154.1145) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 47))
  (segment (start 201.6125 154.1145) (end 200.025 154.1145) (width 0.15) (layer F.Cu) (net 47))
  (segment (start 203.7715 156.2735) (end 201.6125 154.1145) (width 0.15) (layer F.Cu) (net 47))
  (segment (start 191.008 156.718) (end 191.008 154.2415) (width 0.15) (layer B.Cu) (net 47))
  (segment (start 191.643 157.353) (end 191.008 156.718) (width 0.15) (layer B.Cu) (net 47))
  (segment (start 196.0245 157.353) (end 191.643 157.353) (width 0.15) (layer B.Cu) (net 47))
  (segment (start 199.263 154.1145) (end 196.0245 157.353) (width 0.15) (layer B.Cu) (net 47))
  (segment (start 200.025 154.1145) (end 199.263 154.1145) (width 0.15) (layer B.Cu) (net 47))
  (segment (start 205.0415 155.956) (end 201.7395 152.654) (width 0.15) (layer F.Cu) (net 48))
  (segment (start 205.0415 159.069) (end 205.0415 155.956) (width 0.15) (layer F.Cu) (net 48))
  (via (at 201.7395 152.654) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 48))
  (segment (start 192.024 155.6385) (end 192.024 155.321) (width 0.15) (layer B.Cu) (net 48))
  (segment (start 192.024 155.321) (end 191.3255 154.6225) (width 0.15) (layer B.Cu) (net 48))
  (segment (start 192.405 156.0195) (end 192.024 155.6385) (width 0.15) (layer B.Cu) (net 48))
  (segment (start 191.3255 154.6225) (end 191.3255 152.908) (width 0.15) (layer B.Cu) (net 48))
  (segment (start 193.1035 156.0195) (end 192.405 156.0195) (width 0.15) (layer B.Cu) (net 48))
  (segment (start 194.1195 157.0355) (end 193.1035 156.0195) (width 0.15) (layer B.Cu) (net 48))
  (segment (start 200.279 152.654) (end 195.8975 157.0355) (width 0.15) (layer B.Cu) (net 48))
  (segment (start 195.8975 157.0355) (end 194.1195 157.0355) (width 0.15) (layer B.Cu) (net 48))
  (segment (start 201.7395 152.654) (end 200.279 152.654) (width 0.15) (layer B.Cu) (net 48))
  (segment (start 205.6765 154.4955) (end 202.819 151.638) (width 0.15) (layer F.Cu) (net 49))
  (segment (start 205.6765 159.069) (end 205.6765 154.4955) (width 0.15) (layer F.Cu) (net 49))
  (via (at 202.819 151.638) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 49))
  (segment (start 192.151 155.0035) (end 191.643 154.4955) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 193.167 155.0035) (end 192.151 155.0035) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 193.4845 155.321) (end 193.167 155.0035) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 194.2465 156.718) (end 193.4845 155.956) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 195.7705 156.718) (end 194.2465 156.718) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 193.4845 155.956) (end 193.4845 155.321) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 200.8505 151.638) (end 195.7705 156.718) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 191.643 154.4955) (end 191.643 152.9715) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 202.819 151.638) (end 200.8505 151.638) (width 0.15) (layer B.Cu) (net 49))
  (segment (start 206.3115 153.162) (end 203.581 150.4315) (width 0.15) (layer F.Cu) (net 50))
  (segment (start 206.3115 159.069) (end 206.3115 153.162) (width 0.15) (layer F.Cu) (net 50))
  (via (at 203.581 150.4315) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 50))
  (segment (start 191.9605 154.3685) (end 191.9605 152.781) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 192.278 154.686) (end 191.9605 154.3685) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 193.294 154.686) (end 192.278 154.686) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 193.802 155.194) (end 193.294 154.686) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 193.802 155.829) (end 193.802 155.194) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 194.3735 156.4005) (end 193.802 155.829) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 195.6435 156.4005) (end 194.3735 156.4005) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 201.6125 150.4315) (end 195.6435 156.4005) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 203.581 150.4315) (end 201.6125 150.4315) (width 0.15) (layer B.Cu) (net 50))
  (segment (start 196.9135 162.6235) (end 190.627 156.337) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 190.627 100.203) (end 190.627 64.135) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 210.185 162.6235) (end 196.9135 162.6235) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 190.627 156.337) (end 190.627 100.203) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 211.0105 160.2994) (end 211.0105 161.798) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 211.0105 161.798) (end 210.185 162.6235) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 210.7565 160.0454) (end 211.0105 160.2994) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 210.7565 159.069) (end 210.7565 160.0454) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 196.1 45.6) (end 198.35 45.6) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 195.5 45) (end 196.1 45.6) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 194.85 45) (end 195.5 45) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 191.65 49.1) (end 191.65 51.45) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 193.25 47.5) (end 191.65 49.1) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 193.25 45) (end 193.25 47.5) (width 0.15) (layer F.Cu) (net 51))
  (segment (start 225.044 111.5695) (end 228.219 108.3945) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 225.044 119.38) (end 225.044 111.5695) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 228.219 108.3945) (end 232.6005 108.3945) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 224.282 120.142) (end 225.044 119.38) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 222.5675 120.142) (end 224.282 120.142) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 221.2975 121.412) (end 222.5675 120.142) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 219.3815 121.412) (end 221.2975 121.412) (width 0.15) (layer F.Cu) (net 54))
  (segment (start 196.05 45.1) (end 198.4 45.1) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 195.8 44.85) (end 196.05 45.1) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 195.55 43.5) (end 195.8 43.75) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 195.8 43.75) (end 195.8 44.85) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 194.85 43.5) (end 195.55 43.5) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 190.6 45.45) (end 190.6 52.2) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 192.55 43.5) (end 190.6 45.45) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 193.25 43.5) (end 192.55 43.5) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 198.6915 125.592) (end 198.6915 121.158) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 197.0405 119.507) (end 194.5005 119.507) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 194.5005 119.507) (end 191.35 116.3565) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 198.6915 121.158) (end 197.0405 119.507) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 191.35 116.3565) (end 191.35 62.289) (width 0.15) (layer F.Cu) (net 56))
  (segment (start 195.7815 117.602) (end 198.0565 117.602) (width 0.15) (layer F.Cu) (net 57))
  (segment (start 199.8 57.7) (end 199.8 58.95) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 200.95 56.55) (end 199.8 57.7) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 201.1 56.55) (end 200.95 56.55) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 199.8 58.95) (end 200.8 59.95) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 200.8 59.95) (end 200.8 61.85) (width 0.15) (layer F.Cu) (net 58))
  (segment (start 199.2 57.35) (end 199.2 59.25) (width 0.15) (layer F.Cu) (net 59))
  (segment (start 201 55.55) (end 199.2 57.35) (width 0.15) (layer F.Cu) (net 59))
  (segment (start 201.1 55.55) (end 201 55.55) (width 0.15) (layer F.Cu) (net 59))
  (segment (start 198.9 59.75) (end 197.2 61.45) (width 0.15) (layer F.Cu) (net 60))
  (segment (start 198.9 57.1375) (end 198.9 59.75) (width 0.15) (layer F.Cu) (net 60))
  (segment (start 201.1 54.9375) (end 198.9 57.1375) (width 0.15) (layer F.Cu) (net 60))
  (segment (start 201.1 54.55) (end 201.1 54.9375) (width 0.15) (layer F.Cu) (net 60))
  (segment (start 196.9 57.2) (end 196.45 57.65) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 197.95 57.2) (end 196.9 57.2) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 198.8 56.35) (end 197.95 57.2) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 200.675 53.55) (end 198.8 55.425) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 198.8 55.425) (end 198.8 56.35) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 201.1 53.55) (end 200.675 53.55) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 196.45 57.65) (end 196.45 59.55) (width 0.15) (layer F.Cu) (net 61))
  (segment (start 195.85 54.75) (end 195.85 59.15) (width 0.15) (layer F.Cu) (net 62))
  (segment (start 196.2 54.4) (end 195.85 54.75) (width 0.15) (layer F.Cu) (net 62))
  (segment (start 198.95 54.4) (end 196.2 54.4) (width 0.15) (layer F.Cu) (net 62))
  (segment (start 200.8 52.55) (end 198.95 54.4) (width 0.15) (layer F.Cu) (net 62))
  (segment (start 201.1 52.55) (end 200.8 52.55) (width 0.15) (layer F.Cu) (net 62))
  (segment (start 195.55 54.6) (end 195.55 58.7) (width 0.15) (layer F.Cu) (net 63))
  (segment (start 196.05 54.1) (end 195.55 54.6) (width 0.15) (layer F.Cu) (net 63))
  (segment (start 198.8 54.1) (end 196.05 54.1) (width 0.15) (layer F.Cu) (net 63))
  (segment (start 201.1 51.8) (end 198.8 54.1) (width 0.15) (layer F.Cu) (net 63))
  (segment (start 201.1 51.55) (end 201.1 51.8) (width 0.15) (layer F.Cu) (net 63))
  (segment (start 194.95 54.3) (end 194.95 58.65) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 195.75 53.5) (end 194.95 54.3) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 198.05 53.5) (end 195.75 53.5) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 201 50.55) (end 198.05 53.5) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 201.1 50.55) (end 201 50.55) (width 0.15) (layer F.Cu) (net 64))
  (segment (start 194.65 48.8) (end 194.65 58.45) (width 0.15) (layer F.Cu) (net 65))
  (segment (start 196.45 47) (end 194.65 48.8) (width 0.15) (layer F.Cu) (net 65))
  (segment (start 198.55 47.35) (end 198.2 47) (width 0.15) (layer F.Cu) (net 65))
  (segment (start 201.1 49.55) (end 200.1 49.55) (width 0.15) (layer F.Cu) (net 65))
  (segment (start 200.1 49.55) (end 198.55 48) (width 0.15) (layer F.Cu) (net 65))
  (segment (start 198.2 47) (end 196.45 47) (width 0.15) (layer F.Cu) (net 65))
  (segment (start 198.55 48) (end 198.55 47.35) (width 0.15) (layer F.Cu) (net 65))
  (segment (start 193.9 49.1) (end 193.9 58.05) (width 0.15) (layer F.Cu) (net 66))
  (segment (start 198.35 46.7) (end 196.3 46.7) (width 0.15) (layer F.Cu) (net 66))
  (segment (start 199.65 48.55) (end 198.9 47.8) (width 0.15) (layer F.Cu) (net 66))
  (segment (start 198.9 47.25) (end 198.35 46.7) (width 0.15) (layer F.Cu) (net 66))
  (segment (start 198.9 47.8) (end 198.9 47.25) (width 0.15) (layer F.Cu) (net 66))
  (segment (start 196.3 46.7) (end 193.9 49.1) (width 0.15) (layer F.Cu) (net 66))
  (segment (start 201.1 48.55) (end 199.65 48.55) (width 0.15) (layer F.Cu) (net 66))
  (segment (start 192.4 49.6) (end 192.4 56.25) (width 0.15) (layer F.Cu) (net 67))
  (segment (start 195.9 46.1) (end 192.4 49.6) (width 0.15) (layer F.Cu) (net 67))
  (segment (start 198.65 46.1) (end 195.9 46.1) (width 0.15) (layer F.Cu) (net 67))
  (segment (start 200.1 47.55) (end 198.65 46.1) (width 0.15) (layer F.Cu) (net 67))
  (segment (start 201.1 47.55) (end 200.1 47.55) (width 0.15) (layer F.Cu) (net 67))
  (segment (start 201.1 46.55) (end 199.6 46.55) (width 0.15) (layer F.Cu) (net 68))
  (segment (start 201.1 45.55) (end 199.6 45.55) (width 0.15) (layer F.Cu) (net 69))
  (segment (start 201.1 44.55) (end 199.6 44.55) (width 0.15) (layer F.Cu) (net 70))
  (segment (start 201.1 43.55) (end 199.6 43.55) (width 0.15) (layer F.Cu) (net 71))
  (segment (start 202.1 57.55) (end 202.1 58.9) (width 0.15) (layer F.Cu) (net 72))
  (segment (start 202.1 58.9) (end 202.1 59.75) (width 0.15) (layer F.Cu) (net 72))
  (segment (start 202.1 59.75) (end 201.7 60.15) (width 0.15) (layer F.Cu) (net 72))
  (segment (start 201.7 60.15) (end 201.7 61.7) (width 0.15) (layer F.Cu) (net 72))
  (segment (start 203.1 57.55) (end 203.1 59) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 203.1 59) (end 203.1 59.65) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 203.1 59.65) (end 202.3 60.45) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 202.3 60.45) (end 202.3 62.05) (width 0.15) (layer F.Cu) (net 73))
  (segment (start 204.1 57.55) (end 204.1 59.55) (width 0.15) (layer F.Cu) (net 74))
  (segment (start 204.1 59.55) (end 204.4 59.85) (width 0.15) (layer F.Cu) (net 74))
  (segment (start 204.4 59.85) (end 204.4 62.05) (width 0.15) (layer F.Cu) (net 74))
  (segment (start 205.1 59.6) (end 205 59.7) (width 0.15) (layer F.Cu) (net 75))
  (segment (start 205.1 57.55) (end 205.1 59.6) (width 0.15) (layer F.Cu) (net 75))
  (segment (start 205 59.7) (end 205 62) (width 0.15) (layer F.Cu) (net 75))
  (segment (start 206.1 57.55) (end 206.1 58.55) (width 0.15) (layer F.Cu) (net 76))
  (segment (start 206.1 58.55) (end 206.1 59.5) (width 0.15) (layer F.Cu) (net 76))
  (segment (start 206.1 59.5) (end 205.6 60) (width 0.15) (layer F.Cu) (net 76))
  (segment (start 205.6 60) (end 205.6 62.2) (width 0.15) (layer F.Cu) (net 76))
  (segment (start 207.1 57.55) (end 207.1 58.55) (width 0.15) (layer F.Cu) (net 77))
  (segment (start 207.1 58.55) (end 207.1 58.95) (width 0.15) (layer F.Cu) (net 77))
  (segment (start 207.1 58.95) (end 205.9 60.15) (width 0.15) (layer F.Cu) (net 77))
  (segment (start 205.9 60.15) (end 205.9 62.1) (width 0.15) (layer F.Cu) (net 77))
  (segment (start 208.1 57.55) (end 208.1 58.55) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 208.1 58.55) (end 208.1 58.85) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 208.1 58.85) (end 206.5 60.45) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 206.5 60.45) (end 206.5 62.1) (width 0.15) (layer F.Cu) (net 78))
  (segment (start 209.1 57.55) (end 209.1 58.55) (width 0.15) (layer F.Cu) (net 79))
  (segment (start 209.1 58.55) (end 209.1 58.85) (width 0.15) (layer F.Cu) (net 79))
  (segment (start 209.1 58.85) (end 210.7 60.45) (width 0.15) (layer F.Cu) (net 79))
  (segment (start 210.7 60.45) (end 210.7 62) (width 0.15) (layer F.Cu) (net 79))
  (segment (start 202.1 42.55) (end 202.1 41.55) (width 0.15) (layer F.Cu) (net 80))
  (segment (start 202.1 43.55) (end 202.1 43.3) (width 0.15) (layer F.Cu) (net 81))
  (segment (start 202.1 43.3) (end 201.6 42.8) (width 0.15) (layer F.Cu) (net 81))
  (segment (start 201.6 42.8) (end 201.6 41.55) (width 0.15) (layer F.Cu) (net 81))
  (segment (start 201.35 44.05) (end 199.6 44.05) (width 0.15) (layer F.Cu) (net 82))
  (segment (start 201.85 44.55) (end 201.35 44.05) (width 0.15) (layer F.Cu) (net 82))
  (segment (start 202.1 44.55) (end 201.85 44.55) (width 0.15) (layer F.Cu) (net 82))
  (segment (start 202.1 46.55) (end 201.6 46.05) (width 0.15) (layer F.Cu) (net 83))
  (segment (start 201.6 46.05) (end 199.6 46.05) (width 0.15) (layer F.Cu) (net 83))
  (segment (start 193.15 49.3) (end 193.15 56.8) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 196.05 46.4) (end 193.15 49.3) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 198.5 46.4) (end 196.05 46.4) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 199.2 47.1) (end 198.5 46.4) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 199.2 47.55) (end 199.2 47.1) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 199.7 48.05) (end 199.2 47.55) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 201.6 48.05) (end 199.7 48.05) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 202.1 48.55) (end 201.6 48.05) (width 0.15) (layer F.Cu) (net 84))
  (segment (start 195.25 54.45) (end 195.25 58.7) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 195.9 53.8) (end 195.25 54.45) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 198.2 53.8) (end 195.9 53.8) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 200.9 51.1) (end 198.2 53.8) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 201.55 51.1) (end 200.9 51.1) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 202.1 50.55) (end 201.55 51.1) (width 0.15) (layer F.Cu) (net 85))
  (segment (start 196.15 54.9) (end 196.15 59.2) (width 0.15) (layer F.Cu) (net 86))
  (segment (start 196.35 54.7) (end 196.15 54.9) (width 0.15) (layer F.Cu) (net 86))
  (segment (start 201.6 53.05) (end 200.75 53.05) (width 0.15) (layer F.Cu) (net 86))
  (segment (start 200.75 53.05) (end 199.1 54.7) (width 0.15) (layer F.Cu) (net 86))
  (segment (start 199.1 54.7) (end 196.35 54.7) (width 0.15) (layer F.Cu) (net 86))
  (segment (start 202.1 52.55) (end 201.6 53.05) (width 0.15) (layer F.Cu) (net 86))
  (segment (start 196.75 57.9) (end 196.75 59.45) (width 0.15) (layer F.Cu) (net 87))
  (segment (start 197.15 57.5) (end 196.75 57.9) (width 0.15) (layer F.Cu) (net 87))
  (segment (start 198.1 57.5) (end 197.15 57.5) (width 0.15) (layer F.Cu) (net 87))
  (segment (start 199.95 55.65) (end 198.1 57.5) (width 0.15) (layer F.Cu) (net 87))
  (segment (start 199.95 55.05) (end 199.95 55.65) (width 0.15) (layer F.Cu) (net 87))
  (segment (start 200.95 54.05) (end 199.95 55.05) (width 0.15) (layer F.Cu) (net 87))
  (segment (start 201.6 54.05) (end 200.95 54.05) (width 0.15) (layer F.Cu) (net 87))
  (segment (start 202.1 53.55) (end 201.6 54.05) (width 0.15) (layer F.Cu) (net 87))
  (segment (start 202.1 56.8) (end 201.6 57.3) (width 0.15) (layer F.Cu) (net 88))
  (segment (start 201.6 57.3) (end 201.6 59.6) (width 0.15) (layer F.Cu) (net 88))
  (segment (start 202.1 56.55) (end 202.1 56.8) (width 0.15) (layer F.Cu) (net 88))
  (segment (start 201.6 59.6) (end 201.4 59.8) (width 0.15) (layer F.Cu) (net 88))
  (segment (start 201.4 59.8) (end 201.4 61.75) (width 0.15) (layer F.Cu) (net 88))
  (segment (start 199.5 57.5) (end 199.5 59.1) (width 0.15) (layer F.Cu) (net 89))
  (segment (start 200.95 56.05) (end 199.5 57.5) (width 0.15) (layer F.Cu) (net 89))
  (segment (start 201.35 56.05) (end 200.95 56.05) (width 0.15) (layer F.Cu) (net 89))
  (segment (start 201.85 55.55) (end 201.35 56.05) (width 0.15) (layer F.Cu) (net 89))
  (segment (start 202.1 55.55) (end 201.85 55.55) (width 0.15) (layer F.Cu) (net 89))
  (segment (start 199.5 59.1) (end 200.5 60.1) (width 0.15) (layer F.Cu) (net 89))
  (segment (start 200.5 60.1) (end 200.5 61.85) (width 0.15) (layer F.Cu) (net 89))
  (segment (start 202.6 57.05) (end 202.6 58.95) (width 0.15) (layer F.Cu) (net 90))
  (segment (start 203.1 56.55) (end 202.6 57.05) (width 0.15) (layer F.Cu) (net 90))
  (segment (start 202.6 58.95) (end 202.6 59.7) (width 0.15) (layer F.Cu) (net 90))
  (segment (start 202.6 59.7) (end 202 60.3) (width 0.15) (layer F.Cu) (net 90))
  (segment (start 202 60.3) (end 202 61.9) (width 0.15) (layer F.Cu) (net 90))
  (segment (start 201.35 57.05) (end 200.9 57.05) (width 0.15) (layer F.Cu) (net 91))
  (segment (start 201.85 56.05) (end 201.6 56.3) (width 0.15) (layer F.Cu) (net 91))
  (segment (start 200.9 57.05) (end 200.1 57.85) (width 0.15) (layer F.Cu) (net 91))
  (segment (start 201.6 56.8) (end 201.35 57.05) (width 0.15) (layer F.Cu) (net 91))
  (segment (start 200.1 57.85) (end 200.1 58.8) (width 0.15) (layer F.Cu) (net 91))
  (segment (start 202.6 56.05) (end 201.85 56.05) (width 0.15) (layer F.Cu) (net 91))
  (segment (start 201.6 56.3) (end 201.6 56.8) (width 0.15) (layer F.Cu) (net 91))
  (segment (start 203.1 55.55) (end 202.6 56.05) (width 0.15) (layer F.Cu) (net 91))
  (segment (start 200.1 58.8) (end 201.1 59.8) (width 0.15) (layer F.Cu) (net 91))
  (segment (start 201.1 59.8) (end 201.1 61.85) (width 0.15) (layer F.Cu) (net 91))
  (via (at 202.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 92))
  (segment (start 203.1 53.55) (end 202.6 54.05) (width 0.15) (layer F.Cu) (net 92))
  (segment (start 202.6 54.05) (end 202.35 54.05) (width 0.15) (layer B.Cu) (net 92))
  (segment (start 202.35 54.05) (end 202.1 54.3) (width 0.15) (layer B.Cu) (net 92))
  (segment (start 202.1 54.3) (end 201.35 54.3) (width 0.15) (layer B.Cu) (net 92))
  (segment (start 201.35 54.3) (end 199.85 55.8) (width 0.15) (layer B.Cu) (net 92))
  (via (at 202.6 53.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 93))
  (segment (start 203.1 52.55) (end 202.6 53.05) (width 0.15) (layer F.Cu) (net 93))
  (segment (start 202.6 53.05) (end 202.35 53.05) (width 0.15) (layer B.Cu) (net 93))
  (segment (start 202.35 53.05) (end 202.1 53.3) (width 0.15) (layer B.Cu) (net 93))
  (segment (start 202.1 53.3) (end 201.6 53.3) (width 0.15) (layer B.Cu) (net 93))
  (segment (start 201.6 53.3) (end 201.25 53.3) (width 0.15) (layer B.Cu) (net 93))
  (segment (start 201.25 53.3) (end 199.6 54.95) (width 0.15) (layer B.Cu) (net 93))
  (via (at 202.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 94))
  (segment (start 203.1 51.55) (end 202.6 52.05) (width 0.15) (layer F.Cu) (net 94))
  (segment (start 202.6 52.05) (end 202.35 52.05) (width 0.15) (layer B.Cu) (net 94))
  (segment (start 202.35 52.05) (end 201.85 52.55) (width 0.15) (layer B.Cu) (net 94))
  (segment (start 201.85 52.55) (end 200.85 52.55) (width 0.15) (layer B.Cu) (net 94))
  (segment (start 200.85 52.55) (end 198.6 54.8) (width 0.15) (layer B.Cu) (net 94))
  (via (at 202.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 95))
  (segment (start 203.1 50.55) (end 202.6 51.05) (width 0.15) (layer F.Cu) (net 95))
  (segment (start 202.6 51.05) (end 201.35 51.05) (width 0.15) (layer B.Cu) (net 95))
  (segment (start 201.35 51.05) (end 198.6 53.8) (width 0.15) (layer B.Cu) (net 95))
  (via (at 202.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 96))
  (segment (start 203.1 49.55) (end 202.6 49.05) (width 0.15) (layer F.Cu) (net 96))
  (segment (start 202.6 49.05) (end 202.35 49.05) (width 0.15) (layer B.Cu) (net 96))
  (segment (start 202.35 49.05) (end 201.85 48.55) (width 0.15) (layer B.Cu) (net 96))
  (segment (start 201.85 48.55) (end 200.85 48.55) (width 0.15) (layer B.Cu) (net 96))
  (segment (start 200.85 48.55) (end 200.1 47.8) (width 0.15) (layer B.Cu) (net 96))
  (via (at 203.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 97))
  (segment (start 204.1 55.55) (end 203.6 56.05) (width 0.15) (layer F.Cu) (net 97))
  (segment (start 203.6 56.05) (end 203.1 56.55) (width 0.15) (layer B.Cu) (net 97))
  (segment (start 203.1 56.55) (end 203.1 57.7) (width 0.15) (layer B.Cu) (net 97))
  (via (at 203.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 98))
  (segment (start 204.1 53.55) (end 203.6 54.05) (width 0.15) (layer F.Cu) (net 98))
  (segment (start 202.1 55.3) (end 201.1 56.3) (width 0.15) (layer B.Cu) (net 98))
  (segment (start 202.1 54.8) (end 202.1 55.3) (width 0.15) (layer B.Cu) (net 98))
  (segment (start 202.35 54.55) (end 202.1 54.8) (width 0.15) (layer B.Cu) (net 98))
  (segment (start 202.85 54.55) (end 202.35 54.55) (width 0.15) (layer B.Cu) (net 98))
  (segment (start 203.35 54.05) (end 202.85 54.55) (width 0.15) (layer B.Cu) (net 98))
  (segment (start 203.6 54.05) (end 203.35 54.05) (width 0.15) (layer B.Cu) (net 98))
  (via (at 203.6 53.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 99))
  (segment (start 204.1 52.55) (end 203.6 53.05) (width 0.15) (layer F.Cu) (net 99))
  (segment (start 203.6 53.05) (end 203.1 53.55) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 203.1 53.55) (end 202.35 53.55) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 202.35 53.55) (end 202.1 53.8) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 202.1 53.8) (end 201.35 53.8) (width 0.15) (layer B.Cu) (net 99))
  (segment (start 201.35 53.8) (end 199.6 55.55) (width 0.15) (layer B.Cu) (net 99))
  (via (at 203.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 100))
  (segment (start 204.1 50.55) (end 203.6 51.05) (width 0.15) (layer F.Cu) (net 100))
  (segment (start 203.6 51.05) (end 203.1 51.55) (width 0.15) (layer B.Cu) (net 100))
  (segment (start 203.1 51.55) (end 201.35 51.55) (width 0.15) (layer B.Cu) (net 100))
  (segment (start 201.35 51.55) (end 198.6 54.3) (width 0.15) (layer B.Cu) (net 100))
  (via (at 203.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 101))
  (segment (start 204.1 49.55) (end 203.6 49.05) (width 0.15) (layer F.Cu) (net 101))
  (segment (start 200.3 47.45) (end 198.85 47.45) (width 0.15) (layer B.Cu) (net 101))
  (segment (start 201.05 48.2) (end 200.3 47.45) (width 0.15) (layer B.Cu) (net 101))
  (segment (start 202.4 48.55) (end 202.05 48.2) (width 0.15) (layer B.Cu) (net 101))
  (segment (start 202.05 48.2) (end 201.05 48.2) (width 0.15) (layer B.Cu) (net 101))
  (segment (start 203.1 48.55) (end 202.4 48.55) (width 0.15) (layer B.Cu) (net 101))
  (segment (start 203.6 49.05) (end 203.1 48.55) (width 0.15) (layer B.Cu) (net 101))
  (segment (start 204.6 57.05) (end 204.6 59.6) (width 0.15) (layer F.Cu) (net 102))
  (segment (start 205.1 56.55) (end 204.6 57.05) (width 0.15) (layer F.Cu) (net 102))
  (segment (start 204.6 59.6) (end 204.7 59.7) (width 0.15) (layer F.Cu) (net 102))
  (segment (start 204.7 59.7) (end 204.7 62.05) (width 0.15) (layer F.Cu) (net 102))
  (via (at 204.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 103))
  (segment (start 205.1 55.55) (end 204.6 56.05) (width 0.15) (layer F.Cu) (net 103))
  (segment (start 204.6 56.05) (end 204.6 57.65) (width 0.15) (layer B.Cu) (net 103))
  (via (at 204.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 104))
  (segment (start 205.1 54.55) (end 204.6 55.05) (width 0.15) (layer F.Cu) (net 104))
  (segment (start 204.1 55.85) (end 204.1 57.7) (width 0.15) (layer B.Cu) (net 104))
  (segment (start 204.6 55.35) (end 204.1 55.85) (width 0.15) (layer B.Cu) (net 104))
  (segment (start 204.6 55.05) (end 204.6 55.35) (width 0.15) (layer B.Cu) (net 104))
  (via (at 202.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 105))
  (segment (start 203.1 48.55) (end 202.6 48.05) (width 0.15) (layer F.Cu) (net 105))
  (segment (start 200.5 47.15) (end 199.05 47.15) (width 0.15) (layer B.Cu) (net 105))
  (segment (start 201.2 47.85) (end 200.5 47.15) (width 0.15) (layer B.Cu) (net 105))
  (segment (start 202.4 47.85) (end 201.2 47.85) (width 0.15) (layer B.Cu) (net 105))
  (segment (start 202.6 48.05) (end 202.4 47.85) (width 0.15) (layer B.Cu) (net 105))
  (via (at 202.6 47.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 106))
  (segment (start 203.1 47.55) (end 202.6 47.05) (width 0.15) (layer F.Cu) (net 106))
  (segment (start 201.8 46.55) (end 199.85 46.55) (width 0.15) (layer B.Cu) (net 106))
  (segment (start 202.3 47.05) (end 201.8 46.55) (width 0.15) (layer B.Cu) (net 106))
  (segment (start 202.6 47.05) (end 202.3 47.05) (width 0.15) (layer B.Cu) (net 106))
  (via (at 203.6 47.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 107))
  (segment (start 204.1 47.55) (end 203.6 47.05) (width 0.15) (layer F.Cu) (net 107))
  (segment (start 203.6 47.05) (end 203.1 46.55) (width 0.15) (layer B.Cu) (net 107))
  (segment (start 203.1 46.55) (end 202.4 46.55) (width 0.15) (layer B.Cu) (net 107))
  (segment (start 202.4 46.55) (end 202.05 46.2) (width 0.15) (layer B.Cu) (net 107))
  (segment (start 202.05 46.2) (end 199.85 46.2) (width 0.15) (layer B.Cu) (net 107))
  (via (at 203.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 108))
  (segment (start 204.1 46.55) (end 203.6 46.05) (width 0.15) (layer F.Cu) (net 108))
  (segment (start 202.85 45.55) (end 199.85 45.55) (width 0.15) (layer B.Cu) (net 108))
  (segment (start 203.35 46.05) (end 202.85 45.55) (width 0.15) (layer B.Cu) (net 108))
  (segment (start 203.6 46.05) (end 203.35 46.05) (width 0.15) (layer B.Cu) (net 108))
  (via (at 202.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 109))
  (segment (start 203.1 46.55) (end 202.6 46.05) (width 0.15) (layer F.Cu) (net 109))
  (segment (start 202.4 45.85) (end 200.4 45.85) (width 0.15) (layer B.Cu) (net 109))
  (segment (start 202.6 46.05) (end 202.4 45.85) (width 0.15) (layer B.Cu) (net 109))
  (via (at 202.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 110))
  (segment (start 203.1 45.55) (end 202.6 45.05) (width 0.15) (layer F.Cu) (net 110))
  (segment (start 202.6 45.05) (end 202.1 44.55) (width 0.15) (layer B.Cu) (net 110))
  (segment (start 202.1 44.55) (end 200.35 44.55) (width 0.15) (layer B.Cu) (net 110))
  (segment (start 203.1 44.55) (end 202.6 44.05) (width 0.15) (layer F.Cu) (net 111))
  (segment (start 202.6 44.05) (end 201.85 44.05) (width 0.15) (layer F.Cu) (net 111))
  (segment (start 201.85 44.05) (end 201.6 43.8) (width 0.15) (layer F.Cu) (net 111))
  (segment (start 201.6 43.8) (end 201.6 43.3) (width 0.15) (layer F.Cu) (net 111))
  (segment (start 201.6 43.3) (end 201.35 43.05) (width 0.15) (layer F.Cu) (net 111))
  (segment (start 201.35 43.05) (end 199.6 43.05) (width 0.15) (layer F.Cu) (net 111))
  (via (at 203.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 112))
  (segment (start 204.1 44.55) (end 203.6 44.05) (width 0.15) (layer F.Cu) (net 112))
  (segment (start 203.6 44.05) (end 203.1 43.55) (width 0.15) (layer B.Cu) (net 112))
  (segment (start 203.1 43.55) (end 203.1 41.8) (width 0.15) (layer B.Cu) (net 112))
  (segment (start 203.1 43.55) (end 202.6 43.05) (width 0.15) (layer F.Cu) (net 113))
  (segment (start 202.6 43.05) (end 202.6 41.55) (width 0.15) (layer F.Cu) (net 113))
  (segment (start 204.1 42.55) (end 204.1 41.55) (width 0.15) (layer F.Cu) (net 114))
  (segment (start 203.1 42.55) (end 203.1 41.55) (width 0.15) (layer F.Cu) (net 115))
  (via (at 204.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 116))
  (segment (start 205.1 45.55) (end 204.6 45.05) (width 0.15) (layer F.Cu) (net 116))
  (segment (start 204.1 44.3) (end 204.1 42.05) (width 0.15) (layer B.Cu) (net 116))
  (segment (start 204.6 44.8) (end 204.1 44.3) (width 0.15) (layer B.Cu) (net 116))
  (segment (start 204.6 45.05) (end 204.6 44.8) (width 0.15) (layer B.Cu) (net 116))
  (via (at 205.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 117))
  (segment (start 206.1 45.55) (end 205.6 45.05) (width 0.15) (layer F.Cu) (net 117))
  (segment (start 205.6 45.05) (end 205.1 44.55) (width 0.15) (layer B.Cu) (net 117))
  (segment (start 205.1 44.55) (end 205.1 41.8) (width 0.15) (layer B.Cu) (net 117))
  (via (at 206.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 118))
  (segment (start 207.1 44.55) (end 206.6 44.05) (width 0.15) (layer F.Cu) (net 118))
  (segment (start 206.6 44.05) (end 206.6 43.9) (width 0.15) (layer B.Cu) (net 118))
  (segment (start 206.6 43.9) (end 207.1 43.4) (width 0.15) (layer B.Cu) (net 118))
  (segment (start 207.1 43.4) (end 207.1 41.6) (width 0.15) (layer B.Cu) (net 118))
  (via (at 205.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 119))
  (segment (start 206.1 44.55) (end 205.6 44.05) (width 0.15) (layer F.Cu) (net 119))
  (segment (start 205.6 44.05) (end 205.6 41.55) (width 0.15) (layer B.Cu) (net 119))
  (via (at 204.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 120))
  (segment (start 205.1 44.55) (end 204.6 44.05) (width 0.15) (layer F.Cu) (net 120))
  (segment (start 204.6 44.05) (end 204.6 42.24999) (width 0.15) (layer B.Cu) (net 120))
  (segment (start 205.1 43.55) (end 204.6 43.05) (width 0.15) (layer F.Cu) (net 121))
  (segment (start 204.6 43.05) (end 204.6 41.55) (width 0.15) (layer F.Cu) (net 121))
  (segment (start 206.1 43.55) (end 205.6 43.05) (width 0.15) (layer F.Cu) (net 122))
  (segment (start 205.6 43.05) (end 205.6 41.55) (width 0.15) (layer F.Cu) (net 122))
  (segment (start 207.1 42.55) (end 207.1 41.55) (width 0.15) (layer F.Cu) (net 123))
  (segment (start 206.1 42.55) (end 206.1 41.55) (width 0.15) (layer F.Cu) (net 124))
  (segment (start 205.1 42.55) (end 205.1 41.55) (width 0.15) (layer F.Cu) (net 125))
  (segment (start 206.1 56.55) (end 205.6 57.05) (width 0.15) (layer F.Cu) (net 126))
  (segment (start 205.6 57.05) (end 205.6 59.55) (width 0.15) (layer F.Cu) (net 126))
  (segment (start 205.6 59.55) (end 205.3 59.85) (width 0.15) (layer F.Cu) (net 126))
  (segment (start 205.3 59.85) (end 205.3 62.2) (width 0.15) (layer F.Cu) (net 126))
  (via (at 205.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 127))
  (segment (start 206.1 55.55) (end 205.6 56.05) (width 0.15) (layer F.Cu) (net 127))
  (segment (start 205.6 56.05) (end 205.6 57.75) (width 0.15) (layer B.Cu) (net 127))
  (via (at 205.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 128))
  (segment (start 206.1 54.55) (end 205.6 55.05) (width 0.15) (layer F.Cu) (net 128))
  (segment (start 205.6 55.05) (end 205.1 55.55) (width 0.15) (layer B.Cu) (net 128))
  (segment (start 205.1 55.55) (end 205.1 57.95) (width 0.15) (layer B.Cu) (net 128))
  (via (at 206.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 129))
  (segment (start 207.1 55.55) (end 206.6 56.05) (width 0.15) (layer F.Cu) (net 129))
  (segment (start 206.6 56.35) (end 207.05 56.8) (width 0.15) (layer B.Cu) (net 129))
  (segment (start 206.6 56.05) (end 206.6 56.35) (width 0.15) (layer B.Cu) (net 129))
  (segment (start 207.05 56.8) (end 207.1 56.85) (width 0.15) (layer B.Cu) (net 129))
  (segment (start 207.1 56.85) (end 207.1 57.55) (width 0.15) (layer B.Cu) (net 129))
  (segment (start 207.1 57.55) (end 206.8 57.85) (width 0.15) (layer B.Cu) (net 129))
  (segment (start 208.1 56.55) (end 207.6 57.05) (width 0.15) (layer F.Cu) (net 130))
  (segment (start 207.6 57.05) (end 207.6 58.55) (width 0.15) (layer F.Cu) (net 130))
  (segment (start 207.6 58.55) (end 207.6 58.9) (width 0.15) (layer F.Cu) (net 130))
  (segment (start 207.6 58.9) (end 206.2 60.3) (width 0.15) (layer F.Cu) (net 130))
  (segment (start 206.2 60.3) (end 206.2 62.1) (width 0.15) (layer F.Cu) (net 130))
  (via (at 207.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 131))
  (segment (start 208.1 55.55) (end 207.6 56.05) (width 0.15) (layer F.Cu) (net 131))
  (segment (start 207.7 56.15) (end 207.7 57.95) (width 0.15) (layer B.Cu) (net 131))
  (segment (start 207.6 56.05) (end 207.7 56.15) (width 0.15) (layer B.Cu) (net 131))
  (via (at 207.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 132))
  (segment (start 208.1 54.55) (end 207.6 55.05) (width 0.15) (layer F.Cu) (net 132))
  (segment (start 207.4 56.55) (end 207.4 58.05) (width 0.15) (layer B.Cu) (net 132))
  (segment (start 207.1 56.25) (end 207.4 56.55) (width 0.15) (layer B.Cu) (net 132))
  (segment (start 207.1 55.55) (end 207.1 56.25) (width 0.15) (layer B.Cu) (net 132))
  (segment (start 207.6 55.05) (end 207.1 55.55) (width 0.15) (layer B.Cu) (net 132))
  (via (at 209.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 133))
  (segment (start 209.1 54.55) (end 209.6 55.05) (width 0.15) (layer F.Cu) (net 133))
  (segment (start 209.6 55.05) (end 210.1 55.55) (width 0.15) (layer B.Cu) (net 133))
  (segment (start 210.1 55.55) (end 210.1 56.3) (width 0.15) (layer B.Cu) (net 133))
  (segment (start 210.1 56.3) (end 210.4 56.6) (width 0.15) (layer B.Cu) (net 133))
  (segment (start 210.4 56.6) (end 210.4 58) (width 0.15) (layer B.Cu) (net 133))
  (via (at 209.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 134))
  (segment (start 209.1 55.55) (end 209.6 56.05) (width 0.15) (layer F.Cu) (net 134))
  (segment (start 209.6 56.05) (end 209.6 56.3) (width 0.15) (layer B.Cu) (net 134))
  (segment (start 209.6 56.3) (end 210.1 56.8) (width 0.15) (layer B.Cu) (net 134))
  (segment (start 210.1 56.8) (end 210.1 58.05) (width 0.15) (layer B.Cu) (net 134))
  (segment (start 210.1 57.55) (end 210.1 58.55) (width 0.15) (layer F.Cu) (net 135))
  (segment (start 210.1 58.55) (end 210.1 59.4) (width 0.15) (layer F.Cu) (net 135))
  (segment (start 210.1 59.4) (end 211 60.3) (width 0.15) (layer F.Cu) (net 135))
  (segment (start 211 60.3) (end 211 62.1) (width 0.15) (layer F.Cu) (net 135))
  (segment (start 210.1 56.55) (end 210.6 57.05) (width 0.15) (layer F.Cu) (net 136))
  (segment (start 210.6 57.05) (end 210.6 58.55) (width 0.15) (layer F.Cu) (net 136))
  (segment (start 210.6 58.55) (end 210.6 59.45) (width 0.15) (layer F.Cu) (net 136))
  (segment (start 210.6 59.45) (end 211.3 60.15) (width 0.15) (layer F.Cu) (net 136))
  (segment (start 211.3 60.15) (end 211.3 62.05) (width 0.15) (layer F.Cu) (net 136))
  (via (at 210.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 137))
  (segment (start 210.1 55.55) (end 210.6 56.05) (width 0.15) (layer F.Cu) (net 137))
  (segment (start 210.6 56.05) (end 210.7 56.15) (width 0.15) (layer B.Cu) (net 137))
  (segment (start 210.7 56.15) (end 210.7 58.05) (width 0.15) (layer B.Cu) (net 137))
  (via (at 211.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 138))
  (segment (start 211.1 54.55) (end 211.6 55.05) (width 0.15) (layer F.Cu) (net 138))
  (segment (start 211.6 55.05) (end 212.1 55.55) (width 0.15) (layer B.Cu) (net 138))
  (segment (start 212.1 55.55) (end 212.1 56.3) (width 0.15) (layer B.Cu) (net 138))
  (segment (start 212.1 56.3) (end 212.4 56.6) (width 0.15) (layer B.Cu) (net 138))
  (segment (start 212.4 56.6) (end 212.4 58.3) (width 0.15) (layer B.Cu) (net 138))
  (via (at 211.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 139))
  (segment (start 211.1 55.55) (end 211.6 56.05) (width 0.15) (layer F.Cu) (net 139))
  (segment (start 211.6 56.05) (end 211.6 56.3) (width 0.15) (layer B.Cu) (net 139))
  (segment (start 211.6 56.3) (end 212.1 56.8) (width 0.15) (layer B.Cu) (net 139))
  (segment (start 212.1 56.8) (end 212.1 58.3) (width 0.15) (layer B.Cu) (net 139))
  (segment (start 211.1 57.55) (end 211.1 58.55) (width 0.15) (layer F.Cu) (net 140))
  (segment (start 211.1 58.55) (end 211.1 59.5) (width 0.15) (layer F.Cu) (net 140))
  (segment (start 211.1 59.5) (end 211.6 60) (width 0.15) (layer F.Cu) (net 140))
  (segment (start 211.6 60) (end 211.6 62.35) (width 0.15) (layer F.Cu) (net 140))
  (segment (start 212.1 57.55) (end 212.1 58.55) (width 0.15) (layer F.Cu) (net 141))
  (segment (start 212.1 58.55) (end 212.1 59.1) (width 0.15) (layer F.Cu) (net 141))
  (segment (start 212.1 59.1) (end 211.9 59.3) (width 0.15) (layer F.Cu) (net 141))
  (segment (start 211.9 59.3) (end 211.9 62.4) (width 0.15) (layer F.Cu) (net 141))
  (segment (start 212.1 56.55) (end 212.6 57.05) (width 0.15) (layer F.Cu) (net 142))
  (segment (start 212.6 57.05) (end 212.6 58.55) (width 0.15) (layer F.Cu) (net 142))
  (segment (start 212.6 58.55) (end 212.6 59.25) (width 0.15) (layer F.Cu) (net 142))
  (segment (start 212.6 59.25) (end 212.2 59.65) (width 0.15) (layer F.Cu) (net 142))
  (segment (start 212.2 59.65) (end 212.2 62.25) (width 0.15) (layer F.Cu) (net 142))
  (via (at 212.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 143))
  (segment (start 212.1 55.55) (end 212.6 56.05) (width 0.15) (layer F.Cu) (net 143))
  (segment (start 212.6 56.05) (end 212.7 56.15) (width 0.15) (layer B.Cu) (net 143))
  (segment (start 212.7 56.15) (end 212.7 58.3) (width 0.15) (layer B.Cu) (net 143))
  (via (at 212.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 144))
  (segment (start 212.1 54.55) (end 212.6 55.05) (width 0.15) (layer F.Cu) (net 144))
  (segment (start 212.6 55.05) (end 213.1 55.55) (width 0.15) (layer B.Cu) (net 144))
  (segment (start 213.1 55.55) (end 213.1 58.05) (width 0.15) (layer B.Cu) (net 144))
  (via (at 213.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 145))
  (segment (start 213.1 54.55) (end 213.6 55.05) (width 0.15) (layer F.Cu) (net 145))
  (segment (start 214.6 56.8) (end 214.6 58.3) (width 0.15) (layer B.Cu) (net 145))
  (segment (start 214.1 56.3) (end 214.6 56.8) (width 0.15) (layer B.Cu) (net 145))
  (segment (start 214.1 55.85) (end 214.1 56.3) (width 0.15) (layer B.Cu) (net 145))
  (segment (start 213.6 55.35) (end 214.1 55.85) (width 0.15) (layer B.Cu) (net 145))
  (segment (start 213.6 55.05) (end 213.6 55.35) (width 0.15) (layer B.Cu) (net 145))
  (via (at 214.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 146))
  (segment (start 214.1 54.55) (end 214.6 55.05) (width 0.15) (layer F.Cu) (net 146))
  (segment (start 215.6 55.75) (end 215.6 56.9) (width 0.15) (layer B.Cu) (net 146))
  (segment (start 214.9 55.05) (end 215.6 55.75) (width 0.15) (layer B.Cu) (net 146))
  (segment (start 215.6 56.9) (end 215.6 57.8) (width 0.15) (layer B.Cu) (net 146))
  (segment (start 214.6 55.05) (end 214.9 55.05) (width 0.15) (layer B.Cu) (net 146))
  (via (at 213.6 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 147))
  (segment (start 213.1 55.55) (end 213.6 56.05) (width 0.15) (layer F.Cu) (net 147))
  (segment (start 214.1 56.8) (end 214.1 58.05) (width 0.15) (layer B.Cu) (net 147))
  (segment (start 213.6 56.3) (end 214.1 56.8) (width 0.15) (layer B.Cu) (net 147))
  (segment (start 213.6 56.05) (end 213.6 56.3) (width 0.15) (layer B.Cu) (net 147))
  (segment (start 214.1 56.55) (end 214.6 57.05) (width 0.15) (layer F.Cu) (net 148))
  (segment (start 214.6 57.05) (end 214.6 58.55) (width 0.15) (layer F.Cu) (net 148))
  (segment (start 214.6 58.55) (end 214.6 58.7) (width 0.15) (layer F.Cu) (net 148))
  (segment (start 214.6 58.7) (end 214.6 60) (width 0.15) (layer F.Cu) (net 148))
  (segment (start 214.6 60) (end 214.9 60.3) (width 0.15) (layer F.Cu) (net 148))
  (segment (start 214.9 60.3) (end 214.9 62.55) (width 0.15) (layer F.Cu) (net 148))
  (segment (start 215.6 57.05) (end 215.6 58.55) (width 0.15) (layer F.Cu) (net 149))
  (segment (start 215.1 56.55) (end 215.6 57.05) (width 0.15) (layer F.Cu) (net 149))
  (segment (start 215.6 58.55) (end 215.5 58.65) (width 0.15) (layer F.Cu) (net 149))
  (segment (start 215.5 58.65) (end 215.5 61.8) (width 0.15) (layer F.Cu) (net 149))
  (segment (start 213.1 57.55) (end 213.1 58.55) (width 0.15) (layer F.Cu) (net 150))
  (segment (start 213.1 58.55) (end 213.1 59.25) (width 0.15) (layer F.Cu) (net 150))
  (segment (start 213.1 59.25) (end 212.5 59.85) (width 0.15) (layer F.Cu) (net 150))
  (segment (start 212.5 59.85) (end 212.5 62.05) (width 0.15) (layer F.Cu) (net 150))
  (segment (start 214.1 57.55) (end 214.1 59.95) (width 0.15) (layer F.Cu) (net 151))
  (segment (start 214.1 59.95) (end 214.6 60.45) (width 0.15) (layer F.Cu) (net 151))
  (segment (start 214.6 60.45) (end 214.6 62.9) (width 0.15) (layer F.Cu) (net 151))
  (segment (start 215.1 57.55) (end 215.1 58.55) (width 0.15) (layer F.Cu) (net 152))
  (segment (start 215.1 58.55) (end 215.1 60.05) (width 0.15) (layer F.Cu) (net 152))
  (segment (start 215.1 60.05) (end 215.2 60.15) (width 0.15) (layer F.Cu) (net 152))
  (segment (start 215.2 60.15) (end 215.2 62) (width 0.15) (layer F.Cu) (net 152))
  (segment (start 216.1 54.55) (end 218.35 54.55) (width 0.15) (layer F.Cu) (net 153))
  (segment (start 205.1 50.55) (end 204.6 51.05) (width 0.15) (layer F.Cu) (net 154))
  (via (at 204.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 154))
  (segment (start 204.6 51.05) (end 204.1 50.55) (width 0.15) (layer B.Cu) (net 154))
  (segment (start 204.1 50.55) (end 200.45 50.55) (width 0.15) (layer B.Cu) (net 154))
  (via (at 204.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 155))
  (segment (start 205.1 51.55) (end 204.6 52.05) (width 0.15) (layer F.Cu) (net 155))
  (segment (start 204.6 52.05) (end 204.1 52.55) (width 0.15) (layer B.Cu) (net 155))
  (segment (start 204.1 52.55) (end 202.35 52.55) (width 0.15) (layer B.Cu) (net 155))
  (segment (start 202.35 52.55) (end 201.95 52.95) (width 0.15) (layer B.Cu) (net 155))
  (segment (start 201.95 52.95) (end 201.1 52.95) (width 0.15) (layer B.Cu) (net 155))
  (segment (start 201.1 52.95) (end 199.6 54.45) (width 0.15) (layer B.Cu) (net 155))
  (via (at 204.6 53.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 156))
  (segment (start 205.1 52.55) (end 204.6 53.05) (width 0.15) (layer F.Cu) (net 156))
  (segment (start 204.6 53.05) (end 204.1 53.55) (width 0.15) (layer B.Cu) (net 156))
  (segment (start 204.1 53.55) (end 204.1 54.4) (width 0.15) (layer B.Cu) (net 156))
  (segment (start 204.1 54.4) (end 203.95 54.55) (width 0.15) (layer B.Cu) (net 156))
  (segment (start 203.95 54.55) (end 203.3 54.55) (width 0.15) (layer B.Cu) (net 156))
  (segment (start 203.3 54.55) (end 203.1 54.75) (width 0.15) (layer B.Cu) (net 156))
  (segment (start 203.1 54.75) (end 203.1 55.4) (width 0.15) (layer B.Cu) (net 156))
  (segment (start 203.1 55.4) (end 201.65 56.85) (width 0.15) (layer B.Cu) (net 156))
  (via (at 205.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 157))
  (segment (start 206.1 53.55) (end 205.6 54.05) (width 0.15) (layer F.Cu) (net 157))
  (segment (start 205.6 54.05) (end 205.1 54.55) (width 0.15) (layer B.Cu) (net 157))
  (segment (start 205.1 54.55) (end 204.4 54.55) (width 0.15) (layer B.Cu) (net 157))
  (segment (start 204.4 54.55) (end 204.1 54.85) (width 0.15) (layer B.Cu) (net 157))
  (segment (start 204.1 54.85) (end 204.1 55.3) (width 0.15) (layer B.Cu) (net 157))
  (segment (start 204.1 55.3) (end 203.85 55.55) (width 0.15) (layer B.Cu) (net 157))
  (segment (start 203.85 55.55) (end 203.4 55.55) (width 0.15) (layer B.Cu) (net 157))
  (segment (start 203.4 55.55) (end 202.35 56.6) (width 0.15) (layer B.Cu) (net 157))
  (via (at 206.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 160))
  (segment (start 207.1 53.55) (end 206.6 54.05) (width 0.15) (layer F.Cu) (net 160))
  (segment (start 206.6 54.05) (end 206.1 54.55) (width 0.15) (layer B.Cu) (net 160))
  (segment (start 206.1 54.55) (end 206.1 57.85) (width 0.15) (layer B.Cu) (net 160))
  (segment (start 208.1 53.55) (end 207.6 54.05) (width 0.15) (layer F.Cu) (net 162))
  (via (at 207.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 162))
  (segment (start 207.6 54.05) (end 208.1 54.55) (width 0.15) (layer B.Cu) (net 162))
  (segment (start 208.1 54.55) (end 208.1 58) (width 0.15) (layer B.Cu) (net 162))
  (via (at 209.6 53.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 163))
  (segment (start 209.1 52.55) (end 209.6 53.05) (width 0.15) (layer F.Cu) (net 163))
  (segment (start 209.6 53.05) (end 209.1 53.55) (width 0.15) (layer B.Cu) (net 163))
  (segment (start 209.1 53.55) (end 209.1 57.8) (width 0.15) (layer B.Cu) (net 163))
  (via (at 210.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 164))
  (segment (start 210.1 53.55) (end 210.6 54.05) (width 0.15) (layer F.Cu) (net 164))
  (segment (start 211.1 54.55) (end 211.1 57.9) (width 0.15) (layer B.Cu) (net 164))
  (segment (start 210.6 54.05) (end 211.1 54.55) (width 0.15) (layer B.Cu) (net 164))
  (via (at 211.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 168))
  (segment (start 211.1 50.55) (end 211.6 51.05) (width 0.15) (layer F.Cu) (net 168))
  (segment (start 215.95 50.55) (end 216.5 51.1) (width 0.15) (layer B.Cu) (net 168))
  (segment (start 212.1 50.55) (end 215.95 50.55) (width 0.15) (layer B.Cu) (net 168))
  (segment (start 211.6 51.05) (end 212.1 50.55) (width 0.15) (layer B.Cu) (net 168))
  (via (at 212.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 169))
  (segment (start 212.1 53.55) (end 212.6 54.05) (width 0.15) (layer F.Cu) (net 169))
  (segment (start 212.6 54.05) (end 213.1 54.55) (width 0.15) (layer B.Cu) (net 169))
  (segment (start 213.1 54.55) (end 213.8 54.55) (width 0.15) (layer B.Cu) (net 169))
  (segment (start 213.8 54.55) (end 214.1 54.85) (width 0.15) (layer B.Cu) (net 169))
  (segment (start 214.1 54.85) (end 214.1 55.3) (width 0.15) (layer B.Cu) (net 169))
  (segment (start 214.1 55.3) (end 214.35 55.55) (width 0.15) (layer B.Cu) (net 169))
  (segment (start 214.35 55.55) (end 214.9 55.55) (width 0.15) (layer B.Cu) (net 169))
  (segment (start 214.9 55.55) (end 215.15 55.8) (width 0.15) (layer B.Cu) (net 169))
  (segment (start 215.15 55.8) (end 215.15 57.9) (width 0.15) (layer B.Cu) (net 169))
  (via (at 212.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 171))
  (segment (start 212.1 51.55) (end 212.6 52.05) (width 0.15) (layer F.Cu) (net 171))
  (segment (start 213.1 52.55) (end 217.5 52.55) (width 0.15) (layer B.Cu) (net 171))
  (segment (start 212.6 52.05) (end 213.1 52.55) (width 0.15) (layer B.Cu) (net 171))
  (via (at 214.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 172))
  (segment (start 214.1 53.55) (end 214.6 54.05) (width 0.15) (layer F.Cu) (net 172))
  (segment (start 214.8 54.25) (end 217.15 54.25) (width 0.15) (layer B.Cu) (net 172))
  (segment (start 214.6 54.05) (end 214.8 54.25) (width 0.15) (layer B.Cu) (net 172))
  (via (at 214.6 53.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 173))
  (segment (start 214.1 52.55) (end 214.6 53.05) (width 0.15) (layer F.Cu) (net 173))
  (segment (start 214.6 53.05) (end 214.8 53.05) (width 0.15) (layer B.Cu) (net 173))
  (segment (start 214.8 53.05) (end 215.4 53.65) (width 0.15) (layer B.Cu) (net 173))
  (segment (start 215.4 53.65) (end 217.1 53.65) (width 0.15) (layer B.Cu) (net 173))
  (segment (start 215.1 53.55) (end 215.6 54.05) (width 0.15) (layer F.Cu) (net 174))
  (segment (start 215.6 54.05) (end 218.35 54.05) (width 0.15) (layer F.Cu) (net 174))
  (segment (start 216.1 53.55) (end 218.35 53.55) (width 0.15) (layer F.Cu) (net 175))
  (segment (start 216.1 52.55) (end 216.6 53.05) (width 0.15) (layer F.Cu) (net 176))
  (segment (start 216.6 53.05) (end 218.35 53.05) (width 0.15) (layer F.Cu) (net 176))
  (segment (start 218.35 53.05) (end 219.35 54.05) (width 0.15) (layer F.Cu) (net 176))
  (via (at 213.6 54.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 177))
  (segment (start 213.1 53.55) (end 213.6 54.05) (width 0.15) (layer F.Cu) (net 177))
  (segment (start 214.4 54.55) (end 216.85 54.55) (width 0.15) (layer B.Cu) (net 177))
  (segment (start 213.9 54.05) (end 214.4 54.55) (width 0.15) (layer B.Cu) (net 177))
  (segment (start 213.6 54.05) (end 213.9 54.05) (width 0.15) (layer B.Cu) (net 177))
  (via (at 213.6 53.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 178))
  (segment (start 213.1 52.55) (end 213.6 53.05) (width 0.15) (layer F.Cu) (net 178))
  (segment (start 214.8 53.55) (end 215.2 53.95) (width 0.15) (layer B.Cu) (net 178))
  (segment (start 214.1 53.55) (end 214.8 53.55) (width 0.15) (layer B.Cu) (net 178))
  (segment (start 213.6 53.05) (end 214.1 53.55) (width 0.15) (layer B.Cu) (net 178))
  (segment (start 215.2 53.95) (end 217.15 53.95) (width 0.15) (layer B.Cu) (net 178))
  (via (at 214.6 47.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 179))
  (segment (start 214.1 47.55) (end 214.6 47.05) (width 0.15) (layer F.Cu) (net 179))
  (segment (start 215.55 46.35) (end 218.6 46.35) (width 0.15) (layer B.Cu) (net 179))
  (segment (start 214.85 47.05) (end 215.55 46.35) (width 0.15) (layer B.Cu) (net 179))
  (segment (start 214.6 47.05) (end 214.85 47.05) (width 0.15) (layer B.Cu) (net 179))
  (via (at 214.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 180))
  (segment (start 214.1 49.55) (end 214.6 49.05) (width 0.15) (layer F.Cu) (net 180))
  (segment (start 216.2 49.05) (end 216.4 49.25) (width 0.15) (layer B.Cu) (net 180))
  (segment (start 214.6 49.05) (end 216.2 49.05) (width 0.15) (layer B.Cu) (net 180))
  (via (at 214.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 181))
  (segment (start 214.1 50.55) (end 214.6 51.05) (width 0.15) (layer F.Cu) (net 181))
  (segment (start 214.6 51.05) (end 214.85 51.05) (width 0.15) (layer B.Cu) (net 181))
  (segment (start 214.85 51.05) (end 215.45 51.65) (width 0.15) (layer B.Cu) (net 181))
  (segment (start 215.45 51.65) (end 217.8 51.65) (width 0.15) (layer B.Cu) (net 181))
  (via (at 214.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 182))
  (segment (start 214.1 51.55) (end 214.6 52.05) (width 0.15) (layer F.Cu) (net 182))
  (segment (start 214.6 52.05) (end 214.8 52.25) (width 0.15) (layer B.Cu) (net 182))
  (segment (start 214.8 52.25) (end 217.65 52.25) (width 0.15) (layer B.Cu) (net 182))
  (segment (start 215.1 51.55) (end 215.6 52.05) (width 0.15) (layer F.Cu) (net 183))
  (segment (start 215.6 52.05) (end 217.85 52.05) (width 0.15) (layer F.Cu) (net 183))
  (segment (start 217.85 52.05) (end 219.6 53.8) (width 0.15) (layer F.Cu) (net 183))
  (segment (start 221.5 47.25) (end 221.5 49.65) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 218.85 46.7) (end 220.95 46.7) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 218.35 48.4) (end 218.35 47.2) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 216.8 48.75) (end 218 48.75) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 215.1 49.55) (end 215.6 49.05) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 216.5 49.05) (end 216.8 48.75) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 218.35 47.2) (end 218.85 46.7) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 215.6 49.05) (end 216.5 49.05) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 220.95 46.7) (end 221.5 47.25) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 218 48.75) (end 218.35 48.4) (width 0.15) (layer F.Cu) (net 184))
  (segment (start 218 51.55) (end 218.4 51.95) (width 0.15) (layer F.Cu) (net 185))
  (segment (start 216.1 51.55) (end 218 51.55) (width 0.15) (layer F.Cu) (net 185))
  (segment (start 218.3 51.15) (end 218.5 51.35) (width 0.15) (layer F.Cu) (net 186))
  (segment (start 217.5 51.15) (end 218.3 51.15) (width 0.15) (layer F.Cu) (net 186))
  (segment (start 216.9 50.55) (end 217.5 51.15) (width 0.15) (layer F.Cu) (net 186))
  (segment (start 216.1 50.55) (end 216.9 50.55) (width 0.15) (layer F.Cu) (net 186))
  (segment (start 221.1 47.3) (end 221.1 49.8) (width 0.15) (layer F.Cu) (net 187))
  (segment (start 219 47) (end 220.8 47) (width 0.15) (layer F.Cu) (net 187))
  (segment (start 220.8 47) (end 221.1 47.3) (width 0.15) (layer F.Cu) (net 187))
  (segment (start 218.65 47.35) (end 219 47) (width 0.15) (layer F.Cu) (net 187))
  (segment (start 218.65 48.6) (end 218.65 47.35) (width 0.15) (layer F.Cu) (net 187))
  (segment (start 218.65 48.6) (end 218.2 49.05) (width 0.15) (layer F.Cu) (net 187))
  (segment (start 218.2 49.05) (end 217.4 49.05) (width 0.15) (layer F.Cu) (net 187))
  (segment (start 216.9 49.55) (end 216.1 49.55) (width 0.15) (layer F.Cu) (net 187))
  (segment (start 217.4 49.05) (end 216.9 49.55) (width 0.15) (layer F.Cu) (net 187))
  (via (at 213.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 188))
  (segment (start 213.1 50.55) (end 213.6 51.05) (width 0.15) (layer F.Cu) (net 188))
  (segment (start 213.6 51.05) (end 214.1 51.55) (width 0.15) (layer B.Cu) (net 188))
  (segment (start 214.1 51.55) (end 214.8 51.55) (width 0.15) (layer B.Cu) (net 188))
  (segment (start 214.8 51.55) (end 215.2 51.95) (width 0.15) (layer B.Cu) (net 188))
  (segment (start 215.2 51.95) (end 217.7 51.95) (width 0.15) (layer B.Cu) (net 188))
  (via (at 204.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 189))
  (segment (start 205.1 48.55) (end 204.6 48.05) (width 0.15) (layer F.Cu) (net 189))
  (segment (start 204.6 48.05) (end 204.1 47.55) (width 0.15) (layer B.Cu) (net 189))
  (segment (start 204.1 47.55) (end 201.35 47.55) (width 0.15) (layer B.Cu) (net 189))
  (segment (start 201.35 47.55) (end 200.65 46.85) (width 0.15) (layer B.Cu) (net 189))
  (segment (start 200.65 46.85) (end 199.55 46.85) (width 0.15) (layer B.Cu) (net 189))
  (via (at 204.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 191))
  (segment (start 205.1 46.55) (end 204.6 46.05) (width 0.15) (layer F.Cu) (net 191))
  (segment (start 202.35 44.05) (end 200.1 44.05) (width 0.15) (layer B.Cu) (net 191))
  (segment (start 203.1 44.8) (end 202.35 44.05) (width 0.15) (layer B.Cu) (net 191))
  (segment (start 203.1 45.3) (end 203.1 44.8) (width 0.15) (layer B.Cu) (net 191))
  (segment (start 203.35 45.55) (end 203.1 45.3) (width 0.15) (layer B.Cu) (net 191))
  (segment (start 203.85 45.55) (end 203.35 45.55) (width 0.15) (layer B.Cu) (net 191))
  (segment (start 204.35 46.05) (end 203.85 45.55) (width 0.15) (layer B.Cu) (net 191))
  (segment (start 204.6 46.05) (end 204.35 46.05) (width 0.15) (layer B.Cu) (net 191))
  (via (at 205.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 192))
  (segment (start 206.1 49.55) (end 205.6 49.05) (width 0.15) (layer F.Cu) (net 192))
  (segment (start 205.6 49.05) (end 205.1 49.55) (width 0.15) (layer B.Cu) (net 192))
  (segment (start 205.1 49.55) (end 200.6 49.55) (width 0.15) (layer B.Cu) (net 192))
  (via (at 205.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 194))
  (segment (start 206.1 46.55) (end 205.6 46.05) (width 0.15) (layer F.Cu) (net 194))
  (segment (start 205.6 46.05) (end 205.1 45.55) (width 0.15) (layer B.Cu) (net 194))
  (segment (start 205.1 45.55) (end 204.35 45.55) (width 0.15) (layer B.Cu) (net 194))
  (segment (start 204.35 45.55) (end 204.1 45.3) (width 0.15) (layer B.Cu) (net 194))
  (segment (start 204.1 45.3) (end 204.1 44.8) (width 0.15) (layer B.Cu) (net 194))
  (segment (start 204.1 44.8) (end 203.85 44.55) (width 0.15) (layer B.Cu) (net 194))
  (segment (start 203.85 44.55) (end 203.35 44.55) (width 0.15) (layer B.Cu) (net 194))
  (segment (start 203.35 44.55) (end 202.35 43.55) (width 0.15) (layer B.Cu) (net 194))
  (segment (start 202.35 43.55) (end 199.6 43.55) (width 0.15) (layer B.Cu) (net 194))
  (via (at 206.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 195))
  (segment (start 207.1 46.55) (end 206.6 46.05) (width 0.15) (layer F.Cu) (net 195))
  (segment (start 206.6 46.05) (end 206.1 45.55) (width 0.15) (layer B.Cu) (net 195))
  (segment (start 206.1 45.55) (end 206.1 42.8) (width 0.15) (layer B.Cu) (net 195))
  (segment (start 206.1 42.8) (end 206.6 42.3) (width 0.15) (layer B.Cu) (net 195))
  (segment (start 206.6 42.3) (end 206.6 41.3) (width 0.15) (layer B.Cu) (net 195))
  (segment (start 215.1 46.55) (end 215.6 46.05) (width 0.15) (layer F.Cu) (net 197))
  (segment (start 215.6 46.05) (end 217.1 46.05) (width 0.15) (layer F.Cu) (net 197))
  (segment (start 216.1 46.55) (end 217.1 46.55) (width 0.15) (layer F.Cu) (net 198))
  (via (at 207.6 47.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 199))
  (segment (start 208.1 47.55) (end 207.6 47.05) (width 0.15) (layer F.Cu) (net 199))
  (segment (start 207.6 47.05) (end 208.1 46.55) (width 0.15) (layer B.Cu) (net 199))
  (segment (start 208.1 46.55) (end 208.1 41.55) (width 0.15) (layer B.Cu) (net 199))
  (via (at 209.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 201))
  (segment (start 209.1 46.55) (end 209.6 46.05) (width 0.15) (layer F.Cu) (net 201))
  (segment (start 209.6 46.05) (end 209.1 45.55) (width 0.15) (layer B.Cu) (net 201))
  (segment (start 209.1 45.55) (end 209.1 42.3) (width 0.15) (layer B.Cu) (net 201))
  (via (at 207.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 202))
  (segment (start 208.1 45.55) (end 207.6 45.05) (width 0.15) (layer F.Cu) (net 202))
  (segment (start 207.6 45.05) (end 207.1 44.55) (width 0.15) (layer B.Cu) (net 202))
  (segment (start 207.1 44.55) (end 207.1 43.85) (width 0.15) (layer B.Cu) (net 202))
  (segment (start 207.1 43.85) (end 207.45 43.5) (width 0.15) (layer B.Cu) (net 202))
  (segment (start 207.45 43.5) (end 207.45 42.05) (width 0.15) (layer B.Cu) (net 202))
  (via (at 209.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 203))
  (segment (start 209.1 45.55) (end 209.6 45.05) (width 0.15) (layer F.Cu) (net 203))
  (segment (start 209.6 45.05) (end 210.1 44.55) (width 0.15) (layer B.Cu) (net 203))
  (segment (start 210.1 44.55) (end 210.1 43.8) (width 0.15) (layer B.Cu) (net 203))
  (segment (start 210.1 43.8) (end 210.4 43.5) (width 0.15) (layer B.Cu) (net 203))
  (segment (start 210.4 43.5) (end 210.4 41.55) (width 0.15) (layer B.Cu) (net 203))
  (via (at 211.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 204))
  (segment (start 211.1 45.55) (end 211.6 45.05) (width 0.15) (layer F.Cu) (net 204))
  (segment (start 211.6 45.05) (end 212.1 44.55) (width 0.15) (layer B.Cu) (net 204))
  (segment (start 212.1 44.55) (end 212.1 43.8) (width 0.15) (layer B.Cu) (net 204))
  (segment (start 212.1 43.8) (end 212.4 43.5) (width 0.15) (layer B.Cu) (net 204))
  (segment (start 212.4 43.5) (end 212.4 41.55) (width 0.15) (layer B.Cu) (net 204))
  (via (at 212.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 205))
  (segment (start 212.1 45.55) (end 212.6 45.05) (width 0.15) (layer F.Cu) (net 205))
  (segment (start 213.1 44.3) (end 213.1 41.55) (width 0.15) (layer B.Cu) (net 205))
  (segment (start 212.6 44.8) (end 213.1 44.3) (width 0.15) (layer B.Cu) (net 205))
  (segment (start 212.6 45.05) (end 212.6 44.8) (width 0.15) (layer B.Cu) (net 205))
  (segment (start 216.1 45.55) (end 217.1 45.55) (width 0.15) (layer F.Cu) (net 206))
  (via (at 213.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 207))
  (segment (start 213.1 49.55) (end 213.6 49.05) (width 0.15) (layer F.Cu) (net 207))
  (segment (start 218.25 48.55) (end 218.75 48.05) (width 0.15) (layer B.Cu) (net 207))
  (segment (start 214.1 48.55) (end 218.25 48.55) (width 0.15) (layer B.Cu) (net 207))
  (segment (start 213.6 49.05) (end 214.1 48.55) (width 0.15) (layer B.Cu) (net 207))
  (via (at 212.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 208))
  (segment (start 212.1 49.55) (end 212.6 49.05) (width 0.15) (layer F.Cu) (net 208))
  (segment (start 216.7 49.55) (end 217.1 49.15) (width 0.15) (layer B.Cu) (net 208))
  (segment (start 213.1 49.55) (end 216.7 49.55) (width 0.15) (layer B.Cu) (net 208))
  (segment (start 212.6 49.05) (end 213.1 49.55) (width 0.15) (layer B.Cu) (net 208))
  (via (at 212.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 210))
  (segment (start 212.1 48.55) (end 212.6 48.05) (width 0.15) (layer F.Cu) (net 210))
  (segment (start 215.75 46.65) (end 218.45 46.65) (width 0.15) (layer B.Cu) (net 210))
  (segment (start 214.85 47.55) (end 215.75 46.65) (width 0.15) (layer B.Cu) (net 210))
  (segment (start 213.1 47.55) (end 214.85 47.55) (width 0.15) (layer B.Cu) (net 210))
  (segment (start 212.6 48.05) (end 213.1 47.55) (width 0.15) (layer B.Cu) (net 210))
  (segment (start 216.1 44.55) (end 217.1 44.55) (width 0.15) (layer F.Cu) (net 211))
  (segment (start 215.1 44.55) (end 215.6 44.05) (width 0.15) (layer F.Cu) (net 212))
  (segment (start 215.6 44.05) (end 217.1 44.05) (width 0.15) (layer F.Cu) (net 212))
  (segment (start 214.1 44.55) (end 214.6 44.05) (width 0.15) (layer F.Cu) (net 213))
  (segment (start 214.6 44.05) (end 214.6 43.3) (width 0.15) (layer F.Cu) (net 213))
  (segment (start 214.6 43.3) (end 214.85 43.05) (width 0.15) (layer F.Cu) (net 213))
  (segment (start 214.85 43.05) (end 215.35 43.05) (width 0.15) (layer F.Cu) (net 213))
  (segment (start 215.35 43.05) (end 215.6 42.8) (width 0.15) (layer F.Cu) (net 213))
  (segment (start 215.6 42.8) (end 215.6 41.55) (width 0.15) (layer F.Cu) (net 213))
  (via (at 213.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 214))
  (segment (start 213.1 44.55) (end 213.6 44.05) (width 0.15) (layer F.Cu) (net 214))
  (segment (start 213.6 44.05) (end 214.1 43.55) (width 0.15) (layer B.Cu) (net 214))
  (segment (start 214.1 43.55) (end 214.1 41.55) (width 0.15) (layer B.Cu) (net 214))
  (via (at 212.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 215))
  (segment (start 212.1 44.55) (end 212.6 44.05) (width 0.15) (layer F.Cu) (net 215))
  (segment (start 212.6 44.05) (end 212.7 43.95) (width 0.15) (layer B.Cu) (net 215))
  (segment (start 212.7 43.95) (end 212.7 41.55) (width 0.15) (layer B.Cu) (net 215))
  (via (at 211.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 216))
  (segment (start 211.1 44.55) (end 211.6 44.05) (width 0.15) (layer F.Cu) (net 216))
  (segment (start 212.1 43.3) (end 212.1 41.55) (width 0.15) (layer B.Cu) (net 216))
  (segment (start 211.6 43.8) (end 212.1 43.3) (width 0.15) (layer B.Cu) (net 216))
  (segment (start 211.6 44.05) (end 211.6 43.8) (width 0.15) (layer B.Cu) (net 216))
  (via (at 210.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 217))
  (segment (start 210.1 44.55) (end 210.6 44.05) (width 0.15) (layer F.Cu) (net 217))
  (segment (start 210.6 44.05) (end 210.7 43.95) (width 0.15) (layer B.Cu) (net 217))
  (segment (start 210.7 43.95) (end 210.7 41.55) (width 0.15) (layer B.Cu) (net 217))
  (via (at 209.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 218))
  (segment (start 209.1 44.55) (end 209.6 44.05) (width 0.15) (layer F.Cu) (net 218))
  (segment (start 210.1 43.3) (end 210.1 41.55) (width 0.15) (layer B.Cu) (net 218))
  (segment (start 209.6 43.8) (end 210.1 43.3) (width 0.15) (layer B.Cu) (net 218))
  (segment (start 209.6 44.05) (end 209.6 43.8) (width 0.15) (layer B.Cu) (net 218))
  (via (at 207.6 44.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 219) (tstamp 61872596))
  (segment (start 208.1 44.55) (end 207.6 44.05) (width 0.15) (layer F.Cu) (net 219))
  (segment (start 207.6 44.05) (end 207.75 43.9) (width 0.15) (layer B.Cu) (net 219))
  (segment (start 207.75 43.9) (end 207.75 42.25) (width 0.15) (layer B.Cu) (net 219) (tstamp 61872591))
  (segment (start 208.1 43.55) (end 207.6 43.05) (width 0.15) (layer F.Cu) (net 220))
  (segment (start 207.6 43.05) (end 207.6 41.55) (width 0.15) (layer F.Cu) (net 220))
  (segment (start 210.1 43.55) (end 210.6 43.05) (width 0.15) (layer F.Cu) (net 221))
  (segment (start 210.6 43.05) (end 210.6 41.55) (width 0.15) (layer F.Cu) (net 221))
  (segment (start 212.1 43.55) (end 212.6 43.05) (width 0.15) (layer F.Cu) (net 222))
  (segment (start 212.6 43.05) (end 212.6 41.55) (width 0.15) (layer F.Cu) (net 222))
  (segment (start 214.1 43.55) (end 214.1 43.3) (width 0.15) (layer F.Cu) (net 223))
  (segment (start 214.1 43.3) (end 214.6 42.8) (width 0.15) (layer F.Cu) (net 223))
  (segment (start 214.6 42.8) (end 214.6 41.55) (width 0.15) (layer F.Cu) (net 223) (tstamp 6185AEC9))
  (segment (start 215.1 43.55) (end 215.35 43.55) (width 0.15) (layer F.Cu) (net 224))
  (segment (start 215.35 43.55) (end 215.85 43.05) (width 0.15) (layer F.Cu) (net 224))
  (segment (start 215.85 43.05) (end 217.1 43.05) (width 0.15) (layer F.Cu) (net 224))
  (segment (start 216.1 43.55) (end 217.1 43.55) (width 0.15) (layer F.Cu) (net 225))
  (via (at 212.6 47.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 226))
  (segment (start 212.1 47.55) (end 212.6 47.05) (width 0.15) (layer F.Cu) (net 226))
  (segment (start 212.6 47.05) (end 213.1 46.55) (width 0.15) (layer B.Cu) (net 226))
  (segment (start 213.1 46.55) (end 214.85 46.55) (width 0.15) (layer B.Cu) (net 226))
  (segment (start 214.85 46.55) (end 215.35 46.05) (width 0.15) (layer B.Cu) (net 226))
  (segment (start 215.35 46.05) (end 219.1 46.05) (width 0.15) (layer B.Cu) (net 226))
  (via (at 210.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 229))
  (segment (start 210.1 46.55) (end 210.6 46.05) (width 0.15) (layer F.Cu) (net 229))
  (segment (start 210.6 46.05) (end 211.1 45.55) (width 0.15) (layer B.Cu) (net 229))
  (segment (start 211.1 45.55) (end 211.1 41.55) (width 0.15) (layer B.Cu) (net 229))
  (via (at 211.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 230))
  (segment (start 211.1 46.55) (end 211.6 46.05) (width 0.15) (layer F.Cu) (net 230))
  (segment (start 211.6 46.05) (end 212.1 45.55) (width 0.15) (layer B.Cu) (net 230))
  (segment (start 212.1 45.55) (end 212.85 45.55) (width 0.15) (layer B.Cu) (net 230))
  (segment (start 213.1 45.3) (end 213.1 44.8) (width 0.15) (layer B.Cu) (net 230))
  (segment (start 212.85 45.55) (end 213.1 45.3) (width 0.15) (layer B.Cu) (net 230))
  (segment (start 213.85 44.55) (end 214.4 44) (width 0.15) (layer B.Cu) (net 230))
  (segment (start 214.4 44) (end 214.4 41.55) (width 0.15) (layer B.Cu) (net 230))
  (segment (start 213.1 44.8) (end 213.35 44.55) (width 0.15) (layer B.Cu) (net 230))
  (segment (start 213.35 44.55) (end 213.85 44.55) (width 0.15) (layer B.Cu) (net 230))
  (via (at 212.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 231))
  (segment (start 212.1 46.55) (end 212.6 46.05) (width 0.15) (layer F.Cu) (net 231))
  (segment (start 212.6 46.05) (end 212.85 46.05) (width 0.15) (layer B.Cu) (net 231))
  (segment (start 212.85 46.05) (end 213.35 45.55) (width 0.15) (layer B.Cu) (net 231))
  (segment (start 213.35 45.55) (end 213.85 45.55) (width 0.15) (layer B.Cu) (net 231))
  (segment (start 213.85 45.55) (end 214.1 45.3) (width 0.15) (layer B.Cu) (net 231))
  (segment (start 214.1 45.3) (end 214.1 44.8) (width 0.15) (layer B.Cu) (net 231))
  (segment (start 214.1 44.8) (end 214.7 44.2) (width 0.15) (layer B.Cu) (net 231))
  (segment (start 214.7 44.2) (end 214.7 41.55) (width 0.15) (layer B.Cu) (net 231))
  (segment (start 215.1 42.55) (end 215.1 41.55) (width 0.15) (layer F.Cu) (net 232))
  (segment (start 214.1 42.55) (end 214.1 41.55) (width 0.15) (layer F.Cu) (net 233))
  (segment (start 213.1 42.55) (end 213.1 41.55) (width 0.15) (layer F.Cu) (net 234))
  (segment (start 212.1 42.55) (end 212.1 41.55) (width 0.15) (layer F.Cu) (net 235))
  (segment (start 211.1 42.55) (end 211.1 41.55) (width 0.15) (layer F.Cu) (net 236))
  (segment (start 210.1 42.55) (end 210.1 41.55) (width 0.15) (layer F.Cu) (net 237))
  (segment (start 209.1 42.55) (end 209.1 41.55) (width 0.15) (layer F.Cu) (net 238))
  (segment (start 208.1 42.55) (end 208.1 41.55) (width 0.15) (layer F.Cu) (net 239))
  (via (at 196.85 75.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 247))
  (segment (start 195.1 75.7) (end 196.85 75.7) (width 0.15) (layer F.Cu) (net 247))
  (segment (start 199.35 87.85) (end 199.35 89.75) (width 0.15) (layer F.Cu) (net 247) (tstamp 61903FD3))
  (via (at 199.35 89.75) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 247) (tstamp 61903FD6))
  (segment (start 199.35 78.2) (end 196.85 75.7) (width 0.15) (layer B.Cu) (net 247))
  (segment (start 199.35 89.75) (end 199.35 78.2) (width 0.15) (layer B.Cu) (net 247))
  (segment (start 198.6 73.95) (end 196.85 75.7) (width 0.15) (layer F.Cu) (net 247))
  (segment (start 198.6 64.15) (end 198.6 73.95) (width 0.15) (layer F.Cu) (net 247))
  (segment (start 192.05 71.8) (end 192.05 63.7) (width 0.15) (layer F.Cu) (net 248))
  (segment (start 193.55 73.3) (end 192.05 71.8) (width 0.15) (layer F.Cu) (net 248))
  (segment (start 195.1 73.3) (end 193.55 73.3) (width 0.15) (layer F.Cu) (net 248))
  (segment (start 192.75 71.05) (end 192.75 63.75) (width 0.15) (layer F.Cu) (net 249))
  (segment (start 194.2 72.5) (end 192.75 71.05) (width 0.15) (layer F.Cu) (net 249))
  (segment (start 195.1 72.5) (end 194.2 72.5) (width 0.15) (layer F.Cu) (net 249))
  (segment (start 195.1 71.7) (end 196.85 71.7) (width 0.15) (layer F.Cu) (net 250) (tstamp 618E4E42))
  (via (at 196.85 71.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 250) (tstamp 618E4E46))
  (segment (start 212.8 71.7) (end 214.55 71.7) (width 0.15) (layer F.Cu) (net 250) (tstamp 618F53B3))
  (via (at 214.55 71.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 250) (tstamp 618F53B8))
  (segment (start 211.9 71.7) (end 211.45 71.25) (width 0.15) (layer F.Cu) (net 250))
  (segment (start 211.45 71.25) (end 211.45 64.3) (width 0.15) (layer F.Cu) (net 250))
  (segment (start 212.8 71.7) (end 211.9 71.7) (width 0.15) (layer F.Cu) (net 250))
  (segment (start 196.85 71.7) (end 194.3 71.7) (width 0.15) (layer B.Cu) (net 250))
  (segment (start 206.25 71.7) (end 213.6 71.7) (width 0.15) (layer B.Cu) (net 250))
  (segment (start 205.95 71.4) (end 206.25 71.7) (width 0.15) (layer B.Cu) (net 250))
  (segment (start 205.05 71.2) (end 205.25 71.4) (width 0.15) (layer B.Cu) (net 250))
  (segment (start 205.25 71.4) (end 205.95 71.4) (width 0.15) (layer B.Cu) (net 250))
  (segment (start 213.6 71.7) (end 214.55 71.7) (width 0.15) (layer B.Cu) (net 250))
  (segment (start 204.15 71.7) (end 204.65 71.2) (width 0.15) (layer B.Cu) (net 250))
  (segment (start 204.65 71.2) (end 205.05 71.2) (width 0.15) (layer B.Cu) (net 250))
  (segment (start 196.85 71.7) (end 204.15 71.7) (width 0.15) (layer B.Cu) (net 250))
  (via (at 196.25 70.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 251) (tstamp 618E4E47))
  (segment (start 195.1 70.9) (end 196.25 70.9) (width 0.15) (layer F.Cu) (net 251) (tstamp 618E4E48))
  (via (at 213.95 70.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 251) (tstamp 618F53B5))
  (segment (start 212.8 70.9) (end 213.95 70.9) (width 0.15) (layer F.Cu) (net 251) (tstamp 618F53B7))
  (segment (start 212.8 70.9) (end 213.95 70.9) (width 0.15) (layer F.Cu) (net 251) (tstamp 6190C20B))
  (segment (start 195.1 70.9) (end 194.2 70.9) (width 0.15) (layer F.Cu) (net 251))
  (segment (start 194.2 70.9) (end 193.45 70.15) (width 0.15) (layer F.Cu) (net 251))
  (segment (start 193.45 70.15) (end 193.45 63.4) (width 0.15) (layer F.Cu) (net 251))
  (segment (start 196.25 70.9) (end 194.45 70.9) (width 0.15) (layer B.Cu) (net 251))
  (segment (start 206.35 70.9) (end 213.95 70.9) (width 0.15) (layer B.Cu) (net 251))
  (segment (start 205.85 70.4) (end 206.35 70.9) (width 0.15) (layer B.Cu) (net 251))
  (segment (start 205.25 70.4) (end 205.85 70.4) (width 0.15) (layer B.Cu) (net 251))
  (segment (start 205.05 70.6) (end 205.25 70.4) (width 0.15) (layer B.Cu) (net 251))
  (segment (start 204.3 70.6) (end 205.05 70.6) (width 0.15) (layer B.Cu) (net 251))
  (segment (start 204 70.9) (end 204.3 70.6) (width 0.15) (layer B.Cu) (net 251))
  (segment (start 196.25 70.9) (end 204 70.9) (width 0.15) (layer B.Cu) (net 251))
  (via (at 196.85 70.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 252) (tstamp 618E4E41))
  (segment (start 195.1 70.1) (end 196.85 70.1) (width 0.15) (layer F.Cu) (net 252) (tstamp 618E4E45))
  (via (at 214.55 70.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 252) (tstamp 618F53B1))
  (segment (start 212.8 70.1) (end 214.55 70.1) (width 0.15) (layer F.Cu) (net 252) (tstamp 618F53B4))
  (segment (start 196.85 70.1) (end 194.65 70.1) (width 0.15) (layer B.Cu) (net 252))
  (segment (start 213.6 70.1) (end 214.55 70.1) (width 0.15) (layer B.Cu) (net 252))
  (segment (start 213.4 70.3) (end 213.6 70.1) (width 0.15) (layer B.Cu) (net 252))
  (segment (start 206.65 70.3) (end 213.4 70.3) (width 0.15) (layer B.Cu) (net 252))
  (segment (start 206.15 69.8) (end 206.65 70.3) (width 0.15) (layer B.Cu) (net 252))
  (segment (start 205.25 69.8) (end 206.15 69.8) (width 0.15) (layer B.Cu) (net 252))
  (segment (start 205.05 69.6) (end 205.25 69.8) (width 0.15) (layer B.Cu) (net 252))
  (segment (start 204.35 69.6) (end 205.05 69.6) (width 0.15) (layer B.Cu) (net 252))
  (segment (start 203.85 70.1) (end 204.35 69.6) (width 0.15) (layer B.Cu) (net 252))
  (segment (start 196.85 70.1) (end 203.85 70.1) (width 0.15) (layer B.Cu) (net 252))
  (via (at 196.25 69.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 253) (tstamp 618E4E2E))
  (segment (start 195.1 69.3) (end 196.25 69.3) (width 0.15) (layer F.Cu) (net 253) (tstamp 618E4E2F))
  (via (at 213.95 69.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 253) (tstamp 618F53A3))
  (segment (start 212.8 69.3) (end 213.95 69.3) (width 0.15) (layer F.Cu) (net 253) (tstamp 618F53A4))
  (segment (start 212.8 69.3) (end 213.95 69.3) (width 0.15) (layer F.Cu) (net 253) (tstamp 6190CE27))
  (segment (start 196.25 69.3) (end 194.75 69.3) (width 0.15) (layer B.Cu) (net 253))
  (segment (start 203.75 69.3) (end 196.25 69.3) (width 0.15) (layer B.Cu) (net 253))
  (segment (start 204.05 69) (end 203.75 69.3) (width 0.15) (layer B.Cu) (net 253))
  (segment (start 205.25 68.8) (end 205.05 69) (width 0.15) (layer B.Cu) (net 253))
  (segment (start 206.05 68.8) (end 205.25 68.8) (width 0.15) (layer B.Cu) (net 253))
  (segment (start 206.55 69.3) (end 206.05 68.8) (width 0.15) (layer B.Cu) (net 253))
  (segment (start 205.05 69) (end 204.05 69) (width 0.15) (layer B.Cu) (net 253))
  (segment (start 213.95 69.3) (end 206.55 69.3) (width 0.15) (layer B.Cu) (net 253))
  (segment (start 195.1 68.5) (end 196.85 68.5) (width 0.15) (layer F.Cu) (net 254) (tstamp 618E4E2D))
  (via (at 196.85 68.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 254) (tstamp 618E4E30))
  (segment (start 212.8 68.5) (end 214.55 68.5) (width 0.15) (layer F.Cu) (net 254) (tstamp 618F53A1))
  (via (at 214.55 68.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 254) (tstamp 618F53A2))
  (segment (start 196.85 68.5) (end 195 68.5) (width 0.15) (layer B.Cu) (net 254))
  (segment (start 213.6 68.5) (end 214.55 68.5) (width 0.15) (layer B.Cu) (net 254))
  (segment (start 213.4 68.7) (end 213.6 68.5) (width 0.15) (layer B.Cu) (net 254))
  (segment (start 206.85 68.7) (end 213.4 68.7) (width 0.15) (layer B.Cu) (net 254))
  (segment (start 206.35 68.2) (end 206.85 68.7) (width 0.15) (layer B.Cu) (net 254))
  (segment (start 205.25 68.2) (end 206.35 68.2) (width 0.15) (layer B.Cu) (net 254))
  (segment (start 205.05 68) (end 205.25 68.2) (width 0.15) (layer B.Cu) (net 254))
  (segment (start 204.1 68) (end 205.05 68) (width 0.15) (layer B.Cu) (net 254))
  (segment (start 203.6 68.5) (end 204.1 68) (width 0.15) (layer B.Cu) (net 254))
  (segment (start 196.85 68.5) (end 203.6 68.5) (width 0.15) (layer B.Cu) (net 254))
  (via (at 196.25 67.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 255) (tstamp 618E4E27))
  (segment (start 195.1 67.7) (end 196.25 67.7) (width 0.15) (layer F.Cu) (net 255) (tstamp 618E4E28))
  (via (at 213.95 67.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 255) (tstamp 618F53A7))
  (segment (start 212.8 67.7) (end 213.95 67.7) (width 0.15) (layer F.Cu) (net 255) (tstamp 618F53A8))
  (segment (start 212.8 67.7) (end 213.95 67.7) (width 0.15) (layer F.Cu) (net 255) (tstamp 6190CE65))
  (segment (start 213.55 68.1) (end 213.95 67.7) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 207.15 68.1) (end 213.55 68.1) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 206.25 67.2) (end 207.15 68.1) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 205.25 67.2) (end 206.25 67.2) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 196.25 67.7) (end 194.8 67.7) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 205.25 67.2) (end 205.05 67.4) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 205.05 67.4) (end 204.65 67.4) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 204.65 67.4) (end 204.45 67.2) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 204.45 67.2) (end 197.9 67.2) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 197.4 67.7) (end 196.25 67.7) (width 0.15) (layer B.Cu) (net 255))
  (segment (start 197.9 67.2) (end 197.4 67.7) (width 0.15) (layer B.Cu) (net 255))
  (via (at 196.85 66.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 256) (tstamp 618E4E25))
  (segment (start 195.1 66.9) (end 196.85 66.9) (width 0.15) (layer F.Cu) (net 256) (tstamp 618E4E26))
  (segment (start 212.8 66.9) (end 214.55 66.9) (width 0.15) (layer F.Cu) (net 256) (tstamp 618F53A6))
  (via (at 214.55 66.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 256) (tstamp 618F53AA))
  (segment (start 196.85 66.9) (end 195.15 66.9) (width 0.15) (layer B.Cu) (net 256))
  (segment (start 213.6 66.9) (end 214.55 66.9) (width 0.15) (layer B.Cu) (net 256))
  (segment (start 213 67.5) (end 213.6 66.9) (width 0.15) (layer B.Cu) (net 256))
  (segment (start 207.45 67.5) (end 213 67.5) (width 0.15) (layer B.Cu) (net 256))
  (segment (start 206.55 66.6) (end 207.45 67.5) (width 0.15) (layer B.Cu) (net 256))
  (segment (start 205.25 66.6) (end 206.55 66.6) (width 0.15) (layer B.Cu) (net 256))
  (segment (start 205.05 66.4) (end 205.25 66.6) (width 0.15) (layer B.Cu) (net 256))
  (segment (start 197.8 66.4) (end 205.05 66.4) (width 0.15) (layer B.Cu) (net 256))
  (segment (start 197.3 66.9) (end 197.8 66.4) (width 0.15) (layer B.Cu) (net 256))
  (segment (start 196.85 66.9) (end 197.3 66.9) (width 0.15) (layer B.Cu) (net 256))
  (via (at 196.25 66.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 257))
  (segment (start 195.1 66.1) (end 196.25 66.1) (width 0.15) (layer F.Cu) (net 257))
  (via (at 213.95 66.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 257) (tstamp 618F53AD))
  (segment (start 212.8 66.1) (end 213.95 66.1) (width 0.15) (layer F.Cu) (net 257) (tstamp 618F53AE))
  (segment (start 196.25 66.1) (end 195.05 66.1) (width 0.15) (layer B.Cu) (net 257))
  (segment (start 212.7 66.9) (end 213.5 66.1) (width 0.15) (layer B.Cu) (net 257))
  (segment (start 205.25 65.6) (end 206.45 65.6) (width 0.15) (layer B.Cu) (net 257))
  (segment (start 213.5 66.1) (end 213.95 66.1) (width 0.15) (layer B.Cu) (net 257))
  (segment (start 207.75 66.9) (end 212.7 66.9) (width 0.15) (layer B.Cu) (net 257))
  (segment (start 206.45 65.6) (end 207.75 66.9) (width 0.15) (layer B.Cu) (net 257))
  (segment (start 205.25 65.6) (end 205.05 65.8) (width 0.15) (layer B.Cu) (net 257))
  (segment (start 205.05 65.8) (end 197.5 65.8) (width 0.15) (layer B.Cu) (net 257))
  (segment (start 197.2 66.1) (end 196.25 66.1) (width 0.15) (layer B.Cu) (net 257))
  (segment (start 197.5 65.8) (end 197.2 66.1) (width 0.15) (layer B.Cu) (net 257))
  (via (at 196.85 65.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 258))
  (segment (start 195.1 65.3) (end 196.85 65.3) (width 0.15) (layer F.Cu) (net 258))
  (via (at 214.55 65.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 258) (tstamp 618F53A5))
  (segment (start 212.8 65.3) (end 214.55 65.3) (width 0.15) (layer F.Cu) (net 258) (tstamp 618F53A9))
  (segment (start 213.4 65.3) (end 214.55 65.3) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 208.3 65.3) (end 208.3 65.9) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 205.25 65) (end 208 65) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 212.4 66.3) (end 213.4 65.3) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 208.3 65.9) (end 208.7 66.3) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 205.05 64.8) (end 205.25 65) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 197.35 64.8) (end 205.05 64.8) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 208 65) (end 208.3 65.3) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 208.7 66.3) (end 212.4 66.3) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 196.85 65.3) (end 197.35 64.8) (width 0.15) (layer B.Cu) (net 258))
  (segment (start 196.85 65.3) (end 195.5 65.3) (width 0.15) (layer B.Cu) (net 258))
  (via (at 204.85 65.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 259))
  (segment (start 206.6 65.3) (end 204.85 65.3) (width 0.15) (layer F.Cu) (net 259))
  (segment (start 224.3 65.3) (end 222.55 65.3) (width 0.15) (layer F.Cu) (net 259) (tstamp 618F53BA))
  (via (at 222.55 65.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 259) (tstamp 618F53BC))
  (segment (start 221.75 66.1) (end 222.55 65.3) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 214.65 66.1) (end 221.75 66.1) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 214.15 65.6) (end 214.65 66.1) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 213.55 65.6) (end 214.15 65.6) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 212.55 66.6) (end 213.55 65.6) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 206.6 65.3) (end 207.9 66.6) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 207.9 66.6) (end 212.55 66.6) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 204.85 65.3) (end 206.6 65.3) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 204.85 65.3) (end 197.55 65.3) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 197.55 65.3) (end 197.05 65.8) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 197.05 65.8) (end 196.65 65.8) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 196.65 65.8) (end 196.45 65.6) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 196.45 65.6) (end 195.2 65.6) (width 0.15) (layer B.Cu) (net 259))
  (segment (start 206.6 66.1) (end 205.45 66.1) (width 0.15) (layer F.Cu) (net 260) (tstamp 618E6DD9))
  (via (at 205.45 66.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 260) (tstamp 618E6DD0))
  (segment (start 224.3 66.1) (end 223.15 66.1) (width 0.15) (layer F.Cu) (net 260) (tstamp 618F53C5))
  (via (at 223.15 66.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 260) (tstamp 618F53C8))
  (segment (start 214.15 66.6) (end 214.35 66.4) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 222.85 66.4) (end 223.15 66.1) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 205.45 66.1) (end 206.5 66.1) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 213.45 66.6) (end 214.15 66.6) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 214.35 66.4) (end 222.85 66.4) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 212.85 67.2) (end 213.45 66.6) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 207.6 67.2) (end 212.85 67.2) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 206.5 66.1) (end 207.6 67.2) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 205.45 66.1) (end 197.65 66.1) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 197.65 66.1) (end 197.35 66.4) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 197.35 66.4) (end 196.65 66.4) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 196.65 66.4) (end 196.45 66.6) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 196.45 66.6) (end 195.2 66.6) (width 0.15) (layer B.Cu) (net 260))
  (segment (start 206.6 66.9) (end 204.85 66.9) (width 0.15) (layer F.Cu) (net 261) (tstamp 618E6DDC))
  (via (at 204.85 66.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 261) (tstamp 618E6DD3))
  (segment (start 224.3 66.9) (end 222.55 66.9) (width 0.15) (layer F.Cu) (net 261) (tstamp 618F53C4))
  (via (at 222.55 66.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 261) (tstamp 618F53C7))
  (segment (start 222.05 67.4) (end 222.55 66.9) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 214.35 67.4) (end 222.05 67.4) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 214.15 67.2) (end 214.35 67.4) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 206.4 66.9) (end 207.3 67.8) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 207.3 67.8) (end 213.15 67.8) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 213.75 67.2) (end 214.15 67.2) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 213.15 67.8) (end 213.75 67.2) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 204.85 66.9) (end 206.4 66.9) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 204.85 66.9) (end 197.75 66.9) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 197.75 66.9) (end 197.25 67.4) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 197.25 67.4) (end 196.65 67.4) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 196.65 67.4) (end 196.45 67.2) (width 0.15) (layer B.Cu) (net 261))
  (segment (start 196.45 67.2) (end 195.05 67.2) (width 0.15) (layer B.Cu) (net 261))
  (via (at 205.45 67.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 262) (tstamp 618E6DC4))
  (segment (start 206.6 67.7) (end 205.45 67.7) (width 0.15) (layer F.Cu) (net 262) (tstamp 618E6DCA))
  (segment (start 224.3 67.7) (end 223.15 67.7) (width 0.15) (layer F.Cu) (net 262) (tstamp 618F53CA))
  (via (at 223.15 67.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 262) (tstamp 618F53CC))
  (segment (start 214.35 68) (end 222.85 68) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 214.15 68.2) (end 214.35 68) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 213.45 68.2) (end 214.15 68.2) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 222.85 68) (end 223.15 67.7) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 213.25 68.4) (end 213.45 68.2) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 206.3 67.7) (end 207 68.4) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 207 68.4) (end 213.25 68.4) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 205.45 67.7) (end 206.3 67.7) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 205.45 67.7) (end 197.85 67.7) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 197.85 67.7) (end 197.55 68) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 197.55 68) (end 196.65 68) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 196.65 68) (end 196.45 68.2) (width 0.15) (layer B.Cu) (net 262))
  (segment (start 196.45 68.2) (end 194.9 68.2) (width 0.15) (layer B.Cu) (net 262))
  (via (at 204.85 68.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 263) (tstamp 618E6DC1))
  (segment (start 206.6 68.5) (end 204.85 68.5) (width 0.15) (layer F.Cu) (net 263) (tstamp 618E6DE5))
  (segment (start 224.3 68.5) (end 222.55 68.5) (width 0.15) (layer F.Cu) (net 263) (tstamp 618F53C1))
  (via (at 222.55 68.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 263) (tstamp 618F53CD))
  (segment (start 222.05 69) (end 222.55 68.5) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 214.35 69) (end 222.05 69) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 214.15 68.8) (end 214.35 69) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 213.75 68.8) (end 214.15 68.8) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 206.7 69) (end 213.55 69) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 206.2 68.5) (end 206.7 69) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 213.55 69) (end 213.75 68.8) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 204.85 68.5) (end 206.2 68.5) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 196.45 68.8) (end 194.9 68.8) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 203.575 69) (end 196.65 69) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 196.65 69) (end 196.45 68.8) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 204.075 68.5) (end 203.575 69) (width 0.15) (layer B.Cu) (net 263))
  (segment (start 204.85 68.5) (end 204.075 68.5) (width 0.15) (layer B.Cu) (net 263))
  (via (at 205.45 69.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 264) (tstamp 618E6DE2))
  (segment (start 206.6 69.3) (end 205.45 69.3) (width 0.15) (layer F.Cu) (net 264) (tstamp 618E6DE8))
  (segment (start 224.3 69.3) (end 223.15 69.3) (width 0.15) (layer F.Cu) (net 264) (tstamp 618F53C0))
  (via (at 223.15 69.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 264) (tstamp 618F53C2))
  (segment (start 222.85 69.6) (end 223.15 69.3) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 214.35 69.6) (end 222.85 69.6) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 213.45 69.8) (end 214.15 69.8) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 214.15 69.8) (end 214.35 69.6) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 205.45 69.3) (end 206.1 69.3) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 213.25 70) (end 213.45 69.8) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 206.1 69.3) (end 206.8 70) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 206.8 70) (end 213.25 70) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 196.45 69.8) (end 194.8 69.8) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 196.65 69.6) (end 196.45 69.8) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 203.9 69.6) (end 196.65 69.6) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 204.2 69.3) (end 203.9 69.6) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 205.45 69.3) (end 204.2 69.3) (width 0.15) (layer B.Cu) (net 264))
  (segment (start 206.6 70.1) (end 204.85 70.1) (width 0.15) (layer F.Cu) (net 265) (tstamp 618E6DBB))
  (via (at 204.85 70.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 265) (tstamp 618E6DCD))
  (via (at 222.55 70.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 265) (tstamp 618F53C9))
  (segment (start 224.3 70.1) (end 222.55 70.1) (width 0.15) (layer F.Cu) (net 265) (tstamp 618F53CF))
  (segment (start 214.35 70.6) (end 222.05 70.6) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 214.15 70.4) (end 214.35 70.6) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 213.75 70.4) (end 214.15 70.4) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 213.55 70.6) (end 213.75 70.4) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 206.5 70.6) (end 213.55 70.6) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 206 70.1) (end 206.5 70.6) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 222.05 70.6) (end 222.55 70.1) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 204.85 70.1) (end 206 70.1) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 196.45 70.4) (end 194.55 70.4) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 196.65 70.6) (end 196.45 70.4) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 203.85 70.6) (end 196.65 70.6) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 204.35 70.1) (end 203.85 70.6) (width 0.15) (layer B.Cu) (net 265))
  (segment (start 204.85 70.1) (end 204.35 70.1) (width 0.15) (layer B.Cu) (net 265))
  (via (at 205.45 70.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 266) (tstamp 618E6DEE))
  (segment (start 206.6 70.9) (end 205.45 70.9) (width 0.15) (layer F.Cu) (net 266) (tstamp 618E6DB8))
  (via (at 223.15 70.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 266) (tstamp 618F53BE))
  (segment (start 224.3 70.9) (end 223.15 70.9) (width 0.15) (layer F.Cu) (net 266) (tstamp 618F53D0))
  (segment (start 205.45 70.9) (end 204.5 70.9) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 204.5 70.9) (end 204.2 71.2) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 204.2 71.2) (end 196.65 71.2) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 196.65 71.2) (end 196.45 71.4) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 196.45 71.4) (end 194.3 71.4) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 222.85 71.2) (end 223.15 70.9) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 214.15 71.4) (end 214.35 71.2) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 206.4 71.4) (end 214.15 71.4) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 214.35 71.2) (end 222.85 71.2) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 205.9 70.9) (end 206.4 71.4) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 205.45 70.9) (end 205.9 70.9) (width 0.15) (layer B.Cu) (net 266))
  (segment (start 206.6 71.7) (end 204.85 71.7) (width 0.15) (layer F.Cu) (net 267) (tstamp 618E6DF1))
  (via (at 204.85 71.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 267) (tstamp 618E6DEB))
  (segment (start 224.3 71.7) (end 222.55 71.7) (width 0.15) (layer F.Cu) (net 267) (tstamp 618F53BD))
  (via (at 222.55 71.7) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 267) (tstamp 618F53BF))
  (segment (start 196.65 72.2) (end 196.45 72) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 204.35 72.2) (end 196.65 72.2) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 196.45 72) (end 194.3 72) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 204.85 71.7) (end 204.35 72.2) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 221.55 71.7) (end 222.55 71.7) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 221.05 72.2) (end 221.55 71.7) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 214.35 72.2) (end 221.05 72.2) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 214.15 72) (end 214.35 72.2) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 206.1 72) (end 214.15 72) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 205.8 71.7) (end 206.1 72) (width 0.15) (layer B.Cu) (net 267))
  (segment (start 204.85 71.7) (end 205.8 71.7) (width 0.15) (layer B.Cu) (net 267))
  (via (at 205.45 72.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 268) (tstamp 618E6DC7))
  (segment (start 206.6 72.5) (end 205.45 72.5) (width 0.15) (layer F.Cu) (net 268) (tstamp 618E6DD6))
  (segment (start 224.3 72.5) (end 223.15 72.5) (width 0.15) (layer F.Cu) (net 268) (tstamp 618F53C6))
  (via (at 223.15 72.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 268) (tstamp 618F53CB))
  (segment (start 222.05 72.5) (end 223.15 72.5) (width 0.15) (layer B.Cu) (net 268))
  (segment (start 221.55 73) (end 222.05 72.5) (width 0.15) (layer B.Cu) (net 268))
  (segment (start 206.2 73) (end 221.55 73) (width 0.15) (layer B.Cu) (net 268))
  (segment (start 205.7 72.5) (end 206.2 73) (width 0.15) (layer B.Cu) (net 268))
  (segment (start 205.45 72.5) (end 205.7 72.5) (width 0.15) (layer B.Cu) (net 268))
  (segment (start 205.45 72.5) (end 194.3 72.5) (width 0.15) (layer B.Cu) (net 268))
  (via (at 204.85 73.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 269) (tstamp 618E6DBE))
  (segment (start 206.6 73.3) (end 204.85 73.3) (width 0.15) (layer F.Cu) (net 269) (tstamp 618E6DDF))
  (segment (start 221.95 73.3) (end 204.85 73.3) (width 0.15) (layer B.Cu) (net 269))
  (segment (start 224.3 73.3) (end 221.95 73.3) (width 0.15) (layer F.Cu) (net 269))
  (via (at 221.95 73.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 269))
  (segment (start 204.85 73.3) (end 204.35 72.8) (width 0.15) (layer B.Cu) (net 269))
  (segment (start 204.35 72.8) (end 194 72.8) (width 0.15) (layer B.Cu) (net 269))
  (segment (start 206.6 74.1) (end 207.5 74.1) (width 0.15) (layer F.Cu) (net 270))
  (segment (start 207.5 74.1) (end 209.75 71.85) (width 0.15) (layer F.Cu) (net 270))
  (segment (start 209.75 71.85) (end 209.75 64) (width 0.15) (layer F.Cu) (net 270))
  (via (at 222.55 74.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 287))
  (segment (start 224.3 74.1) (end 222.55 74.1) (width 0.15) (layer F.Cu) (net 287))
  (segment (start 222.55 74.1) (end 195 74.1) (width 0.15) (layer B.Cu) (net 287))
  (segment (start 211.25 72.5) (end 210.75 72) (width 0.15) (layer F.Cu) (net 288))
  (segment (start 210.75 72) (end 210.75 64.3) (width 0.15) (layer F.Cu) (net 288))
  (segment (start 212.8 72.5) (end 211.25 72.5) (width 0.15) (layer F.Cu) (net 288))
  (segment (start 210.05 72.7) (end 210.05 64.3) (width 0.15) (layer F.Cu) (net 289))
  (segment (start 210.65 73.3) (end 210.05 72.7) (width 0.15) (layer F.Cu) (net 289))
  (segment (start 212.8 73.3) (end 210.65 73.3) (width 0.15) (layer F.Cu) (net 289))
  (segment (start 203 87.85) (end 203 89.7) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 194.15 87.85) (end 194.15 89.7) (width 0.15) (layer F.Cu) (net 445) (tstamp 6192C14A))
  (segment (start 211.85 87.85) (end 211.85 89.7) (width 0.15) (layer F.Cu) (net 445) (tstamp 6192C15A))
  (segment (start 220.15 90.25) (end 220.7 89.7) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 220.7 89.7) (end 220.7 87.85) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 212.4 90.25) (end 220.15 90.25) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 211.85 89.7) (end 212.4 90.25) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 203.55 90.25) (end 203 89.7) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 211.3 90.25) (end 203.55 90.25) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 211.85 89.7) (end 211.3 90.25) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 194.7 90.25) (end 194.15 89.7) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 202.45 90.25) (end 194.7 90.25) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 203 89.7) (end 202.45 90.25) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 194.15 89.7) (end 193.6 90.25) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 220.7 89.7) (end 221.25 90.25) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 221.25 90.25) (end 226.5 90.25) (width 0.15) (layer F.Cu) (net 445))
  (segment (start 202.35 92.45) (end 203.45 91.35) (width 0.15) (layer F.Cu) (net 446))
  (segment (start 202.35 93.75) (end 202.35 92.45) (width 0.15) (layer F.Cu) (net 446))
  (segment (start 220.05 93.75) (end 220.05 92.45) (width 0.15) (layer F.Cu) (net 446) (tstamp 61935583))
  (segment (start 193.5 92.45) (end 194.6 91.35) (width 0.15) (layer F.Cu) (net 446) (tstamp 61935596))
  (segment (start 211.2 92.45) (end 212.3 91.35) (width 0.15) (layer F.Cu) (net 446) (tstamp 6193559D))
  (segment (start 211.2 93.75) (end 211.2 92.45) (width 0.15) (layer F.Cu) (net 446) (tstamp 619355A9))
  (segment (start 193.5 93.75) (end 193.5 92.45) (width 0.15) (layer F.Cu) (net 446) (tstamp 619355B9))
  (segment (start 201.25 91.35) (end 202.35 92.45) (width 0.15) (layer F.Cu) (net 446))
  (segment (start 194.6 91.35) (end 201.25 91.35) (width 0.15) (layer F.Cu) (net 446))
  (segment (start 210.1 91.35) (end 211.2 92.45) (width 0.15) (layer F.Cu) (net 446))
  (segment (start 203.45 91.35) (end 210.1 91.35) (width 0.15) (layer F.Cu) (net 446))
  (segment (start 218.95 91.35) (end 220.05 92.45) (width 0.15) (layer F.Cu) (net 446))
  (segment (start 212.3 91.35) (end 218.95 91.35) (width 0.15) (layer F.Cu) (net 446))
  (segment (start 220.05 92.45) (end 221.15 91.35) (width 0.15) (layer F.Cu) (net 446) (tstamp 61935572))
  (segment (start 221.15 91.35) (end 226.6 91.35) (width 0.15) (layer F.Cu) (net 446))
  (segment (start 208.05 61.3) (end 208.05 62) (width 0.5) (layer F.Cu) (net 447) (tstamp 6178EF16))
  (via (at 208.05 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 6178EF10))
  (segment (start 208.05 61.3) (end 208.05 60.6) (width 0.5) (layer F.Cu) (net 447) (tstamp 6178EF0A))
  (via (at 208.05 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 6178EF04))
  (segment (start 209.15 61.3) (end 209.15 60.6) (width 0.5) (layer F.Cu) (net 447) (tstamp 6178EF2E))
  (segment (start 209.15 61.3) (end 209.15 62) (width 0.5) (layer F.Cu) (net 447) (tstamp 6178EF1C))
  (via (at 209.15 60.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 6178EF2B))
  (via (at 209.15 62) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 6178EF28))
  (via (at 210.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447))
  (segment (start 210.1 50.55) (end 210.6 51.05) (width 0.4) (layer F.Cu) (net 447))
  (via (at 209.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447))
  (segment (start 209.1 51.55) (end 209.6 52.05) (width 0.4) (layer F.Cu) (net 447))
  (via (at 206.6 52.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447))
  (segment (start 207.1 51.55) (end 206.6 52.05) (width 0.4) (layer F.Cu) (net 447))
  (via (at 207.6 51.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447))
  (segment (start 208.1 50.55) (end 207.6 51.05) (width 0.4) (layer F.Cu) (net 447))
  (via (at 209.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447))
  (segment (start 209.1 49.55) (end 209.6 49.05) (width 0.4) (layer F.Cu) (net 447))
  (via (at 210.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447))
  (segment (start 210.1 48.55) (end 210.6 48.05) (width 0.4) (layer F.Cu) (net 447))
  (via (at 207.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447))
  (segment (start 208.1 48.55) (end 207.6 48.05) (width 0.4) (layer F.Cu) (net 447))
  (via (at 206.6 49.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447))
  (segment (start 207.1 49.55) (end 206.6 49.05) (width 0.4) (layer F.Cu) (net 447))
  (segment (start 208.05 59.5) (end 208.6 58.95) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 209.15 59.5) (end 208.6 58.95) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 209.15 60.6) (end 209.15 59.5) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.05 60.6) (end 208.05 59.5) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 206.6 49.05) (end 206.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 48.05) (end 208.6 48.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 49.05) (end 209.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 49.05) (end 210.1 48.55) (width 0.4) (layer F.Cu) (net 447))
  (segment (start 207.6 51.05) (end 207.1 51.55) (width 0.4) (layer F.Cu) (net 447))
  (segment (start 209.35 49.05) (end 208.6 49.8) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 49.05) (end 209.35 49.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 49.8) (end 208.6 49.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.6 50.3) (end 208.6 49.8) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.6 49.3) (end 208.6 50.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 49.05) (end 209.6 49.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 210.6 50.05) (end 211.1 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 210.6 50.55) (end 211.1 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 210.6 51.05) (end 210.6 50.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 210.6 50.55) (end 210.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 210.1 50.05) (end 210.6 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 210.6 50.55) (end 210.1 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 50.05) (end 210.1 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.1 52.05) (end 208.6 51.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 52.05) (end 208.6 51.55) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.6 52.05) (end 209.1 52.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.1 52.05) (end 208.6 52.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.1 52.05) (end 208.6 52.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 52.55) (end 208.6 52.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 207.6 51.05) (end 208.6 51.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 51.05) (end 208.6 50.3) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.6 51.55) (end 208.6 51.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 207.6 51.05) (end 207.6 50.8) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 50.8) (end 208.35 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.35 50.05) (end 209.6 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 207.6 50.05) (end 208.35 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 207.85 51.05) (end 208.6 50.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 51.05) (end 207.85 51.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.1 48.05) (end 208.6 48.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 48.05) (end 208.1 48.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 48.55) (end 208.6 48.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.6 49.05) (end 208.6 48.55) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.1 48.05) (end 208.6 47.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 47.55) (end 208.6 47.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.6 48.05) (end 208.6 47.55) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 206.6 49.55) (end 207.1 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 206.6 49.05) (end 206.6 49.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.1 50.05) (end 207.6 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 206.6 50.05) (end 207.1 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 206.6 49.05) (end 205.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 206.6 49.55) (end 206.1 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 206.1 50.05) (end 206.6 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 205.6 50.05) (end 206.1 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.6 52.05) (end 208.6 53.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 53.05) (end 208.6 52.55) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.1 49.55) (end 209.1 50.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.85 49.8) (end 208.1 49.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 50.05) (end 207.85 49.8) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.35 49.8) (end 207.85 49.8) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 206.6 49.05) (end 207.35 49.8) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.35 49.8) (end 207.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 52.05) (end 208.85 51.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.85 51.3) (end 208.6 51.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 51.05) (end 208.85 50.8) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.85 50.8) (end 208.85 51.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.85 50.8) (end 209.1 50.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 210.6 51.05) (end 211.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 211.1 50.05) (end 211.6 50.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.1 49.05) (end 208.6 49.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 49.05) (end 209.1 49.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.35 50.3) (end 209.85 50.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.1 50.55) (end 209.35 50.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.85 50.3) (end 209.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 210.6 51.05) (end 209.85 50.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.35 50.3) (end 209.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 51.05) (end 206.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.1 50.05) (end 207.6 50.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 50.55) (end 207.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 51.05) (end 207.6 50.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.35 48.8) (end 208.35 49.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.35 49.3) (end 208.6 49.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.1 49.55) (end 208.35 49.3) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 48.05) (end 208.35 48.8) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.35 48.8) (end 208.6 49.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 49.05) (end 210.6 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 49.3) (end 209.6 49.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.1 50.55) (end 209.1 49.55) (width 0.4) (layer F.Cu) (net 447))
  (segment (start 210.1 50.55) (end 210.1 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 210.1 50.55) (end 209.6 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 209.1 49.55) (end 209.1 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 209.1 49.55) (end 208.6 49.55) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.6 49.55) (end 208.6 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.1 50.55) (end 208.1 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.6 50.05) (end 208.1 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.1 50.55) (end 208.6 50.55) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.6 50.55) (end 208.6 58.95) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.6 50.05) (end 208.6 50.55) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.1 48.55) (end 208.6 48.55) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.1 48.55) (end 208.6 49.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.6 50.3) (end 208.85 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.85 50.05) (end 209.1 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.6 50.05) (end 208.85 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 208.35 50.05) (end 208.6 49.8) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 207.6 51.05) (end 208.6 52.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.1 51.05) (end 208.6 51.55) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 51.05) (end 208.1 51.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 48.55) (end 209.1 49.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 49.05) (end 209.2 49.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.9 47.75) (end 208.6 47.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.6 48.05) (end 207.9 47.75) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 52.05) (end 208.925 51.375) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.275 51.375) (end 207.6 51.05) (width 0.6) (layer B.Cu) (net 447))
  (segment (start 208.925 51.375) (end 207.275 51.375) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 206.6 52.05) (end 207.275 51.375) (width 0.6) (layer B.Cu) (net 447))
  (segment (start 207.275 50.725) (end 207.275 51.375) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 206.6 50.05) (end 207.275 50.725) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 210.6 48.05) (end 209.6 49.05) (width 0.6) (layer B.Cu) (net 447))
  (segment (start 209.2 49.05) (end 207.9 47.75) (width 0.5) (layer B.Cu) (net 447) (tstamp 6199C7E4))
  (segment (start 209.925 48.725) (end 209.925 49.875) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 210.6 48.05) (end 209.925 48.725) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.925 49.875) (end 210.1 50.05) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.6 49.55) (end 209.925 49.875) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 47.05) (end 208.6 48) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 209.325 48.725) (end 209.925 48.725) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 208.6 48) (end 209.325 48.725) (width 0.5) (layer B.Cu) (net 447))
  (segment (start 207.9 60.45) (end 208.05 60.6) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.05 60.6) (end 207.9 60.75) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 207.9 61.85) (end 208.05 62) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 207.9 60.75) (end 207.9 61.85) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.05 62) (end 208.05 60.6) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.15 62) (end 209.15 60.6) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.3 60.45) (end 209.15 60.6) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.3 61.85) (end 209.3 60.45) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.15 62) (end 209.3 61.85) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.3 59.45) (end 209.3 60.45) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 207.9 59.45) (end 207.9 61.85) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.6 53.05) (end 208.6 58.75) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.9 59.05) (end 208.3 59.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.3 59.05) (end 207.9 59.45) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.6 58.75) (end 208.3 59.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.6 58.75) (end 208.9 59.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.9 59.05) (end 209.3 59.45) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.05 60.6) (end 208.05 60.2) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 207.9 60.05) (end 207.9 59.45) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 208.05 60.2) (end 207.9 60.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.15 60.6) (end 209.15 60.2) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.3 60.05) (end 209.3 59.45) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 209.15 60.2) (end 209.3 60.05) (width 0.55) (layer B.Cu) (net 447))
  (segment (start 220.4 49.35) (end 219 49.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A31))
  (segment (start 220.55 49.5) (end 220.4 49.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A32))
  (segment (start 220.4 50.75) (end 220.55 50.6) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A33))
  (segment (start 219.3 50.75) (end 220.4 50.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A34))
  (segment (start 219 50.75) (end 219.15 50.6) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A35))
  (segment (start 219 49.35) (end 219.15 49.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A36))
  (segment (start 209.1 50.05) (end 217.5 50.05) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AA5A37))
  (segment (start 218.05 50.6) (end 217.5 50.05) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AA5A38))
  (segment (start 219.15 50.6) (end 218.05 50.6) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AA5A39))
  (segment (start 219.15 49.5) (end 218.05 49.5) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AA5A3A))
  (segment (start 218.05 49.5) (end 217.5 50.05) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AA5A3B))
  (segment (start 220.55 49.5) (end 219.15 49.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A3C))
  (via (at 220.55 49.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AA5A3D))
  (segment (start 219.85 49.5) (end 220.55 49.5) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AA5A3F))
  (via (at 219.15 49.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AA5A41))
  (segment (start 219.85 49.5) (end 219.15 49.5) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AA5A42))
  (segment (start 219.85 50.6) (end 219.15 50.6) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AA5A47))
  (segment (start 219.85 50.6) (end 220.55 50.6) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AA5A48))
  (via (at 220.55 50.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AA5A49))
  (via (at 219.15 50.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AA5A4B))
  (segment (start 220.55 50.6) (end 219.15 50.6) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A4C))
  (segment (start 219.15 50.6) (end 219.3 50.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A4D))
  (segment (start 218 49.35) (end 219 49.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A4E))
  (segment (start 217.3 50.05) (end 217.6 50.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A4F))
  (segment (start 217.6 50.35) (end 218 50.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A50))
  (segment (start 217.6 49.75) (end 217.6 50.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A51))
  (segment (start 217.6 49.75) (end 218 49.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A52))
  (segment (start 217.3 50.05) (end 217.6 49.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A53))
  (segment (start 211.6 50.05) (end 217.3 50.05) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A54))
  (segment (start 218 50.75) (end 220.4 50.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A55))
  (segment (start 219.15 50.6) (end 218.75 50.6) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A56))
  (segment (start 219.15 49.5) (end 218.75 49.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AA5A57))
  (segment (start 208.6 41.35) (end 208.9 41.05) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A17))
  (segment (start 209.15 38.8) (end 209.15 38.1) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AB4A18))
  (segment (start 209.3 38.25) (end 209.15 38.1) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A1A))
  (segment (start 209.15 39.5) (end 209.3 39.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A1B))
  (via (at 208.05 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AB4A1C))
  (segment (start 209.15 39.5) (end 209.15 40.6) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4A1D))
  (segment (start 209.15 38.1) (end 209.15 39.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A1E))
  (via (at 208.05 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AB4A1F))
  (segment (start 209.15 40.6) (end 208.6 41.15) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4A20))
  (segment (start 208.05 38.1) (end 208.05 39.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A21))
  (segment (start 208.05 39.5) (end 208.05 40.6) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4A24))
  (segment (start 209.3 39.65) (end 209.15 39.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A25))
  (segment (start 208.05 40.6) (end 208.6 41.15) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4A27))
  (segment (start 207.9 39.65) (end 208.05 39.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A28))
  (segment (start 208.6 49.55) (end 208.6 41.15) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4A29))
  (segment (start 207.9 38.25) (end 207.9 39.65) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A2A))
  (segment (start 209.15 38.8) (end 209.15 39.5) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AB4A2B))
  (segment (start 208.05 38.8) (end 208.05 39.5) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AB4A2C))
  (segment (start 207.9 40.65) (end 207.9 39.65) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A2E))
  (segment (start 208.05 38.1) (end 207.9 38.25) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A2F))
  (segment (start 209.3 39.35) (end 209.3 38.25) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A30))
  (via (at 209.15 38.1) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AB4A31))
  (segment (start 208.05 38.8) (end 208.05 38.1) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AB4A34))
  (via (at 209.15 39.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AB4A35))
  (segment (start 208.05 39.5) (end 208.05 39.9) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A36))
  (segment (start 208.3 41.05) (end 208.9 41.05) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A37))
  (segment (start 209.15 39.5) (end 209.15 39.9) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A38))
  (segment (start 208.6 41.35) (end 208.3 41.05) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A39))
  (segment (start 209.3 40.65) (end 209.3 38.25) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A3A))
  (segment (start 208.3 41.05) (end 207.9 40.65) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A3B))
  (segment (start 208.6 47.05) (end 208.6 41.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A3C))
  (segment (start 208.9 41.05) (end 209.3 40.65) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4A3E))
  (segment (start 197.9 49.35) (end 196.8 49.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AE6))
  (segment (start 197.35 50.6) (end 198.05 50.6) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AB4AE8))
  (via (at 196.65 49.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AB4AE9))
  (segment (start 196.65 50.6) (end 196.8 50.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AEC))
  (segment (start 199.2 50.75) (end 198.2 50.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AED))
  (via (at 198.05 50.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AB4AEE))
  (segment (start 199.9 50.05) (end 199.6 49.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AEF))
  (segment (start 198.05 49.5) (end 197.9 49.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AF0))
  (segment (start 196.8 49.35) (end 196.65 49.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AF2))
  (segment (start 198.05 49.5) (end 199.15 49.5) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4AF3))
  (segment (start 197.35 49.5) (end 196.65 49.5) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AB4AF4))
  (segment (start 196.65 49.5) (end 198.05 49.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AF5))
  (via (at 196.65 50.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AB4AF6))
  (segment (start 199.15 49.5) (end 199.7 50.05) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4AF7))
  (segment (start 196.65 50.6) (end 198.05 50.6) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AF8))
  (segment (start 198.05 50.6) (end 199.15 50.6) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4AFB))
  (segment (start 198.2 49.35) (end 198.05 49.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AFC))
  (segment (start 199.15 50.6) (end 199.7 50.05) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4AFE))
  (segment (start 198.2 50.75) (end 198.05 50.6) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4AFF))
  (segment (start 208.1 50.05) (end 199.7 50.05) (width 0.3) (layer F.Cu) (net 447) (tstamp 61AB4B00))
  (segment (start 196.8 50.75) (end 198.2 50.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4B01))
  (segment (start 197.35 49.5) (end 198.05 49.5) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AB4B02))
  (segment (start 199.6 50.35) (end 199.6 49.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4B03))
  (segment (start 198.05 49.5) (end 198.45 49.5) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4B04))
  (segment (start 199.6 50.35) (end 199.2 50.75) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4B06))
  (segment (start 199.9 50.05) (end 199.6 50.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4B07))
  (segment (start 197.35 50.6) (end 196.65 50.6) (width 0.5) (layer F.Cu) (net 447) (tstamp 61AB4B09))
  (segment (start 198.05 50.6) (end 198.45 50.6) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4B0A))
  (segment (start 205.6 50.05) (end 199.9 50.05) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4B0B))
  (segment (start 199.6 49.75) (end 199.2 49.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4B0C))
  (segment (start 199.2 49.35) (end 196.8 49.35) (width 0.55) (layer B.Cu) (net 447) (tstamp 61AB4B0D))
  (via (at 198.05 49.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 447) (tstamp 61AB4B0E))
  (segment (start 207.1 49.55) (end 207.1 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 207.1 49.55) (end 207.6 50.05) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 209.1 51.55) (end 208.6 51.55) (width 0.3) (layer F.Cu) (net 447))
  (segment (start 209.1 51.55) (end 208.6 51.05) (width 0.3) (layer F.Cu) (net 447))
  (via (at 202.6 55.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 455))
  (segment (start 203.1 54.55) (end 202.6 55.05) (width 0.15) (layer F.Cu) (net 455))
  (segment (start 202.6 55.05) (end 202.6 55.3) (width 0.15) (layer B.Cu) (net 455))
  (segment (start 202.6 55.3) (end 201.1 56.8) (width 0.15) (layer B.Cu) (net 455))
  (segment (start 215.6 56.05) (end 217.1 56.05) (width 0.15) (layer F.Cu) (net 456))
  (segment (start 215.1 55.55) (end 215.6 56.05) (width 0.15) (layer F.Cu) (net 456))
  (via (at 217.1 56.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 456))
  (segment (start 217.1 56.05) (end 216.7 56.05) (width 0.15) (layer B.Cu) (net 456))
  (segment (start 216.7 56.05) (end 216.05 56.7) (width 0.15) (layer B.Cu) (net 456))
  (segment (start 216.05 56.7) (end 216.05 58.85) (width 0.15) (layer B.Cu) (net 456))
  (via (at 216.6 57.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 457))
  (segment (start 216.1 56.55) (end 216.6 57.05) (width 0.15) (layer F.Cu) (net 457))
  (via (at 216.8 47.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 458))
  (segment (start 216.1 47.55) (end 216.8 47.55) (width 0.15) (layer F.Cu) (net 458))
  (segment (start 218.6 47.25) (end 217.1 47.25) (width 0.15) (layer B.Cu) (net 458))
  (segment (start 218.9 46.95) (end 218.6 47.25) (width 0.15) (layer B.Cu) (net 458))
  (segment (start 217.1 47.25) (end 216.8 47.55) (width 0.15) (layer B.Cu) (net 458))
  (segment (start 220.7 46.95) (end 218.9 46.95) (width 0.15) (layer B.Cu) (net 458))
  (via (at 214.6 45.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 459))
  (segment (start 214.1 45.55) (end 214.6 45.05) (width 0.15) (layer F.Cu) (net 459))
  (segment (start 215 44.4) (end 215 41.4) (width 0.15) (layer B.Cu) (net 459))
  (segment (start 214.6 44.8) (end 215 44.4) (width 0.15) (layer B.Cu) (net 459))
  (segment (start 214.6 45.05) (end 214.6 44.8) (width 0.15) (layer B.Cu) (net 459))
  (via (at 213.6 47.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 460))
  (segment (start 213.1 47.55) (end 213.6 47.05) (width 0.15) (layer F.Cu) (net 460))
  (via (at 196.977 104.902) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 463))
  (segment (start 195.7815 104.902) (end 196.977 104.902) (width 0.15) (layer F.Cu) (net 463))
  (via (at 196.215 136.779) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 463) (tstamp 61996A05))
  (segment (start 194.1815 136.779) (end 196.215 136.779) (width 0.15) (layer F.Cu) (net 463) (tstamp 61996A06))
  (segment (start 199.7075 98.933) (end 200.7235 98.933) (width 0.15) (layer F.Cu) (net 463))
  (segment (start 198.0565 103.8225) (end 198.0565 100.584) (width 0.15) (layer F.Cu) (net 463))
  (segment (start 198.0565 100.584) (end 199.7075 98.933) (width 0.15) (layer F.Cu) (net 463))
  (segment (start 196.977 104.902) (end 198.0565 103.8225) (width 0.15) (layer F.Cu) (net 463))
  (segment (start 212.9155 134.4295) (end 212.9155 127.3175) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 209.6135 137.7315) (end 212.9155 134.4295) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 197.104 136.779) (end 198.0565 137.7315) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 198.0565 137.7315) (end 209.6135 137.7315) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 196.215 136.779) (end 197.104 136.779) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 196.977 104.902) (end 200.8505 108.7755) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 200.8505 108.7755) (end 200.8505 120.777) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 200.8505 120.777) (end 203.2635 123.19) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 208.788 123.19) (end 212.9155 127.3175) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 203.2635 123.19) (end 208.788 123.19) (width 0.15) (layer B.Cu) (net 463))
  (segment (start 203.65 93.75) (end 203.65 94.85) (width 0.15) (layer F.Cu) (net 463))
  (segment (start 203.65 94.85) (end 202.95 95.55) (width 0.15) (layer F.Cu) (net 463))
  (segment (start 202.95 95.55) (end 202.95 98) (width 0.15) (layer F.Cu) (net 463))
  (segment (start 203 93.75) (end 203 95.05) (width 0.15) (layer F.Cu) (net 464))
  (segment (start 203 95.05) (end 202.65 95.4) (width 0.15) (layer F.Cu) (net 464))
  (segment (start 202.65 95.4) (end 202.65 98.4) (width 0.15) (layer F.Cu) (net 464))
  (via (at 197.4215 100.7745) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 464))
  (via (at 197.0405 137.414) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 464) (tstamp 61996A07))
  (segment (start 194.1815 137.414) (end 197.0405 137.414) (width 0.15) (layer F.Cu) (net 464) (tstamp 61996A08))
  (segment (start 197.4215 101.992) (end 197.4215 100.7745) (width 0.15) (layer F.Cu) (net 464))
  (segment (start 197.4215 100.7745) (end 199.5805 98.6155) (width 0.15) (layer F.Cu) (net 464))
  (segment (start 199.5805 98.6155) (end 200.787 98.6155) (width 0.15) (layer F.Cu) (net 464))
  (segment (start 197.6755 138.049) (end 197.0405 137.414) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 213.233 134.5565) (end 209.7405 138.049) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 210.82 107.823) (end 210.82 121.539) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 209.7405 138.049) (end 197.6755 138.049) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 200.152 105.918) (end 208.915 105.918) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 208.915 105.918) (end 210.82 107.823) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 213.233 123.952) (end 213.233 134.5565) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 197.866 101.219) (end 197.866 103.632) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 197.866 103.632) (end 200.152 105.918) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 210.82 121.539) (end 213.233 123.952) (width 0.15) (layer B.Cu) (net 464))
  (segment (start 197.4215 100.7745) (end 197.866 101.219) (width 0.15) (layer B.Cu) (net 464))
  (via (at 198.6915 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 465))
  (segment (start 198.6915 101.992) (end 198.6915 103.1875) (width 0.15) (layer F.Cu) (net 465))
  (via (at 195.3895 138.049) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 465))
  (segment (start 194.1815 138.049) (end 195.3895 138.049) (width 0.15) (layer F.Cu) (net 465))
  (segment (start 204.3 93.75) (end 204.3 94.65) (width 0.15) (layer F.Cu) (net 465))
  (segment (start 204.3 94.65) (end 203.25 95.7) (width 0.15) (layer F.Cu) (net 465))
  (segment (start 203.25 95.7) (end 203.25 98.05) (width 0.15) (layer F.Cu) (net 465))
  (segment (start 201.1045 105.6005) (end 198.6915 103.1875) (width 0.15) (layer B.Cu) (net 465))
  (segment (start 209.042 105.6005) (end 201.1045 105.6005) (width 0.15) (layer B.Cu) (net 465))
  (segment (start 211.1375 107.696) (end 209.042 105.6005) (width 0.15) (layer B.Cu) (net 465))
  (segment (start 211.1375 121.412) (end 211.1375 107.696) (width 0.15) (layer B.Cu) (net 465))
  (segment (start 213.5505 123.825) (end 211.1375 121.412) (width 0.15) (layer B.Cu) (net 465))
  (segment (start 213.5505 134.6835) (end 213.5505 123.825) (width 0.15) (layer B.Cu) (net 465))
  (segment (start 209.8675 138.3665) (end 213.5505 134.6835) (width 0.15) (layer B.Cu) (net 465))
  (segment (start 196.596 138.3665) (end 209.8675 138.3665) (width 0.15) (layer B.Cu) (net 465))
  (segment (start 196.2785 138.049) (end 196.596 138.3665) (width 0.15) (layer B.Cu) (net 465))
  (segment (start 195.3895 138.049) (end 196.2785 138.049) (width 0.15) (layer B.Cu) (net 465))
  (via (at 199.9615 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 466) (tstamp 61978BBD))
  (segment (start 199.9615 101.992) (end 199.9615 103.1875) (width 0.15) (layer F.Cu) (net 466) (tstamp 61978BBE))
  (via (at 196.215 138.684) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 466))
  (segment (start 196.215 138.684) (end 194.1815 138.684) (width 0.15) (layer F.Cu) (net 466))
  (segment (start 203.55 95.85) (end 203.55 98.15) (width 0.15) (layer F.Cu) (net 466))
  (segment (start 204.55 94.85) (end 203.55 95.85) (width 0.15) (layer F.Cu) (net 466))
  (segment (start 204.75 94.85) (end 204.55 94.85) (width 0.15) (layer F.Cu) (net 466))
  (segment (start 204.95 94.65) (end 204.75 94.85) (width 0.15) (layer F.Cu) (net 466))
  (segment (start 204.95 93.75) (end 204.95 94.65) (width 0.15) (layer F.Cu) (net 466))
  (segment (start 214.5665 134.874) (end 210.7565 138.684) (width 0.15) (layer B.Cu) (net 466))
  (segment (start 210.7565 138.684) (end 196.215 138.684) (width 0.15) (layer B.Cu) (net 466))
  (segment (start 214.5665 130.7465) (end 214.5665 134.874) (width 0.15) (layer B.Cu) (net 466))
  (segment (start 213.868 130.048) (end 214.5665 130.7465) (width 0.15) (layer B.Cu) (net 466))
  (segment (start 213.868 123.698) (end 213.868 130.048) (width 0.15) (layer B.Cu) (net 466))
  (segment (start 211.455 121.285) (end 213.868 123.698) (width 0.15) (layer B.Cu) (net 466))
  (segment (start 211.455 107.569) (end 211.455 121.285) (width 0.15) (layer B.Cu) (net 466))
  (segment (start 199.9615 103.1875) (end 202.057 105.283) (width 0.15) (layer B.Cu) (net 466))
  (segment (start 209.169 105.283) (end 211.455 107.569) (width 0.15) (layer B.Cu) (net 466))
  (segment (start 202.057 105.283) (end 209.169 105.283) (width 0.15) (layer B.Cu) (net 466))
  (via (at 196.215 139.954) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 467) (tstamp 618683F2))
  (segment (start 194.1815 139.954) (end 196.215 139.954) (width 0.15) (layer F.Cu) (net 467) (tstamp 618683EF))
  (via (at 201.2315 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 467) (tstamp 61978BBB))
  (segment (start 201.2315 101.992) (end 201.2315 103.1875) (width 0.15) (layer F.Cu) (net 467) (tstamp 61978BBC))
  (segment (start 203.85 96) (end 203.85 98.25) (width 0.15) (layer F.Cu) (net 467))
  (segment (start 204.9 95.15) (end 204.7 95.15) (width 0.15) (layer F.Cu) (net 467))
  (segment (start 205.2 94.85) (end 204.9 95.15) (width 0.15) (layer F.Cu) (net 467))
  (segment (start 205.4 94.85) (end 205.2 94.85) (width 0.15) (layer F.Cu) (net 467))
  (segment (start 205.6 94.65) (end 205.4 94.85) (width 0.15) (layer F.Cu) (net 467))
  (segment (start 205.6 93.75) (end 205.6 94.65) (width 0.15) (layer F.Cu) (net 467))
  (segment (start 204.7 95.15) (end 203.85 96) (width 0.15) (layer F.Cu) (net 467))
  (segment (start 214.1855 123.571) (end 211.7725 121.158) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 214.1855 129.921) (end 214.1855 123.571) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 214.884 130.6195) (end 214.1855 129.921) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 214.884 135.001) (end 214.884 130.6195) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 209.296 104.9655) (end 203.0095 104.9655) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 210.8835 139.0015) (end 214.884 135.001) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 197.1675 139.0015) (end 210.8835 139.0015) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 203.0095 104.9655) (end 201.2315 103.1875) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 211.7725 107.442) (end 209.296 104.9655) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 211.7725 121.158) (end 211.7725 107.442) (width 0.15) (layer B.Cu) (net 467))
  (segment (start 196.215 139.954) (end 197.1675 139.0015) (width 0.15) (layer B.Cu) (net 467))
  (via (at 202.5015 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 468) (tstamp 61978BC3))
  (segment (start 202.5015 101.992) (end 202.5015 103.1875) (width 0.15) (layer F.Cu) (net 468) (tstamp 61978BC5))
  (via (at 197.0405 140.589) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 468))
  (segment (start 194.1815 140.589) (end 197.0405 140.589) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 204.85 95.45) (end 204.15 96.15) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 206.05 94.85) (end 205.85 94.85) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 206.25 94.65) (end 206.05 94.85) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 204.15 96.15) (end 204.15 98.15) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 206.25 93.75) (end 206.25 94.65) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 205.85 94.85) (end 205.55 95.15) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 205.55 95.15) (end 205.35 95.15) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 205.05 95.45) (end 204.85 95.45) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 205.35 95.15) (end 205.05 95.45) (width 0.15) (layer F.Cu) (net 468))
  (segment (start 203.962 104.648) (end 202.5015 103.1875) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 209.423 104.648) (end 203.962 104.648) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 212.09 107.315) (end 209.423 104.648) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 212.09 121.031) (end 212.09 107.315) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 214.503 123.444) (end 212.09 121.031) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 214.503 129.7305) (end 214.503 123.444) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 215.2015 130.429) (end 214.503 129.7305) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 215.2015 135.128) (end 215.2015 130.429) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 211.0105 139.319) (end 215.2015 135.128) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 198.3105 139.319) (end 211.0105 139.319) (width 0.15) (layer B.Cu) (net 468))
  (segment (start 197.0405 140.589) (end 198.3105 139.319) (width 0.15) (layer B.Cu) (net 468))
  (via (at 195.3895 141.224) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 469) (tstamp 618683F5))
  (segment (start 194.1815 141.224) (end 195.3895 141.224) (width 0.15) (layer F.Cu) (net 469) (tstamp 618683F8))
  (segment (start 203.7715 101.992) (end 203.7715 103.1875) (width 0.15) (layer F.Cu) (net 469) (tstamp 61978BC4))
  (via (at 203.7715 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 469) (tstamp 61978BC6))
  (segment (start 204.45 96.3) (end 204.45 98.2) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 205 95.75) (end 204.45 96.3) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 206.2 95.15) (end 206 95.15) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 206.5 94.85) (end 206.2 95.15) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 206.7 94.85) (end 206.5 94.85) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 206.9 94.65) (end 206.7 94.85) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 206.9 93.75) (end 206.9 94.65) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 206 95.15) (end 205.7 95.45) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 205.7 95.45) (end 205.5 95.45) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 205.2 95.75) (end 205 95.75) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 205.5 95.45) (end 205.2 95.75) (width 0.15) (layer F.Cu) (net 469))
  (segment (start 204.9145 104.3305) (end 203.7715 103.1875) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 212.4075 120.904) (end 212.4075 107.188) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 214.8205 123.317) (end 212.4075 120.904) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 215.519 135.255) (end 215.519 130.302) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 212.4075 107.188) (end 209.55 104.3305) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 215.519 130.302) (end 214.8205 129.6035) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 211.1375 139.6365) (end 215.519 135.255) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 209.55 104.3305) (end 204.9145 104.3305) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 195.3895 141.224) (end 197.104 141.224) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 198.6915 139.6365) (end 211.1375 139.6365) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 214.8205 129.6035) (end 214.8205 123.317) (width 0.15) (layer B.Cu) (net 469))
  (segment (start 197.104 141.224) (end 198.6915 139.6365) (width 0.15) (layer B.Cu) (net 469))
  (via (at 196.215 141.859) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 470) (tstamp 61868077))
  (segment (start 194.1815 141.859) (end 196.215 141.859) (width 0.15) (layer F.Cu) (net 470) (tstamp 61868080))
  (via (at 205.0415 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 470) (tstamp 61978BCF))
  (segment (start 205.0415 101.992) (end 205.0415 103.1875) (width 0.15) (layer F.Cu) (net 470) (tstamp 61978BD0))
  (segment (start 204.75 96.45) (end 204.75 98.2) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 205.15 96.05) (end 204.75 96.45) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 206.35 95.45) (end 206.15 95.45) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 206.65 95.15) (end 206.35 95.45) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 206.85 95.15) (end 206.65 95.15) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 207.15 94.85) (end 206.85 95.15) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 207.35 94.85) (end 207.15 94.85) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 207.55 94.65) (end 207.35 94.85) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 207.55 93.75) (end 207.55 94.65) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 206.15 95.45) (end 205.85 95.75) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 205.85 95.75) (end 205.65 95.75) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 205.35 96.05) (end 205.15 96.05) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 205.65 95.75) (end 205.35 96.05) (width 0.15) (layer F.Cu) (net 470))
  (segment (start 196.9135 141.859) (end 196.215 141.859) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 215.8365 135.382) (end 211.2645 139.954) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 215.8365 130.175) (end 215.8365 135.382) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 215.138 129.4765) (end 215.8365 130.175) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 212.725 120.777) (end 215.138 123.19) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 211.2645 139.954) (end 198.8185 139.954) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 212.725 107.061) (end 212.725 120.777) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 205.867 104.013) (end 209.677 104.013) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 215.138 123.19) (end 215.138 129.4765) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 209.677 104.013) (end 212.725 107.061) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 198.8185 139.954) (end 196.9135 141.859) (width 0.15) (layer B.Cu) (net 470))
  (segment (start 205.0415 103.1875) (end 205.867 104.013) (width 0.15) (layer B.Cu) (net 470))
  (via (at 196.215 143.129) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 471) (tstamp 618683FB))
  (segment (start 194.1815 143.129) (end 196.215 143.129) (width 0.15) (layer F.Cu) (net 471) (tstamp 618683EC))
  (via (at 210.1215 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 471) (tstamp 61978BDA))
  (segment (start 210.1215 101.992) (end 210.1215 103.1875) (width 0.15) (layer F.Cu) (net 471) (tstamp 61978BDB))
  (segment (start 213.0425 106.1085) (end 210.1215 103.1875) (width 0.15) (layer B.Cu) (net 471))
  (segment (start 213.0425 120.65) (end 213.0425 106.1085) (width 0.15) (layer B.Cu) (net 471))
  (segment (start 215.4555 123.063) (end 213.0425 120.65) (width 0.15) (layer B.Cu) (net 471))
  (segment (start 215.4555 129.3495) (end 215.4555 123.063) (width 0.15) (layer B.Cu) (net 471))
  (segment (start 216.154 130.048) (end 215.4555 129.3495) (width 0.15) (layer B.Cu) (net 471))
  (segment (start 216.154 135.509) (end 216.154 130.048) (width 0.15) (layer B.Cu) (net 471))
  (segment (start 211.3915 140.2715) (end 216.154 135.509) (width 0.15) (layer B.Cu) (net 471))
  (segment (start 199.0725 140.2715) (end 211.3915 140.2715) (width 0.15) (layer B.Cu) (net 471))
  (segment (start 196.215 143.129) (end 199.0725 140.2715) (width 0.15) (layer B.Cu) (net 471))
  (via (at 211.3915 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 472) (tstamp 61978BD3))
  (segment (start 211.3915 101.992) (end 211.3915 103.1875) (width 0.15) (layer F.Cu) (net 472) (tstamp 61978BD5))
  (via (at 197.0405 143.764) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 472))
  (segment (start 194.1815 143.764) (end 197.0405 143.764) (width 0.15) (layer F.Cu) (net 472))
  (segment (start 200.2155 140.589) (end 197.0405 143.764) (width 0.15) (layer B.Cu) (net 472))
  (segment (start 211.5185 140.589) (end 200.2155 140.589) (width 0.15) (layer B.Cu) (net 472))
  (segment (start 216.4715 135.636) (end 211.5185 140.589) (width 0.15) (layer B.Cu) (net 472))
  (segment (start 216.4715 129.921) (end 216.4715 135.636) (width 0.15) (layer B.Cu) (net 472))
  (segment (start 215.773 129.2225) (end 216.4715 129.921) (width 0.15) (layer B.Cu) (net 472))
  (segment (start 215.773 122.936) (end 215.773 129.2225) (width 0.15) (layer B.Cu) (net 472))
  (segment (start 213.36 120.523) (end 215.773 122.936) (width 0.15) (layer B.Cu) (net 472))
  (segment (start 213.36 105.156) (end 213.36 120.523) (width 0.15) (layer B.Cu) (net 472))
  (segment (start 211.3915 103.1875) (end 213.36 105.156) (width 0.15) (layer B.Cu) (net 472))
  (via (at 195.3895 144.399) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 473) (tstamp 6186806B))
  (segment (start 194.1815 144.399) (end 195.3895 144.399) (width 0.15) (layer F.Cu) (net 473) (tstamp 61868074))
  (segment (start 212.6615 101.992) (end 212.6615 103.1875) (width 0.15) (layer F.Cu) (net 473) (tstamp 61978BD4))
  (via (at 212.6615 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 473) (tstamp 61978BD6))
  (segment (start 213.6775 104.2035) (end 212.6615 103.1875) (width 0.15) (layer B.Cu) (net 473))
  (segment (start 213.6775 120.396) (end 213.6775 104.2035) (width 0.15) (layer B.Cu) (net 473))
  (segment (start 216.0905 129.0955) (end 216.0905 122.809) (width 0.15) (layer B.Cu) (net 473))
  (segment (start 216.789 129.794) (end 216.0905 129.0955) (width 0.15) (layer B.Cu) (net 473))
  (segment (start 200.5965 140.9065) (end 211.6455 140.9065) (width 0.15) (layer B.Cu) (net 473))
  (segment (start 216.0905 122.809) (end 213.6775 120.396) (width 0.15) (layer B.Cu) (net 473))
  (segment (start 197.104 144.399) (end 200.5965 140.9065) (width 0.15) (layer B.Cu) (net 473))
  (segment (start 216.789 135.763) (end 216.789 129.794) (width 0.15) (layer B.Cu) (net 473))
  (segment (start 211.6455 140.9065) (end 216.789 135.763) (width 0.15) (layer B.Cu) (net 473))
  (segment (start 195.3895 144.399) (end 197.104 144.399) (width 0.15) (layer B.Cu) (net 473))
  (via (at 196.215 145.034) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 474) (tstamp 6186806E))
  (segment (start 194.1815 145.034) (end 196.215 145.034) (width 0.15) (layer F.Cu) (net 474) (tstamp 61868071))
  (via (at 213.9315 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 474) (tstamp 61978BD8))
  (segment (start 213.9315 101.992) (end 213.9315 103.1875) (width 0.15) (layer F.Cu) (net 474) (tstamp 61978BD9))
  (segment (start 196.9135 145.034) (end 196.215 145.034) (width 0.15) (layer B.Cu) (net 474))
  (segment (start 211.7725 141.224) (end 200.7235 141.224) (width 0.15) (layer B.Cu) (net 474))
  (segment (start 200.7235 141.224) (end 196.9135 145.034) (width 0.15) (layer B.Cu) (net 474))
  (segment (start 217.1065 135.89) (end 211.7725 141.224) (width 0.15) (layer B.Cu) (net 474))
  (segment (start 217.1065 129.667) (end 217.1065 135.89) (width 0.15) (layer B.Cu) (net 474))
  (segment (start 216.408 128.9685) (end 217.1065 129.667) (width 0.15) (layer B.Cu) (net 474))
  (segment (start 213.995 103.251) (end 213.995 120.269) (width 0.15) (layer B.Cu) (net 474))
  (segment (start 216.408 122.682) (end 216.408 128.9685) (width 0.15) (layer B.Cu) (net 474))
  (segment (start 213.995 120.269) (end 216.408 122.682) (width 0.15) (layer B.Cu) (net 474))
  (segment (start 213.9315 103.1875) (end 213.995 103.251) (width 0.15) (layer B.Cu) (net 474))
  (via (at 196.215 146.304) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 475) (tstamp 6186840A))
  (segment (start 194.1815 146.304) (end 196.215 146.304) (width 0.15) (layer F.Cu) (net 475) (tstamp 61868416))
  (via (at 215.2015 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 475) (tstamp 61978BD7))
  (segment (start 215.2015 101.992) (end 215.2015 103.1875) (width 0.15) (layer F.Cu) (net 475) (tstamp 61978BDC))
  (segment (start 214.3125 104.0765) (end 215.2015 103.1875) (width 0.15) (layer B.Cu) (net 475))
  (segment (start 214.3125 120.142) (end 214.3125 104.0765) (width 0.15) (layer B.Cu) (net 475))
  (segment (start 216.7255 128.8415) (end 216.7255 122.555) (width 0.15) (layer B.Cu) (net 475))
  (segment (start 217.424 136.017) (end 217.424 129.54) (width 0.15) (layer B.Cu) (net 475))
  (segment (start 211.8995 141.5415) (end 217.424 136.017) (width 0.15) (layer B.Cu) (net 475))
  (segment (start 216.7255 122.555) (end 214.3125 120.142) (width 0.15) (layer B.Cu) (net 475))
  (segment (start 200.9775 141.5415) (end 211.8995 141.5415) (width 0.15) (layer B.Cu) (net 475))
  (segment (start 217.424 129.54) (end 216.7255 128.8415) (width 0.15) (layer B.Cu) (net 475))
  (segment (start 196.215 146.304) (end 200.9775 141.5415) (width 0.15) (layer B.Cu) (net 475))
  (via (at 195.3895 146.939) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 476) (tstamp 618683FE))
  (segment (start 194.1815 146.939) (end 195.3895 146.939) (width 0.15) (layer F.Cu) (net 476) (tstamp 61868401))
  (segment (start 216.4715 101.992) (end 216.4715 103.1875) (width 0.15) (layer F.Cu) (net 476) (tstamp 61978BDD))
  (via (at 216.4715 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 476) (tstamp 61978BDE))
  (segment (start 201.3585 141.859) (end 196.2785 146.939) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 212.0265 141.859) (end 201.3585 141.859) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 217.7415 129.413) (end 217.7415 136.144) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 217.7415 136.144) (end 212.0265 141.859) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 217.043 128.7145) (end 217.7415 129.413) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 214.63 119.507) (end 217.043 121.92) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 216.4715 103.1875) (end 214.63 105.029) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 214.63 105.029) (end 214.63 119.507) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 196.2785 146.939) (end 195.3895 146.939) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 217.043 121.92) (end 217.043 128.7145) (width 0.15) (layer B.Cu) (net 476))
  (segment (start 217.7415 101.992) (end 217.7415 103.1875) (width 0.15) (layer F.Cu) (net 477) (tstamp 61978BEB))
  (via (at 217.7415 103.1875) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 477) (tstamp 61978BEC))
  (via (at 197.0405 147.574) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 477))
  (segment (start 197.0405 147.574) (end 194.1815 147.574) (width 0.15) (layer F.Cu) (net 477))
  (segment (start 214.9475 105.9815) (end 217.7415 103.1875) (width 0.15) (layer B.Cu) (net 477))
  (segment (start 214.9475 119.38) (end 214.9475 105.9815) (width 0.15) (layer B.Cu) (net 477))
  (segment (start 217.3605 121.793) (end 214.9475 119.38) (width 0.15) (layer B.Cu) (net 477))
  (segment (start 217.3605 128.5875) (end 217.3605 121.793) (width 0.15) (layer B.Cu) (net 477))
  (segment (start 218.059 129.286) (end 217.3605 128.5875) (width 0.15) (layer B.Cu) (net 477))
  (segment (start 218.059 136.271) (end 218.059 129.286) (width 0.15) (layer B.Cu) (net 477))
  (segment (start 212.1535 142.1765) (end 218.059 136.271) (width 0.15) (layer B.Cu) (net 477))
  (segment (start 202.438 142.1765) (end 212.1535 142.1765) (width 0.15) (layer B.Cu) (net 477))
  (segment (start 197.0405 147.574) (end 202.438 142.1765) (width 0.15) (layer B.Cu) (net 477))
  (via (at 196.215 148.209) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 478) (tstamp 61868404))
  (segment (start 194.1815 148.209) (end 196.215 148.209) (width 0.15) (layer F.Cu) (net 478) (tstamp 61868407))
  (via (at 218.186 104.902) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 478))
  (segment (start 219.3815 104.902) (end 218.186 104.902) (width 0.15) (layer F.Cu) (net 478))
  (segment (start 220.6625 104.902) (end 221.107 104.4575) (width 0.15) (layer F.Cu) (net 478))
  (segment (start 221.107 104.4575) (end 221.107 103.251) (width 0.15) (layer F.Cu) (net 478))
  (segment (start 219.3815 104.902) (end 220.6625 104.902) (width 0.15) (layer F.Cu) (net 478))
  (segment (start 197.104 148.209) (end 196.215 148.209) (width 0.15) (layer B.Cu) (net 478))
  (segment (start 212.2805 142.494) (end 202.819 142.494) (width 0.15) (layer B.Cu) (net 478))
  (segment (start 218.3765 129.159) (end 218.3765 136.398) (width 0.15) (layer B.Cu) (net 478))
  (segment (start 217.678 121.666) (end 217.678 128.4605) (width 0.15) (layer B.Cu) (net 478))
  (segment (start 202.819 142.494) (end 197.104 148.209) (width 0.15) (layer B.Cu) (net 478))
  (segment (start 217.678 128.4605) (end 218.3765 129.159) (width 0.15) (layer B.Cu) (net 478))
  (segment (start 215.265 119.253) (end 217.678 121.666) (width 0.15) (layer B.Cu) (net 478))
  (segment (start 215.265 107.823) (end 215.265 119.253) (width 0.15) (layer B.Cu) (net 478))
  (segment (start 218.3765 136.398) (end 212.2805 142.494) (width 0.15) (layer B.Cu) (net 478))
  (segment (start 218.186 104.902) (end 215.265 107.823) (width 0.15) (layer B.Cu) (net 478))
  (via (at 218.186 107.442) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 479) (tstamp 61978F5C))
  (segment (start 219.3815 107.442) (end 218.186 107.442) (width 0.15) (layer F.Cu) (net 479) (tstamp 61978F5D))
  (via (at 196.215 149.479) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 479) (tstamp 619882AD))
  (segment (start 194.1815 149.479) (end 196.215 149.479) (width 0.15) (layer F.Cu) (net 479))
  (segment (start 221.4245 104.5845) (end 221.4245 102.9335) (width 0.15) (layer F.Cu) (net 479))
  (segment (start 221.107 104.902) (end 221.4245 104.5845) (width 0.15) (layer F.Cu) (net 479))
  (segment (start 221.107 106.9975) (end 221.107 104.902) (width 0.15) (layer F.Cu) (net 479))
  (segment (start 220.6625 107.442) (end 221.107 106.9975) (width 0.15) (layer F.Cu) (net 479))
  (segment (start 219.3815 107.442) (end 220.6625 107.442) (width 0.15) (layer F.Cu) (net 479))
  (segment (start 196.2785 149.479) (end 196.215 149.479) (width 0.15) (layer B.Cu) (net 479))
  (segment (start 202.946 142.8115) (end 196.2785 149.479) (width 0.15) (layer B.Cu) (net 479))
  (segment (start 212.4075 142.8115) (end 202.946 142.8115) (width 0.15) (layer B.Cu) (net 479))
  (segment (start 218.694 136.525) (end 212.4075 142.8115) (width 0.15) (layer B.Cu) (net 479))
  (segment (start 218.694 122.2375) (end 218.694 136.525) (width 0.15) (layer B.Cu) (net 479))
  (segment (start 215.5825 119.126) (end 218.694 122.2375) (width 0.15) (layer B.Cu) (net 479))
  (segment (start 215.5825 110.0455) (end 215.5825 119.126) (width 0.15) (layer B.Cu) (net 479))
  (segment (start 218.186 107.442) (end 215.5825 110.0455) (width 0.15) (layer B.Cu) (net 479))
  (via (at 218.186 108.712) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 480) (tstamp 61978F60))
  (segment (start 219.3815 108.712) (end 218.186 108.712) (width 0.15) (layer F.Cu) (net 480) (tstamp 61978F61))
  (segment (start 194.1815 150.114) (end 197.0405 150.114) (width 0.15) (layer F.Cu) (net 480))
  (via (at 197.0405 150.114) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 480))
  (segment (start 221.742 104.7115) (end 221.742 102.9335) (width 0.15) (layer F.Cu) (net 480))
  (segment (start 221.4245 105.029) (end 221.742 104.7115) (width 0.15) (layer F.Cu) (net 480))
  (segment (start 221.4245 107.1245) (end 221.4245 105.029) (width 0.15) (layer F.Cu) (net 480))
  (segment (start 221.107 107.442) (end 221.4245 107.1245) (width 0.15) (layer F.Cu) (net 480))
  (segment (start 221.107 108.2675) (end 221.107 107.442) (width 0.15) (layer F.Cu) (net 480))
  (segment (start 220.6625 108.712) (end 221.107 108.2675) (width 0.15) (layer F.Cu) (net 480))
  (segment (start 219.3815 108.712) (end 220.6625 108.712) (width 0.15) (layer F.Cu) (net 480))
  (segment (start 215.9 118.999) (end 215.9 110.998) (width 0.15) (layer B.Cu) (net 480))
  (segment (start 212.5345 143.129) (end 219.0115 136.652) (width 0.15) (layer B.Cu) (net 480))
  (segment (start 219.0115 122.1105) (end 215.9 118.999) (width 0.15) (layer B.Cu) (net 480))
  (segment (start 215.9 110.998) (end 218.186 108.712) (width 0.15) (layer B.Cu) (net 480))
  (segment (start 219.0115 136.652) (end 219.0115 122.1105) (width 0.15) (layer B.Cu) (net 480))
  (segment (start 204.0255 143.129) (end 212.5345 143.129) (width 0.15) (layer B.Cu) (net 480))
  (segment (start 197.0405 150.114) (end 204.0255 143.129) (width 0.15) (layer B.Cu) (net 480))
  (via (at 218.186 109.982) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 481) (tstamp 61978F66))
  (segment (start 219.3815 109.982) (end 218.186 109.982) (width 0.15) (layer F.Cu) (net 481) (tstamp 61978F67))
  (via (at 195.3895 150.749) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 481))
  (segment (start 194.1815 150.749) (end 195.3895 150.749) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 222.0595 104.8385) (end 222.0595 102.743) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 221.742 105.156) (end 222.0595 104.8385) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 221.742 107.2515) (end 221.742 105.156) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 220.6625 109.982) (end 221.107 109.5375) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 221.107 109.5375) (end 221.107 108.712) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 221.4245 108.3945) (end 221.4245 107.569) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 221.107 108.712) (end 221.4245 108.3945) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 221.4245 107.569) (end 221.742 107.2515) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 219.3815 109.982) (end 220.6625 109.982) (width 0.15) (layer F.Cu) (net 481))
  (segment (start 216.2175 111.9505) (end 218.186 109.982) (width 0.15) (layer B.Cu) (net 481))
  (segment (start 219.329 121.9835) (end 216.2175 118.872) (width 0.15) (layer B.Cu) (net 481))
  (segment (start 216.2175 118.872) (end 216.2175 111.9505) (width 0.15) (layer B.Cu) (net 481))
  (segment (start 219.329 136.779) (end 219.329 121.9835) (width 0.15) (layer B.Cu) (net 481))
  (segment (start 195.3895 150.749) (end 197.104 150.749) (width 0.15) (layer B.Cu) (net 481))
  (segment (start 212.6615 143.4465) (end 219.329 136.779) (width 0.15) (layer B.Cu) (net 481))
  (segment (start 204.4065 143.4465) (end 212.6615 143.4465) (width 0.15) (layer B.Cu) (net 481))
  (segment (start 197.104 150.749) (end 204.4065 143.4465) (width 0.15) (layer B.Cu) (net 481))
  (segment (start 219.3815 111.252) (end 218.186 111.252) (width 0.15) (layer F.Cu) (net 482) (tstamp 61978F64))
  (via (at 218.186 111.252) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 482) (tstamp 61978F65))
  (via (at 196.5325 151.384) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 482))
  (segment (start 196.5325 151.384) (end 194.1815 151.384) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 221.107 110.8075) (end 220.6625 111.252) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 221.107 109.982) (end 221.107 110.8075) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 221.488 108.7755) (end 221.488 109.601) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 221.742 107.696) (end 221.742 108.5215) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 221.488 109.601) (end 221.107 109.982) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 221.742 108.5215) (end 221.488 108.7755) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 222.0595 105.283) (end 222.0595 107.3785) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 220.6625 111.252) (end 219.3815 111.252) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 222.377 104.9655) (end 222.0595 105.283) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 222.0595 107.3785) (end 221.742 107.696) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 222.377 102.616) (end 222.377 104.9655) (width 0.15) (layer F.Cu) (net 482))
  (segment (start 196.9135 151.384) (end 196.5325 151.384) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 204.5335 143.764) (end 196.9135 151.384) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 212.7885 143.764) (end 204.5335 143.764) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 219.6465 136.906) (end 212.7885 143.764) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 219.6465 121.8565) (end 219.6465 136.906) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 218.694 120.904) (end 219.6465 121.8565) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 218.694 119.9515) (end 218.694 120.904) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 218.186 111.252) (end 216.535 112.903) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 216.535 117.7925) (end 218.694 119.9515) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 216.535 112.903) (end 216.535 117.7925) (width 0.15) (layer B.Cu) (net 482))
  (segment (start 219.3815 112.522) (end 218.186 112.522) (width 0.15) (layer F.Cu) (net 483) (tstamp 61978F6C))
  (via (at 218.186 112.522) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 483) (tstamp 61978F6F))
  (via (at 196.5325 152.654) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 483))
  (segment (start 194.1815 152.654) (end 196.5325 152.654) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 221.107 111.252) (end 221.107 112.0775) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 222.0595 108.6485) (end 221.8055 108.9025) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 221.4245 110.109) (end 221.4245 110.9345) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 221.107 112.0775) (end 220.6625 112.522) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 221.8055 109.728) (end 221.4245 110.109) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 221.8055 108.9025) (end 221.8055 109.728) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 221.4245 110.9345) (end 221.107 111.252) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 222.0595 107.823) (end 222.0595 108.6485) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 222.377 107.5055) (end 222.0595 107.823) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 222.6945 102.2985) (end 222.6945 105.0925) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 220.6625 112.522) (end 219.3815 112.522) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 222.6945 105.0925) (end 222.377 105.41) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 222.377 105.41) (end 222.377 107.5055) (width 0.15) (layer F.Cu) (net 483))
  (segment (start 216.8525 117.602) (end 216.8525 113.8555) (width 0.15) (layer B.Cu) (net 483))
  (segment (start 219.0115 119.761) (end 216.8525 117.602) (width 0.15) (layer B.Cu) (net 483))
  (segment (start 219.964 121.7295) (end 219.0115 120.777) (width 0.15) (layer B.Cu) (net 483))
  (segment (start 219.964 137.033) (end 219.964 121.7295) (width 0.15) (layer B.Cu) (net 483))
  (segment (start 205.105 144.0815) (end 212.9155 144.0815) (width 0.15) (layer B.Cu) (net 483))
  (segment (start 216.8525 113.8555) (end 218.186 112.522) (width 0.15) (layer B.Cu) (net 483))
  (segment (start 219.0115 120.777) (end 219.0115 119.761) (width 0.15) (layer B.Cu) (net 483))
  (segment (start 212.9155 144.0815) (end 219.964 137.033) (width 0.15) (layer B.Cu) (net 483))
  (segment (start 196.5325 152.654) (end 205.105 144.0815) (width 0.15) (layer B.Cu) (net 483))
  (segment (start 219.3815 113.792) (end 218.186 113.792) (width 0.15) (layer F.Cu) (net 484) (tstamp 61978F6D))
  (via (at 218.186 113.792) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 484) (tstamp 61978F6E))
  (via (at 195.707 153.289) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 484))
  (segment (start 194.1815 153.289) (end 195.707 153.289) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 223.012 105.2195) (end 223.012 102.2985) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 222.6945 105.537) (end 223.012 105.2195) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 222.6945 107.6325) (end 222.6945 105.537) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 222.377 107.95) (end 222.6945 107.6325) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 222.377 108.7755) (end 222.377 107.95) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 222.123 109.0295) (end 222.377 108.7755) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 222.123 109.855) (end 222.123 109.0295) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 221.742 110.236) (end 222.123 109.855) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 221.742 111.0615) (end 221.742 110.236) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 221.4245 111.379) (end 221.742 111.0615) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 221.4245 112.2045) (end 221.4245 111.379) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 221.107 112.522) (end 221.4245 112.2045) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 221.107 113.3475) (end 221.107 112.522) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 220.6625 113.792) (end 221.107 113.3475) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 219.3815 113.792) (end 220.6625 113.792) (width 0.15) (layer F.Cu) (net 484))
  (segment (start 196.596 153.289) (end 195.707 153.289) (width 0.15) (layer B.Cu) (net 484))
  (segment (start 205.486 144.399) (end 196.596 153.289) (width 0.15) (layer B.Cu) (net 484))
  (segment (start 213.0425 144.399) (end 205.486 144.399) (width 0.15) (layer B.Cu) (net 484))
  (segment (start 220.2815 137.16) (end 213.0425 144.399) (width 0.15) (layer B.Cu) (net 484))
  (segment (start 220.2815 121.6025) (end 220.2815 137.16) (width 0.15) (layer B.Cu) (net 484))
  (segment (start 219.329 120.65) (end 220.2815 121.6025) (width 0.15) (layer B.Cu) (net 484))
  (segment (start 218.186 113.792) (end 217.17 114.808) (width 0.15) (layer B.Cu) (net 484))
  (segment (start 219.329 119.634) (end 219.329 120.65) (width 0.15) (layer B.Cu) (net 484))
  (segment (start 217.17 117.475) (end 219.329 119.634) (width 0.15) (layer B.Cu) (net 484))
  (segment (start 217.17 114.808) (end 217.17 117.475) (width 0.15) (layer B.Cu) (net 484))
  (via (at 218.186 115.062) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 485) (tstamp 61978F74))
  (segment (start 219.3815 115.062) (end 218.186 115.062) (width 0.15) (layer F.Cu) (net 485) (tstamp 61978F75))
  (via (at 196.5325 153.924) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 485))
  (segment (start 194.1815 153.924) (end 196.5325 153.924) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 223.3295 105.3465) (end 223.3295 101.981) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 223.012 105.664) (end 223.3295 105.3465) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 223.012 107.7595) (end 223.012 105.664) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 222.6945 108.077) (end 223.012 107.7595) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 222.6945 108.9025) (end 222.6945 108.077) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 222.4405 109.1565) (end 222.6945 108.9025) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 222.4405 109.982) (end 222.4405 109.1565) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 222.0595 110.363) (end 222.4405 109.982) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 221.742 111.506) (end 222.0595 111.1885) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 221.742 112.3315) (end 221.742 111.506) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 222.0595 111.1885) (end 222.0595 110.363) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 221.4245 112.649) (end 221.742 112.3315) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 221.107 113.792) (end 221.4245 113.4745) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 221.4245 113.4745) (end 221.4245 112.649) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 221.107 114.6175) (end 221.107 113.792) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 220.6625 115.062) (end 221.107 114.6175) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 219.3815 115.062) (end 220.6625 115.062) (width 0.15) (layer F.Cu) (net 485))
  (segment (start 217.678 115.57) (end 218.186 115.062) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 217.678 117.5385) (end 217.678 115.57) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 219.6465 119.507) (end 217.678 117.5385) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 219.6465 120.523) (end 219.6465 119.507) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 221.2975 122.174) (end 219.6465 120.523) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 213.1695 144.7165) (end 220.599 137.287) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 220.599 127.4445) (end 221.2975 126.746) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 220.599 137.287) (end 220.599 127.4445) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 221.2975 126.746) (end 221.2975 122.174) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 205.74 144.7165) (end 213.1695 144.7165) (width 0.15) (layer B.Cu) (net 485))
  (segment (start 196.5325 153.924) (end 205.74 144.7165) (width 0.15) (layer B.Cu) (net 485))
  (via (at 218.186 116.332) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 486) (tstamp 61978F76))
  (segment (start 219.3815 116.332) (end 218.186 116.332) (width 0.15) (layer F.Cu) (net 486) (tstamp 61978F77))
  (via (at 195.707 154.559) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 486))
  (segment (start 194.1815 154.559) (end 195.707 154.559) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 223.647 105.4735) (end 223.647 101.7905) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 223.3295 105.791) (end 223.647 105.4735) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 223.3295 107.8865) (end 223.3295 105.791) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 223.012 108.204) (end 223.3295 107.8865) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 223.012 109.0295) (end 223.012 108.204) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 222.758 109.2835) (end 223.012 109.0295) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 222.758 110.109) (end 222.758 109.2835) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 222.377 110.49) (end 222.758 110.109) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 222.377 111.3155) (end 222.377 110.49) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 222.0595 111.633) (end 222.377 111.3155) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 222.0595 112.4585) (end 222.0595 111.633) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 221.742 112.776) (end 222.0595 112.4585) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 221.742 113.6015) (end 221.742 112.776) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 221.4245 113.919) (end 221.742 113.6015) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 221.4245 114.7445) (end 221.4245 113.919) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 221.107 115.062) (end 221.4245 114.7445) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 221.107 115.8875) (end 221.107 115.062) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 220.6625 116.332) (end 221.107 115.8875) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 219.3815 116.332) (end 220.6625 116.332) (width 0.15) (layer F.Cu) (net 486))
  (segment (start 196.596 154.559) (end 195.707 154.559) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 206.121 145.034) (end 196.596 154.559) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 213.2965 145.034) (end 206.121 145.034) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 220.9165 137.414) (end 213.2965 145.034) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 220.9165 127.762) (end 220.9165 137.414) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 221.615 127.0635) (end 220.9165 127.762) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 221.615 122.047) (end 221.615 127.0635) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 219.964 120.396) (end 221.615 122.047) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 219.964 119.38) (end 219.964 120.396) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 218.186 117.602) (end 219.964 119.38) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 218.186 116.332) (end 218.186 117.602) (width 0.15) (layer B.Cu) (net 486))
  (segment (start 195.7815 116.332) (end 196.977 116.332) (width 0.15) (layer F.Cu) (net 487) (tstamp 619792FF))
  (via (at 196.977 116.332) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 487) (tstamp 61979300))
  (via (at 202.5015 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 487))
  (segment (start 202.5015 132.269) (end 202.5015 133.477) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 198.882 114.427) (end 196.977 116.332) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 198.882 106.8705) (end 198.882 114.427) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 197.5485 105.537) (end 198.882 106.8705) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 194.7545 105.537) (end 197.5485 105.537) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 194.3735 105.156) (end 194.7545 105.537) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 194.3735 97.5765) (end 194.3735 105.156) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 195.3 96.65) (end 194.3735 97.5765) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 195.5 96.65) (end 195.3 96.65) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 195.8 96.35) (end 195.5 96.65) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 196 96.35) (end 195.8 96.35) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 196.3 96.05) (end 196 96.35) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 196.5 96.05) (end 196.3 96.05) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 196.8 95.75) (end 196.5 96.05) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 197 95.75) (end 196.8 95.75) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 197.3 95.45) (end 197 95.75) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 197.5 95.45) (end 197.3 95.45) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 197.8 95.15) (end 197.5 95.45) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 198 95.15) (end 197.8 95.15) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 198.3 94.85) (end 198 95.15) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 198.5 94.85) (end 198.3 94.85) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 198.7 94.65) (end 198.5 94.85) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 198.7 93.75) (end 198.7 94.65) (width 0.15) (layer F.Cu) (net 487))
  (segment (start 198.3105 125.857) (end 198.3105 117.6655) (width 0.15) (layer B.Cu) (net 487))
  (segment (start 207.137 128.7145) (end 201.168 128.7145) (width 0.15) (layer B.Cu) (net 487))
  (segment (start 208.3435 129.921) (end 207.137 128.7145) (width 0.15) (layer B.Cu) (net 487))
  (segment (start 207.645 135.1915) (end 208.3435 134.493) (width 0.15) (layer B.Cu) (net 487))
  (segment (start 198.3105 117.6655) (end 196.977 116.332) (width 0.15) (layer B.Cu) (net 487))
  (segment (start 208.3435 134.493) (end 208.3435 129.921) (width 0.15) (layer B.Cu) (net 487))
  (segment (start 201.168 128.7145) (end 198.3105 125.857) (width 0.15) (layer B.Cu) (net 487))
  (segment (start 204.216 135.1915) (end 207.645 135.1915) (width 0.15) (layer B.Cu) (net 487))
  (segment (start 202.5015 133.477) (end 204.216 135.1915) (width 0.15) (layer B.Cu) (net 487))
  (segment (start 195.7815 115.062) (end 196.977 115.062) (width 0.15) (layer F.Cu) (net 488) (tstamp 619792FD))
  (via (at 196.977 115.062) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 488) (tstamp 619792FE))
  (via (at 201.8665 134.3025) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 488) (tstamp 61A260F4))
  (segment (start 201.8665 132.269) (end 201.8665 134.3025) (width 0.15) (layer F.Cu) (net 488) (tstamp 61A260F5))
  (segment (start 198.05 94.65) (end 198.05 93.75) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 197.65 94.85) (end 197.85 94.85) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 197.15 95.15) (end 197.35 95.15) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 197.35 95.15) (end 197.65 94.85) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 196.85 95.45) (end 197.15 95.15) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 196.35 95.75) (end 196.65 95.45) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 195.35 96.35) (end 195.65 96.05) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 194.5005 106.807) (end 194.056 106.3625) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 197.612 106.807) (end 194.5005 106.807) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 195.85 96.05) (end 196.15 95.75) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 196.15 95.75) (end 196.35 95.75) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 195.65 96.05) (end 195.85 96.05) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 195.15 96.35) (end 195.35 96.35) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 196.65 95.45) (end 196.85 95.45) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 194.056 97.444) (end 195.15 96.35) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 198.4375 113.6015) (end 198.4375 107.6325) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 194.056 106.3625) (end 194.056 97.444) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 196.977 115.062) (end 198.4375 113.6015) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 197.85 94.85) (end 198.05 94.65) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 198.4375 107.6325) (end 197.612 106.807) (width 0.15) (layer F.Cu) (net 488))
  (segment (start 198.628 116.713) (end 196.977 115.062) (width 0.15) (layer B.Cu) (net 488))
  (segment (start 198.628 124.7775) (end 198.628 116.713) (width 0.15) (layer B.Cu) (net 488))
  (segment (start 202.2475 128.397) (end 198.628 124.7775) (width 0.15) (layer B.Cu) (net 488))
  (segment (start 207.264 128.397) (end 202.2475 128.397) (width 0.15) (layer B.Cu) (net 488))
  (segment (start 208.661 129.794) (end 207.264 128.397) (width 0.15) (layer B.Cu) (net 488))
  (segment (start 208.661 134.62) (end 208.661 129.794) (width 0.15) (layer B.Cu) (net 488))
  (segment (start 207.772 135.509) (end 208.661 134.62) (width 0.15) (layer B.Cu) (net 488))
  (segment (start 203.073 135.509) (end 207.772 135.509) (width 0.15) (layer B.Cu) (net 488))
  (segment (start 201.8665 134.3025) (end 203.073 135.509) (width 0.15) (layer B.Cu) (net 488))
  (via (at 196.977 113.792) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 489) (tstamp 619792F7))
  (segment (start 195.7815 113.792) (end 196.977 113.792) (width 0.15) (layer F.Cu) (net 489) (tstamp 619792F8))
  (via (at 200.5965 134.3025) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 489) (tstamp 61A260F0))
  (segment (start 200.5965 132.269) (end 200.5965 134.3025) (width 0.15) (layer F.Cu) (net 489) (tstamp 61A260F1))
  (segment (start 196.55 94.85) (end 196.75 94.65) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 196.75 94.65) (end 196.75 93.75) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 196.35 94.85) (end 196.55 94.85) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 196.05 95.15) (end 196.35 94.85) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 195.85 95.15) (end 196.05 95.15) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 195.05 95.75) (end 195.35 95.45) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 194.85 95.75) (end 195.05 95.75) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 193.421 97.179) (end 194.85 95.75) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 194.818 108.0135) (end 193.421 106.6165) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 193.421 106.6165) (end 193.421 97.179) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 195.35 95.45) (end 195.55 95.45) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 197.231 108.0135) (end 194.818 108.0135) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 198.12 112.649) (end 198.12 108.9025) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 195.55 95.45) (end 195.85 95.15) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 198.12 108.9025) (end 197.231 108.0135) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 196.977 113.792) (end 198.12 112.649) (width 0.15) (layer F.Cu) (net 489))
  (segment (start 207.899 135.8265) (end 202.1205 135.8265) (width 0.15) (layer B.Cu) (net 489))
  (segment (start 208.9785 129.667) (end 208.9785 134.747) (width 0.15) (layer B.Cu) (net 489))
  (segment (start 198.9455 115.7605) (end 198.9455 124.6505) (width 0.15) (layer B.Cu) (net 489))
  (segment (start 202.3745 128.0795) (end 207.391 128.0795) (width 0.15) (layer B.Cu) (net 489))
  (segment (start 202.1205 135.8265) (end 200.5965 134.3025) (width 0.15) (layer B.Cu) (net 489))
  (segment (start 207.391 128.0795) (end 208.9785 129.667) (width 0.15) (layer B.Cu) (net 489))
  (segment (start 198.9455 124.6505) (end 202.3745 128.0795) (width 0.15) (layer B.Cu) (net 489))
  (segment (start 208.9785 134.747) (end 207.899 135.8265) (width 0.15) (layer B.Cu) (net 489))
  (segment (start 196.977 113.792) (end 198.9455 115.7605) (width 0.15) (layer B.Cu) (net 489))
  (segment (start 195.7815 112.522) (end 196.977 112.522) (width 0.15) (layer F.Cu) (net 490) (tstamp 619792F5))
  (via (at 196.977 112.522) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 490) (tstamp 619792F6))
  (via (at 199.9615 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 490))
  (segment (start 199.9615 132.269) (end 199.9615 133.477) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 195.45 94.65) (end 195.45 93.75) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 195.25 94.85) (end 195.45 94.65) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 195.05 94.85) (end 195.25 94.85) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 194.75 95.15) (end 195.05 94.85) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 194.55 95.15) (end 194.75 95.15) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 192.786 96.914) (end 194.55 95.15) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 192.786 107.3785) (end 192.786 96.914) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 194.7545 109.347) (end 192.786 107.3785) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 197.8025 111.6965) (end 197.8025 109.728) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 197.8025 109.728) (end 197.4215 109.347) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 197.4215 109.347) (end 194.7545 109.347) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 196.977 112.522) (end 197.8025 111.6965) (width 0.15) (layer F.Cu) (net 490))
  (segment (start 202.5015 127.762) (end 199.263 124.5235) (width 0.15) (layer B.Cu) (net 490))
  (segment (start 207.518 127.762) (end 202.5015 127.762) (width 0.15) (layer B.Cu) (net 490))
  (segment (start 199.263 124.5235) (end 199.263 114.808) (width 0.15) (layer B.Cu) (net 490))
  (segment (start 209.296 129.54) (end 207.518 127.762) (width 0.15) (layer B.Cu) (net 490))
  (segment (start 199.9615 134.366) (end 201.7395 136.144) (width 0.15) (layer B.Cu) (net 490))
  (segment (start 209.296 134.874) (end 209.296 129.54) (width 0.15) (layer B.Cu) (net 490))
  (segment (start 208.026 136.144) (end 209.296 134.874) (width 0.15) (layer B.Cu) (net 490))
  (segment (start 199.263 114.808) (end 196.977 112.522) (width 0.15) (layer B.Cu) (net 490))
  (segment (start 201.7395 136.144) (end 208.026 136.144) (width 0.15) (layer B.Cu) (net 490))
  (segment (start 199.9615 133.477) (end 199.9615 134.366) (width 0.15) (layer B.Cu) (net 490))
  (via (at 196.977 111.252) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 491) (tstamp 619792ED))
  (segment (start 195.7815 111.252) (end 196.977 111.252) (width 0.15) (layer F.Cu) (net 491) (tstamp 619792EE))
  (segment (start 199.3265 132.269) (end 199.3265 134.3025) (width 0.15) (layer F.Cu) (net 491) (tstamp 61A260EC))
  (via (at 199.3265 134.3025) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 491) (tstamp 61A260ED))
  (segment (start 194.6275 111.252) (end 195.7815 111.252) (width 0.15) (layer F.Cu) (net 491))
  (segment (start 192.151 108.7755) (end 194.6275 111.252) (width 0.15) (layer F.Cu) (net 491))
  (segment (start 192.151 96.649) (end 192.151 108.7755) (width 0.15) (layer F.Cu) (net 491))
  (segment (start 194.15 94.65) (end 192.151 96.649) (width 0.15) (layer F.Cu) (net 491))
  (segment (start 194.15 93.75) (end 194.15 94.65) (width 0.15) (layer F.Cu) (net 491))
  (segment (start 210.947 132.6515) (end 210.947 134.62) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 209.1055 136.4615) (end 201.4855 136.4615) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 211.6455 128.524) (end 211.6455 131.953) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 201.4855 136.4615) (end 199.3265 134.3025) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 209.042 125.9205) (end 211.6455 128.524) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 202.438 125.9205) (end 209.042 125.9205) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 211.6455 131.953) (end 210.947 132.6515) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 199.5805 123.063) (end 202.438 125.9205) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 210.947 134.62) (end 209.1055 136.4615) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 199.5805 113.8555) (end 199.5805 123.063) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 196.977 111.252) (end 199.5805 113.8555) (width 0.15) (layer B.Cu) (net 491))
  (segment (start 195.7815 109.982) (end 196.977 109.982) (width 0.15) (layer F.Cu) (net 492) (tstamp 619792EF))
  (via (at 196.977 109.982) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 492) (tstamp 619792F0))
  (via (at 198.6915 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 492))
  (segment (start 198.6915 132.269) (end 198.6915 133.477) (width 0.15) (layer F.Cu) (net 492))
  (segment (start 194.564 109.982) (end 195.7815 109.982) (width 0.15) (layer F.Cu) (net 492))
  (segment (start 192.4685 96.7815) (end 192.4685 107.8865) (width 0.15) (layer F.Cu) (net 492))
  (segment (start 194.6 94.85) (end 194.4 94.85) (width 0.15) (layer F.Cu) (net 492))
  (segment (start 194.8 94.65) (end 194.6 94.85) (width 0.15) (layer F.Cu) (net 492))
  (segment (start 192.4685 107.8865) (end 194.564 109.982) (width 0.15) (layer F.Cu) (net 492))
  (segment (start 194.4 94.85) (end 192.4685 96.7815) (width 0.15) (layer F.Cu) (net 492))
  (segment (start 194.8 93.75) (end 194.8 94.65) (width 0.15) (layer F.Cu) (net 492))
  (segment (start 199.030259 112.035259) (end 196.977 109.982) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 199.898 112.903) (end 199.030259 112.035259) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 209.2325 136.779) (end 211.2645 134.747) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 198.6915 134.366) (end 201.1045 136.779) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 211.963 132.08) (end 211.963 128.397) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 211.2645 132.7785) (end 211.963 132.08) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 201.1045 136.779) (end 209.2325 136.779) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 202.565 125.603) (end 199.898 122.936) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 209.169 125.603) (end 202.565 125.603) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 211.963 128.397) (end 209.169 125.603) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 211.2645 134.747) (end 211.2645 132.7785) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 199.898 122.936) (end 199.898 112.903) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 198.6915 133.477) (end 198.6915 134.366) (width 0.15) (layer B.Cu) (net 492))
  (segment (start 195.7815 108.712) (end 196.977 108.712) (width 0.15) (layer F.Cu) (net 493) (tstamp 619792E9))
  (via (at 196.977 108.712) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 493) (tstamp 619792EA))
  (via (at 198.0565 134.3025) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 493))
  (segment (start 198.0565 132.269) (end 198.0565 134.3025) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 193.1035 107.1245) (end 194.691 108.712) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 193.1035 97.0465) (end 193.1035 107.1245) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 194.7 95.45) (end 193.1035 97.0465) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 195.2 95.15) (end 194.9 95.45) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 194.9 95.45) (end 194.7 95.45) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 195.4 95.15) (end 195.2 95.15) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 196.1 94.65) (end 195.9 94.85) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 195.7 94.85) (end 195.4 95.15) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 195.9 94.85) (end 195.7 94.85) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 194.691 108.712) (end 195.7815 108.712) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 196.1 93.75) (end 196.1 94.65) (width 0.15) (layer F.Cu) (net 493))
  (segment (start 202.692 125.2855) (end 200.2155 122.809) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 212.2805 128.27) (end 209.296 125.2855) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 212.2805 132.2705) (end 212.2805 128.27) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 211.582 132.969) (end 212.2805 132.2705) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 200.2155 111.9505) (end 196.977 108.712) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 200.2155 122.809) (end 200.2155 111.9505) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 211.582 134.874) (end 211.582 132.969) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 198.0565 134.3025) (end 200.8505 137.0965) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 200.8505 137.0965) (end 209.3595 137.0965) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 209.296 125.2855) (end 202.692 125.2855) (width 0.15) (layer B.Cu) (net 493))
  (segment (start 209.3595 137.0965) (end 211.582 134.874) (width 0.15) (layer B.Cu) (net 493))
  (via (at 196.977 107.442) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 494))
  (segment (start 195.7815 107.442) (end 196.977 107.442) (width 0.15) (layer F.Cu) (net 494))
  (via (at 197.4215 133.477) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 494))
  (segment (start 197.4215 132.269) (end 197.4215 133.477) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 208.661 123.5075) (end 203.1365 123.5075) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 212.598 134.3025) (end 212.598 127.4445) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 209.4865 137.414) (end 212.598 134.3025) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 197.4215 134.366) (end 200.4695 137.414) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 200.533 120.904) (end 200.533 110.998) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 203.1365 123.5075) (end 200.533 120.904) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 212.598 127.4445) (end 208.661 123.5075) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 200.4695 137.414) (end 209.4865 137.414) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 200.533 110.998) (end 196.977 107.442) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 197.4215 133.477) (end 197.4215 134.366) (width 0.15) (layer B.Cu) (net 494))
  (segment (start 194.691 107.442) (end 195.7815 107.442) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 193.7385 97.3115) (end 193.7385 106.4895) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 195 96.05) (end 193.7385 97.3115) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 196.2 95.45) (end 196 95.45) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 195.5 95.75) (end 195.2 96.05) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 195.7 95.75) (end 195.5 95.75) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 195.2 96.05) (end 195 96.05) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 197 94.85) (end 196.7 95.15) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 196 95.45) (end 195.7 95.75) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 196.5 95.15) (end 196.2 95.45) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 197.2 94.85) (end 197 94.85) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 197.4 94.65) (end 197.2 94.85) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 196.7 95.15) (end 196.5 95.15) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 193.7385 106.4895) (end 194.691 107.442) (width 0.15) (layer F.Cu) (net 494))
  (segment (start 197.4 93.75) (end 197.4 94.65) (width 0.15) (layer F.Cu) (net 494))
  (via (at 197.4215 157.861) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 495))
  (segment (start 197.4215 159.069) (end 197.4215 157.861) (width 0.15) (layer F.Cu) (net 495))
  (segment (start 223.0755 120.777) (end 223.9645 120.777) (width 0.15) (layer F.Cu) (net 495))
  (segment (start 221.1705 122.682) (end 223.0755 120.777) (width 0.15) (layer F.Cu) (net 495))
  (segment (start 219.3815 122.682) (end 221.1705 122.682) (width 0.15) (layer F.Cu) (net 495))
  (segment (start 221.9325 127.4445) (end 221.9325 121.158) (width 0.15) (layer B.Cu) (net 495))
  (segment (start 221.361 138.43) (end 221.361 128.016) (width 0.15) (layer B.Cu) (net 495))
  (segment (start 221.361 128.016) (end 221.9325 127.4445) (width 0.15) (layer B.Cu) (net 495))
  (segment (start 213.8045 145.9865) (end 221.361 138.43) (width 0.15) (layer B.Cu) (net 495))
  (segment (start 209.296 145.9865) (end 213.8045 145.9865) (width 0.15) (layer B.Cu) (net 495))
  (segment (start 197.4215 157.861) (end 209.296 145.9865) (width 0.15) (layer B.Cu) (net 495))
  (segment (start 215.3285 159.766) (end 216.3445 160.782) (width 0.15) (layer B.Cu) (net 497))
  (segment (start 198.6915 160.274) (end 199.1995 159.766) (width 0.15) (layer B.Cu) (net 497))
  (segment (start 199.1995 159.766) (end 215.3285 159.766) (width 0.15) (layer B.Cu) (net 497))
  (segment (start 198.6915 159.069) (end 198.6915 160.274) (width 0.15) (layer F.Cu) (net 497))
  (via (at 198.6915 160.274) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 497))
  (segment (start 199.3265 159.069) (end 199.3265 157.861) (width 0.15) (layer F.Cu) (net 498))
  (via (at 199.3265 157.861) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 498))
  (segment (start 217.6145 159.4485) (end 218.6305 160.4645) (width 0.15) (layer B.Cu) (net 498))
  (segment (start 200.914 159.4485) (end 217.6145 159.4485) (width 0.15) (layer B.Cu) (net 498))
  (segment (start 199.3265 157.861) (end 200.914 159.4485) (width 0.15) (layer B.Cu) (net 498))
  (via (at 201.8665 157.0355) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 499))
  (segment (start 201.8665 159.069) (end 201.8665 157.0355) (width 0.15) (layer F.Cu) (net 499))
  (segment (start 222.6945 122.6185) (end 223.774 121.539) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 222.6945 128.651) (end 222.6945 122.6185) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 222.885 128.8415) (end 222.6945 128.651) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 222.885 137.922) (end 222.885 128.8415) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 221.6785 139.1285) (end 222.885 137.922) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 221.6785 139.5095) (end 221.6785 139.1285) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 214.1855 147.0025) (end 221.6785 139.5095) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 211.836 147.0025) (end 214.1855 147.0025) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 201.8665 156.972) (end 211.836 147.0025) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 201.8665 157.0355) (end 201.8665 156.972) (width 0.15) (layer B.Cu) (net 499))
  (segment (start 221.742 118.6815) (end 223.8375 118.6815) (width 0.15) (layer F.Cu) (net 499))
  (segment (start 220.9165 119.507) (end 221.742 118.6815) (width 0.15) (layer F.Cu) (net 499))
  (segment (start 213.4235 119.507) (end 220.9165 119.507) (width 0.15) (layer F.Cu) (net 499))
  (segment (start 210.1215 122.809) (end 213.4235 119.507) (width 0.15) (layer F.Cu) (net 499))
  (segment (start 210.1215 125.592) (end 210.1215 122.809) (width 0.15) (layer F.Cu) (net 499))
  (via (at 202.5015 157.861) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 500))
  (segment (start 202.5015 159.069) (end 202.5015 157.861) (width 0.15) (layer F.Cu) (net 500))
  (segment (start 211.3915 122.682) (end 212.4075 121.666) (width 0.15) (layer F.Cu) (net 500))
  (segment (start 211.3915 125.592) (end 211.3915 122.682) (width 0.15) (layer F.Cu) (net 500))
  (segment (start 212.4075 121.666) (end 213.2965 120.777) (width 0.15) (layer F.Cu) (net 500))
  (segment (start 213.2965 120.777) (end 220.9165 120.777) (width 0.15) (layer F.Cu) (net 500))
  (segment (start 220.9165 120.777) (end 222.1865 119.507) (width 0.15) (layer F.Cu) (net 500))
  (segment (start 222.1865 119.507) (end 223.8375 119.507) (width 0.15) (layer F.Cu) (net 500))
  (segment (start 223.2025 128.5875) (end 223.012 128.397) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 223.2025 139.03325) (end 223.2025 128.5875) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 221.488 140.1445) (end 222.09125 140.1445) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 202.3745 157.734) (end 202.3745 156.9085) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 214.249 147.3835) (end 221.488 140.1445) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 202.3745 156.9085) (end 211.8995 147.3835) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 223.012 122.7455) (end 223.9645 121.793) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 223.012 128.397) (end 223.012 122.7455) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 211.8995 147.3835) (end 214.249 147.3835) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 222.09125 140.1445) (end 223.2025 139.03325) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 202.5015 157.861) (end 202.3745 157.734) (width 0.15) (layer B.Cu) (net 500))
  (segment (start 203.1365 159.069) (end 203.1365 157.0355) (width 0.15) (layer F.Cu) (net 501) (tstamp 619F7D28))
  (via (at 203.1365 157.0355) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 501) (tstamp 619F7D2A))
  (segment (start 217.7415 159.131) (end 218.7575 160.147) (width 0.15) (layer B.Cu) (net 501))
  (segment (start 203.6445 159.131) (end 217.7415 159.131) (width 0.15) (layer B.Cu) (net 501))
  (segment (start 203.1365 158.623) (end 203.6445 159.131) (width 0.15) (layer B.Cu) (net 501))
  (segment (start 203.1365 157.0355) (end 203.1365 158.623) (width 0.15) (layer B.Cu) (net 501))
  (via (at 206.9465 157.5435) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 502))
  (segment (start 206.9465 159.069) (end 206.9465 157.5435) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 224.3455 105.791) (end 224.3455 102.1715) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 224.028 106.1085) (end 224.3455 105.791) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 224.028 108.204) (end 224.028 106.1085) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 223.7105 108.5215) (end 224.028 108.204) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 223.7105 109.2835) (end 223.7105 108.5215) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 223.393 109.601) (end 223.7105 109.2835) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 223.393 110.49) (end 223.393 109.601) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 223.0755 110.8075) (end 223.393 110.49) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 223.0755 111.633) (end 223.0755 110.8075) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 222.758 111.9505) (end 223.0755 111.633) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 222.758 112.776) (end 222.758 111.9505) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 222.4405 113.0935) (end 222.758 112.776) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 222.4405 113.919) (end 222.4405 113.0935) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 222.123 114.2365) (end 222.4405 113.919) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 222.123 114.9985) (end 222.123 114.2365) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 221.8055 115.316) (end 222.123 114.9985) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 221.8055 116.1415) (end 221.8055 115.316) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 221.107 116.84) (end 221.8055 116.1415) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 221.107 117.1575) (end 221.107 116.84) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 220.6625 117.602) (end 221.107 117.1575) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 219.3815 117.602) (end 220.6625 117.602) (width 0.15) (layer F.Cu) (net 502))
  (segment (start 224.028 122.3645) (end 224.409 121.9835) (width 0.15) (layer B.Cu) (net 502))
  (segment (start 224.028 126.746) (end 224.028 122.3645) (width 0.15) (layer B.Cu) (net 502))
  (segment (start 224.2185 126.9365) (end 224.028 126.746) (width 0.15) (layer B.Cu) (net 502))
  (segment (start 224.2185 141.2875) (end 224.2185 126.9365) (width 0.15) (layer B.Cu) (net 502))
  (segment (start 209.1055 156.4005) (end 224.2185 141.2875) (width 0.15) (layer B.Cu) (net 502))
  (segment (start 208.534 156.4005) (end 209.1055 156.4005) (width 0.15) (layer B.Cu) (net 502))
  (segment (start 207.391 157.5435) (end 208.534 156.4005) (width 0.15) (layer B.Cu) (net 502))
  (segment (start 206.9465 157.5435) (end 207.391 157.5435) (width 0.15) (layer B.Cu) (net 502))
  (segment (start 208.8515 159.069) (end 208.8515 158.115) (width 0.15) (layer F.Cu) (net 503))
  (via (at 208.7245 156.9085) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 503))
  (segment (start 208.7245 157.988) (end 208.7245 156.9085) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 208.8515 158.115) (end 208.7245 157.988) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 224.028 108.6485) (end 224.3455 108.331) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 224.663 105.918) (end 224.663 101.7905) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 223.393 111.76) (end 223.393 110.96625) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 223.7105 109.728) (end 224.028 109.4105) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 223.0755 112.0775) (end 223.393 111.76) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 223.0755 112.903) (end 223.0755 112.0775) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 224.3455 108.331) (end 224.3455 106.2355) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 222.758 113.2205) (end 223.0755 112.903) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 222.4405 114.3635) (end 222.758 114.046) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 224.3455 106.2355) (end 224.663 105.918) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 223.393 110.96625) (end 223.7105 110.64875) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 219.3815 118.872) (end 220.6625 118.872) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 222.4405 115.1255) (end 222.4405 114.3635) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 222.123 116.2685) (end 222.123 115.443) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 222.123 115.443) (end 222.4405 115.1255) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 221.4245 116.967) (end 222.123 116.2685) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 221.4245 117.2845) (end 221.4245 116.967) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 222.758 114.046) (end 222.758 113.2205) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 221.107 118.4275) (end 221.107 117.602) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 220.6625 118.872) (end 221.107 118.4275) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 224.028 109.4105) (end 224.028 108.6485) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 223.7105 110.64875) (end 223.7105 109.728) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 221.107 117.602) (end 221.4245 117.2845) (width 0.15) (layer F.Cu) (net 503))
  (segment (start 224.3455 126.619) (end 224.3455 122.4915) (width 0.15) (layer B.Cu) (net 503))
  (segment (start 224.536 126.8095) (end 224.3455 126.619) (width 0.15) (layer B.Cu) (net 503))
  (segment (start 224.536 141.4145) (end 224.536 126.8095) (width 0.15) (layer B.Cu) (net 503))
  (segment (start 209.042 156.9085) (end 224.536 141.4145) (width 0.15) (layer B.Cu) (net 503))
  (segment (start 208.7245 156.9085) (end 209.042 156.9085) (width 0.15) (layer B.Cu) (net 503))
  (via (at 212.471 156.9085) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 504))
  (segment (start 212.6615 159.069) (end 212.6615 157.099) (width 0.15) (layer F.Cu) (net 504))
  (segment (start 212.6615 157.099) (end 212.471 156.9085) (width 0.15) (layer F.Cu) (net 504))
  (segment (start 218.2405 158.08) (end 218.532 158.08) (width 0.15) (layer B.Cu) (net 504))
  (segment (start 217.9405 158.38) (end 218.2405 158.08) (width 0.15) (layer B.Cu) (net 504))
  (segment (start 213.1805 158.38) (end 217.9405 158.38) (width 0.15) (layer B.Cu) (net 504))
  (segment (start 212.471 157.6705) (end 213.1805 158.38) (width 0.15) (layer B.Cu) (net 504))
  (segment (start 212.471 156.9085) (end 212.471 157.6705) (width 0.15) (layer B.Cu) (net 504))
  (via (at 213.487 156.9085) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 505))
  (segment (start 213.2965 157.099) (end 213.487 156.9085) (width 0.15) (layer F.Cu) (net 505))
  (segment (start 213.2965 159.069) (end 213.2965 157.099) (width 0.15) (layer F.Cu) (net 505))
  (segment (start 214.7405 157.98) (end 216.9905 157.98) (width 0.15) (layer B.Cu) (net 505))
  (segment (start 213.669 156.9085) (end 214.7405 157.98) (width 0.15) (layer B.Cu) (net 505))
  (segment (start 213.487 156.9085) (end 213.669 156.9085) (width 0.15) (layer B.Cu) (net 505))
  (via (at 214.5665 157.0355) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 506))
  (segment (start 214.5665 159.069) (end 214.5665 157.0355) (width 0.15) (layer F.Cu) (net 506))
  (segment (start 217.551 157.353) (end 218.567 157.353) (width 0.15) (layer B.Cu) (net 506))
  (segment (start 215.211 157.68) (end 217.224 157.68) (width 0.15) (layer B.Cu) (net 506))
  (segment (start 217.224 157.68) (end 217.551 157.353) (width 0.15) (layer B.Cu) (net 506))
  (segment (start 214.5665 157.0355) (end 215.211 157.68) (width 0.15) (layer B.Cu) (net 506))
  (segment (start 215.2015 159.069) (end 215.2015 156.21) (width 0.15) (layer F.Cu) (net 507))
  (via (at 215.2015 156.21) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 507))
  (segment (start 215.2015 156.21) (end 218.3705 156.21) (width 0.15) (layer B.Cu) (net 507))
  (segment (start 216.4715 159.069) (end 216.4715 160.111) (width 0.15) (layer F.Cu) (net 508))
  (segment (start 216.4715 160.111) (end 217.2905 160.93) (width 0.15) (layer F.Cu) (net 508))
  (segment (start 217.2905 160.93) (end 218.2405 160.93) (width 0.15) (layer F.Cu) (net 508))
  (via (at 219.5405 159.63) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 508))
  (segment (start 218.2405 160.93) (end 219.5405 159.63) (width 0.15) (layer F.Cu) (net 508))
  (segment (start 219.5405 159.63) (end 219.7405 159.83) (width 0.15) (layer B.Cu) (net 508))
  (segment (start 216.1 55.55) (end 218.1 55.55) (width 0.15) (layer F.Cu) (net 509))
  (via (at 218.1 55.55) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 509))
  (via (at 214.6 48.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 510))
  (segment (start 214.1 48.55) (end 214.6 48.05) (width 0.15) (layer F.Cu) (net 510))
  (segment (start 214.9 48.05) (end 214.6 48.05) (width 0.15) (layer B.Cu) (net 510))
  (segment (start 215.4 47.55) (end 214.9 48.05) (width 0.15) (layer B.Cu) (net 510))
  (segment (start 215.8 47.55) (end 215.4 47.55) (width 0.15) (layer B.Cu) (net 510))
  (segment (start 216.3 48.05) (end 215.8 47.55) (width 0.15) (layer B.Cu) (net 510))
  (via (at 217.55 47.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 510))
  (segment (start 217.4 48.05) (end 217.55 47.9) (width 0.15) (layer B.Cu) (net 510))
  (segment (start 216.3 48.05) (end 217.4 48.05) (width 0.15) (layer B.Cu) (net 510))
  (segment (start 218.55 46.1) (end 220.35 46.1) (width 0.15) (layer F.Cu) (net 510))
  (segment (start 217.55 47.1) (end 218.55 46.1) (width 0.15) (layer F.Cu) (net 510))
  (segment (start 217.55 47.9) (end 217.55 47.1) (width 0.15) (layer F.Cu) (net 510))
  (segment (start 224 45.45) (end 224.6 46.05) (width 0.15) (layer F.Cu) (net 511))
  (segment (start 218.65 45.45) (end 224 45.45) (width 0.15) (layer F.Cu) (net 511))
  (segment (start 217.05 47.05) (end 218.65 45.45) (width 0.15) (layer F.Cu) (net 511))
  (segment (start 215.6 47.05) (end 217.05 47.05) (width 0.15) (layer F.Cu) (net 511))
  (segment (start 215.1 47.55) (end 215.6 47.05) (width 0.15) (layer F.Cu) (net 511))
  (segment (start 218.05 47.05) (end 218.7 46.4) (width 0.15) (layer F.Cu) (net 512))
  (segment (start 218.05 48.25) (end 218.05 47.05) (width 0.15) (layer F.Cu) (net 512))
  (segment (start 217.9 48.4) (end 218.05 48.25) (width 0.15) (layer F.Cu) (net 512))
  (segment (start 218.7 46.4) (end 220.2 46.4) (width 0.15) (layer F.Cu) (net 512))
  (segment (start 216.25 48.4) (end 217.9 48.4) (width 0.15) (layer F.Cu) (net 512))
  (segment (start 216.1 48.55) (end 216.25 48.4) (width 0.15) (layer F.Cu) (net 512))
  (via (at 214.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 513))
  (segment (start 214.1 46.55) (end 214.6 46.05) (width 0.15) (layer F.Cu) (net 513))
  (segment (start 214.6 46.05) (end 214.8 46.05) (width 0.15) (layer B.Cu) (net 513))
  (segment (start 214.8 46.05) (end 215.3 45.55) (width 0.15) (layer B.Cu) (net 513))
  (segment (start 215.3 45.55) (end 215.8 45.55) (width 0.15) (layer B.Cu) (net 513))
  (segment (start 215.8 45.55) (end 216.1 45.25) (width 0.15) (layer B.Cu) (net 513))
  (segment (start 216.1 45.25) (end 216.1 41) (width 0.15) (layer B.Cu) (net 513))
  (via (at 213.6 46.05) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 514))
  (segment (start 213.1 46.55) (end 213.6 46.05) (width 0.15) (layer F.Cu) (net 514))
  (segment (start 213.6 46.05) (end 213.8 46.05) (width 0.15) (layer B.Cu) (net 514))
  (segment (start 213.8 46.05) (end 214.3 45.55) (width 0.15) (layer B.Cu) (net 514))
  (segment (start 214.3 45.55) (end 214.85 45.55) (width 0.15) (layer B.Cu) (net 514))
  (segment (start 214.85 45.55) (end 215.1 45.3) (width 0.15) (layer B.Cu) (net 514))
  (segment (start 215.1 45.3) (end 215.1 44.8) (width 0.15) (layer B.Cu) (net 514))
  (segment (start 215.1 44.8) (end 215.3 44.6) (width 0.15) (layer B.Cu) (net 514))
  (segment (start 215.3 44.6) (end 215.3 41.5) (width 0.15) (layer B.Cu) (net 514))
  (via (at 230.3 157.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 541))
  (segment (start 228.4 157.6) (end 230.3 157.6) (width 0.15) (layer F.Cu) (net 541))
  (segment (start 230.3 157.6) (end 232.5 157.6) (width 0.15) (layer B.Cu) (net 541))
  (segment (start 232.5 157.6) (end 233 158.1) (width 0.15) (layer B.Cu) (net 541))
  (segment (start 233 158.1) (end 235.4 158.1) (width 0.15) (layer B.Cu) (net 541))
  (segment (start 228.4 158.9) (end 230.3 158.9) (width 0.15) (layer F.Cu) (net 542))
  (via (at 230.3 158.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 542))
  (segment (start 230.3 158.9) (end 232.5 158.9) (width 0.15) (layer B.Cu) (net 542))
  (segment (start 232.5 158.9) (end 233 159.4) (width 0.15) (layer B.Cu) (net 542))
  (segment (start 233 159.4) (end 235.45 159.4) (width 0.15) (layer B.Cu) (net 542))
  (via (at 230.3 160.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 543))
  (segment (start 228.4 160.2) (end 230.3 160.2) (width 0.15) (layer F.Cu) (net 543))
  (segment (start 230.3 160.2) (end 232.5 160.2) (width 0.15) (layer B.Cu) (net 543))
  (segment (start 232.5 160.2) (end 233 160.7) (width 0.15) (layer B.Cu) (net 543))
  (segment (start 233 160.7) (end 235.5 160.7) (width 0.15) (layer B.Cu) (net 543))
  (via (at 230.3 161.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 544))
  (segment (start 228.4 161.5) (end 230.3 161.5) (width 0.15) (layer F.Cu) (net 544))
  (segment (start 230.3 161.5) (end 232.5 161.5) (width 0.15) (layer B.Cu) (net 544))
  (segment (start 232.5 161.5) (end 233 162) (width 0.15) (layer B.Cu) (net 544))
  (segment (start 233 162) (end 235.8 162) (width 0.15) (layer B.Cu) (net 544))
  (segment (start 228.4 156.3) (end 230.3 156.3) (width 0.15) (layer F.Cu) (net 545))
  (via (at 230.3 156.3) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 545))
  (via (at 232.4 156.95) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 545))
  (segment (start 234.3 156.95) (end 232.4 156.95) (width 0.15) (layer F.Cu) (net 545))
  (via (at 233.2 157.6) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 546))
  (segment (start 234.3 157.6) (end 233.2 157.6) (width 0.15) (layer F.Cu) (net 546))
  (segment (start 233.2 157.6) (end 235.5 157.6) (width 0.15) (layer B.Cu) (net 546))
  (via (at 233.2 158.9) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 547))
  (segment (start 234.3 158.9) (end 233.2 158.9) (width 0.15) (layer F.Cu) (net 547))
  (segment (start 233.2 158.9) (end 235.55 158.9) (width 0.15) (layer B.Cu) (net 547))
  (via (at 233.2 160.2) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 548))
  (segment (start 234.3 160.2) (end 233.2 160.2) (width 0.15) (layer F.Cu) (net 548))
  (segment (start 233.2 160.2) (end 235.45 160.2) (width 0.15) (layer B.Cu) (net 548))
  (via (at 233.2 161.5) (size 0.5) (drill 0.2) (layers F.Cu B.Cu) (net 549))
  (segment (start 234.3 161.5) (end 233.2 161.5) (width 0.15) (layer F.Cu) (net 549))
  (segment (start 233.2 161.5) (end 235.4 161.5) (width 0.15) (layer B.Cu) (net 549))

  (zone (net 2) (net_name GND) (layer F.Cu) (tstamp 0) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 272.034 163.957) (xy 189.357 163.957) (xy 189.357 26.162) (xy 272.034 26.162)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (tstamp 6197AC22) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 272.034 163.957) (xy 189.357 163.957) (xy 189.357 26.162) (xy 272.034 26.162)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer In2.Cu) (tstamp 618A8318) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 272.034 163.957) (xy 189.357 163.957) (xy 189.357 26.162) (xy 272.034 26.162)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (tstamp 618A8319) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 272.034 163.957) (xy 189.357 163.957) (xy 189.357 26.162) (xy 272.034 26.162)
      )
    )
  )
)
