Signal Name | Total Product Terms | Product Terms | Location | Power Mode | Pin Number | PinType | Pin Use
--- | --- | --- | --- | --- | --- | --- | ---
ram/RS_FSM_FFd4 | 1 | 1_1 | MC1 | STD |  | (b) | (b)
ram/RS_FSM_FFd3 | 1 | 2_1 | MC2 | STD | 11 | I/O | I
ram/RS_FSM_FFd2 | 1 | 3_1 | MC3 | STD | 12 | I/O | I
ram/RS_FSM_FFd1 | 1 | 4_1 | MC4 | STD |  | (b) | (b)
ram/RASrf | 1 | 5_1 | MC5 | STD | 13 | I/O | I
iobm/Er | 1 | 6_1 | MC6 | STD | 14 | I/O | I
cnt/nIPL2r | 1 | 7_1 | MC7 | STD |  | (b) | (b)
cnt/IS_FSM_FFd1 | 1 | 8_1 | MC8 | STD | 15 | I/O | I
cnt/Er<0> | 1 | 9_1 | MC9 | STD | 16 | I/O | I
ram/RefDone | 2 | 10_1 10_2 | MC10 | STD |  | (b) | (b)
ram/RS_FSM_FFd5 | 2 | 11_1 11_2 | MC11 | STD | 17 | I/O | I
iobs/IOU1 | 2 | 12_1 12_2 | MC12 | STD | 18 | I/O | I
iobs/IOL1 | 2 | 13_1 13_2 | MC13 | STD |  | (b) | (b)
cnt/Timer<0> | 2 | 14_1 14_2 | MC14 | STD | 19 | I/O | I
cnt/IS_FSM_FFd2 | 2 | 15_1 15_2 | MC15 | STD | 20 | I/O | I
RefUrg | 2 | 16_1 16_2 | MC16 | STD |  | (b) | (b)
IOBERR | 2 | 17_1 17_2 | MC17 | STD | 22 | I/O/GCK1 | GCK
iobm/ES<2> | 3 | 18_1 18_2 18_3 | MC18 | STD |  | (b) | (b)

Signals Used By Logic in Function Block

1. E
2. RefReq
3. RefUrg
4. cnt/Er<0>
5. cnt/Er<1>
6. cnt/IS_FSM_FFd1
7. cnt/IS_FSM_FFd2
8. cnt/LTimerTC
9. cnt/Timer<0>
10. cnt/Timer<1>
11. cnt/Timer<2>
12. cnt/Timer<3>
13. cnt/TimerTC
14. cnt/nIPL2r
15. iobm/ES<0>
16. iobm/ES<1>
17. iobm/ES<2>
18. iobm/Er
19. iobs/Load1
20. nAS_IOB
21. nBERR_IOB
22. nIPL2
23. nLDS_FSB
24. nUDS_FSB
25. ram/DTACKr
26. ram/RS_FSM_FFd1
27. ram/RS_FSM_FFd2
28. ram/RS_FSM_FFd3
29. ram/RS_FSM_FFd5
30. ram/RS_FSM_FFd6
31. ram/RS_FSM_FFd7
32. ram/RefDone