Release 14.7 - xst P.20131013 (nt64)
Copyright (c) 1995-2013 Xilinx, Inc.  All rights reserved.
--> Parameter TMPDIR set to xst/projnav.tmp


Total REAL time to Xst completion: 0.00 secs
Total CPU time to Xst completion: 0.09 secs
 
--> Parameter xsthdpdir set to xst


Total REAL time to Xst completion: 0.00 secs
Total CPU time to Xst completion: 0.09 secs
 
--> Reading design: WarpSE.prj

TABLE OF CONTENTS
  1) Synthesis Options Summary
  2) HDL Compilation
  3) Design Hierarchy Analysis
  4) HDL Analysis
  5) HDL Synthesis
     5.1) HDL Synthesis Report
  6) Advanced HDL Synthesis
     6.1) Advanced HDL Synthesis Report
  7) Low Level Synthesis
  8) Partition Report
  9) Final Report

=========================================================================
*                      Synthesis Options Summary                        *
=========================================================================
---- Source Parameters
Input File Name                    : "WarpSE.prj"
Input Format                       : mixed
Ignore Synthesis Constraint File   : NO

---- Target Parameters
Output File Name                   : "WarpSE"
Output Format                      : NGC
Target Device                      : XC9500XL CPLDs

---- Source Options
Top Module Name                    : WarpSE
Automatic FSM Extraction           : YES
FSM Encoding Algorithm             : Auto
Safe Implementation                : No
Mux Extraction                     : Yes
Resource Sharing                   : YES

---- Target Options
Add IO Buffers                     : YES
MACRO Preserve                     : YES
XOR Preserve                       : YES
Equivalent register Removal        : YES

---- General Options
Optimization Goal                  : Speed
Optimization Effort                : 1
Keep Hierarchy                     : Yes
Netlist Hierarchy                  : As_Optimized
RTL Output                         : Yes
Hierarchy Separator                : /
Bus Delimiter                      : <>
Case Specifier                     : Maintain
Verilog 2001                       : YES

---- Other Options
Clock Enable                       : YES
wysiwyg                            : NO

=========================================================================


=========================================================================
*                          HDL Compilation                              *
=========================================================================
Compiling verilog file "../RAM.v" in library work
Compiling verilog file "../IOBS.v" in library work
Module <RAM> compiled
Compiling verilog file "../IOBM.v" in library work
Module <IOBS> compiled
Compiling verilog file "../FSB.v" in library work
Module <IOBM> compiled
Compiling verilog file "../CS.v" in library work
Module <FSB> compiled
Compiling verilog file "../CNT.v" in library work
Module <CS> compiled
Compiling verilog file "../WarpSE.v" in library work
Module <CNT> compiled
Module <WarpSE> compiled
No errors in compilation
Analysis of file <"WarpSE.prj"> succeeded.
 

=========================================================================
*                     Design Hierarchy Analysis                         *
=========================================================================
Analyzing hierarchy for module <WarpSE> in library <work>.

Analyzing hierarchy for module <CS> in library <work>.

Analyzing hierarchy for module <RAM> in library <work>.

Analyzing hierarchy for module <IOBS> in library <work>.

Analyzing hierarchy for module <IOBM> in library <work>.

Analyzing hierarchy for module <CNT> in library <work>.

Analyzing hierarchy for module <FSB> in library <work>.


=========================================================================
*                            HDL Analysis                               *
=========================================================================
Analyzing top module <WarpSE>.
Module <WarpSE> is correct for synthesis.
 
Analyzing module <CS> in library <work>.
Module <CS> is correct for synthesis.
 
Analyzing module <RAM> in library <work>.
Module <RAM> is correct for synthesis.
 
Analyzing module <IOBS> in library <work>.
Module <IOBS> is correct for synthesis.
 
Analyzing module <IOBM> in library <work>.
Module <IOBM> is correct for synthesis.
 
Analyzing module <CNT> in library <work>.
Module <CNT> is correct for synthesis.
 
Analyzing module <FSB> in library <work>.
Module <FSB> is correct for synthesis.
 

=========================================================================
*                           HDL Synthesis                               *
=========================================================================

Performing bidirectional port resolution...

Synthesizing Unit <CS>.
    Related source file is "../CS.v".
    Found 1-bit register for signal <nOverlay>.
Unit <CS> synthesized.


Synthesizing Unit <RAM>.
    Related source file is "../RAM.v".
    Found finite state machine <FSM_0> for signal <RS>.
    -----------------------------------------------------------------------
    | States             | 8                                              |
    | Transitions        | 14                                             |
    | Inputs             | 6                                              |
    | Outputs            | 8                                              |
    | Clock              | CLK                       (rising_edge)        |
    | Power Up State     | 000                                            |
    | Encoding           | automatic                                      |
    | Implementation     | automatic                                      |
    -----------------------------------------------------------------------
    Found 1-bit register for signal <nCAS>.
    Found 1-bit register for signal <nOE>.
    Found 1-bit register for signal <RAMReady>.
    Found 1-bit register for signal <DTACKr>.
    Found 1-bit register for signal <RASEL>.
    Found 1-bit register for signal <RASEN>.
    Found 1-bit register for signal <RASrf>.
    Found 1-bit register for signal <RASrr>.
    Found 1-bit register for signal <RefDone>.
    Summary:
	inferred   1 Finite State Machine(s).
	inferred   8 D-type flip-flop(s).
Unit <RAM> synthesized.


Synthesizing Unit <IOBS>.
    Related source file is "../IOBS.v".
    Found finite state machine <FSM_1> for signal <TS>.
    -----------------------------------------------------------------------
    | States             | 4                                              |
    | Transitions        | 10                                             |
    | Inputs             | 5                                              |
    | Outputs            | 5                                              |
    | Clock              | CLK                       (rising_edge)        |
    | Power Up State     | 00                                             |
    | Encoding           | automatic                                      |
    | Implementation     | automatic                                      |
    -----------------------------------------------------------------------
    Found 1-bit register for signal <IORDREQ>.
    Found 1-bit register for signal <IOL0>.
    Found 1-bit register for signal <IOWRREQ>.
    Found 1-bit register for signal <IONPReady>.
    Found 1-bit register for signal <IOU0>.
    Found 1-bit register for signal <ALE0>.
    Found 1-bit register for signal <ALE1>.
    Found 1-bit register for signal <nBERR_FSB>.
    Found 1-bit register for signal <Clear1>.
    Found 1-bit register for signal <IOACTr>.
    Found 1-bit register for signal <IODONEr>.
    Found 1-bit register for signal <IOL1>.
    Found 1-bit register for signal <IORW1>.
    Found 1-bit register for signal <IOU1>.
    Found 1-bit register for signal <Load1>.
    Found 1-bit register for signal <Sent>.
    Summary:
	inferred   1 Finite State Machine(s).
	inferred  10 D-type flip-flop(s).
Unit <IOBS> synthesized.


Synthesizing Unit <IOBM>.
    Related source file is "../IOBM.v".
    Found finite state machine <FSM_2> for signal <IOS>.
    -----------------------------------------------------------------------
    | States             | 7                                              |
    | Transitions        | 13                                             |
    | Inputs             | 5                                              |
    | Outputs            | 7                                              |
    | Clock              | C16M                      (rising_edge)        |
    | Power Up State     | 000                                            |
    | Encoding           | automatic                                      |
    | Implementation     | automatic                                      |
    -----------------------------------------------------------------------
    Found 1-bit register for signal <IOBERR>.
    Found 1-bit register for signal <nASout>.
    Found 1-bit register for signal <IOACT>.
    Found 1-bit register for signal <IODONE>.
    Found 1-bit register for signal <nLDS>.
    Found 1-bit register for signal <nUDS>.
    Found 1-bit register for signal <nDinLE>.
    Found 1-bit register for signal <ALE0>.
    Found 1-bit register for signal <nVMA>.
    Found 1-bit register for signal <C8Mr>.
    Found 1-bit register for signal <DoutOE>.
    Found 1-bit register for signal <Er>.
    Found 4-bit up counter for signal <ES>.
    Found 1-bit register for signal <IORDREQr>.
    Found 1-bit register for signal <IOS0>.
    Found 1-bit register for signal <IOWRREQr>.
    Found 1-bit register for signal <VPAr>.
    Summary:
	inferred   1 Finite State Machine(s).
	inferred   1 Counter(s).
	inferred  15 D-type flip-flop(s).
Unit <IOBM> synthesized.


Synthesizing Unit <CNT>.
    Related source file is "../CNT.v".
WARNING:Xst:647 - Input <SndROMCS> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <WS> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <nWE> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <RAMCS> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:646 - Signal <C8MFall> is assigned but never used. This unconnected signal will be trimmed during the optimization process.
    Found finite state machine <FSM_3> for signal <IS>.
    -----------------------------------------------------------------------
    | States             | 4                                              |
    | Transitions        | 8                                              |
    | Inputs             | 2                                              |
    | Outputs            | 4                                              |
    | Clock              | CLK                       (rising_edge)        |
    | Power Up State     | 00                                             |
    | Encoding           | automatic                                      |
    | Implementation     | automatic                                      |
    -----------------------------------------------------------------------
    Found 1-bit register for signal <RefUrg>.
    Found 1-bit register for signal <RefReq>.
    Found 1-bit register for signal <nBR_IOB>.
    Found 1-bit register for signal <nRESout>.
    Found 1-bit register for signal <AoutOE>.
    Found 1-bit register for signal <QoSReady>.
    Found 2-bit register for signal <C8Mr>.
    Found 2-bit register for signal <Er>.
    Found 12-bit up counter for signal <LTimer>.
    Found 1-bit register for signal <LTimerTC>.
    Found 1-bit register for signal <nIPL2r>.
    Found 2-bit up counter for signal <QS>.
    Found 4-bit up counter for signal <Timer>.
    Found 1-bit register for signal <TimerTC>.
    Found 5-bit up counter for signal <Wait>.
    Summary:
	inferred   1 Finite State Machine(s).
	inferred   4 Counter(s).
	inferred   9 D-type flip-flop(s).
Unit <CNT> synthesized.


Synthesizing Unit <FSB>.
    Related source file is "../FSB.v".
    Found 1-bit register for signal <nVPA>.
    Found 1-bit register for signal <nDTACK>.
    Found 1-bit register for signal <WS>.
    Found 1-bit register for signal <ASrf>.
    Found 3-bit register for signal <BACTr>.
    Summary:
	inferred   4 D-type flip-flop(s).
Unit <FSB> synthesized.


Synthesizing Unit <WarpSE>.
    Related source file is "../WarpSE.v".
WARNING:Xst:647 - Input <C20MEN> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <SW> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:647 - Input <nBG_IOB> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved.
WARNING:Xst:653 - Signal <SndROMCS> is used but never assigned. This sourceless signal will be automatically connected to value 0.
    Found 1-bit tristate buffer for signal <nAS_IOB>.
    Found 1-bit tristate buffer for signal <nLDS_IOB>.
    Found 1-bit tristate buffer for signal <nRES>.
    Found 1-bit tristate buffer for signal <nUDS_IOB>.
    Found 1-bit tristate buffer for signal <nVMA_IOB>.
    Summary:
	inferred   5 Tristate(s).
Unit <WarpSE> synthesized.


=========================================================================
HDL Synthesis Report

Macro Statistics
# Counters                                             : 5
 12-bit up counter                                     : 1
 2-bit up counter                                      : 1
 4-bit up counter                                      : 2
 5-bit up counter                                      : 1
# Registers                                            : 58
 1-bit register                                        : 55
 2-bit register                                        : 2
 3-bit register                                        : 1
# Tristates                                            : 5
 1-bit tristate buffer                                 : 5

=========================================================================

=========================================================================
*                       Advanced HDL Synthesis                          *
=========================================================================

Analyzing FSM <FSM_3> for best encoding.
Optimizing FSM <cnt/IS/FSM> on signal <IS[1:2]> with johnson encoding.
-------------------
 State | Encoding
-------------------
 00    | 00
 01    | 01
 10    | 11
 11    | 10
-------------------
Analyzing FSM <FSM_2> for best encoding.
Optimizing FSM <iobm/IOS/FSM> on signal <IOS[1:7]> with one-hot encoding.
-------------------
 State | Encoding
-------------------
 000   | 0000001
 010   | 0000010
 011   | 0000100
 100   | 0001000
 101   | 0010000
 110   | 0100000
 111   | 1000000
-------------------
Analyzing FSM <FSM_1> for best encoding.
Optimizing FSM <iobs/TS/FSM> on signal <TS[1:2]> with johnson encoding.
-------------------
 State | Encoding
-------------------
 00    | 00
 11    | 01
 10    | 11
 01    | 10
-------------------
Analyzing FSM <FSM_0> for best encoding.
Optimizing FSM <ram/RS/FSM> on signal <RS[1:8]> with one-hot encoding.
-------------------
 State | Encoding
-------------------
 000   | 00000001
 100   | 00000010
 001   | 00000100
 010   | 00001000
 011   | 00010000
 101   | 00100000
 110   | 01000000
 111   | 10000000
-------------------

=========================================================================
Advanced HDL Synthesis Report

Macro Statistics
# FSMs                                                 : 4
# Counters                                             : 5
 12-bit up counter                                     : 1
 2-bit up counter                                      : 1
 4-bit up counter                                      : 2
 5-bit up counter                                      : 1
# Registers                                            : 46
 Flip-Flops                                            : 46

=========================================================================

=========================================================================
*                         Low Level Synthesis                           *
=========================================================================
WARNING:Xst:2677 - Node <C8Mr_1> of sequential type is unconnected in block <CNT>.
WARNING:Xst:2677 - Node <C8Mr_0> of sequential type is unconnected in block <CNT>.

Optimizing unit <WarpSE> ...

Optimizing unit <CS> ...
  implementation constraint: INIT=r	 : nOverlay

Optimizing unit <RAM> ...
  implementation constraint: INIT=s	 : RS_FSM_FFd8
  implementation constraint: INIT=r	 : RASEL
  implementation constraint: INIT=r	 : RASrr
  implementation constraint: INIT=r	 : RASEN
  implementation constraint: INIT=r	 : RS_FSM_FFd1
  implementation constraint: INIT=r	 : RS_FSM_FFd2
  implementation constraint: INIT=r	 : RS_FSM_FFd3
  implementation constraint: INIT=r	 : RS_FSM_FFd4
  implementation constraint: INIT=r	 : RS_FSM_FFd5
  implementation constraint: INIT=r	 : RS_FSM_FFd6
  implementation constraint: INIT=r	 : RS_FSM_FFd7
  implementation constraint: INIT=r	 : RASrf

Optimizing unit <IOBS> ...
  implementation constraint: INIT=r	 : IOACTr
  implementation constraint: INIT=r	 : TS_FSM_FFd2
  implementation constraint: INIT=r	 : Sent
  implementation constraint: INIT=r	 : TS_FSM_FFd1

Optimizing unit <FSB> ...
  implementation constraint: INIT=r	 : ASrf

Optimizing unit <IOBM> ...
  implementation constraint: INIT=s	 : IOS_FSM_FFd7
  implementation constraint: INIT=r	 : DoutOE
  implementation constraint: INIT=r	 : IOS_FSM_FFd6
  implementation constraint: INIT=r	 : IOS_FSM_FFd1
  implementation constraint: INIT=r	 : IOS_FSM_FFd2
  implementation constraint: INIT=r	 : IOS_FSM_FFd3
  implementation constraint: INIT=r	 : IOS_FSM_FFd4
  implementation constraint: INIT=r	 : IOS_FSM_FFd5

Optimizing unit <CNT> ...
  implementation constraint: INIT=r	 : IS_FSM_FFd1
  implementation constraint: INIT=r	 : Wait_4
  implementation constraint: INIT=r	 : Wait_0
  implementation constraint: INIT=r	 : Wait_1
  implementation constraint: INIT=r	 : Wait_2
  implementation constraint: INIT=r	 : Wait_3
  implementation constraint: INIT=r	 : Timer_3
  implementation constraint: INIT=r	 : IS_FSM_FFd2
  implementation constraint: INIT=r	 : Timer_0
  implementation constraint: INIT=r	 : Timer_1
  implementation constraint: INIT=r	 : Timer_2
WARNING:Xst:2677 - Node <BACTr_2> of sequential type is unconnected in block <fsb>.
WARNING:Xst:2677 - Node <BACTr_1> of sequential type is unconnected in block <fsb>.
WARNING:Xst:2677 - Node <WS> of sequential type is unconnected in block <fsb>.

=========================================================================
*                           Partition Report                            *
=========================================================================

Partition Implementation Status
-------------------------------

  No Partitions were found in this design.

-------------------------------

=========================================================================
*                            Final Report                               *
=========================================================================
Final Results
RTL Top Level Output File Name     : WarpSE.ngr
Top Level Output File Name         : WarpSE
Output Format                      : NGC
Optimization Goal                  : Speed
Keep Hierarchy                     : Yes
Target Technology                  : XC9500XL CPLDs
Macro Preserve                     : YES
XOR Preserve                       : YES
Clock Enable                       : YES
wysiwyg                            : NO

Design Statistics
# IOs                              : 75

Cell Usage :
# BELS                             : 618
#      AND2                        : 197
#      AND3                        : 25
#      AND4                        : 9
#      AND5                        : 3
#      AND7                        : 1
#      AND8                        : 3
#      GND                         : 6
#      INV                         : 232
#      OR2                         : 101
#      OR3                         : 14
#      OR4                         : 4
#      VCC                         : 1
#      XOR2                        : 22
# FlipFlops/Latches                : 103
#      FD                          : 67
#      FDC                         : 2
#      FDCE                        : 33
#      FDP                         : 1
# IO Buffers                       : 70
#      IBUF                        : 35
#      IOBUFE                      : 1
#      OBUF                        : 30
#      OBUFE                       : 4
=========================================================================


Total REAL time to Xst completion: 5.00 secs
Total CPU time to Xst completion: 4.87 secs
 
--> 

Total memory usage is 267300 kilobytes

Number of errors   :    0 (   0 filtered)
Number of warnings :   14 (   0 filtered)
Number of infos    :    0 (   0 filtered)

