MDF Database:  version 1.0
MDF_INFO | WarpSE | XC95144XL-10-TQ100
MACROCELL | 5 | 1 | nVMA_IOBout
ATTRIBUTES | 4622082 | 0
OUTPUTMC | 2 | 5 | 1 | 5 | 9
INPUTS | 8 | nVMA_IOB  | iobm/ES<0>  | iobm/ES<2>  | iobm/ES<1>  | iobm/ES<3>  | IOACT  | iobm/VPAr  | nAoutOE
INPUTMC | 8 | 5 | 1 | 5 | 4 | 0 | 17 | 5 | 6 | 5 | 5 | 5 | 17 | 1 | 10 | 3 | 1
EQ | 6 | 
   nVMA_IOB.T = !nVMA_IOB & !iobm/ES<0> & !iobm/ES<2> & !iobm/ES<1> & 
	!iobm/ES<3>
	# nVMA_IOB & iobm/ES<0> & iobm/ES<2> & !iobm/ES<1> & 
	!iobm/ES<3> & IOACT & iobm/VPAr;
   nVMA_IOB.CLK = C8M;	// GCK
   nVMA_IOB.OE = !nAoutOE;
GLOBALS | 1 | 2 | C8M

MACROCELL | 5 | 11 | nAS_IOBout
ATTRIBUTES | 8816386 | 0
OUTPUTMC | 2 | 0 | 16 | 5 | 9
INPUTS | 9 | iobm/IOS_FSM_FFd3  | iobm/C8Mr  | iobm/IOS_FSM_FFd4  | iobm/IOS_FSM_FFd5  | iobm/IOS_FSM_FFd6  | iobm/IOS_FSM_FFd7  | iobm/IORDREQr  | iobm/IOWRREQr  | nAoutOE
INPUTMC | 9 | 5 | 3 | 1 | 16 | 1 | 13 | 1 | 12 | 5 | 0 | 5 | 2 | 1 | 15 | 1 | 11 | 3 | 1
EQ | 9 | 
   nAS_IOB.D = !iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6
	# !iobm/IOS_FSM_FFd3 & iobm/C8Mr & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6
	# !iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd4 & 
	!iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & !iobm/IORDREQr & 
	!iobm/IOWRREQr;
   !nAS_IOB.CLK = C16M;	// GCK
   nAS_IOB.OE = !nAoutOE;
GLOBALS | 1 | 2 | C16M

MACROCELL | 5 | 8 | nLDS_IOBout
ATTRIBUTES | 8816386 | 0
OUTPUTMC | 1 | 5 | 8
INPUTS | 8 | iobm/IOS_FSM_FFd3  | IOL0  | iobm/IOS_FSM_FFd5  | iobm/IOS_FSM_FFd4  | nLDS_IOB  | iobm/IOS_FSM_FFd6  | iobm/DoutOE.EXP  | nAoutOE
INPUTMC | 8 | 5 | 3 | 3 | 8 | 1 | 12 | 1 | 13 | 5 | 8 | 5 | 0 | 5 | 7 | 3 | 1
IMPORTS | 1 | 5 | 7
EQ | 9 | 
   !nLDS_IOB.D = iobm/IOS_FSM_FFd3 & IOL0
	# iobm/IOS_FSM_FFd4 & IOL0
	# iobm/IOS_FSM_FFd5 & IOL0
	# !nLDS_IOB & iobm/IOS_FSM_FFd6 & IOL0
;Imported pterms FB6_8
	# iobm/IOS_FSM_FFd7 & !iobm/C8Mr & IOL0 & 
	iobm/IORDREQr;
   !nLDS_IOB.CLK = C16M;	// GCK
   nLDS_IOB.OE = !nAoutOE;
GLOBALS | 1 | 2 | C16M

MACROCELL | 5 | 10 | nUDS_IOBout
ATTRIBUTES | 8816386 | 0
OUTPUTMC | 1 | 5 | 10
INPUTS | 8 | iobm/IOS_FSM_FFd3  | IOU0  | iobm/IOS_FSM_FFd5  | iobm/IOS_FSM_FFd4  | nUDS_IOB  | iobm/IOS_FSM_FFd6  | IODONE.EXP  | nAoutOE
INPUTMC | 8 | 5 | 3 | 3 | 3 | 1 | 12 | 1 | 13 | 5 | 10 | 5 | 0 | 5 | 9 | 3 | 1
IMPORTS | 1 | 5 | 9
EQ | 9 | 
   !nUDS_IOB.D = iobm/IOS_FSM_FFd3 & IOU0
	# iobm/IOS_FSM_FFd4 & IOU0
	# iobm/IOS_FSM_FFd5 & IOU0
	# !nUDS_IOB & iobm/IOS_FSM_FFd6 & IOU0
;Imported pterms FB6_10
	# iobm/IOS_FSM_FFd7 & !iobm/C8Mr & IOU0 & 
	iobm/IORDREQr;
   !nUDS_IOB.CLK = C16M;	// GCK
   nUDS_IOB.OE = !nAoutOE;
GLOBALS | 1 | 2 | C16M

MACROCELL | 7 | 17 | iobs/Sent
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 18 | 7 | 17 | 3 | 16 | 4 | 14 | 7 | 11 | 3 | 12 | 3 | 15 | 7 | 6 | 3 | 8 | 3 | 3 | 7 | 2 | 2 | 9 | 3 | 0 | 3 | 11 | 3 | 13 | 3 | 17 | 7 | 0 | 7 | 7 | 7 | 16
INPUTS | 12 | iobs/Sent  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | iobs/TS_FSM_FFd1  | iobs/TS_FSM_FFd2  | nADoutLE1  | A_FSB<22>  | A_FSB<20>  | A_FSB<21>  | EXP20_.EXP  | nRESout.EXP
INPUTMC | 7 | 7 | 17 | 2 | 17 | 7 | 9 | 3 | 15 | 5 | 13 | 7 | 0 | 7 | 16
INPUTP | 5 | 54 | 36 | 30 | 28 | 29
IMPORTS | 2 | 7 | 0 | 7 | 16
EQ | 32 | 
   iobs/Sent.T = iobs/Sent & nAS_FSB & !fsb/ASrf
	# A_FSB<23> & !iobs/Sent & !nAS_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<23> & !iobs/Sent & !iobs/TS_FSM_FFd1 & 
	!iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<22> & A_FSB<21> & !iobs/Sent & !nAS_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<22> & A_FSB<20> & !iobs/Sent & !nAS_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB8_1
	# A_FSB<22> & !iobs/Sent & !cs/nOverlay & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & !nAS_FSB & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & !nAS_FSB & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & fsb/ASrf & nADoutLE1
;Imported pterms FB8_17
	# A_FSB<22> & A_FSB<21> & !iobs/Sent & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<22> & A_FSB<20> & !iobs/Sent & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<22> & !iobs/Sent & !cs/nOverlay & !nAS_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1;
   iobs/Sent.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 15 | cnt/QS<0>
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 2 | 15 | 2 | 0 | 2 | 14
INPUTS | 24 | cnt/QS<0>  | cnt/Er<0>  | cnt/Er<1>  | cnt/TimerTC  | cnt/QS<1>  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<15>  | A_FSB<13>  | A_FSB<14>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | nWE_FSB  | nAS_FSB  | A_FSB<9>  | QoSReady.EXP  | nROMWE_OBUF.EXP
INPUTMC | 7 | 2 | 15 | 0 | 8 | 2 | 2 | 6 | 0 | 2 | 0 | 2 | 14 | 2 | 16
INPUTP | 17 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 21 | 18 | 19 | 17 | 15 | 13 | 47 | 54 | 12
IMPORTS | 2 | 2 | 14 | 2 | 16
EQ | 40 | 
   cnt/QS<0>.D = cnt/QS<0> & !cnt/TimerTC
	# cnt/QS<0> & cnt/Er<0>
	# cnt/QS<0> & !cnt/Er<1>
	# !cnt/QS<0> & cnt/QS<1> & cnt/TimerTC & !cnt/Er<0> & 
	cnt/Er<1>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<9>
;Imported pterms FB3_15
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<8>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<9>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<8>
;Imported pterms FB3_17
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & A_FSB<9> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & A_FSB<8> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & A_FSB<9> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & A_FSB<8> & fsb/ASrf;
   cnt/QS<0>.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 0 | cnt/QS<1>
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 2 | 15 | 2 | 0 | 2 | 14
INPUTS | 7 | cnt/QS<0>  | cnt/QS<1>  | cnt/Er<0>  | cnt/Er<1>  | cnt/TimerTC  | cnt/LTimer<0>.EXP  | fsb/ASrf.EXP
INPUTMC | 7 | 2 | 15 | 2 | 0 | 0 | 8 | 2 | 2 | 6 | 0 | 2 | 1 | 2 | 17
IMPORTS | 2 | 2 | 1 | 2 | 17
EQ | 41 | 
   !cnt/QS<1>.D = !cnt/QS<0> & !cnt/QS<1>
	# !cnt/QS<1> & !cnt/TimerTC
	# !cnt/QS<1> & cnt/Er<0>
	# !cnt/QS<1> & !cnt/Er<1>
	# cnt/QS<0> & cnt/QS<1> & cnt/TimerTC & !cnt/Er<0> & 
	cnt/Er<1>
;Imported pterms FB3_2
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & A_FSB<9> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & A_FSB<8> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & A_FSB<9> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & A_FSB<8> & fsb/ASrf
;Imported pterms FB3_18
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<9>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<8>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<9>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<8>;
   cnt/QS<1>.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 13 | cnt/Timer<0>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 6 | 0 | 13 | 6 | 15 | 6 | 17 | 6 | 16 | 6 | 14 | 6 | 0
INPUTS | 4 | cnt/Timer<0>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 4 | 0 | 13 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 4 | 
   !cnt/Timer<0>.T = !cnt/Timer<0> & cnt/TimerTC & !cnt/Er<0> & 
	cnt/Er<1>;
   cnt/Timer<0>.CLK = FCLK;	// GCK
   cnt/Timer<0>.CE = !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 15 | cnt/Timer<1>
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 6 | 6 | 15 | 6 | 17 | 0 | 15 | 6 | 16 | 6 | 14 | 6 | 0
INPUTS | 5 | cnt/Timer<0>  | cnt/Timer<1>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 5 | 0 | 13 | 6 | 15 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 5 | 
   !cnt/Timer<1>.D = cnt/Timer<0> & cnt/Timer<1>
	# !cnt/Timer<0> & !cnt/Timer<1>
	# cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
   cnt/Timer<1>.CLK = FCLK;	// GCK
   cnt/Timer<1>.CE = !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 17 | cnt/Timer<2>
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 5 | 6 | 17 | 0 | 15 | 6 | 16 | 6 | 14 | 6 | 0
INPUTS | 6 | cnt/Timer<0>  | cnt/Timer<2>  | cnt/Timer<1>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 6 | 0 | 13 | 6 | 17 | 6 | 15 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 6 | 
   !cnt/Timer<2>.D = !cnt/Timer<0> & !cnt/Timer<2>
	# !cnt/Timer<1> & !cnt/Timer<2>
	# cnt/Timer<0> & cnt/Timer<1> & cnt/Timer<2>
	# cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
   cnt/Timer<2>.CLK = FCLK;	// GCK
   cnt/Timer<2>.CE = !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 16 | IOBERR
ATTRIBUTES | 8553232 | 0
OUTPUTMC | 4 | 7 | 11 | 5 | 3 | 5 | 16 | 1 | 17
INPUTS | 2 | nBERR_IOB  | nAS_IOB
INPUTMC | 1 | 5 | 11
INPUTP | 1 | 123
EQ | 3 | 
   IOBERR.D = !nBERR_IOB;
   !IOBERR.CLK = C8M;	// GCK
   IOBERR.AR = nAS_IOB;
GLOBALS | 1 | 2 | C8M

MACROCELL | 5 | 9 | IODONE
ATTRIBUTES | 8553232 | 0
OUTPUTMC | 5 | 5 | 3 | 5 | 16 | 1 | 17 | 1 | 8 | 5 | 10
INPUTS | 12 | nRES.PIN  | nDTACK_IOB  | nVMA_IOB  | iobm/ES<0>  | iobm/ES<2>  | iobm/ES<1>  | iobm/ES<3>  | nAS_IOB  | iobm/IOS_FSM_FFd7  | iobm/C8Mr  | IOU0  | iobm/IORDREQr
INPUTMC | 10 | 5 | 1 | 5 | 4 | 0 | 17 | 5 | 6 | 5 | 5 | 5 | 11 | 5 | 2 | 1 | 16 | 3 | 3 | 1 | 15
INPUTP | 2 | 145 | 127
EXPORTS | 1 | 5 | 10
EQ | 8 | 
   IODONE.D = !nRES.PIN
	# !nDTACK_IOB
	# !nVMA_IOB & !iobm/ES<0> & !iobm/ES<2> & !iobm/ES<1> & 
	iobm/ES<3>;
   !IODONE.CLK = C8M;	// GCK
   IODONE.AR = nAS_IOB;
    IODONE.EXP  =  iobm/IOS_FSM_FFd7 & !iobm/C8Mr & IOU0 & 
	iobm/IORDREQr
GLOBALS | 1 | 2 | C8M

MACROCELL | 0 | 15 | RefUrg
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 13 | 0 | 9 | 4 | 0 | 4 | 9 | 7 | 3 | 4 | 12 | 4 | 17 | 4 | 4 | 4 | 3 | 4 | 5 | 4 | 8 | 4 | 11 | 4 | 16 | 7 | 4
INPUTS | 5 | cnt/Timer<1>  | cnt/Timer<2>  | cnt/Timer<3>  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 5 | 6 | 15 | 6 | 17 | 6 | 16 | 0 | 8 | 2 | 2
EQ | 3 | 
   RefUrg.D = !cnt/Timer<1> & !cnt/Timer<2> & cnt/Timer<3>;
   RefUrg.CLK = FCLK;	// GCK
   RefUrg.CE = !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 1 | cnt/LTimer<0>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 13 | 6 | 13 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 2 | 2 | 0
INPUTS | 21 | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<15>  | A_FSB<13>  | A_FSB<14>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | nWE_FSB  | A_FSB<9>  | fsb/ASrf  | A_FSB<8>
INPUTMC | 4 | 6 | 0 | 0 | 8 | 2 | 2 | 2 | 17
INPUTP | 17 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 21 | 18 | 19 | 17 | 15 | 13 | 47 | 12 | 11
EXPORTS | 1 | 2 | 0
EQ | 19 | 
   cnt/LTimer<0>.T = Vcc;
   cnt/LTimer<0>.CLK = FCLK;	// GCK
   cnt/LTimer<0>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
    cnt/LTimer<0>.EXP  =  !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & A_FSB<9> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & A_FSB<8> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & A_FSB<9> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & A_FSB<8> & fsb/ASrf
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 16 | cnt/Timer<3>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 4 | 0 | 15 | 6 | 16 | 6 | 14 | 6 | 0
INPUTS | 7 | cnt/Timer<0>  | cnt/Timer<1>  | cnt/Timer<2>  | cnt/Er<0>  | cnt/Er<1>  | cnt/Timer<3>  | cnt/TimerTC
INPUTMC | 7 | 0 | 13 | 6 | 15 | 6 | 17 | 0 | 8 | 2 | 2 | 6 | 16 | 6 | 0
EQ | 10 | 
   cnt/Timer<3>.T = cnt/Timer<0> & cnt/Timer<1> & cnt/Timer<2> & 
	!cnt/TimerTC
	# cnt/Timer<0> & cnt/Timer<1> & cnt/Timer<2> & 
	cnt/Er<0>
	# cnt/Timer<0> & cnt/Timer<1> & cnt/Timer<2> & 
	!cnt/Er<1>
	# cnt/Timer<3> & cnt/TimerTC & !cnt/Er<0> & 
	cnt/Er<1>;
   cnt/Timer<3>.CLK = FCLK;	// GCK
   cnt/Timer<3>.CE = !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 0 | cs/nOverlay
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 20 | 7 | 16 | 3 | 0 | 7 | 3 | 7 | 8 | 3 | 13 | 4 | 0 | 7 | 10 | 3 | 4 | 3 | 16 | 7 | 0 | 3 | 11 | 4 | 16 | 3 | 5 | 3 | 10 | 4 | 1 | 4 | 2 | 4 | 15 | 4 | 17 | 7 | 5 | 3 | 17
INPUTS | 18 | nRES.PIN  | cs/nOverlay  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<13>  | iobs/Sent  | nWE_FSB  | iobs/IORW1  | iobs/TS_FSM_FFd1  | nADoutLE1
INPUTMC | 6 | 3 | 0 | 2 | 17 | 7 | 17 | 3 | 16 | 7 | 9 | 5 | 13
INPUTP | 12 | 145 | 54 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 18 | 47
EXPORTS | 1 | 3 | 17
EQ | 10 | 
   cs/nOverlay.T = !nRES.PIN & cs/nOverlay & nAS_FSB & !fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & !A_FSB<21> & !A_FSB<20> & 
	!cs/nOverlay & !nAS_FSB
	# !A_FSB<23> & A_FSB<22> & !A_FSB<21> & !A_FSB<20> & 
	!cs/nOverlay & fsb/ASrf;
   cs/nOverlay.CLK = FCLK;	// GCK
    cs/nOverlay.EXP  =  !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & iobs/TS_FSM_FFd1 & 
	fsb/ASrf & nADoutLE1
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 14 | RefReq
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 7 | 0 | 9 | 4 | 3 | 4 | 8 | 4 | 1 | 4 | 11 | 4 | 15 | 7 | 4
INPUTS | 6 | cnt/Timer<0>  | cnt/Timer<1>  | cnt/Timer<2>  | cnt/Timer<3>  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 6 | 0 | 13 | 6 | 15 | 6 | 17 | 6 | 16 | 0 | 8 | 2 | 2
EQ | 4 | 
   !RefReq.D = !cnt/Timer<0> & cnt/Timer<1> & !cnt/Timer<2> & 
	cnt/Timer<3>;
   RefReq.CLK = FCLK;	// GCK
   RefReq.CE = !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 13 | cnt/LTimer<10>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 2 | 6 | 12 | 6 | 2
INPUTS | 13 | cnt/LTimer<0>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/LTimer<3>  | cnt/LTimer<4>  | cnt/LTimer<5>  | cnt/LTimer<6>  | cnt/LTimer<7>  | cnt/LTimer<8>  | cnt/LTimer<9>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 13 | 2 | 1 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 5 | 
   cnt/LTimer<10>.T = cnt/LTimer<0> & cnt/LTimer<1> & cnt/LTimer<2> & 
	cnt/LTimer<3> & cnt/LTimer<4> & cnt/LTimer<5> & cnt/LTimer<6> & 
	cnt/LTimer<7> & cnt/LTimer<8> & cnt/LTimer<9>;
   cnt/LTimer<10>.CLK = FCLK;	// GCK
   cnt/LTimer<10>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 9 | cnt/LTimer<1>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 12 | 6 | 13 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 2 | 2 | 8
INPUTS | 16 | cnt/LTimer<0>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<13>  | iobs/Sent  | nWE_FSB  | IONPReady  | nADoutLE1  | A_FSB<14>
INPUTMC | 7 | 2 | 1 | 6 | 0 | 0 | 8 | 2 | 2 | 7 | 17 | 4 | 15 | 5 | 13
INPUTP | 9 | 29 | 28 | 26 | 24 | 23 | 22 | 18 | 47 | 19
EXPORTS | 1 | 2 | 8
EQ | 9 | 
   cnt/LTimer<1>.T = cnt/LTimer<0>;
   cnt/LTimer<1>.CLK = FCLK;	// GCK
   cnt/LTimer<1>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
    cnt/LTimer<1>.EXP  =  A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<13> & !iobs/Sent & !nWE_FSB & 
	!IONPReady & !nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<14> & !iobs/Sent & !nWE_FSB & 
	!IONPReady & !nADoutLE1
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 7 | cnt/LTimer<2>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 11 | 6 | 13 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 2 | 2 | 8
INPUTS | 15 | cnt/LTimer<0>  | cnt/LTimer<1>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>  | A_FSB<22>  | IONPReady  | RAMReady  | A_FSB<23>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>
INPUTMC | 7 | 2 | 1 | 2 | 9 | 6 | 0 | 0 | 8 | 2 | 2 | 4 | 15 | 4 | 12
INPUTP | 8 | 30 | 36 | 29 | 28 | 26 | 24 | 23 | 22
EXPORTS | 1 | 2 | 8
EQ | 6 | 
   cnt/LTimer<2>.T = cnt/LTimer<0> & cnt/LTimer<1>;
   cnt/LTimer<2>.CLK = FCLK;	// GCK
   cnt/LTimer<2>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
    cnt/LTimer<2>.EXP  =  !A_FSB<22> & !IONPReady & !RAMReady
	# A_FSB<23> & A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16>
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 6 | cnt/LTimer<3>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 9 | 6 | 13 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 2
INPUTS | 6 | cnt/LTimer<0>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 6 | 2 | 1 | 2 | 9 | 2 | 7 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 3 | 
   cnt/LTimer<3>.T = cnt/LTimer<0> & cnt/LTimer<1> & cnt/LTimer<2>;
   cnt/LTimer<3>.CLK = FCLK;	// GCK
   cnt/LTimer<3>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 5 | cnt/LTimer<4>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 8 | 6 | 13 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 2
INPUTS | 7 | cnt/LTimer<0>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/LTimer<3>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 7 | 2 | 1 | 2 | 9 | 2 | 7 | 2 | 6 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 4 | 
   cnt/LTimer<4>.T = cnt/LTimer<0> & cnt/LTimer<1> & cnt/LTimer<2> & 
	cnt/LTimer<3>;
   cnt/LTimer<4>.CLK = FCLK;	// GCK
   cnt/LTimer<4>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 4 | cnt/LTimer<5>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 7 | 6 | 13 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 2
INPUTS | 8 | cnt/LTimer<0>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/LTimer<3>  | cnt/LTimer<4>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 8 | 2 | 1 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 4 | 
   cnt/LTimer<5>.T = cnt/LTimer<0> & cnt/LTimer<1> & cnt/LTimer<2> & 
	cnt/LTimer<3> & cnt/LTimer<4>;
   cnt/LTimer<5>.CLK = FCLK;	// GCK
   cnt/LTimer<5>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 3 | cnt/LTimer<6>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 6 | 6 | 13 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 2
INPUTS | 9 | cnt/LTimer<0>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/LTimer<3>  | cnt/LTimer<4>  | cnt/LTimer<5>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 9 | 2 | 1 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 4 | 
   cnt/LTimer<6>.T = cnt/LTimer<0> & cnt/LTimer<1> & cnt/LTimer<2> & 
	cnt/LTimer<3> & cnt/LTimer<4> & cnt/LTimer<5>;
   cnt/LTimer<6>.CLK = FCLK;	// GCK
   cnt/LTimer<6>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 9 | cnt/LTimer<7>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 5 | 6 | 13 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 2
INPUTS | 10 | cnt/LTimer<0>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/LTimer<3>  | cnt/LTimer<4>  | cnt/LTimer<5>  | cnt/LTimer<6>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 10 | 2 | 1 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 4 | 
   cnt/LTimer<7>.T = cnt/LTimer<0> & cnt/LTimer<1> & cnt/LTimer<2> & 
	cnt/LTimer<3> & cnt/LTimer<4> & cnt/LTimer<5> & cnt/LTimer<6>;
   cnt/LTimer<7>.CLK = FCLK;	// GCK
   cnt/LTimer<7>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 6 | cnt/LTimer<8>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 4 | 6 | 13 | 6 | 3 | 6 | 12 | 6 | 2
INPUTS | 11 | cnt/LTimer<0>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/LTimer<3>  | cnt/LTimer<4>  | cnt/LTimer<5>  | cnt/LTimer<6>  | cnt/LTimer<7>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 11 | 2 | 1 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 5 | 
   cnt/LTimer<8>.T = cnt/LTimer<0> & cnt/LTimer<1> & cnt/LTimer<2> & 
	cnt/LTimer<3> & cnt/LTimer<4> & cnt/LTimer<5> & cnt/LTimer<6> & 
	cnt/LTimer<7>;
   cnt/LTimer<8>.CLK = FCLK;	// GCK
   cnt/LTimer<8>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 3 | cnt/LTimer<9>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 3 | 6 | 13 | 6 | 12 | 6 | 2
INPUTS | 12 | cnt/LTimer<0>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/LTimer<3>  | cnt/LTimer<4>  | cnt/LTimer<5>  | cnt/LTimer<6>  | cnt/LTimer<7>  | cnt/LTimer<8>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 12 | 2 | 1 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 5 | 
   cnt/LTimer<9>.T = cnt/LTimer<0> & cnt/LTimer<1> & cnt/LTimer<2> & 
	cnt/LTimer<3> & cnt/LTimer<4> & cnt/LTimer<5> & cnt/LTimer<6> & 
	cnt/LTimer<7> & cnt/LTimer<8>;
   cnt/LTimer<9>.CLK = FCLK;	// GCK
   cnt/LTimer<9>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 14 | QoSReady
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 5 | 2 | 14 | 3 | 10 | 2 | 8 | 2 | 13 | 2 | 15
INPUTS | 22 | cnt/QS<0>  | cnt/QS<1>  | QoSReady  | nAS_FSB  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<15>  | A_FSB<13>  | A_FSB<14>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | nWE_FSB  | A_FSB<8>  | A_FSB<9>  | cnt/Wait<1>.EXP
INPUTMC | 4 | 2 | 15 | 2 | 0 | 2 | 14 | 2 | 13
INPUTP | 18 | 54 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 21 | 18 | 19 | 17 | 15 | 13 | 47 | 11 | 12
EXPORTS | 1 | 2 | 15
IMPORTS | 1 | 2 | 13
EQ | 19 | 
   QoSReady.D = !cnt/QS<0> & !cnt/QS<1>
	# QoSReady & !nAS_FSB
;Imported pterms FB3_14
	# QoSReady & fsb/ASrf
	# !cnt/Wait<0> & !cnt/Wait<1> & !cnt/Wait<2> & 
	!cnt/Wait<3> & cnt/Wait<4>;
   QoSReady.CLK = FCLK;	// GCK
    QoSReady.EXP  =  !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<8>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<9>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<8>
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 12 | cnt/LTimer<11>
ATTRIBUTES | 4358976 | 0
OUTPUTMC | 1 | 6 | 2
INPUTS | 14 | cnt/LTimer<0>  | cnt/LTimer<10>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/LTimer<3>  | cnt/LTimer<4>  | cnt/LTimer<5>  | cnt/LTimer<6>  | cnt/LTimer<7>  | cnt/LTimer<8>  | cnt/LTimer<9>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 14 | 2 | 1 | 6 | 13 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 5 | 
   cnt/LTimer<11>.T = cnt/LTimer<0> & cnt/LTimer<10> & cnt/LTimer<1> & 
	cnt/LTimer<2> & cnt/LTimer<3> & cnt/LTimer<4> & cnt/LTimer<5> & 
	cnt/LTimer<6> & cnt/LTimer<7> & cnt/LTimer<8> & cnt/LTimer<9>;
   cnt/LTimer<11>.CLK = FCLK;	// GCK
   cnt/LTimer<11>.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 0 | cnt/TimerTC
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 21 | 2 | 15 | 2 | 0 | 0 | 13 | 6 | 15 | 6 | 17 | 2 | 1 | 6 | 16 | 6 | 13 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 2 | 0 | 7 | 0 | 14
INPUTS | 6 | cnt/Timer<0>  | cnt/Timer<1>  | cnt/Timer<2>  | cnt/Timer<3>  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 6 | 0 | 13 | 6 | 15 | 6 | 17 | 6 | 16 | 0 | 8 | 2 | 2
EQ | 4 | 
   cnt/TimerTC.D = cnt/Timer<0> & !cnt/Timer<1> & !cnt/Timer<2> & 
	cnt/Timer<3>;
   cnt/TimerTC.CLK = FCLK;	// GCK
   cnt/TimerTC.CE = !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 16 | iobs/IORW1
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 6 | 3 | 16 | 7 | 1 | 3 | 12 | 3 | 0 | 3 | 17 | 3 | 15
INPUTS | 18 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<14>  | iobs/Sent  | nWE_FSB  | iobs/IORW1  | nAS_FSB  | iobs/TS_FSM_FFd2  | nADoutLE1  | A_FSB<13>  | cs/nOverlay  | EXP15_.EXP
INPUTMC | 6 | 7 | 17 | 3 | 16 | 3 | 15 | 5 | 13 | 3 | 0 | 3 | 17
INPUTP | 12 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 19 | 47 | 54 | 18
EXPORTS | 1 | 3 | 15
IMPORTS | 1 | 3 | 17
EQ | 41 | 
   iobs/IORW1.T = !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & !nAS_FSB & 
	iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & !nAS_FSB & 
	iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_18
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & !nAS_FSB & 
	iobs/TS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & iobs/TS_FSM_FFd2 & 
	fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & !nAS_FSB & 
	iobs/TS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & iobs/TS_FSM_FFd1 & 
	fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & iobs/TS_FSM_FFd2 & 
	fsb/ASrf & nADoutLE1
;Imported pterms FB4_1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & iobs/TS_FSM_FFd1 & 
	fsb/ASrf & nADoutLE1;
   iobs/IORW1.CLK = FCLK;	// GCK
    iobs/IORW1.EXP  =  !A_FSB<23> & !A_FSB<22> & !A_FSB<19> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<13> & !A_FSB<14> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<21> & !A_FSB<20> & cs/nOverlay & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 9 | ram/RefDone
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 13 | 0 | 9 | 4 | 0 | 4 | 9 | 7 | 3 | 4 | 12 | 4 | 17 | 4 | 3 | 4 | 1 | 4 | 8 | 4 | 11 | 4 | 15 | 4 | 16 | 7 | 4
INPUTS | 7 | ram/RefDone  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd7  | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | RefUrg  | RefReq
INPUTMC | 7 | 0 | 9 | 0 | 3 | 7 | 3 | 0 | 2 | 0 | 1 | 0 | 15 | 6 | 14
EQ | 4 | 
   !ram/RefDone.D = !RefUrg & !RefReq
	# !ram/RefDone & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd7 & 
	!ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3;
   ram/RefDone.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 4 | 15 | IONPReady
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 6 | 4 | 14 | 3 | 10 | 2 | 8 | 2 | 7 | 2 | 9 | 4 | 16
INPUTS | 11 | A_FSB<23>  | RefReq  | ram/RefDone  | nAS_FSB  | ram/RS_FSM_FFd8  | BACTr  | fsb/ASrf  | A_FSB<22>  | cs/nOverlay  | ram/RASEN  | RA_6_OBUF.EXP
INPUTMC | 8 | 6 | 14 | 0 | 9 | 4 | 0 | 7 | 13 | 2 | 17 | 3 | 0 | 4 | 9 | 4 | 14
INPUTP | 3 | 36 | 54 | 30
EXPORTS | 1 | 4 | 16
IMPORTS | 1 | 4 | 14
EQ | 21 | 
   !IONPReady.D = ;Imported pterms FB5_15
	  !iobs/Sent & !IONPReady
	# !IONPReady & !iobs/IODONEr
	# nAS_FSB & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!nWE_FSB & !IONPReady
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!nWE_FSB & !IONPReady;
   IONPReady.CLK = FCLK;	// GCK
    IONPReady.EXP  =  A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & 
	ram/RS_FSM_FFd8 & ram/RASEN & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 2 | cnt/LTimerTC
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 2 | 0 | 7 | 0 | 14
INPUTS | 15 | cnt/LTimer<0>  | cnt/LTimer<10>  | cnt/LTimer<1>  | cnt/LTimer<2>  | cnt/LTimer<3>  | cnt/LTimer<4>  | cnt/LTimer<5>  | cnt/LTimer<6>  | cnt/LTimer<7>  | cnt/LTimer<8>  | cnt/LTimer<9>  | cnt/LTimer<11>  | cnt/TimerTC  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 15 | 2 | 1 | 6 | 13 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 0 | 0 | 8 | 2 | 2
EQ | 6 | 
   cnt/LTimerTC.D = !cnt/LTimer<0> & cnt/LTimer<10> & cnt/LTimer<1> & 
	cnt/LTimer<2> & cnt/LTimer<3> & cnt/LTimer<4> & cnt/LTimer<5> & 
	cnt/LTimer<6> & cnt/LTimer<7> & cnt/LTimer<8> & cnt/LTimer<9> & 
	cnt/LTimer<11>;
   cnt/LTimerTC.CLK = FCLK;	// GCK
   cnt/LTimerTC.CE = cnt/TimerTC & !cnt/Er<0> & cnt/Er<1>;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 12 | iobs/IOL1
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 2 | 3 | 8 | 3 | 7
INPUTS | 2 | nLDS_FSB  | iobs/Load1
INPUTMC | 1 | 7 | 6
INPUTP | 1 | 49
EQ | 3 | 
   iobs/IOL1.D = !nLDS_FSB;
   iobs/IOL1.CLK = FCLK;	// GCK
   iobs/IOL1.CE = iobs/Load1;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 11 | iobs/IOU1
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 2 | 3 | 3 | 3 | 2
INPUTS | 2 | nUDS_FSB  | iobs/Load1
INPUTMC | 1 | 7 | 6
INPUTP | 1 | 56
EQ | 3 | 
   iobs/IOU1.D = !nUDS_FSB;
   iobs/IOU1.CLK = FCLK;	// GCK
   iobs/IOU1.CE = iobs/Load1;
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 11 | nBERR_FSB_OBUF
ATTRIBUTES | 8815362 | 0
OUTPUTMC | 1 | 7 | 11
INPUTS | 5 | nAS_FSB  | fsb/ASrf  | iobs/Sent  | nBERR_FSB  | IOBERR
INPUTMC | 4 | 2 | 17 | 7 | 17 | 7 | 11 | 0 | 16
INPUTP | 1 | 54
EQ | 4 | 
   nBERR_FSB.D = !iobs/Sent & nBERR_FSB
	# !IOBERR & nBERR_FSB
	# nAS_FSB & !fsb/ASrf;
   nBERR_FSB.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 10 | nVPA_FSB_OBUF
ATTRIBUTES | 8684418 | 0
OUTPUTMC | 1 | 3 | 9
INPUTS | 17 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | QoSReady  | IONPReady  | nAS_FSB  | fsb/ASrf  | A_FSB<13>  | A_FSB<14>  | iobs/TS_FSM_FFd2  | nADoutLE1  | cs/nOverlay
INPUTMC | 6 | 2 | 14 | 4 | 15 | 2 | 17 | 3 | 15 | 5 | 13 | 3 | 0
INPUTP | 11 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 54 | 18 | 19
EXPORTS | 1 | 3 | 9
EQ | 12 | 
   !nVPA_FSB.D = A_FSB<23> & A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & QoSReady & 
	IONPReady & !nAS_FSB
	# A_FSB<23> & A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & QoSReady & 
	IONPReady & fsb/ASrf;
   nVPA_FSB.CLK = FCLK;	// GCK
   nVPA_FSB.AP = nAS_FSB;
    nVPA_FSB_OBUF.EXP  =  !A_FSB<23> & !A_FSB<22> & !A_FSB<13> & !A_FSB<14> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<21> & !A_FSB<20> & cs/nOverlay & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 4 | nRAS_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 7 | 3
INPUTS | 10 | RefUrg  | ram/RefDone  | nAS_FSB  | ram/RS_FSM_FFd8  | fsb/ASrf  | A_FSB<23>  | RefReq  | BACTr  | A_FSB<22>  | nRAMLWE_OBUF.EXP
INPUTMC | 7 | 0 | 15 | 0 | 9 | 4 | 0 | 2 | 17 | 6 | 14 | 7 | 13 | 7 | 5
INPUTP | 3 | 54 | 36 | 30
EXPORTS | 1 | 7 | 3
IMPORTS | 1 | 7 | 5
EQ | 15 | 
   !nRAS = ;Imported pterms FB8_6
	  ram/RASrf
	# ram/RASrr
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & !nAS_FSB & 
	ram/RASEN;
    nRAS_OBUF.EXP  =  RefUrg & !ram/RefDone & nAS_FSB & 
	ram/RS_FSM_FFd8 & !fsb/ASrf
	# A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf

MACROCELL | 7 | 14 | nBR_IOB_OBUF
ATTRIBUTES | 4621058 | 0
OUTPUTMC | 2 | 7 | 14 | 3 | 1
INPUTS | 4 | nBR_IOB  | cnt/IS_FSM_FFd1  | cnt/IS_FSM_FFd2  | cnt/nIPL2r
INPUTMC | 4 | 7 | 14 | 0 | 7 | 0 | 14 | 0 | 6
EQ | 4 | 
   nBR_IOB.T = nBR_IOB & !cnt/IS_FSM_FFd1 & !cnt/IS_FSM_FFd2
	# !nBR_IOB & !cnt/IS_FSM_FFd1 & cnt/IS_FSM_FFd2 & 
	!cnt/nIPL2r;
   nBR_IOB.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 4 | 10 | RA_11_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 11
INPUTS | 5 | A_FSB<19>  | ram/RASEL  | A_FSB<20>  | A_FSB<12>  | A_FSB<4>
INPUTMC | 1 | 7 | 8
INPUTP | 4 | 26 | 28 | 17 | 157
EXPORTS | 1 | 4 | 11
EQ | 4 | 
   RA<3> = A_FSB<20> & ram/RASEL
	# A_FSB<19> & !ram/RASEL;
    RA_11_OBUF.EXP  =  A_FSB<12> & !ram/RASEL
	# ram/RASEL & A_FSB<4>

MACROCELL | 2 | 8 | nDTACK_FSB_OBUF
ATTRIBUTES | 8815362 | 0
OUTPUTMC | 1 | 1 | 7
INPUTS | 10 | QoSReady  | A_FSB<23>  | IONPReady  | nAS_FSB  | fsb/ASrf  | A_FSB<22>  | A_FSB<20>  | A_FSB<21>  | cnt/LTimer<2>.EXP  | cnt/LTimer<1>.EXP
INPUTMC | 5 | 2 | 14 | 4 | 15 | 2 | 17 | 2 | 7 | 2 | 9
INPUTP | 5 | 36 | 54 | 30 | 28 | 29
IMPORTS | 2 | 2 | 7 | 2 | 9
EQ | 17 | 
   nDTACK_FSB.D = !QoSReady
	# A_FSB<23> & !IONPReady
	# nAS_FSB & !fsb/ASrf
	# A_FSB<22> & A_FSB<21> & !IONPReady
	# A_FSB<22> & A_FSB<20> & !IONPReady
;Imported pterms FB3_8
	# !A_FSB<22> & !IONPReady & !RAMReady
	# A_FSB<23> & A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16>
;Imported pterms FB3_10
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<13> & !iobs/Sent & !nWE_FSB & 
	!IONPReady & !nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<14> & !iobs/Sent & !nWE_FSB & 
	!IONPReady & !nADoutLE1;
   nDTACK_FSB.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 8 | ram/RASEL
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 12 | 4 | 10 | 6 | 5 | 6 | 8 | 6 | 1 | 4 | 13 | 4 | 7 | 7 | 7 | 7 | 5 | 6 | 4 | 6 | 7 | 6 | 10 | 7 | 1
INPUTS | 8 | ram/RS_FSM_FFd6  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay  | nAS_FSB  | ram/RS_FSM_FFd8  | ram/RASEN  | fsb/ASrf
INPUTMC | 5 | 7 | 10 | 3 | 0 | 4 | 0 | 4 | 9 | 2 | 17
INPUTP | 3 | 36 | 30 | 54
EQ | 6 | 
   ram/RASEL.D = ram/RS_FSM_FFd6
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & !nAS_FSB & 
	ram/RS_FSM_FFd8 & ram/RASEN
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & 
	ram/RS_FSM_FFd8 & ram/RASEN & fsb/ASrf;
   ram/RASEL.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 9 | iobs/TS_FSM_FFd1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 16 | 7 | 17 | 3 | 13 | 7 | 9 | 3 | 15 | 7 | 6 | 3 | 8 | 3 | 3 | 7 | 2 | 3 | 12 | 7 | 15 | 3 | 0 | 3 | 11 | 3 | 17 | 7 | 0 | 7 | 7 | 7 | 16
INPUTS | 3 | iobs/TS_FSM_FFd2  | iobs/TS_FSM_FFd1  | iobs/IOACTr
INPUTMC | 3 | 3 | 15 | 7 | 9 | 1 | 9
EQ | 3 | 
   iobs/TS_FSM_FFd1.D = iobs/TS_FSM_FFd2
	# iobs/TS_FSM_FFd1 & iobs/IOACTr;
   iobs/TS_FSM_FFd1.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 15 | iobs/TS_FSM_FFd2
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 25 | 7 | 17 | 3 | 16 | 7 | 9 | 3 | 15 | 7 | 6 | 3 | 8 | 3 | 3 | 7 | 2 | 3 | 12 | 7 | 12 | 7 | 15 | 3 | 1 | 3 | 2 | 3 | 4 | 3 | 7 | 3 | 9 | 3 | 10 | 3 | 11 | 3 | 13 | 3 | 14 | 3 | 17 | 7 | 0 | 7 | 1 | 7 | 3 | 7 | 16
INPUTS | 12 | iobs/TS_FSM_FFd1  | iobs/TS_FSM_FFd2  | iobs/IOACTr  | iobs/Sent  | nADoutLE1  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | nWE_FSB  | EXP14_.EXP  | iobs/IORW1.EXP
INPUTMC | 8 | 7 | 9 | 3 | 15 | 1 | 9 | 7 | 17 | 5 | 13 | 2 | 17 | 3 | 14 | 3 | 16
INPUTP | 4 | 54 | 36 | 30 | 47
IMPORTS | 2 | 3 | 14 | 3 | 16
EQ | 26 | 
   !iobs/TS_FSM_FFd2.D = iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2
	# iobs/TS_FSM_FFd1 & iobs/IOACTr
	# iobs/Sent & !iobs/TS_FSM_FFd2 & nADoutLE1
	# nAS_FSB & !iobs/TS_FSM_FFd2 & !fsb/ASrf & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & nWE_FSB & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_15
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<20> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<18> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<17> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<16> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_17
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<19> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<13> & !A_FSB<14> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<21> & !A_FSB<20> & cs/nOverlay & 
	!iobs/TS_FSM_FFd2 & nADoutLE1;
   iobs/TS_FSM_FFd2.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 5 | 2 | iobm/IOS_FSM_FFd7
ATTRIBUTES | 8553220 | 0
OUTPUTMC | 9 | 5 | 11 | 5 | 12 | 5 | 9 | 5 | 2 | 5 | 0 | 5 | 17 | 5 | 15 | 5 | 7 | 5 | 16
INPUTS | 6 | iobm/IOS_FSM_FFd7  | iobm/IOS_FSM_FFd1  | iobm/C8Mr  | iobm/IORDREQr  | nAoutOE  | iobm/IOWRREQr
INPUTMC | 6 | 5 | 2 | 1 | 14 | 1 | 16 | 1 | 15 | 3 | 1 | 1 | 11
EQ | 6 | 
   !iobm/IOS_FSM_FFd7.D = !iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd1
	# !iobm/C8Mr & !iobm/IOS_FSM_FFd1 & iobm/IORDREQr & 
	!nAoutOE
	# !iobm/C8Mr & !iobm/IOS_FSM_FFd1 & iobm/IOWRREQr & 
	!nAoutOE;
   iobm/IOS_FSM_FFd7.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 5 | 3 | iobm/IOS_FSM_FFd3
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 10 | 5 | 11 | 5 | 8 | 5 | 10 | 5 | 3 | 5 | 17 | 1 | 17 | 5 | 15 | 5 | 7 | 5 | 12 | 5 | 16
INPUTS | 5 | iobm/IOS_FSM_FFd4  | iobm/IOS_FSM_FFd3  | iobm/C8Mr  | IOBERR  | IODONE
INPUTMC | 5 | 1 | 13 | 5 | 3 | 1 | 16 | 0 | 16 | 5 | 9
EQ | 4 | 
   iobm/IOS_FSM_FFd3.D = iobm/IOS_FSM_FFd4
	# iobm/IOS_FSM_FFd3 & iobm/C8Mr
	# !IOBERR & !IODONE & iobm/IOS_FSM_FFd3;
   iobm/IOS_FSM_FFd3.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 1 | 16 | iobm/C8Mr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 9 | 5 | 11 | 5 | 12 | 5 | 9 | 5 | 2 | 5 | 3 | 5 | 0 | 5 | 17 | 1 | 17 | 5 | 7
INPUTS | 1 | C8M
INPUTP | 1 | 35
EQ | 2 | 
   iobm/C8Mr.D = C8M;
   iobm/C8Mr.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 5 | 4 | iobm/ES<0>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 6 | 5 | 1 | 5 | 9 | 5 | 4 | 0 | 17 | 5 | 6 | 5 | 5
INPUTS | 6 | iobm/ES<0>  | E  | iobm/Er  | iobm/ES<2>  | iobm/ES<1>  | iobm/ES<3>
INPUTMC | 5 | 5 | 4 | 0 | 5 | 0 | 17 | 5 | 6 | 5 | 5
INPUTP | 1 | 37
EQ | 6 | 
   !iobm/ES<0>.T = iobm/ES<0> & !E & iobm/Er
	# !iobm/ES<0> & !iobm/ES<2> & !iobm/ES<1> & 
	!iobm/ES<3> & E
	# !iobm/ES<0> & !iobm/ES<2> & !iobm/ES<1> & 
	!iobm/ES<3> & !iobm/Er;
   !iobm/ES<0>.CLK = C8M;	// GCK
GLOBALS | 1 | 2 | C8M

MACROCELL | 1 | 13 | iobm/IOS_FSM_FFd4
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 9 | 5 | 11 | 5 | 8 | 5 | 10 | 5 | 3 | 5 | 17 | 5 | 15 | 5 | 7 | 5 | 12 | 5 | 16
INPUTS | 1 | iobm/IOS_FSM_FFd5
INPUTMC | 1 | 1 | 12
EQ | 2 | 
   iobm/IOS_FSM_FFd4.D = iobm/IOS_FSM_FFd5;
   iobm/IOS_FSM_FFd4.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 0 | 17 | iobm/ES<2>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 6 | 5 | 1 | 5 | 9 | 5 | 4 | 0 | 17 | 5 | 6 | 5 | 5
INPUTS | 5 | iobm/ES<0>  | iobm/ES<1>  | iobm/Er  | E  | iobm/ES<2>
INPUTMC | 4 | 5 | 4 | 5 | 6 | 0 | 5 | 0 | 17
INPUTP | 1 | 37
EQ | 4 | 
   iobm/ES<2>.T = iobm/ES<0> & iobm/ES<1> & E
	# iobm/ES<0> & iobm/ES<1> & !iobm/Er
	# iobm/ES<2> & !E & iobm/Er;
   !iobm/ES<2>.CLK = C8M;	// GCK
GLOBALS | 1 | 2 | C8M

MACROCELL | 1 | 12 | iobm/IOS_FSM_FFd5
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 8 | 5 | 11 | 5 | 8 | 5 | 10 | 1 | 13 | 5 | 17 | 5 | 15 | 5 | 7 | 5 | 12
INPUTS | 1 | iobm/IOS_FSM_FFd6
INPUTMC | 1 | 5 | 0
EQ | 2 | 
   iobm/IOS_FSM_FFd5.D = iobm/IOS_FSM_FFd6;
   iobm/IOS_FSM_FFd5.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 5 | 0 | iobm/IOS_FSM_FFd6
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 8 | 5 | 11 | 5 | 8 | 5 | 10 | 1 | 12 | 5 | 17 | 5 | 15 | 5 | 7 | 5 | 12
INPUTS | 5 | iobm/IOS_FSM_FFd7  | iobm/C8Mr  | iobm/IORDREQr  | nAoutOE  | iobm/IOWRREQr
INPUTMC | 5 | 5 | 2 | 1 | 16 | 1 | 15 | 3 | 1 | 1 | 11
EQ | 5 | 
   iobm/IOS_FSM_FFd6.D = iobm/IOS_FSM_FFd7 & !iobm/C8Mr & iobm/IORDREQr & 
	!nAoutOE
	# iobm/IOS_FSM_FFd7 & !iobm/C8Mr & iobm/IOWRREQr & 
	!nAoutOE;
   iobm/IOS_FSM_FFd6.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 4 | 0 | ram/RS_FSM_FFd8
ATTRIBUTES | 8553220 | 0
OUTPUTMC | 12 | 7 | 8 | 4 | 0 | 4 | 9 | 7 | 10 | 7 | 3 | 4 | 12 | 4 | 16 | 4 | 3 | 4 | 5 | 4 | 15 | 4 | 17 | 7 | 4
INPUTS | 11 | RefUrg  | cs/nOverlay  | ram/RefDone  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd8  | ram/RS_FSM_FFd4  | A_FSB<22>  | A_FSB<23>  | ram/RASEN  | nROMCS_OBUF.EXP  | ram/RASrr.EXP
INPUTMC | 9 | 0 | 15 | 3 | 0 | 0 | 9 | 0 | 3 | 4 | 0 | 0 | 0 | 4 | 9 | 4 | 1 | 4 | 17
INPUTP | 2 | 30 | 36
IMPORTS | 2 | 4 | 1 | 4 | 17
EQ | 29 | 
   !ram/RS_FSM_FFd8.D = !ram/RS_FSM_FFd8 & !ram/RS_FSM_FFd4 & 
	!ram/RS_FSM_FFd1
	# A_FSB<23> & RefUrg & !ram/RefDone & 
	!ram/RS_FSM_FFd1
	# A_FSB<22> & RefUrg & !ram/RefDone & 
	!ram/RS_FSM_FFd1
	# RefUrg & cs/nOverlay & !ram/RefDone & 
	!ram/RS_FSM_FFd1
	# RefUrg & !ram/RefDone & !ram/RASEN & 
	!ram/RS_FSM_FFd1
;Imported pterms FB5_2
	# A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & 
	!ram/RS_FSM_FFd4 & ram/RASEN & !ram/RS_FSM_FFd1 & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr & fsb/ASrf
;Imported pterms FB5_18
	# RefUrg & !ram/RefDone & !ram/RS_FSM_FFd8 & 
	!ram/RS_FSM_FFd1
	# RefUrg & !ram/RefDone & nAS_FSB & 
	!ram/RS_FSM_FFd1 & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & ram/RASEN & !ram/RS_FSM_FFd1;
   ram/RS_FSM_FFd8.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 5 | 6 | iobm/ES<1>
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 6 | 5 | 1 | 5 | 9 | 5 | 4 | 0 | 17 | 5 | 6 | 5 | 5
INPUTS | 6 | iobm/ES<0>  | iobm/ES<1>  | E  | iobm/Er  | iobm/ES<2>  | iobm/ES<3>
INPUTMC | 5 | 5 | 4 | 5 | 6 | 0 | 5 | 0 | 17 | 5 | 5
INPUTP | 1 | 37
EQ | 5 | 
   !iobm/ES<1>.D = iobm/ES<0> & iobm/ES<1>
	# !iobm/ES<0> & !iobm/ES<1>
	# !E & iobm/Er
	# iobm/ES<0> & !iobm/ES<2> & iobm/ES<3>;
   !iobm/ES<1>.CLK = C8M;	// GCK
GLOBALS | 1 | 2 | C8M

MACROCELL | 5 | 5 | iobm/ES<3>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 5 | 5 | 1 | 5 | 9 | 5 | 4 | 5 | 6 | 5 | 5
INPUTS | 6 | iobm/ES<3>  | E  | iobm/Er  | iobm/ES<0>  | iobm/ES<2>  | iobm/ES<1>
INPUTMC | 5 | 5 | 5 | 0 | 5 | 5 | 4 | 0 | 17 | 5 | 6
INPUTP | 1 | 37
EQ | 6 | 
   iobm/ES<3>.T = iobm/ES<3> & !E & iobm/Er
	# iobm/ES<0> & iobm/ES<2> & iobm/ES<1> & E
	# iobm/ES<0> & iobm/ES<2> & iobm/ES<1> & !iobm/Er
	# iobm/ES<0> & !iobm/ES<2> & !iobm/ES<1> & 
	iobm/ES<3>;
   !iobm/ES<3>.CLK = C8M;	// GCK
GLOBALS | 1 | 2 | C8M

MACROCELL | 0 | 7 | cnt/IS_FSM_FFd1
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 5 | 7 | 14 | 0 | 7 | 0 | 14 | 7 | 16 | 3 | 1
INPUTS | 7 | cnt/TimerTC  | cnt/LTimerTC  | cnt/IS_FSM_FFd1  | cnt/IS_FSM_FFd2  | cnt/Er<0>  | cnt/nIPL2r  | cnt/Er<1>
INPUTMC | 7 | 6 | 0 | 6 | 2 | 0 | 7 | 0 | 14 | 0 | 8 | 0 | 6 | 2 | 2
EQ | 3 | 
   cnt/IS_FSM_FFd1.T = cnt/TimerTC & cnt/LTimerTC & !cnt/IS_FSM_FFd1 & 
	cnt/IS_FSM_FFd2 & !cnt/Er<0> & cnt/nIPL2r & cnt/Er<1>;
   cnt/IS_FSM_FFd1.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 14 | cnt/IS_FSM_FFd2
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 5 | 7 | 14 | 0 | 7 | 0 | 14 | 7 | 16 | 3 | 1
INPUTS | 6 | cnt/TimerTC  | cnt/LTimerTC  | cnt/IS_FSM_FFd1  | cnt/IS_FSM_FFd2  | cnt/Er<0>  | cnt/Er<1>
INPUTMC | 6 | 6 | 0 | 6 | 2 | 0 | 7 | 0 | 14 | 0 | 8 | 2 | 2
EQ | 5 | 
   cnt/IS_FSM_FFd2.T = cnt/TimerTC & cnt/LTimerTC & cnt/IS_FSM_FFd1 & 
	cnt/IS_FSM_FFd2 & !cnt/Er<0> & cnt/Er<1>
	# cnt/TimerTC & cnt/LTimerTC & !cnt/IS_FSM_FFd1 & 
	!cnt/IS_FSM_FFd2 & !cnt/Er<0> & cnt/Er<1>;
   cnt/IS_FSM_FFd2.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 0 | ram/RS_FSM_FFd4
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 9 | 4 | 0 | 4 | 9 | 7 | 3 | 4 | 12 | 4 | 17 | 4 | 3 | 4 | 1 | 4 | 8 | 4 | 11
INPUTS | 2 | ram/DTACKr  | ram/RS_FSM_FFd5
INPUTMC | 2 | 1 | 7 | 0 | 10
EQ | 2 | 
   ram/RS_FSM_FFd4.D = ram/DTACKr & ram/RS_FSM_FFd5;
   ram/RS_FSM_FFd4.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 4 | 9 | ram/RASEN
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 12 | 4 | 17 | 7 | 8 | 4 | 0 | 4 | 9 | 7 | 10 | 7 | 3 | 4 | 12 | 4 | 16 | 4 | 1 | 4 | 5 | 4 | 15 | 7 | 5
INPUTS | 9 | ram/RS_FSM_FFd8  | ram/RS_FSM_FFd4  | ram/RS_FSM_FFd1  | A_FSB<22>  | RefUrg  | ram/RefDone  | A_FSB<23>  | ram/RASEN  | RA_4_OBUF.EXP
INPUTMC | 7 | 4 | 0 | 0 | 0 | 0 | 3 | 0 | 15 | 0 | 9 | 4 | 9 | 4 | 8
INPUTP | 2 | 30 | 36
IMPORTS | 1 | 4 | 8
EQ | 22 | 
   !ram/RASEN.D = !ram/RS_FSM_FFd8 & !ram/RS_FSM_FFd4 & 
	!ram/RS_FSM_FFd1
	# A_FSB<23> & RefUrg & !ram/RefDone & 
	!ram/RS_FSM_FFd1
	# A_FSB<22> & RefUrg & !ram/RefDone & 
	!ram/RS_FSM_FFd1
	# RefUrg & !ram/RefDone & !ram/RS_FSM_FFd8 & 
	!ram/RS_FSM_FFd1
	# RefUrg & !ram/RefDone & !ram/RASEN & 
	!ram/RS_FSM_FFd1
;Imported pterms FB5_9
	# RefUrg & !ram/RefDone & nAS_FSB & 
	!ram/RS_FSM_FFd1 & !fsb/ASrf
	# A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr & fsb/ASrf;
   ram/RASEN.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 3 | ram/RS_FSM_FFd1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 9 | 0 | 9 | 4 | 0 | 4 | 9 | 4 | 12 | 4 | 4 | 4 | 1 | 4 | 8 | 4 | 11 | 4 | 17
INPUTS | 1 | ram/RS_FSM_FFd2
INPUTMC | 1 | 0 | 2
EQ | 2 | 
   ram/RS_FSM_FFd1.D = ram/RS_FSM_FFd2;
   ram/RS_FSM_FFd1.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 5 | 17 | IOACT
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 5 | 1 | 5 | 16 | 1 | 9
INPUTS | 9 | iobm/IOS_FSM_FFd5  | iobm/IOS_FSM_FFd6  | iobm/IOS_FSM_FFd4  | iobm/IOS_FSM_FFd3  | iobm/C8Mr  | iobm/IOS_FSM_FFd7  | iobm/IORDREQr  | nAoutOE  | nDinLE_OBUF.EXP
INPUTMC | 9 | 1 | 12 | 5 | 0 | 1 | 13 | 5 | 3 | 1 | 16 | 5 | 2 | 1 | 15 | 3 | 1 | 5 | 16
IMPORTS | 1 | 5 | 16
EQ | 11 | 
   IOACT.D = iobm/IOS_FSM_FFd4
	# iobm/IOS_FSM_FFd5
	# iobm/IOS_FSM_FFd6
	# iobm/IOS_FSM_FFd3 & iobm/C8Mr
	# iobm/IOS_FSM_FFd7 & iobm/IORDREQr & !nAoutOE
;Imported pterms FB6_17
	# !IOBERR & !IODONE & iobm/IOS_FSM_FFd3
	# iobm/IOS_FSM_FFd7 & iobm/IOWRREQr & !nAoutOE
	# !iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & IOACT & 
	!iobm/IOS_FSM_FFd1 & !iobm/IOS_FSM_FFd2;
   IOACT.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 4 | 7 | cnt/Wait<0>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 6 | 2 | 10 | 4 | 7 | 2 | 13 | 2 | 12 | 2 | 11 | 4 | 8
INPUTS | 6 | nAS_FSB  | cnt/Wait<0>  | fsb/ASrf  | A_FSB<11>  | ram/RASEL  | A_FSB<3>
INPUTMC | 3 | 4 | 7 | 2 | 17 | 7 | 8
INPUTP | 3 | 54 | 15 | 155
EXPORTS | 1 | 4 | 8
EQ | 4 | 
   !cnt/Wait<0>.T = nAS_FSB & !cnt/Wait<0> & !fsb/ASrf;
   cnt/Wait<0>.CLK = FCLK;	// GCK
    cnt/Wait<0>.EXP  =  A_FSB<11> & !ram/RASEL
	# ram/RASEL & A_FSB<3>
GLOBALS | 1 | 2 | FCLK

MACROCELL | 1 | 14 | iobm/IOS_FSM_FFd1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 5 | 2 | 5 | 16 | 5 | 15 | 5 | 12
INPUTS | 1 | iobm/IOS_FSM_FFd2
INPUTMC | 1 | 1 | 17
EQ | 2 | 
   iobm/IOS_FSM_FFd1.D = iobm/IOS_FSM_FFd2;
   iobm/IOS_FSM_FFd1.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 1 | 17 | iobm/IOS_FSM_FFd2
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 5 | 16 | 1 | 14 | 5 | 15 | 5 | 12
INPUTS | 4 | IODONE  | iobm/IOS_FSM_FFd3  | iobm/C8Mr  | IOBERR
INPUTMC | 4 | 5 | 9 | 5 | 3 | 1 | 16 | 0 | 16
EQ | 3 | 
   iobm/IOS_FSM_FFd2.D = IOBERR & iobm/IOS_FSM_FFd3 & !iobm/C8Mr
	# IODONE & iobm/IOS_FSM_FFd3 & !iobm/C8Mr;
   iobm/IOS_FSM_FFd2.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 1 | 9 | iobs/IOACTr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 7 | 9 | 3 | 15 | 7 | 2 | 3 | 12
INPUTS | 1 | IOACT
INPUTMC | 1 | 5 | 17
EQ | 2 | 
   iobs/IOACTr.D = IOACT;
   iobs/IOACTr.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 6 | iobs/Load1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 0 | 12 | 0 | 11 | 5 | 13
INPUTS | 18 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<14>  | iobs/Sent  | nWE_FSB  | nAS_FSB  | iobs/TS_FSM_FFd2  | nADoutLE1  | A_FSB<13>  | fsb/ASrf  | iobs/TS_FSM_FFd1  | nRAMUWE_OBUF.EXP
INPUTMC | 6 | 7 | 17 | 3 | 15 | 5 | 13 | 2 | 17 | 7 | 9 | 7 | 7
INPUTP | 12 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 19 | 47 | 54 | 18
IMPORTS | 1 | 7 | 7
EQ | 34 | 
   iobs/Load1.D = !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & !nAS_FSB & iobs/TS_FSM_FFd2 & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/TS_FSM_FFd2 & fsb/ASrf & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & !nAS_FSB & iobs/TS_FSM_FFd1 & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & !nAS_FSB & iobs/TS_FSM_FFd2 & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/TS_FSM_FFd2 & fsb/ASrf & 
	nADoutLE1
;Imported pterms FB8_8
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & !nAS_FSB & iobs/TS_FSM_FFd1 & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/TS_FSM_FFd1 & fsb/ASrf & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/TS_FSM_FFd1 & fsb/ASrf & 
	nADoutLE1;
   iobs/Load1.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 1 | 7 | ram/DTACKr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 0 | 0 | 0 | 10 | 4 | 4 | 4 | 6
INPUTS | 1 | nDTACK_FSB
INPUTMC | 1 | 2 | 8
EQ | 2 | 
   ram/DTACKr.D = !nDTACK_FSB;
   ram/DTACKr.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 10 | ram/RS_FSM_FFd5
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 5 | 0 | 0 | 0 | 10 | 4 | 12 | 4 | 4 | 4 | 11
INPUTS | 3 | ram/RS_FSM_FFd6  | ram/DTACKr  | ram/RS_FSM_FFd5
INPUTMC | 3 | 7 | 10 | 1 | 7 | 0 | 10
EQ | 3 | 
   ram/RS_FSM_FFd5.D = ram/RS_FSM_FFd6
	# !ram/DTACKr & ram/RS_FSM_FFd5;
   ram/RS_FSM_FFd5.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 10 | ram/RS_FSM_FFd6
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 5 | 7 | 8 | 0 | 10 | 4 | 12 | 0 | 4 | 4 | 11
INPUTS | 7 | A_FSB<23>  | A_FSB<22>  | cs/nOverlay  | nAS_FSB  | ram/RS_FSM_FFd8  | ram/RASEN  | fsb/ASrf
INPUTMC | 4 | 3 | 0 | 4 | 0 | 4 | 9 | 2 | 17
INPUTP | 3 | 36 | 30 | 54
EQ | 5 | 
   ram/RS_FSM_FFd6.D = !A_FSB<23> & !A_FSB<22> & cs/nOverlay & !nAS_FSB & 
	ram/RS_FSM_FFd8 & ram/RASEN
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & 
	ram/RS_FSM_FFd8 & ram/RASEN & fsb/ASrf;
   ram/RS_FSM_FFd6.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 3 | ram/RS_FSM_FFd7
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 6 | 0 | 9 | 0 | 1 | 4 | 17 | 4 | 4 | 4 | 3 | 7 | 2
INPUTS | 13 | RefUrg  | ram/RefDone  | ram/RS_FSM_FFd4  | A_FSB<22>  | ram/RS_FSM_FFd8  | A_FSB<23>  | ram/RASEN  | A_FSB<21>  | A_FSB<20>  | cs/nOverlay  | iobs/TS_FSM_FFd2  | nADoutLE1  | nRAS_OBUF.EXP
INPUTMC | 9 | 0 | 15 | 0 | 9 | 0 | 0 | 4 | 0 | 4 | 9 | 3 | 0 | 3 | 15 | 5 | 13 | 7 | 4
INPUTP | 4 | 30 | 36 | 29 | 28
EXPORTS | 1 | 7 | 2
IMPORTS | 1 | 7 | 4
EQ | 21 | 
   ram/RS_FSM_FFd7.D = RefUrg & !ram/RefDone & ram/RS_FSM_FFd4
	# A_FSB<23> & RefUrg & !ram/RefDone & 
	ram/RS_FSM_FFd8
	# A_FSB<22> & RefUrg & !ram/RefDone & 
	ram/RS_FSM_FFd8
	# RefUrg & !ram/RefDone & ram/RS_FSM_FFd8 & 
	!ram/RASEN
;Imported pterms FB8_5
	# RefUrg & !ram/RefDone & nAS_FSB & 
	ram/RS_FSM_FFd8 & !fsb/ASrf
	# A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf;
   ram/RS_FSM_FFd7.CLK = FCLK;	// GCK
    ram/RS_FSM_FFd7.EXP  =  !A_FSB<23> & !A_FSB<21> & !A_FSB<20> & cs/nOverlay & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 8 | IOL0
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 4 | 5 | 8 | 3 | 8 | 3 | 7 | 5 | 7
INPUTS | 9 | iobs/TS_FSM_FFd1  | iobs/Sent  | iobs/TS_FSM_FFd2  | nADoutLE1  | nLDS_FSB  | IOL0  | iobs/IOL1  | N0.EXP  | EXP11_.EXP
INPUTMC | 8 | 7 | 9 | 7 | 17 | 3 | 15 | 5 | 13 | 3 | 8 | 0 | 12 | 3 | 7 | 3 | 9
INPUTP | 1 | 49
IMPORTS | 2 | 3 | 7 | 3 | 9
EQ | 30 | 
   !IOL0.T = iobs/TS_FSM_FFd1
	# iobs/Sent & !iobs/TS_FSM_FFd2 & nADoutLE1
	# nLDS_FSB & !IOL0 & nADoutLE1
	# !nLDS_FSB & IOL0 & nADoutLE1
	# iobs/IOL1 & IOL0 & !nADoutLE1
;Imported pterms FB4_8
	# !iobs/IOL1 & !IOL0 & !nADoutLE1
	# nAS_FSB & !iobs/TS_FSM_FFd2 & !fsb/ASrf & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<20> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & nWE_FSB & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_10
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<19> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<18> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<17> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<16> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_11
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<13> & !A_FSB<14> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<21> & !A_FSB<20> & cs/nOverlay & 
	!iobs/TS_FSM_FFd2 & nADoutLE1;
   IOL0.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 3 | IOU0
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 4 | 5 | 10 | 3 | 3 | 3 | 2 | 5 | 9
INPUTS | 9 | iobs/TS_FSM_FFd1  | iobs/Sent  | iobs/TS_FSM_FFd2  | nADoutLE1  | nUDS_FSB  | IOU0  | iobs/IOU1  | EXP10_.EXP  | nDoutOE_OBUF.EXP
INPUTMC | 8 | 7 | 9 | 7 | 17 | 3 | 15 | 5 | 13 | 3 | 3 | 0 | 11 | 3 | 2 | 3 | 4
INPUTP | 1 | 56
IMPORTS | 2 | 3 | 2 | 3 | 4
EQ | 30 | 
   !IOU0.T = iobs/TS_FSM_FFd1
	# iobs/Sent & !iobs/TS_FSM_FFd2 & nADoutLE1
	# nUDS_FSB & !IOU0 & nADoutLE1
	# !nUDS_FSB & IOU0 & nADoutLE1
	# iobs/IOU1 & IOU0 & !nADoutLE1
;Imported pterms FB4_3
	# !iobs/IOU1 & !IOU0 & !nADoutLE1
	# nAS_FSB & !iobs/TS_FSM_FFd2 & !fsb/ASrf & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<20> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & nWE_FSB & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_2
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<13> & !A_FSB<14> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_5
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<19> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<18> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<17> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<16> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<21> & !A_FSB<20> & cs/nOverlay & 
	!iobs/TS_FSM_FFd2 & nADoutLE1;
   IOU0.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 13 | cnt/Wait<1>
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 5 | 2 | 10 | 2 | 13 | 2 | 12 | 2 | 11 | 2 | 14
INPUTS | 8 | cnt/Wait<0>  | cnt/Wait<1>  | nAS_FSB  | fsb/ASrf  | QoSReady  | cnt/Wait<2>  | cnt/Wait<3>  | cnt/Wait<4>
INPUTMC | 7 | 4 | 7 | 2 | 13 | 2 | 17 | 2 | 14 | 2 | 12 | 2 | 11 | 2 | 10
INPUTP | 1 | 54
EXPORTS | 1 | 2 | 14
EQ | 7 | 
   !cnt/Wait<1>.D = nAS_FSB & !fsb/ASrf
	# cnt/Wait<0> & cnt/Wait<1>
	# !cnt/Wait<0> & !cnt/Wait<1>;
   cnt/Wait<1>.CLK = FCLK;	// GCK
    cnt/Wait<1>.EXP  =  QoSReady & fsb/ASrf
	# !cnt/Wait<0> & !cnt/Wait<1> & !cnt/Wait<2> & 
	!cnt/Wait<3> & cnt/Wait<4>
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 12 | cnt/Wait<2>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 4 | 2 | 13 | 2 | 12 | 2 | 11 | 2 | 10
INPUTS | 5 | nAS_FSB  | cnt/Wait<0>  | cnt/Wait<1>  | fsb/ASrf  | cnt/Wait<2>
INPUTMC | 4 | 4 | 7 | 2 | 13 | 2 | 17 | 2 | 12
INPUTP | 1 | 54
EQ | 4 | 
   cnt/Wait<2>.T = nAS_FSB & cnt/Wait<2> & !fsb/ASrf
	# !nAS_FSB & cnt/Wait<0> & cnt/Wait<1>
	# cnt/Wait<0> & cnt/Wait<1> & fsb/ASrf;
   cnt/Wait<2>.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 11 | cnt/Wait<3>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 3 | 2 | 13 | 2 | 11 | 2 | 10
INPUTS | 6 | nAS_FSB  | cnt/Wait<3>  | fsb/ASrf  | cnt/Wait<0>  | cnt/Wait<1>  | cnt/Wait<2>
INPUTMC | 5 | 2 | 11 | 2 | 17 | 4 | 7 | 2 | 13 | 2 | 12
INPUTP | 1 | 54
EQ | 6 | 
   cnt/Wait<3>.T = nAS_FSB & cnt/Wait<3> & !fsb/ASrf
	# !nAS_FSB & cnt/Wait<0> & cnt/Wait<1> & 
	cnt/Wait<2>
	# cnt/Wait<0> & cnt/Wait<1> & cnt/Wait<2> & 
	fsb/ASrf;
   cnt/Wait<3>.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 1 | 15 | iobm/IORDREQr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 9 | 5 | 11 | 5 | 7 | 5 | 9 | 5 | 2 | 5 | 0 | 5 | 17 | 5 | 15 | 5 | 12 | 3 | 5
INPUTS | 1 | IORDREQ
INPUTMC | 1 | 7 | 2
EQ | 2 | 
   iobm/IORDREQr.D = IORDREQ;
   iobm/IORDREQr.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 0 | 2 | ram/RS_FSM_FFd2
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 0 | 9 | 0 | 3 | 4 | 4
INPUTS | 1 | ram/RS_FSM_FFd3
INPUTMC | 1 | 0 | 1
EQ | 2 | 
   ram/RS_FSM_FFd2.D = ram/RS_FSM_FFd3;
   ram/RS_FSM_FFd2.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 1 | ram/RS_FSM_FFd3
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 0 | 9 | 0 | 2 | 4 | 4
INPUTS | 1 | ram/RS_FSM_FFd7
INPUTMC | 1 | 7 | 3
EQ | 2 | 
   ram/RS_FSM_FFd3.D = ram/RS_FSM_FFd7;
   ram/RS_FSM_FFd3.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 5 | 15 | ALE0M
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 5 | 15 | 5 | 14
INPUTS | 11 | iobm/IOS_FSM_FFd7  | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd4  | iobm/IOS_FSM_FFd5  | iobm/IOS_FSM_FFd6  | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd2  | ALE0M  | nAoutOE  | iobm/IORDREQr  | iobm/IOWRREQr
INPUTMC | 11 | 5 | 2 | 5 | 3 | 1 | 13 | 1 | 12 | 5 | 0 | 1 | 14 | 1 | 17 | 5 | 15 | 3 | 1 | 1 | 15 | 1 | 11
EQ | 14 | 
   !ALE0M.D = iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & nAoutOE
	# !iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & 
	iobm/IOS_FSM_FFd1
	# !iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & 
	iobm/IOS_FSM_FFd2
	# !iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & !ALE0M
	# iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & 
	!iobm/IORDREQr & !iobm/IOWRREQr;
   ALE0M.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 7 | 13 | BACTr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 7 | 4 | 1 | 4 | 8 | 4 | 6 | 4 | 11 | 4 | 15 | 4 | 5 | 7 | 4
INPUTS | 2 | nAS_FSB  | fsb/ASrf
INPUTMC | 1 | 2 | 17
INPUTP | 1 | 54
EQ | 2 | 
   !BACTr.D = nAS_FSB & !fsb/ASrf;
   BACTr.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 2 | IORDREQ
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 1 | 15 | 7 | 2
INPUTS | 9 | iobs/TS_FSM_FFd1  | iobs/TS_FSM_FFd2  | iobs/IOACTr  | IORDREQ  | nWE_FSB  | nADoutLE1  | iobs/Sent  | RA_11_OBUF$BUF0.EXP  | ram/RS_FSM_FFd7.EXP
INPUTMC | 8 | 7 | 9 | 3 | 15 | 1 | 9 | 7 | 2 | 5 | 13 | 7 | 17 | 7 | 1 | 7 | 3
INPUTP | 1 | 47
IMPORTS | 2 | 7 | 1 | 7 | 3
EQ | 15 | 
   !IORDREQ.D = iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2
	# iobs/TS_FSM_FFd1 & iobs/IOACTr
	# iobs/TS_FSM_FFd2 & !IORDREQ
	# iobs/Sent & !iobs/TS_FSM_FFd2 & nADoutLE1
	# !nWE_FSB & !iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB8_2
	# !iobs/IORW1 & !iobs/TS_FSM_FFd2 & !nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !iobs/TS_FSM_FFd2 & 
	nADoutLE1
	# nAS_FSB & !iobs/TS_FSM_FFd2 & !fsb/ASrf & 
	nADoutLE1
;Imported pterms FB8_4
	# !A_FSB<23> & !A_FSB<21> & !A_FSB<20> & cs/nOverlay & 
	!iobs/TS_FSM_FFd2 & nADoutLE1;
   IORDREQ.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 12 | IOWRREQ
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 3 | 12 | 1 | 11
INPUTS | 13 | iobs/TS_FSM_FFd1  | iobs/TS_FSM_FFd2  | IOWRREQ  | iobs/IOACTr  | iobs/IORW1  | nADoutLE1  | A_FSB<23>  | iobs/Sent  | nWE_FSB  | nAS_FSB  | fsb/ASrf  | EXP12_.EXP  | EXP13_.EXP
INPUTMC | 10 | 7 | 9 | 3 | 15 | 3 | 12 | 1 | 9 | 3 | 16 | 5 | 13 | 7 | 17 | 2 | 17 | 3 | 11 | 3 | 13
INPUTP | 3 | 36 | 47 | 54
IMPORTS | 2 | 3 | 11 | 3 | 13
EQ | 35 | 
   IOWRREQ.D = !iobs/TS_FSM_FFd1 & iobs/TS_FSM_FFd2 & IOWRREQ
	# iobs/TS_FSM_FFd2 & !iobs/IOACTr & IOWRREQ
	# !iobs/IORW1 & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & 
	!nADoutLE1
	# A_FSB<23> & !iobs/Sent & !nWE_FSB & !nAS_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<23> & !iobs/Sent & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
;Imported pterms FB4_12
	# A_FSB<22> & A_FSB<21> & !iobs/Sent & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<22> & A_FSB<21> & !iobs/Sent & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<22> & A_FSB<20> & !iobs/Sent & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<22> & A_FSB<20> & !iobs/Sent & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<22> & !iobs/Sent & !cs/nOverlay & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_14
	# A_FSB<22> & !iobs/Sent & !cs/nOverlay & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<13> & !iobs/Sent & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<13> & !iobs/Sent & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<14> & !iobs/Sent & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<14> & !iobs/Sent & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1;
   IOWRREQ.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 8 | cnt/Er<0>
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 25 | 2 | 15 | 2 | 0 | 0 | 13 | 6 | 15 | 6 | 17 | 0 | 15 | 2 | 1 | 6 | 16 | 6 | 14 | 6 | 13 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 0 | 6 | 2 | 0 | 7 | 0 | 14 | 2 | 2
INPUTS | 1 | E
INPUTP | 1 | 37
EQ | 2 | 
   cnt/Er<0>.D = E;
   cnt/Er<0>.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 10 | cnt/Wait<4>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 2 | 2 | 13 | 2 | 10
INPUTS | 7 | nAS_FSB  | cnt/Wait<4>  | fsb/ASrf  | cnt/Wait<0>  | cnt/Wait<1>  | cnt/Wait<2>  | cnt/Wait<3>
INPUTMC | 6 | 2 | 10 | 2 | 17 | 4 | 7 | 2 | 13 | 2 | 12 | 2 | 11
INPUTP | 1 | 54
EQ | 6 | 
   cnt/Wait<4>.T = nAS_FSB & cnt/Wait<4> & !fsb/ASrf
	# !nAS_FSB & cnt/Wait<0> & cnt/Wait<1> & 
	cnt/Wait<2> & cnt/Wait<3>
	# cnt/Wait<0> & cnt/Wait<1> & cnt/Wait<2> & 
	cnt/Wait<3> & fsb/ASrf;
   cnt/Wait<4>.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 6 | cnt/nIPL2r
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 7 | 14 | 0 | 7
INPUTS | 1 | nIPL2
INPUTP | 1 | 146
EQ | 2 | 
   cnt/nIPL2r.D = nIPL2;
   cnt/nIPL2r.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 5 | 7 | iobm/DoutOE
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 3 | 5 | 7 | 3 | 5 | 5 | 8
INPUTS | 10 | iobm/IOS_FSM_FFd7  | iobm/C8Mr  | iobm/DoutOE  | iobm/IOWRREQr  | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd4  | iobm/IOS_FSM_FFd5  | iobm/IOS_FSM_FFd6  | IOL0  | iobm/IORDREQr
INPUTMC | 10 | 5 | 2 | 1 | 16 | 5 | 7 | 1 | 11 | 5 | 3 | 1 | 13 | 1 | 12 | 5 | 0 | 3 | 8 | 1 | 15
EXPORTS | 1 | 5 | 8
EQ | 13 | 
   iobm/DoutOE.T = iobm/IOS_FSM_FFd7 & !iobm/C8Mr & !iobm/DoutOE & 
	iobm/IOWRREQr
	# !iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & 
	iobm/DoutOE
	# !iobm/IOS_FSM_FFd3 & iobm/C8Mr & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & 
	iobm/DoutOE
	# !iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd4 & 
	!iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & iobm/DoutOE & !iobm/IOWRREQr;
   iobm/DoutOE.CLK = C16M;	// GCK
    iobm/DoutOE.EXP  =  iobm/IOS_FSM_FFd7 & !iobm/C8Mr & IOL0 & 
	iobm/IORDREQr
GLOBALS | 1 | 2 | C16M

MACROCELL | 0 | 5 | iobm/Er
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 5 | 4 | 0 | 17 | 5 | 6 | 5 | 5
INPUTS | 1 | E
INPUTP | 1 | 37
EQ | 2 | 
   iobm/Er.D = E;
   !iobm/Er.CLK = C8M;	// GCK
GLOBALS | 1 | 2 | C8M

MACROCELL | 5 | 12 | iobm/IOS0
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 5 | 12 | 3 | 5
INPUTS | 12 | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd7  | iobm/C8Mr  | nAoutOE  | iobm/IORDREQr  | iobm/IOWRREQr  | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd4  | iobm/IOS_FSM_FFd5  | iobm/IOS_FSM_FFd6  | iobm/IOS_FSM_FFd2  | iobm/IOS0
INPUTMC | 12 | 1 | 14 | 5 | 2 | 1 | 16 | 3 | 1 | 1 | 15 | 1 | 11 | 5 | 3 | 1 | 13 | 1 | 12 | 5 | 0 | 1 | 17 | 5 | 12
EQ | 9 | 
   iobm/IOS0.D = iobm/IOS_FSM_FFd1
	# iobm/IOS_FSM_FFd7 & iobm/C8Mr
	# iobm/IOS_FSM_FFd7 & nAoutOE
	# iobm/IOS_FSM_FFd7 & !iobm/IORDREQr & 
	!iobm/IOWRREQr
	# !iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd4 & !iobm/IOS_FSM_FFd5 & !iobm/IOS_FSM_FFd6 & 
	!iobm/IOS_FSM_FFd2 & iobm/IOS0;
   iobm/IOS0.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 1 | 11 | iobm/IOWRREQr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 8 | 5 | 11 | 5 | 2 | 5 | 0 | 5 | 16 | 5 | 15 | 5 | 7 | 5 | 12 | 3 | 5
INPUTS | 1 | IOWRREQ
INPUTMC | 1 | 3 | 12
EQ | 2 | 
   iobm/IOWRREQr.D = IOWRREQ;
   iobm/IOWRREQr.CLK = C16M;	// GCK
GLOBALS | 1 | 2 | C16M

MACROCELL | 1 | 10 | iobm/VPAr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 5 | 1
INPUTS | 1 | nVPA_IOB
INPUTP | 1 | 125
EQ | 2 | 
   iobm/VPAr.D = !nVPA_IOB;
   !iobm/VPAr.CLK = C8M;	// GCK
GLOBALS | 1 | 2 | C8M

MACROCELL | 7 | 12 | ALE0S
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 5 | 14
INPUTS | 1 | iobs/TS_FSM_FFd2
INPUTMC | 1 | 3 | 15
EQ | 2 | 
   ALE0S.D = iobs/TS_FSM_FFd2;
   ALE0S.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 4 | 12 | RAMReady
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 2 | 7
INPUTS | 11 | ram/RS_FSM_FFd8  | ram/RS_FSM_FFd4  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd5  | ram/RS_FSM_FFd6  | A_FSB<22>  | RefUrg  | ram/RefDone  | A_FSB<23>  | ram/RASEN  | RA_5_OBUF.EXP
INPUTMC | 9 | 4 | 0 | 0 | 0 | 0 | 3 | 0 | 10 | 7 | 10 | 0 | 15 | 0 | 9 | 4 | 9 | 4 | 11
INPUTP | 2 | 30 | 36
IMPORTS | 1 | 4 | 11
EQ | 26 | 
   !RAMReady.D = !ram/RS_FSM_FFd8 & !ram/RS_FSM_FFd4 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & !ram/RS_FSM_FFd6
	# A_FSB<23> & RefUrg & !ram/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & !ram/RS_FSM_FFd6
	# A_FSB<22> & RefUrg & !ram/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & !ram/RS_FSM_FFd6
	# RefUrg & !ram/RefDone & !ram/RS_FSM_FFd8 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & !ram/RS_FSM_FFd6
	# RefUrg & !ram/RefDone & !ram/RASEN & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & !ram/RS_FSM_FFd6
;Imported pterms FB5_12
	# RefUrg & !ram/RefDone & nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & !ram/RS_FSM_FFd6 & !fsb/ASrf
	# A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & 
	!ram/RS_FSM_FFd6 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & 
	!ram/RS_FSM_FFd6 & !BACTr & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & 
	!ram/RS_FSM_FFd6 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & 
	!ram/RS_FSM_FFd6 & !BACTr & fsb/ASrf;
   RAMReady.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 2 | cnt/Er<1>
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 24 | 2 | 15 | 2 | 0 | 0 | 13 | 6 | 15 | 6 | 17 | 0 | 15 | 2 | 1 | 6 | 16 | 6 | 14 | 6 | 13 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 6 | 12 | 6 | 0 | 6 | 2 | 0 | 7 | 0 | 14
INPUTS | 1 | cnt/Er<0>
INPUTMC | 1 | 0 | 8
EQ | 2 | 
   cnt/Er<1>.D = cnt/Er<0>;
   cnt/Er<1>.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 2 | 17 | fsb/ASrf
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 38 | 7 | 17 | 4 | 1 | 3 | 11 | 3 | 0 | 2 | 1 | 3 | 13 | 4 | 14 | 7 | 11 | 3 | 10 | 2 | 8 | 7 | 8 | 3 | 15 | 3 | 17 | 4 | 8 | 4 | 7 | 7 | 6 | 7 | 10 | 7 | 0 | 3 | 7 | 3 | 2 | 2 | 13 | 2 | 12 | 2 | 11 | 7 | 13 | 7 | 1 | 3 | 12 | 2 | 10 | 4 | 11 | 4 | 16 | 2 | 16 | 4 | 5 | 4 | 6 | 4 | 15 | 4 | 17 | 7 | 4 | 7 | 7 | 7 | 16 | 2 | 0
INPUTS | 18 | nAS_FSB  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<15>  | A_FSB<13>  | A_FSB<14>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | nWE_FSB  | A_FSB<9>  | A_FSB<8>
INPUTP | 18 | 54 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 21 | 18 | 19 | 17 | 15 | 13 | 47 | 12 | 11
EXPORTS | 1 | 2 | 0
EQ | 18 | 
   fsb/ASrf.D = !nAS_FSB;
   !fsb/ASrf.CLK = FCLK;	// GCK
    fsb/ASrf.EXP  =  !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<9>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<8>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<9>
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & !nAS_FSB & A_FSB<8>
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 15 | iobs/Clear1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 5 | 13
INPUTS | 2 | iobs/TS_FSM_FFd1  | iobs/TS_FSM_FFd2
INPUTMC | 2 | 7 | 9 | 3 | 15
EQ | 2 | 
   iobs/Clear1.D = !iobs/TS_FSM_FFd1 & iobs/TS_FSM_FFd2;
   iobs/Clear1.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 1 | 8 | iobs/IODONEr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 4 | 14
INPUTS | 1 | IODONE
INPUTMC | 1 | 5 | 9
EQ | 2 | 
   iobs/IODONEr.D = IODONE;
   iobs/IODONEr.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 7 | 16 | nRESout
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 3 | 7 | 7 | 17
INPUTS | 12 | cnt/IS_FSM_FFd1  | cnt/IS_FSM_FFd2  | A_FSB<22>  | A_FSB<21>  | iobs/Sent  | iobs/TS_FSM_FFd1  | iobs/TS_FSM_FFd2  | fsb/ASrf  | nADoutLE1  | A_FSB<20>  | cs/nOverlay  | nAS_FSB
INPUTMC | 8 | 0 | 7 | 0 | 14 | 7 | 17 | 7 | 9 | 3 | 15 | 2 | 17 | 5 | 13 | 3 | 0
INPUTP | 4 | 30 | 29 | 28 | 54
EXPORTS | 1 | 7 | 17
EQ | 8 | 
   nRESout.D = cnt/IS_FSM_FFd1 & !cnt/IS_FSM_FFd2;
   nRESout.CLK = FCLK;	// GCK
    nRESout.EXP  =  A_FSB<22> & A_FSB<21> & !iobs/Sent & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<22> & A_FSB<20> & !iobs/Sent & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<22> & !iobs/Sent & !cs/nOverlay & !nAS_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
GLOBALS | 1 | 2 | FCLK

MACROCELL | 0 | 4 | ram/RASrf
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 7 | 5
INPUTS | 1 | ram/RS_FSM_FFd6
INPUTMC | 1 | 7 | 10
EQ | 2 | 
   ram/RASrf.D = ram/RS_FSM_FFd6;
   !ram/RASrf.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 4 | 17 | ram/RASrr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 7 | 5 | 4 | 0
INPUTS | 13 | ram/RS_FSM_FFd7  | RefUrg  | ram/RefDone  | ram/RS_FSM_FFd4  | ram/RS_FSM_FFd8  | ram/RS_FSM_FFd1  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay  | ram/RASEN  | EXP19_.EXP
INPUTMC | 10 | 7 | 3 | 0 | 15 | 0 | 9 | 0 | 0 | 4 | 0 | 0 | 3 | 2 | 17 | 3 | 0 | 4 | 9 | 4 | 16
INPUTP | 3 | 54 | 36 | 30
EXPORTS | 1 | 4 | 0
IMPORTS | 1 | 4 | 16
EQ | 31 | 
   ram/RASrr.D = ram/RS_FSM_FFd7
	# RefUrg & !ram/RefDone & ram/RS_FSM_FFd4
;Imported pterms FB5_17
	# A_FSB<23> & RefUrg & !ram/RefDone & 
	ram/RS_FSM_FFd8
	# A_FSB<22> & RefUrg & !ram/RefDone & 
	ram/RS_FSM_FFd8
	# RefUrg & !ram/RefDone & ram/RS_FSM_FFd8 & 
	!ram/RASEN
	# RefUrg & !ram/RefDone & nAS_FSB & 
	ram/RS_FSM_FFd8 & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & !nAS_FSB & 
	ram/RS_FSM_FFd8 & ram/RASEN
;Imported pterms FB5_16
	# A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & 
	ram/RS_FSM_FFd8 & ram/RASEN & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf;
   ram/RASrr.CLK = FCLK;	// GCK
    ram/RASrr.EXP  =  RefUrg & !ram/RefDone & !ram/RS_FSM_FFd8 & 
	!ram/RS_FSM_FFd1
	# RefUrg & !ram/RefDone & nAS_FSB & 
	!ram/RS_FSM_FFd1 & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & ram/RASEN & !ram/RS_FSM_FFd1
GLOBALS | 1 | 2 | FCLK

MACROCELL | 6 | 5 | RA_0_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 3 | ram/RASEL  | A_FSB<1>  | A_FSB<9>
INPUTMC | 1 | 7 | 8
INPUTP | 2 | 149 | 12
EQ | 2 | 
   RA<0> = ram/RASEL & A_FSB<1>
	# !ram/RASEL & A_FSB<9>;

MACROCELL | 6 | 8 | RA_10_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 3 | A_FSB<17>  | ram/RASEL  | A_FSB<7>
INPUTMC | 1 | 7 | 8
INPUTP | 2 | 23 | 8
EQ | 2 | 
   RA<10> = A_FSB<17> & !ram/RASEL
	# ram/RASEL & A_FSB<7>;

MACROCELL | 6 | 1 | RA_1_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 3 | A_FSB<10>  | ram/RASEL  | A_FSB<2>
INPUTMC | 1 | 7 | 8
INPUTP | 2 | 13 | 153
EQ | 2 | 
   RA<1> = A_FSB<10> & !ram/RASEL
	# ram/RASEL & A_FSB<2>;

MACROCELL | 4 | 13 | RA_2_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 14
INPUTS | 5 | A_FSB<16>  | ram/RASEL  | A_FSB<7>  | A_FSB<13>  | A_FSB<5>
INPUTMC | 1 | 7 | 8
INPUTP | 4 | 22 | 8 | 18 | 4
EXPORTS | 1 | 4 | 14
EQ | 4 | 
   RA<2> = A_FSB<16> & !ram/RASEL
	# ram/RASEL & A_FSB<7>;
    RA_2_OBUF.EXP  =  A_FSB<13> & !ram/RASEL
	# ram/RASEL & A_FSB<5>

MACROCELL | 4 | 8 | RA_4_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 9
INPUTS | 11 | RefUrg  | ram/RefDone  | nAS_FSB  | ram/RS_FSM_FFd1  | fsb/ASrf  | A_FSB<23>  | RefReq  | ram/RS_FSM_FFd4  | BACTr  | A_FSB<22>  | cnt/Wait<0>.EXP
INPUTMC | 8 | 0 | 15 | 0 | 9 | 0 | 3 | 2 | 17 | 6 | 14 | 0 | 0 | 7 | 13 | 4 | 7
INPUTP | 3 | 54 | 36 | 30
EXPORTS | 1 | 4 | 9
IMPORTS | 1 | 4 | 7
EQ | 13 | 
   RA<4> = ;Imported pterms FB5_8
	  A_FSB<11> & !ram/RASEL
	# ram/RASEL & A_FSB<3>;
    RA_4_OBUF.EXP  =  RefUrg & !ram/RefDone & nAS_FSB & 
	!ram/RS_FSM_FFd1 & !fsb/ASrf
	# A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr & fsb/ASrf

MACROCELL | 4 | 11 | RA_5_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 12
INPUTS | 13 | RefUrg  | ram/RefDone  | nAS_FSB  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd5  | ram/RS_FSM_FFd6  | fsb/ASrf  | A_FSB<23>  | RefReq  | ram/RS_FSM_FFd4  | BACTr  | A_FSB<22>  | RA_11_OBUF.EXP
INPUTMC | 10 | 0 | 15 | 0 | 9 | 0 | 3 | 0 | 10 | 7 | 10 | 2 | 17 | 6 | 14 | 0 | 0 | 7 | 13 | 4 | 10
INPUTP | 3 | 54 | 36 | 30
EXPORTS | 1 | 4 | 12
IMPORTS | 1 | 4 | 10
EQ | 17 | 
   RA<5> = ;Imported pterms FB5_11
	  A_FSB<12> & !ram/RASEL
	# ram/RASEL & A_FSB<4>;
    RA_5_OBUF.EXP  =  RefUrg & !ram/RefDone & nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & !ram/RS_FSM_FFd6 & !fsb/ASrf
	# A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & 
	!ram/RS_FSM_FFd6 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & 
	!ram/RS_FSM_FFd6 & !BACTr & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & 
	!ram/RS_FSM_FFd6 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd5 & 
	!ram/RS_FSM_FFd6 & !BACTr & fsb/ASrf

MACROCELL | 4 | 14 | RA_6_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 15
INPUTS | 17 | iobs/Sent  | IONPReady  | iobs/IODONEr  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<13>  | nWE_FSB  | A_FSB<14>  | RA_2_OBUF.EXP
INPUTMC | 5 | 7 | 17 | 4 | 15 | 1 | 8 | 2 | 17 | 4 | 13
INPUTP | 12 | 54 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 18 | 47 | 19
EXPORTS | 1 | 4 | 15
IMPORTS | 1 | 4 | 13
EQ | 12 | 
   RA<6> = ;Imported pterms FB5_14
	  A_FSB<13> & !ram/RASEL
	# ram/RASEL & A_FSB<5>;
    RA_6_OBUF.EXP  =  !iobs/Sent & !IONPReady
	# !IONPReady & !iobs/IODONEr
	# nAS_FSB & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!nWE_FSB & !IONPReady
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!nWE_FSB & !IONPReady

MACROCELL | 6 | 4 | RA_7_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 3 | A_FSB<14>  | ram/RASEL  | A_FSB<6>
INPUTMC | 1 | 7 | 8
INPUTP | 2 | 19 | 6
EQ | 2 | 
   RA<7> = A_FSB<14> & !ram/RASEL
	# ram/RASEL & A_FSB<6>;

MACROCELL | 6 | 7 | RA_8_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 3 | A_FSB<18>  | ram/RASEL  | A_FSB<21>
INPUTMC | 1 | 7 | 8
INPUTP | 2 | 24 | 29
EQ | 2 | 
   RA<8> = A_FSB<21> & ram/RASEL
	# A_FSB<18> & !ram/RASEL;

MACROCELL | 6 | 10 | RA_9_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 3 | A_FSB<15>  | ram/RASEL  | A_FSB<8>
INPUTMC | 1 | 7 | 8
INPUTP | 2 | 21 | 11
EQ | 2 | 
   RA<9> = A_FSB<15> & !ram/RASEL
	# ram/RASEL & A_FSB<8>;

MACROCELL | 2 | 16 | nROMWE_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 2 | 15
INPUTS | 19 | nWE_FSB  | nAS_FSB  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<15>  | A_FSB<13>  | A_FSB<14>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<9>  | fsb/ASrf  | A_FSB<8>
INPUTMC | 1 | 2 | 17
INPUTP | 18 | 47 | 54 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 21 | 18 | 19 | 17 | 15 | 13 | 12 | 11
EXPORTS | 1 | 2 | 15
EQ | 17 | 
   !nROMWE = !nWE_FSB & !nAS_FSB;
    nROMWE_OBUF.EXP  =  !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & A_FSB<9> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & A_FSB<14> & A_FSB<12> & A_FSB<11> & A_FSB<10> & 
	!nWE_FSB & A_FSB<8> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & A_FSB<9> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<15> & 
	A_FSB<13> & !A_FSB<14> & !A_FSB<12> & !A_FSB<11> & !A_FSB<10> & 
	!nWE_FSB & A_FSB<8> & fsb/ASrf

MACROCELL | 5 | 14 | nADoutLE0_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 2 | ALE0M  | ALE0S
INPUTMC | 2 | 5 | 15 | 7 | 12
EQ | 1 | 
   nADoutLE0 = !ALE0M & !ALE0S;

MACROCELL | 4 | 4 | nCAS_OBUF
ATTRIBUTES | 8684290 | 0
INPUTS | 9 | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | ram/RS_FSM_FFd1  | ram/DTACKr  | ram/RS_FSM_FFd5  | RefUrg  | ram/RS_FSM_FFd7  | EXP17_.EXP  | nOE_OBUF.EXP
INPUTMC | 9 | 0 | 2 | 0 | 1 | 0 | 3 | 1 | 7 | 0 | 10 | 0 | 15 | 7 | 3 | 4 | 3 | 4 | 5
IMPORTS | 2 | 4 | 3 | 4 | 5
EQ | 21 | 
   nCAS.D = ram/RS_FSM_FFd1
	# ram/RS_FSM_FFd2
	# ram/RS_FSM_FFd3
	# !RefUrg & ram/RS_FSM_FFd7
	# ram/DTACKr & ram/RS_FSM_FFd5
;Imported pterms FB5_4
	# !RefUrg & ram/RS_FSM_FFd4
	# ram/RefDone & ram/RS_FSM_FFd8
	# ram/RefDone & ram/RS_FSM_FFd4
	# ram/RefDone & ram/RS_FSM_FFd7
	# !RefUrg & !RefReq & ram/RS_FSM_FFd8
;Imported pterms FB5_6
	# !RefUrg & ram/RS_FSM_FFd8 & BACTr
	# !A_FSB<23> & !A_FSB<22> & !RefUrg & 
	ram/RS_FSM_FFd8
	# !RefUrg & nAS_FSB & ram/RS_FSM_FFd8 & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & !nAS_FSB & 
	ram/RS_FSM_FFd8 & ram/RASEN
	# !A_FSB<23> & !A_FSB<22> & ram/RS_FSM_FFd8 & 
	ram/RASEN & fsb/ASrf;
   !nCAS.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 5 | 16 | nDinLE_OBUF
ATTRIBUTES | 8684290 | 0
OUTPUTMC | 1 | 5 | 17
INPUTS | 10 | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd4  | IOBERR  | IODONE  | iobm/IOS_FSM_FFd7  | iobm/IOWRREQr  | nAoutOE  | IOACT  | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd2
INPUTMC | 10 | 5 | 3 | 1 | 13 | 0 | 16 | 5 | 9 | 5 | 2 | 1 | 11 | 3 | 1 | 5 | 17 | 1 | 14 | 1 | 17
EXPORTS | 1 | 5 | 17
EQ | 6 | 
   !nDinLE.D = !iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd4;
   !nDinLE.CLK = C16M;	// GCK
    nDinLE_OBUF.EXP  =  !IOBERR & !IODONE & iobm/IOS_FSM_FFd3
	# iobm/IOS_FSM_FFd7 & iobm/IOWRREQr & !nAoutOE
	# !iobm/IOS_FSM_FFd7 & !iobm/IOS_FSM_FFd3 & IOACT & 
	!iobm/IOS_FSM_FFd1 & !iobm/IOS_FSM_FFd2
GLOBALS | 1 | 2 | C16M

MACROCELL | 4 | 5 | nOE_OBUF
ATTRIBUTES | 8684290 | 0
OUTPUTMC | 1 | 4 | 4
INPUTS | 9 | RefUrg  | ram/RS_FSM_FFd8  | BACTr  | A_FSB<23>  | A_FSB<22>  | nAS_FSB  | fsb/ASrf  | ram/RASEN  | EXP18_.EXP
INPUTMC | 6 | 0 | 15 | 4 | 0 | 7 | 13 | 2 | 17 | 4 | 9 | 4 | 6
INPUTP | 3 | 36 | 30 | 54
EXPORTS | 1 | 4 | 4
IMPORTS | 1 | 4 | 6
EQ | 13 | 
   nOE.D = ;Imported pterms FB5_7
	  !nWE_FSB
	# nAS_FSB & !fsb/ASrf
	# ram/DTACKr & BACTr;
   nOE.CLK = FCLK;	// GCK
    nOE_OBUF.EXP  =  !RefUrg & ram/RS_FSM_FFd8 & BACTr
	# !A_FSB<23> & !A_FSB<22> & !RefUrg & 
	ram/RS_FSM_FFd8
	# !RefUrg & nAS_FSB & ram/RS_FSM_FFd8 & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & !nAS_FSB & 
	ram/RS_FSM_FFd8 & ram/RASEN
	# !A_FSB<23> & !A_FSB<22> & ram/RS_FSM_FFd8 & 
	ram/RASEN & fsb/ASrf
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 7 | N0
ATTRIBUTES | 265986 | 0
OUTPUTMC | 1 | 3 | 8
INPUTS | 11 | nRESout  | iobs/IOL1  | IOL0  | nADoutLE1  | nAS_FSB  | iobs/TS_FSM_FFd2  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | A_FSB<20>  | nWE_FSB
INPUTMC | 6 | 7 | 16 | 0 | 12 | 3 | 8 | 5 | 13 | 3 | 15 | 2 | 17
INPUTP | 5 | 54 | 36 | 30 | 28 | 47
EXPORTS | 1 | 3 | 8
EQ | 9 | 
   nRES = Gnd;
   nRES.OE = !nRESout;
    N0.EXP  =  !iobs/IOL1 & !IOL0 & !nADoutLE1
	# nAS_FSB & !iobs/TS_FSM_FFd2 & !fsb/ASrf & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<20> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & nWE_FSB & 
	!iobs/TS_FSM_FFd2 & nADoutLE1

MACROCELL | 7 | 1 | RA_11_OBUF$BUF0
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 7 | 2
INPUTS | 10 | A_FSB<19>  | ram/RASEL  | A_FSB<20>  | iobs/IORW1  | iobs/TS_FSM_FFd2  | nADoutLE1  | A_FSB<23>  | A_FSB<22>  | nAS_FSB  | fsb/ASrf
INPUTMC | 5 | 7 | 8 | 3 | 16 | 3 | 15 | 5 | 13 | 2 | 17
INPUTP | 5 | 26 | 28 | 36 | 30 | 54
EXPORTS | 1 | 7 | 2
EQ | 7 | 
   RA<11> = A_FSB<20> & ram/RASEL
	# A_FSB<19> & !ram/RASEL;
    RA_11_OBUF$BUF0.EXP  =  !iobs/IORW1 & !iobs/TS_FSM_FFd2 & !nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !iobs/TS_FSM_FFd2 & 
	nADoutLE1
	# nAS_FSB & !iobs/TS_FSM_FFd2 & !fsb/ASrf & 
	nADoutLE1

MACROCELL | 5 | 13 | nADoutLE1_OBUF
ATTRIBUTES | 8815366 | 0
OUTPUTMC | 26 | 7 | 17 | 3 | 16 | 5 | 13 | 3 | 15 | 7 | 6 | 3 | 8 | 3 | 3 | 7 | 2 | 3 | 12 | 2 | 9 | 3 | 0 | 3 | 1 | 3 | 2 | 3 | 4 | 3 | 7 | 3 | 9 | 3 | 10 | 3 | 11 | 3 | 13 | 3 | 14 | 3 | 17 | 7 | 0 | 7 | 1 | 7 | 3 | 7 | 7 | 7 | 16
INPUTS | 3 | iobs/Clear1  | nADoutLE1  | iobs/Load1
INPUTMC | 3 | 7 | 15 | 5 | 13 | 7 | 6
EQ | 3 | 
   !nADoutLE1.D = iobs/Load1
	# !iobs/Clear1 & !nADoutLE1;
   nADoutLE1.CLK = FCLK;	// GCK
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 1 | nAoutOE_OBUF
ATTRIBUTES | 8815366 | 0
OUTPUTMC | 13 | 5 | 1 | 5 | 11 | 5 | 8 | 5 | 10 | 5 | 2 | 5 | 0 | 5 | 17 | 5 | 15 | 5 | 12 | 3 | 1 | 3 | 5 | 5 | 16 | 3 | 2
INPUTS | 10 | nBR_IOB  | cnt/IS_FSM_FFd1  | cnt/IS_FSM_FFd2  | nAoutOE  | A_FSB<23>  | A_FSB<22>  | A_FSB<13>  | A_FSB<14>  | iobs/TS_FSM_FFd2  | nADoutLE1
INPUTMC | 6 | 7 | 14 | 0 | 7 | 0 | 14 | 3 | 1 | 3 | 15 | 5 | 13
INPUTP | 4 | 36 | 30 | 18 | 19
EXPORTS | 1 | 3 | 2
EQ | 5 | 
   !nAoutOE.D = !nBR_IOB & cnt/IS_FSM_FFd1 & cnt/IS_FSM_FFd2
	# cnt/IS_FSM_FFd1 & !cnt/IS_FSM_FFd2 & !nAoutOE;
   nAoutOE.CLK = FCLK;	// GCK
    nAoutOE_OBUF.EXP  =  !A_FSB<23> & !A_FSB<22> & !A_FSB<13> & !A_FSB<14> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
GLOBALS | 1 | 2 | FCLK

MACROCELL | 3 | 5 | nDinOE_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 3 | 4
INPUTS | 12 | A_FSB<23>  | cs/nOverlay  | nWE_FSB  | nAS_FSB  | A_FSB<22>  | A_FSB<20>  | A_FSB<21>  | iobm/DoutOE  | nAoutOE  | iobm/IORDREQr  | iobm/IOS0  | iobm/IOWRREQr
INPUTMC | 6 | 3 | 0 | 5 | 7 | 3 | 1 | 1 | 15 | 5 | 12 | 1 | 11
INPUTP | 6 | 36 | 47 | 54 | 30 | 28 | 29
EXPORTS | 1 | 3 | 4
EQ | 8 | 
   !nDinOE = A_FSB<23> & cs/nOverlay & nWE_FSB & !nAS_FSB
	# A_FSB<22> & A_FSB<21> & cs/nOverlay & nWE_FSB & 
	!nAS_FSB
	# A_FSB<22> & A_FSB<20> & cs/nOverlay & nWE_FSB & 
	!nAS_FSB;
    nDinOE_OBUF.EXP  =  iobm/DoutOE & !nAoutOE
	# !iobm/IORDREQr & iobm/IOS0 & !iobm/IOWRREQr & 
	!nAoutOE

MACROCELL | 3 | 4 | nDoutOE_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 3 | 3
INPUTS | 12 | A_FSB<23>  | A_FSB<22>  | A_FSB<19>  | iobs/TS_FSM_FFd2  | nADoutLE1  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<21>  | A_FSB<20>  | cs/nOverlay  | nDinOE_OBUF.EXP
INPUTMC | 4 | 3 | 15 | 5 | 13 | 3 | 0 | 3 | 5
INPUTP | 8 | 36 | 30 | 26 | 24 | 23 | 22 | 29 | 28
EXPORTS | 1 | 3 | 3
IMPORTS | 1 | 3 | 5
EQ | 14 | 
   !nDoutOE = ;Imported pterms FB4_6
	  iobm/DoutOE & !nAoutOE
	# !iobm/IORDREQr & iobm/IOS0 & !iobm/IOWRREQr & 
	!nAoutOE;
    nDoutOE_OBUF.EXP  =  !A_FSB<23> & !A_FSB<22> & !A_FSB<19> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<18> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<17> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<16> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<21> & !A_FSB<20> & cs/nOverlay & 
	!iobs/TS_FSM_FFd2 & nADoutLE1

MACROCELL | 7 | 5 | nRAMLWE_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 7 | 4
INPUTS | 10 | nWE_FSB  | nLDS_FSB  | ram/RASEL  | ram/RASrf  | ram/RASrr  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay  | nAS_FSB  | ram/RASEN
INPUTMC | 5 | 7 | 8 | 0 | 4 | 4 | 17 | 3 | 0 | 4 | 9
INPUTP | 5 | 47 | 49 | 36 | 30 | 54
EXPORTS | 1 | 7 | 4
EQ | 5 | 
   !nRAMLWE = !nWE_FSB & !nLDS_FSB & ram/RASEL;
    nRAMLWE_OBUF.EXP  =  ram/RASrf
	# ram/RASrr
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & !nAS_FSB & 
	ram/RASEN

MACROCELL | 7 | 7 | nRAMUWE_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 7 | 6
INPUTS | 18 | nWE_FSB  | nUDS_FSB  | ram/RASEL  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<13>  | iobs/Sent  | nAS_FSB  | iobs/TS_FSM_FFd1  | nADoutLE1  | fsb/ASrf  | A_FSB<14>
INPUTMC | 5 | 7 | 8 | 7 | 17 | 7 | 9 | 5 | 13 | 2 | 17
INPUTP | 13 | 47 | 56 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 18 | 54 | 19
EXPORTS | 1 | 7 | 6
EQ | 13 | 
   !nRAMUWE = !nWE_FSB & !nUDS_FSB & ram/RASEL;
    nRAMUWE_OBUF.EXP  =  !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & !nAS_FSB & iobs/TS_FSM_FFd1 & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/TS_FSM_FFd1 & fsb/ASrf & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/TS_FSM_FFd1 & fsb/ASrf & 
	nADoutLE1

MACROCELL | 4 | 1 | nROMCS_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 0
INPUTS | 12 | A_FSB<23>  | RefReq  | ram/RefDone  | nAS_FSB  | ram/RS_FSM_FFd4  | ram/RS_FSM_FFd1  | BACTr  | fsb/ASrf  | A_FSB<22>  | cs/nOverlay  | ram/RASEN  | EXP16_.EXP
INPUTMC | 9 | 6 | 14 | 0 | 9 | 0 | 0 | 0 | 3 | 7 | 13 | 2 | 17 | 3 | 0 | 4 | 9 | 4 | 2
INPUTP | 3 | 36 | 54 | 30
EXPORTS | 1 | 4 | 0
IMPORTS | 1 | 4 | 2
EQ | 13 | 
   !nROMCS = ;Imported pterms FB5_3
	  !cs/nOverlay
	# !A_FSB<23> & A_FSB<22> & !A_FSB<21> & !A_FSB<20>;
    nROMCS_OBUF.EXP  =  A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & 
	!ram/RS_FSM_FFd4 & ram/RASEN & !ram/RS_FSM_FFd1 & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	!ram/RS_FSM_FFd4 & !ram/RS_FSM_FFd1 & !BACTr & fsb/ASrf

MACROCELL | 6 | 11 | C25MEN_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 0
EQ | 1 | 
   C25MEN = Vcc;

MACROCELL | 3 | 2 | EXP10_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 3 | 3
INPUTS | 12 | iobs/IOU1  | IOU0  | nADoutLE1  | nAS_FSB  | iobs/TS_FSM_FFd2  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | nWE_FSB  | nAoutOE_OBUF.EXP
INPUTMC | 6 | 0 | 11 | 3 | 3 | 5 | 13 | 3 | 15 | 2 | 17 | 3 | 1
INPUTP | 6 | 54 | 36 | 30 | 29 | 28 | 47
EXPORTS | 1 | 3 | 3
IMPORTS | 1 | 3 | 1
EQ | 12 | 
       EXP10_.EXP  =  !iobs/IOU1 & !IOU0 & !nADoutLE1
	# nAS_FSB & !iobs/TS_FSM_FFd2 & !fsb/ASrf & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<20> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & nWE_FSB & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_2
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<13> & !A_FSB<14> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1

MACROCELL | 3 | 9 | EXP11_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 3 | 8
INPUTS | 10 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | iobs/TS_FSM_FFd2  | nADoutLE1  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nVPA_FSB_OBUF.EXP
INPUTMC | 3 | 3 | 15 | 5 | 13 | 3 | 10
INPUTP | 7 | 36 | 30 | 29 | 26 | 24 | 23 | 22
EXPORTS | 1 | 3 | 8
IMPORTS | 1 | 3 | 10
EQ | 15 | 
       EXP11_.EXP  =  !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<19> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<18> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<17> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<16> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
;Imported pterms FB4_11
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<13> & !A_FSB<14> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<21> & !A_FSB<20> & cs/nOverlay & 
	!iobs/TS_FSM_FFd2 & nADoutLE1

MACROCELL | 3 | 11 | EXP12_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 3 | 12
INPUTS | 11 | A_FSB<22>  | A_FSB<21>  | iobs/Sent  | nWE_FSB  | nAS_FSB  | iobs/TS_FSM_FFd1  | iobs/TS_FSM_FFd2  | nADoutLE1  | fsb/ASrf  | A_FSB<20>  | cs/nOverlay
INPUTMC | 6 | 7 | 17 | 7 | 9 | 3 | 15 | 5 | 13 | 2 | 17 | 3 | 0
INPUTP | 5 | 30 | 29 | 47 | 54 | 28
EXPORTS | 1 | 3 | 12
EQ | 10 | 
       EXP12_.EXP  =  A_FSB<22> & A_FSB<21> & !iobs/Sent & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<22> & A_FSB<21> & !iobs/Sent & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<22> & A_FSB<20> & !iobs/Sent & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<22> & A_FSB<20> & !iobs/Sent & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<22> & !iobs/Sent & !cs/nOverlay & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1

MACROCELL | 3 | 13 | EXP13_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 3 | 12
INPUTS | 17 | A_FSB<22>  | iobs/Sent  | cs/nOverlay  | nWE_FSB  | iobs/TS_FSM_FFd1  | iobs/TS_FSM_FFd2  | fsb/ASrf  | nADoutLE1  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<13>  | nAS_FSB  | A_FSB<14>
INPUTMC | 6 | 7 | 17 | 3 | 0 | 7 | 9 | 3 | 15 | 2 | 17 | 5 | 13
INPUTP | 11 | 30 | 47 | 29 | 28 | 26 | 24 | 23 | 22 | 18 | 54 | 19
EXPORTS | 1 | 3 | 12
EQ | 14 | 
       EXP13_.EXP  =  A_FSB<22> & !iobs/Sent & !cs/nOverlay & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<13> & !iobs/Sent & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<13> & !iobs/Sent & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<14> & !iobs/Sent & !nWE_FSB & 
	!nAS_FSB & !iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & nADoutLE1
	# A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & A_FSB<14> & !iobs/Sent & !nWE_FSB & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1

MACROCELL | 3 | 14 | EXP14_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 3 | 15
INPUTS | 9 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | iobs/TS_FSM_FFd2  | nADoutLE1  | A_FSB<20>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>
INPUTMC | 2 | 3 | 15 | 5 | 13
INPUTP | 7 | 36 | 30 | 29 | 28 | 24 | 23 | 22
EXPORTS | 1 | 3 | 15
EQ | 10 | 
       EXP14_.EXP  =  !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<20> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<18> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<17> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<16> & 
	!iobs/TS_FSM_FFd2 & nADoutLE1

MACROCELL | 3 | 17 | EXP15_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 3 | 16
INPUTS | 19 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<13>  | iobs/Sent  | nWE_FSB  | iobs/IORW1  | nAS_FSB  | iobs/TS_FSM_FFd1  | nADoutLE1  | iobs/TS_FSM_FFd2  | fsb/ASrf  | A_FSB<14>  | cs/nOverlay.EXP
INPUTMC | 7 | 7 | 17 | 3 | 16 | 7 | 9 | 5 | 13 | 3 | 15 | 2 | 17 | 3 | 0
INPUTP | 12 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 18 | 47 | 54 | 19
EXPORTS | 1 | 3 | 16
IMPORTS | 1 | 3 | 0
EQ | 25 | 
       EXP15_.EXP  =  !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & !nAS_FSB & 
	iobs/TS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & iobs/TS_FSM_FFd2 & 
	fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & !nAS_FSB & 
	iobs/TS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & iobs/TS_FSM_FFd1 & 
	fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & iobs/TS_FSM_FFd2 & 
	fsb/ASrf & nADoutLE1
;Imported pterms FB4_1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & iobs/IORW1 & iobs/TS_FSM_FFd1 & 
	fsb/ASrf & nADoutLE1

MACROCELL | 4 | 2 | EXP16_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 4 | 1
INPUTS | 5 | cs/nOverlay  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>
INPUTMC | 1 | 3 | 0
INPUTP | 4 | 36 | 30 | 29 | 28
EXPORTS | 1 | 4 | 1
EQ | 2 | 
       EXP16_.EXP  =  !cs/nOverlay
	# !A_FSB<23> & A_FSB<22> & !A_FSB<21> & !A_FSB<20>

MACROCELL | 4 | 3 | EXP17_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 4 | 4
INPUTS | 6 | RefUrg  | ram/RS_FSM_FFd4  | ram/RefDone  | ram/RS_FSM_FFd8  | ram/RS_FSM_FFd7  | RefReq
INPUTMC | 6 | 0 | 15 | 0 | 0 | 0 | 9 | 4 | 0 | 7 | 3 | 6 | 14
EXPORTS | 1 | 4 | 4
EQ | 5 | 
       EXP17_.EXP  =  !RefUrg & ram/RS_FSM_FFd4
	# ram/RefDone & ram/RS_FSM_FFd8
	# ram/RefDone & ram/RS_FSM_FFd4
	# ram/RefDone & ram/RS_FSM_FFd7
	# !RefUrg & !RefReq & ram/RS_FSM_FFd8

MACROCELL | 4 | 6 | EXP18_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 4 | 5
INPUTS | 5 | nWE_FSB  | nAS_FSB  | fsb/ASrf  | ram/DTACKr  | BACTr
INPUTMC | 3 | 2 | 17 | 1 | 7 | 7 | 13
INPUTP | 2 | 47 | 54
EXPORTS | 1 | 4 | 5
EQ | 3 | 
       EXP18_.EXP  =  !nWE_FSB
	# nAS_FSB & !fsb/ASrf
	# ram/DTACKr & BACTr

MACROCELL | 4 | 16 | EXP19_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 4 | 17
INPUTS | 10 | A_FSB<23>  | RefUrg  | ram/RefDone  | ram/RS_FSM_FFd8  | A_FSB<22>  | ram/RASEN  | nAS_FSB  | fsb/ASrf  | cs/nOverlay  | IONPReady.EXP
INPUTMC | 7 | 0 | 15 | 0 | 9 | 4 | 0 | 4 | 9 | 2 | 17 | 3 | 0 | 4 | 15
INPUTP | 3 | 36 | 30 | 54
EXPORTS | 1 | 4 | 17
IMPORTS | 1 | 4 | 15
EQ | 21 | 
       EXP19_.EXP  =  A_FSB<23> & RefUrg & !ram/RefDone & 
	ram/RS_FSM_FFd8
	# A_FSB<22> & RefUrg & !ram/RefDone & 
	ram/RS_FSM_FFd8
	# RefUrg & !ram/RefDone & ram/RS_FSM_FFd8 & 
	!ram/RASEN
	# RefUrg & !ram/RefDone & nAS_FSB & 
	ram/RS_FSM_FFd8 & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & !nAS_FSB & 
	ram/RS_FSM_FFd8 & ram/RASEN
;Imported pterms FB5_16
	# A_FSB<23> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<23> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay & 
	ram/RS_FSM_FFd8 & ram/RASEN & fsb/ASrf
	# A_FSB<22> & RefReq & !ram/RefDone & !nAS_FSB & 
	ram/RS_FSM_FFd8 & !BACTr
	# A_FSB<22> & RefReq & !ram/RefDone & 
	ram/RS_FSM_FFd8 & !BACTr & fsb/ASrf

MACROCELL | 7 | 0 | EXP20_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 7 | 17
INPUTS | 18 | A_FSB<22>  | iobs/Sent  | cs/nOverlay  | iobs/TS_FSM_FFd1  | iobs/TS_FSM_FFd2  | fsb/ASrf  | nADoutLE1  | A_FSB<23>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<13>  | nWE_FSB  | nAS_FSB  | A_FSB<14>
INPUTMC | 6 | 7 | 17 | 3 | 0 | 7 | 9 | 3 | 15 | 2 | 17 | 5 | 13
INPUTP | 12 | 30 | 36 | 29 | 28 | 26 | 24 | 23 | 22 | 18 | 47 | 54 | 19
EXPORTS | 1 | 7 | 17
EQ | 14 | 
       EXP20_.EXP  =  A_FSB<22> & !iobs/Sent & !cs/nOverlay & 
	!iobs/TS_FSM_FFd1 & !iobs/TS_FSM_FFd2 & fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & !nAS_FSB & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<13> & 
	!iobs/Sent & !nWE_FSB & fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & !nAS_FSB & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & A_FSB<14> & 
	!iobs/Sent & !nWE_FSB & fsb/ASrf & nADoutLE1

PIN | A_FSB<23> | 64 | 0 | N/A | 36 | 42 | 7 | 17 | 2 | 15 | 3 | 17 | 3 | 0 | 3 | 16 | 4 | 14 | 3 | 10 | 7 | 0 | 2 | 8 | 7 | 8 | 3 | 15 | 4 | 0 | 4 | 9 | 7 | 6 | 7 | 10 | 7 | 3 | 3 | 7 | 3 | 2 | 7 | 1 | 3 | 12 | 4 | 12 | 4 | 16 | 4 | 2 | 3 | 5 | 2 | 1 | 2 | 7 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 1 | 3 | 4 | 3 | 9 | 3 | 14 | 4 | 1 | 4 | 5 | 4 | 8 | 4 | 11 | 4 | 15 | 4 | 17 | 7 | 4 | 7 | 5 | 7 | 7
PIN | A_FSB<22> | 64 | 0 | N/A | 30 | 44 | 7 | 17 | 2 | 15 | 3 | 17 | 3 | 0 | 3 | 16 | 4 | 14 | 3 | 10 | 7 | 0 | 2 | 8 | 7 | 8 | 3 | 15 | 4 | 0 | 4 | 9 | 7 | 6 | 7 | 10 | 7 | 3 | 3 | 7 | 3 | 2 | 7 | 1 | 3 | 11 | 4 | 12 | 4 | 16 | 4 | 2 | 3 | 5 | 2 | 1 | 2 | 7 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 1 | 3 | 4 | 3 | 9 | 3 | 13 | 3 | 14 | 4 | 1 | 4 | 5 | 4 | 8 | 4 | 11 | 4 | 15 | 4 | 17 | 7 | 4 | 7 | 5 | 7 | 7 | 7 | 16
PIN | A_FSB<21> | 64 | 0 | N/A | 29 | 28 | 7 | 17 | 2 | 15 | 3 | 17 | 3 | 0 | 3 | 16 | 4 | 14 | 3 | 10 | 2 | 8 | 3 | 14 | 7 | 6 | 3 | 4 | 3 | 2 | 7 | 0 | 3 | 11 | 6 | 7 | 3 | 5 | 2 | 1 | 2 | 7 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 9 | 3 | 13 | 4 | 2 | 7 | 3 | 7 | 7 | 7 | 16
PIN | A_FSB<20> | 64 | 0 | N/A | 28 | 29 | 7 | 17 | 2 | 15 | 3 | 17 | 3 | 0 | 3 | 16 | 4 | 14 | 3 | 10 | 4 | 10 | 2 | 8 | 3 | 14 | 7 | 6 | 3 | 7 | 3 | 2 | 7 | 0 | 3 | 11 | 7 | 1 | 3 | 5 | 2 | 1 | 2 | 7 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 4 | 3 | 13 | 4 | 2 | 7 | 3 | 7 | 7 | 7 | 16
PIN | A_FSB<19> | 64 | 0 | N/A | 26 | 20 | 7 | 7 | 2 | 15 | 7 | 1 | 3 | 16 | 4 | 14 | 3 | 10 | 4 | 10 | 2 | 7 | 3 | 13 | 7 | 6 | 3 | 4 | 3 | 0 | 3 | 9 | 2 | 1 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 17 | 7 | 0
PIN | A_FSB<18> | 64 | 0 | N/A | 24 | 20 | 7 | 7 | 2 | 15 | 6 | 7 | 3 | 16 | 4 | 14 | 3 | 10 | 2 | 7 | 3 | 14 | 7 | 6 | 3 | 4 | 3 | 0 | 3 | 9 | 2 | 1 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 13 | 3 | 17 | 7 | 0
PIN | A_FSB<17> | 64 | 0 | N/A | 23 | 20 | 7 | 7 | 2 | 15 | 6 | 8 | 3 | 16 | 4 | 14 | 3 | 10 | 2 | 7 | 3 | 14 | 7 | 6 | 3 | 4 | 3 | 0 | 3 | 9 | 2 | 1 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 13 | 3 | 17 | 7 | 0
PIN | A_FSB<16> | 64 | 0 | N/A | 22 | 20 | 7 | 7 | 2 | 15 | 4 | 13 | 3 | 16 | 4 | 14 | 3 | 10 | 2 | 7 | 3 | 14 | 7 | 6 | 3 | 4 | 3 | 0 | 3 | 9 | 2 | 1 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 13 | 3 | 17 | 7 | 0
PIN | A_FSB<15> | 64 | 0 | N/A | 21 | 6 | 2 | 15 | 6 | 10 | 2 | 1 | 2 | 14 | 2 | 16 | 2 | 17
PIN | A_FSB<13> | 64 | 0 | N/A | 18 | 17 | 7 | 7 | 2 | 15 | 4 | 13 | 3 | 16 | 4 | 14 | 2 | 1 | 3 | 13 | 7 | 6 | 3 | 0 | 3 | 1 | 3 | 10 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 17 | 7 | 0
PIN | C8M | 8256 | 0 | N/A | 35 | 10 | 1 | 16 | 5 | 1 | 0 | 16 | 5 | 9 | 5 | 4 | 0 | 17 | 5 | 6 | 5 | 5 | 0 | 5 | 1 | 10
PIN | C16M | 4096 | 0 | N/A | 33 | 18 | 5 | 2 | 5 | 3 | 1 | 16 | 1 | 13 | 1 | 12 | 5 | 0 | 5 | 17 | 1 | 14 | 1 | 17 | 1 | 15 | 5 | 15 | 5 | 7 | 5 | 12 | 1 | 11 | 5 | 11 | 5 | 8 | 5 | 10 | 5 | 16
PIN | A_FSB<14> | 64 | 0 | N/A | 19 | 16 | 7 | 7 | 2 | 15 | 6 | 4 | 3 | 16 | 4 | 14 | 2 | 1 | 3 | 13 | 7 | 6 | 2 | 17 | 3 | 1 | 3 | 10 | 2 | 9 | 2 | 14 | 2 | 16 | 3 | 17 | 7 | 0
PIN | A_FSB<12> | 64 | 0 | N/A | 17 | 6 | 2 | 15 | 4 | 10 | 2 | 1 | 2 | 14 | 2 | 16 | 2 | 17
PIN | A_FSB<11> | 64 | 0 | N/A | 15 | 6 | 2 | 15 | 4 | 7 | 2 | 1 | 2 | 14 | 2 | 16 | 2 | 17
PIN | A_FSB<10> | 64 | 0 | N/A | 13 | 6 | 2 | 15 | 6 | 1 | 2 | 1 | 2 | 14 | 2 | 16 | 2 | 17
PIN | FCLK | 16384 | 0 | N/A | 42 | 76 | 7 | 17 | 2 | 15 | 2 | 0 | 0 | 13 | 6 | 15 | 6 | 17 | 0 | 15 | 2 | 1 | 6 | 16 | 3 | 0 | 6 | 14 | 6 | 13 | 2 | 9 | 2 | 7 | 2 | 6 | 2 | 5 | 2 | 4 | 2 | 3 | 6 | 9 | 6 | 6 | 6 | 3 | 2 | 14 | 6 | 12 | 6 | 0 | 3 | 16 | 0 | 9 | 4 | 15 | 6 | 2 | 0 | 12 | 0 | 11 | 7 | 11 | 3 | 10 | 7 | 14 | 2 | 8 | 7 | 8 | 7 | 9 | 3 | 15 | 4 | 0 | 0 | 7 | 0 | 14 | 0 | 0 | 4 | 9 | 0 | 3 | 4 | 7 | 1 | 9 | 7 | 6 | 1 | 7 | 0 | 10 | 7 | 10 | 7 | 3 | 3 | 8 | 3 | 3 | 2 | 13 | 2 | 12 | 2 | 11 | 0 | 2 | 0 | 1 | 7 | 13 | 7 | 2 | 3 | 12 | 0 | 8 | 2 | 10 | 0 | 6 | 7 | 12 | 4 | 12 | 2 | 2 | 7 | 15 | 1 | 8 | 7 | 16 | 4 | 17 | 4 | 5 | 5 | 13 | 3 | 1 | 2 | 17 | 0 | 4 | 4 | 4
PIN | nAS_FSB | 64 | 0 | N/A | 54 | 42 | 7 | 17 | 2 | 15 | 3 | 5 | 3 | 0 | 2 | 14 | 3 | 16 | 4 | 14 | 7 | 11 | 3 | 10 | 4 | 17 | 2 | 8 | 7 | 8 | 3 | 15 | 3 | 17 | 4 | 8 | 4 | 7 | 7 | 6 | 7 | 10 | 7 | 0 | 3 | 7 | 3 | 2 | 2 | 13 | 2 | 12 | 2 | 11 | 7 | 13 | 7 | 1 | 3 | 12 | 2 | 10 | 4 | 11 | 2 | 17 | 4 | 16 | 2 | 16 | 4 | 1 | 3 | 13 | 3 | 11 | 4 | 5 | 4 | 6 | 4 | 15 | 7 | 4 | 7 | 5 | 7 | 7 | 7 | 16
PIN | nWE_FSB | 64 | 0 | N/A | 47 | 23 | 7 | 0 | 2 | 15 | 7 | 7 | 3 | 16 | 4 | 14 | 2 | 1 | 3 | 15 | 7 | 6 | 3 | 7 | 3 | 2 | 7 | 2 | 3 | 12 | 2 | 16 | 3 | 17 | 3 | 5 | 7 | 5 | 2 | 9 | 2 | 14 | 2 | 17 | 3 | 0 | 3 | 11 | 3 | 13 | 4 | 6
PIN | A_FSB<9> | 64 | 0 | N/A | 12 | 6 | 2 | 15 | 6 | 5 | 2 | 1 | 2 | 14 | 2 | 16 | 2 | 17
PIN | A_FSB<8> | 64 | 0 | N/A | 11 | 5 | 2 | 14 | 6 | 10 | 2 | 1 | 2 | 16 | 2 | 17
PIN | nBERR_IOB | 64 | 0 | N/A | 123 | 1 | 0 | 16
PIN | nDTACK_IOB | 64 | 0 | N/A | 127 | 1 | 5 | 9
PIN | nLDS_FSB | 64 | 0 | N/A | 49 | 3 | 0 | 12 | 3 | 8 | 7 | 5
PIN | nUDS_FSB | 64 | 0 | N/A | 56 | 3 | 0 | 11 | 3 | 3 | 7 | 7
PIN | E | 64 | 0 | N/A | 37 | 6 | 5 | 4 | 0 | 17 | 5 | 6 | 5 | 5 | 0 | 8 | 0 | 5
PIN | nIPL2 | 64 | 0 | N/A | 146 | 1 | 0 | 6
PIN | nVPA_IOB | 64 | 0 | N/A | 125 | 1 | 1 | 10
PIN | A_FSB<1> | 64 | 0 | N/A | 149 | 1 | 6 | 5
PIN | A_FSB<7> | 64 | 0 | N/A | 8 | 2 | 6 | 8 | 4 | 13
PIN | A_FSB<2> | 64 | 0 | N/A | 153 | 1 | 6 | 1
PIN | A_FSB<3> | 64 | 0 | N/A | 155 | 1 | 4 | 7
PIN | A_FSB<4> | 64 | 0 | N/A | 157 | 1 | 4 | 10
PIN | A_FSB<5> | 64 | 0 | N/A | 4 | 1 | 4 | 13
PIN | A_FSB<6> | 64 | 0 | N/A | 6 | 1 | 6 | 4
PIN | nVMA_IOB | 536871040 | 0 | N/A | 118
PIN | nAS_IOB | 536871040 | 0 | N/A | 135
PIN | nLDS_IOB | 536871040 | 0 | N/A | 130
PIN | nUDS_IOB | 536871040 | 0 | N/A | 134
PIN | nBERR_FSB | 536871040 | 0 | N/A | 112
PIN | nVPA_FSB | 536871040 | 0 | N/A | 147
PIN | nRAS | 536871040 | 0 | N/A | 103
PIN | nBR_IOB | 536871040 | 0 | N/A | 116
PIN | RA<3> | 536871040 | 0 | N/A | 64
PIN | nDTACK_FSB | 536871040 | 0 | N/A | 44
PIN | RA<0> | 536871040 | 0 | N/A | 86
PIN | RA<10> | 536871040 | 0 | N/A | 90
PIN | RA<1> | 536871040 | 0 | N/A | 79
PIN | RA<2> | 536871040 | 0 | N/A | 69
PIN | RA<4> | 536871040 | 0 | N/A | 63
PIN | RA<5> | 536871040 | 0 | N/A | 68
PIN | RA<6> | 536871040 | 0 | N/A | 72
PIN | RA<7> | 536871040 | 0 | N/A | 82
PIN | RA<8> | 536871040 | 0 | N/A | 88
PIN | RA<9> | 536871040 | 0 | N/A | 92
PIN | nROMWE | 536871040 | 0 | N/A | 57
PIN | nADoutLE0 | 536871040 | 0 | N/A | 139
PIN | nCAS | 536871040 | 0 | N/A | 59
PIN | nDinLE | 536871040 | 0 | N/A | 140
PIN | nOE | 536871040 | 0 | N/A | 60
PIN | RA<11> | 536871040 | 0 | N/A | 102
PIN | nADoutLE1 | 536871040 | 0 | N/A | 136
PIN | nAoutOE | 536871040 | 0 | N/A | 141
PIN | nDinOE | 536871040 | 0 | N/A | 144
PIN | nDoutOE | 536871040 | 0 | N/A | 143
PIN | nRAMLWE | 536871040 | 0 | N/A | 104
PIN | nRAMUWE | 536871040 | 0 | N/A | 105
PIN | nROMCS | 536871040 | 0 | N/A | 58
PIN | C25MEN | 536871040 | 0 | N/A | 95
PIN | nRES | 536870976 | 0 | N/A | 145 | 2 | 5 | 9 | 3 | 0
