# Timing report for WarpSE
Author: Copyright (c) 1995-2013 Xilinx, Inc. All rights reserved.

# Timing Report

Need help reading this report?

Design Name | WarpSE
Device, Speed (SpeedFile Version) | XC95144XL, -10 (3.0)
Date Created | Mon Mar 28 09:47:06 2022
Created By | Timing Report Generator: version P.20131013
Copyright | Copyright (c) 1995-2013 Xilinx, Inc. All rights reserved.

## Summary

Performance Summary
Min. Clock Period | 19.500 ns.
Max. Clock Frequency (fSYSTEM) | 51.282 MHz.
Limited by Cycle Time for CLK_FSB
Clock to Setup (tCYC) | 19.500 ns.
Pad to Pad Delay (tPD) | 11.000 ns.
Setup to Clock at the Pad (tSU) | 16.000 ns.
Clock Pad to Output Pad Delay (tCO) | 14.500 ns.

## Timing Constraints

Constraint Name | Requirement (ns) | Delay (ns) | Paths | Paths Failing
--- | --- | --- | --- | ---
TS_CLK_IOB | 142.8 | 0.0 | 0 | 0
TS_CLK_FSB | 40.0 | 19.5 | 291 | 0
TS_CLK2X_IOB | 66.6 | 11.0 | 105 | 0

### Constraint: TS_CLK_IOB

Description: PERIOD:CLK_IOB:142.857nS:HIGH:71.428nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---

### Constraint: TS_CLK_FSB

Description: PERIOD:CLK_FSB:40.000nS:HIGH:20.000nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---
fsb/ASrf.Q to fsb/VPA.D | 20.000 | 19.500 | 0.500
cnt/TimeoutA.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
cnt/TimeoutB.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
cnt/TimeoutB.Q to nDTACK_FSB.D | 40.000 | 11.800 | 28.200
cs/nOverlay1.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
fsb/ASrf.Q to nDTACK_FSB.D | 20.000 | 11.800 | 8.200
fsb/BERR0r.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
fsb/BERR0r.Q to nDTACK_FSB.D | 40.000 | 11.800 | 28.200
fsb/BERR1r.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
fsb/BERR1r.Q to nDTACK_FSB.D | 40.000 | 11.800 | 28.200
fsb/Ready1r.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
fsb/Ready1r.Q to nDTACK_FSB.D | 40.000 | 11.800 | 28.200
fsb/Ready2r.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
fsb/VPA.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
iobs/BERR.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
iobs/BERR.Q to nDTACK_FSB.D | 40.000 | 11.800 | 28.200
iobs/IOReady.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
iobs/IOReady.Q to nDTACK_FSB.D | 40.000 | 11.800 | 28.200
nBR_IOB.Q to fsb/VPA.D | 40.000 | 11.800 | 28.200
nBR_IOB.Q to nDTACK_FSB.D | 40.000 | 11.800 | 28.200
cnt/RefCnt<5>.Q to ram/RAMDIS1.D | 40.000 | 11.400 | 28.600
cnt/RefCnt<5>.Q to ram/RASEL.D | 40.000 | 11.400 | 28.600
cnt/RefCnt<6>.Q to ram/RAMDIS1.D | 40.000 | 11.400 | 28.600
cnt/RefCnt<6>.Q to ram/RASEL.D | 40.000 | 11.400 | 28.600
cnt/RefCnt<7>.Q to ram/RAMDIS1.D | 40.000 | 11.400 | 28.600
cnt/RefCnt<7>.Q to ram/RASEL.D | 40.000 | 11.400 | 28.600
cnt/RefDone.Q to ram/RAMDIS1.D | 40.000 | 11.400 | 28.600
cnt/RefDone.Q to ram/RASEL.D | 40.000 | 11.400 | 28.600
cs/nOverlay1.Q to fsb/Ready1r.D | 40.000 | 11.400 | 28.600
cs/nOverlay1.Q to iobs/IORW1.D | 40.000 | 11.400 | 28.600
cs/nOverlay1.Q to iobs/Once.D | 40.000 | 11.400 | 28.600
cs/nOverlay1.Q to nDTACK_FSB.D | 40.000 | 11.400 | 28.600
cs/nOverlay1.Q to ram/RAMDIS1.D | 40.000 | 11.400 | 28.600
cs/nOverlay1.Q to ram/RASEL.D | 40.000 | 11.400 | 28.600
fsb/ASrf.Q to ram/RASEL.D | 20.000 | 11.400 | 8.600
fsb/Ready0r.Q to nDTACK_FSB.D | 40.000 | 11.400 | 28.600
fsb/Ready1r.Q to fsb/Ready1r.D | 40.000 | 11.400 | 28.600
iobs/IORW0.Q to iobs/IORW0.D | 40.000 | 11.400 | 28.600
iobs/IOReady.Q to fsb/Ready1r.D | 40.000 | 11.400 | 28.600
iobs/Once.Q to iobs/IORW0.D | 40.000 | 11.400 | 28.600
iobs/Once.Q to iobs/Once.D | 40.000 | 11.400 | 28.600
iobs/PS_FSM_FFd1.Q to iobs/IORW0.D | 40.000 | 11.400 | 28.600
iobs/PS_FSM_FFd2.Q to iobs/IORW0.D | 40.000 | 11.400 | 28.600
nADoutLE1.Q to fsb/Ready1r.D | 40.000 | 11.400 | 28.600
nADoutLE1.Q to fsb/VPA.D | 40.000 | 11.400 | 28.600
nADoutLE1.Q to iobs/IORW0.D | 40.000 | 11.400 | 28.600
nDTACK_FSB.Q to nDTACK_FSB.D | 40.000 | 11.400 | 28.600
ram/Once.Q to ram/RASEL.D | 40.000 | 11.400 | 28.600
ram/RAMReady.Q to nDTACK_FSB.D | 40.000 | 11.400 | 28.600
ram/RS_FSM_FFd1.Q to ram/RAMDIS1.D | 40.000 | 11.400 | 28.600
ram/RS_FSM_FFd1.Q to ram/RASEL.D | 40.000 | 11.400 | 28.600
ram/RS_FSM_FFd2.Q to ram/RASEL.D | 40.000 | 11.400 | 28.600
ram/RS_FSM_FFd3.Q to ram/RAMDIS1.D | 40.000 | 11.400 | 28.600
cnt/RefCnt<5>.Q to ram/RAMDIS2.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<5>.Q to ram/RS_FSM_FFd1.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<5>.Q to ram/RS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<5>.Q to ram/RS_FSM_FFd3.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<6>.Q to ram/RAMDIS2.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<6>.Q to ram/RS_FSM_FFd1.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<6>.Q to ram/RS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<6>.Q to ram/RS_FSM_FFd3.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<7>.Q to ram/RAMDIS2.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<7>.Q to ram/RS_FSM_FFd1.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<7>.Q to ram/RS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
cnt/RefCnt<7>.Q to ram/RS_FSM_FFd3.D | 40.000 | 11.000 | 29.000
cnt/RefDone.Q to ram/RAMDIS2.D | 40.000 | 11.000 | 29.000
cnt/RefDone.Q to ram/RAMReady.D | 40.000 | 11.000 | 29.000
cnt/RefDone.Q to ram/RS_FSM_FFd1.D | 40.000 | 11.000 | 29.000
cnt/RefDone.Q to ram/RS_FSM_FFd3.D | 40.000 | 11.000 | 29.000
cnt/TimeoutA.Q to fsb/Ready2r.D | 40.000 | 11.000 | 29.000
cnt/TimeoutA.Q to nDTACK_FSB.D | 40.000 | 11.000 | 29.000
cs/nOverlay1.Q to fsb/Ready2r.D | 40.000 | 11.000 | 29.000
cs/nOverlay1.Q to iobs/IOREQ.D | 40.000 | 11.000 | 29.000
cs/nOverlay1.Q to iobs/Load1.D | 40.000 | 11.000 | 29.000
cs/nOverlay1.Q to iobs/PS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
cs/nOverlay1.Q to ram/RAMDIS2.D | 40.000 | 11.000 | 29.000
cs/nOverlay1.Q to ram/RAMReady.D | 40.000 | 11.000 | 29.000
cs/nOverlay1.Q to ram/RS_FSM_FFd1.D | 40.000 | 11.000 | 29.000
cs/nOverlay1.Q to ram/RS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
cs/nOverlay1.Q to ram/RS_FSM_FFd3.D | 40.000 | 11.000 | 29.000
fsb/ASrf.Q to fsb/Ready0r.D | 20.000 | 11.000 | 9.000
fsb/ASrf.Q to fsb/Ready2r.D | 20.000 | 11.000 | 9.000
fsb/ASrf.Q to iobs/IORW0.D | 20.000 | 11.000 | 9.000
fsb/ASrf.Q to iobs/IORW1.D | 20.000 | 11.000 | 9.000
fsb/ASrf.Q to ram/RAMDIS1.D | 20.000 | 11.000 | 9.000
fsb/ASrf.Q to ram/RAMDIS2.D | 20.000 | 11.000 | 9.000
fsb/ASrf.Q to ram/RAMReady.D | 20.000 | 11.000 | 9.000
fsb/ASrf.Q to ram/RS_FSM_FFd1.D | 20.000 | 11.000 | 9.000
fsb/ASrf.Q to ram/RS_FSM_FFd2.D | 20.000 | 11.000 | 9.000
fsb/ASrf.Q to ram/RS_FSM_FFd3.D | 20.000 | 11.000 | 9.000
fsb/Ready0r.Q to fsb/VPA.D | 40.000 | 11.000 | 29.000
fsb/Ready2r.Q to fsb/Ready2r.D | 40.000 | 11.000 | 29.000
fsb/Ready2r.Q to nDTACK_FSB.D | 40.000 | 11.000 | 29.000
iobs/IORW1.Q to iobs/IORW0.D | 40.000 | 11.000 | 29.000
iobs/PS_FSM_FFd1.Q to iobs/IORW1.D | 40.000 | 11.000 | 29.000
iobs/PS_FSM_FFd1.Q to iobs/Once.D | 40.000 | 11.000 | 29.000
iobs/PS_FSM_FFd1.Q to iobs/PS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
iobs/PS_FSM_FFd2.Q to iobs/IOREQ.D | 40.000 | 11.000 | 29.000
iobs/PS_FSM_FFd2.Q to iobs/IORW1.D | 40.000 | 11.000 | 29.000
iobs/PS_FSM_FFd2.Q to iobs/PS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
nADoutLE1.Q to iobs/IOREQ.D | 40.000 | 11.000 | 29.000
nADoutLE1.Q to iobs/Once.D | 40.000 | 11.000 | 29.000
nADoutLE1.Q to iobs/PS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
nADoutLE1.Q to nDTACK_FSB.D | 40.000 | 11.000 | 29.000
ram/BACTr.Q to ram/RAMDIS1.D | 40.000 | 11.000 | 29.000
ram/BACTr.Q to ram/RAMReady.D | 40.000 | 11.000 | 29.000
ram/BACTr.Q to ram/RASEL.D | 40.000 | 11.000 | 29.000
ram/BACTr.Q to ram/RS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
ram/Once.Q to ram/RAMDIS1.D | 40.000 | 11.000 | 29.000
ram/Once.Q to ram/RAMDIS2.D | 40.000 | 11.000 | 29.000
ram/Once.Q to ram/RAMReady.D | 40.000 | 11.000 | 29.000
ram/Once.Q to ram/RS_FSM_FFd1.D | 40.000 | 11.000 | 29.000
ram/RAMDIS2.Q to ram/RAMDIS2.D | 40.000 | 11.000 | 29.000
ram/RAMReady.Q to fsb/VPA.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd1.Q to ram/RAMReady.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd1.Q to ram/RS_FSM_FFd1.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd1.Q to ram/RS_FSM_FFd3.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd2.Q to ram/RAMDIS2.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd2.Q to ram/RS_FSM_FFd1.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd2.Q to ram/RS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd2.Q to ram/RS_FSM_FFd3.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd3.Q to ram/RAMDIS2.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd3.Q to ram/RS_FSM_FFd2.D | 40.000 | 11.000 | 29.000
ram/RS_FSM_FFd3.Q to ram/RS_FSM_FFd3.D | 40.000 | 11.000 | 29.000
IPL2r0.Q to IPL2r1.D | 40.000 | 10.000 | 30.000
IPL2r0.Q to nBR_IOB.CE | 40.000 | 10.000 | 30.000
IPL2r1.Q to nBR_IOB.CE | 40.000 | 10.000 | 30.000
RESDone.Q to nBR_IOB.CE | 40.000 | 10.000 | 30.000
RESr0.Q to RESDone.CE | 40.000 | 10.000 | 30.000
RESr0.Q to RESr1.D | 40.000 | 10.000 | 30.000
RESr0.Q to nBR_IOB.CE | 40.000 | 10.000 | 30.000
RESr1.Q to RESDone.CE | 40.000 | 10.000 | 30.000
RESr1.Q to RESr2.D | 40.000 | 10.000 | 30.000
RESr1.Q to nBR_IOB.CE | 40.000 | 10.000 | 30.000
RESr2.Q to RESDone.CE | 40.000 | 10.000 | 30.000
RESr2.Q to nBR_IOB.CE | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/RefCnt<1>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/RefCnt<2>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/RefCnt<3>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/RefCnt<4>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/RefCnt<5>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/RefCnt<6>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/RefCnt<7>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/TimeoutA.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<0>.Q to cnt/TimeoutBPre.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/RefCnt<2>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/RefCnt<3>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/RefCnt<4>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/RefCnt<5>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/RefCnt<6>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/RefCnt<7>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/TimeoutA.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<1>.Q to cnt/TimeoutBPre.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<2>.Q to cnt/RefCnt<3>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<2>.Q to cnt/RefCnt<4>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<2>.Q to cnt/RefCnt<5>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<2>.Q to cnt/RefCnt<6>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<2>.Q to cnt/RefCnt<7>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<2>.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<2>.Q to cnt/TimeoutA.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<2>.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<2>.Q to cnt/TimeoutBPre.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<3>.Q to cnt/RefCnt<4>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<3>.Q to cnt/RefCnt<5>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<3>.Q to cnt/RefCnt<6>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<3>.Q to cnt/RefCnt<7>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<3>.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<3>.Q to cnt/TimeoutA.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<3>.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<3>.Q to cnt/TimeoutBPre.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<4>.Q to cnt/RefCnt<5>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<4>.Q to cnt/RefCnt<6>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<4>.Q to cnt/RefCnt<7>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<4>.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<4>.Q to cnt/TimeoutA.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<4>.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<4>.Q to cnt/TimeoutBPre.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<5>.Q to cnt/RefCnt<6>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<5>.Q to cnt/RefCnt<7>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<5>.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<5>.Q to cnt/TimeoutA.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<5>.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<5>.Q to cnt/TimeoutBPre.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<5>.Q to ram/RAMReady.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<6>.Q to cnt/RefCnt<7>.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<6>.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<6>.Q to cnt/TimeoutA.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<6>.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<6>.Q to cnt/TimeoutBPre.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<6>.Q to ram/RAMReady.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<7>.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<7>.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<7>.Q to cnt/TimeoutBPre.D | 40.000 | 10.000 | 30.000
cnt/RefCnt<7>.Q to ram/RAMReady.D | 40.000 | 10.000 | 30.000
cnt/RefDone.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000
cnt/RefDone.Q to ram/RS_FSM_FFd2.D | 40.000 | 10.000 | 30.000
cnt/TimeoutA.Q to cnt/TimeoutA.D | 40.000 | 10.000 | 30.000
cnt/TimeoutB.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/TimeoutB.Q to fsb/BERR0r.D | 40.000 | 10.000 | 30.000
cnt/TimeoutBPre.Q to cnt/TimeoutB.D | 40.000 | 10.000 | 30.000
cnt/TimeoutBPre.Q to cnt/TimeoutBPre.D | 40.000 | 10.000 | 30.000
cs/nOverlay0.Q to cs/nOverlay0.D | 40.000 | 10.000 | 30.000
cs/nOverlay0.Q to cs/nOverlay1.D | 40.000 | 10.000 | 30.000
cs/nOverlay1.Q to fsb/Ready0r.D | 40.000 | 10.000 | 30.000
cs/nOverlay1.Q to iobs/IORW0.D | 40.000 | 10.000 | 30.000
cs/nOverlay1.Q to ram/Once.D | 40.000 | 10.000 | 30.000
fsb/ASrf.Q to cnt/TimeoutA.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to cnt/TimeoutB.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to cnt/TimeoutBPre.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to cs/nOverlay0.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to cs/nOverlay1.CE | 40.000 | 10.000 | 30.000
fsb/ASrf.Q to fsb/BERR0r.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to fsb/BERR1r.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to fsb/Ready1r.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to iobs/BERR.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to iobs/IOREQ.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to iobs/IOReady.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to iobs/Load1.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to iobs/Once.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to iobs/PS_FSM_FFd2.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to ram/BACTr.D | 20.000 | 10.000 | 10.000
fsb/ASrf.Q to ram/Once.D | 20.000 | 10.000 | 10.000
fsb/BERR0r.Q to fsb/BERR0r.D | 40.000 | 10.000 | 30.000
fsb/BERR1r.Q to fsb/BERR1r.D | 40.000 | 10.000 | 30.000
fsb/Ready0r.Q to fsb/Ready0r.D | 40.000 | 10.000 | 30.000
iobs/BERR.Q to fsb/BERR1r.D | 40.000 | 10.000 | 30.000
iobs/BERR.Q to iobs/BERR.D | 40.000 | 10.000 | 30.000
iobs/Clear1.Q to nADoutLE1.D | 40.000 | 10.000 | 30.000
iobs/IOACTr.Q to iobs/BERR.D | 40.000 | 10.000 | 30.000
iobs/IOACTr.Q to iobs/IOREQ.D | 40.000 | 10.000 | 30.000
iobs/IOACTr.Q to iobs/IOReady.D | 40.000 | 10.000 | 30.000
iobs/IOACTr.Q to iobs/PS_FSM_FFd1.D | 40.000 | 10.000 | 30.000
iobs/IOACTr.Q to iobs/PS_FSM_FFd2.D | 40.000 | 10.000 | 30.000
iobs/IOL1.Q to iobs/IOL0.D | 40.000 | 10.000 | 30.000
iobs/IORW1.Q to iobs/IORW1.D | 40.000 | 10.000 | 30.000
iobs/IOReady.Q to iobs/IOReady.D | 40.000 | 10.000 | 30.000
iobs/IOU1.Q to iobs/IOU0.D | 40.000 | 10.000 | 30.000
iobs/Load1.Q to iobs/IOL1.CE | 40.000 | 10.000 | 30.000
iobs/Load1.Q to iobs/IOU1.CE | 40.000 | 10.000 | 30.000
iobs/Load1.Q to nADoutLE1.D | 40.000 | 10.000 | 30.000
iobs/Once.Q to iobs/BERR.D | 40.000 | 10.000 | 30.000
iobs/Once.Q to iobs/IOREQ.D | 40.000 | 10.000 | 30.000
iobs/Once.Q to iobs/IORW1.D | 40.000 | 10.000 | 30.000
iobs/Once.Q to iobs/IOReady.D | 40.000 | 10.000 | 30.000
iobs/Once.Q to iobs/Load1.D | 40.000 | 10.000 | 30.000
iobs/Once.Q to iobs/PS_FSM_FFd2.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd1.Q to iobs/ALE0.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd1.Q to iobs/Clear1.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd1.Q to iobs/IOL0.CE | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd1.Q to iobs/IOREQ.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd1.Q to iobs/IOU0.CE | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd1.Q to iobs/Load1.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd1.Q to iobs/PS_FSM_FFd1.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd2.Q to iobs/ALE0.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd2.Q to iobs/BERR.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd2.Q to iobs/Clear1.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd2.Q to iobs/IOL0.CE | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd2.Q to iobs/IOReady.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd2.Q to iobs/IOU0.CE | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd2.Q to iobs/Load1.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd2.Q to iobs/Once.D | 40.000 | 10.000 | 30.000
iobs/PS_FSM_FFd2.Q to iobs/PS_FSM_FFd1.D | 40.000 | 10.000 | 30.000
nADoutLE1.Q to iobs/BERR.D | 40.000 | 10.000 | 30.000
nADoutLE1.Q to iobs/Clear1.D | 40.000 | 10.000 | 30.000
nADoutLE1.Q to iobs/IOL0.D | 40.000 | 10.000 | 30.000
nADoutLE1.Q to iobs/IORW1.D | 40.000 | 10.000 | 30.000
nADoutLE1.Q to iobs/IOReady.D | 40.000 | 10.000 | 30.000
nADoutLE1.Q to iobs/IOU0.D | 40.000 | 10.000 | 30.000
nADoutLE1.Q to iobs/Load1.D | 40.000 | 10.000 | 30.000
nADoutLE1.Q to nADoutLE1.D | 40.000 | 10.000 | 30.000
ram/Once.Q to ram/Once.D | 40.000 | 10.000 | 30.000
ram/Once.Q to ram/RS_FSM_FFd3.D | 40.000 | 10.000 | 30.000
ram/RAMReady.Q to fsb/Ready0r.D | 40.000 | 10.000 | 30.000
ram/RASEL.Q to nCAS.D | 20.000 | 10.000 | 10.000
ram/RS_FSM_FFd1.Q to ram/Once.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd1.Q to ram/RAMDIS2.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd1.Q to ram/RS_FSM_FFd2.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd1.Q to ram/RefRAS.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd2.Q to ram/Once.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd2.Q to ram/RAMDIS1.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd2.Q to ram/RAMReady.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd2.Q to ram/RefRAS.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd3.Q to ram/Once.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd3.Q to ram/RAMReady.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd3.Q to ram/RASEL.D | 40.000 | 10.000 | 30.000
ram/RS_FSM_FFd3.Q to ram/RS_FSM_FFd1.D | 40.000 | 10.000 | 30.000
ram/RefRAS.Q to cnt/RefDone.D | 40.000 | 10.000 | 30.000

### Constraint: TS_CLK2X_IOB

Description: PERIOD:CLK2X_IOB:66.666nS:HIGH:33.333nS
Path | Requirement (ns) | Delay (ns) | Slack (ns)
--- | --- | --- | ---
iobm/BERRrf.Q to iobm/IOBERR.D | 33.300 | 11.000 | 22.300
iobm/BERRrr.Q to iobm/IOBERR.D | 66.600 | 11.000 | 55.600
iobm/DTACKrf.Q to iobm/IOACT.D | 33.300 | 11.000 | 22.300
iobm/DTACKrf.Q to iobm/IOBERR.D | 33.300 | 11.000 | 22.300
iobm/DTACKrr.Q to iobm/IOACT.D | 66.600 | 11.000 | 55.600
iobm/DTACKrr.Q to iobm/IOBERR.D | 66.600 | 11.000 | 55.600
iobm/IOBERR.Q to iobm/IOBERR.D | 66.600 | 11.000 | 55.600
iobm/IOS_FSM_FFd1.Q to iobm/IOACT.D | 66.600 | 11.000 | 55.600
iobm/IOS_FSM_FFd1.Q to iobm/IOBERR.D | 66.600 | 11.000 | 55.600
iobm/IOS_FSM_FFd2.Q to iobm/IOBERR.D | 66.600 | 11.000 | 55.600
iobm/IOS_FSM_FFd3.Q to iobm/IOACT.D | 66.600 | 11.000 | 55.600
iobm/IOS_FSM_FFd3.Q to iobm/IOBERR.D | 66.600 | 11.000 | 55.600
iobm/RESrf.Q to iobm/IOACT.D | 33.300 | 11.000 | 22.300
iobm/RESrf.Q to iobm/IOBERR.D | 33.300 | 11.000 | 22.300
iobm/RESrr.Q to iobm/IOACT.D | 66.600 | 11.000 | 55.600
iobm/RESrr.Q to iobm/IOBERR.D | 66.600 | 11.000 | 55.600
iobm/BERRrf.Q to iobm/IOACT.D | 33.300 | 10.000 | 23.300
iobm/BERRrf.Q to iobm/IOS_FSM_FFd2.D | 33.300 | 10.000 | 23.300
iobm/BERRrr.Q to iobm/IOACT.D | 66.600 | 10.000 | 56.600
iobm/BERRrr.Q to iobm/IOS_FSM_FFd2.D | 66.600 | 10.000 | 56.600
iobm/BGr0.Q to iobm/BGr1.D | 66.600 | 10.000 | 56.600
iobm/BGr0.Q to nAoutOE.D | 66.600 | 10.000 | 56.600
iobm/BGr1.Q to nAoutOE.D | 66.600 | 10.000 | 56.600
iobm/DTACKrf.Q to iobm/IOS_FSM_FFd2.D | 33.300 | 10.000 | 23.300
iobm/DTACKrr.Q to iobm/IOS_FSM_FFd2.D | 66.600 | 10.000 | 56.600
iobm/ES<0>.Q to iobm/ES<0>.D | 66.600 | 10.000 | 56.600
iobm/ES<0>.Q to iobm/ES<1>.D | 66.600 | 10.000 | 56.600
iobm/ES<0>.Q to iobm/ES<2>.D | 66.600 | 10.000 | 56.600
iobm/ES<0>.Q to iobm/ES<3>.D | 66.600 | 10.000 | 56.600
iobm/ES<0>.Q to iobm/ES<4>.D | 66.600 | 10.000 | 56.600
iobm/ES<0>.Q to iobm/ETACK.D | 66.600 | 10.000 | 56.600
iobm/ES<0>.Q to nVMA_IOB.D | 66.600 | 10.000 | 56.600
iobm/ES<1>.Q to iobm/ES<0>.D | 66.600 | 10.000 | 56.600
iobm/ES<1>.Q to iobm/ES<1>.D | 66.600 | 10.000 | 56.600
iobm/ES<1>.Q to iobm/ES<2>.D | 66.600 | 10.000 | 56.600
iobm/ES<1>.Q to iobm/ES<3>.D | 66.600 | 10.000 | 56.600
iobm/ES<1>.Q to iobm/ES<4>.D | 66.600 | 10.000 | 56.600
iobm/ES<1>.Q to iobm/ETACK.D | 66.600 | 10.000 | 56.600
iobm/ES<1>.Q to nVMA_IOB.D | 66.600 | 10.000 | 56.600
iobm/ES<2>.Q to iobm/ES<0>.D | 66.600 | 10.000 | 56.600
iobm/ES<2>.Q to iobm/ES<2>.D | 66.600 | 10.000 | 56.600
iobm/ES<2>.Q to iobm/ES<3>.D | 66.600 | 10.000 | 56.600
iobm/ES<2>.Q to iobm/ES<4>.D | 66.600 | 10.000 | 56.600
iobm/ES<2>.Q to iobm/ETACK.D | 66.600 | 10.000 | 56.600
iobm/ES<2>.Q to nVMA_IOB.D | 66.600 | 10.000 | 56.600
iobm/ES<3>.Q to iobm/ES<0>.D | 66.600 | 10.000 | 56.600
iobm/ES<3>.Q to iobm/ES<2>.D | 66.600 | 10.000 | 56.600
iobm/ES<3>.Q to iobm/ES<3>.D | 66.600 | 10.000 | 56.600
iobm/ES<3>.Q to iobm/ES<4>.D | 66.600 | 10.000 | 56.600
iobm/ES<3>.Q to iobm/ETACK.D | 66.600 | 10.000 | 56.600
iobm/ES<3>.Q to nVMA_IOB.D | 66.600 | 10.000 | 56.600
iobm/ES<4>.Q to iobm/ES<0>.D | 66.600 | 10.000 | 56.600
iobm/ES<4>.Q to iobm/ES<2>.D | 66.600 | 10.000 | 56.600
iobm/ES<4>.Q to iobm/ES<4>.D | 66.600 | 10.000 | 56.600
iobm/ES<4>.Q to iobm/ETACK.D | 66.600 | 10.000 | 56.600
iobm/ES<4>.Q to nVMA_IOB.D | 66.600 | 10.000 | 56.600
iobm/ETACK.Q to iobm/IOACT.D | 66.600 | 10.000 | 56.600
iobm/ETACK.Q to iobm/IOBERR.D | 66.600 | 10.000 | 56.600
iobm/ETACK.Q to iobm/IOS_FSM_FFd2.D | 66.600 | 10.000 | 56.600
iobm/Er2.Q to iobm/ES<0>.D | 66.600 | 10.000 | 56.600
iobm/Er2.Q to iobm/ES<1>.D | 66.600 | 10.000 | 56.600
iobm/Er2.Q to iobm/ES<2>.D | 66.600 | 10.000 | 56.600
iobm/Er2.Q to iobm/ES<3>.D | 66.600 | 10.000 | 56.600
iobm/Er2.Q to iobm/ES<4>.D | 66.600 | 10.000 | 56.600
iobm/IOACT.Q to nVMA_IOB.D | 66.600 | 10.000 | 56.600
iobm/IOREQr.Q to iobm/ALE0.D | 33.300 | 10.000 | 23.300
iobm/IOREQr.Q to iobm/IOACT.D | 33.300 | 10.000 | 23.300
iobm/IOREQr.Q to iobm/IOS_FSM_FFd3.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd1.Q to iobm/ALE0.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd1.Q to iobm/IOS_FSM_FFd1.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd1.Q to iobm/IOS_FSM_FFd2.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd1.Q to iobm/IOS_FSM_FFd3.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd1.Q to nAS_IOB.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd1.Q to nDinLE.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd1.Q to nLDS_IOB.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd1.Q to nUDS_IOB.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd2.Q to iobm/ALE0.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd2.Q to iobm/IOACT.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd2.Q to iobm/IOS_FSM_FFd1.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd2.Q to iobm/IOS_FSM_FFd2.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd2.Q to iobm/IOS_FSM_FFd3.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd2.Q to nAS_IOB.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd2.Q to nDinLE.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd2.Q to nDoutOE.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd2.Q to nLDS_IOB.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd2.Q to nUDS_IOB.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd3.Q to iobm/ALE0.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd3.Q to iobm/IOS_FSM_FFd1.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd3.Q to iobm/IOS_FSM_FFd2.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd3.Q to iobm/IOS_FSM_FFd3.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd3.Q to nAS_IOB.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd3.Q to nDoutOE.D | 66.600 | 10.000 | 56.600
iobm/IOS_FSM_FFd3.Q to nLDS_IOB.D | 33.300 | 10.000 | 23.300
iobm/IOS_FSM_FFd3.Q to nUDS_IOB.D | 33.300 | 10.000 | 23.300
iobm/RESrf.Q to iobm/IOS_FSM_FFd2.D | 33.300 | 10.000 | 23.300
iobm/RESrr.Q to iobm/IOS_FSM_FFd2.D | 66.600 | 10.000 | 56.600
iobm/VPArf.Q to nVMA_IOB.D | 33.300 | 10.000 | 23.300
iobm/VPArr.Q to nVMA_IOB.D | 66.600 | 10.000 | 56.600
nAS_IOB.Q to nAoutOE.D | 33.300 | 10.000 | 23.300
nAoutOE.Q to iobm/ALE0.D | 66.600 | 10.000 | 56.600
nAoutOE.Q to iobm/IOACT.D | 66.600 | 10.000 | 56.600
nAoutOE.Q to iobm/IOS_FSM_FFd3.D | 66.600 | 10.000 | 56.600
nAoutOE.Q to nAoutOE.D | 66.600 | 10.000 | 56.600
nVMA_IOB.Q to iobm/ETACK.D | 66.600 | 10.000 | 56.600
nVMA_IOB.Q to nVMA_IOB.D | 66.600 | 10.000 | 56.600

Number of constraints not met: 0

## Data Sheet Report

### Maximum External Clock Speeds

Clock | fEXT (MHz) | Reason
--- | --- | ---
CLK_IOB | 111.111 | Limited by Clock Pulse Width for CLK_IOB
CLK_FSB | 51.282 | Limited by Cycle Time for CLK_FSB
CLK2X_IOB | 90.909 | Limited by Cycle Time for CLK2X_IOB

### Setup/Hold Times for Clocks

Setup/Hold Times for Clock CLK_IOB
Source Pad | Setup to clk (edge) | Hold to clk (edge)
--- | --- | ---
E_IOB | 6.500 | 0.000

Setup/Hold Times for Clock CLK_FSB
Source Pad | Setup to clk (edge) | Hold to clk (edge)
--- | --- | ---
A_FSB<10> | 8.300 | 0.000
A_FSB<11> | 8.300 | 0.000
A_FSB<12> | 8.300 | 0.000
A_FSB<13> | 8.300 | 0.000
A_FSB<14> | 8.300 | 0.000
A_FSB<15> | 8.300 | 0.000
A_FSB<16> | 8.300 | 0.000
A_FSB<17> | 8.300 | 0.000
A_FSB<18> | 8.300 | 0.000
A_FSB<19> | 8.300 | 0.000
A_FSB<20> | 8.300 | 0.000
A_FSB<21> | 8.300 | 0.000
A_FSB<22> | 8.300 | 0.000
A_FSB<23> | 8.300 | 0.000
A_FSB<8> | 8.300 | 0.000
A_FSB<9> | 8.300 | 0.000
SW<1> | 7.900 | 0.000
nAS_FSB | 16.000 | 0.000
nIPL2 | 6.500 | 0.000
nLDS_FSB | 6.500 | 0.000
nRES | 6.500 | 0.000
nUDS_FSB | 6.500 | 0.000
nWE_FSB | 8.300 | 0.000

Setup/Hold Times for Clock CLK2X_IOB
Source Pad | Setup to clk (edge) | Hold to clk (edge)
--- | --- | ---
CLK_IOB | 7.500 | 0.000
nBERR_IOB | 7.500 | 0.000
nBG_IOB | 6.500 | 0.000
nDTACK_IOB | 6.500 | 0.000
nRES | 6.500 | 0.000
nVPA_IOB | 6.500 | 0.000

### Clock to Pad Timing

Clock CLK_FSB to Pad
Destination Pad | Clock (edge) to Pad
--- | ---
RA<2> | 14.500
RA<5> | 14.500
RA<8> | 14.500
RA<9> | 14.500
nBERR_FSB | 14.500
nRAMUWE | 14.500
nRAS | 14.500
RA<0> | 13.500
RA<1> | 13.500
RA<3> | 13.500
RA<4> | 13.500
RA<6> | 13.500
RA<7> | 13.500
nADoutLE0 | 13.500
nRAMLWE | 13.500
nROMCS | 13.500
nVPA_FSB | 13.500
nADoutLE1 | 5.800
nBR_IOB | 5.800
nCAS | 5.800
nDTACK_FSB | 5.800

Clock CLK2X_IOB to Pad
Destination Pad | Clock (edge) to Pad
--- | ---
nAS_IOB | 14.500
nLDS_IOB | 14.500
nUDS_IOB | 14.500
nVMA_IOB | 14.500
nADoutLE0 | 13.500
nAoutOE | 5.800
nDinLE | 5.800
nDoutOE | 5.800

### Clock to Setup Times for Clocks

Clock to Setup for clock CLK_FSB
Source | Destination | Delay
--- | --- | ---
fsb/ASrf.Q | fsb/VPA.D | 19.500
cnt/TimeoutA.Q | fsb/VPA.D | 11.800
cnt/TimeoutB.Q | fsb/VPA.D | 11.800
cnt/TimeoutB.Q | nDTACK_FSB.D | 11.800
cs/nOverlay1.Q | fsb/VPA.D | 11.800
fsb/ASrf.Q | nDTACK_FSB.D | 11.800
fsb/BERR0r.Q | fsb/VPA.D | 11.800
fsb/BERR0r.Q | nDTACK_FSB.D | 11.800
fsb/BERR1r.Q | fsb/VPA.D | 11.800
fsb/BERR1r.Q | nDTACK_FSB.D | 11.800
fsb/Ready1r.Q | fsb/VPA.D | 11.800
fsb/Ready1r.Q | nDTACK_FSB.D | 11.800
fsb/Ready2r.Q | fsb/VPA.D | 11.800
fsb/VPA.Q | fsb/VPA.D | 11.800
iobs/BERR.Q | fsb/VPA.D | 11.800
iobs/BERR.Q | nDTACK_FSB.D | 11.800
iobs/IOReady.Q | fsb/VPA.D | 11.800
iobs/IOReady.Q | nDTACK_FSB.D | 11.800
nBR_IOB.Q | fsb/VPA.D | 11.800
nBR_IOB.Q | nDTACK_FSB.D | 11.800
cnt/RefCnt<5>.Q | ram/RAMDIS1.D | 11.400
cnt/RefCnt<5>.Q | ram/RASEL.D | 11.400
cnt/RefCnt<6>.Q | ram/RAMDIS1.D | 11.400
cnt/RefCnt<6>.Q | ram/RASEL.D | 11.400
cnt/RefCnt<7>.Q | ram/RAMDIS1.D | 11.400
cnt/RefCnt<7>.Q | ram/RASEL.D | 11.400
cnt/RefDone.Q | ram/RAMDIS1.D | 11.400
cnt/RefDone.Q | ram/RASEL.D | 11.400
cs/nOverlay1.Q | fsb/Ready1r.D | 11.400
cs/nOverlay1.Q | iobs/IORW1.D | 11.400
cs/nOverlay1.Q | iobs/Once.D | 11.400
cs/nOverlay1.Q | nDTACK_FSB.D | 11.400
cs/nOverlay1.Q | ram/RAMDIS1.D | 11.400
cs/nOverlay1.Q | ram/RASEL.D | 11.400
fsb/ASrf.Q | ram/RASEL.D | 11.400
fsb/Ready0r.Q | nDTACK_FSB.D | 11.400
fsb/Ready1r.Q | fsb/Ready1r.D | 11.400
iobs/IORW0.Q | iobs/IORW0.D | 11.400
iobs/IOReady.Q | fsb/Ready1r.D | 11.400
iobs/Once.Q | iobs/IORW0.D | 11.400
iobs/Once.Q | iobs/Once.D | 11.400
iobs/PS_FSM_FFd1.Q | iobs/IORW0.D | 11.400
iobs/PS_FSM_FFd2.Q | iobs/IORW0.D | 11.400
nADoutLE1.Q | fsb/Ready1r.D | 11.400
nADoutLE1.Q | fsb/VPA.D | 11.400
nADoutLE1.Q | iobs/IORW0.D | 11.400
nDTACK_FSB.Q | nDTACK_FSB.D | 11.400
ram/Once.Q | ram/RASEL.D | 11.400
ram/RAMReady.Q | nDTACK_FSB.D | 11.400
ram/RS_FSM_FFd1.Q | ram/RAMDIS1.D | 11.400
ram/RS_FSM_FFd1.Q | ram/RASEL.D | 11.400
ram/RS_FSM_FFd2.Q | ram/RASEL.D | 11.400
ram/RS_FSM_FFd3.Q | ram/RAMDIS1.D | 11.400
cnt/RefCnt<5>.Q | ram/RAMDIS2.D | 11.000
cnt/RefCnt<5>.Q | ram/RS_FSM_FFd1.D | 11.000
cnt/RefCnt<5>.Q | ram/RS_FSM_FFd2.D | 11.000
cnt/RefCnt<5>.Q | ram/RS_FSM_FFd3.D | 11.000
cnt/RefCnt<6>.Q | ram/RAMDIS2.D | 11.000
cnt/RefCnt<6>.Q | ram/RS_FSM_FFd1.D | 11.000
cnt/RefCnt<6>.Q | ram/RS_FSM_FFd2.D | 11.000
cnt/RefCnt<6>.Q | ram/RS_FSM_FFd3.D | 11.000
cnt/RefCnt<7>.Q | ram/RAMDIS2.D | 11.000
cnt/RefCnt<7>.Q | ram/RS_FSM_FFd1.D | 11.000
cnt/RefCnt<7>.Q | ram/RS_FSM_FFd2.D | 11.000
cnt/RefCnt<7>.Q | ram/RS_FSM_FFd3.D | 11.000
cnt/RefDone.Q | ram/RAMDIS2.D | 11.000
cnt/RefDone.Q | ram/RAMReady.D | 11.000
cnt/RefDone.Q | ram/RS_FSM_FFd1.D | 11.000
cnt/RefDone.Q | ram/RS_FSM_FFd3.D | 11.000
cnt/TimeoutA.Q | fsb/Ready2r.D | 11.000
cnt/TimeoutA.Q | nDTACK_FSB.D | 11.000
cs/nOverlay1.Q | fsb/Ready2r.D | 11.000
cs/nOverlay1.Q | iobs/IOREQ.D | 11.000
cs/nOverlay1.Q | iobs/Load1.D | 11.000
cs/nOverlay1.Q | iobs/PS_FSM_FFd2.D | 11.000
cs/nOverlay1.Q | ram/RAMDIS2.D | 11.000
cs/nOverlay1.Q | ram/RAMReady.D | 11.000
cs/nOverlay1.Q | ram/RS_FSM_FFd1.D | 11.000
cs/nOverlay1.Q | ram/RS_FSM_FFd2.D | 11.000
cs/nOverlay1.Q | ram/RS_FSM_FFd3.D | 11.000
fsb/ASrf.Q | fsb/Ready0r.D | 11.000
fsb/ASrf.Q | fsb/Ready2r.D | 11.000
fsb/ASrf.Q | iobs/IORW0.D | 11.000
fsb/ASrf.Q | iobs/IORW1.D | 11.000
fsb/ASrf.Q | ram/RAMDIS1.D | 11.000
fsb/ASrf.Q | ram/RAMDIS2.D | 11.000
fsb/ASrf.Q | ram/RAMReady.D | 11.000
fsb/ASrf.Q | ram/RS_FSM_FFd1.D | 11.000
fsb/ASrf.Q | ram/RS_FSM_FFd2.D | 11.000
fsb/ASrf.Q | ram/RS_FSM_FFd3.D | 11.000
fsb/Ready0r.Q | fsb/VPA.D | 11.000
fsb/Ready2r.Q | fsb/Ready2r.D | 11.000
fsb/Ready2r.Q | nDTACK_FSB.D | 11.000
iobs/IORW1.Q | iobs/IORW0.D | 11.000
iobs/PS_FSM_FFd1.Q | iobs/IORW1.D | 11.000
iobs/PS_FSM_FFd1.Q | iobs/Once.D | 11.000
iobs/PS_FSM_FFd1.Q | iobs/PS_FSM_FFd2.D | 11.000
iobs/PS_FSM_FFd2.Q | iobs/IOREQ.D | 11.000
iobs/PS_FSM_FFd2.Q | iobs/IORW1.D | 11.000
iobs/PS_FSM_FFd2.Q | iobs/PS_FSM_FFd2.D | 11.000
nADoutLE1.Q | iobs/IOREQ.D | 11.000
nADoutLE1.Q | iobs/Once.D | 11.000
nADoutLE1.Q | iobs/PS_FSM_FFd2.D | 11.000
nADoutLE1.Q | nDTACK_FSB.D | 11.000
ram/BACTr.Q | ram/RAMDIS1.D | 11.000
ram/BACTr.Q | ram/RAMReady.D | 11.000
ram/BACTr.Q | ram/RASEL.D | 11.000
ram/BACTr.Q | ram/RS_FSM_FFd2.D | 11.000
ram/Once.Q | ram/RAMDIS1.D | 11.000
ram/Once.Q | ram/RAMDIS2.D | 11.000
ram/Once.Q | ram/RAMReady.D | 11.000
ram/Once.Q | ram/RS_FSM_FFd1.D | 11.000
ram/RAMDIS2.Q | ram/RAMDIS2.D | 11.000
ram/RAMReady.Q | fsb/VPA.D | 11.000
ram/RS_FSM_FFd1.Q | ram/RAMReady.D | 11.000
ram/RS_FSM_FFd1.Q | ram/RS_FSM_FFd1.D | 11.000
ram/RS_FSM_FFd1.Q | ram/RS_FSM_FFd3.D | 11.000
ram/RS_FSM_FFd2.Q | ram/RAMDIS2.D | 11.000
ram/RS_FSM_FFd2.Q | ram/RS_FSM_FFd1.D | 11.000
ram/RS_FSM_FFd2.Q | ram/RS_FSM_FFd2.D | 11.000
ram/RS_FSM_FFd2.Q | ram/RS_FSM_FFd3.D | 11.000
ram/RS_FSM_FFd3.Q | ram/RAMDIS2.D | 11.000
ram/RS_FSM_FFd3.Q | ram/RS_FSM_FFd2.D | 11.000
ram/RS_FSM_FFd3.Q | ram/RS_FSM_FFd3.D | 11.000
IPL2r0.Q | IPL2r1.D | 10.000
IPL2r0.Q | nBR_IOB.CE | 10.000
IPL2r1.Q | nBR_IOB.CE | 10.000
RESDone.Q | nBR_IOB.CE | 10.000
RESr0.Q | RESDone.CE | 10.000
RESr0.Q | RESr1.D | 10.000
RESr0.Q | nBR_IOB.CE | 10.000
RESr1.Q | RESDone.CE | 10.000
RESr1.Q | RESr2.D | 10.000
RESr1.Q | nBR_IOB.CE | 10.000
RESr2.Q | RESDone.CE | 10.000
RESr2.Q | nBR_IOB.CE | 10.000
cnt/RefCnt<0>.Q | cnt/RefCnt<1>.D | 10.000
cnt/RefCnt<0>.Q | cnt/RefCnt<2>.D | 10.000
cnt/RefCnt<0>.Q | cnt/RefCnt<3>.D | 10.000
cnt/RefCnt<0>.Q | cnt/RefCnt<4>.D | 10.000
cnt/RefCnt<0>.Q | cnt/RefCnt<5>.D | 10.000
cnt/RefCnt<0>.Q | cnt/RefCnt<6>.D | 10.000
cnt/RefCnt<0>.Q | cnt/RefCnt<7>.D | 10.000
cnt/RefCnt<0>.Q | cnt/RefDone.D | 10.000
cnt/RefCnt<0>.Q | cnt/TimeoutA.D | 10.000
cnt/RefCnt<0>.Q | cnt/TimeoutB.D | 10.000
cnt/RefCnt<0>.Q | cnt/TimeoutBPre.D | 10.000
cnt/RefCnt<1>.Q | cnt/RefCnt<2>.D | 10.000
cnt/RefCnt<1>.Q | cnt/RefCnt<3>.D | 10.000
cnt/RefCnt<1>.Q | cnt/RefCnt<4>.D | 10.000
cnt/RefCnt<1>.Q | cnt/RefCnt<5>.D | 10.000
cnt/RefCnt<1>.Q | cnt/RefCnt<6>.D | 10.000
cnt/RefCnt<1>.Q | cnt/RefCnt<7>.D | 10.000
cnt/RefCnt<1>.Q | cnt/RefDone.D | 10.000
cnt/RefCnt<1>.Q | cnt/TimeoutA.D | 10.000
cnt/RefCnt<1>.Q | cnt/TimeoutB.D | 10.000
cnt/RefCnt<1>.Q | cnt/TimeoutBPre.D | 10.000
cnt/RefCnt<2>.Q | cnt/RefCnt<3>.D | 10.000
cnt/RefCnt<2>.Q | cnt/RefCnt<4>.D | 10.000
cnt/RefCnt<2>.Q | cnt/RefCnt<5>.D | 10.000
cnt/RefCnt<2>.Q | cnt/RefCnt<6>.D | 10.000
cnt/RefCnt<2>.Q | cnt/RefCnt<7>.D | 10.000
cnt/RefCnt<2>.Q | cnt/RefDone.D | 10.000
cnt/RefCnt<2>.Q | cnt/TimeoutA.D | 10.000
cnt/RefCnt<2>.Q | cnt/TimeoutB.D | 10.000
cnt/RefCnt<2>.Q | cnt/TimeoutBPre.D | 10.000
cnt/RefCnt<3>.Q | cnt/RefCnt<4>.D | 10.000
cnt/RefCnt<3>.Q | cnt/RefCnt<5>.D | 10.000
cnt/RefCnt<3>.Q | cnt/RefCnt<6>.D | 10.000
cnt/RefCnt<3>.Q | cnt/RefCnt<7>.D | 10.000
cnt/RefCnt<3>.Q | cnt/RefDone.D | 10.000
cnt/RefCnt<3>.Q | cnt/TimeoutA.D | 10.000
cnt/RefCnt<3>.Q | cnt/TimeoutB.D | 10.000
cnt/RefCnt<3>.Q | cnt/TimeoutBPre.D | 10.000
cnt/RefCnt<4>.Q | cnt/RefCnt<5>.D | 10.000
cnt/RefCnt<4>.Q | cnt/RefCnt<6>.D | 10.000
cnt/RefCnt<4>.Q | cnt/RefCnt<7>.D | 10.000
cnt/RefCnt<4>.Q | cnt/RefDone.D | 10.000
cnt/RefCnt<4>.Q | cnt/TimeoutA.D | 10.000
cnt/RefCnt<4>.Q | cnt/TimeoutB.D | 10.000
cnt/RefCnt<4>.Q | cnt/TimeoutBPre.D | 10.000
cnt/RefCnt<5>.Q | cnt/RefCnt<6>.D | 10.000
cnt/RefCnt<5>.Q | cnt/RefCnt<7>.D | 10.000
cnt/RefCnt<5>.Q | cnt/RefDone.D | 10.000
cnt/RefCnt<5>.Q | cnt/TimeoutA.D | 10.000
cnt/RefCnt<5>.Q | cnt/TimeoutB.D | 10.000
cnt/RefCnt<5>.Q | cnt/TimeoutBPre.D | 10.000
cnt/RefCnt<5>.Q | ram/RAMReady.D | 10.000
cnt/RefCnt<6>.Q | cnt/RefCnt<7>.D | 10.000
cnt/RefCnt<6>.Q | cnt/RefDone.D | 10.000
cnt/RefCnt<6>.Q | cnt/TimeoutA.D | 10.000
cnt/RefCnt<6>.Q | cnt/TimeoutB.D | 10.000
cnt/RefCnt<6>.Q | cnt/TimeoutBPre.D | 10.000
cnt/RefCnt<6>.Q | ram/RAMReady.D | 10.000
cnt/RefCnt<7>.Q | cnt/RefDone.D | 10.000
cnt/RefCnt<7>.Q | cnt/TimeoutB.D | 10.000
cnt/RefCnt<7>.Q | cnt/TimeoutBPre.D | 10.000
cnt/RefCnt<7>.Q | ram/RAMReady.D | 10.000
cnt/RefDone.Q | cnt/RefDone.D | 10.000
cnt/RefDone.Q | ram/RS_FSM_FFd2.D | 10.000
cnt/TimeoutA.Q | cnt/TimeoutA.D | 10.000
cnt/TimeoutB.Q | cnt/TimeoutB.D | 10.000
cnt/TimeoutB.Q | fsb/BERR0r.D | 10.000
cnt/TimeoutBPre.Q | cnt/TimeoutB.D | 10.000
cnt/TimeoutBPre.Q | cnt/TimeoutBPre.D | 10.000
cs/nOverlay0.Q | cs/nOverlay0.D | 10.000
cs/nOverlay0.Q | cs/nOverlay1.D | 10.000
cs/nOverlay1.Q | fsb/Ready0r.D | 10.000
cs/nOverlay1.Q | iobs/IORW0.D | 10.000
cs/nOverlay1.Q | ram/Once.D | 10.000
fsb/ASrf.Q | cnt/TimeoutA.D | 10.000
fsb/ASrf.Q | cnt/TimeoutB.D | 10.000
fsb/ASrf.Q | cnt/TimeoutBPre.D | 10.000
fsb/ASrf.Q | cs/nOverlay0.D | 10.000
fsb/ASrf.Q | cs/nOverlay1.CE | 10.000
fsb/ASrf.Q | fsb/BERR0r.D | 10.000
fsb/ASrf.Q | fsb/BERR1r.D | 10.000
fsb/ASrf.Q | fsb/Ready1r.D | 10.000
fsb/ASrf.Q | iobs/BERR.D | 10.000
fsb/ASrf.Q | iobs/IOREQ.D | 10.000
fsb/ASrf.Q | iobs/IOReady.D | 10.000
fsb/ASrf.Q | iobs/Load1.D | 10.000
fsb/ASrf.Q | iobs/Once.D | 10.000
fsb/ASrf.Q | iobs/PS_FSM_FFd2.D | 10.000
fsb/ASrf.Q | ram/BACTr.D | 10.000
fsb/ASrf.Q | ram/Once.D | 10.000
fsb/BERR0r.Q | fsb/BERR0r.D | 10.000
fsb/BERR1r.Q | fsb/BERR1r.D | 10.000
fsb/Ready0r.Q | fsb/Ready0r.D | 10.000
iobs/BERR.Q | fsb/BERR1r.D | 10.000
iobs/BERR.Q | iobs/BERR.D | 10.000
iobs/Clear1.Q | nADoutLE1.D | 10.000
iobs/IOACTr.Q | iobs/BERR.D | 10.000
iobs/IOACTr.Q | iobs/IOREQ.D | 10.000
iobs/IOACTr.Q | iobs/IOReady.D | 10.000
iobs/IOACTr.Q | iobs/PS_FSM_FFd1.D | 10.000
iobs/IOACTr.Q | iobs/PS_FSM_FFd2.D | 10.000
iobs/IOL1.Q | iobs/IOL0.D | 10.000
iobs/IORW1.Q | iobs/IORW1.D | 10.000
iobs/IOReady.Q | iobs/IOReady.D | 10.000
iobs/IOU1.Q | iobs/IOU0.D | 10.000
iobs/Load1.Q | iobs/IOL1.CE | 10.000
iobs/Load1.Q | iobs/IOU1.CE | 10.000
iobs/Load1.Q | nADoutLE1.D | 10.000
iobs/Once.Q | iobs/BERR.D | 10.000
iobs/Once.Q | iobs/IOREQ.D | 10.000
iobs/Once.Q | iobs/IORW1.D | 10.000
iobs/Once.Q | iobs/IOReady.D | 10.000
iobs/Once.Q | iobs/Load1.D | 10.000
iobs/Once.Q | iobs/PS_FSM_FFd2.D | 10.000
iobs/PS_FSM_FFd1.Q | iobs/ALE0.D | 10.000
iobs/PS_FSM_FFd1.Q | iobs/Clear1.D | 10.000
iobs/PS_FSM_FFd1.Q | iobs/IOL0.CE | 10.000
iobs/PS_FSM_FFd1.Q | iobs/IOREQ.D | 10.000
iobs/PS_FSM_FFd1.Q | iobs/IOU0.CE | 10.000
iobs/PS_FSM_FFd1.Q | iobs/Load1.D | 10.000
iobs/PS_FSM_FFd1.Q | iobs/PS_FSM_FFd1.D | 10.000
iobs/PS_FSM_FFd2.Q | iobs/ALE0.D | 10.000
iobs/PS_FSM_FFd2.Q | iobs/BERR.D | 10.000
iobs/PS_FSM_FFd2.Q | iobs/Clear1.D | 10.000
iobs/PS_FSM_FFd2.Q | iobs/IOL0.CE | 10.000
iobs/PS_FSM_FFd2.Q | iobs/IOReady.D | 10.000
iobs/PS_FSM_FFd2.Q | iobs/IOU0.CE | 10.000
iobs/PS_FSM_FFd2.Q | iobs/Load1.D | 10.000
iobs/PS_FSM_FFd2.Q | iobs/Once.D | 10.000
iobs/PS_FSM_FFd2.Q | iobs/PS_FSM_FFd1.D | 10.000
nADoutLE1.Q | iobs/BERR.D | 10.000
nADoutLE1.Q | iobs/Clear1.D | 10.000
nADoutLE1.Q | iobs/IOL0.D | 10.000
nADoutLE1.Q | iobs/IORW1.D | 10.000
nADoutLE1.Q | iobs/IOReady.D | 10.000
nADoutLE1.Q | iobs/IOU0.D | 10.000
nADoutLE1.Q | iobs/Load1.D | 10.000
nADoutLE1.Q | nADoutLE1.D | 10.000
ram/Once.Q | ram/Once.D | 10.000
ram/Once.Q | ram/RS_FSM_FFd3.D | 10.000
ram/RAMReady.Q | fsb/Ready0r.D | 10.000
ram/RASEL.Q | nCAS.D | 10.000
ram/RS_FSM_FFd1.Q | ram/Once.D | 10.000
ram/RS_FSM_FFd1.Q | ram/RAMDIS2.D | 10.000
ram/RS_FSM_FFd1.Q | ram/RS_FSM_FFd2.D | 10.000
ram/RS_FSM_FFd1.Q | ram/RefRAS.D | 10.000
ram/RS_FSM_FFd2.Q | ram/Once.D | 10.000
ram/RS_FSM_FFd2.Q | ram/RAMDIS1.D | 10.000
ram/RS_FSM_FFd2.Q | ram/RAMReady.D | 10.000
ram/RS_FSM_FFd2.Q | ram/RefRAS.D | 10.000
ram/RS_FSM_FFd3.Q | ram/Once.D | 10.000
ram/RS_FSM_FFd3.Q | ram/RAMReady.D | 10.000
ram/RS_FSM_FFd3.Q | ram/RASEL.D | 10.000
ram/RS_FSM_FFd3.Q | ram/RS_FSM_FFd1.D | 10.000
ram/RefRAS.Q | cnt/RefDone.D | 10.000

Clock to Setup for clock CLK2X_IOB
Source | Destination | Delay
--- | --- | ---
iobm/BERRrf.Q | iobm/IOBERR.D | 11.000
iobm/BERRrr.Q | iobm/IOBERR.D | 11.000
iobm/DTACKrf.Q | iobm/IOACT.D | 11.000
iobm/DTACKrf.Q | iobm/IOBERR.D | 11.000
iobm/DTACKrr.Q | iobm/IOACT.D | 11.000
iobm/DTACKrr.Q | iobm/IOBERR.D | 11.000
iobm/IOBERR.Q | iobm/IOBERR.D | 11.000
iobm/IOS_FSM_FFd1.Q | iobm/IOACT.D | 11.000
iobm/IOS_FSM_FFd1.Q | iobm/IOBERR.D | 11.000
iobm/IOS_FSM_FFd2.Q | iobm/IOBERR.D | 11.000
iobm/IOS_FSM_FFd3.Q | iobm/IOACT.D | 11.000
iobm/IOS_FSM_FFd3.Q | iobm/IOBERR.D | 11.000
iobm/RESrf.Q | iobm/IOACT.D | 11.000
iobm/RESrf.Q | iobm/IOBERR.D | 11.000
iobm/RESrr.Q | iobm/IOACT.D | 11.000
iobm/RESrr.Q | iobm/IOBERR.D | 11.000
iobm/BERRrf.Q | iobm/IOACT.D | 10.000
iobm/BERRrf.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/BERRrr.Q | iobm/IOACT.D | 10.000
iobm/BERRrr.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/BGr0.Q | iobm/BGr1.D | 10.000
iobm/BGr0.Q | nAoutOE.D | 10.000
iobm/BGr1.Q | nAoutOE.D | 10.000
iobm/DTACKrf.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/DTACKrr.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/ES<0>.Q | iobm/ES<0>.D | 10.000
iobm/ES<0>.Q | iobm/ES<1>.D | 10.000
iobm/ES<0>.Q | iobm/ES<2>.D | 10.000
iobm/ES<0>.Q | iobm/ES<3>.D | 10.000
iobm/ES<0>.Q | iobm/ES<4>.D | 10.000
iobm/ES<0>.Q | iobm/ETACK.D | 10.000
iobm/ES<0>.Q | nVMA_IOB.D | 10.000
iobm/ES<1>.Q | iobm/ES<0>.D | 10.000
iobm/ES<1>.Q | iobm/ES<1>.D | 10.000
iobm/ES<1>.Q | iobm/ES<2>.D | 10.000
iobm/ES<1>.Q | iobm/ES<3>.D | 10.000
iobm/ES<1>.Q | iobm/ES<4>.D | 10.000
iobm/ES<1>.Q | iobm/ETACK.D | 10.000
iobm/ES<1>.Q | nVMA_IOB.D | 10.000
iobm/ES<2>.Q | iobm/ES<0>.D | 10.000
iobm/ES<2>.Q | iobm/ES<2>.D | 10.000
iobm/ES<2>.Q | iobm/ES<3>.D | 10.000
iobm/ES<2>.Q | iobm/ES<4>.D | 10.000
iobm/ES<2>.Q | iobm/ETACK.D | 10.000
iobm/ES<2>.Q | nVMA_IOB.D | 10.000
iobm/ES<3>.Q | iobm/ES<0>.D | 10.000
iobm/ES<3>.Q | iobm/ES<2>.D | 10.000
iobm/ES<3>.Q | iobm/ES<3>.D | 10.000
iobm/ES<3>.Q | iobm/ES<4>.D | 10.000
iobm/ES<3>.Q | iobm/ETACK.D | 10.000
iobm/ES<3>.Q | nVMA_IOB.D | 10.000
iobm/ES<4>.Q | iobm/ES<0>.D | 10.000
iobm/ES<4>.Q | iobm/ES<2>.D | 10.000
iobm/ES<4>.Q | iobm/ES<4>.D | 10.000
iobm/ES<4>.Q | iobm/ETACK.D | 10.000
iobm/ES<4>.Q | nVMA_IOB.D | 10.000
iobm/ETACK.Q | iobm/IOACT.D | 10.000
iobm/ETACK.Q | iobm/IOBERR.D | 10.000
iobm/ETACK.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/Er2.Q | iobm/ES<0>.D | 10.000
iobm/Er2.Q | iobm/ES<1>.D | 10.000
iobm/Er2.Q | iobm/ES<2>.D | 10.000
iobm/Er2.Q | iobm/ES<3>.D | 10.000
iobm/Er2.Q | iobm/ES<4>.D | 10.000
iobm/IOACT.Q | nVMA_IOB.D | 10.000
iobm/IOREQr.Q | iobm/ALE0.D | 10.000
iobm/IOREQr.Q | iobm/IOACT.D | 10.000
iobm/IOREQr.Q | iobm/IOS_FSM_FFd3.D | 10.000
iobm/IOS_FSM_FFd1.Q | iobm/ALE0.D | 10.000
iobm/IOS_FSM_FFd1.Q | iobm/IOS_FSM_FFd1.D | 10.000
iobm/IOS_FSM_FFd1.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/IOS_FSM_FFd1.Q | iobm/IOS_FSM_FFd3.D | 10.000
iobm/IOS_FSM_FFd1.Q | nAS_IOB.D | 10.000
iobm/IOS_FSM_FFd1.Q | nDinLE.D | 10.000
iobm/IOS_FSM_FFd1.Q | nLDS_IOB.D | 10.000
iobm/IOS_FSM_FFd1.Q | nUDS_IOB.D | 10.000
iobm/IOS_FSM_FFd2.Q | iobm/ALE0.D | 10.000
iobm/IOS_FSM_FFd2.Q | iobm/IOACT.D | 10.000
iobm/IOS_FSM_FFd2.Q | iobm/IOS_FSM_FFd1.D | 10.000
iobm/IOS_FSM_FFd2.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/IOS_FSM_FFd2.Q | iobm/IOS_FSM_FFd3.D | 10.000
iobm/IOS_FSM_FFd2.Q | nAS_IOB.D | 10.000
iobm/IOS_FSM_FFd2.Q | nDinLE.D | 10.000
iobm/IOS_FSM_FFd2.Q | nDoutOE.D | 10.000
iobm/IOS_FSM_FFd2.Q | nLDS_IOB.D | 10.000
iobm/IOS_FSM_FFd2.Q | nUDS_IOB.D | 10.000
iobm/IOS_FSM_FFd3.Q | iobm/ALE0.D | 10.000
iobm/IOS_FSM_FFd3.Q | iobm/IOS_FSM_FFd1.D | 10.000
iobm/IOS_FSM_FFd3.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/IOS_FSM_FFd3.Q | iobm/IOS_FSM_FFd3.D | 10.000
iobm/IOS_FSM_FFd3.Q | nAS_IOB.D | 10.000
iobm/IOS_FSM_FFd3.Q | nDoutOE.D | 10.000
iobm/IOS_FSM_FFd3.Q | nLDS_IOB.D | 10.000
iobm/IOS_FSM_FFd3.Q | nUDS_IOB.D | 10.000
iobm/RESrf.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/RESrr.Q | iobm/IOS_FSM_FFd2.D | 10.000
iobm/VPArf.Q | nVMA_IOB.D | 10.000
iobm/VPArr.Q | nVMA_IOB.D | 10.000
nAS_IOB.Q | nAoutOE.D | 10.000
nAoutOE.Q | iobm/ALE0.D | 10.000
nAoutOE.Q | iobm/IOACT.D | 10.000
nAoutOE.Q | iobm/IOS_FSM_FFd3.D | 10.000
nAoutOE.Q | nAoutOE.D | 10.000
nVMA_IOB.Q | iobm/ETACK.D | 10.000
nVMA_IOB.Q | nVMA_IOB.D | 10.000

### Pad to Pad List

Source Pad | Destination Pad | Delay
--- | --- | ---
A_FSB<12> | RA<2> | 11.000
A_FSB<15> | RA<5> | 11.000
A_FSB<19> | RA<9> | 11.000
A_FSB<20> | RA<9> | 11.000
A_FSB<20> | nBERR_FSB | 11.000
A_FSB<21> | RA<8> | 11.000
A_FSB<21> | nBERR_FSB | 11.000
A_FSB<21> | nRAS | 11.000
A_FSB<22> | RA<8> | 11.000
A_FSB<22> | nBERR_FSB | 11.000
A_FSB<22> | nRAS | 11.000
A_FSB<23> | RA<8> | 11.000
A_FSB<23> | nBERR_FSB | 11.000
A_FSB<23> | nRAS | 11.000
A_FSB<3> | RA<2> | 11.000
A_FSB<6> | RA<5> | 11.000
A_FSB<9> | RA<8> | 11.000
SW<0> | CLK20EN | 11.000
nAS_FSB | nOE | 11.000
nAS_FSB | nRAMUWE | 11.000
nAS_FSB | nRAS | 11.000
nUDS_FSB | nRAMUWE | 11.000
nWE_FSB | nOE | 11.000
nWE_FSB | nRAMUWE | 11.000
A_FSB<10> | RA<0> | 10.000
A_FSB<11> | RA<1> | 10.000
A_FSB<13> | RA<3> | 10.000
A_FSB<14> | RA<4> | 10.000
A_FSB<16> | RA<6> | 10.000
A_FSB<17> | RA<7> | 10.000
A_FSB<18> | RA<8> | 10.000
A_FSB<19> | RA<11> | 10.000
A_FSB<1> | RA<0> | 10.000
A_FSB<20> | nDinOE | 10.000
A_FSB<20> | nROMCS | 10.000
A_FSB<21> | RA<10> | 10.000
A_FSB<21> | nDinOE | 10.000
A_FSB<21> | nROMCS | 10.000
A_FSB<22> | nDinOE | 10.000
A_FSB<22> | nROMCS | 10.000
A_FSB<23> | nDinOE | 10.000
A_FSB<23> | nROMCS | 10.000
A_FSB<2> | RA<1> | 10.000
A_FSB<4> | RA<3> | 10.000
A_FSB<5> | RA<4> | 10.000
A_FSB<7> | RA<6> | 10.000
A_FSB<8> | RA<7> | 10.000
SW<0> | CLK25EN | 10.000
SW<1> | nDinOE | 10.000
SW<1> | nROMCS | 10.000
nAS_FSB | nBERR_FSB | 10.000
nAS_FSB | nDinOE | 10.000
nAS_FSB | nRAMLWE | 10.000
nAS_FSB | nROMWE | 10.000
nAS_FSB | nVPA_FSB | 10.000
nLDS_FSB | nRAMLWE | 10.000
nWE_FSB | nDinOE | 10.000
nWE_FSB | nRAMLWE | 10.000
nWE_FSB | nROMWE | 10.000

Number of paths analyzed: 396
Number of Timing errors: 0
Analysis Completed: Mon Mar 28 09:47:21 2022