MDF Database:  version 1.0
MDF_INFO | WarpSE | XC95144XL-10-TQ100
MACROCELL | 5 | 1 | iobm/nVMA
ATTRIBUTES | 4622082 | 0
OUTPUTMC | 2 | 5 | 1 | 5 | 0
INPUTS | 10 | nVMA_IOB  | iobm/ES<0>  | iobm/ES<1>  | iobm/ES<2>  | iobm/ES<3>  | iobm/ES<4>  | iobm/IOACT  | iobm/VPArf  | iobm/VPArr  | nAoutOE
INPUTMC | 10 | 5 | 1 | 5 | 5 | 5 | 4 | 5 | 12 | 5 | 3 | 5 | 7 | 5 | 15 | 1 | 8 | 1 | 7 | 3 | 1
EQ | 7 | 
   nVMA_IOB.T = !nVMA_IOB & !iobm/ES<0> & !iobm/ES<1> & !iobm/ES<2> & 
	!iobm/ES<3> & !iobm/ES<4>
	# nVMA_IOB & iobm/ES<0> & iobm/ES<1> & iobm/ES<2> & 
	!iobm/ES<3> & !iobm/ES<4> & iobm/IOACT & iobm/VPArf & 
	iobm/VPArr;
   nVMA_IOB.CLK = CLK2X_IOB;	// GCK
   nVMA_IOB.OE = !nAoutOE;
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 5 | 11 | iobm/nASout
ATTRIBUTES | 8816386 | 0
OUTPUTMC | 1 | 3 | 1
INPUTS | 4 | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd2  | iobm/IOS_FSM_FFd3  | nAoutOE
INPUTMC | 4 | 0 | 15 | 5 | 9 | 5 | 2 | 3 | 1
EQ | 4 | 
   nAS_IOB.D = !iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd2
	# iobm/IOS_FSM_FFd1 & !iobm/IOS_FSM_FFd2;
   !nAS_IOB.CLK = CLK2X_IOB;	// GCK
   nAS_IOB.OE = !nAoutOE;
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 5 | 8 | iobm/nLDS
ATTRIBUTES | 8685314 | 0
INPUTS | 6 | iobs/IOL0  | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd2  | iobm/IOS_FSM_FFd1  | iobs/IORW0  | nAoutOE
INPUTMC | 6 | 4 | 3 | 5 | 2 | 5 | 9 | 0 | 15 | 7 | 17 | 3 | 1
EQ | 8 | 
   !nLDS_IOB.D = iobs/IOL0 & !iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd2
	# iobs/IOL0 & iobm/IOS_FSM_FFd1 & 
	iobm/IOS_FSM_FFd2
	# !iobs/IORW0 & iobs/IOL0 & iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd1;
   !nLDS_IOB.CLK = CLK2X_IOB;	// GCK
   nLDS_IOB.OE = !nAoutOE;
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 5 | 10 | iobm/nUDS
ATTRIBUTES | 8685314 | 0
INPUTS | 6 | iobs/IOU0  | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd2  | iobm/IOS_FSM_FFd1  | iobs/IORW0  | nAoutOE
INPUTMC | 6 | 3 | 14 | 5 | 2 | 5 | 9 | 0 | 15 | 7 | 17 | 3 | 1
EQ | 8 | 
   !nUDS_IOB.D = iobs/IOU0 & !iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd2
	# iobs/IOU0 & iobm/IOS_FSM_FFd1 & 
	iobm/IOS_FSM_FFd2
	# !iobs/IORW0 & iobs/IOU0 & iobm/IOS_FSM_FFd3 & 
	!iobm/IOS_FSM_FFd1;
   !nUDS_IOB.CLK = CLK2X_IOB;	// GCK
   nUDS_IOB.OE = !nAoutOE;
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 3 | 13 | cnt/RefDone
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 20 | 3 | 13 | 4 | 2 | 3 | 17 | 4 | 17 | 6 | 9 | 6 | 2 | 6 | 17 | 6 | 14 | 3 | 0 | 3 | 16 | 4 | 0 | 4 | 1 | 4 | 15 | 4 | 16 | 6 | 0 | 6 | 1 | 6 | 4 | 6 | 13 | 6 | 15 | 6 | 16
INPUTS | 10 | cnt/RefDone  | ram/RefRAS  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<0>  | cnt/RefCnt<7>  | cnt/RefCnt<1>  | cnt/RefCnt<3>  | cnt/RefCnt<2>  | cnt/RefCnt<4>
INPUTMC | 10 | 3 | 13 | 0 | 0 | 3 | 7 | 3 | 6 | 1 | 17 | 3 | 3 | 0 | 6 | 3 | 9 | 3 | 11 | 3 | 8
EQ | 5 | 
   !cnt/RefDone.D = !cnt/RefDone & !ram/RefRAS
	# !cnt/RefCnt<5> & !cnt/RefCnt<6> & !cnt/RefCnt<0> & 
	!cnt/RefCnt<7> & !cnt/RefCnt<1> & !cnt/RefCnt<3> & !cnt/RefCnt<2> & 
	!cnt/RefCnt<4>;
   cnt/RefDone.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 4 | 9 | ram/Once
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 12 | 4 | 9 | 4 | 2 | 3 | 17 | 4 | 16 | 6 | 3 | 6 | 15 | 6 | 13 | 3 | 0 | 3 | 16 | 4 | 1 | 4 | 15 | 6 | 0
INPUTS | 10 | ram/Once  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | A_FSB<21>
INPUTMC | 6 | 4 | 9 | 0 | 5 | 0 | 17 | 3 | 17 | 6 | 9 | 6 | 3
INPUTP | 4 | 54 | 36 | 30 | 29
EQ | 13 | 
   ram/Once.T = ram/Once & nAS_FSB & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	!ram/RS_FSM_FFd3
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	!ram/RS_FSM_FFd3
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	!ram/RS_FSM_FFd3 & fsb/ASrf;
   ram/Once.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 4 | 6 | iobs/Once
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 11 | 4 | 6 | 7 | 15 | 7 | 1 | 7 | 13 | 3 | 16 | 7 | 3 | 4 | 12 | 7 | 8 | 4 | 5 | 4 | 7 | 4 | 8
INPUTS | 10 | A_FSB<22>  | iobs/Once  | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | nADoutLE1  | nOE_OBUF.EXP  | EXP25_.EXP
INPUTMC | 7 | 4 | 6 | 7 | 3 | 3 | 12 | 0 | 5 | 5 | 13 | 4 | 5 | 4 | 7
INPUTP | 3 | 30 | 54 | 36
IMPORTS | 2 | 4 | 5 | 4 | 7
EQ | 25 | 
   !iobs/Once.D = nAS_FSB & !fsb/ASrf
	# A_FSB<23> & !iobs/Once & iobs/PS_FSM_FFd2
	# A_FSB<22> & !iobs/Once & iobs/PS_FSM_FFd2
	# A_FSB<22> & !iobs/Once & iobs/PS_FSM_FFd1
	# !iobs/Once & iobs/PS_FSM_FFd2 & !nADoutLE1
;Imported pterms FB5_6
	# A_FSB<23> & !iobs/Once & iobs/PS_FSM_FFd1
	# !iobs/Once & iobs/PS_FSM_FFd1 & !nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & !iobs/Once
	# !A_FSB<23> & !A_FSB<22> & !iobs/Once & 
	!cs/nOverlay1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20> & !iobs/Once
;Imported pterms FB5_8
	# !A_FSB<23> & A_FSB<21> & !A_FSB<19> & !iobs/Once
	# !A_FSB<23> & A_FSB<21> & !A_FSB<18> & !iobs/Once
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17> & !iobs/Once
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16> & !iobs/Once
	# !A_FSB<23> & A_FSB<21> & nWE_FSB & !iobs/Once
;Imported pterms FB5_9
	# !A_FSB<23> & !A_FSB<20> & !iobs/Once & SW<1>
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21> & 
	!iobs/Once
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !iobs/Once & 
	cs/nOverlay1;
   iobs/Once.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 17 | cs/nOverlay1
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 44 | 4 | 9 | 4 | 5 | 7 | 17 | 2 | 3 | 2 | 13 | 2 | 15 | 4 | 1 | 7 | 12 | 4 | 2 | 2 | 8 | 3 | 17 | 4 | 16 | 6 | 6 | 6 | 3 | 7 | 3 | 4 | 12 | 7 | 8 | 6 | 16 | 6 | 13 | 6 | 7 | 6 | 15 | 2 | 1 | 2 | 2 | 2 | 6 | 2 | 7 | 2 | 9 | 2 | 12 | 2 | 14 | 2 | 16 | 3 | 0 | 3 | 16 | 4 | 0 | 4 | 8 | 4 | 13 | 4 | 15 | 6 | 0 | 6 | 1 | 6 | 2 | 6 | 4 | 6 | 10 | 7 | 4 | 7 | 5 | 7 | 9 | 7 | 11
INPUTS | 3 | cs/nOverlay0  | nAS_FSB  | fsb/ASrf
INPUTMC | 2 | 2 | 12 | 0 | 5
INPUTP | 1 | 54
EQ | 3 | 
   cs/nOverlay1.D = cs/nOverlay0;
   cs/nOverlay1.CLK = CLK_FSB;	// GCK
   cs/nOverlay1.CE = nAS_FSB & !fsb/ASrf;
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 7 | 15 | iobs/BERR
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 9 | 7 | 15 | 0 | 16 | 2 | 0 | 2 | 5 | 7 | 11 | 2 | 3 | 2 | 10 | 2 | 11 | 7 | 10
INPUTS | 8 | iobs/BERR  | nAS_FSB  | fsb/ASrf  | iobs/Once  | iobs/PS_FSM_FFd2  | iobs/IOACTr  | iobm/IOBERR  | nADoutLE1
INPUTMC | 7 | 7 | 15 | 0 | 5 | 4 | 6 | 7 | 3 | 1 | 6 | 5 | 17 | 5 | 13
INPUTP | 1 | 54
EQ | 8 | 
   iobs/BERR.T = iobs/BERR & nAS_FSB & !fsb/ASrf
	# iobs/Once & iobs/BERR & !iobs/PS_FSM_FFd2 & 
	!iobs/IOACTr & !iobm/IOBERR & nADoutLE1
	# iobs/Once & !iobs/BERR & !nAS_FSB & 
	!iobs/PS_FSM_FFd2 & !iobs/IOACTr & iobm/IOBERR & nADoutLE1
	# iobs/Once & !iobs/BERR & !iobs/PS_FSM_FFd2 & 
	!iobs/IOACTr & iobm/IOBERR & fsb/ASrf & nADoutLE1;
   iobs/BERR.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 7 | 17 | iobs/IORW0
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 6 | 5 | 8 | 5 | 10 | 7 | 17 | 3 | 4 | 7 | 0 | 7 | 1
INPUTS | 12 | A_FSB<14>  | A_FSB<13>  | A_FSB<23>  | A_FSB<21>  | nADoutLE1  | A_FSB<22>  | cs/nOverlay1  | A_FSB<20>  | nWE_FSB  | iobs/IORW0  | EXP32_.EXP  | EXP37_.EXP
INPUTMC | 5 | 5 | 13 | 0 | 17 | 7 | 17 | 7 | 0 | 7 | 16
INPUTP | 7 | 19 | 18 | 36 | 29 | 30 | 28 | 47
IMPORTS | 2 | 7 | 0 | 7 | 16
EQ | 26 | 
   !iobs/IORW0.T = !nWE_FSB & !iobs/IORW0 & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !cs/nOverlay1 & 
	nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20> & nADoutLE1
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21> & 
	nADoutLE1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1 & nADoutLE1
;Imported pterms FB8_1
	# iobs/IORW0 & iobs/IORW1 & !nADoutLE1
	# !iobs/IORW0 & !iobs/IORW1 & !nADoutLE1
	# nAS_FSB & !fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !iobs/IORW0 & nADoutLE1
;Imported pterms FB8_2
	# iobs/PS_FSM_FFd2
	# iobs/PS_FSM_FFd1
	# iobs/Once & nADoutLE1
	# nWE_FSB & iobs/IORW0 & nADoutLE1
;Imported pterms FB8_17
	# !A_FSB<23> & A_FSB<21> & !A_FSB<19> & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<18> & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17> & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16> & nADoutLE1
	# !A_FSB<23> & !A_FSB<20> & SW<1> & nADoutLE1;
   iobs/IORW0.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 2 | 12 | cs/nOverlay0
ATTRIBUTES | 4358928 | 0
OUTPUTMC | 3 | 0 | 17 | 2 | 12 | 2 | 13
INPUTS | 19 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | cs/nOverlay0  | nAS_FSB  | fsb/ASrf  | nRES  | A_FSB<14>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | cs/nOverlay1  | fsb/Ready1r  | iobs/IOReady  | nADoutLE1  | A_FSB<13>
INPUTMC | 6 | 2 | 12 | 0 | 5 | 0 | 17 | 2 | 14 | 3 | 16 | 5 | 13
INPUTP | 13 | 36 | 30 | 29 | 28 | 54 | 145 | 19 | 26 | 24 | 23 | 22 | 47 | 18
EXPORTS | 1 | 2 | 13
EQ | 12 | 
   cs/nOverlay0.T = !A_FSB<23> & A_FSB<22> & !A_FSB<21> & !A_FSB<20> & 
	!cs/nOverlay0 & !nAS_FSB
	# !A_FSB<23> & A_FSB<22> & !A_FSB<21> & !A_FSB<20> & 
	!cs/nOverlay0 & fsb/ASrf;
   cs/nOverlay0.CLK = CLK_FSB;	// GCK
   cs/nOverlay0.AR = !nRES;
    cs/nOverlay0.EXP  =  A_FSB<14> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & !nADoutLE1
	# A_FSB<13> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & !nADoutLE1
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 15 | cnt/TimeoutA
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 8 | 3 | 15 | 2 | 15 | 2 | 8 | 2 | 2 | 2 | 3 | 2 | 7 | 2 | 14 | 2 | 16
INPUTS | 10 | cnt/TimeoutA  | nAS_FSB  | fsb/ASrf  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<0>  | cnt/RefCnt<1>  | cnt/RefCnt<3>  | cnt/RefCnt<2>  | cnt/RefCnt<4>
INPUTMC | 9 | 3 | 15 | 0 | 5 | 3 | 7 | 3 | 6 | 1 | 17 | 0 | 6 | 3 | 9 | 3 | 11 | 3 | 8
INPUTP | 1 | 54
EQ | 8 | 
   cnt/TimeoutA.T = cnt/TimeoutA & nAS_FSB & !fsb/ASrf
	# !cnt/TimeoutA & !nAS_FSB & !cnt/RefCnt<5> & 
	!cnt/RefCnt<6> & !cnt/RefCnt<0> & !cnt/RefCnt<1> & !cnt/RefCnt<3> & 
	!cnt/RefCnt<2> & !cnt/RefCnt<4>
	# !cnt/TimeoutA & !cnt/RefCnt<5> & !cnt/RefCnt<6> & 
	!cnt/RefCnt<0> & !cnt/RefCnt<1> & !cnt/RefCnt<3> & !cnt/RefCnt<2> & 
	!cnt/RefCnt<4> & fsb/ASrf;
   cnt/TimeoutA.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 6 | 12 | cnt/TimeoutB
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 10 | 6 | 12 | 2 | 11 | 2 | 0 | 2 | 6 | 7 | 11 | 2 | 3 | 2 | 5 | 2 | 10 | 2 | 17 | 6 | 13
INPUTS | 13 | cnt/TimeoutB  | nAS_FSB  | fsb/ASrf  | cnt/TimeoutBPre  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<0>  | cnt/RefCnt<7>  | cnt/RefCnt<1>  | cnt/RefCnt<3>  | cnt/RefCnt<2>  | cnt/RefCnt<4>  | SW<0>
INPUTMC | 11 | 6 | 12 | 0 | 5 | 6 | 6 | 3 | 7 | 3 | 6 | 1 | 17 | 3 | 3 | 0 | 6 | 3 | 9 | 3 | 11 | 3 | 8
INPUTP | 2 | 54 | 98
EXPORTS | 1 | 6 | 13
EQ | 9 | 
   cnt/TimeoutB.T = cnt/TimeoutB & nAS_FSB & !fsb/ASrf
	# !cnt/TimeoutB & cnt/TimeoutBPre & !nAS_FSB & 
	!cnt/RefCnt<5> & !cnt/RefCnt<6> & !cnt/RefCnt<0> & !cnt/RefCnt<7> & 
	!cnt/RefCnt<1> & !cnt/RefCnt<3> & !cnt/RefCnt<2> & !cnt/RefCnt<4>
	# !cnt/TimeoutB & cnt/TimeoutBPre & !cnt/RefCnt<5> & 
	!cnt/RefCnt<6> & !cnt/RefCnt<0> & !cnt/RefCnt<7> & !cnt/RefCnt<1> & 
	!cnt/RefCnt<3> & !cnt/RefCnt<2> & !cnt/RefCnt<4> & fsb/ASrf;
   cnt/TimeoutB.CLK = CLK_FSB;	// GCK
    cnt/TimeoutB.EXP  =  SW<0>
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 6 | 6 | cnt/TimeoutBPre
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 3 | 6 | 12 | 6 | 6 | 6 | 7
INPUTS | 17 | cnt/TimeoutBPre  | nAS_FSB  | fsb/ASrf  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<0>  | cnt/RefCnt<7>  | cnt/RefCnt<1>  | cnt/RefCnt<3>  | cnt/RefCnt<2>  | cnt/RefCnt<4>  | A_FSB<9>  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | ram/RASEL  | A_FSB<21>
INPUTMC | 12 | 6 | 6 | 0 | 5 | 3 | 7 | 3 | 6 | 1 | 17 | 3 | 3 | 0 | 6 | 3 | 9 | 3 | 11 | 3 | 8 | 0 | 17 | 4 | 17
INPUTP | 5 | 54 | 12 | 36 | 30 | 29
EXPORTS | 1 | 6 | 7
EQ | 12 | 
   cnt/TimeoutBPre.T = cnt/TimeoutBPre & nAS_FSB & !fsb/ASrf
	# !cnt/TimeoutBPre & !nAS_FSB & !cnt/RefCnt<5> & 
	!cnt/RefCnt<6> & !cnt/RefCnt<0> & !cnt/RefCnt<7> & !cnt/RefCnt<1> & 
	!cnt/RefCnt<3> & !cnt/RefCnt<2> & !cnt/RefCnt<4>
	# !cnt/TimeoutBPre & !cnt/RefCnt<5> & !cnt/RefCnt<6> & 
	!cnt/RefCnt<0> & !cnt/RefCnt<7> & !cnt/RefCnt<1> & !cnt/RefCnt<3> & 
	!cnt/RefCnt<2> & !cnt/RefCnt<4> & fsb/ASrf;
   cnt/TimeoutBPre.CLK = CLK_FSB;	// GCK
    cnt/TimeoutBPre.EXP  =  A_FSB<9> & !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	ram/RASEL
	# A_FSB<9> & !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & ram/RASEL
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 2 | 11 | fsb/BERR0r
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 7 | 2 | 11 | 2 | 0 | 2 | 5 | 7 | 11 | 2 | 3 | 2 | 10 | 7 | 10
INPUTS | 24 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | fsb/BERR0r  | cnt/TimeoutB  | nAS_FSB  | fsb/ASrf  | A_FSB<9>  | A_FSB<8>  | A_FSB<15>  | A_FSB<14>  | A_FSB<13>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | iobs/BERR  | fsb/BERR1r  | fsb/Ready1r  | nBR_IOB
INPUTMC | 7 | 2 | 11 | 6 | 12 | 0 | 5 | 7 | 15 | 0 | 16 | 2 | 14 | 7 | 14
INPUTP | 17 | 36 | 30 | 29 | 28 | 54 | 12 | 11 | 21 | 19 | 18 | 17 | 15 | 13 | 26 | 24 | 23 | 22
EXPORTS | 1 | 2 | 10
EQ | 10 | 
   !fsb/BERR0r.D = !cnt/TimeoutB & !fsb/BERR0r
	# nAS_FSB & !fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & !A_FSB<21> & A_FSB<20> & 
	!fsb/BERR0r;
   fsb/BERR0r.CLK = CLK_FSB;	// GCK
    fsb/BERR0r.EXP  =  A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & fsb/Ready1r & nBR_IOB
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 16 | fsb/BERR1r
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 8 | 0 | 16 | 2 | 0 | 2 | 5 | 7 | 11 | 2 | 3 | 2 | 10 | 2 | 11 | 7 | 10
INPUTS | 4 | iobs/BERR  | fsb/BERR1r  | nAS_FSB  | fsb/ASrf
INPUTMC | 3 | 7 | 15 | 0 | 16 | 0 | 5
INPUTP | 1 | 54
EQ | 3 | 
   !fsb/BERR1r.D = !iobs/BERR & !fsb/BERR1r
	# nAS_FSB & !fsb/ASrf;
   fsb/BERR1r.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 2 | 3 | fsb/Ready0r
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 5 | 2 | 3 | 2 | 6 | 2 | 1 | 2 | 9 | 2 | 2
INPUTS | 32 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | cs/nOverlay1  | fsb/Ready0r  | ram/RAMReady  | A_FSB<8>  | A_FSB<15>  | A_FSB<14>  | A_FSB<13>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | cnt/TimeoutA  | fsb/Ready2r  | fsb/VPA  | $OpTx$FX_DC$591  | A_FSB<9>  | iobs/BERR  | cnt/TimeoutB  | fsb/BERR0r  | fsb/BERR1r  | fsb/Ready1r  | nBR_IOB  | iobs/IOReady  | EXP16_.EXP
INPUTMC | 15 | 0 | 17 | 2 | 3 | 6 | 14 | 3 | 15 | 2 | 15 | 2 | 0 | 0 | 12 | 7 | 15 | 6 | 12 | 2 | 11 | 0 | 16 | 2 | 14 | 7 | 14 | 3 | 16 | 2 | 4
INPUTP | 17 | 36 | 30 | 29 | 11 | 21 | 19 | 18 | 17 | 15 | 13 | 28 | 26 | 24 | 23 | 22 | 47 | 12
EXPORTS | 1 | 2 | 2
IMPORTS | 1 | 2 | 4
EQ | 24 | 
   !fsb/Ready0r.D = !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!fsb/Ready0r & !ram/RAMReady
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !fsb/Ready0r & !ram/RAMReady
;Imported pterms FB3_5
	# nAS_FSB & !fsb/ASrf;
   fsb/Ready0r.CLK = CLK_FSB;	// GCK
    fsb/Ready0r.EXP  =  A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & fsb/Ready1r & nBR_IOB & 
	!$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & iobs/IOReady & nBR_IOB & 
	!$OpTx$FX_DC$591
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 2 | 14 | fsb/Ready1r
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 11 | 2 | 13 | 2 | 7 | 2 | 1 | 2 | 3 | 2 | 6 | 2 | 9 | 2 | 11 | 2 | 12 | 2 | 16 | 2 | 17 | 2 | 15
INPUTS | 22 | nAS_FSB  | fsb/ASrf  | A_FSB<8>  | A_FSB<15>  | A_FSB<14>  | A_FSB<13>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | cs/nOverlay1  | cnt/TimeoutA  | fsb/Ready2r  | EXP22_.EXP
INPUTMC | 5 | 0 | 5 | 0 | 17 | 3 | 15 | 2 | 15 | 2 | 13
INPUTP | 17 | 54 | 11 | 21 | 19 | 18 | 17 | 15 | 13 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 47
EXPORTS | 1 | 2 | 15
IMPORTS | 1 | 2 | 13
EQ | 37 | 
   !fsb/Ready1r.D = nAS_FSB & !fsb/ASrf
;Imported pterms FB3_14
	# A_FSB<23> & !fsb/Ready1r & !iobs/IOReady
	# A_FSB<22> & !A_FSB<21> & A_FSB<20> & !fsb/Ready1r & 
	!iobs/IOReady
	# A_FSB<22> & !A_FSB<21> & !fsb/Ready1r & 
	!iobs/IOReady & !SW<1>
	# A_FSB<14> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & !iobs/IOReady
	# A_FSB<13> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & !iobs/IOReady
;Imported pterms FB3_13
	# A_FSB<14> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & !nADoutLE1
	# A_FSB<13> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & !nADoutLE1;
   fsb/Ready1r.CLK = CLK_FSB;	// GCK
    fsb/Ready1r.EXP  =  nAS_FSB & !fsb/ASrf
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 2 | 15 | fsb/Ready2r
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 7 | 2 | 15 | 2 | 8 | 2 | 2 | 2 | 3 | 2 | 7 | 2 | 14 | 2 | 16
INPUTS | 21 | A_FSB<9>  | A_FSB<15>  | A_FSB<14>  | A_FSB<13>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | cs/nOverlay1  | cnt/TimeoutA  | fsb/Ready2r  | A_FSB<8>  | fsb/Ready1r.EXP
INPUTMC | 4 | 0 | 17 | 3 | 15 | 2 | 15 | 2 | 14
INPUTP | 17 | 12 | 21 | 19 | 18 | 17 | 15 | 13 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 47 | 11
IMPORTS | 1 | 2 | 14
EQ | 43 | 
   !fsb/Ready2r.D = A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
	# A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
;Imported pterms FB3_15
	# nAS_FSB & !fsb/ASrf
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r;
   fsb/Ready2r.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 2 | 0 | fsb/VPA
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 7 | 2 | 0 | 3 | 10 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 16 | 2 | 17
INPUTS | 10 | fsb/VPA  | nBR_IOB  | $OpTx$FX_DC$591  | fsb/BERR0r  | fsb/BERR1r  | iobs/BERR  | A_FSB<20>  | cnt/TimeoutB  | EXP14_.EXP  | EXP23_.EXP
INPUTMC | 9 | 2 | 0 | 7 | 14 | 0 | 12 | 2 | 11 | 0 | 16 | 7 | 15 | 6 | 12 | 2 | 1 | 2 | 17
INPUTP | 1 | 28
IMPORTS | 2 | 2 | 1 | 2 | 17
EQ | 95 | 
   fsb/VPA.D = iobs/BERR & fsb/VPA & !$OpTx$FX_DC$591
	# fsb/BERR0r & fsb/VPA & !$OpTx$FX_DC$591
	# fsb/BERR1r & fsb/VPA & !$OpTx$FX_DC$591
	# fsb/VPA & !nBR_IOB & !$OpTx$FX_DC$591
	# !A_FSB<20> & cnt/TimeoutB & fsb/VPA & 
	!$OpTx$FX_DC$591
;Imported pterms FB3_2
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!fsb/Ready0r & fsb/VPA & !ram/RAMReady & !$OpTx$FX_DC$591
	# A_FSB<22> & !A_FSB<21> & !fsb/Ready1r & fsb/VPA & 
	!iobs/IOReady & !SW<1> & !$OpTx$FX_DC$591
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !fsb/Ready0r & fsb/VPA & !ram/RAMReady & 
	!$OpTx$FX_DC$591
	# A_FSB<14> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & fsb/VPA & !iobs/IOReady & !$OpTx$FX_DC$591
	# A_FSB<13> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & fsb/VPA & !iobs/IOReady & !$OpTx$FX_DC$591
;Imported pterms FB3_3
	# A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
;Imported pterms FB3_4
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & fsb/Ready1r & nBR_IOB & 
	!$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & iobs/IOReady & nBR_IOB & 
	!$OpTx$FX_DC$591
;Imported pterms FB3_18
	# A_FSB<23> & cnt/TimeoutB & fsb/VPA & 
	!$OpTx$FX_DC$591
	# !A_FSB<22> & cnt/TimeoutB & fsb/VPA & 
	!$OpTx$FX_DC$591
	# A_FSB<21> & cnt/TimeoutB & fsb/VPA & 
	!$OpTx$FX_DC$591
	# A_FSB<23> & !fsb/Ready1r & fsb/VPA & 
	!iobs/IOReady & !$OpTx$FX_DC$591
	# A_FSB<22> & !A_FSB<21> & A_FSB<20> & !fsb/Ready1r & 
	fsb/VPA & !iobs/IOReady & !$OpTx$FX_DC$591
;Imported pterms FB3_17
	# A_FSB<14> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & fsb/VPA & !iobs/IOReady & 
	!nADoutLE1 & !$OpTx$FX_DC$591
	# A_FSB<13> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & fsb/VPA & !iobs/IOReady & 
	!nADoutLE1 & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591;
   fsb/VPA.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 4 | 3 | iobs/IOL0
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 1 | 5 | 8
INPUTS | 5 | iobs/IOL1  | nADoutLE1  | nLDS_FSB  | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1
INPUTMC | 4 | 0 | 14 | 5 | 13 | 7 | 3 | 3 | 12
INPUTP | 1 | 49
EQ | 4 | 
   iobs/IOL0.D = !nLDS_FSB & nADoutLE1
	# iobs/IOL1 & !nADoutLE1;
   iobs/IOL0.CLK = CLK_FSB;	// GCK
   iobs/IOL0.CE = iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1;
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 14 | iobs/IOL1
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 1 | 4 | 3
INPUTS | 2 | nLDS_FSB  | iobs/Load1
INPUTMC | 1 | 4 | 12
INPUTP | 1 | 49
EQ | 3 | 
   iobs/IOL1.D = !nLDS_FSB;
   iobs/IOL1.CLK = CLK_FSB;	// GCK
   iobs/IOL1.CE = iobs/Load1;
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 7 | 13 | iobs/IORW1
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 2 | 7 | 0 | 7 | 13
INPUTS | 8 | A_FSB<23>  | A_FSB<21>  | iobs/IORW1  | nADoutLE1  | iobs/Once  | nWE_FSB  | EXP36_.EXP  | Park.EXP
INPUTMC | 5 | 7 | 13 | 5 | 13 | 4 | 6 | 7 | 12 | 7 | 14
INPUTP | 3 | 36 | 29 | 47
IMPORTS | 2 | 7 | 12 | 7 | 14
EQ | 22 | 
   !iobs/IORW1.T = iobs/Once
	# !nADoutLE1
	# nWE_FSB & iobs/IORW1
	# !nWE_FSB & !iobs/IORW1
	# !A_FSB<23> & A_FSB<21> & !iobs/IORW1
;Imported pterms FB8_13
	# nAS_FSB & !fsb/ASrf
	# !iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21>
	# !A_FSB<23> & !A_FSB<22> & !cs/nOverlay1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20>
;Imported pterms FB8_12
	# !A_FSB<23> & !A_FSB<20> & SW<1>
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1
;Imported pterms FB8_15
	# !A_FSB<23> & A_FSB<21> & !A_FSB<19>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<18>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16>;
   iobs/IORW1.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 16 | iobs/IOReady
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 12 | 2 | 13 | 2 | 7 | 3 | 16 | 2 | 1 | 2 | 3 | 2 | 5 | 2 | 6 | 2 | 9 | 2 | 12 | 2 | 16 | 2 | 17 | 3 | 17
INPUTS | 18 | iobs/IOReady  | nAS_FSB  | fsb/ASrf  | iobs/Once  | iobs/PS_FSM_FFd2  | iobs/IOACTr  | iobm/IOBERR  | nADoutLE1  | A_FSB<23>  | A_FSB<22>  | cnt/RefDone  | ram/Once  | cs/nOverlay1  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>
INPUTMC | 15 | 3 | 16 | 0 | 5 | 4 | 6 | 7 | 3 | 1 | 6 | 5 | 17 | 5 | 13 | 3 | 13 | 4 | 9 | 0 | 17 | 3 | 17 | 6 | 9 | 3 | 7 | 3 | 6 | 3 | 3
INPUTP | 3 | 54 | 36 | 30
EXPORTS | 1 | 3 | 17
EQ | 11 | 
   iobs/IOReady.T = iobs/IOReady & nAS_FSB & !fsb/ASrf
	# iobs/Once & iobs/IOReady & !iobs/PS_FSM_FFd2 & 
	!iobs/IOACTr & iobm/IOBERR & nADoutLE1
	# iobs/Once & !iobs/IOReady & !nAS_FSB & 
	!iobs/PS_FSM_FFd2 & !iobs/IOACTr & !iobm/IOBERR & nADoutLE1
	# iobs/Once & !iobs/IOReady & !iobs/PS_FSM_FFd2 & 
	!iobs/IOACTr & !iobm/IOBERR & fsb/ASrf & nADoutLE1;
   iobs/IOReady.CLK = CLK_FSB;	// GCK
    iobs/IOReady.EXP  =  !A_FSB<23> & !A_FSB<22> & !cnt/RefDone & ram/Once & 
	cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 14 | iobs/IOU0
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 1 | 5 | 10
INPUTS | 5 | iobs/IOU1  | nADoutLE1  | nUDS_FSB  | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1
INPUTMC | 4 | 0 | 13 | 5 | 13 | 7 | 3 | 3 | 12
INPUTP | 1 | 56
EQ | 4 | 
   iobs/IOU0.D = !nUDS_FSB & nADoutLE1
	# iobs/IOU1 & !nADoutLE1;
   iobs/IOU0.CLK = CLK_FSB;	// GCK
   iobs/IOU0.CE = iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1;
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 13 | iobs/IOU1
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 1 | 3 | 14
INPUTS | 2 | nUDS_FSB  | iobs/Load1
INPUTMC | 1 | 4 | 12
INPUTP | 1 | 56
EQ | 3 | 
   iobs/IOU1.D = !nUDS_FSB;
   iobs/IOU1.CLK = CLK_FSB;	// GCK
   iobs/IOU1.CE = iobs/Load1;
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 4 | 2 | ram/RAMDIS2
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 4 | 4 | 2 | 4 | 1 | 7 | 5 | 7 | 6
INPUTS | 15 | ram/RAMDIS2  | nAS_FSB  | fsb/ASrf  | cnt/RefDone  | ram/Once  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | nROMCS_OBUF.EXP
INPUTMC | 12 | 4 | 2 | 0 | 5 | 3 | 13 | 4 | 9 | 3 | 17 | 6 | 9 | 6 | 3 | 3 | 7 | 3 | 6 | 3 | 3 | 0 | 17 | 4 | 1
INPUTP | 3 | 54 | 36 | 30
IMPORTS | 1 | 4 | 1
EQ | 23 | 
   ram/RAMDIS2.T = ram/RAMDIS2 & nAS_FSB & !fsb/ASrf
	# !cnt/RefDone & ram/Once & !ram/RAMDIS2 & !nAS_FSB & 
	ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !cnt/RefDone & ram/Once & !ram/RAMDIS2 & 
	ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & !cnt/RefDone & ram/Once & 
	cs/nOverlay1 & !ram/RAMDIS2 & !nAS_FSB & !ram/RS_FSM_FFd2 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !A_FSB<23> & !A_FSB<22> & !cnt/RefDone & ram/Once & 
	cs/nOverlay1 & !ram/RAMDIS2 & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf
;Imported pterms FB5_2
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	ram/Once & !cs/nOverlay1 & !ram/RAMDIS2 & !nAS_FSB & 
	!ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	ram/Once & !cs/nOverlay1 & !ram/RAMDIS2 & !ram/RS_FSM_FFd2 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & 
	fsb/ASrf;
   ram/RAMDIS2.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 2 | 8 | fsb/nDTACK
ATTRIBUTES | 8815362 | 0
OUTPUTMC | 5 | 2 | 8 | 2 | 6 | 2 | 7 | 2 | 9 | 2 | 10
INPUTS | 23 | A_FSB<9>  | A_FSB<15>  | A_FSB<14>  | A_FSB<13>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | cs/nOverlay1  | cnt/TimeoutA  | fsb/Ready2r  | nDTACK_FSB  | A_FSB<8>  | EXP19_.EXP  | EXP20_.EXP
INPUTMC | 6 | 0 | 17 | 3 | 15 | 2 | 15 | 2 | 8 | 2 | 7 | 2 | 9
INPUTP | 17 | 12 | 21 | 19 | 18 | 17 | 15 | 13 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 47 | 11
IMPORTS | 2 | 2 | 7 | 2 | 9
EQ | 90 | 
   nDTACK_FSB.D = A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
	# A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
;Imported pterms FB3_8
	# A_FSB<14> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & !iobs/IOReady & nDTACK_FSB
	# A_FSB<14> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & nDTACK_FSB & 
	!nADoutLE1
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
;Imported pterms FB3_7
	# A_FSB<23> & cnt/TimeoutB & nDTACK_FSB
	# !A_FSB<22> & cnt/TimeoutB & nDTACK_FSB
	# !A_FSB<20> & cnt/TimeoutB & nDTACK_FSB
	# A_FSB<23> & !fsb/Ready1r & !iobs/IOReady & 
	nDTACK_FSB
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!fsb/Ready0r & nDTACK_FSB & !ram/RAMReady
;Imported pterms FB3_6
	# nAS_FSB & !fsb/ASrf
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & iobs/IOReady & nBR_IOB
;Imported pterms FB3_10
	# A_FSB<22> & !A_FSB<21> & A_FSB<20> & !fsb/Ready1r & 
	!iobs/IOReady & nDTACK_FSB
	# A_FSB<22> & !A_FSB<21> & !fsb/Ready1r & 
	!iobs/IOReady & nDTACK_FSB & !SW<1>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !fsb/Ready0r & nDTACK_FSB & !ram/RAMReady
	# A_FSB<13> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & !iobs/IOReady & nDTACK_FSB
	# A_FSB<13> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & nDTACK_FSB & 
	!nADoutLE1
;Imported pterms FB3_11
	# iobs/BERR & nDTACK_FSB
	# fsb/BERR0r & nDTACK_FSB
	# fsb/BERR1r & nDTACK_FSB
	# nDTACK_FSB & !nBR_IOB
	# A_FSB<21> & cnt/TimeoutB & nDTACK_FSB
;Imported pterms FB3_12
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & fsb/Ready1r & nBR_IOB;
   nDTACK_FSB.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 17 | ram/RS_FSM_FFd1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 21 | 4 | 9 | 4 | 2 | 3 | 17 | 4 | 17 | 6 | 9 | 6 | 3 | 0 | 0 | 6 | 17 | 6 | 14 | 3 | 0 | 3 | 16 | 4 | 0 | 4 | 15 | 4 | 16 | 6 | 0 | 6 | 1 | 6 | 2 | 6 | 4 | 6 | 13 | 6 | 15 | 6 | 16
INPUTS | 15 | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | cnt/RefDone  | nAS_FSB  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | ram/Once  | cs/nOverlay1  | iobs/Clear1.EXP  | iobs/IOReady.EXP
INPUTMC | 12 | 3 | 17 | 6 | 9 | 6 | 3 | 3 | 13 | 3 | 7 | 3 | 6 | 3 | 3 | 0 | 5 | 4 | 9 | 0 | 17 | 3 | 0 | 3 | 16
INPUTP | 3 | 54 | 36 | 30
IMPORTS | 2 | 3 | 0 | 3 | 16
EQ | 21 | 
   ram/RS_FSM_FFd1.D = ram/RS_FSM_FFd1 & ram/RS_FSM_FFd2
	# !ram/RS_FSM_FFd1 & ram/RS_FSM_FFd3
	# !cnt/RefDone & !nAS_FSB & ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !cnt/RefDone & ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & !cnt/RefDone & ram/Once & 
	cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
;Imported pterms FB4_1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	ram/Once & !cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	ram/Once & !cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf
;Imported pterms FB4_17
	# !A_FSB<23> & !A_FSB<22> & !cnt/RefDone & ram/Once & 
	cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf;
   ram/RS_FSM_FFd1.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 4 | 17 | ram/RASEL
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 10 | 6 | 5 | 6 | 1 | 6 | 6 | 4 | 10 | 4 | 8 | 4 | 4 | 4 | 14 | 6 | 4 | 6 | 7 | 6 | 11
INPUTS | 13 | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | ram/RS_FSM_FFd1  | A_FSB<23>  | cnt/RefDone  | nAS_FSB  | ram/BACTr  | fsb/ASrf  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | EXP24_.EXP  | EXP27_.EXP
INPUTMC | 11 | 6 | 9 | 6 | 3 | 3 | 17 | 3 | 13 | 0 | 1 | 0 | 5 | 3 | 7 | 3 | 6 | 3 | 3 | 4 | 0 | 4 | 16
INPUTP | 2 | 36 | 54
IMPORTS | 2 | 4 | 0 | 4 | 16
EQ | 44 | 
   ram/RASEL.D = !ram/RS_FSM_FFd2 & ram/RS_FSM_FFd3
	# !ram/RS_FSM_FFd1 & ram/RS_FSM_FFd2 & 
	!ram/RS_FSM_FFd3
	# A_FSB<23> & !cnt/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr
	# A_FSB<23> & !cnt/RefDone & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd2 & !ram/BACTr & fsb/ASrf
	# !cnt/RefDone & nAS_FSB & !ram/RS_FSM_FFd2 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & !fsb/ASrf
;Imported pterms FB5_1
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr & fsb/ASrf
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr & fsb/ASrf
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
;Imported pterms FB5_17
	# A_FSB<23> & !cnt/RefDone & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & fsb/ASrf
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr & fsb/ASrf
;Imported pterms FB5_16
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & fsb/ASrf
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>;
   ram/RASEL.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 6 | 9 | ram/RS_FSM_FFd2
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 18 | 4 | 9 | 4 | 2 | 3 | 17 | 4 | 17 | 6 | 9 | 6 | 3 | 0 | 0 | 6 | 17 | 6 | 14 | 3 | 0 | 3 | 16 | 4 | 0 | 4 | 1 | 4 | 15 | 4 | 16 | 6 | 2 | 6 | 8 | 6 | 10
INPUTS | 10 | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | nAS_FSB  | ram/RS_FSM_FFd3  | fsb/ASrf  | cnt/RefDone  | cnt/RefCnt<7>  | ram/BACTr  | A_FSB_21_IBUF$BUF0.EXP  | RA_9_OBUF.EXP
INPUTMC | 9 | 3 | 17 | 6 | 9 | 6 | 3 | 0 | 5 | 3 | 13 | 3 | 3 | 0 | 1 | 6 | 8 | 6 | 10
INPUTP | 1 | 54
IMPORTS | 2 | 6 | 8 | 6 | 10
EQ | 27 | 
   !ram/RS_FSM_FFd2.D = ram/RS_FSM_FFd1 & ram/RS_FSM_FFd2
	# cnt/RefDone & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3
	# !nAS_FSB & ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3
	# ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & fsb/ASrf
	# !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<7> & ram/BACTr
;Imported pterms FB7_9
	# !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<5> & ram/BACTr
	# !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<6> & ram/BACTr
	# nAS_FSB & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<5> & !fsb/ASrf
	# nAS_FSB & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<7> & !fsb/ASrf
;Imported pterms FB7_11
	# nAS_FSB & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<6> & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & !nAS_FSB & 
	!ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & fsb/ASrf;
   ram/RS_FSM_FFd2.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 5 | 2 | iobm/IOS_FSM_FFd3
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 13 | 5 | 11 | 5 | 8 | 5 | 10 | 5 | 2 | 0 | 15 | 5 | 9 | 5 | 17 | 5 | 15 | 5 | 6 | 3 | 4 | 5 | 0 | 5 | 14 | 5 | 16
INPUTS | 6 | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd2  | iobm/IOS_FSM_FFd3  | CLK_IOB  | iobm/IOREQr  | nAoutOE
INPUTMC | 5 | 0 | 15 | 5 | 9 | 5 | 2 | 1 | 9 | 3 | 1
INPUTP | 1 | 35
EQ | 6 | 
   iobm/IOS_FSM_FFd3.D = iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2
	# iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd1 & 
	!iobm/IOS_FSM_FFd2
	# !CLK_IOB & !iobm/IOS_FSM_FFd1 & !iobm/IOS_FSM_FFd2 & 
	iobm/IOREQr & !nAoutOE;
   iobm/IOS_FSM_FFd3.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 0 | 15 | iobm/IOS_FSM_FFd1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 12 | 5 | 11 | 5 | 8 | 5 | 10 | 5 | 2 | 0 | 15 | 5 | 9 | 5 | 17 | 5 | 15 | 5 | 6 | 5 | 16 | 5 | 0 | 5 | 14
INPUTS | 3 | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd2  | iobm/IOS_FSM_FFd1
INPUTMC | 3 | 5 | 2 | 5 | 9 | 0 | 15
EQ | 3 | 
   iobm/IOS_FSM_FFd1.D = iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1
	# !iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd2;
   iobm/IOS_FSM_FFd1.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 5 | 9 | iobm/IOS_FSM_FFd2
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 12 | 5 | 11 | 5 | 8 | 5 | 10 | 5 | 2 | 0 | 15 | 5 | 9 | 5 | 17 | 5 | 15 | 5 | 6 | 5 | 16 | 3 | 4 | 5 | 0
INPUTS | 11 | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd2  | CLK_IOB  | iobm/ETACK  | iobm/BERRrf  | iobm/BERRrr  | iobm/DTACKrf  | iobm/DTACKrr  | iobm/RESrf  | iobm/RESrr
INPUTMC | 10 | 5 | 2 | 0 | 15 | 5 | 9 | 5 | 0 | 0 | 4 | 1 | 16 | 1 | 13 | 1 | 12 | 0 | 3 | 0 | 2
INPUTP | 1 | 35
EQ | 11 | 
   iobm/IOS_FSM_FFd2.T = iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd1 & 
	!iobm/IOS_FSM_FFd2
	# CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/IOS_FSM_FFd2 & iobm/ETACK
	# CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/IOS_FSM_FFd2 & iobm/BERRrf & iobm/BERRrr
	# CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/IOS_FSM_FFd2 & iobm/DTACKrf & iobm/DTACKrr
	# CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/IOS_FSM_FFd2 & iobm/RESrf & iobm/RESrr;
   iobm/IOS_FSM_FFd2.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 6 | 3 | ram/RS_FSM_FFd3
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 16 | 4 | 9 | 4 | 2 | 3 | 17 | 4 | 17 | 6 | 9 | 6 | 3 | 6 | 17 | 6 | 14 | 4 | 1 | 6 | 0 | 6 | 1 | 6 | 2 | 6 | 4 | 6 | 8 | 6 | 10 | 6 | 16
INPUTS | 12 | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | A_FSB<23>  | A_FSB<22>  | ram/Once  | cs/nOverlay1  | nAS_FSB  | ram/RS_FSM_FFd3  | fsb/ASrf  | A_FSB<21>  | EXP29_.EXP  | RA_7_OBUF.EXP
INPUTMC | 8 | 3 | 17 | 6 | 9 | 4 | 9 | 0 | 17 | 6 | 3 | 0 | 5 | 6 | 2 | 6 | 4
INPUTP | 4 | 36 | 30 | 54 | 29
IMPORTS | 2 | 6 | 2 | 6 | 4
EQ | 30 | 
   ram/RS_FSM_FFd3.D = !ram/RS_FSM_FFd1 & ram/RS_FSM_FFd2
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & fsb/ASrf
;Imported pterms FB7_3
	# !cnt/RefDone & !nAS_FSB & ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !cnt/RefDone & ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & 
	fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & !cnt/RefDone & 
	cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !A_FSB<23> & !A_FSB<22> & !cnt/RefDone & 
	cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
;Imported pterms FB7_5
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf;
   ram/RS_FSM_FFd3.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 7 | 3 | iobs/PS_FSM_FFd2
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 17 | 4 | 6 | 7 | 15 | 7 | 9 | 4 | 3 | 7 | 12 | 3 | 16 | 3 | 14 | 7 | 3 | 3 | 12 | 4 | 12 | 3 | 2 | 3 | 0 | 7 | 8 | 7 | 1 | 7 | 2 | 7 | 4 | 7 | 7
INPUTS | 12 | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | iobs/IOACTr  | iobs/Once  | nADoutLE1  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | EXP33_.EXP  | nRAS_OBUF.EXP
INPUTMC | 9 | 7 | 3 | 3 | 12 | 1 | 6 | 4 | 6 | 5 | 13 | 0 | 5 | 0 | 17 | 7 | 2 | 7 | 4
INPUTP | 3 | 54 | 36 | 30
IMPORTS | 2 | 7 | 2 | 7 | 4
EQ | 33 | 
   !iobs/PS_FSM_FFd2.D = iobs/PS_FSM_FFd2 & iobs/PS_FSM_FFd1 & 
	iobs/IOACTr
	# !iobs/PS_FSM_FFd2 & iobs/PS_FSM_FFd1 & 
	!iobs/IOACTr
	# iobs/Once & !iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & 
	nADoutLE1
	# nAS_FSB & !iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & 
	!fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !cs/nOverlay1 & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
;Imported pterms FB8_3
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<19> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
;Imported pterms FB8_5
	# !A_FSB<23> & A_FSB<21> & !A_FSB<18> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & nWE_FSB & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & !A_FSB<20> & !iobs/PS_FSM_FFd2 & 
	!iobs/PS_FSM_FFd1 & SW<1> & nADoutLE1
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1 & !iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1;
   iobs/PS_FSM_FFd2.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 7 | cnt/RefCnt<5>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 22 | 3 | 13 | 3 | 15 | 6 | 12 | 6 | 6 | 4 | 2 | 3 | 17 | 4 | 17 | 6 | 8 | 6 | 2 | 3 | 6 | 3 | 3 | 6 | 17 | 6 | 14 | 3 | 0 | 3 | 16 | 4 | 0 | 4 | 1 | 4 | 15 | 4 | 16 | 6 | 0 | 6 | 1 | 6 | 4
INPUTS | 5 | cnt/RefCnt<0>  | cnt/RefCnt<1>  | cnt/RefCnt<3>  | cnt/RefCnt<2>  | cnt/RefCnt<4>
INPUTMC | 5 | 1 | 17 | 0 | 6 | 3 | 9 | 3 | 11 | 3 | 8
EQ | 3 | 
   cnt/RefCnt<5>.T = cnt/RefCnt<0> & cnt/RefCnt<1> & cnt/RefCnt<3> & 
	cnt/RefCnt<2> & cnt/RefCnt<4>;
   cnt/RefCnt<5>.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 6 | cnt/RefCnt<6>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 22 | 3 | 13 | 3 | 15 | 6 | 12 | 6 | 6 | 4 | 2 | 3 | 17 | 4 | 17 | 6 | 8 | 6 | 2 | 3 | 3 | 6 | 17 | 6 | 14 | 3 | 0 | 3 | 16 | 4 | 0 | 4 | 1 | 4 | 15 | 4 | 16 | 6 | 0 | 6 | 1 | 6 | 4 | 6 | 10
INPUTS | 6 | cnt/RefCnt<5>  | cnt/RefCnt<0>  | cnt/RefCnt<1>  | cnt/RefCnt<3>  | cnt/RefCnt<2>  | cnt/RefCnt<4>
INPUTMC | 6 | 3 | 7 | 1 | 17 | 0 | 6 | 3 | 9 | 3 | 11 | 3 | 8
EQ | 3 | 
   cnt/RefCnt<6>.T = cnt/RefCnt<5> & cnt/RefCnt<0> & cnt/RefCnt<1> & 
	cnt/RefCnt<3> & cnt/RefCnt<2> & cnt/RefCnt<4>;
   cnt/RefCnt<6>.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 5 | 5 | iobm/ES<0>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 7 | 5 | 1 | 5 | 5 | 5 | 4 | 5 | 12 | 5 | 3 | 5 | 7 | 5 | 0
INPUTS | 7 | iobm/ES<0>  | iobm/Er  | iobm/Er2  | iobm/ES<1>  | iobm/ES<2>  | iobm/ES<3>  | iobm/ES<4>
INPUTMC | 7 | 5 | 5 | 1 | 11 | 1 | 10 | 5 | 4 | 5 | 12 | 5 | 3 | 5 | 7
EQ | 6 | 
   !iobm/ES<0>.T = iobm/ES<0> & !iobm/Er & iobm/Er2
	# !iobm/ES<0> & !iobm/ES<1> & !iobm/ES<2> & 
	!iobm/ES<3> & !iobm/ES<4> & iobm/Er
	# !iobm/ES<0> & !iobm/ES<1> & !iobm/ES<2> & 
	!iobm/ES<3> & !iobm/ES<4> & !iobm/Er2;
   iobm/ES<0>.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 3 | 12 | iobs/PS_FSM_FFd1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 14 | 4 | 6 | 7 | 4 | 4 | 3 | 7 | 12 | 3 | 14 | 7 | 3 | 3 | 12 | 4 | 12 | 3 | 2 | 3 | 0 | 7 | 8 | 4 | 5 | 7 | 1 | 7 | 2
INPUTS | 3 | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | iobs/IOACTr
INPUTMC | 3 | 7 | 3 | 3 | 12 | 1 | 6
EQ | 3 | 
   iobs/PS_FSM_FFd1.D = iobs/PS_FSM_FFd2
	# iobs/PS_FSM_FFd1 & iobs/IOACTr;
   iobs/PS_FSM_FFd1.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 5 | 4 | iobm/ES<1>
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 7 | 5 | 1 | 5 | 5 | 5 | 4 | 5 | 12 | 5 | 3 | 5 | 7 | 5 | 0
INPUTS | 4 | iobm/ES<0>  | iobm/ES<1>  | iobm/Er  | iobm/Er2
INPUTMC | 4 | 5 | 5 | 5 | 4 | 1 | 11 | 1 | 10
EQ | 4 | 
   !iobm/ES<1>.D = iobm/ES<0> & iobm/ES<1>
	# !iobm/ES<0> & !iobm/ES<1>
	# !iobm/Er & iobm/Er2;
   iobm/ES<1>.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 17 | cnt/RefCnt<0>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 11 | 3 | 13 | 3 | 15 | 6 | 12 | 6 | 6 | 3 | 7 | 3 | 6 | 3 | 3 | 0 | 6 | 3 | 9 | 3 | 11 | 3 | 8
INPUTS | 0
EQ | 2 | 
   cnt/RefCnt<0>.T = Vcc;
   cnt/RefCnt<0>.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 3 | cnt/RefCnt<7>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 20 | 3 | 13 | 6 | 12 | 6 | 6 | 4 | 2 | 3 | 17 | 4 | 17 | 6 | 9 | 6 | 2 | 6 | 17 | 6 | 14 | 3 | 0 | 3 | 16 | 4 | 0 | 4 | 1 | 4 | 15 | 4 | 16 | 6 | 0 | 6 | 1 | 6 | 4 | 6 | 8
INPUTS | 7 | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<0>  | cnt/RefCnt<1>  | cnt/RefCnt<3>  | cnt/RefCnt<2>  | cnt/RefCnt<4>
INPUTMC | 7 | 3 | 7 | 3 | 6 | 1 | 17 | 0 | 6 | 3 | 9 | 3 | 11 | 3 | 8
EQ | 3 | 
   cnt/RefCnt<7>.T = cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<0> & 
	cnt/RefCnt<1> & cnt/RefCnt<3> & cnt/RefCnt<2> & cnt/RefCnt<4>;
   cnt/RefCnt<7>.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 5 | 12 | iobm/ES<2>
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 6 | 5 | 1 | 5 | 5 | 5 | 12 | 5 | 3 | 5 | 7 | 5 | 0
INPUTS | 7 | iobm/ES<0>  | iobm/ES<2>  | iobm/ES<1>  | iobm/Er  | iobm/Er2  | iobm/ES<3>  | iobm/ES<4>
INPUTMC | 7 | 5 | 5 | 5 | 12 | 5 | 4 | 1 | 11 | 1 | 10 | 5 | 3 | 5 | 7
EQ | 6 | 
   !iobm/ES<2>.D = !iobm/ES<0> & !iobm/ES<2>
	# !iobm/ES<1> & !iobm/ES<2>
	# !iobm/Er & iobm/Er2
	# iobm/ES<0> & iobm/ES<1> & iobm/ES<2>
	# !iobm/ES<2> & !iobm/ES<3> & iobm/ES<4>;
   iobm/ES<2>.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 5 | 3 | iobm/ES<3>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 6 | 5 | 1 | 5 | 5 | 5 | 12 | 5 | 3 | 5 | 7 | 5 | 0
INPUTS | 6 | iobm/ES<3>  | iobm/Er  | iobm/Er2  | iobm/ES<0>  | iobm/ES<1>  | iobm/ES<2>
INPUTMC | 6 | 5 | 3 | 1 | 11 | 1 | 10 | 5 | 5 | 5 | 4 | 5 | 12
EQ | 4 | 
   iobm/ES<3>.T = iobm/ES<3> & !iobm/Er & iobm/Er2
	# iobm/ES<0> & iobm/ES<1> & iobm/ES<2> & iobm/Er
	# iobm/ES<0> & iobm/ES<1> & iobm/ES<2> & !iobm/Er2;
   iobm/ES<3>.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 5 | 7 | iobm/ES<4>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 5 | 5 | 1 | 5 | 5 | 5 | 12 | 5 | 7 | 5 | 0
INPUTS | 7 | iobm/ES<4>  | iobm/Er  | iobm/Er2  | iobm/ES<0>  | iobm/ES<1>  | iobm/ES<2>  | iobm/ES<3>
INPUTMC | 7 | 5 | 7 | 1 | 11 | 1 | 10 | 5 | 5 | 5 | 4 | 5 | 12 | 5 | 3
EQ | 8 | 
   iobm/ES<4>.T = iobm/ES<4> & !iobm/Er & iobm/Er2
	# iobm/ES<0> & iobm/ES<1> & iobm/ES<2> & 
	iobm/ES<3> & iobm/Er
	# iobm/ES<0> & iobm/ES<1> & iobm/ES<2> & 
	iobm/ES<3> & !iobm/Er2
	# iobm/ES<0> & iobm/ES<1> & !iobm/ES<2> & 
	!iobm/ES<3> & iobm/ES<4>;
   iobm/ES<4>.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 0 | 6 | cnt/RefCnt<1>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 10 | 3 | 13 | 3 | 15 | 6 | 12 | 6 | 6 | 3 | 7 | 3 | 6 | 3 | 3 | 3 | 9 | 3 | 11 | 3 | 8
INPUTS | 1 | cnt/RefCnt<0>
INPUTMC | 1 | 1 | 17
EQ | 2 | 
   cnt/RefCnt<1>.T = cnt/RefCnt<0>;
   cnt/RefCnt<1>.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 9 | cnt/RefCnt<3>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 8 | 3 | 13 | 3 | 15 | 6 | 12 | 6 | 6 | 3 | 7 | 3 | 6 | 3 | 3 | 3 | 8
INPUTS | 3 | cnt/RefCnt<0>  | cnt/RefCnt<1>  | cnt/RefCnt<2>
INPUTMC | 3 | 1 | 17 | 0 | 6 | 3 | 11
EQ | 2 | 
   cnt/RefCnt<3>.T = cnt/RefCnt<0> & cnt/RefCnt<1> & cnt/RefCnt<2>;
   cnt/RefCnt<3>.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 1 | 6 | iobs/IOACTr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 5 | 7 | 15 | 3 | 16 | 7 | 3 | 3 | 12 | 7 | 8
INPUTS | 1 | iobm/IOACT
INPUTMC | 1 | 5 | 15
EQ | 2 | 
   iobs/IOACTr.D = iobm/IOACT;
   iobs/IOACTr.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 11 | cnt/RefCnt<2>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 9 | 3 | 13 | 3 | 15 | 6 | 12 | 6 | 6 | 3 | 7 | 3 | 6 | 3 | 3 | 3 | 9 | 3 | 8
INPUTS | 2 | cnt/RefCnt<0>  | cnt/RefCnt<1>
INPUTMC | 2 | 1 | 17 | 0 | 6
EQ | 2 | 
   cnt/RefCnt<2>.T = cnt/RefCnt<0> & cnt/RefCnt<1>;
   cnt/RefCnt<2>.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 8 | cnt/RefCnt<4>
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 7 | 3 | 13 | 3 | 15 | 6 | 12 | 6 | 6 | 3 | 7 | 3 | 6 | 3 | 3
INPUTS | 4 | cnt/RefCnt<0>  | cnt/RefCnt<1>  | cnt/RefCnt<3>  | cnt/RefCnt<2>
INPUTMC | 4 | 1 | 17 | 0 | 6 | 3 | 9 | 3 | 11
EQ | 3 | 
   cnt/RefCnt<4>.T = cnt/RefCnt<0> & cnt/RefCnt<1> & cnt/RefCnt<3> & 
	cnt/RefCnt<2>;
   cnt/RefCnt<4>.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 4 | 12 | iobs/Load1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 0 | 14 | 0 | 13 | 5 | 13
INPUTS | 11 | nADoutLE1  | iobs/Once  | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | RA_5_OBUF.EXP  | RA_2_OBUF.EXP
INPUTMC | 8 | 5 | 13 | 4 | 6 | 7 | 3 | 3 | 12 | 0 | 5 | 0 | 17 | 4 | 11 | 4 | 13
INPUTP | 3 | 54 | 36 | 30
IMPORTS | 2 | 4 | 11 | 4 | 13
EQ | 19 | 
   !iobs/Load1.D = iobs/Once
	# !nADoutLE1
	# nAS_FSB & !fsb/ASrf
	# !iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1
	# !A_FSB<23> & !A_FSB<22> & !cs/nOverlay1
;Imported pterms FB5_12
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<19>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16>
;Imported pterms FB5_14
	# !A_FSB<23> & A_FSB<21> & !A_FSB<18>
	# !A_FSB<23> & A_FSB<21> & nWE_FSB
	# !A_FSB<23> & !A_FSB<20> & SW<1>
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1;
   iobs/Load1.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 1 | ram/BACTr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 11 | 4 | 17 | 6 | 9 | 6 | 17 | 6 | 14 | 4 | 0 | 4 | 16 | 6 | 0 | 6 | 8 | 6 | 13 | 6 | 15 | 6 | 16
INPUTS | 2 | nAS_FSB  | fsb/ASrf
INPUTMC | 1 | 0 | 5
INPUTP | 1 | 54
EQ | 2 | 
   !ram/BACTr.D = nAS_FSB & !fsb/ASrf;
   ram/BACTr.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 9 | RESr0
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 0 | 8 | 7 | 6 | 7 | 14
INPUTS | 1 | nRES
INPUTP | 1 | 145
EQ | 2 | 
   RESr0.D = !nRES;
   RESr0.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 8 | RESr1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 0 | 7 | 7 | 6 | 7 | 14
INPUTS | 1 | RESr0
INPUTMC | 1 | 0 | 9
EQ | 2 | 
   RESr1.D = RESr0;
   RESr1.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 5 | 17 | iobm/IOBERR
ATTRIBUTES | 4358912 | 0
OUTPUTMC | 4 | 7 | 15 | 3 | 16 | 5 | 17 | 5 | 0
INPUTS | 12 | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd2  | iobm/IOBERR  | CLK_IOB  | nBERR_IOB  | iobm/ETACK  | iobm/BERRrf  | iobm/BERRrr  | iobm/DTACKrf  | iobm/DTACKrr  | iobm/ETACK.EXP
INPUTMC | 10 | 5 | 2 | 0 | 15 | 5 | 9 | 5 | 17 | 5 | 0 | 0 | 4 | 1 | 16 | 1 | 13 | 1 | 12 | 5 | 0
INPUTP | 2 | 35 | 123
IMPORTS | 1 | 5 | 0
EQ | 26 | 
   iobm/IOBERR.T = iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd1 & 
	!iobm/IOS_FSM_FFd2 & iobm/IOBERR
	# CLK_IOB & nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & iobm/IOBERR & iobm/ETACK
	# CLK_IOB & !nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & !iobm/IOBERR & iobm/ETACK
	# CLK_IOB & nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & iobm/IOBERR & iobm/BERRrf & 
	iobm/BERRrr
	# CLK_IOB & nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & iobm/IOBERR & iobm/DTACKrf & 
	iobm/DTACKrr
;Imported pterms FB6_1
	# CLK_IOB & nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & iobm/IOBERR & iobm/RESrf & 
	iobm/RESrr
	# CLK_IOB & !nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & !iobm/IOBERR & iobm/BERRrf & 
	iobm/BERRrr
	# CLK_IOB & !nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & !iobm/IOBERR & iobm/DTACKrf & 
	iobm/DTACKrr
	# CLK_IOB & !nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & !iobm/IOBERR & iobm/RESrf & 
	iobm/RESrr;
   iobm/IOBERR.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 0 | 11 | IPL2r0
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 0 | 10 | 7 | 14
INPUTS | 1 | nIPL2
INPUTP | 1 | 146
EQ | 2 | 
   IPL2r0.D = !nIPL2;
   IPL2r0.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 7 | RESr2
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 7 | 6 | 7 | 14
INPUTS | 1 | RESr1
INPUTMC | 1 | 0 | 8
EQ | 2 | 
   RESr2.D = RESr1;
   RESr2.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 1 | 15 | iobm/BGr0
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 1 | 14 | 3 | 1
INPUTS | 1 | nBG_IOB
INPUTP | 1 | 117
EQ | 2 | 
   iobm/BGr0.D = !nBG_IOB;
   iobm/BGr0.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 5 | 0 | iobm/ETACK
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 5 | 9 | 5 | 17 | 5 | 15
INPUTS | 18 | nVMA_IOB  | iobm/ES<0>  | iobm/ES<1>  | iobm/ES<2>  | iobm/ES<3>  | iobm/ES<4>  | CLK_IOB  | nBERR_IOB  | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd2  | iobm/IOBERR  | iobm/RESrf  | iobm/RESrr  | iobm/BERRrf  | iobm/BERRrr  | iobm/DTACKrf  | iobm/DTACKrr
INPUTMC | 16 | 5 | 1 | 5 | 5 | 5 | 4 | 5 | 12 | 5 | 3 | 5 | 7 | 5 | 2 | 0 | 15 | 5 | 9 | 5 | 17 | 0 | 3 | 0 | 2 | 0 | 4 | 1 | 16 | 1 | 13 | 1 | 12
INPUTP | 2 | 35 | 123
EXPORTS | 1 | 5 | 17
EQ | 15 | 
   iobm/ETACK.D = !nVMA_IOB & !iobm/ES<0> & !iobm/ES<1> & !iobm/ES<2> & 
	!iobm/ES<3> & iobm/ES<4>;
   iobm/ETACK.CLK = CLK2X_IOB;	// GCK
    iobm/ETACK.EXP  =  CLK_IOB & nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & iobm/IOBERR & iobm/RESrf & 
	iobm/RESrr
	# CLK_IOB & !nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & !iobm/IOBERR & iobm/BERRrf & 
	iobm/BERRrr
	# CLK_IOB & !nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & !iobm/IOBERR & iobm/DTACKrf & 
	iobm/DTACKrr
	# CLK_IOB & !nBERR_IOB & iobm/IOS_FSM_FFd3 & 
	iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2 & !iobm/IOBERR & iobm/RESrf & 
	iobm/RESrr
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 11 | iobm/Er
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 6 | 5 | 5 | 5 | 4 | 5 | 12 | 5 | 3 | 5 | 7 | 1 | 10
INPUTS | 1 | E_IOB
INPUTP | 1 | 37
EQ | 2 | 
   iobm/Er.D = E_IOB;
   !iobm/Er.CLK = CLK_IOB;	// GCK
GLOBALS | 1 | 2 | CLK_IOB

MACROCELL | 5 | 15 | iobm/IOACT
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 5 | 1 | 1 | 6
INPUTS | 11 | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd2  | iobm/IOS_FSM_FFd3  | iobm/IOREQr  | nAoutOE  | CLK_IOB  | iobm/ETACK  | iobm/BERRrf  | iobm/BERRrr  | nADoutLE0_OBUF.EXP  | iobm/nDinLE.EXP
INPUTMC | 10 | 0 | 15 | 5 | 9 | 5 | 2 | 1 | 9 | 3 | 1 | 5 | 0 | 0 | 4 | 1 | 16 | 5 | 14 | 5 | 16
INPUTP | 1 | 35
IMPORTS | 2 | 5 | 14 | 5 | 16
EQ | 15 | 
   !iobm/IOACT.D = iobm/IOS_FSM_FFd1 & !iobm/IOS_FSM_FFd2
	# !iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd2 & 
	!iobm/IOREQr
	# !iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd2 & nAoutOE
	# CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/ETACK
	# CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/BERRrf & iobm/BERRrr
;Imported pterms FB6_15
	# CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/DTACKrf & iobm/DTACKrr
;Imported pterms FB6_17
	# CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/RESrf & iobm/RESrr;
   iobm/IOACT.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 9 | iobm/IOREQr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 5 | 2 | 5 | 15 | 5 | 6
INPUTS | 1 | iobs/IOREQ
INPUTMC | 1 | 7 | 8
EQ | 2 | 
   iobm/IOREQr.D = iobs/IOREQ;
   !iobm/IOREQr.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 0 | 0 | ram/RefRAS
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 3 | 13 | 7 | 5
INPUTS | 2 | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2
INPUTMC | 2 | 3 | 17 | 6 | 9
EQ | 2 | 
   ram/RefRAS.D = !ram/RS_FSM_FFd1 & ram/RS_FSM_FFd2;
   ram/RefRAS.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 7 | 6 | RESDone
ATTRIBUTES | 8553280 | 0
OUTPUTMC | 2 | 7 | 14 | 7 | 7
INPUTS | 8 | RESr0  | RESr1  | RESr2  | nWE_FSB  | nUDS_FSB  | ram/RAMDIS2  | nAS_FSB  | ram/RAMDIS1
INPUTMC | 5 | 0 | 9 | 0 | 8 | 0 | 7 | 4 | 2 | 6 | 17
INPUTP | 3 | 47 | 56 | 54
EXPORTS | 1 | 7 | 7
EQ | 5 | 
   RESDone.D = Vcc;
   RESDone.CLK = CLK_FSB;	// GCK
   RESDone.CE = !RESr0 & !RESr1 & RESr2;
    RESDone.EXP  =  !nWE_FSB & !nUDS_FSB & !ram/RAMDIS2 & !nAS_FSB & 
	!ram/RAMDIS1
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 10 | IPL2r1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 7 | 14
INPUTS | 1 | IPL2r0
INPUTMC | 1 | 0 | 11
EQ | 2 | 
   IPL2r1.D = IPL2r0;
   IPL2r1.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 0 | 5 | fsb/ASrf
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 41 | 4 | 9 | 4 | 6 | 0 | 17 | 7 | 15 | 7 | 0 | 2 | 12 | 3 | 15 | 6 | 12 | 6 | 6 | 2 | 11 | 0 | 16 | 0 | 12 | 2 | 14 | 2 | 4 | 7 | 12 | 3 | 16 | 4 | 2 | 2 | 5 | 3 | 17 | 4 | 17 | 6 | 9 | 6 | 3 | 7 | 3 | 4 | 12 | 0 | 1 | 7 | 8 | 6 | 17 | 6 | 14 | 3 | 0 | 4 | 0 | 4 | 1 | 4 | 15 | 4 | 16 | 6 | 0 | 6 | 2 | 6 | 4 | 6 | 8 | 6 | 10 | 6 | 13 | 6 | 15 | 6 | 16
INPUTS | 1 | nAS_FSB
INPUTP | 1 | 54
EQ | 2 | 
   fsb/ASrf.D = !nAS_FSB;
   !fsb/ASrf.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 5 | 6 | iobm/ALE0
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 5 | 14
INPUTS | 5 | iobm/IOS_FSM_FFd2  | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd1  | iobm/IOREQr  | nAoutOE
INPUTMC | 5 | 5 | 9 | 5 | 2 | 0 | 15 | 1 | 9 | 3 | 1
EQ | 4 | 
   iobm/ALE0.D = iobm/IOS_FSM_FFd2
	# iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd1
	# !iobm/IOS_FSM_FFd1 & iobm/IOREQr & !nAoutOE;
   iobm/ALE0.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 0 | 4 | iobm/BERRrf
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 5 | 9 | 5 | 17 | 5 | 15 | 5 | 0
INPUTS | 1 | nBERR_IOB
INPUTP | 1 | 123
EQ | 2 | 
   iobm/BERRrf.D = !nBERR_IOB;
   !iobm/BERRrf.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 16 | iobm/BERRrr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 5 | 9 | 5 | 17 | 5 | 15 | 5 | 0
INPUTS | 1 | nBERR_IOB
INPUTP | 1 | 123
EQ | 2 | 
   iobm/BERRrr.D = !nBERR_IOB;
   iobm/BERRrr.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 14 | iobm/BGr1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 3 | 1
INPUTS | 1 | iobm/BGr0
INPUTMC | 1 | 1 | 15
EQ | 2 | 
   iobm/BGr1.D = iobm/BGr0;
   iobm/BGr1.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 13 | iobm/DTACKrf
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 5 | 9 | 5 | 17 | 5 | 14 | 5 | 0
INPUTS | 1 | nDTACK_IOB
INPUTP | 1 | 127
EQ | 2 | 
   iobm/DTACKrf.D = !nDTACK_IOB;
   !iobm/DTACKrf.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 12 | iobm/DTACKrr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 5 | 9 | 5 | 17 | 5 | 14 | 5 | 0
INPUTS | 1 | nDTACK_IOB
INPUTP | 1 | 127
EQ | 2 | 
   iobm/DTACKrr.D = !nDTACK_IOB;
   iobm/DTACKrr.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 10 | iobm/Er2
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 5 | 5 | 5 | 5 | 4 | 5 | 12 | 5 | 3 | 5 | 7
INPUTS | 1 | iobm/Er
INPUTMC | 1 | 1 | 11
EQ | 2 | 
   iobm/Er2.D = iobm/Er;
   iobm/Er2.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 0 | 3 | iobm/RESrf
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 5 | 9 | 5 | 16 | 5 | 0
INPUTS | 1 | nRES
INPUTP | 1 | 145
EQ | 2 | 
   iobm/RESrf.D = !nRES;
   !iobm/RESrf.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 0 | 2 | iobm/RESrr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 3 | 5 | 9 | 5 | 16 | 5 | 0
INPUTS | 1 | nRES
INPUTP | 1 | 145
EQ | 2 | 
   iobm/RESrr.D = !nRES;
   iobm/RESrr.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 8 | iobm/VPArf
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 5 | 1
INPUTS | 1 | nVPA_IOB
INPUTP | 1 | 125
EQ | 2 | 
   iobm/VPArf.D = !nVPA_IOB;
   !iobm/VPArf.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 1 | 7 | iobm/VPArr
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 5 | 1
INPUTS | 1 | nVPA_IOB
INPUTP | 1 | 125
EQ | 2 | 
   iobm/VPArr.D = !nVPA_IOB;
   iobm/VPArr.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 3 | 2 | iobs/ALE0
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 5 | 14
INPUTS | 2 | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1
INPUTMC | 2 | 7 | 3 | 3 | 12
EQ | 2 | 
   iobs/ALE0.D = iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1;
   iobs/ALE0.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 0 | iobs/Clear1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 5 | 13 | 3 | 17
INPUTS | 16 | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | nADoutLE1  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | cnt/RefDone  | ram/Once  | cs/nOverlay1  | nAS_FSB  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | fsb/ASrf
INPUTMC | 12 | 7 | 3 | 3 | 12 | 5 | 13 | 3 | 13 | 4 | 9 | 0 | 17 | 3 | 17 | 6 | 9 | 3 | 7 | 3 | 6 | 3 | 3 | 0 | 5
INPUTP | 4 | 36 | 30 | 29 | 54
EXPORTS | 1 | 3 | 17
EQ | 8 | 
   iobs/Clear1.D = iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & !nADoutLE1;
   iobs/Clear1.CLK = CLK_FSB;	// GCK
    iobs/Clear1.EXP  =  !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	ram/Once & !cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	ram/Once & !cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 7 | 8 | iobs/IOREQ
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 1 | 1 | 9
INPUTS | 12 | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | iobs/IOACTr  | iobs/Once  | nADoutLE1  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | nRAMUWE_OBUF.EXP  | EXP34_.EXP
INPUTMC | 9 | 7 | 3 | 3 | 12 | 1 | 6 | 4 | 6 | 5 | 13 | 0 | 5 | 0 | 17 | 7 | 7 | 7 | 9
INPUTP | 3 | 54 | 36 | 30
IMPORTS | 2 | 7 | 7 | 7 | 9
EQ | 30 | 
   !iobs/IOREQ.D = !iobs/PS_FSM_FFd2 & iobs/PS_FSM_FFd1
	# iobs/PS_FSM_FFd1 & iobs/IOACTr
	# iobs/Once & !iobs/PS_FSM_FFd2 & nADoutLE1
	# nAS_FSB & !iobs/PS_FSM_FFd2 & !fsb/ASrf & 
	nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !cs/nOverlay1 & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
;Imported pterms FB8_8
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<19> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
;Imported pterms FB8_10
	# !A_FSB<23> & A_FSB<21> & !A_FSB<18> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & nWE_FSB & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<20> & !iobs/PS_FSM_FFd2 & 
	SW<1> & nADoutLE1
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1 & !iobs/PS_FSM_FFd2 & nADoutLE1;
   iobs/IOREQ.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 6 | 17 | ram/RAMDIS1
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 2 | 7 | 6 | 7 | 5
INPUTS | 13 | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd3  | ram/RS_FSM_FFd2  | A_FSB<23>  | cnt/RefDone  | nAS_FSB  | ram/BACTr  | fsb/ASrf  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | EXP28_.EXP  | EXP31_.EXP
INPUTMC | 11 | 3 | 17 | 6 | 3 | 6 | 9 | 3 | 13 | 0 | 1 | 0 | 5 | 3 | 7 | 3 | 6 | 3 | 3 | 6 | 0 | 6 | 16
INPUTP | 2 | 36 | 54
IMPORTS | 2 | 6 | 0 | 6 | 16
EQ | 40 | 
   ram/RAMDIS1.D = ram/RS_FSM_FFd1 & ram/RS_FSM_FFd3
	# !ram/RS_FSM_FFd1 & ram/RS_FSM_FFd2
	# A_FSB<23> & !cnt/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr
	# A_FSB<23> & !cnt/RefDone & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd3 & !ram/BACTr & fsb/ASrf
	# !cnt/RefDone & ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
;Imported pterms FB7_1
	# A_FSB<23> & !cnt/RefDone & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr & fsb/ASrf
	# !cnt/RefDone & ram/Once & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !cnt/RefDone & nAS_FSB & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & 
	!fsb/ASrf
;Imported pterms FB7_2
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
;Imported pterms FB7_17
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr & fsb/ASrf
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr & fsb/ASrf
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr;
   ram/RAMDIS1.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 6 | 14 | ram/RAMReady
ATTRIBUTES | 8553216 | 0
OUTPUTMC | 4 | 2 | 3 | 2 | 6 | 2 | 1 | 2 | 9
INPUTS | 13 | ram/RS_FSM_FFd3  | ram/RS_FSM_FFd2  | cnt/RefDone  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | A_FSB<23>  | nAS_FSB  | ram/RS_FSM_FFd1  | ram/BACTr  | fsb/ASrf  | CLK20EN_OBUF$BUF0.EXP  | EXP30_.EXP
INPUTMC | 11 | 6 | 3 | 6 | 9 | 3 | 13 | 3 | 7 | 3 | 6 | 3 | 3 | 3 | 17 | 0 | 1 | 0 | 5 | 6 | 13 | 6 | 15
INPUTP | 2 | 36 | 54
IMPORTS | 2 | 6 | 13 | 6 | 15
EQ | 31 | 
   !ram/RAMReady.D = ram/RS_FSM_FFd2
	# ram/RS_FSM_FFd3
	# !cnt/RefDone & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# A_FSB<23> & !cnt/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/BACTr
	# A_FSB<23> & !cnt/RefDone & !ram/RS_FSM_FFd1 & 
	!ram/BACTr & fsb/ASrf
;Imported pterms FB7_14
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & fsb/ASrf
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/BACTr
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/BACTr
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/BACTr
;Imported pterms FB7_16
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/BACTr & fsb/ASrf
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/BACTr & fsb/ASrf
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/BACTr & fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd1 & fsb/ASrf;
   ram/RAMReady.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 6 | 5 | RA_0_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 3 | A_FSB<10>  | ram/RASEL  | A_FSB<1>
INPUTMC | 1 | 4 | 17
INPUTP | 2 | 13 | 149
EQ | 2 | 
   RA<0> = A_FSB<10> & !ram/RASEL
	# ram/RASEL & A_FSB<1>;

MACROCELL | 6 | 1 | RA_1_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 6 | 0
INPUTS | 11 | A_FSB<11>  | ram/RASEL  | A_FSB<2>  | A_FSB<22>  | cnt/RefDone  | cs/nOverlay1  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd3  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>
INPUTMC | 8 | 4 | 17 | 3 | 13 | 0 | 17 | 3 | 17 | 6 | 3 | 3 | 7 | 3 | 6 | 3 | 3
INPUTP | 3 | 15 | 153 | 30
EXPORTS | 1 | 6 | 0
EQ | 8 | 
   RA<1> = A_FSB<11> & !ram/RASEL
	# ram/RASEL & A_FSB<2>;
    RA_1_OBUF.EXP  =  A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>

MACROCELL | 4 | 13 | RA_2_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 12
INPUTS | 11 | A_FSB<23>  | A_FSB<21>  | A_FSB<18>  | nWE_FSB  | A_FSB<20>  | SW<1>  | A_FSB<14>  | A_FSB<13>  | A_FSB<22>  | cs/nOverlay1  | RA_6_OBUF.EXP
INPUTMC | 2 | 0 | 17 | 4 | 14
INPUTP | 9 | 36 | 29 | 24 | 47 | 28 | 97 | 19 | 18 | 30
EXPORTS | 1 | 4 | 12
IMPORTS | 1 | 4 | 14
EQ | 9 | 
   RA<2> = ;Imported pterms FB5_15
	  A_FSB<12> & !ram/RASEL
	# ram/RASEL & A_FSB<3>;
    RA_2_OBUF.EXP  =  !A_FSB<23> & A_FSB<21> & !A_FSB<18>
	# !A_FSB<23> & A_FSB<21> & nWE_FSB
	# !A_FSB<23> & !A_FSB<20> & SW<1>
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1

MACROCELL | 4 | 10 | RA_3_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 11
INPUTS | 5 | A_FSB<13>  | ram/RASEL  | A_FSB<4>  | A_FSB<15>  | A_FSB<6>
INPUTMC | 1 | 4 | 17
INPUTP | 4 | 18 | 157 | 21 | 6
EXPORTS | 1 | 4 | 11
EQ | 4 | 
   RA<3> = A_FSB<13> & !ram/RASEL
	# ram/RASEL & A_FSB<4>;
    RA_3_OBUF.EXP  =  A_FSB<15> & !ram/RASEL
	# ram/RASEL & A_FSB<6>

MACROCELL | 4 | 8 | RA_4_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 7
INPUTS | 11 | A_FSB<14>  | ram/RASEL  | A_FSB<5>  | A_FSB<23>  | A_FSB<20>  | iobs/Once  | SW<1>  | A_FSB<13>  | A_FSB<21>  | A_FSB<22>  | cs/nOverlay1
INPUTMC | 3 | 4 | 17 | 4 | 6 | 0 | 17
INPUTP | 8 | 19 | 4 | 36 | 28 | 97 | 18 | 29 | 30
EXPORTS | 1 | 4 | 7
EQ | 7 | 
   RA<4> = A_FSB<14> & !ram/RASEL
	# ram/RASEL & A_FSB<5>;
    RA_4_OBUF.EXP  =  !A_FSB<23> & !A_FSB<20> & !iobs/Once & SW<1>
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21> & 
	!iobs/Once
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !iobs/Once & 
	cs/nOverlay1

MACROCELL | 4 | 11 | RA_5_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 12
INPUTS | 8 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<17>  | A_FSB<16>  | RA_3_OBUF.EXP
INPUTMC | 1 | 4 | 10
INPUTP | 7 | 36 | 30 | 29 | 28 | 26 | 23 | 22
EXPORTS | 1 | 4 | 12
IMPORTS | 1 | 4 | 10
EQ | 8 | 
   RA<5> = ;Imported pterms FB5_11
	  A_FSB<15> & !ram/RASEL
	# ram/RASEL & A_FSB<6>;
    RA_5_OBUF.EXP  =  !A_FSB<23> & !A_FSB<22> & !A_FSB<21>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<19>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16>

MACROCELL | 4 | 14 | RA_6_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 13
INPUTS | 5 | A_FSB<16>  | ram/RASEL  | A_FSB<7>  | A_FSB<12>  | A_FSB<3>
INPUTMC | 1 | 4 | 17
INPUTP | 4 | 22 | 8 | 17 | 155
EXPORTS | 1 | 4 | 13
EQ | 4 | 
   RA<6> = A_FSB<16> & !ram/RASEL
	# ram/RASEL & A_FSB<7>;
    RA_6_OBUF.EXP  =  A_FSB<12> & !ram/RASEL
	# ram/RASEL & A_FSB<3>

MACROCELL | 6 | 4 | RA_7_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 6 | 3
INPUTS | 14 | A_FSB<17>  | ram/RASEL  | A_FSB<8>  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | cnt/RefDone  | cs/nOverlay1  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd3  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | fsb/ASrf
INPUTMC | 9 | 4 | 17 | 3 | 13 | 0 | 17 | 3 | 17 | 6 | 3 | 3 | 7 | 3 | 6 | 3 | 3 | 0 | 5
INPUTP | 5 | 23 | 11 | 36 | 30 | 29
EXPORTS | 1 | 6 | 3
EQ | 5 | 
   RA<7> = A_FSB<8> & ram/RASEL
	# A_FSB<17> & !ram/RASEL;
    RA_7_OBUF.EXP  =  !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf

MACROCELL | 6 | 7 | RA_8_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 7 | A_FSB<23>  | A_FSB<18>  | ram/RASEL  | A_FSB<22>  | A_FSB<21>  | cs/nOverlay1  | cnt/TimeoutBPre.EXP
INPUTMC | 3 | 4 | 17 | 0 | 17 | 6 | 6
INPUTP | 4 | 36 | 24 | 30 | 29
IMPORTS | 1 | 6 | 6
EQ | 10 | 
   RA<8> = A_FSB<23> & A_FSB<18>
	# A_FSB<18> & !ram/RASEL
	# A_FSB<22> & !A_FSB<21> & A_FSB<18>
	# A_FSB<22> & A_FSB<18> & cs/nOverlay1
	# !A_FSB<22> & A_FSB<18> & !cs/nOverlay1
;Imported pterms FB7_7
	# A_FSB<9> & !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	ram/RASEL
	# A_FSB<9> & !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & ram/RASEL;

MACROCELL | 6 | 10 | RA_9_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 6 | 9
INPUTS | 10 | nAS_FSB  | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | cnt/RefCnt<6>  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | A_FSB<21>  | CLK25EN_OBUF.EXP
INPUTMC | 6 | 6 | 9 | 6 | 3 | 3 | 6 | 0 | 5 | 0 | 17 | 6 | 11
INPUTP | 4 | 54 | 36 | 30 | 29
EXPORTS | 1 | 6 | 9
IMPORTS | 1 | 6 | 11
EQ | 13 | 
   RA<9> = ;Imported pterms FB7_12
	  A_FSB<20> & ram/RASEL
	# A_FSB<19> & !ram/RASEL;
    RA_9_OBUF.EXP  =  nAS_FSB & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<6> & !fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & !nAS_FSB & 
	!ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & fsb/ASrf

MACROCELL | 7 | 11 | nBERR_FSB_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 7 | 12
INPUTS | 14 | nAS_FSB  | iobs/BERR  | cnt/TimeoutB  | fsb/BERR0r  | fsb/BERR1r  | A_FSB<23>  | A_FSB<20>  | SW<1>  | A_FSB<14>  | A_FSB<13>  | A_FSB<21>  | A_FSB<22>  | cs/nOverlay1  | EXP35_.EXP
INPUTMC | 6 | 7 | 15 | 6 | 12 | 2 | 11 | 0 | 16 | 0 | 17 | 7 | 10
INPUTP | 8 | 54 | 36 | 28 | 97 | 19 | 18 | 29 | 30
EXPORTS | 1 | 7 | 12
IMPORTS | 1 | 7 | 10
EQ | 10 | 
   nBERR_FSB = nAS_FSB
	# !iobs/BERR & !cnt/TimeoutB & !fsb/BERR0r & 
	!fsb/BERR1r
;Imported pterms FB8_11
	# !A_FSB<23> & A_FSB<22> & !A_FSB<21> & A_FSB<20> & 
	!iobs/BERR & !fsb/BERR0r & !fsb/BERR1r;
    nBERR_FSB_OBUF.EXP  =  !A_FSB<23> & !A_FSB<20> & SW<1>
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1

MACROCELL | 4 | 5 | nOE_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 6
INPUTS | 9 | A_FSB<23>  | iobs/Once  | iobs/PS_FSM_FFd1  | nADoutLE1  | A_FSB<22>  | A_FSB<21>  | cs/nOverlay1  | A_FSB<20>  | ram/nCAS.EXP
INPUTMC | 5 | 4 | 6 | 3 | 12 | 5 | 13 | 0 | 17 | 4 | 4
INPUTP | 4 | 36 | 30 | 29 | 28
EXPORTS | 1 | 4 | 6
IMPORTS | 1 | 4 | 4
EQ | 8 | 
   !nOE = ;Imported pterms FB5_5
	  nWE_FSB & !nAS_FSB;
    nOE_OBUF.EXP  =  A_FSB<23> & !iobs/Once & iobs/PS_FSM_FFd1
	# !iobs/Once & iobs/PS_FSM_FFd1 & !nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & !iobs/Once
	# !A_FSB<23> & !A_FSB<22> & !iobs/Once & 
	!cs/nOverlay1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20> & !iobs/Once

MACROCELL | 2 | 16 | nROMWE_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 2 | 17
INPUTS | 26 | nWE_FSB  | nAS_FSB  | A_FSB<14>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | cs/nOverlay1  | fsb/Ready1r  | fsb/VPA  | iobs/IOReady  | nADoutLE1  | $OpTx$FX_DC$591  | A_FSB<13>  | A_FSB<9>  | A_FSB<15>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<23>  | cnt/TimeoutA  | fsb/Ready2r  | A_FSB<8>
INPUTMC | 8 | 0 | 17 | 2 | 14 | 2 | 0 | 3 | 16 | 5 | 13 | 0 | 12 | 3 | 15 | 2 | 15
INPUTP | 18 | 47 | 54 | 19 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 18 | 12 | 21 | 17 | 15 | 13 | 36 | 11
EXPORTS | 1 | 2 | 17
EQ | 19 | 
   !nROMWE = !nWE_FSB & !nAS_FSB;
    nROMWE_OBUF.EXP  =  A_FSB<14> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & fsb/VPA & !iobs/IOReady & 
	!nADoutLE1 & !$OpTx$FX_DC$591
	# A_FSB<13> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & fsb/VPA & !iobs/IOReady & 
	!nADoutLE1 & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591

MACROCELL | 3 | 10 | nVPA_FSB_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 2 | fsb/VPA  | nAS_FSB
INPUTMC | 1 | 2 | 0
INPUTP | 1 | 54
EQ | 1 | 
   !nVPA_FSB = fsb/VPA & !nAS_FSB;

MACROCELL | 5 | 16 | iobm/nDinLE
ATTRIBUTES | 8684290 | 0
OUTPUTMC | 1 | 5 | 15
INPUTS | 6 | iobm/IOS_FSM_FFd1  | iobm/IOS_FSM_FFd2  | CLK_IOB  | iobm/IOS_FSM_FFd3  | iobm/RESrf  | iobm/RESrr
INPUTMC | 5 | 0 | 15 | 5 | 9 | 5 | 2 | 0 | 3 | 0 | 2
INPUTP | 1 | 35
EXPORTS | 1 | 5 | 15
EQ | 4 | 
   nDinLE.D = iobm/IOS_FSM_FFd1 & iobm/IOS_FSM_FFd2;
   !nDinLE.CLK = CLK2X_IOB;	// GCK
    iobm/nDinLE.EXP  =  CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/RESrf & iobm/RESrr
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 3 | 4 | iobm/nDoutOE
ATTRIBUTES | 8684290 | 0
INPUTS | 3 | iobs/IORW0  | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd2
INPUTMC | 3 | 7 | 17 | 5 | 2 | 5 | 9
EQ | 3 | 
   nDoutOE.D = !iobs/IORW0
	# !iobm/IOS_FSM_FFd3 & !iobm/IOS_FSM_FFd2;
   nDoutOE.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 5 | 14 | nADoutLE0_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 5 | 15
INPUTS | 7 | iobm/ALE0  | iobs/ALE0  | CLK_IOB  | iobm/IOS_FSM_FFd3  | iobm/IOS_FSM_FFd1  | iobm/DTACKrf  | iobm/DTACKrr
INPUTMC | 6 | 5 | 6 | 3 | 2 | 5 | 2 | 0 | 15 | 1 | 13 | 1 | 12
INPUTP | 1 | 35
EXPORTS | 1 | 5 | 15
EQ | 3 | 
   nADoutLE0 = !iobm/ALE0 & !iobs/ALE0;
    nADoutLE0_OBUF.EXP  =  CLK_IOB & iobm/IOS_FSM_FFd3 & iobm/IOS_FSM_FFd1 & 
	iobm/DTACKrf & iobm/DTACKrr

MACROCELL | 3 | 5 | nDinOE_OBUF
ATTRIBUTES | 264962 | 0
INPUTS | 7 | A_FSB<23>  | nWE_FSB  | nAS_FSB  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | SW<1>
INPUTP | 7 | 36 | 47 | 54 | 30 | 29 | 28 | 97
EQ | 5 | 
   nDinOE = A_FSB<23> & nWE_FSB & !nAS_FSB
	# A_FSB<22> & !A_FSB<21> & A_FSB<20> & nWE_FSB & 
	!nAS_FSB
	# A_FSB<22> & !A_FSB<21> & nWE_FSB & !nAS_FSB & 
	!SW<1>;

MACROCELL | 7 | 4 | nRAS_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 7 | 3
INPUTS | 14 | A_FSB<23>  | A_FSB<21>  | A_FSB<18>  | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | nADoutLE1  | nWE_FSB  | A_FSB<20>  | SW<1>  | A_FSB<14>  | A_FSB<13>  | A_FSB<22>  | cs/nOverlay1  | nRAMLWE_OBUF.EXP
INPUTMC | 5 | 7 | 3 | 3 | 12 | 5 | 13 | 0 | 17 | 7 | 5
INPUTP | 9 | 36 | 29 | 24 | 47 | 28 | 97 | 19 | 18 | 30
EXPORTS | 1 | 7 | 3
IMPORTS | 1 | 7 | 5
EQ | 16 | 
   !nRAS = ;Imported pterms FB8_6
	  ram/RefRAS
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!ram/RAMDIS2 & !nAS_FSB & !ram/RAMDIS1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !ram/RAMDIS2 & !nAS_FSB & !ram/RAMDIS1;
    nRAS_OBUF.EXP  =  !A_FSB<23> & A_FSB<21> & !A_FSB<18> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & nWE_FSB & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & !A_FSB<20> & !iobs/PS_FSM_FFd2 & 
	!iobs/PS_FSM_FFd1 & SW<1> & nADoutLE1
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1 & !iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1

MACROCELL | 4 | 4 | ram/nCAS
ATTRIBUTES | 8684290 | 0
OUTPUTMC | 1 | 4 | 5
INPUTS | 3 | ram/RASEL  | nWE_FSB  | nAS_FSB
INPUTMC | 1 | 4 | 17
INPUTP | 2 | 47 | 54
EXPORTS | 1 | 4 | 5
EQ | 3 | 
   nCAS.D = !ram/RASEL;
   !nCAS.CLK = CLK_FSB;	// GCK
    ram/nCAS.EXP  =  nWE_FSB & !nAS_FSB
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 7 | 1 | A_FSB_19_IBUF$BUF0
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 7 | 0
INPUTS | 7 | A_FSB<19>  | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | iobs/Once  | nADoutLE1  | nWE_FSB  | iobs/IORW0
INPUTMC | 5 | 7 | 3 | 3 | 12 | 4 | 6 | 5 | 13 | 7 | 17
INPUTP | 2 | 26 | 47
EXPORTS | 1 | 7 | 0
EQ | 5 | 
   RA<11> = A_FSB<19>;
    A_FSB_19_IBUF$BUF0.EXP  =  iobs/PS_FSM_FFd2
	# iobs/PS_FSM_FFd1
	# iobs/Once & nADoutLE1
	# nWE_FSB & iobs/IORW0 & nADoutLE1

MACROCELL | 6 | 8 | A_FSB_21_IBUF$BUF0
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 6 | 9
INPUTS | 9 | A_FSB<21>  | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | cnt/RefCnt<5>  | ram/BACTr  | cnt/RefCnt<6>  | nAS_FSB  | fsb/ASrf  | cnt/RefCnt<7>
INPUTMC | 7 | 6 | 9 | 6 | 3 | 3 | 7 | 0 | 1 | 3 | 6 | 0 | 5 | 3 | 3
INPUTP | 2 | 29 | 54
EXPORTS | 1 | 6 | 9
EQ | 9 | 
   RA<10> = A_FSB<21>;
    A_FSB_21_IBUF$BUF0.EXP  =  !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<5> & ram/BACTr
	# !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<6> & ram/BACTr
	# nAS_FSB & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<5> & !fsb/ASrf
	# nAS_FSB & !ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & 
	!cnt/RefCnt<7> & !fsb/ASrf

MACROCELL | 6 | 13 | CLK20EN_OBUF$BUF0
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 6 | 14
INPUTS | 11 | A_FSB<23>  | A_FSB<22>  | ram/Once  | cs/nOverlay1  | nAS_FSB  | ram/RS_FSM_FFd1  | fsb/ASrf  | A_FSB<21>  | cnt/RefDone  | ram/BACTr  | cnt/TimeoutB.EXP
INPUTMC | 7 | 4 | 9 | 0 | 17 | 3 | 17 | 0 | 5 | 3 | 13 | 0 | 1 | 6 | 12
INPUTP | 4 | 36 | 30 | 54 | 29
EXPORTS | 1 | 6 | 14
IMPORTS | 1 | 6 | 12
EQ | 12 | 
   CLK20EN = ;Imported pterms FB7_13
	  SW<0>;
    CLK20EN_OBUF$BUF0.EXP  =  !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & fsb/ASrf
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/BACTr
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/BACTr
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/BACTr

MACROCELL | 6 | 11 | CLK25EN_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 6 | 10
INPUTS | 4 | SW<0>  | A_FSB<20>  | ram/RASEL  | A_FSB<19>
INPUTMC | 1 | 4 | 17
INPUTP | 3 | 98 | 28 | 26
EXPORTS | 1 | 6 | 10
EQ | 3 | 
   CLK25EN = !SW<0>;
    CLK25EN_OBUF.EXP  =  A_FSB<20> & ram/RASEL
	# A_FSB<19> & !ram/RASEL

MACROCELL | 7 | 14 | Park
ATTRIBUTES | 8815430 | 0
OUTPUTMC | 6 | 2 | 0 | 2 | 5 | 2 | 3 | 2 | 10 | 2 | 11 | 7 | 13
INPUTS | 12 | RESr0  | RESr1  | IPL2r0  | RESr2  | RESDone  | IPL2r1  | A_FSB<23>  | A_FSB<21>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>
INPUTMC | 6 | 0 | 9 | 0 | 8 | 0 | 11 | 0 | 7 | 7 | 6 | 0 | 10
INPUTP | 6 | 36 | 29 | 26 | 24 | 23 | 22
EXPORTS | 1 | 7 | 13
EQ | 8 | 
   nBR_IOB.D = Gnd;
   nBR_IOB.CLK = CLK_FSB;	// GCK
   nBR_IOB.CE = RESr0 & RESr1 & IPL2r0 & RESr2 & !RESDone & 
	IPL2r1;
    Park.EXP  =  !A_FSB<23> & A_FSB<21> & !A_FSB<19>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<18>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17>
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16>
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 5 | 13 | nADoutLE1_OBUF
ATTRIBUTES | 8815366 | 0
OUTPUTMC | 24 | 4 | 6 | 7 | 15 | 7 | 17 | 2 | 12 | 5 | 13 | 4 | 3 | 7 | 13 | 3 | 16 | 3 | 14 | 2 | 7 | 7 | 3 | 4 | 12 | 3 | 0 | 7 | 8 | 2 | 9 | 2 | 16 | 4 | 5 | 7 | 0 | 7 | 1 | 7 | 2 | 7 | 4 | 7 | 7 | 7 | 9 | 7 | 16
INPUTS | 3 | iobs/Clear1  | nADoutLE1  | iobs/Load1
INPUTMC | 3 | 3 | 0 | 5 | 13 | 4 | 12
EQ | 3 | 
   !nADoutLE1.D = iobs/Load1
	# !iobs/Clear1 & !nADoutLE1;
   nADoutLE1.CLK = CLK_FSB;	// GCK
GLOBALS | 1 | 2 | CLK_FSB

MACROCELL | 3 | 1 | nAoutOE_OBUF
ATTRIBUTES | 8815366 | 0
OUTPUTMC | 8 | 5 | 1 | 5 | 11 | 5 | 8 | 5 | 10 | 5 | 2 | 5 | 15 | 5 | 6 | 3 | 1
INPUTS | 4 | iobm/BGr1  | nAoutOE  | iobm/BGr0  | nAS_IOB
INPUTMC | 4 | 1 | 14 | 3 | 1 | 1 | 15 | 5 | 11
EQ | 4 | 
   nAoutOE.D = !iobm/BGr0 & !iobm/BGr1
	# !iobm/BGr1 & nAoutOE
	# !nAS_IOB & !iobm/BGr0 & !nAoutOE;
   nAoutOE.CLK = CLK2X_IOB;	// GCK
GLOBALS | 1 | 2 | CLK2X_IOB

MACROCELL | 7 | 5 | nRAMLWE_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 7 | 4
INPUTS | 10 | nWE_FSB  | nLDS_FSB  | ram/RAMDIS2  | nAS_FSB  | ram/RAMDIS1  | ram/RefRAS  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | A_FSB<21>
INPUTMC | 4 | 4 | 2 | 6 | 17 | 0 | 0 | 0 | 17
INPUTP | 6 | 47 | 49 | 54 | 36 | 30 | 29
EXPORTS | 1 | 7 | 4
EQ | 7 | 
   !nRAMLWE = !nWE_FSB & !nLDS_FSB & !ram/RAMDIS2 & !nAS_FSB & 
	!ram/RAMDIS1;
    nRAMLWE_OBUF.EXP  =  ram/RefRAS
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!ram/RAMDIS2 & !nAS_FSB & !ram/RAMDIS1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !ram/RAMDIS2 & !nAS_FSB & !ram/RAMDIS1

MACROCELL | 7 | 7 | nRAMUWE_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 7 | 8
INPUTS | 10 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | iobs/PS_FSM_FFd2  | nADoutLE1  | A_FSB<20>  | A_FSB<19>  | A_FSB<17>  | A_FSB<16>  | RESDone.EXP
INPUTMC | 3 | 7 | 3 | 5 | 13 | 7 | 6
INPUTP | 7 | 36 | 30 | 29 | 28 | 26 | 23 | 22
EXPORTS | 1 | 7 | 8
IMPORTS | 1 | 7 | 6
EQ | 13 | 
   !nRAMUWE = ;Imported pterms FB8_7
	  !nWE_FSB & !nUDS_FSB & !ram/RAMDIS2 & !nAS_FSB & 
	!ram/RAMDIS1;
    nRAMUWE_OBUF.EXP  =  !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<19> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1

MACROCELL | 4 | 1 | nROMCS_OBUF
ATTRIBUTES | 264962 | 0
OUTPUTMC | 1 | 4 | 2
INPUTS | 16 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | SW<1>  | cs/nOverlay1  | cnt/RefDone  | ram/Once  | ram/RAMDIS2  | nAS_FSB  | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | fsb/ASrf
INPUTMC | 10 | 0 | 17 | 3 | 13 | 4 | 9 | 4 | 2 | 6 | 9 | 6 | 3 | 3 | 7 | 3 | 6 | 3 | 3 | 0 | 5
INPUTP | 6 | 36 | 30 | 29 | 28 | 97 | 54
EXPORTS | 1 | 4 | 2
EQ | 14 | 
   !nROMCS = A_FSB<23> & !A_FSB<22> & !A_FSB<21> & !A_FSB<20> & 
	!SW<1>
	# !A_FSB<23> & A_FSB<22> & !A_FSB<21> & !A_FSB<20> & 
	SW<1>
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & !A_FSB<20> & 
	!cs/nOverlay1;
    nROMCS_OBUF.EXP  =  !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	ram/Once & !cs/nOverlay1 & !ram/RAMDIS2 & !nAS_FSB & 
	!ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	ram/Once & !cs/nOverlay1 & !ram/RAMDIS2 & !ram/RS_FSM_FFd2 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & 
	fsb/ASrf

MACROCELL | 0 | 12 | $OpTx$FX_DC$591
ATTRIBUTES | 133888 | 0
OUTPUTMC | 6 | 2 | 0 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 16 | 2 | 17
INPUTS | 2 | nAS_FSB  | fsb/ASrf
INPUTMC | 1 | 0 | 5
INPUTP | 1 | 54
EQ | 1 | 
   $OpTx$FX_DC$591 = nAS_FSB & !fsb/ASrf;

MACROCELL | 2 | 1 | EXP14_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 0
INPUTS | 20 | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | fsb/Ready0r  | fsb/VPA  | ram/RAMReady  | $OpTx$FX_DC$591  | A_FSB<21>  | fsb/Ready1r  | iobs/IOReady  | SW<1>  | A_FSB<14>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | A_FSB<13>  | EXP15_.EXP
INPUTMC | 8 | 0 | 17 | 2 | 3 | 2 | 0 | 6 | 14 | 0 | 12 | 2 | 14 | 3 | 16 | 2 | 2
INPUTP | 12 | 36 | 30 | 29 | 97 | 19 | 28 | 26 | 24 | 23 | 22 | 47 | 18
EXPORTS | 1 | 2 | 0
IMPORTS | 1 | 2 | 2
EQ | 57 | 
       EXP14_.EXP  =  !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!fsb/Ready0r & fsb/VPA & !ram/RAMReady & !$OpTx$FX_DC$591
	# A_FSB<22> & !A_FSB<21> & !fsb/Ready1r & fsb/VPA & 
	!iobs/IOReady & !SW<1> & !$OpTx$FX_DC$591
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !fsb/Ready0r & fsb/VPA & !ram/RAMReady & 
	!$OpTx$FX_DC$591
	# A_FSB<14> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & fsb/VPA & !iobs/IOReady & !$OpTx$FX_DC$591
	# A_FSB<13> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & fsb/VPA & !iobs/IOReady & !$OpTx$FX_DC$591
;Imported pterms FB3_3
	# A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
;Imported pterms FB3_4
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & fsb/Ready1r & nBR_IOB & 
	!$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & iobs/IOReady & nBR_IOB & 
	!$OpTx$FX_DC$591

MACROCELL | 2 | 2 | EXP15_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 1
INPUTS | 23 | A_FSB<9>  | A_FSB<15>  | A_FSB<14>  | A_FSB<13>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | cs/nOverlay1  | cnt/TimeoutA  | fsb/Ready2r  | fsb/VPA  | $OpTx$FX_DC$591  | A_FSB<8>  | fsb/Ready0r.EXP
INPUTMC | 6 | 0 | 17 | 3 | 15 | 2 | 15 | 2 | 0 | 0 | 12 | 2 | 3
INPUTP | 17 | 12 | 21 | 19 | 18 | 17 | 15 | 13 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22 | 47 | 11
EXPORTS | 1 | 2 | 1
IMPORTS | 1 | 2 | 3
EQ | 43 | 
       EXP15_.EXP  =  A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
;Imported pterms FB3_4
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & fsb/Ready1r & nBR_IOB & 
	!$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & iobs/IOReady & nBR_IOB & 
	!$OpTx$FX_DC$591

MACROCELL | 2 | 4 | EXP16_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 3
INPUTS | 2 | nAS_FSB  | fsb/ASrf
INPUTMC | 1 | 0 | 5
INPUTP | 1 | 54
EXPORTS | 1 | 2 | 3
EQ | 1 | 
       EXP16_.EXP  =  nAS_FSB & !fsb/ASrf

MACROCELL | 2 | 5 | EXP17_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 6
INPUTS | 24 | nAS_FSB  | fsb/ASrf  | A_FSB<9>  | A_FSB<8>  | A_FSB<15>  | A_FSB<14>  | A_FSB<13>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | iobs/BERR  | cnt/TimeoutB  | fsb/BERR0r  | fsb/BERR1r  | iobs/IOReady  | nBR_IOB
INPUTMC | 7 | 0 | 5 | 7 | 15 | 6 | 12 | 2 | 11 | 0 | 16 | 3 | 16 | 7 | 14
INPUTP | 17 | 54 | 12 | 11 | 21 | 19 | 18 | 17 | 15 | 13 | 36 | 30 | 29 | 28 | 26 | 24 | 23 | 22
EXPORTS | 1 | 2 | 6
EQ | 6 | 
       EXP17_.EXP  =  nAS_FSB & !fsb/ASrf
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & iobs/IOReady & nBR_IOB

MACROCELL | 2 | 6 | EXP18_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 7
INPUTS | 11 | A_FSB<23>  | cnt/TimeoutB  | nDTACK_FSB  | A_FSB<22>  | A_FSB<20>  | fsb/Ready1r  | iobs/IOReady  | cs/nOverlay1  | fsb/Ready0r  | ram/RAMReady  | EXP17_.EXP
INPUTMC | 8 | 6 | 12 | 2 | 8 | 2 | 14 | 3 | 16 | 0 | 17 | 2 | 3 | 6 | 14 | 2 | 5
INPUTP | 3 | 36 | 30 | 28
EXPORTS | 1 | 2 | 7
IMPORTS | 1 | 2 | 5
EQ | 14 | 
       EXP18_.EXP  =  A_FSB<23> & cnt/TimeoutB & nDTACK_FSB
	# !A_FSB<22> & cnt/TimeoutB & nDTACK_FSB
	# !A_FSB<20> & cnt/TimeoutB & nDTACK_FSB
	# A_FSB<23> & !fsb/Ready1r & !iobs/IOReady & 
	nDTACK_FSB
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!fsb/Ready0r & nDTACK_FSB & !ram/RAMReady
;Imported pterms FB3_6
	# nAS_FSB & !fsb/ASrf
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & iobs/IOReady & nBR_IOB

MACROCELL | 2 | 7 | EXP19_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 8
INPUTS | 24 | A_FSB<14>  | A_FSB<22>  | A_FSB<20>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | cs/nOverlay1  | fsb/Ready1r  | iobs/IOReady  | nDTACK_FSB  | A_FSB<21>  | nADoutLE1  | A_FSB<8>  | A_FSB<15>  | A_FSB<13>  | A_FSB<12>  | A_FSB<11>  | A_FSB<10>  | A_FSB<23>  | cnt/TimeoutA  | fsb/Ready2r  | EXP18_.EXP
INPUTMC | 8 | 0 | 17 | 2 | 14 | 3 | 16 | 2 | 8 | 5 | 13 | 3 | 15 | 2 | 15 | 2 | 6
INPUTP | 16 | 19 | 30 | 28 | 26 | 24 | 23 | 22 | 47 | 29 | 11 | 21 | 18 | 17 | 15 | 13 | 36
EXPORTS | 1 | 2 | 8
IMPORTS | 1 | 2 | 6
EQ | 37 | 
       EXP19_.EXP  =  A_FSB<14> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & !iobs/IOReady & nDTACK_FSB
	# A_FSB<14> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & nDTACK_FSB & 
	!nADoutLE1
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
	# A_FSB<8> & A_FSB<15> & !A_FSB<14> & A_FSB<13> & 
	!A_FSB<12> & !A_FSB<11> & !A_FSB<10> & !A_FSB<23> & A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & nDTACK_FSB
;Imported pterms FB3_7
	# A_FSB<23> & cnt/TimeoutB & nDTACK_FSB
	# !A_FSB<22> & cnt/TimeoutB & nDTACK_FSB
	# !A_FSB<20> & cnt/TimeoutB & nDTACK_FSB
	# A_FSB<23> & !fsb/Ready1r & !iobs/IOReady & 
	nDTACK_FSB
	# !A_FSB<23> & !A_FSB<22> & cs/nOverlay1 & 
	!fsb/Ready0r & nDTACK_FSB & !ram/RAMReady
;Imported pterms FB3_6
	# nAS_FSB & !fsb/ASrf
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & iobs/IOReady & nBR_IOB

MACROCELL | 2 | 9 | EXP20_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 8
INPUTS | 19 | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | fsb/Ready1r  | iobs/IOReady  | nDTACK_FSB  | SW<1>  | A_FSB<23>  | cs/nOverlay1  | fsb/Ready0r  | ram/RAMReady  | A_FSB<13>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | nADoutLE1  | EXP21_.EXP
INPUTMC | 8 | 2 | 14 | 3 | 16 | 2 | 8 | 0 | 17 | 2 | 3 | 6 | 14 | 5 | 13 | 2 | 10
INPUTP | 11 | 30 | 29 | 28 | 97 | 36 | 18 | 26 | 24 | 23 | 22 | 47
EXPORTS | 1 | 2 | 8
IMPORTS | 1 | 2 | 10
EQ | 25 | 
       EXP20_.EXP  =  A_FSB<22> & !A_FSB<21> & A_FSB<20> & !fsb/Ready1r & 
	!iobs/IOReady & nDTACK_FSB
	# A_FSB<22> & !A_FSB<21> & !fsb/Ready1r & 
	!iobs/IOReady & nDTACK_FSB & !SW<1>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	!cs/nOverlay1 & !fsb/Ready0r & nDTACK_FSB & !ram/RAMReady
	# A_FSB<13> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & !iobs/IOReady & nDTACK_FSB
	# A_FSB<13> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & nDTACK_FSB & 
	!nADoutLE1
;Imported pterms FB3_11
	# iobs/BERR & nDTACK_FSB
	# fsb/BERR0r & nDTACK_FSB
	# fsb/BERR1r & nDTACK_FSB
	# nDTACK_FSB & !nBR_IOB
	# A_FSB<21> & cnt/TimeoutB & nDTACK_FSB
;Imported pterms FB3_12
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & fsb/Ready1r & nBR_IOB

MACROCELL | 2 | 10 | EXP21_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 9
INPUTS | 8 | iobs/BERR  | nDTACK_FSB  | fsb/BERR0r  | fsb/BERR1r  | nBR_IOB  | A_FSB<21>  | cnt/TimeoutB  | fsb/BERR0r.EXP
INPUTMC | 7 | 7 | 15 | 2 | 8 | 2 | 11 | 0 | 16 | 7 | 14 | 6 | 12 | 2 | 11
INPUTP | 1 | 29
EXPORTS | 1 | 2 | 9
IMPORTS | 1 | 2 | 11
EQ | 11 | 
       EXP21_.EXP  =  iobs/BERR & nDTACK_FSB
	# fsb/BERR0r & nDTACK_FSB
	# fsb/BERR1r & nDTACK_FSB
	# nDTACK_FSB & !nBR_IOB
	# A_FSB<21> & cnt/TimeoutB & nDTACK_FSB
;Imported pterms FB3_12
	# A_FSB<9> & A_FSB<8> & A_FSB<15> & A_FSB<14> & 
	A_FSB<13> & A_FSB<12> & A_FSB<11> & A_FSB<10> & A_FSB<23> & 
	A_FSB<22> & A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & 
	A_FSB<17> & A_FSB<16> & !iobs/BERR & !cnt/TimeoutB & 
	!fsb/BERR0r & !fsb/BERR1r & fsb/Ready1r & nBR_IOB

MACROCELL | 2 | 13 | EXP22_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 14
INPUTS | 16 | A_FSB<23>  | fsb/Ready1r  | iobs/IOReady  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | SW<1>  | A_FSB<14>  | A_FSB<19>  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | cs/nOverlay1  | A_FSB<13>  | cs/nOverlay0.EXP
INPUTMC | 4 | 2 | 14 | 3 | 16 | 0 | 17 | 2 | 12
INPUTP | 12 | 36 | 30 | 29 | 28 | 97 | 19 | 26 | 24 | 23 | 22 | 47 | 18
EXPORTS | 1 | 2 | 14
IMPORTS | 1 | 2 | 12
EQ | 18 | 
       EXP22_.EXP  =  A_FSB<23> & !fsb/Ready1r & !iobs/IOReady
	# A_FSB<22> & !A_FSB<21> & A_FSB<20> & !fsb/Ready1r & 
	!iobs/IOReady
	# A_FSB<22> & !A_FSB<21> & !fsb/Ready1r & 
	!iobs/IOReady & !SW<1>
	# A_FSB<14> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & !iobs/IOReady
	# A_FSB<13> & A_FSB<22> & A_FSB<20> & A_FSB<19> & 
	A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & !cs/nOverlay1 & 
	!fsb/Ready1r & !iobs/IOReady
;Imported pterms FB3_13
	# A_FSB<14> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & !nADoutLE1
	# A_FSB<13> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & !iobs/IOReady & !nADoutLE1

MACROCELL | 2 | 17 | EXP23_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 2 | 0
INPUTS | 10 | A_FSB<23>  | cnt/TimeoutB  | fsb/VPA  | $OpTx$FX_DC$591  | A_FSB<22>  | A_FSB<21>  | fsb/Ready1r  | iobs/IOReady  | A_FSB<20>  | nROMWE_OBUF.EXP
INPUTMC | 6 | 6 | 12 | 2 | 0 | 0 | 12 | 2 | 14 | 3 | 16 | 2 | 16
INPUTP | 4 | 36 | 30 | 29 | 28
EXPORTS | 1 | 2 | 0
IMPORTS | 1 | 2 | 16
EQ | 29 | 
       EXP23_.EXP  =  A_FSB<23> & cnt/TimeoutB & fsb/VPA & 
	!$OpTx$FX_DC$591
	# !A_FSB<22> & cnt/TimeoutB & fsb/VPA & 
	!$OpTx$FX_DC$591
	# A_FSB<21> & cnt/TimeoutB & fsb/VPA & 
	!$OpTx$FX_DC$591
	# A_FSB<23> & !fsb/Ready1r & fsb/VPA & 
	!iobs/IOReady & !$OpTx$FX_DC$591
	# A_FSB<22> & !A_FSB<21> & A_FSB<20> & !fsb/Ready1r & 
	fsb/VPA & !iobs/IOReady & !$OpTx$FX_DC$591
;Imported pterms FB3_17
	# A_FSB<14> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & fsb/VPA & !iobs/IOReady & 
	!nADoutLE1 & !$OpTx$FX_DC$591
	# A_FSB<13> & !A_FSB<22> & A_FSB<21> & A_FSB<20> & 
	A_FSB<19> & A_FSB<18> & A_FSB<17> & A_FSB<16> & !nWE_FSB & 
	cs/nOverlay1 & !fsb/Ready1r & fsb/VPA & !iobs/IOReady & 
	!nADoutLE1 & !$OpTx$FX_DC$591
	# A_FSB<9> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591
	# A_FSB<8> & A_FSB<15> & A_FSB<14> & A_FSB<13> & 
	A_FSB<12> & A_FSB<11> & A_FSB<10> & !A_FSB<23> & !A_FSB<22> & 
	A_FSB<21> & A_FSB<20> & A_FSB<19> & A_FSB<18> & A_FSB<17> & 
	A_FSB<16> & !nWE_FSB & cs/nOverlay1 & !cnt/TimeoutA & 
	!fsb/Ready2r & fsb/VPA & !$OpTx$FX_DC$591

MACROCELL | 4 | 0 | EXP24_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 4 | 17
INPUTS | 12 | A_FSB<22>  | cnt/RefDone  | cs/nOverlay1  | nAS_FSB  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | ram/BACTr  | fsb/ASrf  | A_FSB<21>  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>
INPUTMC | 9 | 3 | 13 | 0 | 17 | 3 | 17 | 6 | 9 | 0 | 1 | 0 | 5 | 3 | 7 | 3 | 6 | 3 | 3
INPUTP | 3 | 30 | 54 | 29
EXPORTS | 1 | 4 | 17
EQ | 11 | 
       EXP24_.EXP  =  A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr & fsb/ASrf
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr & fsb/ASrf
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>

MACROCELL | 4 | 7 | EXP25_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 4 | 6
INPUTS | 9 | A_FSB<23>  | A_FSB<21>  | A_FSB<19>  | iobs/Once  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | nWE_FSB  | RA_4_OBUF.EXP
INPUTMC | 2 | 4 | 6 | 4 | 8
INPUTP | 7 | 36 | 29 | 26 | 24 | 23 | 22 | 47
EXPORTS | 1 | 4 | 6
IMPORTS | 1 | 4 | 8
EQ | 11 | 
       EXP25_.EXP  =  !A_FSB<23> & A_FSB<21> & !A_FSB<19> & !iobs/Once
	# !A_FSB<23> & A_FSB<21> & !A_FSB<18> & !iobs/Once
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17> & !iobs/Once
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16> & !iobs/Once
	# !A_FSB<23> & A_FSB<21> & nWE_FSB & !iobs/Once
;Imported pterms FB5_9
	# !A_FSB<23> & !A_FSB<20> & !iobs/Once & SW<1>
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21> & 
	!iobs/Once
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !iobs/Once & 
	cs/nOverlay1

MACROCELL | 4 | 15 | EXP26_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 4 | 16
INPUTS | 13 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | ram/Once  | cs/nOverlay1  | nAS_FSB  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | fsb/ASrf  | cnt/RefDone  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>
INPUTMC | 9 | 4 | 9 | 0 | 17 | 3 | 17 | 6 | 9 | 0 | 5 | 3 | 13 | 3 | 7 | 3 | 6 | 3 | 3
INPUTP | 4 | 36 | 30 | 29 | 54
EXPORTS | 1 | 4 | 16
EQ | 10 | 
       EXP26_.EXP  =  !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & fsb/ASrf
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>

MACROCELL | 4 | 16 | EXP27_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 4 | 17
INPUTS | 15 | A_FSB<23>  | cnt/RefDone  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | A_FSB<22>  | ram/Once  | cs/nOverlay1  | nAS_FSB  | fsb/ASrf  | A_FSB<21>  | ram/BACTr  | EXP26_.EXP
INPUTMC | 11 | 3 | 13 | 3 | 17 | 6 | 9 | 3 | 7 | 3 | 6 | 3 | 3 | 4 | 9 | 0 | 17 | 0 | 5 | 0 | 1 | 4 | 15
INPUTP | 4 | 36 | 30 | 54 | 29
EXPORTS | 1 | 4 | 17
IMPORTS | 1 | 4 | 15
EQ | 21 | 
       EXP27_.EXP  =  A_FSB<23> & !cnt/RefDone & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2
	# !A_FSB<23> & !A_FSB<22> & !ram/Once & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & fsb/ASrf
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & !ram/BACTr & fsb/ASrf
;Imported pterms FB5_16
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & fsb/ASrf
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>

MACROCELL | 6 | 0 | EXP28_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 6 | 17
INPUTS | 15 | A_FSB<23>  | cnt/RefDone  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd3  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | A_FSB<22>  | cs/nOverlay1  | ram/BACTr  | fsb/ASrf  | ram/Once  | A_FSB<21>  | nAS_FSB  | RA_1_OBUF.EXP
INPUTMC | 11 | 3 | 13 | 3 | 17 | 6 | 3 | 3 | 7 | 3 | 6 | 3 | 3 | 0 | 17 | 0 | 1 | 0 | 5 | 4 | 9 | 6 | 1
INPUTP | 4 | 36 | 30 | 29 | 54
EXPORTS | 1 | 6 | 17
IMPORTS | 1 | 6 | 1
EQ | 19 | 
       EXP28_.EXP  =  A_FSB<23> & !cnt/RefDone & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr & fsb/ASrf
	# !cnt/RefDone & ram/Once & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !cnt/RefDone & nAS_FSB & !ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & 
	!fsb/ASrf
;Imported pterms FB7_2
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>

MACROCELL | 6 | 2 | EXP29_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 6 | 3
INPUTS | 13 | cnt/RefDone  | nAS_FSB  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd2  | ram/RS_FSM_FFd3  | cnt/RefCnt<5>  | cnt/RefCnt<6>  | cnt/RefCnt<7>  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | cs/nOverlay1  | A_FSB<21>
INPUTMC | 9 | 3 | 13 | 3 | 17 | 6 | 9 | 6 | 3 | 3 | 7 | 3 | 6 | 3 | 3 | 0 | 5 | 0 | 17
INPUTP | 4 | 54 | 36 | 30 | 29
EXPORTS | 1 | 6 | 3
EQ | 15 | 
       EXP29_.EXP  =  !cnt/RefDone & !nAS_FSB & ram/RS_FSM_FFd1 & 
	!ram/RS_FSM_FFd2 & !ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & 
	cnt/RefCnt<7>
	# !cnt/RefDone & ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd2 & 
	!ram/RS_FSM_FFd3 & cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & 
	fsb/ASrf
	# !A_FSB<23> & !A_FSB<22> & !cnt/RefDone & 
	cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>
	# !A_FSB<23> & !A_FSB<22> & !cnt/RefDone & 
	cs/nOverlay1 & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7> & fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !cnt/RefDone & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & 
	cnt/RefCnt<5> & cnt/RefCnt<6> & cnt/RefCnt<7>

MACROCELL | 6 | 15 | EXP30_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 6 | 14
INPUTS | 10 | A_FSB<22>  | A_FSB<21>  | cnt/RefDone  | ram/RS_FSM_FFd1  | ram/BACTr  | fsb/ASrf  | cs/nOverlay1  | A_FSB<23>  | ram/Once  | nAS_FSB
INPUTMC | 6 | 3 | 13 | 3 | 17 | 0 | 1 | 0 | 5 | 0 | 17 | 4 | 9
INPUTP | 4 | 30 | 29 | 36 | 54
EXPORTS | 1 | 6 | 14
EQ | 10 | 
       EXP30_.EXP  =  A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/BACTr & fsb/ASrf
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/BACTr & fsb/ASrf
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/BACTr & fsb/ASrf
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !nAS_FSB & !ram/RS_FSM_FFd1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & !ram/Once & 
	!cs/nOverlay1 & !ram/RS_FSM_FFd1 & fsb/ASrf

MACROCELL | 6 | 16 | EXP31_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 6 | 17
INPUTS | 9 | A_FSB<22>  | A_FSB<21>  | cnt/RefDone  | nAS_FSB  | ram/RS_FSM_FFd1  | ram/RS_FSM_FFd3  | ram/BACTr  | fsb/ASrf  | cs/nOverlay1
INPUTMC | 6 | 3 | 13 | 3 | 17 | 6 | 3 | 0 | 1 | 0 | 5 | 0 | 17
INPUTP | 3 | 30 | 29 | 54
EXPORTS | 1 | 6 | 17
EQ | 10 | 
       EXP31_.EXP  =  A_FSB<22> & !A_FSB<21> & !cnt/RefDone & !nAS_FSB & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr
	# A_FSB<22> & !A_FSB<21> & !cnt/RefDone & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr & fsb/ASrf
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr
	# A_FSB<22> & !cnt/RefDone & cs/nOverlay1 & 
	!ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr & fsb/ASrf
	# !A_FSB<22> & !cnt/RefDone & !cs/nOverlay1 & 
	!nAS_FSB & !ram/RS_FSM_FFd1 & !ram/RS_FSM_FFd3 & !ram/BACTr

MACROCELL | 7 | 0 | EXP32_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 7 | 17
INPUTS | 9 | iobs/IORW0  | iobs/IORW1  | nADoutLE1  | nAS_FSB  | fsb/ASrf  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB_19_IBUF$BUF0.EXP
INPUTMC | 5 | 7 | 17 | 7 | 13 | 5 | 13 | 0 | 5 | 7 | 1
INPUTP | 4 | 54 | 36 | 30 | 29
EXPORTS | 1 | 7 | 17
IMPORTS | 1 | 7 | 1
EQ | 10 | 
       EXP32_.EXP  =  iobs/IORW0 & iobs/IORW1 & !nADoutLE1
	# !iobs/IORW0 & !iobs/IORW1 & !nADoutLE1
	# nAS_FSB & !fsb/ASrf & nADoutLE1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !iobs/IORW0 & nADoutLE1
;Imported pterms FB8_2
	# iobs/PS_FSM_FFd2
	# iobs/PS_FSM_FFd1
	# iobs/Once & nADoutLE1
	# nWE_FSB & iobs/IORW0 & nADoutLE1

MACROCELL | 7 | 2 | EXP33_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 7 | 3
INPUTS | 10 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | nADoutLE1  | A_FSB<20>  | A_FSB<19>  | A_FSB<17>  | A_FSB<16>
INPUTMC | 3 | 7 | 3 | 3 | 12 | 5 | 13
INPUTP | 7 | 36 | 30 | 29 | 28 | 26 | 23 | 22
EXPORTS | 1 | 7 | 3
EQ | 10 | 
       EXP33_.EXP  =  !A_FSB<23> & !A_FSB<22> & !A_FSB<21> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<19> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16> & 
	!iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1 & nADoutLE1

MACROCELL | 7 | 9 | EXP34_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 7 | 8
INPUTS | 12 | A_FSB<23>  | A_FSB<21>  | A_FSB<18>  | iobs/PS_FSM_FFd2  | nADoutLE1  | nWE_FSB  | A_FSB<20>  | SW<1>  | A_FSB<14>  | A_FSB<13>  | A_FSB<22>  | cs/nOverlay1
INPUTMC | 3 | 7 | 3 | 5 | 13 | 0 | 17
INPUTP | 9 | 36 | 29 | 24 | 47 | 28 | 97 | 19 | 18 | 30
EXPORTS | 1 | 7 | 8
EQ | 10 | 
       EXP34_.EXP  =  !A_FSB<23> & A_FSB<21> & !A_FSB<18> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & nWE_FSB & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & !A_FSB<20> & !iobs/PS_FSM_FFd2 & 
	SW<1> & nADoutLE1
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21> & 
	!iobs/PS_FSM_FFd2 & nADoutLE1
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1 & !iobs/PS_FSM_FFd2 & nADoutLE1

MACROCELL | 7 | 10 | EXP35_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 7 | 11
INPUTS | 7 | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | A_FSB<20>  | iobs/BERR  | fsb/BERR0r  | fsb/BERR1r
INPUTMC | 3 | 7 | 15 | 2 | 11 | 0 | 16
INPUTP | 4 | 36 | 30 | 29 | 28
EXPORTS | 1 | 7 | 11
EQ | 2 | 
       EXP35_.EXP  =  !A_FSB<23> & A_FSB<22> & !A_FSB<21> & A_FSB<20> & 
	!iobs/BERR & !fsb/BERR0r & !fsb/BERR1r

MACROCELL | 7 | 12 | EXP36_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 7 | 13
INPUTS | 10 | nAS_FSB  | fsb/ASrf  | iobs/PS_FSM_FFd2  | iobs/PS_FSM_FFd1  | A_FSB<23>  | A_FSB<22>  | A_FSB<21>  | cs/nOverlay1  | A_FSB<20>  | nBERR_FSB_OBUF.EXP
INPUTMC | 5 | 0 | 5 | 7 | 3 | 3 | 12 | 0 | 17 | 7 | 11
INPUTP | 5 | 54 | 36 | 30 | 29 | 28
EXPORTS | 1 | 7 | 13
IMPORTS | 1 | 7 | 11
EQ | 10 | 
       EXP36_.EXP  =  nAS_FSB & !fsb/ASrf
	# !iobs/PS_FSM_FFd2 & !iobs/PS_FSM_FFd1
	# !A_FSB<23> & !A_FSB<22> & !A_FSB<21>
	# !A_FSB<23> & !A_FSB<22> & !cs/nOverlay1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<20>
;Imported pterms FB8_12
	# !A_FSB<23> & !A_FSB<20> & SW<1>
	# !A_FSB<14> & !A_FSB<13> & !A_FSB<23> & A_FSB<21>
	# !A_FSB<23> & A_FSB<22> & A_FSB<21> & 
	cs/nOverlay1

MACROCELL | 7 | 16 | EXP37_
ATTRIBUTES | 2048 | 0
OUTPUTMC | 1 | 7 | 17
INPUTS | 9 | A_FSB<23>  | A_FSB<21>  | A_FSB<19>  | nADoutLE1  | A_FSB<18>  | A_FSB<17>  | A_FSB<16>  | A_FSB<20>  | SW<1>
INPUTMC | 1 | 5 | 13
INPUTP | 8 | 36 | 29 | 26 | 24 | 23 | 22 | 28 | 97
EXPORTS | 1 | 7 | 17
EQ | 5 | 
       EXP37_.EXP  =  !A_FSB<23> & A_FSB<21> & !A_FSB<19> & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<18> & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<17> & nADoutLE1
	# !A_FSB<23> & A_FSB<21> & !A_FSB<16> & nADoutLE1
	# !A_FSB<23> & !A_FSB<20> & SW<1> & nADoutLE1

PIN | A_FSB<9> | 64 | 0 | N/A | 12 | 8 | 2 | 15 | 6 | 6 | 2 | 8 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 11 | 2 | 16
PIN | A_FSB<8> | 64 | 0 | N/A | 11 | 10 | 2 | 15 | 6 | 4 | 2 | 8 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 11 | 2 | 14 | 2 | 16
PIN | A_FSB<15> | 64 | 0 | N/A | 21 | 10 | 2 | 15 | 4 | 10 | 2 | 8 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 11 | 2 | 14 | 2 | 16
PIN | A_FSB<14> | 64 | 0 | N/A | 19 | 18 | 2 | 16 | 7 | 17 | 2 | 13 | 2 | 15 | 4 | 8 | 7 | 11 | 2 | 8 | 4 | 13 | 2 | 14 | 7 | 4 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 11 | 2 | 12 | 7 | 9
PIN | A_FSB<13> | 64 | 0 | N/A | 18 | 20 | 2 | 16 | 7 | 17 | 2 | 13 | 2 | 15 | 4 | 10 | 7 | 11 | 2 | 8 | 4 | 13 | 4 | 8 | 7 | 4 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 9 | 2 | 11 | 2 | 12 | 2 | 14 | 7 | 9
PIN | A_FSB<12> | 64 | 0 | N/A | 17 | 10 | 2 | 15 | 2 | 16 | 2 | 8 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 11 | 2 | 14 | 4 | 14
PIN | A_FSB<11> | 64 | 0 | N/A | 15 | 10 | 2 | 15 | 6 | 1 | 2 | 8 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 11 | 2 | 14 | 2 | 16
PIN | A_FSB<10> | 64 | 0 | N/A | 13 | 10 | 2 | 15 | 6 | 5 | 2 | 8 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 11 | 2 | 14 | 2 | 16
PIN | A_FSB<23> | 64 | 0 | N/A | 36 | 58 | 4 | 9 | 4 | 6 | 7 | 17 | 2 | 12 | 2 | 11 | 2 | 3 | 2 | 13 | 2 | 15 | 4 | 1 | 7 | 13 | 4 | 2 | 2 | 8 | 3 | 17 | 4 | 17 | 6 | 6 | 6 | 3 | 7 | 3 | 4 | 12 | 7 | 8 | 6 | 17 | 6 | 14 | 6 | 7 | 7 | 10 | 3 | 5 | 7 | 2 | 2 | 1 | 2 | 2 | 2 | 5 | 2 | 6 | 2 | 7 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 0 | 3 | 16 | 4 | 5 | 4 | 7 | 4 | 8 | 4 | 11 | 4 | 13 | 4 | 15 | 4 | 16 | 6 | 0 | 6 | 2 | 6 | 4 | 6 | 10 | 6 | 13 | 6 | 15 | 7 | 0 | 7 | 4 | 7 | 5 | 7 | 7 | 7 | 9 | 7 | 11 | 7 | 12 | 7 | 14 | 7 | 16
PIN | A_FSB<22> | 64 | 0 | N/A | 30 | 54 | 4 | 9 | 4 | 6 | 7 | 17 | 2 | 12 | 2 | 11 | 2 | 3 | 2 | 13 | 2 | 15 | 4 | 1 | 7 | 12 | 4 | 2 | 2 | 8 | 3 | 17 | 4 | 16 | 6 | 6 | 6 | 3 | 7 | 3 | 4 | 12 | 7 | 8 | 6 | 16 | 6 | 13 | 6 | 7 | 7 | 10 | 3 | 5 | 7 | 2 | 2 | 1 | 2 | 2 | 2 | 5 | 2 | 6 | 2 | 7 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 3 | 0 | 3 | 16 | 4 | 0 | 4 | 5 | 4 | 8 | 4 | 11 | 4 | 13 | 4 | 15 | 6 | 0 | 6 | 1 | 6 | 2 | 6 | 4 | 6 | 10 | 6 | 15 | 7 | 0 | 7 | 4 | 7 | 5 | 7 | 7 | 7 | 9 | 7 | 11
PIN | A_FSB<21> | 64 | 0 | N/A | 29 | 51 | 4 | 9 | 4 | 5 | 7 | 17 | 2 | 12 | 2 | 11 | 2 | 3 | 2 | 13 | 2 | 15 | 4 | 1 | 7 | 13 | 4 | 0 | 2 | 8 | 3 | 0 | 4 | 16 | 6 | 6 | 6 | 3 | 7 | 2 | 4 | 11 | 7 | 7 | 6 | 16 | 6 | 13 | 6 | 7 | 7 | 10 | 3 | 5 | 7 | 0 | 6 | 8 | 2 | 1 | 2 | 2 | 2 | 5 | 2 | 7 | 2 | 9 | 2 | 10 | 2 | 14 | 2 | 16 | 2 | 17 | 4 | 7 | 4 | 8 | 4 | 13 | 4 | 15 | 6 | 0 | 6 | 2 | 6 | 4 | 6 | 10 | 6 | 15 | 7 | 4 | 7 | 5 | 7 | 9 | 7 | 11 | 7 | 12 | 7 | 14 | 7 | 16
PIN | A_FSB<20> | 64 | 0 | N/A | 28 | 32 | 4 | 5 | 7 | 17 | 2 | 12 | 2 | 11 | 2 | 13 | 2 | 15 | 2 | 0 | 7 | 12 | 2 | 8 | 7 | 2 | 4 | 11 | 7 | 7 | 4 | 13 | 7 | 10 | 3 | 5 | 4 | 1 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 6 | 2 | 7 | 2 | 9 | 2 | 14 | 2 | 16 | 2 | 17 | 4 | 8 | 6 | 11 | 7 | 4 | 7 | 9 | 7 | 11 | 7 | 16
PIN | A_FSB<19> | 64 | 0 | N/A | 26 | 21 | 2 | 16 | 7 | 16 | 2 | 13 | 2 | 15 | 7 | 1 | 6 | 11 | 2 | 8 | 7 | 2 | 4 | 11 | 7 | 7 | 4 | 7 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 9 | 2 | 11 | 2 | 12 | 2 | 14 | 7 | 14
PIN | A_FSB<18> | 64 | 0 | N/A | 24 | 20 | 2 | 16 | 7 | 16 | 2 | 13 | 2 | 15 | 6 | 7 | 7 | 9 | 2 | 8 | 4 | 13 | 4 | 7 | 7 | 4 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 9 | 2 | 11 | 2 | 12 | 2 | 14 | 7 | 14
PIN | A_FSB<17> | 64 | 0 | N/A | 23 | 20 | 2 | 16 | 7 | 16 | 2 | 13 | 2 | 15 | 6 | 4 | 4 | 7 | 2 | 8 | 7 | 2 | 4 | 11 | 7 | 7 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 9 | 2 | 11 | 2 | 12 | 2 | 14 | 7 | 14
PIN | A_FSB<16> | 64 | 0 | N/A | 22 | 20 | 2 | 16 | 7 | 16 | 2 | 13 | 2 | 15 | 4 | 14 | 4 | 7 | 2 | 8 | 7 | 2 | 4 | 11 | 7 | 7 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 5 | 2 | 7 | 2 | 9 | 2 | 11 | 2 | 12 | 2 | 14 | 7 | 14
PIN | CLK2X_IOB | 4096 | 0 | N/A | 33 | 31 | 5 | 1 | 5 | 2 | 0 | 15 | 5 | 9 | 5 | 5 | 5 | 4 | 5 | 12 | 5 | 3 | 5 | 7 | 5 | 17 | 1 | 15 | 5 | 0 | 5 | 15 | 5 | 6 | 1 | 16 | 1 | 14 | 1 | 12 | 1 | 10 | 0 | 2 | 1 | 7 | 3 | 4 | 3 | 1 | 5 | 11 | 5 | 8 | 5 | 10 | 1 | 9 | 0 | 4 | 1 | 13 | 0 | 3 | 1 | 8 | 5 | 16
PIN | nWE_FSB | 64 | 0 | N/A | 47 | 22 | 2 | 14 | 7 | 17 | 2 | 13 | 2 | 15 | 7 | 6 | 7 | 13 | 2 | 8 | 7 | 1 | 4 | 7 | 7 | 4 | 4 | 4 | 2 | 16 | 3 | 5 | 7 | 5 | 2 | 1 | 2 | 2 | 2 | 3 | 2 | 7 | 2 | 9 | 2 | 12 | 4 | 13 | 7 | 9
PIN | CLK_FSB | 16384 | 0 | N/A | 42 | 57 | 3 | 13 | 4 | 9 | 4 | 6 | 0 | 17 | 7 | 15 | 7 | 17 | 2 | 12 | 3 | 15 | 6 | 12 | 6 | 6 | 2 | 11 | 0 | 16 | 2 | 3 | 2 | 14 | 2 | 15 | 2 | 0 | 4 | 3 | 0 | 14 | 7 | 13 | 3 | 16 | 3 | 14 | 0 | 13 | 4 | 2 | 2 | 8 | 3 | 17 | 4 | 17 | 6 | 9 | 6 | 3 | 7 | 3 | 3 | 7 | 3 | 6 | 3 | 12 | 1 | 17 | 3 | 3 | 0 | 6 | 3 | 9 | 1 | 6 | 3 | 11 | 3 | 8 | 4 | 12 | 0 | 1 | 0 | 9 | 0 | 8 | 0 | 11 | 0 | 7 | 0 | 0 | 7 | 6 | 0 | 10 | 3 | 2 | 3 | 0 | 7 | 8 | 6 | 17 | 6 | 14 | 7 | 14 | 5 | 13 | 0 | 5 | 4 | 4
PIN | nAS_FSB | 64 | 0 | N/A | 54 | 48 | 4 | 9 | 4 | 6 | 0 | 17 | 7 | 15 | 6 | 16 | 2 | 12 | 3 | 15 | 6 | 12 | 6 | 6 | 2 | 11 | 0 | 16 | 0 | 12 | 2 | 14 | 2 | 4 | 7 | 12 | 3 | 16 | 4 | 2 | 2 | 5 | 3 | 17 | 4 | 17 | 6 | 9 | 6 | 3 | 7 | 3 | 4 | 12 | 0 | 1 | 0 | 5 | 7 | 8 | 6 | 17 | 6 | 14 | 7 | 11 | 4 | 4 | 2 | 16 | 3 | 10 | 3 | 5 | 7 | 0 | 7 | 5 | 7 | 6 | 3 | 0 | 4 | 0 | 4 | 1 | 4 | 15 | 4 | 16 | 6 | 0 | 6 | 2 | 6 | 8 | 6 | 10 | 6 | 13 | 6 | 15
PIN | SW<1> | 64 | 0 | N/A | 97 | 11 | 2 | 9 | 7 | 16 | 2 | 13 | 4 | 1 | 7 | 11 | 2 | 1 | 4 | 13 | 4 | 8 | 7 | 4 | 3 | 5 | 7 | 9
PIN | nRES | 64 | 0 | N/A | 145 | 4 | 2 | 12 | 0 | 9 | 0 | 3 | 0 | 2
PIN | nLDS_FSB | 64 | 0 | N/A | 49 | 3 | 4 | 3 | 0 | 14 | 7 | 5
PIN | nUDS_FSB | 64 | 0 | N/A | 56 | 3 | 3 | 14 | 0 | 13 | 7 | 6
PIN | CLK_IOB | 8256 | 0 | N/A | 35 | 8 | 5 | 2 | 5 | 9 | 5 | 17 | 5 | 15 | 5 | 0 | 5 | 14 | 5 | 16 | 1 | 11
PIN | nBERR_IOB | 64 | 0 | N/A | 123 | 4 | 5 | 17 | 0 | 4 | 1 | 16 | 5 | 0
PIN | nIPL2 | 64 | 0 | N/A | 146 | 1 | 0 | 11
PIN | nBG_IOB | 64 | 0 | N/A | 117 | 1 | 1 | 15
PIN | E_IOB | 64 | 0 | N/A | 37 | 1 | 1 | 11
PIN | nDTACK_IOB | 64 | 0 | N/A | 127 | 2 | 1 | 13 | 1 | 12
PIN | nVPA_IOB | 64 | 0 | N/A | 125 | 2 | 1 | 8 | 1 | 7
PIN | A_FSB<1> | 64 | 0 | N/A | 149 | 1 | 6 | 5
PIN | A_FSB<2> | 64 | 0 | N/A | 153 | 1 | 6 | 1
PIN | A_FSB<3> | 64 | 0 | N/A | 155 | 1 | 4 | 14
PIN | A_FSB<4> | 64 | 0 | N/A | 157 | 1 | 4 | 10
PIN | A_FSB<5> | 64 | 0 | N/A | 4 | 1 | 4 | 8
PIN | A_FSB<6> | 64 | 0 | N/A | 6 | 1 | 4 | 10
PIN | A_FSB<7> | 64 | 0 | N/A | 8 | 1 | 4 | 14
PIN | SW<0> | 64 | 0 | N/A | 98 | 2 | 6 | 12 | 6 | 11
PIN | nVMA_IOB | 536871040 | 0 | N/A | 118
PIN | nAS_IOB | 536871040 | 0 | N/A | 135
PIN | nLDS_IOB | 536871040 | 0 | N/A | 130
PIN | nUDS_IOB | 536871040 | 0 | N/A | 134
PIN | nDTACK_FSB | 536871040 | 0 | N/A | 44
PIN | RA<0> | 536871040 | 0 | N/A | 86
PIN | RA<1> | 536871040 | 0 | N/A | 79
PIN | RA<2> | 536871040 | 0 | N/A | 69
PIN | RA<3> | 536871040 | 0 | N/A | 64
PIN | RA<4> | 536871040 | 0 | N/A | 63
PIN | RA<5> | 536871040 | 0 | N/A | 68
PIN | RA<6> | 536871040 | 0 | N/A | 72
PIN | RA<7> | 536871040 | 0 | N/A | 82
PIN | RA<8> | 536871040 | 0 | N/A | 88
PIN | RA<9> | 536871040 | 0 | N/A | 92
PIN | nBERR_FSB | 536871040 | 0 | N/A | 112
PIN | nOE | 536871040 | 0 | N/A | 60
PIN | nROMWE | 536871040 | 0 | N/A | 57
PIN | nVPA_FSB | 536871040 | 0 | N/A | 147
PIN | nDinLE | 536871040 | 0 | N/A | 140
PIN | nDoutOE | 536871040 | 0 | N/A | 143
PIN | nADoutLE0 | 536871040 | 0 | N/A | 139
PIN | nDinOE | 536871040 | 0 | N/A | 144
PIN | nRAS | 536871040 | 0 | N/A | 103
PIN | nCAS | 536871040 | 0 | N/A | 59
PIN | RA<11> | 536871040 | 0 | N/A | 102
PIN | RA<10> | 536871040 | 0 | N/A | 90
PIN | CLK20EN | 536871040 | 0 | N/A | 96
PIN | CLK25EN | 536871040 | 0 | N/A | 95
PIN | nBR_IOB | 536871040 | 0 | N/A | 116
PIN | nADoutLE1 | 536871040 | 0 | N/A | 136
PIN | nAoutOE | 536871040 | 0 | N/A | 141
PIN | nRAMLWE | 536871040 | 0 | N/A | 104
PIN | nRAMUWE | 536871040 | 0 | N/A | 105
PIN | nROMCS | 536871040 | 0 | N/A | 58
