Signal Name | Total Product Terms | Product Terms | Location | Power Mode | Pin Number | PinType | Pin Use
--- | --- | --- | --- | --- | --- | --- | ---
(unused) | 0 |  | MC1 |  |  | (b) |
(unused) | 0 |  | MC2 |  | 99 | I/O/GSR |
(unused) | 0 |  | MC3 |  |  | (b) |
(unused) | 0 |  | MC4 |  |  | (b) |
(unused) | 0 |  | MC5 |  | 1 | I/O/GTS3 |
(unused) | 0 |  | MC6 |  | 2 | I/O/GTS4 | I
iobs/IOACTr | 1 | 7_1 | MC7 | STD |  | (b) | (b)
iobm/VPArr | 1 | 8_1 | MC8 | STD | 3 | I/O/GTS1 | I
iobm/VPArf | 1 | 9_1 | MC9 | STD | 4 | I/O/GTS2 | I
iobm/IOREQr | 1 | 10_1 | MC10 | STD |  | (b) | (b)
iobm/Er2 | 1 | 11_1 | MC11 | STD | 6 | I/O | I
iobm/Er | 1 | 12_1 | MC12 | STD | 7 | I/O | I
iobm/DTACKrr | 1 | 13_1 | MC13 | STD |  | (b) | (b)
iobm/DTACKrf | 1 | 14_1 | MC14 | STD | 8 | I/O | I
iobm/BGr1 | 1 | 15_1 | MC15 | STD | 9 | I/O | I
iobm/BGr0 | 1 | 16_1 | MC16 | STD |  | (b) | (b)
iobm/BERRrr | 1 | 17_1 | MC17 | STD | 10 | I/O | I
cnt/RefCnt<0> | 0 |  | MC18 | STD |  | (b) | (b)

Signals Used By Logic in Function Block

1. E_IOB
2. iobm/BGr0
3. iobm/Er
4. iobm/IOACT
5. iobs/IOREQ
6. nBERR_IOB
7. nBG_IOB
8. nDTACK_IOB
9. nVPA_IOB