Signal Name | Total Product Terms | Product Terms | Location | Power Mode | Pin Number | PinType | Pin Use
--- | --- | --- | --- | --- | --- | --- | ---
ram/RefRAS | 1 | 1_1 | MC1 | STD |  | (b) | (b)
ram/BACTr | 1 | 2_1 | MC2 | STD | 11 | I/O | I
iobm/RESrr | 1 | 3_1 | MC3 | STD | 12 | I/O | I
iobm/RESrf | 1 | 4_1 | MC4 | STD |  | (b) | (b)
iobm/BERRrf | 1 | 5_1 | MC5 | STD | 13 | I/O | I
fsb/ASrf | 1 | 6_1 | MC6 | STD | 14 | I/O | I
cnt/RefCnt<1> | 1 | 7_1 | MC7 | STD |  | (b) | (b)
RESr2 | 1 | 8_1 | MC8 | STD | 15 | I/O | I
RESr1 | 1 | 9_1 | MC9 | STD | 16 | I/O | I
RESr0 | 1 | 10_1 | MC10 | STD |  | (b) | (b)
IPL2r1 | 1 | 11_1 | MC11 | STD | 17 | I/O | I
IPL2r0 | 1 | 12_1 | MC12 | STD | 18 | I/O | I
$OpTx$FX_DC$591 | 1 | 13_1 | MC13 | STD |  | (b) | (b)
iobs/IOU1 | 2 | 14_1 14_2 | MC14 | STD | 19 | I/O | I
iobs/IOL1 | 2 | 15_1 15_2 | MC15 | STD | 20 | I/O | I
iobm/IOS_FSM_FFd1 | 2 | 16_1 16_2 | MC16 | STD |  | (b) | (b)
fsb/BERR1r | 2 | 17_1 17_2 | MC17 | STD | 22 | I/O/GCK1 | GCK
cs/nOverlay1 | 2 | 18_1 18_2 | MC18 | STD |  | (b) | (b)

Signals Used By Logic in Function Block

1. IPL2r0
2. RESr0
3. RESr1
4. cnt/RefCnt<0>
5. cs/nOverlay0
6. fsb/ASrf
7. fsb/BERR1r
8. iobm/IOS_FSM_FFd1
9. iobm/IOS_FSM_FFd2
10. iobm/IOS_FSM_FFd3
11. iobs/BERR
12. iobs/Load1
13. nAS_FSB
14. nBERR_IOB
15. nIPL2
16. nLDS_FSB
17. nRES
18. nUDS_FSB
19. ram/RS_FSM_FFd1
20. ram/RS_FSM_FFd2