Signal Name | Total Product Terms | Product Terms | Location | Power Mode | Pin Number | PinType | Pin Use
--- | --- | --- | --- | --- | --- | --- | ---
iobs/Clear1 | 1 | 1_1 | MC1 | STD |  | (b) | (b)
nAoutOE | 3 | 2_1 2_2 2_3 | MC2 | STD | 87 | I/O | O
iobs/ALE0 | 1 | 3_1 | MC3 | STD |  | (b) | (b)
cnt/RefCnt<7> | 1 | 4_1 | MC4 | STD |  | (b) | (b)
nDoutOE | 2 | 5_1 5_2 | MC5 | STD | 89 | I/O | O
nDinOE | 3 | 6_1 6_2 6_3 | MC6 | STD | 90 | I/O | O
cnt/RefCnt<6> | 1 | 7_1 | MC7 | STD |  | (b) | (b)
cnt/RefCnt<5> | 1 | 8_1 | MC8 | STD | 91 | I/O | I
cnt/RefCnt<4> | 1 | 9_1 | MC9 | STD | 92 | I/O | I
cnt/RefCnt<3> | 1 | 10_1 | MC10 | STD |  | (b) | (b)
nVPA_FSB | 1 | 11_1 | MC11 | STD | 93 | I/O | O
cnt/RefCnt<2> | 1 | 12_1 | MC12 | STD | 94 | I/O | I
iobs/PS_FSM_FFd1 | 2 | 13_1 13_2 | MC13 | STD |  | (b) | (b)
cnt/RefDone | 2 | 14_1 14_2 | MC14 | STD | 95 | I/O | I
iobs/IOU0 | 3 | 15_1 15_2 15_3 | MC15 | STD | 96 | I/O | I
cnt/TimeoutA | 3 | 16_1 16_2 16_3 | MC16 | STD |  | (b) | (b)
iobs/IOReady | 4 | 17_1 17_2 17_3 17_4 | MC17 | STD | 97 | I/O | I
ram/RS_FSM_FFd1 | 8 | 17_5 18_1 18_2 18_3 18_4 18_5 1_2 1_3 | MC18 | STD |  | (b) | (b)

Signals Used By Logic in Function Block

1. A_FSB<20>
2. A_FSB<21>
3. A_FSB<22>
4. A_FSB<23>
5. SW<1>
6. cnt/RefCnt<0>
7. cnt/RefCnt<1>
8. cnt/RefCnt<2>
9. cnt/RefCnt<3>
10. cnt/RefCnt<4>
11. cnt/RefCnt<5>
12. cnt/RefCnt<6>
13. cnt/RefCnt<7>
14. cnt/RefDone
15. cnt/TimeoutA
16. cs/nOverlay1
17. fsb/ASrf
18. fsb/VPA
19. iobm/BGr0
20. iobm/BGr1
21. iobm/IOBERR
22. iobm/IOS_FSM_FFd2
23. iobm/IOS_FSM_FFd3
24. iobs/IOACTr
25. iobs/IORW0
26. iobs/IOReady
27. iobs/IOU1
28. iobs/Once
29. iobs/PS_FSM_FFd1
30. iobs/PS_FSM_FFd2
31. nADoutLE1
32. nAS_FSB
33. nAS_IOB
34. nAoutOE
35. nUDS_FSB
36. nWE_FSB
37. ram/Once
38. ram/RS_FSM_FFd1
39. ram/RS_FSM_FFd2
40. ram/RS_FSM_FFd3
41. ram/RefRAS