#Created by Constraints Editor (xc95144xl-tq100-10) - 2022/02/07
NET "CLK_FSB" TNM_NET = CLK_FSB;
TIMESPEC TS_CLK_FSB = PERIOD "CLK_FSB" 25 MHz HIGH 50%;
NET "CLK2X_IOB" TNM_NET = CLK2X_IOB;
TIMESPEC TS_CLK2X_IOB = PERIOD "CLK2X_IOB" 15.6672 MHz HIGH 50%;
NET "CLK_IOB" TNM_NET = CLK_IOB;
TIMESPEC TS_CLK_IOB = PERIOD "CLK_IOB" 7.8336 MHz HIGH 50%;
#PACE: Start of Constraints generated by PACE

#PACE: Start of PACE I/O Pin Assignments
NET "A_FSB<10>"  LOC = "P8"  ; 
NET "A_FSB<11>"  LOC = "P9"  ; 
NET "A_FSB<12>"  LOC = "P10"  ; 
NET "A_FSB<13>"  LOC = "P11"  ; 
NET "A_FSB<14>"  LOC = "P12"  ; 
NET "A_FSB<15>"  LOC = "P13"  ; 
NET "A_FSB<16>"  LOC = "P14"  ; 
NET "A_FSB<17>"  LOC = "P15"  ; 
NET "A_FSB<18>"  LOC = "P16"  ; 
NET "A_FSB<19>"  LOC = "P17"  ; 
NET "A_FSB<1>"  LOC = "P94"  ; 
NET "A_FSB<20>"  LOC = "P18"  ; 
NET "A_FSB<21>"  LOC = "P19"  ; 
NET "A_FSB<22>"  LOC = "P20"  ; 
NET "A_FSB<23>"  LOC = "P24"  ; 
NET "A_FSB<2>"  LOC = "P95"  ; 
NET "A_FSB<3>"  LOC = "P96"  ; 
NET "A_FSB<4>"  LOC = "P97"  ; 
NET "A_FSB<5>"  LOC = "P2"  ; 
NET "A_FSB<6>"  LOC = "P3"  ; 
NET "A_FSB<7>"  LOC = "P4"  ; 
NET "A_FSB<8>"  LOC = "P6"  ; 
NET "A_FSB<9>"  LOC = "P7"  ; 
NET "CLK20EN"  LOC = "P59"  ;
NET "CLK25EN"  LOC = "P58"  ;
NET "CLK2X_IOB"  LOC = "P22"  ; 
NET "CLK_FSB"  LOC = "P27"  ; 
NET "CLK_IOB"  LOC = "P23"  ; 
NET "E_IOB"  LOC = "P25"  ; 
NET "nADoutLE0"  LOC = "P85"  ; 
NET "nADoutLE1"  LOC = "P82"  ; 
NET "nAoutOE"  LOC = "P87"  ; 
NET "nAS_FSB"  LOC = "P32"  ; 
NET "nAS_IOB"  LOC = "P81"  ; 
NET "nBERR_FSB"  LOC = "P70"  ; 
NET "nBERR_IOB"  LOC = "P76"  ; 
NET "nBG_IOB"  LOC = "P73"  ;
NET "nBR_IOB"  LOC = "P72"  ;
NET "nCAS"  LOC = "P36"  ; 
NET "nDinLE"  LOC = "P86"  ; 
NET "nDinOE"  LOC = "P90"  ; 
NET "nDoutOE"  LOC = "P89"  ; 
NET "nDTACK_FSB"  LOC = "P28"  ; 
NET "nDTACK_IOB"  LOC = "P78"  ; 
NET "nIPL2"  LOC = "P92"  ;
NET "nLDS_FSB"  LOC = "P30"  ; 
NET "nLDS_IOB"  LOC = "P79"  ; 
NET "nOE"  LOC = "P37"  ; 
NET "nRAMLWE"  LOC = "P65"  ; 
NET "nRAMUWE"  LOC = "P66"  ; 
NET "nRAS"  LOC = "P64"  ; 
NET "nRES"  LOC = "P91"  ; 
NET "nROMCS"  LOC = "P35"  ; 
NET "nROMWE"  LOC = "P34"  ; 
NET "nUDS_FSB"  LOC = "P33"  ; 
NET "nUDS_IOB"  LOC = "P80"  ; 
NET "nVMA_IOB"  LOC = "P74"  ; 
NET "nVPA_FSB"  LOC = "P93"  ; 
NET "nVPA_IOB"  LOC = "P77"  ; 
NET "nWE_FSB"  LOC = "P29"  ; 
NET "RA<0>"  LOC = "P53"  ; 
NET "RA<10>"  LOC = "P55"  ; 
NET "RA<11>"  LOC = "P63"  ; 
NET "RA<1>"  LOC = "P50"  ; 
NET "RA<2>"  LOC = "P43"  ; 
NET "RA<3>"  LOC = "P41"  ; 
NET "RA<4>"  LOC = "P40"  ; 
NET "RA<5>"  LOC = "P42"  ; 
NET "RA<6>"  LOC = "P46"  ; 
NET "RA<7>"  LOC = "P52"  ; 
NET "RA<8>"  LOC = "P54"  ; 
NET "RA<9>"  LOC = "P56"  ; 
NET "SW<0>"  LOC = "P61"  ;
NET "SW<1>"  LOC = "P60"  ;
NET "SW<2>"  LOC = "P67"  ;

#PACE: Start of PACE Area Constraints

#PACE: Start of PACE Prohibit Constraints

#PACE: End of Constraints generated by PACE
