(module "0.5 AA to CR2032 pads" (layer F.Cu) (tedit 60C2A6F8)
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "0.5 AA to CR2032 pads" (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole oval (at -13 0) (size 2 19) (drill oval 1 18) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 13 0) (size 2 19) (drill oval 1 18) (layers *.Cu *.Mask))
)
