#PACE: Start of Constraints generated by PACE

#PACE: Start of PACE I/O Pin Assignments
NET "a10"  LOC = "P38"  ;
NET "a8"  LOC = "P36"  ;
NET "a9"  LOC = "P37"  ;
NET "addr<0>"  LOC = "P19"  ;
NET "addr<1>"  LOC = "P18"  ;
NET "b10"  LOC = "P22"  ;
NET "b8"  LOC = "P26"  ;
NET "b9"  LOC = "P27"  ;
NET "card"  LOC = "P33"  ;
NET "data<0>"  LOC = "P3"  ;
NET "data<1>"  LOC = "P4"  ;
NET "data<2>"  LOC = "P5"  ;
NET "data<3>"  LOC = "P6"  ;
NET "data<4>"  LOC = "P7"  ;
NET "data<5>"  LOC = "P9"  ;
NET "data<6>"  LOC = "P11"  ;
NET "data<7>"  LOC = "P13"  ;
NET "clk_7m"  LOC = "P43"  ;
NET "led"  LOC = "P29"  ;
NET "ndev_sel"  LOC = "P24"  ;
NET "ng"  LOC = "P12"  ;
NET "nio_sel"  LOC = "P14"  ;
NET "nio_stb"  LOC = "P42"  ;
NET "noe"  LOC = "P25"  ;
NET "clk_phi0"  LOC = "P8"  ;
NET "nreset"  LOC = "P20"  ;
NET "nrw"  LOC = "P1"  ;
NET "spi_miso"  LOC = "P40"  ;
NET "spi_mosi"  LOC = "P35"  ;
NET "spi_Nsel"  LOC = "P28"  ;
NET "spi_sclk"  LOC = "P34"  ;
NET "wp"  LOC = "P39"  ;

#PACE: Start of PACE Area Constraints

#PACE: Start of PACE Prohibit Constraints

#PACE: End of Constraints generated by PACE
