
palette	equ	$c000
vidmem	equ	$0
wdogx39	equ	$cbff

Start:
	ldx	#0
Loop:
        lda	>PALCONST,x
        sta	palette,x
        leax	1,x
        cpx	#16
        bne	Loop
        
	ldx	#0
Loop2:
        lda	#$39
        sta	wdogx39
        stx	,x
        leax	1,x
        cpx	#$9800
        bne	Loop2
        
	jmp	Loop	; endless loop

PALCONST:
	fcb	$1,$2,$4,$8,$10,$20,$40,$80
	fcb	$88,$c0,$e0,$f0,$f8,$fc,$fe,$ff
