/* Atari VCS C02 Program Template */

#include <vcshead.h02>  //TIA and RIOT Registers

//ROM Start Address  - $F800 for 2K, $F000 for 4K Cartridge
#pragma origin $F000

irqbrk: //Code to Execute when BRK Instruction is Encountered
start:  //Start of Program Code
  goto start;

#include <vcsfoot.h02>  //Finalization Code

