/* Joystick Module Header File for VIC-20 */

#define JYSTKS $01 //Number of Joysticks

#define JOYUP $04 //Bit 2 - Up    
#define JOYDN $08 //Bit 3 - Down  
#define JOYLF $10 //Bit 4 - Left  
#define JOYRT $01 //Bit 1 - Right 
#define JOYB0 $20 //Bit 5 - Button

/* Read Joystick State             *
 * Args: n = Joystick Number       *
 * Returns: Joystick Status        *
 *          $FF = Invalid Argument */
char joystk(); 
