/* C02 Minimal Header File for Apple II */

/* Monitor Variables */

//PIA 6820 Registers
char kbd;         //Keyboard Data
char kbdcr;       //Keyboard Control Register

//Monitor Subroutines
void echo();      //Print Character in Accumulator
void prbyte();    //Print Accumulator as Hexadadecimal number
void prhex();     //Print Low Nybble of Accumulator as Hex Digit

//System Subroutines
char rdkey();     //Wait for raw character from Keyboard
