__constant struct MOS6526_CIA * const CIA2 = (struct MOS6526_CIA *) 56576
__constant char * const CIA2_INTERRUPT = (char *) 56589
__constant const char CIA_INTERRUPT_CLEAR = $7f
__constant void (** const KERNEL_NMI)() = (void (**)()) 792
__constant char OFFSET_STRUCT_MOS6526_CIA_INTERRUPT = $d
__constant char OFFSET_STRUCT_MOS6526_CIA_TIMER_A = 4
__constant char OFFSET_STRUCT_MOS6526_CIA_TIMER_A_CONTROL = $e
__constant char OFFSET_STRUCT_MOS6569_VICII_BORDER_COLOR = $20
__constant char OFFSET_STRUCT_MOS6581_SID_VOLUME_FILTER_MODE = $18
__constant char SAMPLE[SAMPLE_SIZE] = kickasm {{ .import binary "moments_sample.bin"  }}
__constant const unsigned int SAMPLE_SIZE = $6100
__constant struct MOS6581_SID * const SID = (struct MOS6581_SID *) 54272
__constant struct MOS6569_VICII * const VICII = (struct MOS6569_VICII *) 53248
void __start()
void main()
__interrupt(hardware_clobber) void nmi()
char nmi::$1 // reg byte a 4.0
__interrupt(hardware_clobber) void nmi2()
char nmi2::$1 // reg byte a 4.0
char nmi2::$2 // reg byte a 4.0
__loadstore char * volatile sample // zp[2]:2 1.9999999999999996

zp[2]:2 [ sample ]
reg byte a [ nmi2::$1 ]
reg byte a [ nmi2::$2 ]
reg byte a [ nmi::$1 ]
